# Static Call Graph for image flexspi_nor_release\LED_I2C_TEST.out

#<CALLGRAPH># ARM Linker, 6220000: Last Updated: Sun Mar 16 20:47:13 2025

### Maximum Stack Usage = 176 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ IS31FL3729_Init ⇒ I2C_WriteReg ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady

### Functions with no stack information

- Reset_Handler
- ACMP1_IRQHandler
- ACMP2_IRQHandler
- ACMP3_IRQHandler
- ACMP4_IRQHandler
- ADC1_IRQHandler
- ADC2_IRQHandler
- ADC_ETC_ERROR_IRQ_IRQHandler
- ADC_ETC_IRQ0_IRQHandler
- ADC_ETC_IRQ1_IRQHandler
- ADC_ETC_IRQ2_IRQHandler
- BEE_IRQHandler
- BusFault_Handler
- CAN1_DriverIRQHandler
- CAN2_DriverIRQHandler
- CAN3_DriverIRQHandler
- CCM_1_IRQHandler
- CCM_2_IRQHandler
- CORE_IRQHandler
- CSI_IRQHandler
- CSU_IRQHandler
- CTI0_ERROR_IRQHandler
- CTI1_ERROR_IRQHandler
- DCDC_IRQHandler
- DCP_IRQHandler
- DCP_VMI_IRQHandler
- DMA0_DMA16_DriverIRQHandler
- DMA10_DMA26_DriverIRQHandler
- DMA11_DMA27_DriverIRQHandler
- DMA12_DMA28_DriverIRQHandler
- DMA13_DMA29_DriverIRQHandler
- DMA14_DMA30_DriverIRQHandler
- DMA15_DMA31_DriverIRQHandler
- DMA1_DMA17_DriverIRQHandler
- DMA2_DMA18_DriverIRQHandler
- DMA3_DMA19_DriverIRQHandler
- DMA4_DMA20_DriverIRQHandler
- DMA5_DMA21_DriverIRQHandler
- DMA6_DMA22_DriverIRQHandler
- DMA7_DMA23_DriverIRQHandler
- DMA8_DMA24_DriverIRQHandler
- DMA9_DMA25_DriverIRQHandler
- DMA_ERROR_DriverIRQHandler
- DebugMon_Handler
- DefaultISR
- ENC1_IRQHandler
- ENC2_IRQHandler
- ENC3_IRQHandler
- ENC4_IRQHandler
- ENET2_1588_Timer_DriverIRQHandler
- ENET2_DriverIRQHandler
- ENET_1588_Timer_DriverIRQHandler
- ENET_DriverIRQHandler
- EWM_IRQHandler
- FLEXIO1_DriverIRQHandler
- FLEXIO2_DriverIRQHandler
- FLEXIO3_DriverIRQHandler
- FLEXRAM_IRQHandler
- FLEXSPI2_DriverIRQHandler
- FLEXSPI_DriverIRQHandler
- GPC_IRQHandler
- GPIO10_Combined_0_31_IRQHandler
- GPIO1_Combined_0_15_IRQHandler
- GPIO1_Combined_16_31_IRQHandler
- GPIO1_INT0_IRQHandler
- GPIO1_INT1_IRQHandler
- GPIO1_INT2_IRQHandler
- GPIO1_INT3_IRQHandler
- GPIO1_INT4_IRQHandler
- GPIO1_INT5_IRQHandler
- GPIO1_INT6_IRQHandler
- GPIO1_INT7_IRQHandler
- GPIO2_Combined_0_15_IRQHandler
- GPIO2_Combined_16_31_IRQHandler
- GPIO3_Combined_0_15_IRQHandler
- GPIO3_Combined_16_31_IRQHandler
- GPIO4_Combined_0_15_IRQHandler
- GPIO4_Combined_16_31_IRQHandler
- GPIO5_Combined_0_15_IRQHandler
- GPIO5_Combined_16_31_IRQHandler
- GPIO6_7_8_9_IRQHandler
- GPR_IRQ_IRQHandler
- GPT1_IRQHandler
- GPT2_IRQHandler
- KPP_IRQHandler
- LCDIF_IRQHandler
- LPSPI1_DriverIRQHandler
- LPSPI2_DriverIRQHandler
- LPSPI3_DriverIRQHandler
- LPSPI4_DriverIRQHandler
- MemManage_Handler
- PIT_IRQHandler
- PMU_EVENT_IRQHandler
- PWM1_0_IRQHandler
- PWM1_1_IRQHandler
- PWM1_2_IRQHandler
- PWM1_3_IRQHandler
- PWM1_FAULT_IRQHandler
- PWM2_0_IRQHandler
- PWM2_1_IRQHandler
- PWM2_2_IRQHandler
- PWM2_3_IRQHandler
- PWM2_FAULT_IRQHandler
- PWM3_0_IRQHandler
- PWM3_1_IRQHandler
- PWM3_2_IRQHandler
- PWM3_3_IRQHandler
- PWM3_FAULT_IRQHandler
- PWM4_0_IRQHandler
- PWM4_1_IRQHandler
- PWM4_2_IRQHandler
- PWM4_3_IRQHandler
- PWM4_FAULT_IRQHandler
- PXP_IRQHandler
- RTWDOG_IRQHandler
- Reserved115_IRQHandler
- Reserved143_IRQHandler
- Reserved144_IRQHandler
- Reserved171_IRQHandler
- Reserved68_IRQHandler
- Reserved78_IRQHandler
- Reserved86_IRQHandler
- SAI1_DriverIRQHandler
- SAI2_DriverIRQHandler
- SAI3_RX_DriverIRQHandler
- SAI3_TX_DriverIRQHandler
- SEMC_IRQHandler
- SJC_IRQHandler
- SNVS_HP_WRAPPER_IRQHandler
- SNVS_HP_WRAPPER_TZ_IRQHandler
- SNVS_LP_WRAPPER_IRQHandler
- SPDIF_DriverIRQHandler
- SRC_IRQHandler
- TEMP_LOW_HIGH_IRQHandler
- TEMP_PANIC_IRQHandler
- TMR1_IRQHandler
- TMR2_IRQHandler
- TMR3_IRQHandler
- TMR4_IRQHandler
- TRNG_IRQHandler
- TSC_DIG_IRQHandler
- USB_OTG1_IRQHandler
- USB_OTG2_IRQHandler
- USB_PHY1_IRQHandler
- USB_PHY2_IRQHandler
- USDHC1_DriverIRQHandler
- USDHC2_DriverIRQHandler
- UsageFault_Handler
- WDOG1_IRQHandler
- WDOG2_IRQHandler
- XBAR1_IRQ_0_1_IRQHandler
- XBAR1_IRQ_2_3_IRQHandler
- NMI_Handler
- HardFault_Handler
- SVC_Handler
- PendSV_Handler
- SysTick_Handler
- DMA0_DMA16_IRQHandler
- DMA1_DMA17_IRQHandler
- DMA2_DMA18_IRQHandler
- DMA3_DMA19_IRQHandler
- DMA4_DMA20_IRQHandler
- DMA5_DMA21_IRQHandler
- DMA6_DMA22_IRQHandler
- DMA7_DMA23_IRQHandler
- DMA8_DMA24_IRQHandler
- DMA9_DMA25_IRQHandler
- DMA10_DMA26_IRQHandler
- DMA11_DMA27_IRQHandler
- DMA12_DMA28_IRQHandler
- DMA13_DMA29_IRQHandler
- DMA14_DMA30_IRQHandler
- DMA15_DMA31_IRQHandler
- DMA_ERROR_IRQHandler
- LPUART1_IRQHandler
- LPUART2_IRQHandler
- LPUART3_IRQHandler
- LPUART4_IRQHandler
- LPUART5_IRQHandler
- LPUART6_IRQHandler
- LPUART7_IRQHandler
- LPUART8_IRQHandler
- LPI2C1_IRQHandler
- LPI2C2_IRQHandler
- LPI2C3_IRQHandler
- LPI2C4_IRQHandler
- LPSPI1_IRQHandler
- LPSPI2_IRQHandler
- LPSPI3_IRQHandler
- LPSPI4_IRQHandler
- CAN1_IRQHandler
- CAN2_IRQHandler
- SAI1_IRQHandler
- SAI2_IRQHandler
- SAI3_RX_IRQHandler
- SAI3_TX_IRQHandler
- SPDIF_IRQHandler
- FLEXIO1_IRQHandler
- FLEXIO2_IRQHandler
- FLEXSPI2_IRQHandler
- FLEXSPI_IRQHandler
- USDHC1_IRQHandler
- USDHC2_IRQHandler
- ENET_IRQHandler
- ENET_1588_Timer_IRQHandler
- ENET2_IRQHandler
- ENET2_1588_Timer_IRQHandler
- CAN3_IRQHandler
- FLEXIO3_IRQHandler

### Mutually Recursive functions

- LPUART_WriteBlocking ⇒ LPUART_WriteBlocking

  ### Function Pointers

  - ACMP1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ACMP2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ACMP3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ACMP4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ADC1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ADC2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ADC_ETC_ERROR_IRQ_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ADC_ETC_IRQ0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ADC_ETC_IRQ1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ADC_ETC_IRQ2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - BEE_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - BusFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CAN1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - CAN1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CAN2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - CAN2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CAN3_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - CAN3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CCM_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CCM_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CLOCK_DisableClock from clock_config.o(.text.CLOCK_DisableClock) referenced from clock_config.o(.text.BOARD_BootClockRUN)
  - CLOCK_InitSysPfd from fsl_clock.o(.text.CLOCK_InitSysPfd) referenced from clock_config.o(.text.BOARD_BootClockRUN)
  - CLOCK_SetDiv from clock_config.o(.text.CLOCK_SetDiv) referenced from clock_config.o(.text.BOARD_BootClockRUN)
  - CLOCK_SetMux from clock_config.o(.text.CLOCK_SetMux) referenced from clock_config.o(.text.BOARD_BootClockRUN)
  - CORE_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CSI_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CSU_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CTI0_ERROR_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - CTI1_ERROR_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DCDC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DCP_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DCP_VMI_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA0_DMA16_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA0_DMA16_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA10_DMA26_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA10_DMA26_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA11_DMA27_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA11_DMA27_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA12_DMA28_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA12_DMA28_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA13_DMA29_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA13_DMA29_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA14_DMA30_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA14_DMA30_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA15_DMA31_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA15_DMA31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA1_DMA17_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA1_DMA17_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA2_DMA18_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA2_DMA18_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA3_DMA19_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA3_DMA19_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA4_DMA20_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA4_DMA20_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA5_DMA21_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA5_DMA21_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA6_DMA22_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA6_DMA22_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA7_DMA23_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA7_DMA23_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA8_DMA24_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA8_DMA24_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA9_DMA25_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA9_DMA25_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DMA_ERROR_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - DMA_ERROR_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DebugMon_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - DefaultISR from startup_mimxrt1062.o(.text) referenced 9 times from fsl_lpuart.o(.data.s_lpuartIsr)
  - DefaultISR from startup_mimxrt1062.o(.text) referenced 81 times from startup_mimxrt1062.o(.isr_vector)
  - ENC1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ENC2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ENC3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ENC4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ENET2_1588_Timer_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - ENET2_1588_Timer_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ENET2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - ENET2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ENET_1588_Timer_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - ENET_1588_Timer_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - ENET_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - ENET_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - EWM_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - FLEXIO1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - FLEXIO1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - FLEXIO2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - FLEXIO2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - FLEXIO3_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - FLEXIO3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - FLEXRAM_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - FLEXSPI2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - FLEXSPI2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - FLEXSPI_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - FLEXSPI_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO10_Combined_0_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT5_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT6_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO1_INT7_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO2_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO2_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO3_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO3_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO4_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO4_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO5_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO5_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPIO6_7_8_9_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPR_IRQ_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPT1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - GPT2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - HAL_UartReceiveBlocking from fsl_adapter_lpuart.o(.text.HAL_UartReceiveBlocking) referenced from fsl_debug_console.o(.text.DbgConsole_Init)
  - HAL_UartSendBlocking from fsl_adapter_lpuart.o(.text.HAL_UartSendBlocking) referenced from fsl_debug_console.o(.text.DbgConsole_Init)
  - HardFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - HardFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - KPP_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LCDIF_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPI2C1_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C1_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPI2C1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPI2C2_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C2_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPI2C2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPI2C3_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C3_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPI2C3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPI2C4_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C4_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPI2C4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPSPI1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - LPSPI1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPSPI2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - LPSPI2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPSPI3_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - LPSPI3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPSPI4_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - LPSPI4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART1_DriverIRQHandler from fsl_lpuart.o(.text.LPUART1_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART2_DriverIRQHandler from fsl_lpuart.o(.text.LPUART2_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART3_DriverIRQHandler from fsl_lpuart.o(.text.LPUART3_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART4_DriverIRQHandler from fsl_lpuart.o(.text.LPUART4_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART5_DriverIRQHandler from fsl_lpuart.o(.text.LPUART5_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART5_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART6_DriverIRQHandler from fsl_lpuart.o(.text.LPUART6_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART6_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART7_DriverIRQHandler from fsl_lpuart.o(.text.LPUART7_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART7_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - LPUART8_DriverIRQHandler from fsl_lpuart.o(.text.LPUART8_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
  - LPUART8_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - MemManage_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - NMI_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - NMI_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - PIT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PMU_EVENT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM1_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM1_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM1_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM1_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM1_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM2_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM2_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM2_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM2_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM2_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM3_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM3_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM3_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM3_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM3_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM4_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM4_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM4_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM4_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PWM4_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PXP_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PendSV_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - PendSV_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - RTWDOG_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reserved115_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reserved143_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reserved144_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reserved171_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reserved68_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reserved78_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reserved86_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - Reset_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SAI1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - SAI1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SAI2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - SAI2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SAI3_RX_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - SAI3_RX_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SAI3_TX_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - SAI3_TX_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SEMC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SJC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SNVS_HP_WRAPPER_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SNVS_HP_WRAPPER_TZ_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SNVS_LP_WRAPPER_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SPDIF_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - SPDIF_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SRC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SVC_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SVC_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - SysTick_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - SysTick_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - SystemInit from system_mimxrt1062.o(.text.SystemInit) referenced from startup_mimxrt1062.o(.text)
  - TEMP_LOW_HIGH_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - TEMP_PANIC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - TMR1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - TMR2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - TMR3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - TMR4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - TRNG_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - TSC_DIG_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - USB_OTG1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - USB_OTG2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - USB_PHY1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - USB_PHY2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - USDHC1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - USDHC1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - USDHC2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
  - USDHC2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - UsageFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - WDOG1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - WDOG2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - XBAR1_IRQ_0_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - XBAR1_IRQ_2_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_mimxrt1062.o(.text)
  - main from main.o(.text.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry4.o(.ARM.Collect$$$$00000003))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 40 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ACMP1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Calls]

  - >> DefaultISR
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.isr_vector)

  ACMP2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ACMP3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ACMP4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ADC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ADC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ADC_ETC_ERROR_IRQ_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ADC_ETC_IRQ0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ADC_ETC_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ADC_ETC_IRQ2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  BEE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  BusFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CAN1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  CAN2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  CAN3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  CCM_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CCM_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CORE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CSI_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CSU_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CTI0_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CTI1_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DCDC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DCP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DCP_VMI_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA0_DMA16_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA10_DMA26_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA11_DMA27_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA12_DMA28_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA13_DMA29_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA14_DMA30_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA15_DMA31_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA1_DMA17_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA2_DMA18_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA3_DMA19_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA4_DMA20_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA5_DMA21_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA6_DMA22_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA7_DMA23_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA8_DMA24_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA9_DMA25_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DMA_ERROR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  DebugMon_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DefaultISR (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Called By]

  - >> ACMP1_IRQHandler
  [Address Reference Count : 2]
  - startup_mimxrt1062.o(.isr_vector)
  - fsl_lpuart.o(.data.s_lpuartIsr)

  ENC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENC3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENC4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENET2_1588_Timer_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  ENET2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  ENET_1588_Timer_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  ENET_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  EWM_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  FLEXIO1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  FLEXIO2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  FLEXIO3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  FLEXRAM_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  FLEXSPI2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  FLEXSPI_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  GPC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO10_Combined_0_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO1_INT7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO2_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO2_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO3_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO3_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO4_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO4_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO5_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO5_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPIO6_7_8_9_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPR_IRQ_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  GPT2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  KPP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LCDIF_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPSPI1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  LPSPI2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  LPSPI3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  LPSPI4_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  MemManage_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PIT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PMU_EVENT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM1_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM1_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM1_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM1_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM1_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM2_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM2_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM2_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM2_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM2_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM3_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM3_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM3_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM3_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM3_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM4_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM4_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM4_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM4_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PWM4_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  PXP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  RTWDOG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  Reserved115_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  Reserved143_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  Reserved144_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  Reserved171_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  Reserved68_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  Reserved78_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  Reserved86_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SAI1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  SAI2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  SAI3_RX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  SAI3_TX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  SEMC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SJC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SNVS_HP_WRAPPER_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SNVS_HP_WRAPPER_TZ_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SNVS_LP_WRAPPER_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SPDIF_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  SRC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TEMP_LOW_HIGH_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TEMP_PANIC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TMR1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TMR2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TMR3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TMR4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TRNG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  TSC_DIG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  USB_OTG1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  USB_OTG2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  USB_PHY1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  USB_PHY2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  USDHC1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  USDHC2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.text)

  UsageFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  WDOG1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  WDOG2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  XBAR1_IRQ_0_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  XBAR1_IRQ_2_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  NMI_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 2]

  - startup_mimxrt1062.o(.text)
  - startup_mimxrt1062.o(.isr_vector)

  HardFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 2]

  - startup_mimxrt1062.o(.text)
  - startup_mimxrt1062.o(.isr_vector)

  SVC_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 2]

  - startup_mimxrt1062.o(.text)
  - startup_mimxrt1062.o(.isr_vector)

  PendSV_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 2]

  - startup_mimxrt1062.o(.text)
  - startup_mimxrt1062.o(.isr_vector)

  SysTick_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 2]

  - startup_mimxrt1062.o(.text)
  - startup_mimxrt1062.o(.isr_vector)

  DMA0_DMA16_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA1_DMA17_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA2_DMA18_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA3_DMA19_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA4_DMA20_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA5_DMA21_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA6_DMA22_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA7_DMA23_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA8_DMA24_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA9_DMA25_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA10_DMA26_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA11_DMA27_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA12_DMA28_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA13_DMA29_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA14_DMA30_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA15_DMA31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  DMA_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPUART8_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPI2C1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPI2C2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPI2C3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPI2C4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPSPI1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPSPI2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPSPI3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  LPSPI4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CAN1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CAN2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SAI1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SAI2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SAI3_RX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SAI3_TX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  SPDIF_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  FLEXIO1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  FLEXIO2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  FLEXSPI2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  FLEXSPI_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  USDHC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  USDHC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENET_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENET_1588_Timer_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENET2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  ENET2_1588_Timer_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  CAN3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  FLEXIO3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
  [Address Reference Count : 1]

  - startup_mimxrt1062.o(.isr_vector)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> SDK_DelayAtLeastUs
  - >> OUTLINED_FUNCTION_12
  - >> SystemCoreClockUpdate

  memset (Thumb, 18 bytes, Stack size 8 bytes, memset.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = memset
  [Called By]
  - >> LPI2C_SlaveTransferHandleIRQ
  - >> LPI2C_MasterGetDefaultConfig
  - >> LPUART_GetDefaultConfig

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __scatterload (Thumb, 38 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BOARD_BootClockRUN (Thumb, 876 bytes, Stack size 40 bytes, clock_config.o(.text.BOARD_BootClockRUN))
  [Stack]

  - Max Depth = 56
  - Call Chain = BOARD_BootClockRUN ⇒ CLOCK_SetMux
  [Calls]
  - >> CLOCK_DeinitAudioPll
  - >> CLOCK_InitSysPll
  - >> CLOCK_InitArmPll
  - >> CLOCK_SwitchOsc
  - >> CLOCK_InitRcOsc24M
  - >> CLOCK_InitExternalClk
  - >> OUTLINED_FUNCTION_1
  - >> OUTLINED_FUNCTION_3
  - >> OUTLINED_FUNCTION_8
  - >> OUTLINED_FUNCTION_2
  - >> OUTLINED_FUNCTION_6
  - >> OUTLINED_FUNCTION_0
  - >> CLOCK_SetMux
  - >> OUTLINED_FUNCTION_7
  - >> OUTLINED_FUNCTION_5
  [Called By]
  - >> BOARD_InitBootClocks

  BOARD_ConfigMPU (Thumb, 520 bytes, Stack size 24 bytes, board.o(.text.BOARD_ConfigMPU))
  [Stack]

  - Max Depth = 24
  - Call Chain = BOARD_ConfigMPU
  [Called By]
  - >> BOARD_InitHardware

  BOARD_DebugConsoleSrcFreq (Thumb, 52 bytes, Stack size 8 bytes, board.o(.text.BOARD_DebugConsoleSrcFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = BOARD_DebugConsoleSrcFreq ⇒ CLOCK_GetPllFreq
  [Calls]
  - >> CLOCK_GetPllFreq
  [Called By]
  - >> BOARD_InitDebugConsole

  BOARD_InitBootClocks (Thumb, 4 bytes, Stack size 0 bytes, clock_config.o(.text.BOARD_InitBootClocks))
  [Stack]

  - Max Depth = 56
  - Call Chain = BOARD_InitBootClocks ⇒ BOARD_BootClockRUN ⇒ CLOCK_SetMux
  [Calls]
  - >> BOARD_BootClockRUN
  [Called By]
  - >> BOARD_InitHardware

  BOARD_InitBootPins (Thumb, 4 bytes, Stack size 0 bytes, pin_mux.o(.text.BOARD_InitBootPins))
  [Calls]

  - >> BOARD_InitPins
  [Called By]
  - >> BOARD_InitHardware

  BOARD_InitDebugConsole (Thumb, 24 bytes, Stack size 8 bytes, board.o(.text.BOARD_InitDebugConsole))
  [Stack]

  - Max Depth = 136
  - Call Chain = BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ LPUART_Init ⇒ CLOCK_ControlGate
  [Calls]
  - >> DbgConsole_Init
  - >> BOARD_DebugConsoleSrcFreq
  [Called By]
  - >> BOARD_InitHardware

  BOARD_InitHardware (Thumb, 64 bytes, Stack size 8 bytes, hardware_init.o(.text.BOARD_InitHardware))
  [Stack]

  - Max Depth = 144
  - Call Chain = BOARD_InitHardware ⇒ BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ LPUART_Init ⇒ CLOCK_ControlGate
  [Calls]
  - >> SystemCoreClockUpdate
  - >> BOARD_InitBootPins
  - >> BOARD_InitBootClocks
  - >> BOARD_ConfigMPU
  - >> BOARD_InitDebugConsole
  [Called By]
  - >> main

  BOARD_InitPins (Thumb, 48 bytes, Stack size 0 bytes, pin_mux.o(.text.BOARD_InitPins))
  [Called By]

  - >> BOARD_InitBootPins

  CLOCK_DeinitAudioPll (Thumb, 8 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_DeinitAudioPll))
  [Calls]

  - >> OUTLINED_FUNCTION_4
  [Called By]
  - >> BOARD_BootClockRUN

  CLOCK_DeinitEnetPll (Thumb, 8 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_DeinitEnetPll))
  [Calls]

  - >> OUTLINED_FUNCTION_4
  [Called By]
  - >> OUTLINED_FUNCTION_6

  CLOCK_DeinitUsb2Pll (Thumb, 8 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_DeinitUsb2Pll))
  [Called By]

  - >> OUTLINED_FUNCTION_2

  CLOCK_GetAhbFreq (Thumb, 24 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetAhbFreq))
  [Stack]

  - Max Depth = 64
  - Call Chain = CLOCK_GetAhbFreq ⇒ CLOCK_GetPeriphClkFreq ⇒ CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> CLOCK_GetPeriphClkFreq
  [Called By]
  - >> CLOCK_GetFreq
  - >> CLOCK_GetIpgFreq

  CLOCK_GetFreq (Thumb, 244 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetFreq))
  [Stack]

  - Max Depth = 88
  - Call Chain = CLOCK_GetFreq ⇒ CLOCK_GetPerClkFreq ⇒ CLOCK_GetIpgFreq ⇒ CLOCK_GetAhbFreq ⇒ CLOCK_GetPeriphClkFreq ⇒ CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> CLOCK_GetPerClkFreq
  - >> CLOCK_GetIpgFreq
  - >> CLOCK_GetUsb1PfdFreq
  - >> CLOCK_GetSemcFreq
  - >> CLOCK_GetSysPfdFreq
  - >> CLOCK_GetAhbFreq
  - >> CLOCK_GetPllUsb1SWFreq
  - >> CLOCK_GetPllFreq
  [Called By]
  - >> IS31FL3729_Init
  - >> main
  - >> OUTLINED_FUNCTION_1

  CLOCK_GetIpgFreq (Thumb, 24 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetIpgFreq))
  [Stack]

  - Max Depth = 72
  - Call Chain = CLOCK_GetIpgFreq ⇒ CLOCK_GetAhbFreq ⇒ CLOCK_GetPeriphClkFreq ⇒ CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> CLOCK_GetAhbFreq
  [Called By]
  - >> CLOCK_GetFreq
  - >> CLOCK_GetPerClkFreq

  CLOCK_GetPerClkFreq (Thumb, 40 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetPerClkFreq))
  [Stack]

  - Max Depth = 80
  - Call Chain = CLOCK_GetPerClkFreq ⇒ CLOCK_GetIpgFreq ⇒ CLOCK_GetAhbFreq ⇒ CLOCK_GetPeriphClkFreq ⇒ CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> CLOCK_GetIpgFreq
  - >> OUTLINED_FUNCTION_5
  [Called By]
  - >> CLOCK_GetFreq

  CLOCK_GetPllFreq (Thumb, 420 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetPllFreq))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_GetPllFreq
  [Calls]
  - >> OUTLINED_FUNCTION_9
  [Called By]
  - >> CLOCK_GetFreq
  - >> CLOCK_GetUsb1PfdFreq
  - >> CLOCK_GetSysPfdFreq
  - >> CLOCK_GetPllUsb1SWFreq
  - >> CLOCK_GetPeriphClkFreq
  - >> BOARD_DebugConsoleSrcFreq

  CLOCK_GetSemcFreq (Thumb, 48 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetSemcFreq))
  [Stack]

  - Max Depth = 64
  - Call Chain = CLOCK_GetSemcFreq ⇒ CLOCK_GetPeriphClkFreq ⇒ CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> CLOCK_GetUsb1PfdFreq
  - >> CLOCK_GetSysPfdFreq
  - >> OUTLINED_FUNCTION_5
  - >> CLOCK_GetPeriphClkFreq
  [Called By]
  - >> CLOCK_GetFreq

  CLOCK_GetSysPfdFreq (Thumb, 68 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetSysPfdFreq))
  [Stack]

  - Max Depth = 48
  - Call Chain = CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> OUTLINED_FUNCTION_12
  - >> CLOCK_GetPllFreq
  [Called By]
  - >> CLOCK_GetFreq
  - >> CLOCK_GetSemcFreq
  - >> CLOCK_GetPeriphClkFreq

  CLOCK_GetUsb1PfdFreq (Thumb, 68 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetUsb1PfdFreq))
  [Stack]

  - Max Depth = 48
  - Call Chain = CLOCK_GetUsb1PfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> OUTLINED_FUNCTION_12
  - >> CLOCK_GetPllFreq
  [Called By]
  - >> CLOCK_GetFreq
  - >> CLOCK_GetSemcFreq

  CLOCK_InitArmPll (Thumb, 56 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitArmPll))
  [Calls]

  - >> OUTLINED_FUNCTION_3
  [Called By]
  - >> BOARD_BootClockRUN

  CLOCK_InitExternalClk (Thumb, 36 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitExternalClk))
  [Called By]

  - >> BOARD_BootClockRUN

  CLOCK_InitRcOsc24M (Thumb, 12 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitRcOsc24M))
  [Called By]

  - >> BOARD_BootClockRUN

  CLOCK_InitSysPfd (Thumb, 8 bytes, Stack size 16 bytes, fsl_clock.o(.text.CLOCK_InitSysPfd))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_InitSysPfd
  [Calls]
  - >> OUTLINED_FUNCTION_1
  [Address Reference Count : 1]
  - clock_config.o(.text.BOARD_BootClockRUN)

  CLOCK_InitSysPll (Thumb, 92 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitSysPll))
  [Calls]

  - >> OUTLINED_FUNCTION_3
  [Called By]
  - >> BOARD_BootClockRUN

  CLOCK_SwitchOsc (Thumb, 24 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_SwitchOsc))
  [Called By]

  - >> BOARD_BootClockRUN

  DbgConsole_Init (Thumb, 60 bytes, Stack size 40 bytes, fsl_debug_console.o(.text.DbgConsole_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = DbgConsole_Init ⇒ HAL_UartInit ⇒ LPUART_Init ⇒ CLOCK_ControlGate
  [Calls]
  - >> HAL_UartInit
  [Called By]
  - >> BOARD_InitDebugConsole

  HAL_UartInit (Thumb, 152 bytes, Stack size 40 bytes, fsl_adapter_lpuart.o(.text.HAL_UartInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UartInit ⇒ LPUART_Init ⇒ CLOCK_ControlGate
  [Calls]
  - >> LPUART_Init
  - >> LPUART_GetDefaultConfig
  [Called By]
  - >> DbgConsole_Init

  HAL_UartReceiveBlocking (Thumb, 24 bytes, Stack size 8 bytes, fsl_adapter_lpuart.o(.text.HAL_UartReceiveBlocking))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_UartReceiveBlocking ⇒ LPUART_ReadBlocking ⇒ OUTLINED_FUNCTION_1
  [Calls]
  - >> LPUART_ReadBlocking
  [Address Reference Count : 1]
  - fsl_debug_console.o(.text.DbgConsole_Init)

  HAL_UartSendBlocking (Thumb, 20 bytes, Stack size 8 bytes, fsl_adapter_lpuart.o(.text.HAL_UartSendBlocking))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UartSendBlocking
  [Calls]
  - >> LPUART_WriteBlocking
  [Address Reference Count : 1]
  - fsl_debug_console.o(.text.DbgConsole_Init)

  IS31FL3729_EnableOutput (Thumb, 8 bytes, Stack size 0 bytes, is31fl3729.o(.text.IS31FL3729_EnableOutput))
  [Stack]

  - Max Depth = 112
  - Call Chain = IS31FL3729_EnableOutput ⇒ I2C_WriteReg ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> I2C_WriteReg
  [Called By]
  - >> main

  IS31FL3729_Init (Thumb, 196 bytes, Stack size 48 bytes, is31fl3729.o(.text.IS31FL3729_Init))
  [Stack]

  - Max Depth = 160
  - Call Chain = IS31FL3729_Init ⇒ I2C_WriteReg ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> LPI2C_MasterInit
  - >> LPI2C_MasterGetDefaultConfig
  - >> SDK_DelayAtLeastUs
  - >> CLOCK_GetFreq
  - >> OUTLINED_FUNCTION_0
  - >> OUTLINED_FUNCTION_1
  - >> I2C_WriteReg
  [Called By]
  - >> main

  IS31FL3729_SetLED (Thumb, 30 bytes, Stack size 0 bytes, is31fl3729.o(.text.IS31FL3729_SetLED))
  [Stack]

  - Max Depth = 112
  - Call Chain = IS31FL3729_SetLED ⇒ I2C_WriteReg ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> I2C_WriteReg
  [Called By]
  - >> main

  LPI2C1_DriverIRQHandler (Thumb, 8 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.LPI2C1_DriverIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LPI2C1_DriverIRQHandler ⇒ LPI2C_CommonIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset
  [Calls]
  - >> LPI2C_CommonIRQHandler
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPI2C2_DriverIRQHandler (Thumb, 8 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.LPI2C2_DriverIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LPI2C2_DriverIRQHandler ⇒ LPI2C_CommonIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset
  [Calls]
  - >> LPI2C_CommonIRQHandler
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPI2C3_DriverIRQHandler (Thumb, 8 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.LPI2C3_DriverIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LPI2C3_DriverIRQHandler ⇒ LPI2C_CommonIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset
  [Calls]
  - >> LPI2C_CommonIRQHandler
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPI2C4_DriverIRQHandler (Thumb, 8 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.LPI2C4_DriverIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LPI2C4_DriverIRQHandler ⇒ LPI2C_CommonIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset
  [Calls]
  - >> LPI2C_CommonIRQHandler
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPI2C_GetInstance (Thumb, 24 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.LPI2C_GetInstance))
  [Called By]

  - >> LPI2C_MasterInit

  LPI2C_MasterCheckAndClearError (Thumb, 78 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.LPI2C_MasterCheckAndClearError))
  [Called By]

  - >> LPI2C_MasterReceive
  - >> LPI2C_MasterStop
  - >> LPI2C_MasterWaitForTxReady

  LPI2C_MasterGetDefaultConfig (Thumb, 44 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_MasterGetDefaultConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = LPI2C_MasterGetDefaultConfig ⇒ memset
  [Calls]
  - >> memset
  [Called By]
  - >> IS31FL3729_Init

  LPI2C_MasterInit (Thumb, 216 bytes, Stack size 24 bytes, fsl_lpi2c.o(.text.LPI2C_MasterInit))
  [Stack]

  - Max Depth = 84
  - Call Chain = LPI2C_MasterInit ⇒ LPI2C_MasterSetBaudRate
  [Calls]
  - >> LPI2C_MasterSetBaudRate
  - >> LPI2C_GetInstance
  - >> OUTLINED_FUNCTION_2
  - >> LPI2C_GetCyclesForWidth
  - >> CLOCK_EnableClock
  [Called By]
  - >> IS31FL3729_Init

  LPI2C_MasterReceive (Thumb, 96 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_MasterReceive))
  [Stack]

  - Max Depth = 32
  - Call Chain = LPI2C_MasterReceive ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> LPI2C_MasterCheckAndClearError
  - >> LPI2C_MasterWaitForTxReady
  [Called By]
  - >> LPI2C_MasterTransferBlocking

  LPI2C_MasterSend (Thumb, 32 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_MasterSend))
  [Stack]

  - Max Depth = 32
  - Call Chain = LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> LPI2C_MasterWaitForTxReady
  [Called By]
  - >> LPI2C_MasterTransferBlocking

  LPI2C_MasterSetBaudRate (Thumb, 354 bytes, Stack size 60 bytes, fsl_lpi2c.o(.text.LPI2C_MasterSetBaudRate))
  [Stack]

  - Max Depth = 60
  - Call Chain = LPI2C_MasterSetBaudRate
  [Called By]
  - >> LPI2C_MasterInit

  LPI2C_MasterStop (Thumb, 50 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_MasterStop))
  [Stack]

  - Max Depth = 32
  - Call Chain = LPI2C_MasterStop ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> LPI2C_MasterCheckAndClearError
  - >> LPI2C_MasterWaitForTxReady
  [Called By]
  - >> LPI2C_MasterTransferBlocking

  LPI2C_MasterTransferBlocking (Thumb, 326 bytes, Stack size 40 bytes, fsl_lpi2c.o(.text.LPI2C_MasterTransferBlocking))
  [Stack]

  - Max Depth = 72
  - Call Chain = LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> LPI2C_MasterSend
  - >> LPI2C_MasterReceive
  - >> LPI2C_MasterStop
  - >> LPI2C_MasterWaitForTxReady
  [Called By]
  - >> I2C_WriteReg

  LPI2C_SlaveTransferHandleIRQ (Thumb, 328 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_SlaveTransferHandleIRQ))
  [Stack]

  - Max Depth = 24
  - Call Chain = LPI2C_SlaveTransferHandleIRQ ⇒ memset
  [Calls]
  - >> OUTLINED_FUNCTION_0
  - >> LPI2C_SlaveCheckAndClearError
  - >> memset
  [Called By]
  - >> LPI2C_CommonIRQHandler

  LPUART1_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART1_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART1_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART2_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART2_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART2_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART3_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART3_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART3_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART4_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART4_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART4_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART5_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART5_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART5_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART6_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART6_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART6_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART7_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART7_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART7_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART8_DriverIRQHandler (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART8_DriverIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = LPUART8_DriverIRQHandler
  [Calls]
  - >> OUTLINED_FUNCTION_0
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  LPUART_ClearStatusFlags (Thumb, 56 bytes, Stack size 0 bytes, fsl_lpuart.o(.text.LPUART_ClearStatusFlags))
  [Called By]

  - >> OUTLINED_FUNCTION_1
  - >> LPUART_ReadBlocking

  LPUART_GetDefaultConfig (Thumb, 32 bytes, Stack size 16 bytes, fsl_lpuart.o(.text.LPUART_GetDefaultConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = LPUART_GetDefaultConfig ⇒ memset
  [Calls]
  - >> memset
  [Called By]
  - >> HAL_UartInit

  LPUART_GetInstance (Thumb, 24 bytes, Stack size 0 bytes, fsl_lpuart.o(.text.LPUART_GetInstance))
  [Called By]

  - >> LPUART_Init

  LPUART_Init (Thumb, 484 bytes, Stack size 40 bytes, fsl_lpuart.o(.text.LPUART_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = LPUART_Init ⇒ CLOCK_ControlGate
  [Calls]
  - >> LPUART_GetInstance
  - >> CLOCK_ControlGate
  [Called By]
  - >> HAL_UartInit

  LPUART_ReadBlocking (Thumb, 168 bytes, Stack size 32 bytes, fsl_lpuart.o(.text.LPUART_ReadBlocking))
  [Stack]

  - Max Depth = 40
  - Call Chain = LPUART_ReadBlocking ⇒ OUTLINED_FUNCTION_1
  [Calls]
  - >> LPUART_ClearStatusFlags
  - >> OUTLINED_FUNCTION_1
  [Called By]
  - >> HAL_UartReceiveBlocking

  LPUART_WriteBlocking (Thumb, 28 bytes, Stack size 0 bytes, fsl_lpuart.o(.text.LPUART_WriteBlocking))
  [Calls]

  - >> LPUART_WriteBlocking
  [Called By]
  - >> LPUART_WriteBlocking
  - >> HAL_UartSendBlocking

  SDK_DelayAtLeastUs (Thumb, 32 bytes, Stack size 8 bytes, fsl_common_arm.o(.text.SDK_DelayAtLeastUs))
  [Stack]

  - Max Depth = 48
  - Call Chain = SDK_DelayAtLeastUs ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> IS31FL3729_Init
  - >> main
  - >> OUTLINED_FUNCTION_0

  SystemCoreClockUpdate (Thumb, 236 bytes, Stack size 24 bytes, system_mimxrt1062.o(.text.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 64
  - Call Chain = SystemCoreClockUpdate ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> BOARD_InitHardware

  SystemInit (Thumb, 168 bytes, Stack size 0 bytes, system_mimxrt1062.o(.text.SystemInit))
  [Calls]

  - >> SystemInitHook
  [Address Reference Count : 1]
  - startup_mimxrt1062.o(.text)

  SystemInitHook (Thumb, 2 bytes, Stack size 0 bytes, system_mimxrt1062.o(.text.SystemInitHook))
  [Called By]

  - >> SystemInit

  main (Thumb, 88 bytes, Stack size 16 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 176
  - Call Chain = main ⇒ IS31FL3729_Init ⇒ I2C_WriteReg ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> IS31FL3729_SetLED
  - >> IS31FL3729_EnableOutput
  - >> IS31FL3729_Init
  - >> SDK_DelayAtLeastUs
  - >> CLOCK_GetFreq
  - >> BOARD_InitHardware
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  OUTLINED_FUNCTION_5 (Thumb, 26 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_5))
  [Called By]

  - >> BOARD_BootClockRUN

  OUTLINED_FUNCTION_7 (Thumb, 16 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_7))
  [Called By]

  - >> BOARD_BootClockRUN

  CLOCK_SetMux (Thumb, 24 bytes, Stack size 16 bytes, clock_config.o(.text.CLOCK_SetMux))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SetMux
  [Calls]
  - >> OUTLINED_FUNCTION_4
  [Called By]
  - >> BOARD_BootClockRUN
  [Address Reference Count : 1]
  - clock_config.o(.text.BOARD_BootClockRUN)

  OUTLINED_FUNCTION_0 (Thumb, 94 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_0))
  [Called By]

  - >> BOARD_BootClockRUN

  OUTLINED_FUNCTION_6 (Thumb, 12 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_6))
  [Calls]

  - >> CLOCK_DeinitEnetPll
  [Called By]
  - >> BOARD_BootClockRUN

  OUTLINED_FUNCTION_2 (Thumb, 70 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_2))
  [Calls]

  - >> CLOCK_DeinitUsb2Pll
  [Called By]
  - >> BOARD_BootClockRUN

  OUTLINED_FUNCTION_8 (Thumb, 14 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_8))
  [Called By]

  - >> BOARD_BootClockRUN

  OUTLINED_FUNCTION_3 (Thumb, 68 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_3))
  [Called By]

  - >> BOARD_BootClockRUN

  OUTLINED_FUNCTION_1 (Thumb, 80 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_1))
  [Called By]

  - >> BOARD_BootClockRUN

  CLOCK_SetDiv (Thumb, 24 bytes, Stack size 16 bytes, clock_config.o(.text.CLOCK_SetDiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SetDiv
  [Calls]
  - >> OUTLINED_FUNCTION_4
  [Address Reference Count : 1]
  - clock_config.o(.text.BOARD_BootClockRUN)

  CLOCK_DisableClock (Thumb, 36 bytes, Stack size 0 bytes, clock_config.o(.text.CLOCK_DisableClock))
  [Address Reference Count : 1]

  - clock_config.o(.text.BOARD_BootClockRUN)

  OUTLINED_FUNCTION_4 (Thumb, 36 bytes, Stack size 0 bytes, clock_config.o(.text.OUTLINED_FUNCTION_4))
  [Called By]

  - >> CLOCK_SetDiv
  - >> CLOCK_SetMux

  CLOCK_GetPeriphClkFreq (Thumb, 116 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetPeriphClkFreq))
  [Stack]

  - Max Depth = 56
  - Call Chain = CLOCK_GetPeriphClkFreq ⇒ CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> CLOCK_GetSysPfdFreq
  - >> OUTLINED_FUNCTION_5
  - >> CLOCK_GetPllFreq
  [Called By]
  - >> CLOCK_GetSemcFreq
  - >> CLOCK_GetAhbFreq

  OUTLINED_FUNCTION_5 (Thumb, 8 bytes, Stack size 0 bytes, fsl_clock.o(.text.OUTLINED_FUNCTION_5))
  [Called By]

  - >> CLOCK_GetPerClkFreq
  - >> CLOCK_GetSemcFreq
  - >> CLOCK_GetPeriphClkFreq

  OUTLINED_FUNCTION_12 (Thumb, 10 bytes, Stack size 0 bytes, fsl_clock.o(.text.OUTLINED_FUNCTION_12))
  [Stack]

  - Max Depth = 40
  - Call Chain = OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> CLOCK_GetUsb1PfdFreq
  - >> CLOCK_GetSysPfdFreq

  CLOCK_GetPllUsb1SWFreq (Thumb, 20 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_GetPllUsb1SWFreq))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_GetPllUsb1SWFreq ⇒ CLOCK_GetPllFreq
  [Calls]
  - >> CLOCK_GetPllFreq
  [Called By]
  - >> CLOCK_GetFreq

  OUTLINED_FUNCTION_9 (Thumb, 22 bytes, Stack size 0 bytes, fsl_clock.o(.text.OUTLINED_FUNCTION_9))
  [Called By]

  - >> CLOCK_GetPllFreq

  OUTLINED_FUNCTION_3 (Thumb, 10 bytes, Stack size 0 bytes, fsl_clock.o(.text.OUTLINED_FUNCTION_3))
  [Called By]

  - >> CLOCK_InitSysPll
  - >> CLOCK_InitArmPll

  OUTLINED_FUNCTION_4 (Thumb, 8 bytes, Stack size 0 bytes, fsl_clock.o(.text.OUTLINED_FUNCTION_4))
  [Called By]

  - >> CLOCK_DeinitEnetPll
  - >> CLOCK_DeinitAudioPll

  OUTLINED_FUNCTION_1 (Thumb, 34 bytes, Stack size 0 bytes, fsl_clock.o(.text.OUTLINED_FUNCTION_1))
  [Called By]

  - >> CLOCK_InitSysPfd

  CLOCK_ControlGate (Thumb, 44 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.CLOCK_ControlGate))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_ControlGate
  [Called By]
  - >> LPUART_Init

  OUTLINED_FUNCTION_1 (Thumb, 20 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.OUTLINED_FUNCTION_1))
  [Stack]

  - Max Depth = 8
  - Call Chain = OUTLINED_FUNCTION_1
  [Calls]
  - >> LPUART_ClearStatusFlags
  [Called By]
  - >> LPUART_ReadBlocking

  OUTLINED_FUNCTION_0 (Thumb, 6 bytes, Stack size 0 bytes, fsl_lpuart.o(.text.OUTLINED_FUNCTION_0))
  [Called By]

  - >> LPUART8_DriverIRQHandler
  - >> LPUART7_DriverIRQHandler
  - >> LPUART6_DriverIRQHandler
  - >> LPUART5_DriverIRQHandler
  - >> LPUART4_DriverIRQHandler
  - >> LPUART3_DriverIRQHandler
  - >> LPUART2_DriverIRQHandler
  - >> LPUART1_DriverIRQHandler

  CLOCK_EnableClock (Thumb, 6 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.CLOCK_EnableClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_EnableClock ⇒ CLOCK_ControlGate
  [Calls]
  - >> CLOCK_ControlGate
  [Called By]
  - >> LPI2C_MasterInit

  LPI2C_GetCyclesForWidth (Thumb, 68 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_GetCyclesForWidth))
  [Stack]

  - Max Depth = 16
  - Call Chain = LPI2C_GetCyclesForWidth
  [Called By]
  - >> LPI2C_MasterInit
  - >> OUTLINED_FUNCTION_2

  OUTLINED_FUNCTION_2 (Thumb, 14 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.OUTLINED_FUNCTION_2))
  [Stack]

  - Max Depth = 16
  - Call Chain = OUTLINED_FUNCTION_2 ⇒ LPI2C_GetCyclesForWidth
  [Calls]
  - >> LPI2C_GetCyclesForWidth
  [Called By]
  - >> LPI2C_MasterInit

  CLOCK_ControlGate (Thumb, 44 bytes, Stack size 8 bytes, fsl_lpi2c.o(.text.CLOCK_ControlGate))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_ControlGate
  [Called By]
  - >> CLOCK_EnableClock

  LPI2C_MasterWaitForTxReady (Thumb, 26 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_MasterWaitForTxReady))
  [Stack]

  - Max Depth = 16
  - Call Chain = LPI2C_MasterWaitForTxReady
  [Calls]
  - >> LPI2C_MasterCheckAndClearError
  [Called By]
  - >> LPI2C_MasterTransferBlocking
  - >> LPI2C_MasterSend
  - >> LPI2C_MasterReceive
  - >> LPI2C_MasterStop

  LPI2C_SlaveCheckAndClearError (Thumb, 34 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.LPI2C_SlaveCheckAndClearError))
  [Called By]

  - >> LPI2C_SlaveTransferHandleIRQ

  OUTLINED_FUNCTION_0 (Thumb, 8 bytes, Stack size 0 bytes, fsl_lpi2c.o(.text.OUTLINED_FUNCTION_0))
  [Called By]

  - >> LPI2C_SlaveTransferHandleIRQ

  LPI2C_CommonIRQHandler (Thumb, 64 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_CommonIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LPI2C_CommonIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset
  [Calls]
  - >> LPI2C_SlaveTransferHandleIRQ
  [Called By]
  - >> LPI2C4_DriverIRQHandler
  - >> LPI2C3_DriverIRQHandler
  - >> LPI2C2_DriverIRQHandler
  - >> LPI2C1_DriverIRQHandler

  I2C_WriteReg (Thumb, 72 bytes, Stack size 40 bytes, is31fl3729.o(.text.I2C_WriteReg))
  [Stack]

  - Max Depth = 112
  - Call Chain = I2C_WriteReg ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterSend ⇒ LPI2C_MasterWaitForTxReady
  [Calls]
  - >> LPI2C_MasterTransferBlocking
  [Called By]
  - >> IS31FL3729_SetLED
  - >> IS31FL3729_EnableOutput
  - >> IS31FL3729_Init

  OUTLINED_FUNCTION_1 (Thumb, 8 bytes, Stack size 0 bytes, is31fl3729.o(.text.OUTLINED_FUNCTION_1))
  [Stack]

  - Max Depth = 88
  - Call Chain = OUTLINED_FUNCTION_1 ⇒ CLOCK_GetFreq ⇒ CLOCK_GetPerClkFreq ⇒ CLOCK_GetIpgFreq ⇒ CLOCK_GetAhbFreq ⇒ CLOCK_GetPeriphClkFreq ⇒ CLOCK_GetSysPfdFreq ⇒ OUTLINED_FUNCTION_12 ⇒ __aeabi_uldivmod
  [Calls]
  - >> CLOCK_GetFreq
  [Called By]
  - >> IS31FL3729_Init

  OUTLINED_FUNCTION_0 (Thumb, 10 bytes, Stack size 0 bytes, is31fl3729.o(.text.OUTLINED_FUNCTION_0))
  [Stack]

  - Max Depth = 48
  - Call Chain = OUTLINED_FUNCTION_0 ⇒ SDK_DelayAtLeastUs ⇒ __aeabi_uldivmod
  [Calls]
  - >> SDK_DelayAtLeastUs
  [Called By]
  - >> IS31FL3729_Init

  ### Undefined Global Symbols