# Static Call Graph for image sdram_debug\LED_I2C_TEST.out

#<CALLGRAPH># ARM Linker, 6220000: Last Updated: Sun Mar 16 20:49:43 2025

### Maximum Stack Usage = 304 bytes + Unknown(Functions without stacksize, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ IS31FL3729_Init ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterReceive ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

### Functions with no stack information

- Reset_Handler
- ACMP1_IRQHandler
- ACMP2_IRQHandler
- ACMP3_IRQHandler
- ACMP4_IRQHandler
- ADC1_IRQHandler
- ADC2_IRQHandler
- ADC_ETC_ERROR_IRQ_IRQHandler
- ADC_ETC_IRQ0_IRQHandler
- ADC_ETC_IRQ1_IRQHandler
- ADC_ETC_IRQ2_IRQHandler
- BEE_IRQHandler
- BusFault_Handler
- CAN1_DriverIRQHandler
- CAN2_DriverIRQHandler
- CAN3_DriverIRQHandler
- CCM_1_IRQHandler
- CCM_2_IRQHandler
- CORE_IRQHandler
- CSI_IRQHandler
- CSU_IRQHandler
- CTI0_ERROR_IRQHandler
- CTI1_ERROR_IRQHandler
- DCDC_IRQHandler
- DCP_IRQHandler
- DCP_VMI_IRQHandler
- DMA0_DMA16_DriverIRQHandler
- DMA10_DMA26_DriverIRQHandler
- DMA11_DMA27_DriverIRQHandler
- DMA12_DMA28_DriverIRQHandler
- DMA13_DMA29_DriverIRQHandler
- DMA14_DMA30_DriverIRQHandler
- DMA15_DMA31_DriverIRQHandler
- DMA1_DMA17_DriverIRQHandler
- DMA2_DMA18_DriverIRQHandler
- DMA3_DMA19_DriverIRQHandler
- DMA4_DMA20_DriverIRQHandler
- DMA5_DMA21_DriverIRQHandler
- DMA6_DMA22_DriverIRQHandler
- DMA7_DMA23_DriverIRQHandler
- DMA8_DMA24_DriverIRQHandler
- DMA9_DMA25_DriverIRQHandler
- DMA_ERROR_DriverIRQHandler
- DebugMon_Handler
- DefaultISR
- ENC1_IRQHandler
- ENC2_IRQHandler
- ENC3_IRQHandler
- ENC4_IRQHandler
- ENET2_1588_Timer_DriverIRQHandler
- ENET2_DriverIRQHandler
- ENET_1588_Timer_DriverIRQHandler
- ENET_DriverIRQHandler
- EWM_IRQHandler
- FLEXIO1_DriverIRQHandler
- FLEXIO2_DriverIRQHandler
- FLEXIO3_DriverIRQHandler
- FLEXRAM_IRQHandler
- FLEXSPI2_DriverIRQHandler
- FLEXSPI_DriverIRQHandler
- GPC_IRQHandler
- GPIO10_Combined_0_31_IRQHandler
- GPIO1_Combined_0_15_IRQHandler
- GPIO1_Combined_16_31_IRQHandler
- GPIO1_INT0_IRQHandler
- GPIO1_INT1_IRQHandler
- GPIO1_INT2_IRQHandler
- GPIO1_INT3_IRQHandler
- GPIO1_INT4_IRQHandler
- GPIO1_INT5_IRQHandler
- GPIO1_INT6_IRQHandler
- GPIO1_INT7_IRQHandler
- GPIO2_Combined_0_15_IRQHandler
- GPIO2_Combined_16_31_IRQHandler
- GPIO3_Combined_0_15_IRQHandler
- GPIO3_Combined_16_31_IRQHandler
- GPIO4_Combined_0_15_IRQHandler
- GPIO4_Combined_16_31_IRQHandler
- GPIO5_Combined_0_15_IRQHandler
- GPIO5_Combined_16_31_IRQHandler
- GPIO6_7_8_9_IRQHandler
- GPR_IRQ_IRQHandler
- GPT1_IRQHandler
- GPT2_IRQHandler
- KPP_IRQHandler
- LCDIF_IRQHandler
- LPSPI1_DriverIRQHandler
- LPSPI2_DriverIRQHandler
- LPSPI3_DriverIRQHandler
- LPSPI4_DriverIRQHandler
- MemManage_Handler
- PIT_IRQHandler
- PMU_EVENT_IRQHandler
- PWM1_0_IRQHandler
- PWM1_1_IRQHandler
- PWM1_2_IRQHandler
- PWM1_3_IRQHandler
- PWM1_FAULT_IRQHandler
- PWM2_0_IRQHandler
- PWM2_1_IRQHandler
- PWM2_2_IRQHandler
- PWM2_3_IRQHandler
- PWM2_FAULT_IRQHandler
- PWM3_0_IRQHandler
- PWM3_1_IRQHandler
- PWM3_2_IRQHandler
- PWM3_3_IRQHandler
- PWM3_FAULT_IRQHandler
- PWM4_0_IRQHandler
- PWM4_1_IRQHandler
- PWM4_2_IRQHandler
- PWM4_3_IRQHandler
- PWM4_FAULT_IRQHandler
- PXP_IRQHandler
- RTWDOG_IRQHandler
- Reserved115_IRQHandler
- Reserved143_IRQHandler
- Reserved144_IRQHandler
- Reserved171_IRQHandler
- Reserved68_IRQHandler
- Reserved78_IRQHandler
- Reserved86_IRQHandler
- SAI1_DriverIRQHandler
- SAI2_DriverIRQHandler
- SAI3_RX_DriverIRQHandler
- SAI3_TX_DriverIRQHandler
- SEMC_IRQHandler
- SJC_IRQHandler
- SNVS_HP_WRAPPER_IRQHandler
- SNVS_HP_WRAPPER_TZ_IRQHandler
- SNVS_LP_WRAPPER_IRQHandler
- SPDIF_DriverIRQHandler
- SRC_IRQHandler
- TEMP_LOW_HIGH_IRQHandler
- TEMP_PANIC_IRQHandler
- TMR1_IRQHandler
- TMR2_IRQHandler
- TMR3_IRQHandler
- TMR4_IRQHandler
- TRNG_IRQHandler
- TSC_DIG_IRQHandler
- USB_OTG1_IRQHandler
- USB_OTG2_IRQHandler
- USB_PHY1_IRQHandler
- USB_PHY2_IRQHandler
- USDHC1_DriverIRQHandler
- USDHC2_DriverIRQHandler
- UsageFault_Handler
- WDOG1_IRQHandler
- WDOG2_IRQHandler
- XBAR1_IRQ_0_1_IRQHandler
- XBAR1_IRQ_2_3_IRQHandler
- NMI_Handler
- HardFault_Handler
- SVC_Handler
- PendSV_Handler
- SysTick_Handler
- DMA0_DMA16_IRQHandler
- DMA1_DMA17_IRQHandler
- DMA2_DMA18_IRQHandler
- DMA3_DMA19_IRQHandler
- DMA4_DMA20_IRQHandler
- DMA5_DMA21_IRQHandler
- DMA6_DMA22_IRQHandler
- DMA7_DMA23_IRQHandler
- DMA8_DMA24_IRQHandler
- DMA9_DMA25_IRQHandler
- DMA10_DMA26_IRQHandler
- DMA11_DMA27_IRQHandler
- DMA12_DMA28_IRQHandler
- DMA13_DMA29_IRQHandler
- DMA14_DMA30_IRQHandler
- DMA15_DMA31_IRQHandler
- DMA_ERROR_IRQHandler
- LPUART1_IRQHandler
- LPUART2_IRQHandler
- LPUART3_IRQHandler
- LPUART4_IRQHandler
- LPUART5_IRQHandler
- LPUART6_IRQHandler
- LPUART7_IRQHandler
- LPUART8_IRQHandler
- LPI2C1_IRQHandler
- LPI2C2_IRQHandler
- LPI2C3_IRQHandler
- LPI2C4_IRQHandler
- LPSPI1_IRQHandler
- LPSPI2_IRQHandler
- LPSPI3_IRQHandler
- LPSPI4_IRQHandler
- CAN1_IRQHandler
- CAN2_IRQHandler
- SAI1_IRQHandler
- SAI2_IRQHandler
- SAI3_RX_IRQHandler
- SAI3_TX_IRQHandler
- SPDIF_IRQHandler
- FLEXIO1_IRQHandler
- FLEXIO2_IRQHandler
- FLEXSPI2_IRQHandler
- FLEXSPI_IRQHandler
- USDHC1_IRQHandler
- USDHC2_IRQHandler
- ENET_IRQHandler
- ENET_1588_Timer_IRQHandler
- ENET2_IRQHandler
- ENET2_1588_Timer_IRQHandler
- CAN3_IRQHandler
- FLEXIO3_IRQHandler
- memcpy

### Function Pointers

- ACMP1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ACMP2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ACMP3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ACMP4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ADC1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ADC2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ADC_ETC_ERROR_IRQ_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ADC_ETC_IRQ0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ADC_ETC_IRQ1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ADC_ETC_IRQ2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- BEE_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- BusFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CAN1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- CAN1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CAN2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- CAN2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CAN3_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- CAN3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CCM_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CCM_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CORE_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CSI_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CSU_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CTI0_ERROR_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- CTI1_ERROR_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DCDC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DCP_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DCP_VMI_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA0_DMA16_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA0_DMA16_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA10_DMA26_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA10_DMA26_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA11_DMA27_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA11_DMA27_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA12_DMA28_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA12_DMA28_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA13_DMA29_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA13_DMA29_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA14_DMA30_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA14_DMA30_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA15_DMA31_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA15_DMA31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA1_DMA17_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA1_DMA17_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA2_DMA18_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA2_DMA18_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA3_DMA19_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA3_DMA19_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA4_DMA20_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA4_DMA20_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA5_DMA21_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA5_DMA21_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA6_DMA22_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA6_DMA22_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA7_DMA23_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA7_DMA23_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA8_DMA24_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA8_DMA24_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA9_DMA25_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA9_DMA25_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DMA_ERROR_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- DMA_ERROR_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DebugMon_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- DefaultISR from startup_mimxrt1062.o(.text) referenced 9 times from fsl_lpuart.o(.data.s_lpuartIsr)
- DefaultISR from startup_mimxrt1062.o(.text) referenced 81 times from startup_mimxrt1062.o(.isr_vector)
- ENC1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ENC2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ENC3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ENC4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ENET2_1588_Timer_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- ENET2_1588_Timer_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ENET2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- ENET2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ENET_1588_Timer_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- ENET_1588_Timer_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- ENET_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- ENET_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- EWM_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- FLEXIO1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- FLEXIO1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- FLEXIO2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- FLEXIO2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- FLEXIO3_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- FLEXIO3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- FLEXRAM_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- FLEXSPI2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- FLEXSPI2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- FLEXSPI_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- FLEXSPI_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO10_Combined_0_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT5_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT6_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO1_INT7_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO2_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO2_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO3_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO3_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO4_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO4_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO5_Combined_0_15_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO5_Combined_16_31_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPIO6_7_8_9_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPR_IRQ_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPT1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- GPT2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- HAL_UartReceiveBlocking from fsl_adapter_lpuart.o(.text.HAL_UartReceiveBlocking) referenced 2 times from fsl_debug_console.o(.text.DbgConsole_Init)
- HAL_UartSendBlocking from fsl_adapter_lpuart.o(.text.HAL_UartSendBlocking) referenced 2 times from fsl_debug_console.o(.text.DbgConsole_Init)
- HardFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- HardFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- KPP_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LCDIF_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPI2C1_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C1_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPI2C1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPI2C2_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C2_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPI2C2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPI2C3_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C3_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPI2C3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPI2C4_DriverIRQHandler from fsl_lpi2c.o(.text.LPI2C4_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPI2C4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPSPI1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- LPSPI1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPSPI2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- LPSPI2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPSPI3_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- LPSPI3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPSPI4_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- LPSPI4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART1_DriverIRQHandler from fsl_lpuart.o(.text.LPUART1_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART2_DriverIRQHandler from fsl_lpuart.o(.text.LPUART2_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART3_DriverIRQHandler from fsl_lpuart.o(.text.LPUART3_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART4_DriverIRQHandler from fsl_lpuart.o(.text.LPUART4_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART5_DriverIRQHandler from fsl_lpuart.o(.text.LPUART5_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART5_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART6_DriverIRQHandler from fsl_lpuart.o(.text.LPUART6_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART6_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART7_DriverIRQHandler from fsl_lpuart.o(.text.LPUART7_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART7_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- LPUART8_DriverIRQHandler from fsl_lpuart.o(.text.LPUART8_DriverIRQHandler) referenced from startup_mimxrt1062.o(.text)
- LPUART8_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- MemManage_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- NMI_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- NMI_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- PIT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PMU_EVENT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM1_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM1_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM1_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM1_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM1_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM2_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM2_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM2_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM2_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM2_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM3_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM3_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM3_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM3_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM3_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM4_0_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM4_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM4_2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM4_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PWM4_FAULT_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PXP_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PendSV_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- PendSV_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- RTWDOG_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reserved115_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reserved143_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reserved144_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reserved171_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reserved68_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reserved78_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reserved86_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- Reset_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SAI1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- SAI1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SAI2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- SAI2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SAI3_RX_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- SAI3_RX_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SAI3_TX_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- SAI3_TX_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SEMC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SJC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SNVS_HP_WRAPPER_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SNVS_HP_WRAPPER_TZ_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SNVS_LP_WRAPPER_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SPDIF_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- SPDIF_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SRC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SVC_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SVC_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- SysTick_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- SysTick_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- SystemInit from system_mimxrt1062.o(.text.SystemInit) referenced from startup_mimxrt1062.o(.text)
- TEMP_LOW_HIGH_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- TEMP_PANIC_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- TMR1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- TMR2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- TMR3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- TMR4_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- TRNG_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- TSC_DIG_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- USB_OTG1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- USB_OTG2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- USB_PHY1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- USB_PHY2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- USDHC1_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- USDHC1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- USDHC2_DriverIRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.text)
- USDHC2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- UsageFault_Handler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- WDOG1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- WDOG2_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- XBAR1_IRQ_0_1_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- XBAR1_IRQ_2_3_IRQHandler from startup_mimxrt1062.o(.text) referenced from startup_mimxrt1062.o(.isr_vector)
- __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_mimxrt1062.o(.text)
- main from main.o(.text.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

### Global Symbols

__main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

_main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry4.o(.ARM.Collect$$$$00000003))

_main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Calls]

- >> __scatterload

__main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Called By]

- >> __scatterload

_main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

_main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

_main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

__rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

__rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

Reset_Handler (Thumb, 40 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ACMP1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ACMP2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ACMP3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ACMP4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ADC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ADC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ADC_ETC_ERROR_IRQ_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ADC_ETC_IRQ0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ADC_ETC_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ADC_ETC_IRQ2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

BEE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

BusFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CAN1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

CAN2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

CAN3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

CCM_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CCM_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CORE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CSI_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CSU_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CTI0_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CTI1_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DCDC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DCP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DCP_VMI_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA0_DMA16_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA10_DMA26_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA11_DMA27_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA12_DMA28_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA13_DMA29_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA14_DMA30_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA15_DMA31_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA1_DMA17_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA2_DMA18_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA3_DMA19_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA4_DMA20_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA5_DMA21_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA6_DMA22_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA7_DMA23_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA8_DMA24_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA9_DMA25_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DMA_ERROR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

DebugMon_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DefaultISR (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Called By]

- >> ACMP1_IRQHandler

[Address Reference Count : 2]

- startup_mimxrt1062.o(.isr_vector)
- fsl_lpuart.o(.data.s_lpuartIsr)

ENC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENC3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENC4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENET2_1588_Timer_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

ENET2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

ENET_1588_Timer_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

ENET_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

EWM_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

FLEXIO1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

FLEXIO2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

FLEXIO3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

FLEXRAM_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

FLEXSPI2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

FLEXSPI_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

GPC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO10_Combined_0_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO1_INT7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO2_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO2_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO3_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO3_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO4_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO4_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO5_Combined_0_15_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO5_Combined_16_31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPIO6_7_8_9_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPR_IRQ_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

GPT2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

KPP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LCDIF_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPSPI1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPSPI2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPSPI3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPSPI4_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

MemManage_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PIT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PMU_EVENT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM1_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM1_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM1_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM1_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM1_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM2_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM2_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM2_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM2_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM2_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM3_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM3_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM3_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM3_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM3_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM4_0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM4_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM4_2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM4_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PWM4_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

PXP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

RTWDOG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

Reserved115_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

Reserved143_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

Reserved144_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

Reserved171_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

Reserved68_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

Reserved78_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

Reserved86_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SAI1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

SAI2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

SAI3_RX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

SAI3_TX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

SEMC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SJC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SNVS_HP_WRAPPER_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SNVS_HP_WRAPPER_TZ_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SNVS_LP_WRAPPER_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SPDIF_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

SRC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TEMP_LOW_HIGH_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TEMP_PANIC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TMR1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TMR2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TMR3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TMR4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TRNG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

TSC_DIG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

USB_OTG1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

USB_OTG2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

USB_PHY1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

USB_PHY2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

USDHC1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

USDHC2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

UsageFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

WDOG1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

WDOG2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

XBAR1_IRQ_0_1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

XBAR1_IRQ_2_3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

NMI_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 2]

- startup_mimxrt1062.o(.text)
- startup_mimxrt1062.o(.isr_vector)

HardFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 2]

- startup_mimxrt1062.o(.text)
- startup_mimxrt1062.o(.isr_vector)

SVC_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 2]

- startup_mimxrt1062.o(.text)
- startup_mimxrt1062.o(.isr_vector)

PendSV_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 2]

- startup_mimxrt1062.o(.text)
- startup_mimxrt1062.o(.isr_vector)

SysTick_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 2]

- startup_mimxrt1062.o(.text)
- startup_mimxrt1062.o(.isr_vector)

DMA0_DMA16_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA1_DMA17_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA2_DMA18_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA3_DMA19_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA4_DMA20_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA5_DMA21_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA6_DMA22_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA7_DMA23_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA8_DMA24_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA9_DMA25_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA10_DMA26_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA11_DMA27_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA12_DMA28_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA13_DMA29_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA14_DMA30_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA15_DMA31_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

DMA_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPUART8_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPI2C1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPI2C2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPI2C3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPI2C4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPSPI1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPSPI2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPSPI3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

LPSPI4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CAN1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CAN2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SAI1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SAI2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SAI3_RX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SAI3_TX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

SPDIF_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

FLEXIO1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

FLEXIO2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

FLEXSPI2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

FLEXSPI_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

USDHC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

USDHC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENET_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENET_1588_Timer_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENET2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

ENET2_1588_Timer_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

CAN3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

FLEXIO3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_mimxrt1062.o(.text))
[Address Reference Count : 1]

- startup_mimxrt1062.o(.isr_vector)

memcpy (Thumb, 0 bytes, Stack size unknown bytes, fsl_memcpy.o(.text))
[Called By]

- >> DbgConsole_Vprintf

__aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
[Stack]

- Max Depth = 40
- Call Chain = __aeabi_uldivmod

[Calls]

- >> __aeabi_llsr
- >> __aeabi_llsl

[Called By]

- >> SDK_DelayAtLeastUs
- >> CLOCK_GetFreq
- >> CLOCK_GetSemcFreq
- >> CLOCK_GetPeriphClkFreq
- >> SystemCoreClockUpdate

memset (Thumb, 18 bytes, Stack size 8 bytes, memset.o(.text))
[Stack]

- Max Depth = 8
- Call Chain = memset

[Called By]

- >> LPI2C_SlaveTransferHandleIRQ
- >> LPI2C_MasterGetDefaultConfig
- >> LPUART_GetDefaultConfig

strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
[Called By]

- >> DbgConsole_Vprintf

__aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
[Called By]

- >> __aeabi_uldivmod

_ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

__aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
[Called By]

- >> __aeabi_uldivmod

_ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

__scatterload (Thumb, 38 bytes, Stack size 0 bytes, init.o(.text))
[Calls]

- >> __main_after_scatterload

[Called By]

- >> _main_scatterload

__scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

BOARD_BootClockRUN (Thumb, 2150 bytes, Stack size 32 bytes, clock_config.o(.text.BOARD_BootClockRUN))
[Stack]

- Max Depth = 160 + Unknown Stack Size
- Call Chain = BOARD_BootClockRUN ⇒ CLOCK_InitExternalClk ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> CLOCK_DeinitUsb2Pll
- >> CLOCK_DeinitEnetPll
- >> CLOCK_DeinitAudioPll
- >> CLOCK_InitUsb1Pfd
- >> CLOCK_InitUsb1Pll
- >> CLOCK_InitArmPll
- >> CLOCK_SwitchOsc
- >> CLOCK_InitRcOsc24M
- >> CLOCK_InitExternalClk

[Called By]

- >> BOARD_InitBootClocks

BOARD_ConfigMPU (Thumb, 700 bytes, Stack size 32 bytes, board.o(.text.BOARD_ConfigMPU))
[Stack]

- Max Depth = 160 + Unknown Stack Size
- Call Chain = BOARD_ConfigMPU ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_assert

[Called By]

- >> BOARD_InitHardware

BOARD_InitBootClocks (Thumb, 4 bytes, Stack size 0 bytes, clock_config.o(.text.BOARD_InitBootClocks))
[Stack]

- Max Depth = 160 + Unknown Stack Size
- Call Chain = BOARD_InitBootClocks ⇒ BOARD_BootClockRUN ⇒ CLOCK_InitExternalClk ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> BOARD_BootClockRUN

[Called By]

- >> BOARD_InitHardware

BOARD_InitBootPins (Thumb, 66 bytes, Stack size 0 bytes, pin_mux.o(.text.BOARD_InitBootPins))
[Called By]

- >> BOARD_InitHardware

BOARD_InitDebugConsole (Thumb, 104 bytes, Stack size 8 bytes, board.o(.text.BOARD_InitDebugConsole))
[Stack]

- Max Depth = 256 + Unknown Stack Size
- Call Chain = BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ LPUART_Init ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> DbgConsole_Init
- >> CLOCK_GetPllFreq

[Called By]

- >> BOARD_InitHardware

BOARD_InitHardware (Thumb, 76 bytes, Stack size 8 bytes, hardware_init.o(.text.BOARD_InitHardware))
[Stack]

- Max Depth = 264 + Unknown Stack Size
- Call Chain = BOARD_InitHardware ⇒ BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ LPUART_Init ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> SystemCoreClockUpdate
- >> BOARD_InitBootPins
- >> BOARD_InitBootClocks
- >> BOARD_ConfigMPU
- >> BOARD_InitDebugConsole

[Called By]

- >> main

CLOCK_DeinitAudioPll (Thumb, 16 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_DeinitAudioPll))
[Called By]

- >> BOARD_BootClockRUN

CLOCK_DeinitEnetPll (Thumb, 16 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_DeinitEnetPll))
[Called By]

- >> BOARD_BootClockRUN

CLOCK_DeinitUsb2Pll (Thumb, 14 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_DeinitUsb2Pll))
[Called By]

- >> BOARD_BootClockRUN

CLOCK_GetFreq (Thumb, 2214 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetFreq))
[Stack]

- Max Depth = 136 + Unknown Stack Size
- Call Chain = CLOCK_GetFreq ⇒ CLOCK_GetPllFreq ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_uldivmod
- >> CLOCK_GetSemcFreq
- >> CLOCK_GetPeriphClkFreq
- >> CLOCK_GetPllFreq

[Called By]

- >> IS31FL3729_Init
- >> main

CLOCK_GetPllFreq (Thumb, 610 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_GetPllFreq))
[Stack]

- Max Depth = 128 + Unknown Stack Size
- Call Chain = CLOCK_GetPllFreq ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_assert

[Called By]

- >> CLOCK_GetFreq
- >> BOARD_InitDebugConsole

CLOCK_GetSemcFreq (Thumb, 264 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetSemcFreq))
[Stack]

- Max Depth = 56
- Call Chain = CLOCK_GetSemcFreq ⇒ CLOCK_GetPeriphClkFreq ⇒ __aeabi_uldivmod

[Calls]

- >> __aeabi_uldivmod
- >> CLOCK_GetPeriphClkFreq

[Called By]

- >> CLOCK_GetFreq

CLOCK_InitArmPll (Thumb, 70 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitArmPll))
[Called By]

- >> BOARD_BootClockRUN

CLOCK_InitExternalClk (Thumb, 64 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitExternalClk))
[Stack]

- Max Depth = 128 + Unknown Stack Size
- Call Chain = CLOCK_InitExternalClk ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_assert

[Called By]

- >> BOARD_BootClockRUN

CLOCK_InitRcOsc24M (Thumb, 18 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitRcOsc24M))
[Called By]

- >> BOARD_BootClockRUN

CLOCK_InitUsb1Pfd (Thumb, 54 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_InitUsb1Pfd))
[Stack]

- Max Depth = 8
- Call Chain = CLOCK_InitUsb1Pfd

[Called By]

- >> BOARD_BootClockRUN

CLOCK_InitUsb1Pll (Thumb, 66 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_InitUsb1Pll))
[Called By]

- >> BOARD_BootClockRUN

CLOCK_SwitchOsc (Thumb, 24 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_SwitchOsc))
[Called By]

- >> BOARD_BootClockRUN

DbgConsole_Init (Thumb, 82 bytes, Stack size 40 bytes, fsl_debug_console.o(.text.DbgConsole_Init))
[Stack]

- Max Depth = 248 + Unknown Stack Size
- Call Chain = DbgConsole_Init ⇒ HAL_UartInit ⇒ LPUART_Init ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> HAL_UartInit

[Called By]

- >> BOARD_InitDebugConsole

DbgConsole_Printf (Thumb, 32 bytes, Stack size 24 bytes, fsl_debug_console.o(.text.DbgConsole_Printf))
[Stack]

- Max Depth = 128 + Unknown Stack Size
- Call Chain = DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> DbgConsole_Vprintf

[Called By]

- >> __aeabi_assert

DbgConsole_Vprintf (Thumb, 1064 bytes, Stack size 104 bytes, fsl_debug_console.o(.text.DbgConsole_Vprintf))
[Stack]

- Max Depth = 104 + Unknown Stack Size
- Call Chain = DbgConsole_Vprintf

[Calls]

- >> strlen
- >> memcpy

[Called By]

- >> DbgConsole_Printf

HAL_UartInit (Thumb, 264 bytes, Stack size 40 bytes, fsl_adapter_lpuart.o(.text.HAL_UartInit))
[Stack]

- Max Depth = 208 + Unknown Stack Size
- Call Chain = HAL_UartInit ⇒ LPUART_Init ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPUART_Init
- >> LPUART_GetDefaultConfig
- >> __aeabi_assert

[Called By]

- >> DbgConsole_Init

HAL_UartReceiveBlocking (Thumb, 108 bytes, Stack size 8 bytes, fsl_adapter_lpuart.o(.text.HAL_UartReceiveBlocking))
[Stack]

- Max Depth = 144 + Unknown Stack Size
- Call Chain = HAL_UartReceiveBlocking ⇒ LPUART_ReadBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPUART_ReadBlocking
- >> __aeabi_assert

[Address Reference Count : 1]

- fsl_debug_console.o(.text.DbgConsole_Init)

HAL_UartSendBlocking (Thumb, 102 bytes, Stack size 8 bytes, fsl_adapter_lpuart.o(.text.HAL_UartSendBlocking))
[Stack]

- Max Depth = 136 + Unknown Stack Size
- Call Chain = HAL_UartSendBlocking ⇒ LPUART_WriteBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPUART_WriteBlocking
- >> __aeabi_assert

[Address Reference Count : 1]

- fsl_debug_console.o(.text.DbgConsole_Init)

IS31FL3729_EnableOutput (Thumb, 66 bytes, Stack size 40 bytes, is31fl3729.o(.text.IS31FL3729_EnableOutput))
[Stack]

- Max Depth = 232 + Unknown Stack Size
- Call Chain = IS31FL3729_EnableOutput ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterReceive ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPI2C_MasterTransferBlocking

[Called By]

- >> main

IS31FL3729_Init (Thumb, 498 bytes, Stack size 96 bytes, is31fl3729.o(.text.IS31FL3729_Init))
[Stack]

- Max Depth = 288 + Unknown Stack Size
- Call Chain = IS31FL3729_Init ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterReceive ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPI2C_MasterTransferBlocking
- >> LPI2C_MasterInit
- >> LPI2C_MasterGetDefaultConfig
- >> SDK_DelayAtLeastUs
- >> CLOCK_GetFreq

[Called By]

- >> main

IS31FL3729_SetLED (Thumb, 116 bytes, Stack size 40 bytes, is31fl3729.o(.text.IS31FL3729_SetLED))
[Stack]

- Max Depth = 232 + Unknown Stack Size
- Call Chain = IS31FL3729_SetLED ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterReceive ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPI2C_MasterTransferBlocking

[Called By]

- >> main

LPI2C1_DriverIRQHandler (Thumb, 82 bytes, Stack size 8 bytes, fsl_lpi2c.o(.text.LPI2C1_DriverIRQHandler))
[Stack]

- Max Depth = 48
- Call Chain = LPI2C1_DriverIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset

[Calls]

- >> LPI2C_SlaveTransferHandleIRQ

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPI2C2_DriverIRQHandler (Thumb, 84 bytes, Stack size 8 bytes, fsl_lpi2c.o(.text.LPI2C2_DriverIRQHandler))
[Stack]

- Max Depth = 48
- Call Chain = LPI2C2_DriverIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset

[Calls]

- >> LPI2C_SlaveTransferHandleIRQ

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPI2C3_DriverIRQHandler (Thumb, 84 bytes, Stack size 8 bytes, fsl_lpi2c.o(.text.LPI2C3_DriverIRQHandler))
[Stack]

- Max Depth = 48
- Call Chain = LPI2C3_DriverIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset

[Calls]

- >> LPI2C_SlaveTransferHandleIRQ

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPI2C4_DriverIRQHandler (Thumb, 84 bytes, Stack size 8 bytes, fsl_lpi2c.o(.text.LPI2C4_DriverIRQHandler))
[Stack]

- Max Depth = 48
- Call Chain = LPI2C4_DriverIRQHandler ⇒ LPI2C_SlaveTransferHandleIRQ ⇒ memset

[Calls]

- >> LPI2C_SlaveTransferHandleIRQ

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPI2C_MasterGetDefaultConfig (Thumb, 48 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_MasterGetDefaultConfig))
[Stack]

- Max Depth = 24
- Call Chain = LPI2C_MasterGetDefaultConfig ⇒ memset

[Calls]

- >> memset

[Called By]

- >> IS31FL3729_Init

LPI2C_MasterInit (Thumb, 622 bytes, Stack size 40 bytes, fsl_lpi2c.o(.text.LPI2C_MasterInit))
[Stack]

- Max Depth = 168 + Unknown Stack Size
- Call Chain = LPI2C_MasterInit ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPI2C_MasterSetBaudRate
- >> __aeabi_assert

[Called By]

- >> IS31FL3729_Init

LPI2C_MasterReceive (Thumb, 328 bytes, Stack size 16 bytes, fsl_lpi2c.o(.text.LPI2C_MasterReceive))
[Stack]

- Max Depth = 144 + Unknown Stack Size
- Call Chain = LPI2C_MasterReceive ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_assert

[Called By]

- >> LPI2C_MasterTransferBlocking

LPI2C_MasterSetBaudRate (Thumb, 376 bytes, Stack size 52 bytes, fsl_lpi2c.o(.text.LPI2C_MasterSetBaudRate))
[Stack]

- Max Depth = 52
- Call Chain = LPI2C_MasterSetBaudRate

[Called By]

- >> LPI2C_MasterInit

LPI2C_MasterStop (Thumb, 218 bytes, Stack size 8 bytes, fsl_lpi2c.o(.text.LPI2C_MasterStop))
[Stack]

- Max Depth = 8
- Call Chain = LPI2C_MasterStop

[Called By]

- >> LPI2C_MasterTransferBlocking

LPI2C_MasterTransferBlocking (Thumb, 618 bytes, Stack size 48 bytes, fsl_lpi2c.o(.text.LPI2C_MasterTransferBlocking))
[Stack]

- Max Depth = 192 + Unknown Stack Size
- Call Chain = LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterReceive ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> LPI2C_MasterReceive
- >> LPI2C_MasterStop
- >> __aeabi_assert

[Called By]

- >> IS31FL3729_SetLED
- >> IS31FL3729_EnableOutput
- >> IS31FL3729_Init

LPI2C_SlaveTransferHandleIRQ (Thumb, 402 bytes, Stack size 32 bytes, fsl_lpi2c.o(.text.LPI2C_SlaveTransferHandleIRQ))
[Stack]

- Max Depth = 40
- Call Chain = LPI2C_SlaveTransferHandleIRQ ⇒ memset

[Calls]

- >> memset

[Called By]

- >> LPI2C4_DriverIRQHandler
- >> LPI2C3_DriverIRQHandler
- >> LPI2C2_DriverIRQHandler
- >> LPI2C1_DriverIRQHandler

LPUART1_DriverIRQHandler (Thumb, 38 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART1_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART1_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART2_DriverIRQHandler (Thumb, 38 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART2_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART2_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART3_DriverIRQHandler (Thumb, 38 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART3_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART3_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART4_DriverIRQHandler (Thumb, 36 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART4_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART4_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART5_DriverIRQHandler (Thumb, 38 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART5_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART5_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART6_DriverIRQHandler (Thumb, 38 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART6_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART6_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART7_DriverIRQHandler (Thumb, 38 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART7_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART7_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART8_DriverIRQHandler (Thumb, 36 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART8_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = LPUART8_DriverIRQHandler

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

LPUART_GetDefaultConfig (Thumb, 58 bytes, Stack size 16 bytes, fsl_lpuart.o(.text.LPUART_GetDefaultConfig))
[Stack]

- Max Depth = 144 + Unknown Stack Size
- Call Chain = LPUART_GetDefaultConfig ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> memset
- >> __aeabi_assert

[Called By]

- >> HAL_UartInit

LPUART_Init (Thumb, 664 bytes, Stack size 40 bytes, fsl_lpuart.o(.text.LPUART_Init))
[Stack]

- Max Depth = 168 + Unknown Stack Size
- Call Chain = LPUART_Init ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_assert

[Called By]

- >> HAL_UartInit

LPUART_ReadBlocking (Thumb, 276 bytes, Stack size 8 bytes, fsl_lpuart.o(.text.LPUART_ReadBlocking))
[Stack]

- Max Depth = 136 + Unknown Stack Size
- Call Chain = LPUART_ReadBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_assert

[Called By]

- >> HAL_UartReceiveBlocking

LPUART_WriteBlocking (Thumb, 54 bytes, Stack size 0 bytes, fsl_lpuart.o(.text.LPUART_WriteBlocking))
[Stack]

- Max Depth = 128 + Unknown Stack Size
- Call Chain = LPUART_WriteBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_assert

[Called By]

- >> HAL_UartSendBlocking

SDK_DelayAtLeastUs (Thumb, 68 bytes, Stack size 8 bytes, fsl_common_arm.o(.text.SDK_DelayAtLeastUs))
[Stack]

- Max Depth = 136 + Unknown Stack Size
- Call Chain = SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> __aeabi_uldivmod
- >> __aeabi_assert

[Called By]

- >> IS31FL3729_Init
- >> main

SystemCoreClockUpdate (Thumb, 302 bytes, Stack size 24 bytes, system_mimxrt1062.o(.text.SystemCoreClockUpdate))
[Stack]

- Max Depth = 64
- Call Chain = SystemCoreClockUpdate ⇒ __aeabi_uldivmod

[Calls]

- >> __aeabi_uldivmod

[Called By]

- >> BOARD_InitHardware

SystemInit (Thumb, 210 bytes, Stack size 0 bytes, system_mimxrt1062.o(.text.SystemInit))
[Calls]

- >> SystemInitHook

[Address Reference Count : 1]

- startup_mimxrt1062.o(.text)

SystemInitHook (Thumb, 2 bytes, Stack size 0 bytes, system_mimxrt1062.o(.text.SystemInitHook))
[Called By]

- >> SystemInit

__aeabi_assert (Thumb, 32 bytes, Stack size 0 bytes, fsl_assert.o(.text.__aeabi_assert))
[Stack]

- Max Depth = 128 + Unknown Stack Size
- Call Chain = __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> fsl_assert_hook
- >> DbgConsole_Printf

[Called By]

- >> LPI2C_MasterTransferBlocking
- >> LPI2C_MasterReceive
- >> LPI2C_MasterInit
- >> SDK_DelayAtLeastUs
- >> LPUART_WriteBlocking
- >> HAL_UartSendBlocking
- >> LPUART_ReadBlocking
- >> HAL_UartReceiveBlocking
- >> LPUART_Init
- >> LPUART_GetDefaultConfig
- >> HAL_UartInit
- >> CLOCK_InitExternalClk
- >> BOARD_ConfigMPU
- >> CLOCK_GetPllFreq

fsl_assert_hook (Thumb, 4 bytes, Stack size 0 bytes, fsl_assert.o(.text.fsl_assert_hook))
[Called By]

- >> __aeabi_assert

main (Thumb, 112 bytes, Stack size 16 bytes, main.o(.text.main))
[Stack]

- Max Depth = 304 + Unknown Stack Size
- Call Chain = main ⇒ IS31FL3729_Init ⇒ LPI2C_MasterTransferBlocking ⇒ LPI2C_MasterReceive ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf

[Calls]

- >> IS31FL3729_SetLED
- >> IS31FL3729_EnableOutput
- >> IS31FL3729_Init
- >> SDK_DelayAtLeastUs
- >> CLOCK_GetFreq
- >> BOARD_InitHardware

[Address Reference Count : 1]

- entry9a.o(.ARM.Collect$$$$0000000B)

__scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

__scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

__scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

### Local Symbols

CLOCK_GetPeriphClkFreq (Thumb, 806 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetPeriphClkFreq))
[Stack]

- Max Depth = 48
- Call Chain = CLOCK_GetPeriphClkFreq ⇒ __aeabi_uldivmod

[Calls]

- >> __aeabi_uldivmod

[Called By]

- >> CLOCK_GetFreq
- >> CLOCK_GetSemcFreq

### Undefined Global Symbols