/*!
    @page ftm_pwm_s32k144_group FTM PWM 
    @brief Example application showing the FTM's PWM functionality
    
    ## Application description ##
    ______
    The purpose of this demo application is to show you the usage of the PWM mode of the FlexTimer module found on the S32K144 using S32 SDK API.
    The examples does the following operations:
    -   increment or decrement duty cycle
    -   Update channel duty cycle
    -   Wait for a number of cycles to make
        the change visible
    
    Run the example
        1. After reset, The RED LED of EVB board will increment or decrement light intensity
        2. Use oscilloscope to verify the output signal
    ## Prerequisites ##
    ______
    To run the example you will need to have the following items:
    - 1 S32K144 board
    - 1 Power Adapter 12V (if the board cannot be powered from the USB port)
    - 1 Personal Computer
    - 1 Dupont female to female cable
    - 1 Jlink Lite Debugger (optional, users can use Open SDA)
    
    ## Boards supported ##
    ______
    The following boards are supported by this application:
    - S32K144EVB-Q100
    - S32K144-MB
    
    ## Hardware Wiring ##
    ______
    
    The following connections must be done to for this example application to work:
    
    PIN FUNCTION                    | S32K144EVB-Q100              | S32K144-MB
    --------------------------------|------------------------------|----------------
    FTM0 Channel 0 (\b PTD15)       | RGB_RED - wired on the board | J11.31 - J12.18
    
    ## How to run ##
    ______
    
    #### 1. Importing the project into the workspace ####
    After opening S32 Design Studio, go to \b File -> \b New \b S32DS \b Project \b From... and select \b ftm_pwm_s32k144. Then click on \b Finish. \n
    The project should now be copied into you current workspace.
    #### 2. Generating the Processor Expert configuration ####
    First go to \b Project \b Explorer View in S32 DS and select the current project(\b ftm_pwm_s32k144). Then go to \b Project and click on \b Generate \b Processor \b Expert \b Code \n
    Wait for the code generation to be completed before continuing to the next step.
    #### 3. Building the project ####
    Select the configuration to be built \b FLASH (Debug_FLASH) or \b RAM (Debug_RAM) by left clicking on the downward arrow corresponding to the \b build button(@image hammer.png). 
    Wait for the build action to be completed before continuing to the next step.
    #### 4. Running the project ####
    Go to \b Run and select \b Debug \b Configurations. There will be four debug configurations for this project:
     Configuration Name | Description
     -------------------|------------
     \b ftm_pwm_s32k144_debug_ram_jlink | Debug the RAM configuration using Segger Jlink debuggers
     \b ftm_pwm_s32k144_debug_flash_jlink | Debug the FLASH configuration using Segger Jlink debuggers
     \b ftm_pwm_s32k144_debug_ram_pemicro | Debug the RAM configuration using PEMicro debuggers 
     \b ftm_pwm_s32k144_debug_flash_pemicro | Debug the FLASH configuration using PEMicro debuggers 
    \n Select the desired debug configuration and click on \b Launch. Now the perspective will change to the \b Debug \b Perspective. \n
    Use the controls to control the program flow.
    
    @note For more detailed information related to S32 Design Studio usage please consult the available documentation.
    

*/
