Uses FTM PWM functionality using a single channel to light a LED on the board. The light's intensity is increased and decreased periodically
The example documentation can be found in the S32 SDK documentation at Examples and Demos section. (<SDK_PATH>/doc/Start_Here.html)