Project: S32K344_SecureBootCfg_Example_100_341_FW0110
Example Description:
    This example project to configure secure boot on S32K3xx.
Hardware:
    SCH-47478 REV A/SCH-47478 REV C
Environment:
    S32DS 3.4.1
Software:
    SW32K3_RTD_4.4_1.0.0
    HSE_FW_S32K3X4_0_1_1_0(Full_Mem)
Test steps:
S32K344_SecureBootCfg_Example_100_341_FW0110 is referred to as "Cfg" 
S32K344_SecureBootApp_Example_100_341_FW0110 is referred to as "App" 
    1. build App project first(DEBUG_FLASH), the linkfile(.ld) of the cfg project will reference the binary file(.bin) compiled by the app project.
    2. build Cfg project(DEBUG_FLASH), connect uart console@9600bps
    3. Debug the application on the board(S32K3 white board SCH-47478)
    4. run Cfg program, out put info via uart and wait it completed, change IVT BOOT SEQ to run App
    5. run App program

    
