## Project Name: Landworld_OBC_APP

### Date Created: 2023-11-12, 17:55:24

## PIN Assignments for S32K144_100 100 LQFP100 package

|  | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
|  | PTD13 | PTD14 | PTE9 | PTD15 | PTD16 | PTD17 | PTE12 | PTE3 | PTE14 | XTAL | EXTAL | VSS | VREFL | VREFH | VDDA | VDD | CAN0_RX | CAN0_TX | PTE13 | PTE10 | PTE11 | PTD0 | PTD1 | PTE15 | PTE16 |  |
26 | CMP0_IN3 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PTA8 | 100
27 | PTB5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PTA9 | 99
28 | LPSPI0_SOUT |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | JTAG_TMS/SWD_DIO | 98
29 | PTC3 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | RESET_b | 97
30 | PTC2 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | JTAG_TCLK/SWD_CLK | 96
31 | CMP0_IN6 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | JTAG_TDI | 95
32 | CMP0_IN7 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | LPSPI0_SCK | 94
33 | PTD5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | LPSPI0_SIN | 93
34 | PTD12 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | JTAG_TDO | 92
35 | PTD11 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PTA11 | 91
36 | PTD10 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | CAN1_RX | 90
37 | VSS |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | CAN1_TX | 89
38 | VDD |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PTA14 | 88
39 | PTC1 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | VDD | 87
40 | PTC0 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | VSS | 86
41 | PTD9 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC1_SE10 | 85
42 | PTD8 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC1_SE11 | 84
43 | ADC0_SE15 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC1_SE12 | 83
44 | ADC0_SE14 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC1_SE13 | 82
45 | ADC0_SE13 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC1_SE4 | 81
46 | ADC0_SE12 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC1_SE5 | 80
47 | ADC0_SE7 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC0_SE0/CMP0_IN0 | 79
48 | ADC0_SE6 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | ADC0_SE1/CMP0_IN1 | 78
49 | PTC13 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PTB8 | 77
50 | PTC12 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PTB9 | 76
|  | PTC11 | PTC10 | ADC0_SE5/ADC1_SE15 | LPSPI0_PCS0 | PTC9 | PTC8 | ADC0_SE3 | ADC0_SE2 | PTE7 | VSS | VDD | PTA17 | LPSPI1_PCS3 | LPSPI1_SOUT | LPSPI1_SIN | LPSPI1_SCK | CAN2_TX | CAN2_RX | ADC1_SE6 | ADC1_SE3 | ADC1_SE2 | ADC1_SE1 | ADC1_SE0 | PTB11 | PTB10 |  |
|  | 51 | 52 | 53 | 54 | 55 | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63 | 64 | 65 | 66 | 67 | 68 | 69 | 70 | 71 | 72 | 73 | 74 | 75 |  |

## Pin Allocation Report

Peripheral | Custom peripheral name | Peripheral description
--- | --- | ---
ADC0 | ADC0 | Analog-to-Digital Converter
ADC1 | ADC1 | Analog-to-Digital Converter
CAN0 | CAN0 | Flex Controller Area Network module
CAN1 | CAN1 | Flex Controller Area Network module
CAN2 | CAN2 | Flex Controller Area Network module
CMP0 | CMP0 | Analog comparator
EWM | EWM | External Watchdog Monitor
FLEXIO | FLEXIO | Flexible IO
FTM0 | FTM0 | FlexTimer Module
FTM1 | FTM1 | FlexTimer Module
FTM2 | FTM2 | FlexTimer Module
FTM3 | FTM3 | FlexTimer Module
JTAG | JTAG | Joint Test Action Group (JTAG)
LPI2C0 | LPI2C0 | The LPI2C Memory Map/Register Definition can be found here.
LPSPI0 | LPSPI0 | The LPSPI Memory Map/Register Definition can be found here.
LPSPI1 | LPSPI1 | The LPSPI Memory Map/Register Definition can be found here.
LPSPI2 | LPSPI2 | The LPSPI Memory Map/Register Definition can be found here.
LPTMR0 | LPTMR0 | Low Power Timer
LPUART0 | LPUART0 | Universal Asynchronous Receiver/Transmitter
LPUART1 | LPUART1 | Universal Asynchronous Receiver/Transmitter
LPUART2 | LPUART2 | Universal Asynchronous Receiver/Transmitter
PTA | PTA | General Purpose Input/Output
PTB | PTB | General Purpose Input/Output
PTC | PTC | General Purpose Input/Output
PTD | PTD | General Purpose Input/Output
PTE | PTE | General Purpose Input/Output
Platform | Platform | Platform (Platform)
PowerAndGround | PowerAndGround | Power And Ground (PowerAndGround)
RTC | RTC | Secure Real Time Clock
SWD | SWD | Serial Wire Debug (SWD)
TRGMUX | TRGMUX | TRGMUX

## Routed Pins

| Assigned Pin Function(s)
Package Pin # | Pin Name | User Assigned Signal Name | Assigned Peripheral | Assigned Function | Package Function | Dir
--- | --- | --- | --- | --- | --- | ---
1 | PTE16 | same |  |  |  |
2 | PTE15 | same | PTE | port15 | alt1 | Output
3 | PTD1 | same |  |  |  |
4 | PTD0 | same | PTD | port0 | alt1 | Output
5 | PTE11 | same |  |  |  |
6 | PTE10 | same |  |  |  |
7 | PTE13 | same |  |  |  |
8 | PTE5 | same | CAN0 | can_txtxd | alt5 | Output
9 | PTE4 | same | CAN0 | can_rxrxd | alt5 | Input
10 | VDD10 | same | PowerAndGround | VDD10 | alt0 | Input
11 | VDDA | same | PowerAndGround | VDDA11 | alt0 | Input
12 | VREFH | same | Platform | VREFH12 | alt0 | Input
13 | VREFL | same | Platform | VREFL13 | alt0 | Input
14 | VSS14 | same | PowerAndGround | VSS14 | alt0 | Output
15 | PTB7 | same | Platform | extal15 | alt0 | Input
16 | PTB6 | same | Platform | xtal16 | alt0 | Output
17 | PTE14 | same |  |  |  |
18 | PTE3 | same |  |  |  |
19 | PTE12 | same |  |  |  |
20 | PTD17 | same |  |  |  |
21 | PTD16 | same | PTD | port16 | alt1 | Output
22 | PTD15 | same | PTD | port15 | alt1 | Output
23 | PTE9 | same |  |  |  |
24 | PTD14 | same |  |  |  |
25 | PTD13 | same |  |  |  |
26 | PTE8 | same | CMP0 | acmp_in3 | alt0 | Input
27 | PTB5 | same | PTB | port5 | alt1 | Output
28 | PTB4 | same | LPSPI0 | lpspi_sout | alt3 | Output
29 | PTC3 | same | PTC | port3 | alt1 | Output
30 | PTC2 | same | PTC | port2 | alt1 | Output
31 | PTD7 | same | CMP0 | acmp_in6 | alt0 | Input
32 | PTD6 | same | CMP0 | acmp_in7 | alt0 | Input
33 | PTD5 | same |  |  |  |
34 | PTD12 | same |  |  |  |
35 | PTD11 | same |  |  |  |
36 | PTD10 | same |  |  |  |
37 | VSS37 | same | PowerAndGround | VSS37 | alt0 | Output
38 | VDD38 | same | PowerAndGround | VDD38 | alt0 | Input
39 | PTC1 | same | PTC | port1 | alt1 | Output
40 | PTC0 | same | PTC | port0 | alt1 | Output
41 | PTD9 | same |  |  |  |
42 | PTD8 | same |  |  |  |
43 | PTC17 | same | ADC0 | adc_se15 | alt0 | Input
44 | PTC16 | same | ADC0 | adc_se14 | alt0 | Input
45 | PTC15 | same | ADC0 | adc_se13 | alt0 | Input
46 | PTC14 | same | ADC0 | adc_se12 | alt0 | Input
47 | PTB3 | same | ADC0 | adc_se7 | alt0 | Input
48 | PTB2 | same | ADC0 | adc_se6 | alt0 | Input
49 | PTC13 | same | PTC | port13 | alt1 | Input
50 | PTC12 | same | PTC | port12 | alt1 | Input
51 | PTC11 | same |  |  |  |
52 | PTC10 | same |  |  |  |
53 | PTB1 | same | ADC0 | adc_se5 | alt0 | Input
54 | PTB0 | same | LPSPI0 | lpspi_pcs0 | alt3 | Output
55 | PTC9 | same |  |  |  |
56 | PTC8 | same |  |  |  |
57 | PTA7 | same | ADC0 | adc_se3 | alt0 | Input
58 | PTA6 | same | ADC0 | adc_se2 | alt0 | Input
59 | PTE7 | same |  |  |  |
60 | VSS60 | same | PowerAndGround | VSS60 | alt0 | Output
61 | VDD61 | same | PowerAndGround | VDD61 | alt0 | Input
62 | PTA17 | same |  |  |  |
63 | PTB17 | same | LPSPI1 | lpspi_pcs3 | alt3 | Output
64 | PTB16 | same | LPSPI1 | lpspi_sout | alt3 | Output
65 | PTB15 | same | LPSPI1 | lpspi_sin | alt3 | Input
66 | PTB14 | same | LPSPI1 | lpspi_scksck | alt3 | Output
67 | PTB13 | same | CAN2 | can_txtxd | alt4 | Output
68 | PTB12 | same | CAN2 | can_rxrxd | alt4 | Input
69 | PTD4 | same | ADC1 | adc_se6 | alt0 | Input
70 | PTD3 | same | ADC1 | adc_se3 | alt0 | Input
71 | PTD2 | same | ADC1 | adc_se2 | alt0 | Input
72 | PTA3 | same | ADC1 | adc_se1 | alt0 | Input
73 | PTA2 | same | ADC1 | adc_se0 | alt0 | Input
74 | PTB11 | same |  |  |  |
75 | PTB10 | same |  |  |  |
76 | PTB9 | same |  |  |  |
77 | PTB8 | same |  |  |  |
78 | PTA1 | same | ADC0 | adc_se1 | alt0 | Input
CMP0 | acmp_in1 | alt0 | Input
79 | PTA0 | same | ADC0 | adc_se0 | alt0 | Input
CMP0 | acmp_in0 | alt0 | Input
80 | PTC7 | same | ADC1 | adc_se5 | alt0 | Input
81 | PTC6 | same | ADC1 | adc_se4 | alt0 | Input
82 | PTA16 | same | ADC1 | adc_se13 | alt0 | Input
83 | PTA15 | same | ADC1 | adc_se12 | alt0 | Input
84 | PTE6 | same | ADC1 | adc_se11 | alt0 | Input
85 | PTE2 | same | ADC1 | adc_se10 | alt0 | Input
86 | VSS86 | same | PowerAndGround | VSS86 | alt0 | Output
87 | VDD87 | same | PowerAndGround | VDD87 | alt0 | Input
88 | PTA14 | same |  |  |  |
89 | PTA13 | same | CAN1 | can_txtxd | alt3 | Output
90 | PTA12 | same | CAN1 | can_rxrxd | alt3 | Input
91 | PTA11 | same |  |  |  |
92 | PTA10 | same | JTAG | jtag_tdo | alt7 | Output
93 | PTE1 | same | LPSPI0 | lpspi_sin | alt2 | Input
94 | PTE0 | same | LPSPI0 | lpspi_scksck | alt2 | Output
95 | PTC5 | same | JTAG | jtag_tdi | alt7 | Input
96 | PTC4 | same | JTAG | jtag_tclk | alt7 | Input
SWD | swd_clk | alt7 | Input
97 | PTA5 | same | Platform | RESET_b97 | alt7 | Output
98 | PTA4 | same | JTAG | jtag_tms | alt7 | Input/Output
SWD | swd_dio | alt7 | Input/Output
99 | PTA9 | same |  |  |  |
100 | PTA8 | same |  |  |  |

## Routable Pins

| alt0 | alt1 | alt2 | alt3 | alt4 | alt5 | alt6 | alt7
Package Pin # | Pin Name | User Assigned Signal Name | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir | Peripheral | Function | Dir
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | PTE16 | same |  |  |  | PTE | port16 | Input, Output | LPUART1 | lpuart_rts | Output | LPSPI2 | lpspi_sin | Input, Output, Input/Output | FTM2 | ftm_ch7 | Input, Output |  |  |  | FLEXIO | fxio_d3 | Input/Output | TRGMUX | TRGMUX_OUT7 | Output
2 | PTE15 | same |  |  |  | PTE | port15 | Input, Output | LPUART1 | lpuart_cts | Input | LPSPI2 | lpspi_scksck | Input, Output, Input/Output | FTM2 | ftm_ch6 | Input, Output |  |  |  | FLEXIO | fxio_d2 | Input/Output | TRGMUX | TRGMUX_OUT6 | Output
3 | PTD1 | same |  |  |  | PTD | port1 | Input, Output | FTM0 | ftm_ch3 | Input, Output | LPSPI1 | lpspi_sin | Input, Output, Input/Output | FTM2 | ftm_ch1 | Input, Output |  |  |  | FLEXIO | fxio_d1 | Input/Output | TRGMUX | TRGMUX_OUT2 | Output
4 | PTD0 | same |  |  |  | PTD | port0 | Input, Output | FTM0 | ftm_ch2 | Input, Output | LPSPI1 | lpspi_scksck | Input, Output, Input/Output | FTM2 | ftm_ch0 | Input, Output |  |  |  | FLEXIO | fxio_d0 | Input/Output | TRGMUX | TRGMUX_OUT1 | Output
5 | PTE11 | same |  |  |  | PTE | port11 | Input, Output | LPSPI2 | lpspi_pcs0 | Input, Output, Input/Output | LPTMR0 | lptmr_alt1 | Input | FTM2 | ftm_ch5 | Input, Output |  |  |  | FLEXIO | fxio_d5 | Input/Output | TRGMUX | TRGMUX_OUT5 | Output
6 | PTE10 | same |  |  |  | PTE | port10 | Input, Output | Platform | CLKOUT6 | Output | LPSPI2 | lpspi_pcs1 | Input, Output, Input/Output | FTM2 | ftm_ch4 | Input, Output |  |  |  | FLEXIO | fxio_d4 | Input/Output | TRGMUX | TRGMUX_OUT4 | Output
7 | PTE13 | same |  |  |  | PTE | port13 | Input, Output |  |  |  | LPSPI2 | lpspi_pcs2 | Input, Output, Input/Output | FTM2 | ftm_flt0 | Input |  |  |  |  |  |  |  |  |
8 | PTE5 | same |  |  |  | PTE | port5 | Input, Output | FTM2 | TCLK2 | Input | FTM2 | ftm_QD_PHA | Input | FTM2 | ftm_ch3 | Input, Output | CAN0 | can_txtxd | Output | FLEXIO | fxio_d7 | Input/Output | EWM | ewm_in | Input
9 | PTE4 | same |  |  |  | PTE | port4 | Input, Output |  |  |  | FTM2 | ftm_QD_PHB | Input | FTM2 | ftm_ch2 | Input, Output | CAN0 | can_rxrxd | Input | FLEXIO | fxio_d6 | Input/Output | EWM | ewm_out_b | Output
10 | VDD10 | same | PowerAndGround | VDD10 | Input |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
11 | VDDA | same | PowerAndGround | VDDA11 | Input |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
12 | VREFH | same | Platform | VREFH12 | Input |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
13 | VREFL | same | Platform | VREFL13 | Input |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
14 | VSS14 | same | PowerAndGround | VSS14 | Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
15 | PTB7 | same | Platform | extal15 | Input | PTB | port7 | Input, Output | LPI2C0 | lpi2c_sclscl | Input/Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
16 | PTB6 | same | Platform | xtal16 | Output | PTB | port6 | Input, Output | LPI2C0 | lpi2c_sdasda | Input/Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
17 | PTE14 | same |  |  |  | PTE | port14 | Input, Output | FTM0 | ftm_flt1 | Input |  |  |  | FTM2 | ftm_flt1 | Input |  |  |  |  |  |  |  |  |
18 | PTE3 | same |  |  |  | PTE | port3 | Input, Output | FTM0 | ftm_flt0 | Input | LPUART2 | lpuart_rts | Output | FTM2 | ftm_flt0 | Input |  |  |  | TRGMUX | TRGMUX_IN6 | Input | CMP0 | acmp_out | Output
19 | PTE12 | same |  |  |  | PTE | port12 | Input, Output | FTM0 | ftm_flt3 | Input | LPUART2 | lpuart_tx | Input, Output, Input/Output |  |  |  |  |  |  |  |  |  |  |  |
20 | PTD17 | same |  |  |  | PTD | port17 | Input, Output | FTM0 | ftm_flt2 | Input | LPUART2 | lpuart_rx | Input |  |  |  |  |  |  |  |  |  |  |  |
21 | PTD16 | same |  |  |  | PTD | port16 | Input, Output | FTM0 | ftm_ch1 | Input, Output |  |  |  | LPSPI0 | lpspi_sin | Input, Output, Input/Output | CMP0 | acmp_rrt | Output |  |  |  |  |  |
22 | PTD15 | same |  |  |  | PTD | port15 | Input, Output | FTM0 | ftm_ch0 | Input, Output |  |  |  | LPSPI0 | lpspi_scksck | Input, Output, Input/Output |  |  |  |  |  |  |  |  |
23 | PTE9 | same |  |  |  | PTE | port9 | Input, Output | FTM0 | ftm_ch7 | Input, Output | LPUART2 | lpuart_cts | Input |  |  |  |  |  |  |  |  |  |  |  |
24 | PTD14 | same |  |  |  | PTD | port14 | Input, Output | FTM2 | ftm_ch5 | Input, Output | LPUART1 | lpuart_tx | Input, Output, Input/Output |  |  |  |  |  |  |  |  |  | Platform | CLKOUT24 | Output
25 | PTD13 | same |  |  |  | PTD | port13 | Input, Output | FTM2 | ftm_ch4 | Input, Output | LPUART1 | lpuart_rx | Input |  |  |  |  |  |  |  |  |  | RTC | RTC_CLKOUT | Output
26 | PTE8 | same | CMP0 | acmp_in3 | Input | PTE | port8 | Input, Output | FTM0 | ftm_ch6 | Input, Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
27 | PTB5 | same |  |  |  | PTB | port5 | Input, Output | FTM0 | ftm_ch5 | Input, Output | LPSPI0 | lpspi_pcs1 | Input, Output, Input/Output | LPSPI0 | lpspi_pcs0 | Input, Output, Input/Output | Platform | CLKOUT27 | Output | TRGMUX | TRGMUX_IN0 | Input |  |  |
28 | PTB4 | same |  |  |  | PTB | port4 | Input, Output | FTM0 | ftm_ch4 | Input, Output | LPSPI0 | lpspi_sout | Input, Output, Input/Output |  |  |  |  |  |  | TRGMUX | TRGMUX_IN1 | Input |  |  |
29 | PTC3 | same | ADC0 CMP0 | adc_se11 acmp_in4 | Input | PTC | port3 | Input, Output | FTM0 | ftm_ch3 | Input, Output | CAN0 | can_txtxd | Output | LPUART0 | lpuart_tx | Input, Output, Input/Output |  |  |  |  |  |  |  |  |
30 | PTC2 | same | ADC0 CMP0 | adc_se10 acmp_in5 | Input | PTC | port2 | Input, Output | FTM0 | ftm_ch2 | Input, Output | CAN0 | can_rxrxd | Input | LPUART0 | lpuart_rx | Input |  |  |  |  |  |  |  |  |
31 | PTD7 | same | CMP0 | acmp_in6 | Input | PTD | port7 | Input, Output | LPUART2 | lpuart_tx | Input, Output, Input/Output |  |  |  | FTM2 | ftm_flt3 | Input |  |  |  |  |  |  |  |  |
32 | PTD6 | same | CMP0 | acmp_in7 | Input | PTD | port6 | Input, Output | LPUART2 | lpuart_rx | Input |  |  |  | FTM2 | ftm_flt2 | Input |  |  |  |  |  |  |  |  |
33 | PTD5 | same |  |  |  | PTD | port5 | Input, Output | FTM2 | ftm_ch3 | Input, Output | LPTMR0 | lptmr_alt2 | Input | FTM2 | ftm_flt1 | Input |  |  |  | TRGMUX | TRGMUX_IN7 | Input |  |  |
34 | PTD12 | same |  |  |  | PTD | port12 | Input, Output | FTM2 | ftm_ch2 | Input, Output |  |  |  |  |  |  |  |  |  | LPUART2 | lpuart_rts | Output |  |  |
35 | PTD11 | same |  |  |  | PTD | port11 | Input, Output | FTM2 | ftm_ch1 | Input, Output | FTM2 | ftm_QD_PHA | Input |  |  |  |  |  |  | LPUART2 | lpuart_cts | Input |  |  |
36 | PTD10 | same |  |  |  | PTD | port10 | Input, Output | FTM2 | ftm_ch0 | Input, Output | FTM2 | ftm_QD_PHB | Input |  |  |  |  |  |  |  |  |  |  |  |
37 | VSS37 | same | PowerAndGround | VSS37 | Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
38 | VDD38 | same | PowerAndGround | VDD38 | Input |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
39 | PTC1 | same | ADC0 | adc_se9 | Input | PTC | port1 | Input, Output | FTM0 | ftm_ch1 | Input, Output | LPSPI2 | lpspi_sout | Input, Output, Input/Output |  |  |  |  |  |  | FTM1 | ftm_ch7 | Input, Output |  |  |
40 | PTC0 | same | ADC0 | adc_se8 | Input | PTC | port0 | Input, Output | FTM0 | ftm_ch0 | Input, Output | LPSPI2 | lpspi_sin | Input, Output, Input/Output |  |  |  |  |  |  | FTM1 | ftm_ch6 | Input, Output |  |  |
41 | PTD9 | same |  |  |  | PTD | port9 | Input, Output |  |  |  | FLEXIO | fxio_d0 | Input/Output | FTM2 | ftm_flt3 | Input |  |  |  | FTM1 | ftm_ch5 | Input, Output |  |  |
42 | PTD8 | same |  |  |  | PTD | port8 | Input, Output |  |  |  |  |  |  | FTM2 | ftm_flt2 | Input | FLEXIO | fxio_d1 | Input/Output | FTM1 | ftm_ch4 | Input, Output |  |  |
43 | PTC17 | same | ADC0 | adc_se15 | Input | PTC | port17 | Input, Output | FTM1 | ftm_flt3 | Input | CAN2 | can_txtxd | Output |  |  |  |  |  |  |  |  |  |  |  |
44 | PTC16 | same | ADC0 | adc_se14 | Input | PTC | port16 | Input, Output | FTM1 | ftm_flt2 | Input | CAN2 | can_rxrxd | Input |  |  |  |  |  |  |  |  |  |  |  |
45 | PTC15 | same | ADC0 | adc_se13 | Input | PTC | port15 | Input, Output | FTM1 | ftm_ch3 | Input, Output | LPSPI2 | lpspi_scksck | Input, Output, Input/Output |  |  |  |  |  |  | TRGMUX | TRGMUX_IN8 | Input |  |  |
46 | PTC14 | same | ADC0 | adc_se12 | Input | PTC | port14 | Input, Output | FTM1 | ftm_ch2 | Input, Output | LPSPI2 | lpspi_pcs0 | Input, Output, Input/Output |  |  |  |  |  |  | TRGMUX | TRGMUX_IN9 | Input |  |  |
47 | PTB3 | same | ADC0 | adc_se7 | Input | PTB | port3 | Input, Output | FTM1 | ftm_ch1 | Input, Output | LPSPI0 | lpspi_sin | Input, Output, Input/Output | FTM1 | ftm_QD_PHA | Input |  |  |  | TRGMUX | TRGMUX_IN2 | Input |  |  |
48 | PTB2 | same | ADC0 | adc_se6 | Input | PTB | port2 | Input, Output | FTM1 | ftm_ch0 | Input, Output | LPSPI0 | lpspi_scksck | Input, Output, Input/Output | FTM1 | ftm_QD_PHB | Input |  |  |  | TRGMUX | TRGMUX_IN3 | Input |  |  |
49 | PTC13 | same |  |  |  | PTC | port13 | Input, Output | FTM3 | ftm_ch7 | Input, Output | FTM2 | ftm_ch7 | Input, Output | LPUART2 | lpuart_rts | Output |  |  |  |  |  |  |  |  |
50 | PTC12 | same |  |  |  | PTC | port12 | Input, Output | FTM3 | ftm_ch6 | Input, Output | FTM2 | ftm_ch6 | Input, Output | LPUART2 | lpuart_cts | Input |  |  |  |  |  |  |  |  |
51 | PTC11 | same |  |  |  | PTC | port11 | Input, Output | FTM3 | ftm_ch5 | Input, Output |  |  |  |  |  |  |  |  |  | TRGMUX | TRGMUX_IN10 | Input |  |  |
52 | PTC10 | same |  |  |  | PTC | port10 | Input, Output | FTM3 | ftm_ch4 | Input, Output |  |  |  |  |  |  |  |  |  | TRGMUX | TRGMUX_IN11 | Input |  |  |
53 | PTB1 | same | ADC0 ADC1 | adc_se5 adc_se15 | Input | PTB | port1 | Input, Output | LPUART0 | lpuart_tx | Input, Output, Input/Output | LPSPI0 | lpspi_sout | Input, Output, Input/Output | FTM0 | TCLK0 | Input | CAN0 | can_txtxd | Output |  |  |  |  |  |
54 | PTB0 | same | ADC0 ADC1 | adc_se4 adc_se14 | Input | PTB | port0 | Input, Output | LPUART0 | lpuart_rx | Input | LPSPI0 | lpspi_pcs0 | Input, Output, Input/Output | LPTMR0 | lptmr_alt3 | Input | CAN0 | can_rxrxd | Input |  |  |  |  |  |
55 | PTC9 | same |  |  |  | PTC | port9 | Input, Output | LPUART1 | lpuart_tx | Input, Output, Input/Output | FTM1 | ftm_flt1 | Input |  |  |  |  |  |  | LPUART0 | lpuart_rts | Output |  |  |
56 | PTC8 | same |  |  |  | PTC | port8 | Input, Output | LPUART1 | lpuart_rx | Input | FTM1 | ftm_flt0 | Input |  |  |  |  |  |  | LPUART0 | lpuart_cts | Input |  |  |
57 | PTA7 | same | ADC0 | adc_se3 | Input | PTA | port7 | Input, Output | FTM0 | ftm_flt2 | Input |  |  |  | RTC | RTC_CLKIN | Input |  |  |  | LPUART1 | lpuart_rts | Output |  |  |
58 | PTA6 | same | ADC0 | adc_se2 | Input | PTA | port6 | Input, Output | FTM0 | ftm_flt1 | Input | LPSPI1 | lpspi_pcs1 | Input, Output, Input/Output |  |  |  |  |  |  | LPUART1 | lpuart_cts | Input |  |  |
59 | PTE7 | same |  |  |  | PTE | port7 | Input, Output | FTM0 | ftm_ch7 | Input, Output | FTM3 | ftm_flt0 | Input |  |  |  |  |  |  |  |  |  |  |  |
60 | VSS60 | same | PowerAndGround | VSS60 | Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
61 | VDD61 | same | PowerAndGround | VDD61 | Input |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
62 | PTA17 | same |  |  |  | PTA | port17 | Input, Output | FTM0 | ftm_ch6 | Input, Output | FTM3 | ftm_flt0 | Input | EWM | ewm_out_b | Output |  |  |  |  |  |  |  |  |
63 | PTB17 | same |  |  |  | PTB | port17 | Input, Output | FTM0 | ftm_ch5 | Input, Output | LPSPI1 | lpspi_pcs3 | Input, Output, Input/Output |  |  |  |  |  |  |  |  |  |  |  |
64 | PTB16 | same | ADC1 | adc_se15 | Input | PTB | port16 | Input, Output | FTM0 | ftm_ch4 | Input, Output | LPSPI1 | lpspi_sout | Input, Output, Input/Output |  |  |  |  |  |  |  |  |  |  |  |
65 | PTB15 | same | ADC1 | adc_se14 | Input | PTB | port15 | Input, Output | FTM0 | ftm_ch3 | Input, Output | LPSPI1 | lpspi_sin | Input, Output, Input/Output |  |  |  |  |  |  |  |  |  |  |  |
66 | PTB14 | same | ADC1 ADC0 | adc_se9 | Input | PTB | port14 | Input, Output | FTM0 | ftm_ch2 | Input, Output | LPSPI1 | lpspi_scksck | Input, Output, Input/Output |  |  |  |  |  |  |  |  |  |  |  |
67 | PTB13 | same | ADC1 ADC0 | adc_se8 | Input | PTB | port13 | Input, Output | FTM0 | ftm_ch1 | Input, Output | FTM3 | ftm_flt1 | Input | CAN2 | can_txtxd | Output |  |  |  |  |  |  |  |  |
68 | PTB12 | same | ADC1 | adc_se7 | Input | PTB | port12 | Input, Output | FTM0 | ftm_ch0 | Input, Output | FTM3 | ftm_flt2 | Input | CAN2 | can_rxrxd | Input |  |  |  |  |  |  |  |  |
69 | PTD4 | same | ADC1 | adc_se6 | Input | PTD | port4 | Input, Output | FTM0 | ftm_flt3 | Input | FTM3 | ftm_flt3 | Input |  |  |  |  |  |  |  |  |  |  |  |
70 | PTD3 | same | ADC1 | adc_se3 | Input | PTD | port3 | Input, Output | FTM3 | ftm_ch5 | Input, Output | LPSPI1 | lpspi_pcs0 | Input, Output, Input/Output | FLEXIO | fxio_d5 | Input/Output | FLEXIO | fxio_d7 | Input/Output | TRGMUX | TRGMUX_IN4 | Input | Platform | NMI_b70 | Input
71 | PTD2 | same | ADC1 | adc_se2 | Input | PTD | port2 | Input, Output | FTM3 | ftm_ch4 | Input, Output | LPSPI1 | lpspi_sout | Input, Output, Input/Output | FLEXIO | fxio_d4 | Input/Output | FLEXIO | fxio_d6 | Input/Output | TRGMUX | TRGMUX_IN5 | Input |  |  |
72 | PTA3 | same | ADC1 | adc_se1 | Input | PTA | port3 | Input, Output | FTM3 | ftm_ch1 | Input, Output | LPI2C0 | lpi2c_sclscl | Input/Output | EWM | ewm_in | Input | FLEXIO | fxio_d5 | Input/Output | LPUART0 | lpuart_tx | Input, Output, Input/Output |  |  |
73 | PTA2 | same | ADC1 | adc_se0 | Input | PTA | port2 | Input, Output | FTM3 | ftm_ch0 | Input, Output | LPI2C0 | lpi2c_sdasda | Input/Output | EWM | ewm_out_b | Output | FLEXIO | fxio_d4 | Input/Output | LPUART0 | lpuart_rx | Input |  |  |
74 | PTB11 | same |  |  |  | PTB | port11 | Input, Output | FTM3 | ftm_ch3 | Input, Output | LPI2C0 | lpi2c_hreqhreq | Input |  |  |  |  |  |  |  |  |  |  |  |
75 | PTB10 | same |  |  |  | PTB | port10 | Input, Output | FTM3 | ftm_ch2 | Input, Output | LPI2C0 | lpi2c_sdassdas | Input/Output |  |  |  |  |  |  |  |  |  |  |  |
76 | PTB9 | same |  |  |  | PTB | port9 | Input, Output | FTM3 | ftm_ch1 | Input, Output | LPI2C0 | lpi2c_sclsscls | Input/Output |  |  |  |  |  |  |  |  |  |  |  |
77 | PTB8 | same |  |  |  | PTB | port8 | Input, Output | FTM3 | ftm_ch0 | Input, Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
78 | PTA1 | same | ADC0 CMP0 | adc_se1 acmp_in1 | Input | PTA | port1 | Input, Output | FTM1 | ftm_ch1 | Input, Output | LPI2C0 | lpi2c_sdassdas | Input/Output | FLEXIO | fxio_d3 | Input/Output | FTM1 | ftm_QD_PHA | Input | LPUART0 | lpuart_rts | Output | TRGMUX | TRGMUX_OUT0 | Output
79 | PTA0 | same | ADC0 CMP0 | adc_se0 acmp_in0 | Input | PTA | port0 | Input, Output | FTM2 | ftm_ch1 | Input, Output | LPI2C0 | lpi2c_sclsscls | Input/Output | FLEXIO | fxio_d2 | Input/Output | FTM2 | ftm_QD_PHA | Input | LPUART0 | lpuart_cts | Input | TRGMUX | TRGMUX_OUT3 | Output
80 | PTC7 | same | ADC1 | adc_se5 | Input | PTC | port7 | Input, Output | LPUART1 | lpuart_tx | Input, Output, Input/Output | CAN1 | can_txtxd | Output | FTM3 | ftm_ch3 | Input, Output |  |  |  | FTM1 | ftm_QD_PHA | Input |  |  |
81 | PTC6 | same | ADC1 | adc_se4 | Input | PTC | port6 | Input, Output | LPUART1 | lpuart_rx | Input | CAN1 | can_rxrxd | Input | FTM3 | ftm_ch2 | Input, Output |  |  |  | FTM1 | ftm_QD_PHB | Input |  |  |
82 | PTA16 | same | ADC1 | adc_se13 | Input | PTA | port16 | Input, Output | FTM1 | ftm_ch3 | Input, Output | LPSPI1 | lpspi_pcs2 | Input, Output, Input/Output |  |  |  |  |  |  |  |  |  |  |  |
83 | PTA15 | same | ADC1 | adc_se12 | Input | PTA | port15 | Input, Output | FTM1 | ftm_ch2 | Input, Output | LPSPI0 | lpspi_pcs3 | Input, Output, Input/Output | LPSPI2 | lpspi_pcs3 | Input, Output, Input/Output |  |  |  |  |  |  |  |  |
84 | PTE6 | same | ADC1 | adc_se11 | Input | PTE | port6 | Input, Output | LPSPI0 | lpspi_pcs2 | Input, Output, Input/Output |  |  |  | FTM3 | ftm_ch7 | Input, Output |  |  |  | LPUART1 | lpuart_rts | Output |  |  |
85 | PTE2 | same | ADC1 | adc_se10 | Input | PTE | port2 | Input, Output | LPSPI0 | lpspi_sout | Input, Output, Input/Output | LPTMR0 | lptmr_alt3 | Input | FTM3 | ftm_ch6 | Input, Output |  |  |  | LPUART1 | lpuart_cts | Input |  |  |
86 | VSS86 | same | PowerAndGround | VSS86 | Output |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
87 | VDD87 | same | PowerAndGround | VDD87 | Input |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
88 | PTA14 | same |  |  |  | PTA | port14 | Input, Output | FTM0 | ftm_flt0 | Input | FTM3 | ftm_flt1 | Input | EWM | ewm_in | Input |  |  |  | FTM1 | ftm_flt0 | Input |  |  |
89 | PTA13 | same |  |  |  | PTA | port13 | Input, Output | FTM1 | ftm_ch7 | Input, Output | CAN1 | can_txtxd | Output |  |  |  |  |  |  | FTM2 | ftm_QD_PHA | Input |  |  |
90 | PTA12 | same |  |  |  | PTA | port12 | Input, Output | FTM1 | ftm_ch6 | Input, Output | CAN1 | can_rxrxd | Input |  |  |  |  |  |  | FTM2 | ftm_QD_PHB | Input |  |  |
91 | PTA11 | same |  |  |  | PTA | port11 | Input, Output | FTM1 | ftm_ch5 | Input, Output |  |  |  | FLEXIO | fxio_d1 | Input/Output | CMP0 | acmp_rrt | Output |  |  |  |  |  |
92 | PTA10 | same |  |  |  | PTA | port10 | Input, Output | FTM1 | ftm_ch4 | Input, Output |  |  |  | FLEXIO | fxio_d0 | Input/Output |  |  |  |  |  |  | JTAG | jtag_tdo | Output
93 | PTE1 | same |  |  |  | PTE | port1 | Input, Output | LPSPI0 | lpspi_sin | Input, Output, Input/Output | LPI2C0 | lpi2c_hreqhreq | Input |  |  |  | LPSPI1 | lpspi_pcs0 | Input, Output, Input/Output | FTM1 | ftm_flt1 | Input |  |  |
94 | PTE0 | same |  |  |  | PTE | port0 | Input, Output | LPSPI0 | lpspi_scksck | Input, Output, Input/Output | FTM1 | TCLK1 | Input |  |  |  | LPSPI1 | lpspi_sout | Input, Output, Input/Output | FTM1 | ftm_flt2 | Input |  |  |
95 | PTC5 | same |  |  |  | PTC | port5 | Input, Output | FTM2 | ftm_ch0 | Input, Output | RTC | RTC_CLKOUT | Output |  |  |  |  |  |  | FTM2 | ftm_QD_PHB | Input | JTAG | jtag_tdi | Input
96 | PTC4 | same | CMP0 | acmp_in2 | Input | PTC | port4 | Input, Output | FTM1 | ftm_ch0 | Input, Output | RTC | RTC_CLKOUT | Output |  |  |  | EWM | ewm_in | Input | FTM1 | ftm_QD_PHB | Input | JTAG SWD | jtag_tclk swd_clk | Input
97 | PTA5 | same |  |  |  | PTA | port5 | Input, Output |  |  |  | FTM1 | TCLK1 | Input |  |  |  |  |  |  |  |  |  | Platform | RESET_b97 | Output
98 | PTA4 | same |  |  |  | PTA | port4 | Input, Output |  |  |  |  |  |  | CMP0 | acmp_out | Output | EWM | ewm_out_b | Output |  |  |  | JTAG SWD | jtag_tms swd_dio | Input/Output
99 | PTA9 | same |  |  |  | PTA | port9 | Input, Output | LPUART2 | lpuart_tx | Input, Output, Input/Output | LPSPI2 | lpspi_pcs0 | Input, Output, Input/Output | FLEXIO | fxio_d7 | Input/Output | FTM3 | ftm_flt2 | Input | FTM1 | ftm_flt3 | Input |  |  |
100 | PTA8 | same |  |  |  | PTA | port8 | Input, Output | LPUART2 | lpuart_rx | Input | LPSPI2 | lpspi_sout | Input, Output, Input/Output | FLEXIO | fxio_d6 | Input/Output | FTM3 | ftm_flt3 | Input |  |  |  |  |  |