From edad341a3ea59b15fca9a6c26b5fdc10c46eb753 Mon Sep 17 00:00:00 2001
From: b19715 <b19715@freescale.com>
Date: Fri, 11 Jun 2021 17:15:56 +0800
Subject: [PATCH 3/3] ISL79987: Support blending mode de-interlace for iMX8QXP.

---
 arch/arm64/boot/dts/freescale/imx8qxp-mek-isl7998x.dts | 13 ++++++++-----
 1 file changed, 8 insertions(+), 5 deletions(-)

diff --git a/arch/arm64/boot/dts/freescale/imx8qxp-mek-isl7998x.dts b/arch/arm64/boot/dts/freescale/imx8qxp-mek-isl7998x.dts
index 4c58b97..1e078e1 100644
--- a/arch/arm64/boot/dts/freescale/imx8qxp-mek-isl7998x.dts
+++ b/arch/arm64/boot/dts/freescale/imx8qxp-mek-isl7998x.dts
@@ -34,10 +34,7 @@
 
 &isi_0 {
 	interface = <2 0 2>;
-	deinterlace_mode = <2>;  /* 0 ~ 1: No de-interlacing,
-				    2: Odd even weave, 3: Even odd weave
-				    4: Odd even blending, 5: Even odd blending
-				    6 ~ 7: Line doubling */
+	deinterlace_blending;
 	ntsc_top = <0>;		/* 0 for ISL79987. */
 	status = "okay";
 };
@@ -73,7 +70,13 @@
 };
 
 &isi_4 {
-	status = "disabled";
+	interface = <2 0 2>;
+	deinterlace_mode = <4>;	/* 0 ~ 1: No de-interlacing,
+				   2: Odd even weave, 3: Even odd weave
+				   4: Odd even blending, 5: Even odd blending
+				   6 ~ 7: Line doubling */
+	ntsc_top = <0>;		/* 0 for ISL79987. */
+	status = "okay";
 };
 
 &isi_5 {
-- 
1.9.1

