Callisto4Bootloader: run_bootloader_ctx_t Union Reference

Callisto4Bootloader

Data Fields
run_bootloader_ctx_t Union Reference

`#include <bl_api.h>`

## Data Fields

struct {
uint32_t imageIndex: 4
uint32_t reserved: 12
uint32_t serialBootInterface: 4
uint32_t bootMode: 4
uint32_t tag: 8
} | B
uint32_t | U

## Detailed Description

Definition at line 153 of file bl_api.h.

## Field Documentation

## ◆ B

struct { ... } run_bootloader_ctx_t::B

## ◆ bootMode

uint32_t run_bootloader_ctx_t::bootMode

Definition at line 160 of file bl_api.h.

## ◆ imageIndex

uint32_t run_bootloader_ctx_t::imageIndex

Definition at line 157 of file bl_api.h.

## ◆ reserved

uint32_t run_bootloader_ctx_t::reserved

Definition at line 158 of file bl_api.h.

## ◆ serialBootInterface

uint32_t run_bootloader_ctx_t::serialBootInterface

Definition at line 159 of file bl_api.h.

## ◆ tag

uint32_t run_bootloader_ctx_t::tag

Definition at line 161 of file bl_api.h.

## ◆ U

uint32_t run_bootloader_ctx_t::U

Definition at line 163 of file bl_api.h.

The documentation for this union was generated from the following file:

- lib/bl_api.h