Callisto4Bootloader: XBARA_Type Struct Reference

Callisto4Bootloader

Data Fields
XBARA_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » XBARA Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint16_t | SEL0
__IO uint16_t | SEL1
__IO uint16_t | SEL2
__IO uint16_t | SEL3
__IO uint16_t | SEL4
__IO uint16_t | SEL5
__IO uint16_t | SEL6
__IO uint16_t | SEL7
__IO uint16_t | SEL8
__IO uint16_t | SEL9
__IO uint16_t | SEL10
__IO uint16_t | SEL11
__IO uint16_t | SEL12
__IO uint16_t | SEL13
__IO uint16_t | SEL14
__IO uint16_t | SEL15
__IO uint16_t | SEL16
__IO uint16_t | SEL17
__IO uint16_t | SEL18
__IO uint16_t | SEL19
__IO uint16_t | SEL20
__IO uint16_t | SEL21
__IO uint16_t | SEL22
__IO uint16_t | SEL23
__IO uint16_t | SEL24
__IO uint16_t | SEL25
__IO uint16_t | SEL26
__IO uint16_t | SEL27
__IO uint16_t | SEL28
__IO uint16_t | SEL29
__IO uint16_t | SEL30
__IO uint16_t | SEL31
__IO uint16_t | SEL32
__IO uint16_t | SEL33
__IO uint16_t | SEL34
__IO uint16_t | SEL35
__IO uint16_t | SEL36
__IO uint16_t | SEL37
__IO uint16_t | SEL38
__IO uint16_t | SEL39
__IO uint16_t | SEL40
__IO uint16_t | SEL41
__IO uint16_t | SEL42
__IO uint16_t | SEL43
__IO uint16_t | SEL44
__IO uint16_t | SEL45
__IO uint16_t | SEL46
__IO uint16_t | SEL47
__IO uint16_t | SEL48
__IO uint16_t | SEL49
__IO uint16_t | SEL50
__IO uint16_t | SEL51
__IO uint16_t | SEL52
__IO uint16_t | SEL53
__IO uint16_t | SEL54
__IO uint16_t | SEL55
__IO uint16_t | SEL56
__IO uint16_t | SEL57
__IO uint16_t | SEL58
__IO uint16_t | SEL59
__IO uint16_t | SEL60
__IO uint16_t | SEL61
__IO uint16_t | SEL62
__IO uint16_t | SEL63
__IO uint16_t | SEL64
__IO uint16_t | SEL65
__IO uint16_t | CTRL0
__IO uint16_t | CTRL1

## Detailed Description

XBARA - Register Layout Typedef

Definition at line 46519 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h