Callisto4Bootloader: EWM Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
EWM Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| EWM Register Masks

## Data Structures

struct | EWM_Type

## Macros

#define | EWM_BASE (0x400B4000u)
#define | EWM ((EWM_Type *)EWM_BASE)
#define | EWM_BASE_ADDRS { EWM_BASE }
#define | EWM_BASE_PTRS { EWM }
#define | EWM_IRQS { EWM_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ EWM

#define EWM ((EWM_Type *)EWM_BASE)

Peripheral EWM base pointer

Definition at line 18531 of file MIMXRT1062.h.

## ◆ EWM_BASE

#define EWM_BASE (0x400B4000u)

Peripheral EWM base address

Definition at line 18529 of file MIMXRT1062.h.

## ◆ EWM_BASE_ADDRS

#define EWM_BASE_ADDRS { EWM_BASE }

Array initializer of EWM peripheral base addresses

Definition at line 18533 of file MIMXRT1062.h.

## ◆ EWM_BASE_PTRS

#define EWM_BASE_PTRS { EWM }

Array initializer of EWM peripheral base pointers

Definition at line 18535 of file MIMXRT1062.h.

## ◆ EWM_IRQS

#define EWM_IRQS { EWM_IRQn }

Interrupt vectors for the EWM peripheral type

Definition at line 18537 of file MIMXRT1062.h.