Callisto4Bootloader: CCM_ANALOG Register Masks

Callisto4Bootloader

CCM_ANALOG Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » CCM_ANALOG Peripheral Access Layer

## PLL_ARM - Analog ARM PLL control Register

#define | CCM_ANALOG_PLL_ARM_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_ARM_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ARM_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ARM_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ARM_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ARM_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ARM_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ARM_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ARM_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ARM_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ARM_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ARM_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ARM_PLL_SEL_MASK (0x80000U)
#define | CCM_ANALOG_PLL_ARM_PLL_SEL_SHIFT (19U)
#define | CCM_ANALOG_PLL_ARM_PLL_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_PLL_SEL_MASK)
#define | CCM_ANALOG_PLL_ARM_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ARM_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ARM_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_LOCK_MASK)

## PLL_ARM_SET - Analog ARM PLL control Register

#define | CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ARM_SET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ARM_SET_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ARM_SET_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ARM_SET_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ARM_SET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ARM_SET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ARM_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ARM_SET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ARM_SET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ARM_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ARM_SET_PLL_SEL_MASK (0x80000U)
#define | CCM_ANALOG_PLL_ARM_SET_PLL_SEL_SHIFT (19U)
#define | CCM_ANALOG_PLL_ARM_SET_PLL_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_PLL_SEL_MASK)
#define | CCM_ANALOG_PLL_ARM_SET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ARM_SET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ARM_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_LOCK_MASK)

## PLL_ARM_CLR - Analog ARM PLL control Register

#define | CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ARM_CLR_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ARM_CLR_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ARM_CLR_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ARM_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ARM_CLR_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ARM_CLR_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ARM_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_MASK (0x80000U)
#define | CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_SHIFT (19U)
#define | CCM_ANALOG_PLL_ARM_CLR_PLL_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_MASK)
#define | CCM_ANALOG_PLL_ARM_CLR_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ARM_CLR_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ARM_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_LOCK_MASK)

## PLL_ARM_TOG - Analog ARM PLL control Register

#define | CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ARM_TOG_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ARM_TOG_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ARM_TOG_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ARM_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ARM_TOG_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ARM_TOG_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ARM_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_MASK (0x80000U)
#define | CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_SHIFT (19U)
#define | CCM_ANALOG_PLL_ARM_TOG_PLL_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_MASK)
#define | CCM_ANALOG_PLL_ARM_TOG_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ARM_TOG_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ARM_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_LOCK_MASK)

## PLL_USB1 - Analog USB1 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB1_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB1_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB1_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB1_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB1_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB1_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB1_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB1_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB1_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_POWER_MASK)
#define | CCM_ANALOG_PLL_USB1_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB1_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB1_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB1_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB1_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB1_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB1_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB1_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB1_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_LOCK_MASK)

## PLL_USB1_SET - Analog USB1 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB1_SET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB1_SET_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB1_SET_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB1_SET_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_POWER_MASK)
#define | CCM_ANALOG_PLL_USB1_SET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB1_SET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB1_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB1_SET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB1_SET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB1_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB1_SET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB1_SET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB1_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_LOCK_MASK)

## PLL_USB1_CLR - Analog USB1 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB1_CLR_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB1_CLR_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB1_CLR_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_POWER_MASK)
#define | CCM_ANALOG_PLL_USB1_CLR_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB1_CLR_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB1_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB1_CLR_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB1_CLR_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB1_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB1_CLR_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB1_CLR_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB1_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_LOCK_MASK)

## PLL_USB1_TOG - Analog USB1 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB1_TOG_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB1_TOG_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB1_TOG_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_POWER_MASK)
#define | CCM_ANALOG_PLL_USB1_TOG_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB1_TOG_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB1_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB1_TOG_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB1_TOG_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB1_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB1_TOG_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB1_TOG_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB1_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_LOCK_MASK)

## PLL_USB2 - Analog USB2 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB2_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB2_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB2_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB2_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB2_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB2_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB2_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB2_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB2_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_POWER_MASK)
#define | CCM_ANALOG_PLL_USB2_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB2_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB2_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB2_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB2_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB2_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB2_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB2_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB2_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_LOCK_MASK)

## PLL_USB2_SET - Analog USB2 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB2_SET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB2_SET_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB2_SET_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB2_SET_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_POWER_MASK)
#define | CCM_ANALOG_PLL_USB2_SET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB2_SET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB2_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB2_SET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB2_SET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB2_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB2_SET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB2_SET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB2_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_LOCK_MASK)

## PLL_USB2_CLR - Analog USB2 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB2_CLR_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB2_CLR_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB2_CLR_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_POWER_MASK)
#define | CCM_ANALOG_PLL_USB2_CLR_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB2_CLR_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB2_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB2_CLR_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB2_CLR_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB2_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB2_CLR_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB2_CLR_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB2_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_LOCK_MASK)

## PLL_USB2_TOG - Analog USB2 480MHz PLL Control Register

#define | CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_MASK (0x2U)
#define | CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_SHIFT (1U)
#define | CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_MASK (0x40U)
#define | CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_SHIFT (6U)
#define | CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_MASK)
#define | CCM_ANALOG_PLL_USB2_TOG_POWER_MASK (0x1000U)
#define | CCM_ANALOG_PLL_USB2_TOG_POWER_SHIFT (12U)
#define | CCM_ANALOG_PLL_USB2_TOG_POWER(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_POWER_MASK)
#define | CCM_ANALOG_PLL_USB2_TOG_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_USB2_TOG_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_USB2_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_ENABLE_MASK)
#define | CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_USB2_TOG_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_USB2_TOG_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_USB2_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_BYPASS_MASK)
#define | CCM_ANALOG_PLL_USB2_TOG_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_USB2_TOG_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_USB2_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_LOCK_MASK)

## PLL_SYS - Analog System PLL Control Register

#define | CCM_ANALOG_PLL_SYS_DIV_SELECT_MASK (0x1U)
#define | CCM_ANALOG_PLL_SYS_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_SYS_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_SYS_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_SYS_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_SYS_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_SYS_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_SYS_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_SYS_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_ENABLE_MASK)
#define | CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_SYS_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_SYS_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_SYS_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_BYPASS_MASK)
#define | CCM_ANALOG_PLL_SYS_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_SYS_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_SYS_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_LOCK_MASK)

## PLL_SYS_SET - Analog System PLL Control Register

#define | CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_MASK (0x1U)
#define | CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_SYS_SET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_SYS_SET_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_SYS_SET_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_SYS_SET_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_SYS_SET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_SYS_SET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_SYS_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_SYS_SET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_SYS_SET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_SYS_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_SYS_SET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_SYS_SET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_SYS_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_LOCK_MASK)

## PLL_SYS_CLR - Analog System PLL Control Register

#define | CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_MASK (0x1U)
#define | CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_SYS_CLR_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_SYS_CLR_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_SYS_CLR_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_SYS_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_ENABLE_MASK)
#define | CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_SYS_CLR_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_SYS_CLR_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_SYS_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_BYPASS_MASK)
#define | CCM_ANALOG_PLL_SYS_CLR_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_SYS_CLR_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_SYS_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_LOCK_MASK)

## PLL_SYS_TOG - Analog System PLL Control Register

#define | CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_MASK (0x1U)
#define | CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_SYS_TOG_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_SYS_TOG_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_SYS_TOG_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_SYS_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_ENABLE_MASK)
#define | CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_SYS_TOG_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_SYS_TOG_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_SYS_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_BYPASS_MASK)
#define | CCM_ANALOG_PLL_SYS_TOG_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_SYS_TOG_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_SYS_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_LOCK_MASK)

## PLL_SYS_SS - 528MHz System PLL Spread Spectrum Register

#define | CCM_ANALOG_PLL_SYS_SS_STEP_MASK (0x7FFFU)
#define | CCM_ANALOG_PLL_SYS_SS_STEP_SHIFT (0U)
#define | CCM_ANALOG_PLL_SYS_SS_STEP(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SS_STEP_SHIFT)) & CCM_ANALOG_PLL_SYS_SS_STEP_MASK)
#define | CCM_ANALOG_PLL_SYS_SS_ENABLE_MASK (0x8000U)
#define | CCM_ANALOG_PLL_SYS_SS_ENABLE_SHIFT (15U)
#define | CCM_ANALOG_PLL_SYS_SS_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SS_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_SS_ENABLE_MASK)
#define | CCM_ANALOG_PLL_SYS_SS_STOP_MASK (0xFFFF0000U)
#define | CCM_ANALOG_PLL_SYS_SS_STOP_SHIFT (16U)
#define | CCM_ANALOG_PLL_SYS_SS_STOP(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SS_STOP_SHIFT)) & CCM_ANALOG_PLL_SYS_SS_STOP_MASK)

## PLL_SYS_NUM - Numerator of 528MHz System PLL Fractional Loop Divider Register

#define | CCM_ANALOG_PLL_SYS_NUM_A_MASK (0x3FFFFFFFU)
#define | CCM_ANALOG_PLL_SYS_NUM_A_SHIFT (0U)
#define | CCM_ANALOG_PLL_SYS_NUM_A(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_NUM_A_SHIFT)) & CCM_ANALOG_PLL_SYS_NUM_A_MASK)

## PLL_SYS_DENOM - Denominator of 528MHz System PLL Fractional Loop Divider Register

#define | CCM_ANALOG_PLL_SYS_DENOM_B_MASK (0x3FFFFFFFU)
#define | CCM_ANALOG_PLL_SYS_DENOM_B_SHIFT (0U)
#define | CCM_ANALOG_PLL_SYS_DENOM_B(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_DENOM_B_SHIFT)) & CCM_ANALOG_PLL_SYS_DENOM_B_MASK)

## PLL_AUDIO - Analog Audio PLL control Register

#define | CCM_ANALOG_PLL_AUDIO_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_AUDIO_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_AUDIO_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_AUDIO_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_AUDIO_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_AUDIO_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_AUDIO_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_AUDIO_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_ENABLE_MASK)
#define | CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_AUDIO_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_AUDIO_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_AUDIO_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_BYPASS_MASK)
#define | CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_AUDIO_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_AUDIO_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_LOCK_MASK)

## PLL_AUDIO_SET - Analog Audio PLL control Register

#define | CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_AUDIO_SET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_AUDIO_SET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_AUDIO_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_AUDIO_SET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_AUDIO_SET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_AUDIO_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_SET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_AUDIO_SET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_AUDIO_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_LOCK_MASK)

## PLL_AUDIO_CLR - Analog Audio PLL control Register

#define | CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_MASK)
#define | CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_MASK)
#define | CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_CLR_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_AUDIO_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_LOCK_MASK)

## PLL_AUDIO_TOG - Analog Audio PLL control Register

#define | CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_MASK)
#define | CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_MASK)
#define | CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_AUDIO_TOG_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_AUDIO_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_LOCK_MASK)

## PLL_AUDIO_NUM - Numerator of Audio PLL Fractional Loop Divider Register

#define | CCM_ANALOG_PLL_AUDIO_NUM_A_MASK (0x3FFFFFFFU)
#define | CCM_ANALOG_PLL_AUDIO_NUM_A_SHIFT (0U)
#define | CCM_ANALOG_PLL_AUDIO_NUM_A(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_NUM_A_SHIFT)) & CCM_ANALOG_PLL_AUDIO_NUM_A_MASK)

## PLL_AUDIO_DENOM - Denominator of Audio PLL Fractional Loop Divider Register

#define | CCM_ANALOG_PLL_AUDIO_DENOM_B_MASK (0x3FFFFFFFU)
#define | CCM_ANALOG_PLL_AUDIO_DENOM_B_SHIFT (0U)
#define | CCM_ANALOG_PLL_AUDIO_DENOM_B(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_DENOM_B_SHIFT)) & CCM_ANALOG_PLL_AUDIO_DENOM_B_MASK)

## PLL_VIDEO - Analog Video PLL control Register

#define | CCM_ANALOG_PLL_VIDEO_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_VIDEO_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_VIDEO_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_VIDEO_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_VIDEO_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_VIDEO_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_VIDEO_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_VIDEO_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_ENABLE_MASK)
#define | CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_VIDEO_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_VIDEO_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_VIDEO_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_BYPASS_MASK)
#define | CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_VIDEO_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_VIDEO_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_LOCK_MASK)

## PLL_VIDEO_SET - Analog Video PLL control Register

#define | CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_VIDEO_SET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_VIDEO_SET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_VIDEO_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_VIDEO_SET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_VIDEO_SET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_VIDEO_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_SET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_VIDEO_SET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_VIDEO_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_LOCK_MASK)

## PLL_VIDEO_CLR - Analog Video PLL control Register

#define | CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_MASK)
#define | CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_MASK)
#define | CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_CLR_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_VIDEO_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_LOCK_MASK)

## PLL_VIDEO_TOG - Analog Video PLL control Register

#define | CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_MASK (0x7FU)
#define | CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_MASK)
#define | CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_MASK)
#define | CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_MASK (0x180000U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_SHIFT (19U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_VIDEO_TOG_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_VIDEO_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_LOCK_MASK)

## PLL_VIDEO_NUM - Numerator of Video PLL Fractional Loop Divider Register

#define | CCM_ANALOG_PLL_VIDEO_NUM_A_MASK (0x3FFFFFFFU)
#define | CCM_ANALOG_PLL_VIDEO_NUM_A_SHIFT (0U)
#define | CCM_ANALOG_PLL_VIDEO_NUM_A(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_NUM_A_SHIFT)) & CCM_ANALOG_PLL_VIDEO_NUM_A_MASK)

## PLL_VIDEO_DENOM - Denominator of Video PLL Fractional Loop Divider Register

#define | CCM_ANALOG_PLL_VIDEO_DENOM_B_MASK (0x3FFFFFFFU)
#define | CCM_ANALOG_PLL_VIDEO_DENOM_B_SHIFT (0U)
#define | CCM_ANALOG_PLL_VIDEO_DENOM_B(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_DENOM_B_SHIFT)) & CCM_ANALOG_PLL_VIDEO_DENOM_B_MASK)

## PLL_ENET - Analog ENET PLL Control Register

#define | CCM_ANALOG_PLL_ENET_DIV_SELECT_MASK (0x3U)
#define | CCM_ANALOG_PLL_ENET_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ENET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_MASK (0xCU)
#define | CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_SHIFT (2U)
#define | CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ENET_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ENET_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ENET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ENET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ENET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ENET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ENET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ENET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ENET_ENET2_REF_EN_MASK (0x100000U)
#define | CCM_ANALOG_PLL_ENET_ENET2_REF_EN_SHIFT (20U)
#define | CCM_ANALOG_PLL_ENET_ENET2_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_ENET2_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_MASK (0x200000U)
#define | CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_SHIFT (21U)
#define | CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ENET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ENET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_LOCK_MASK)

## PLL_ENET_SET - Analog ENET PLL Control Register

#define | CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_MASK (0x3U)
#define | CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ENET_SET_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_MASK (0xCU)
#define | CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_SHIFT (2U)
#define | CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ENET_SET_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ENET_SET_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ENET_SET_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ENET_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ENET_SET_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ENET_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_MASK (0x100000U)
#define | CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_SHIFT (20U)
#define | CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_MASK (0x200000U)
#define | CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_SHIFT (21U)
#define | CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_SET_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ENET_SET_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ENET_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_LOCK_MASK)

## PLL_ENET_CLR - Analog ENET PLL Control Register

#define | CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_MASK (0x3U)
#define | CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_MASK (0xCU)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_SHIFT (2U)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ENET_CLR_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ENET_CLR_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ENET_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ENET_CLR_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ENET_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_MASK (0x100000U)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_SHIFT (20U)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_MASK (0x200000U)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_SHIFT (21U)
#define | CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_CLR_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ENET_CLR_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ENET_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_LOCK_MASK)

## PLL_ENET_TOG - Analog ENET PLL Control Register

#define | CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_MASK (0x3U)
#define | CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_SHIFT (0U)
#define | CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_MASK (0xCU)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_SHIFT (2U)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_MASK (0x1000U)
#define | CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_SHIFT (12U)
#define | CCM_ANALOG_PLL_ENET_TOG_POWERDOWN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_ENABLE_MASK (0x2000U)
#define | CCM_ANALOG_PLL_ENET_TOG_ENABLE_SHIFT (13U)
#define | CCM_ANALOG_PLL_ENET_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENABLE_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_MASK (0xC000U)
#define | CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_SHIFT (14U)
#define | CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_BYPASS_MASK (0x10000U)
#define | CCM_ANALOG_PLL_ENET_TOG_BYPASS_SHIFT (16U)
#define | CCM_ANALOG_PLL_ENET_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_BYPASS_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_MASK (0x100000U)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_SHIFT (20U)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_MASK (0x200000U)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_SHIFT (21U)
#define | CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_MASK)
#define | CCM_ANALOG_PLL_ENET_TOG_LOCK_MASK (0x80000000U)
#define | CCM_ANALOG_PLL_ENET_TOG_LOCK_SHIFT (31U)
#define | CCM_ANALOG_PLL_ENET_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_LOCK_MASK)

## PFD_480 - 480MHz Clock (PLL3) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_480_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_480_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_480_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_480_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_480_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_480_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_480_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_480_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_480_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_480_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_480_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_480_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_480_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_480_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_480_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_480_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_480_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_480_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_480_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_480_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_480_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_480_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_480_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_480_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_480_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD3_CLKGATE_MASK)

## PFD_480_SET - 480MHz Clock (PLL3) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_480_SET_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_480_SET_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_480_SET_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_480_SET_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_480_SET_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_480_SET_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_480_SET_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_480_SET_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_480_SET_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_480_SET_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_480_SET_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_480_SET_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_480_SET_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_480_SET_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_480_SET_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_480_SET_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_480_SET_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_MASK)

## PFD_480_CLR - 480MHz Clock (PLL3) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_MASK)

## PFD_480_TOG - 480MHz Clock (PLL3) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_MASK)

## PFD_528 - 528MHz Clock (PLL2) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_528_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_528_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_528_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_528_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_528_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_528_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_528_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_528_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_528_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_528_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_528_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_528_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_528_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_528_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_528_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_528_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_528_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_528_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_528_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_528_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_528_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_528_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_528_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_528_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_528_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD3_CLKGATE_MASK)

## PFD_528_SET - 528MHz Clock (PLL2) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_528_SET_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_528_SET_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_528_SET_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_528_SET_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_528_SET_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_528_SET_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_528_SET_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_528_SET_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_528_SET_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_528_SET_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_528_SET_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_528_SET_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_528_SET_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_528_SET_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_528_SET_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_528_SET_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_528_SET_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_MASK)

## PFD_528_CLR - 528MHz Clock (PLL2) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_MASK)

## PFD_528_TOG - 528MHz Clock (PLL2) Phase Fractional Divider Control Register

#define | CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_MASK (0x3FU)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_SHIFT (0U)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_MASK (0x40U)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_SHIFT (6U)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_MASK (0x80U)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_SHIFT (7U)
#define | CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_MASK (0x3F00U)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_SHIFT (8U)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_MASK (0x4000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_SHIFT (14U)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_MASK (0x8000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_SHIFT (15U)
#define | CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_MASK (0x3F0000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_SHIFT (16U)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_MASK (0x400000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_SHIFT (22U)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_MASK (0x800000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_SHIFT (23U)
#define | CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_MASK (0x3F000000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_SHIFT (24U)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_FRAC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_MASK (0x40000000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_SHIFT (30U)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_STABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_MASK)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_MASK (0x80000000U)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_SHIFT (31U)
#define | CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_MASK)

## MISC0 - Miscellaneous Register 0

#define | CCM_ANALOG_MISC0_REFTOP_PWD_MASK (0x1U)
#define | CCM_ANALOG_MISC0_REFTOP_PWD_SHIFT (0U)
#define | CCM_ANALOG_MISC0_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_PWD_MASK)
#define | CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_MASK)
#define | CCM_ANALOG_MISC0_REFTOP_VBGADJ_MASK (0x70U)
#define | CCM_ANALOG_MISC0_REFTOP_VBGADJ_SHIFT (4U)
#define | CCM_ANALOG_MISC0_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_VBGADJ_MASK)
#define | CCM_ANALOG_MISC0_REFTOP_VBGUP_MASK (0x80U)
#define | CCM_ANALOG_MISC0_REFTOP_VBGUP_SHIFT (7U)
#define | CCM_ANALOG_MISC0_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_VBGUP_MASK)
#define | CCM_ANALOG_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)
#define | CCM_ANALOG_MISC0_STOP_MODE_CONFIG_SHIFT (10U)
#define | CCM_ANALOG_MISC0_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_STOP_MODE_CONFIG_MASK)
#define | CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)
#define | CCM_ANALOG_MISC0_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_MASK)
#define | CCM_ANALOG_MISC0_OSC_I_MASK (0x6000U)
#define | CCM_ANALOG_MISC0_OSC_I_SHIFT (13U)
#define | CCM_ANALOG_MISC0_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_OSC_I_MASK)
#define | CCM_ANALOG_MISC0_OSC_XTALOK_MASK (0x8000U)
#define | CCM_ANALOG_MISC0_OSC_XTALOK_SHIFT (15U)
#define | CCM_ANALOG_MISC0_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_OSC_XTALOK_MASK)
#define | CCM_ANALOG_MISC0_OSC_XTALOK_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC0_OSC_XTALOK_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC0_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_OSC_XTALOK_EN_MASK)
#define | CCM_ANALOG_MISC0_CLKGATE_CTRL_MASK (0x2000000U)
#define | CCM_ANALOG_MISC0_CLKGATE_CTRL_SHIFT (25U)
#define | CCM_ANALOG_MISC0_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_CLKGATE_CTRL_MASK)
#define | CCM_ANALOG_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)
#define | CCM_ANALOG_MISC0_CLKGATE_DELAY_SHIFT (26U)
#define | CCM_ANALOG_MISC0_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_CLKGATE_DELAY_MASK)
#define | CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)
#define | CCM_ANALOG_MISC0_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_MASK)
#define | CCM_ANALOG_MISC0_XTAL_24M_PWD_MASK (0x40000000U)
#define | CCM_ANALOG_MISC0_XTAL_24M_PWD_SHIFT (30U)
#define | CCM_ANALOG_MISC0_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_REFTOP_PWD_MASK (0x1U)
#define | PMU_MISC0_REFTOP_PWD_SHIFT (0U)
#define | PMU_MISC0_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_PWD_SHIFT)) & PMU_MISC0_REFTOP_PWD_MASK)
#define | PMU_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | PMU_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | PMU_MISC0_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_REFTOP_SELFBIASOFF_MASK)
#define | PMU_MISC0_REFTOP_VBGADJ_MASK (0x70U)
#define | PMU_MISC0_REFTOP_VBGADJ_SHIFT (4U)
#define | PMU_MISC0_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_REFTOP_VBGADJ_MASK)
#define | PMU_MISC0_REFTOP_VBGUP_MASK (0x80U)
#define | PMU_MISC0_REFTOP_VBGUP_SHIFT (7U)
#define | PMU_MISC0_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_REFTOP_VBGUP_MASK)
#define | PMU_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)
#define | PMU_MISC0_STOP_MODE_CONFIG_SHIFT (10U)
#define | PMU_MISC0_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_STOP_MODE_CONFIG_MASK)
#define | PMU_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | PMU_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)
#define | PMU_MISC0_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_DISCON_HIGH_SNVS_MASK)
#define | PMU_MISC0_OSC_I_MASK (0x6000U)
#define | PMU_MISC0_OSC_I_SHIFT (13U)
#define | PMU_MISC0_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_OSC_I_SHIFT)) & PMU_MISC0_OSC_I_MASK)
#define | PMU_MISC0_OSC_XTALOK_MASK (0x8000U)
#define | PMU_MISC0_OSC_XTALOK_SHIFT (15U)
#define | PMU_MISC0_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_OSC_XTALOK_SHIFT)) & PMU_MISC0_OSC_XTALOK_MASK)
#define | PMU_MISC0_OSC_XTALOK_EN_MASK (0x10000U)
#define | PMU_MISC0_OSC_XTALOK_EN_SHIFT (16U)
#define | PMU_MISC0_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_OSC_XTALOK_EN_MASK)
#define | PMU_MISC0_CLKGATE_CTRL_MASK (0x2000000U)
#define | PMU_MISC0_CLKGATE_CTRL_SHIFT (25U)
#define | PMU_MISC0_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_CLKGATE_CTRL_MASK)
#define | PMU_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)
#define | PMU_MISC0_CLKGATE_DELAY_SHIFT (26U)
#define | PMU_MISC0_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_CLKGATE_DELAY_MASK)
#define | PMU_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | PMU_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)
#define | PMU_MISC0_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_RTC_XTAL_SOURCE_MASK)
#define | PMU_MISC0_XTAL_24M_PWD_MASK (0x40000000U)
#define | PMU_MISC0_XTAL_24M_PWD_SHIFT (30U)
#define | PMU_MISC0_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_VID_PLL_PREDIV_MASK (0x80000000U)
#define | PMU_MISC0_VID_PLL_PREDIV_SHIFT (31U)
#define | PMU_MISC0_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_VID_PLL_PREDIV_MASK)
#define | XTALOSC24M_MISC0_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_I_SHIFT)) & XTALOSC24M_MISC0_OSC_I_MASK)
#define | XTALOSC24M_MISC0_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK)

## MISC0_SET - Miscellaneous Register 0

#define | CCM_ANALOG_MISC0_SET_REFTOP_PWD_MASK (0x1U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_PWD_SHIFT (0U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_PWD_MASK)
#define | CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_MASK)
#define | CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_MASK)
#define | CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)
#define | CCM_ANALOG_MISC0_SET_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_MASK)
#define | CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)
#define | CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)
#define | CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_MASK)
#define | CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)
#define | CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_MASK)
#define | CCM_ANALOG_MISC0_SET_OSC_I_MASK (0x6000U)
#define | CCM_ANALOG_MISC0_SET_OSC_I_SHIFT (13U)
#define | CCM_ANALOG_MISC0_SET_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_SET_OSC_I_MASK)
#define | CCM_ANALOG_MISC0_SET_OSC_XTALOK_MASK (0x8000U)
#define | CCM_ANALOG_MISC0_SET_OSC_XTALOK_SHIFT (15U)
#define | CCM_ANALOG_MISC0_SET_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_SET_OSC_XTALOK_MASK)
#define | CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_MASK)
#define | CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)
#define | CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)
#define | CCM_ANALOG_MISC0_SET_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_MASK)
#define | CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)
#define | CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)
#define | CCM_ANALOG_MISC0_SET_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_MASK)
#define | CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)
#define | CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_MASK)
#define | CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)
#define | CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)
#define | CCM_ANALOG_MISC0_SET_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_SET_REFTOP_PWD_MASK (0x1U)
#define | PMU_MISC0_SET_REFTOP_PWD_SHIFT (0U)
#define | PMU_MISC0_SET_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_PWD_SHIFT)) & PMU_MISC0_SET_REFTOP_PWD_MASK)
#define | PMU_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | PMU_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | PMU_MISC0_SET_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_SET_REFTOP_SELFBIASOFF_MASK)
#define | PMU_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)
#define | PMU_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)
#define | PMU_MISC0_SET_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_SET_REFTOP_VBGADJ_MASK)
#define | PMU_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)
#define | PMU_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)
#define | PMU_MISC0_SET_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_SET_REFTOP_VBGUP_MASK)
#define | PMU_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)
#define | PMU_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)
#define | PMU_MISC0_SET_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_SET_STOP_MODE_CONFIG_MASK)
#define | PMU_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | PMU_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)
#define | PMU_MISC0_SET_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_SET_DISCON_HIGH_SNVS_MASK)
#define | PMU_MISC0_SET_OSC_I_MASK (0x6000U)
#define | PMU_MISC0_SET_OSC_I_SHIFT (13U)
#define | PMU_MISC0_SET_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_OSC_I_SHIFT)) & PMU_MISC0_SET_OSC_I_MASK)
#define | PMU_MISC0_SET_OSC_XTALOK_MASK (0x8000U)
#define | PMU_MISC0_SET_OSC_XTALOK_SHIFT (15U)
#define | PMU_MISC0_SET_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_OSC_XTALOK_SHIFT)) & PMU_MISC0_SET_OSC_XTALOK_MASK)
#define | PMU_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)
#define | PMU_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)
#define | PMU_MISC0_SET_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_SET_OSC_XTALOK_EN_MASK)
#define | PMU_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)
#define | PMU_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)
#define | PMU_MISC0_SET_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_SET_CLKGATE_CTRL_MASK)
#define | PMU_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)
#define | PMU_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)
#define | PMU_MISC0_SET_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_SET_CLKGATE_DELAY_MASK)
#define | PMU_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | PMU_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)
#define | PMU_MISC0_SET_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_SET_RTC_XTAL_SOURCE_MASK)
#define | PMU_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)
#define | PMU_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)
#define | PMU_MISC0_SET_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_SET_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_SET_VID_PLL_PREDIV_MASK (0x80000000U)
#define | PMU_MISC0_SET_VID_PLL_PREDIV_SHIFT (31U)
#define | PMU_MISC0_SET_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_SET_VID_PLL_PREDIV_MASK)
#define | XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_SET_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_SET_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_SET_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_SET_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_I_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_I_MASK)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_SET_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_SET_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK)

## MISC0_CLR - Miscellaneous Register 0

#define | CCM_ANALOG_MISC0_CLR_REFTOP_PWD_MASK (0x1U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_PWD_SHIFT (0U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_PWD_MASK)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_MASK)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)
#define | CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_MASK)
#define | CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)
#define | CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)
#define | CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_MASK)
#define | CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)
#define | CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_MASK)
#define | CCM_ANALOG_MISC0_CLR_OSC_I_MASK (0x6000U)
#define | CCM_ANALOG_MISC0_CLR_OSC_I_SHIFT (13U)
#define | CCM_ANALOG_MISC0_CLR_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_CLR_OSC_I_MASK)
#define | CCM_ANALOG_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)
#define | CCM_ANALOG_MISC0_CLR_OSC_XTALOK_SHIFT (15U)
#define | CCM_ANALOG_MISC0_CLR_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_CLR_OSC_XTALOK_MASK)
#define | CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_MASK)
#define | CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)
#define | CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)
#define | CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_MASK)
#define | CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)
#define | CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)
#define | CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_MASK)
#define | CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)
#define | CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_MASK)
#define | CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)
#define | CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)
#define | CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_CLR_REFTOP_PWD_MASK (0x1U)
#define | PMU_MISC0_CLR_REFTOP_PWD_SHIFT (0U)
#define | PMU_MISC0_CLR_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_PWD_SHIFT)) & PMU_MISC0_CLR_REFTOP_PWD_MASK)
#define | PMU_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | PMU_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | PMU_MISC0_CLR_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)
#define | PMU_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)
#define | PMU_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)
#define | PMU_MISC0_CLR_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_CLR_REFTOP_VBGADJ_MASK)
#define | PMU_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)
#define | PMU_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)
#define | PMU_MISC0_CLR_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_CLR_REFTOP_VBGUP_MASK)
#define | PMU_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)
#define | PMU_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)
#define | PMU_MISC0_CLR_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_CLR_STOP_MODE_CONFIG_MASK)
#define | PMU_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | PMU_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)
#define | PMU_MISC0_CLR_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_CLR_DISCON_HIGH_SNVS_MASK)
#define | PMU_MISC0_CLR_OSC_I_MASK (0x6000U)
#define | PMU_MISC0_CLR_OSC_I_SHIFT (13U)
#define | PMU_MISC0_CLR_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_OSC_I_SHIFT)) & PMU_MISC0_CLR_OSC_I_MASK)
#define | PMU_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)
#define | PMU_MISC0_CLR_OSC_XTALOK_SHIFT (15U)
#define | PMU_MISC0_CLR_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_OSC_XTALOK_SHIFT)) & PMU_MISC0_CLR_OSC_XTALOK_MASK)
#define | PMU_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)
#define | PMU_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)
#define | PMU_MISC0_CLR_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_CLR_OSC_XTALOK_EN_MASK)
#define | PMU_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)
#define | PMU_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)
#define | PMU_MISC0_CLR_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_CLR_CLKGATE_CTRL_MASK)
#define | PMU_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)
#define | PMU_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)
#define | PMU_MISC0_CLR_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_CLR_CLKGATE_DELAY_MASK)
#define | PMU_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | PMU_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)
#define | PMU_MISC0_CLR_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_CLR_RTC_XTAL_SOURCE_MASK)
#define | PMU_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)
#define | PMU_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)
#define | PMU_MISC0_CLR_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_CLR_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_CLR_VID_PLL_PREDIV_MASK (0x80000000U)
#define | PMU_MISC0_CLR_VID_PLL_PREDIV_SHIFT (31U)
#define | PMU_MISC0_CLR_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_CLR_VID_PLL_PREDIV_MASK)
#define | XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_CLR_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_CLR_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_CLR_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_I_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_I_MASK)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_CLR_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK)

## MISC0_TOG - Miscellaneous Register 0

#define | CCM_ANALOG_MISC0_TOG_REFTOP_PWD_MASK (0x1U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_PWD_SHIFT (0U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_PWD_MASK)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_MASK)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)
#define | CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_MASK)
#define | CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)
#define | CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)
#define | CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_MASK)
#define | CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)
#define | CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_MASK)
#define | CCM_ANALOG_MISC0_TOG_OSC_I_MASK (0x6000U)
#define | CCM_ANALOG_MISC0_TOG_OSC_I_SHIFT (13U)
#define | CCM_ANALOG_MISC0_TOG_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_TOG_OSC_I_MASK)
#define | CCM_ANALOG_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)
#define | CCM_ANALOG_MISC0_TOG_OSC_XTALOK_SHIFT (15U)
#define | CCM_ANALOG_MISC0_TOG_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_TOG_OSC_XTALOK_MASK)
#define | CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_MASK)
#define | CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)
#define | CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)
#define | CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_MASK)
#define | CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)
#define | CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)
#define | CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_MASK)
#define | CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)
#define | CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_MASK)
#define | CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)
#define | CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)
#define | CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_TOG_REFTOP_PWD_MASK (0x1U)
#define | PMU_MISC0_TOG_REFTOP_PWD_SHIFT (0U)
#define | PMU_MISC0_TOG_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_PWD_SHIFT)) & PMU_MISC0_TOG_REFTOP_PWD_MASK)
#define | PMU_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | PMU_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | PMU_MISC0_TOG_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)
#define | PMU_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)
#define | PMU_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)
#define | PMU_MISC0_TOG_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_TOG_REFTOP_VBGADJ_MASK)
#define | PMU_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)
#define | PMU_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)
#define | PMU_MISC0_TOG_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_TOG_REFTOP_VBGUP_MASK)
#define | PMU_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)
#define | PMU_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)
#define | PMU_MISC0_TOG_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_TOG_STOP_MODE_CONFIG_MASK)
#define | PMU_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | PMU_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)
#define | PMU_MISC0_TOG_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_TOG_DISCON_HIGH_SNVS_MASK)
#define | PMU_MISC0_TOG_OSC_I_MASK (0x6000U)
#define | PMU_MISC0_TOG_OSC_I_SHIFT (13U)
#define | PMU_MISC0_TOG_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_OSC_I_SHIFT)) & PMU_MISC0_TOG_OSC_I_MASK)
#define | PMU_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)
#define | PMU_MISC0_TOG_OSC_XTALOK_SHIFT (15U)
#define | PMU_MISC0_TOG_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_OSC_XTALOK_SHIFT)) & PMU_MISC0_TOG_OSC_XTALOK_MASK)
#define | PMU_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)
#define | PMU_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)
#define | PMU_MISC0_TOG_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_TOG_OSC_XTALOK_EN_MASK)
#define | PMU_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)
#define | PMU_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)
#define | PMU_MISC0_TOG_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_TOG_CLKGATE_CTRL_MASK)
#define | PMU_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)
#define | PMU_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)
#define | PMU_MISC0_TOG_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_TOG_CLKGATE_DELAY_MASK)
#define | PMU_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | PMU_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)
#define | PMU_MISC0_TOG_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_TOG_RTC_XTAL_SOURCE_MASK)
#define | PMU_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)
#define | PMU_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)
#define | PMU_MISC0_TOG_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_TOG_XTAL_24M_PWD_MASK)
#define | PMU_MISC0_TOG_VID_PLL_PREDIV_MASK (0x80000000U)
#define | PMU_MISC0_TOG_VID_PLL_PREDIV_SHIFT (31U)
#define | PMU_MISC0_TOG_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_TOG_VID_PLL_PREDIV_MASK)
#define | XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_TOG_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_TOG_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_TOG_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_I_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_I_MASK)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_TOG_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK)

## MISC1 - Miscellaneous Register 1

#define | CCM_ANALOG_MISC1_LVDS1_CLK_SEL_MASK (0x1FU)
#define | CCM_ANALOG_MISC1_LVDS1_CLK_SEL_SHIFT (0U)
#define | CCM_ANALOG_MISC1_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_LVDS1_CLK_SEL_MASK)
#define | CCM_ANALOG_MISC1_LVDSCLK1_OBEN_MASK (0x400U)
#define | CCM_ANALOG_MISC1_LVDSCLK1_OBEN_SHIFT (10U)
#define | CCM_ANALOG_MISC1_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_LVDSCLK1_OBEN_MASK)
#define | CCM_ANALOG_MISC1_LVDSCLK1_IBEN_MASK (0x1000U)
#define | CCM_ANALOG_MISC1_LVDSCLK1_IBEN_SHIFT (12U)
#define | CCM_ANALOG_MISC1_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_LVDSCLK1_IBEN_MASK)
#define | CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | CCM_ANALOG_MISC1_IRQ_TEMPPANIC_SHIFT (27U)
#define | CCM_ANALOG_MISC1_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_IRQ_TEMPPANIC_MASK)
#define | CCM_ANALOG_MISC1_IRQ_TEMPLOW_MASK (0x10000000U)
#define | CCM_ANALOG_MISC1_IRQ_TEMPLOW_SHIFT (28U)
#define | CCM_ANALOG_MISC1_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_IRQ_TEMPLOW_MASK)
#define | CCM_ANALOG_MISC1_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | CCM_ANALOG_MISC1_IRQ_TEMPHIGH_SHIFT (29U)
#define | CCM_ANALOG_MISC1_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_IRQ_TEMPHIGH_MASK)
#define | CCM_ANALOG_MISC1_IRQ_ANA_BO_MASK (0x40000000U)
#define | CCM_ANALOG_MISC1_IRQ_ANA_BO_SHIFT (30U)
#define | CCM_ANALOG_MISC1_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_IRQ_ANA_BO_MASK)
#define | CCM_ANALOG_MISC1_IRQ_DIG_BO_MASK (0x80000000U)
#define | CCM_ANALOG_MISC1_IRQ_DIG_BO_SHIFT (31U)
#define | CCM_ANALOG_MISC1_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_IRQ_DIG_BO_MASK)
#define | PMU_MISC1_LVDS1_CLK_SEL_MASK (0x1FU)
#define | PMU_MISC1_LVDS1_CLK_SEL_SHIFT (0U)
#define | PMU_MISC1_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_LVDS1_CLK_SEL_MASK)
#define | PMU_MISC1_LVDS2_CLK_SEL_MASK (0x3E0U)
#define | PMU_MISC1_LVDS2_CLK_SEL_SHIFT (5U)
#define | PMU_MISC1_LVDS2_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_LVDS2_CLK_SEL_MASK)
#define | PMU_MISC1_LVDSCLK1_OBEN_MASK (0x400U)
#define | PMU_MISC1_LVDSCLK1_OBEN_SHIFT (10U)
#define | PMU_MISC1_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_LVDSCLK1_OBEN_MASK)
#define | PMU_MISC1_LVDSCLK2_OBEN_MASK (0x800U)
#define | PMU_MISC1_LVDSCLK2_OBEN_SHIFT (11U)
#define | PMU_MISC1_LVDSCLK2_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_LVDSCLK2_OBEN_MASK)
#define | PMU_MISC1_LVDSCLK1_IBEN_MASK (0x1000U)
#define | PMU_MISC1_LVDSCLK1_IBEN_SHIFT (12U)
#define | PMU_MISC1_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_LVDSCLK1_IBEN_MASK)
#define | PMU_MISC1_LVDSCLK2_IBEN_MASK (0x2000U)
#define | PMU_MISC1_LVDSCLK2_IBEN_SHIFT (13U)
#define | PMU_MISC1_LVDSCLK2_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_LVDSCLK2_IBEN_MASK)
#define | PMU_MISC1_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | PMU_MISC1_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | PMU_MISC1_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_PFD_480_AUTOGATE_EN_MASK)
#define | PMU_MISC1_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | PMU_MISC1_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | PMU_MISC1_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_PFD_528_AUTOGATE_EN_MASK)
#define | PMU_MISC1_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | PMU_MISC1_IRQ_TEMPPANIC_SHIFT (27U)
#define | PMU_MISC1_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_IRQ_TEMPPANIC_MASK)
#define | PMU_MISC1_IRQ_TEMPLOW_MASK (0x10000000U)
#define | PMU_MISC1_IRQ_TEMPLOW_SHIFT (28U)
#define | PMU_MISC1_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_IRQ_TEMPLOW_MASK)
#define | PMU_MISC1_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | PMU_MISC1_IRQ_TEMPHIGH_SHIFT (29U)
#define | PMU_MISC1_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_IRQ_TEMPHIGH_MASK)
#define | PMU_MISC1_IRQ_ANA_BO_MASK (0x40000000U)
#define | PMU_MISC1_IRQ_ANA_BO_SHIFT (30U)
#define | PMU_MISC1_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_IRQ_ANA_BO_MASK)
#define | PMU_MISC1_IRQ_DIG_BO_MASK (0x80000000U)
#define | PMU_MISC1_IRQ_DIG_BO_SHIFT (31U)
#define | PMU_MISC1_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_IRQ_DIG_BO_MASK)

## MISC1_SET - Miscellaneous Register 1

#define | CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_MASK (0x1FU)
#define | CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_SHIFT (0U)
#define | CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_MASK)
#define | CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_MASK (0x400U)
#define | CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_SHIFT (10U)
#define | CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_MASK)
#define | CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_MASK (0x1000U)
#define | CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_SHIFT (12U)
#define | CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_MASK)
#define | CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_SHIFT (27U)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_MASK)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_MASK (0x10000000U)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_SHIFT (28U)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_MASK)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_SHIFT (29U)
#define | CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_MASK)
#define | CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_MASK (0x40000000U)
#define | CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_SHIFT (30U)
#define | CCM_ANALOG_MISC1_SET_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_MASK)
#define | CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_MASK (0x80000000U)
#define | CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_SHIFT (31U)
#define | CCM_ANALOG_MISC1_SET_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_MASK)
#define | PMU_MISC1_SET_LVDS1_CLK_SEL_MASK (0x1FU)
#define | PMU_MISC1_SET_LVDS1_CLK_SEL_SHIFT (0U)
#define | PMU_MISC1_SET_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_SET_LVDS1_CLK_SEL_MASK)
#define | PMU_MISC1_SET_LVDS2_CLK_SEL_MASK (0x3E0U)
#define | PMU_MISC1_SET_LVDS2_CLK_SEL_SHIFT (5U)
#define | PMU_MISC1_SET_LVDS2_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_SET_LVDS2_CLK_SEL_MASK)
#define | PMU_MISC1_SET_LVDSCLK1_OBEN_MASK (0x400U)
#define | PMU_MISC1_SET_LVDSCLK1_OBEN_SHIFT (10U)
#define | PMU_MISC1_SET_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK1_OBEN_MASK)
#define | PMU_MISC1_SET_LVDSCLK2_OBEN_MASK (0x800U)
#define | PMU_MISC1_SET_LVDSCLK2_OBEN_SHIFT (11U)
#define | PMU_MISC1_SET_LVDSCLK2_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK2_OBEN_MASK)
#define | PMU_MISC1_SET_LVDSCLK1_IBEN_MASK (0x1000U)
#define | PMU_MISC1_SET_LVDSCLK1_IBEN_SHIFT (12U)
#define | PMU_MISC1_SET_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK1_IBEN_MASK)
#define | PMU_MISC1_SET_LVDSCLK2_IBEN_MASK (0x2000U)
#define | PMU_MISC1_SET_LVDSCLK2_IBEN_SHIFT (13U)
#define | PMU_MISC1_SET_LVDSCLK2_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK2_IBEN_MASK)
#define | PMU_MISC1_SET_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | PMU_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | PMU_MISC1_SET_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_SET_PFD_480_AUTOGATE_EN_MASK)
#define | PMU_MISC1_SET_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | PMU_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | PMU_MISC1_SET_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_SET_PFD_528_AUTOGATE_EN_MASK)
#define | PMU_MISC1_SET_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | PMU_MISC1_SET_IRQ_TEMPPANIC_SHIFT (27U)
#define | PMU_MISC1_SET_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_SET_IRQ_TEMPPANIC_MASK)
#define | PMU_MISC1_SET_IRQ_TEMPLOW_MASK (0x10000000U)
#define | PMU_MISC1_SET_IRQ_TEMPLOW_SHIFT (28U)
#define | PMU_MISC1_SET_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_SET_IRQ_TEMPLOW_MASK)
#define | PMU_MISC1_SET_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | PMU_MISC1_SET_IRQ_TEMPHIGH_SHIFT (29U)
#define | PMU_MISC1_SET_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_SET_IRQ_TEMPHIGH_MASK)
#define | PMU_MISC1_SET_IRQ_ANA_BO_MASK (0x40000000U)
#define | PMU_MISC1_SET_IRQ_ANA_BO_SHIFT (30U)
#define | PMU_MISC1_SET_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_SET_IRQ_ANA_BO_MASK)
#define | PMU_MISC1_SET_IRQ_DIG_BO_MASK (0x80000000U)
#define | PMU_MISC1_SET_IRQ_DIG_BO_SHIFT (31U)
#define | PMU_MISC1_SET_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_SET_IRQ_DIG_BO_MASK)

## MISC1_CLR - Miscellaneous Register 1

#define | CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_MASK (0x1FU)
#define | CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_SHIFT (0U)
#define | CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_MASK)
#define | CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_MASK (0x400U)
#define | CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_SHIFT (10U)
#define | CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_MASK)
#define | CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_MASK (0x1000U)
#define | CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_SHIFT (12U)
#define | CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_MASK)
#define | CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_SHIFT (27U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_MASK)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_MASK (0x10000000U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_SHIFT (28U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_MASK)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_SHIFT (29U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_MASK)
#define | CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_MASK (0x40000000U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_SHIFT (30U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_MASK)
#define | CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_MASK (0x80000000U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_SHIFT (31U)
#define | CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_MASK)
#define | PMU_MISC1_CLR_LVDS1_CLK_SEL_MASK (0x1FU)
#define | PMU_MISC1_CLR_LVDS1_CLK_SEL_SHIFT (0U)
#define | PMU_MISC1_CLR_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_CLR_LVDS1_CLK_SEL_MASK)
#define | PMU_MISC1_CLR_LVDS2_CLK_SEL_MASK (0x3E0U)
#define | PMU_MISC1_CLR_LVDS2_CLK_SEL_SHIFT (5U)
#define | PMU_MISC1_CLR_LVDS2_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_CLR_LVDS2_CLK_SEL_MASK)
#define | PMU_MISC1_CLR_LVDSCLK1_OBEN_MASK (0x400U)
#define | PMU_MISC1_CLR_LVDSCLK1_OBEN_SHIFT (10U)
#define | PMU_MISC1_CLR_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK1_OBEN_MASK)
#define | PMU_MISC1_CLR_LVDSCLK2_OBEN_MASK (0x800U)
#define | PMU_MISC1_CLR_LVDSCLK2_OBEN_SHIFT (11U)
#define | PMU_MISC1_CLR_LVDSCLK2_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK2_OBEN_MASK)
#define | PMU_MISC1_CLR_LVDSCLK1_IBEN_MASK (0x1000U)
#define | PMU_MISC1_CLR_LVDSCLK1_IBEN_SHIFT (12U)
#define | PMU_MISC1_CLR_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK1_IBEN_MASK)
#define | PMU_MISC1_CLR_LVDSCLK2_IBEN_MASK (0x2000U)
#define | PMU_MISC1_CLR_LVDSCLK2_IBEN_SHIFT (13U)
#define | PMU_MISC1_CLR_LVDSCLK2_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK2_IBEN_MASK)
#define | PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | PMU_MISC1_CLR_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK)
#define | PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | PMU_MISC1_CLR_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK)
#define | PMU_MISC1_CLR_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | PMU_MISC1_CLR_IRQ_TEMPPANIC_SHIFT (27U)
#define | PMU_MISC1_CLR_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_CLR_IRQ_TEMPPANIC_MASK)
#define | PMU_MISC1_CLR_IRQ_TEMPLOW_MASK (0x10000000U)
#define | PMU_MISC1_CLR_IRQ_TEMPLOW_SHIFT (28U)
#define | PMU_MISC1_CLR_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_CLR_IRQ_TEMPLOW_MASK)
#define | PMU_MISC1_CLR_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | PMU_MISC1_CLR_IRQ_TEMPHIGH_SHIFT (29U)
#define | PMU_MISC1_CLR_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_CLR_IRQ_TEMPHIGH_MASK)
#define | PMU_MISC1_CLR_IRQ_ANA_BO_MASK (0x40000000U)
#define | PMU_MISC1_CLR_IRQ_ANA_BO_SHIFT (30U)
#define | PMU_MISC1_CLR_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_CLR_IRQ_ANA_BO_MASK)
#define | PMU_MISC1_CLR_IRQ_DIG_BO_MASK (0x80000000U)
#define | PMU_MISC1_CLR_IRQ_DIG_BO_SHIFT (31U)
#define | PMU_MISC1_CLR_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_CLR_IRQ_DIG_BO_MASK)

## MISC1_TOG - Miscellaneous Register 1

#define | CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_MASK (0x1FU)
#define | CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_SHIFT (0U)
#define | CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_MASK)
#define | CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_MASK (0x400U)
#define | CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_SHIFT (10U)
#define | CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_MASK)
#define | CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_MASK (0x1000U)
#define | CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_SHIFT (12U)
#define | CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_MASK)
#define | CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_SHIFT (27U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_MASK)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_MASK (0x10000000U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_SHIFT (28U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_MASK)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_SHIFT (29U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_MASK)
#define | CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_MASK (0x40000000U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_SHIFT (30U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_MASK)
#define | CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_MASK (0x80000000U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_SHIFT (31U)
#define | CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_MASK)
#define | PMU_MISC1_TOG_LVDS1_CLK_SEL_MASK (0x1FU)
#define | PMU_MISC1_TOG_LVDS1_CLK_SEL_SHIFT (0U)
#define | PMU_MISC1_TOG_LVDS1_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_TOG_LVDS1_CLK_SEL_MASK)
#define | PMU_MISC1_TOG_LVDS2_CLK_SEL_MASK (0x3E0U)
#define | PMU_MISC1_TOG_LVDS2_CLK_SEL_SHIFT (5U)
#define | PMU_MISC1_TOG_LVDS2_CLK_SEL(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_TOG_LVDS2_CLK_SEL_MASK)
#define | PMU_MISC1_TOG_LVDSCLK1_OBEN_MASK (0x400U)
#define | PMU_MISC1_TOG_LVDSCLK1_OBEN_SHIFT (10U)
#define | PMU_MISC1_TOG_LVDSCLK1_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK1_OBEN_MASK)
#define | PMU_MISC1_TOG_LVDSCLK2_OBEN_MASK (0x800U)
#define | PMU_MISC1_TOG_LVDSCLK2_OBEN_SHIFT (11U)
#define | PMU_MISC1_TOG_LVDSCLK2_OBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK2_OBEN_MASK)
#define | PMU_MISC1_TOG_LVDSCLK1_IBEN_MASK (0x1000U)
#define | PMU_MISC1_TOG_LVDSCLK1_IBEN_SHIFT (12U)
#define | PMU_MISC1_TOG_LVDSCLK1_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK1_IBEN_MASK)
#define | PMU_MISC1_TOG_LVDSCLK2_IBEN_MASK (0x2000U)
#define | PMU_MISC1_TOG_LVDSCLK2_IBEN_SHIFT (13U)
#define | PMU_MISC1_TOG_LVDSCLK2_IBEN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK2_IBEN_MASK)
#define | PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK (0x10000U)
#define | PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT (16U)
#define | PMU_MISC1_TOG_PFD_480_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK)
#define | PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK (0x20000U)
#define | PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT (17U)
#define | PMU_MISC1_TOG_PFD_528_AUTOGATE_EN(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK)
#define | PMU_MISC1_TOG_IRQ_TEMPPANIC_MASK (0x8000000U)
#define | PMU_MISC1_TOG_IRQ_TEMPPANIC_SHIFT (27U)
#define | PMU_MISC1_TOG_IRQ_TEMPPANIC(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_TOG_IRQ_TEMPPANIC_MASK)
#define | PMU_MISC1_TOG_IRQ_TEMPLOW_MASK (0x10000000U)
#define | PMU_MISC1_TOG_IRQ_TEMPLOW_SHIFT (28U)
#define | PMU_MISC1_TOG_IRQ_TEMPLOW(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_TOG_IRQ_TEMPLOW_MASK)
#define | PMU_MISC1_TOG_IRQ_TEMPHIGH_MASK (0x20000000U)
#define | PMU_MISC1_TOG_IRQ_TEMPHIGH_SHIFT (29U)
#define | PMU_MISC1_TOG_IRQ_TEMPHIGH(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_TOG_IRQ_TEMPHIGH_MASK)
#define | PMU_MISC1_TOG_IRQ_ANA_BO_MASK (0x40000000U)
#define | PMU_MISC1_TOG_IRQ_ANA_BO_SHIFT (30U)
#define | PMU_MISC1_TOG_IRQ_ANA_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_TOG_IRQ_ANA_BO_MASK)
#define | PMU_MISC1_TOG_IRQ_DIG_BO_MASK (0x80000000U)
#define | PMU_MISC1_TOG_IRQ_DIG_BO_SHIFT (31U)
#define | PMU_MISC1_TOG_IRQ_DIG_BO(x) (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_TOG_IRQ_DIG_BO_MASK)

## MISC2 - Miscellaneous Register 2

#define | CCM_ANALOG_MISC2_REG0_BO_OFFSET_MASK (0x7U)
#define | CCM_ANALOG_MISC2_REG0_BO_OFFSET_SHIFT (0U)
#define | CCM_ANALOG_MISC2_REG0_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_REG0_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_REG0_BO_STATUS_MASK (0x8U)
#define | CCM_ANALOG_MISC2_REG0_BO_STATUS_SHIFT (3U)
#define | CCM_ANALOG_MISC2_REG0_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_REG0_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_REG0_ENABLE_BO_MASK (0x20U)
#define | CCM_ANALOG_MISC2_REG0_ENABLE_BO_SHIFT (5U)
#define | CCM_ANALOG_MISC2_REG0_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_REG0_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_REG0_OK_MASK (0x40U)
#define | CCM_ANALOG_MISC2_REG0_OK_SHIFT (6U)
#define | CCM_ANALOG_MISC2_REG0_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_REG0_OK_MASK)
#define | CCM_ANALOG_MISC2_PLL3_DISABLE_MASK (0x80U)
#define | CCM_ANALOG_MISC2_PLL3_DISABLE_SHIFT (7U)
#define | CCM_ANALOG_MISC2_PLL3_DISABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_PLL3_DISABLE_MASK)
#define | CCM_ANALOG_MISC2_REG1_BO_OFFSET_MASK (0x700U)
#define | CCM_ANALOG_MISC2_REG1_BO_OFFSET_SHIFT (8U)
#define | CCM_ANALOG_MISC2_REG1_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_REG1_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_REG1_BO_STATUS_MASK (0x800U)
#define | CCM_ANALOG_MISC2_REG1_BO_STATUS_SHIFT (11U)
#define | CCM_ANALOG_MISC2_REG1_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_REG1_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_REG1_ENABLE_BO_MASK (0x2000U)
#define | CCM_ANALOG_MISC2_REG1_ENABLE_BO_SHIFT (13U)
#define | CCM_ANALOG_MISC2_REG1_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_REG1_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_REG1_OK_MASK (0x4000U)
#define | CCM_ANALOG_MISC2_REG1_OK_SHIFT (14U)
#define | CCM_ANALOG_MISC2_REG1_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_REG1_OK_MASK)
#define | CCM_ANALOG_MISC2_AUDIO_DIV_LSB_MASK (0x8000U)
#define | CCM_ANALOG_MISC2_AUDIO_DIV_LSB_SHIFT (15U)
#define | CCM_ANALOG_MISC2_AUDIO_DIV_LSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_AUDIO_DIV_LSB_MASK)
#define | CCM_ANALOG_MISC2_REG2_BO_OFFSET_MASK (0x70000U)
#define | CCM_ANALOG_MISC2_REG2_BO_OFFSET_SHIFT (16U)
#define | CCM_ANALOG_MISC2_REG2_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_REG2_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_REG2_BO_STATUS_MASK (0x80000U)
#define | CCM_ANALOG_MISC2_REG2_BO_STATUS_SHIFT (19U)
#define | CCM_ANALOG_MISC2_REG2_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_REG2_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_REG2_ENABLE_BO_MASK (0x200000U)
#define | CCM_ANALOG_MISC2_REG2_ENABLE_BO_SHIFT (21U)
#define | CCM_ANALOG_MISC2_REG2_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_REG2_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_REG2_OK_MASK (0x400000U)
#define | CCM_ANALOG_MISC2_REG2_OK_SHIFT (22U)
#define | CCM_ANALOG_MISC2_REG2_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_REG2_OK_MASK)
#define | CCM_ANALOG_MISC2_AUDIO_DIV_MSB_MASK (0x800000U)
#define | CCM_ANALOG_MISC2_AUDIO_DIV_MSB_SHIFT (23U)
#define | CCM_ANALOG_MISC2_AUDIO_DIV_MSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_AUDIO_DIV_MSB_MASK)
#define | CCM_ANALOG_MISC2_REG0_STEP_TIME_MASK (0x3000000U)
#define | CCM_ANALOG_MISC2_REG0_STEP_TIME_SHIFT (24U)
#define | CCM_ANALOG_MISC2_REG0_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_REG0_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_REG1_STEP_TIME_MASK (0xC000000U)
#define | CCM_ANALOG_MISC2_REG1_STEP_TIME_SHIFT (26U)
#define | CCM_ANALOG_MISC2_REG1_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_REG1_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_REG2_STEP_TIME_MASK (0x30000000U)
#define | CCM_ANALOG_MISC2_REG2_STEP_TIME_SHIFT (28U)
#define | CCM_ANALOG_MISC2_REG2_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_REG2_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_VIDEO_DIV_MASK (0xC0000000U)
#define | CCM_ANALOG_MISC2_VIDEO_DIV_SHIFT (30U)
#define | CCM_ANALOG_MISC2_VIDEO_DIV(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_VIDEO_DIV_MASK)

## MISC2_SET - Miscellaneous Register 2

#define | CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_MASK (0x7U)
#define | CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_SHIFT (0U)
#define | CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_MASK (0x8U)
#define | CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_SHIFT (3U)
#define | CCM_ANALOG_MISC2_SET_REG0_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_MASK (0x20U)
#define | CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_SHIFT (5U)
#define | CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_SET_REG0_OK_MASK (0x40U)
#define | CCM_ANALOG_MISC2_SET_REG0_OK_SHIFT (6U)
#define | CCM_ANALOG_MISC2_SET_REG0_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_OK_MASK)
#define | CCM_ANALOG_MISC2_SET_PLL3_DISABLE_MASK (0x80U)
#define | CCM_ANALOG_MISC2_SET_PLL3_DISABLE_SHIFT (7U)
#define | CCM_ANALOG_MISC2_SET_PLL3_DISABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_SET_PLL3_DISABLE_MASK)
#define | CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_MASK (0x700U)
#define | CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_SHIFT (8U)
#define | CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_MASK (0x800U)
#define | CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_SHIFT (11U)
#define | CCM_ANALOG_MISC2_SET_REG1_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_MASK (0x2000U)
#define | CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_SHIFT (13U)
#define | CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_SET_REG1_OK_MASK (0x4000U)
#define | CCM_ANALOG_MISC2_SET_REG1_OK_SHIFT (14U)
#define | CCM_ANALOG_MISC2_SET_REG1_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_OK_MASK)
#define | CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_MASK (0x8000U)
#define | CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_SHIFT (15U)
#define | CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_MASK)
#define | CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_MASK (0x70000U)
#define | CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_SHIFT (16U)
#define | CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_MASK (0x80000U)
#define | CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_SHIFT (19U)
#define | CCM_ANALOG_MISC2_SET_REG2_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_MASK (0x200000U)
#define | CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_SHIFT (21U)
#define | CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_SET_REG2_OK_MASK (0x400000U)
#define | CCM_ANALOG_MISC2_SET_REG2_OK_SHIFT (22U)
#define | CCM_ANALOG_MISC2_SET_REG2_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_OK_MASK)
#define | CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_MASK (0x800000U)
#define | CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_SHIFT (23U)
#define | CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_MASK)
#define | CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_MASK (0x3000000U)
#define | CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_SHIFT (24U)
#define | CCM_ANALOG_MISC2_SET_REG0_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_MASK (0xC000000U)
#define | CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_SHIFT (26U)
#define | CCM_ANALOG_MISC2_SET_REG1_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_MASK (0x30000000U)
#define | CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_SHIFT (28U)
#define | CCM_ANALOG_MISC2_SET_REG2_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_SET_VIDEO_DIV_MASK (0xC0000000U)
#define | CCM_ANALOG_MISC2_SET_VIDEO_DIV_SHIFT (30U)
#define | CCM_ANALOG_MISC2_SET_VIDEO_DIV(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_SET_VIDEO_DIV_MASK)

## MISC2_CLR - Miscellaneous Register 2

#define | CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_MASK (0x7U)
#define | CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_SHIFT (0U)
#define | CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_MASK (0x8U)
#define | CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_SHIFT (3U)
#define | CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_MASK (0x20U)
#define | CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_SHIFT (5U)
#define | CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG0_OK_MASK (0x40U)
#define | CCM_ANALOG_MISC2_CLR_REG0_OK_SHIFT (6U)
#define | CCM_ANALOG_MISC2_CLR_REG0_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_OK_MASK)
#define | CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_MASK (0x80U)
#define | CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_SHIFT (7U)
#define | CCM_ANALOG_MISC2_CLR_PLL3_DISABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_MASK (0x700U)
#define | CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_SHIFT (8U)
#define | CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_MASK (0x800U)
#define | CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_SHIFT (11U)
#define | CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_MASK (0x2000U)
#define | CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_SHIFT (13U)
#define | CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG1_OK_MASK (0x4000U)
#define | CCM_ANALOG_MISC2_CLR_REG1_OK_SHIFT (14U)
#define | CCM_ANALOG_MISC2_CLR_REG1_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_OK_MASK)
#define | CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_MASK (0x8000U)
#define | CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_SHIFT (15U)
#define | CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_MASK (0x70000U)
#define | CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_SHIFT (16U)
#define | CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_MASK (0x80000U)
#define | CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_SHIFT (19U)
#define | CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_MASK (0x200000U)
#define | CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_SHIFT (21U)
#define | CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG2_OK_MASK (0x400000U)
#define | CCM_ANALOG_MISC2_CLR_REG2_OK_SHIFT (22U)
#define | CCM_ANALOG_MISC2_CLR_REG2_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_OK_MASK)
#define | CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_MASK (0x800000U)
#define | CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_SHIFT (23U)
#define | CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_MASK (0x3000000U)
#define | CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_SHIFT (24U)
#define | CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_MASK (0xC000000U)
#define | CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_SHIFT (26U)
#define | CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_MASK (0x30000000U)
#define | CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_SHIFT (28U)
#define | CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_CLR_VIDEO_DIV_MASK (0xC0000000U)
#define | CCM_ANALOG_MISC2_CLR_VIDEO_DIV_SHIFT (30U)
#define | CCM_ANALOG_MISC2_CLR_VIDEO_DIV(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_CLR_VIDEO_DIV_MASK)

## MISC2_TOG - Miscellaneous Register 2

#define | CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_MASK (0x7U)
#define | CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_SHIFT (0U)
#define | CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_MASK (0x8U)
#define | CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_SHIFT (3U)
#define | CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_MASK (0x20U)
#define | CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_SHIFT (5U)
#define | CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG0_OK_MASK (0x40U)
#define | CCM_ANALOG_MISC2_TOG_REG0_OK_SHIFT (6U)
#define | CCM_ANALOG_MISC2_TOG_REG0_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_OK_MASK)
#define | CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_MASK (0x80U)
#define | CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_SHIFT (7U)
#define | CCM_ANALOG_MISC2_TOG_PLL3_DISABLE(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_MASK (0x700U)
#define | CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_SHIFT (8U)
#define | CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_MASK (0x800U)
#define | CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_SHIFT (11U)
#define | CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_MASK (0x2000U)
#define | CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_SHIFT (13U)
#define | CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG1_OK_MASK (0x4000U)
#define | CCM_ANALOG_MISC2_TOG_REG1_OK_SHIFT (14U)
#define | CCM_ANALOG_MISC2_TOG_REG1_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_OK_MASK)
#define | CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_MASK (0x8000U)
#define | CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_SHIFT (15U)
#define | CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_MASK (0x70000U)
#define | CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_SHIFT (16U)
#define | CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_MASK (0x80000U)
#define | CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_SHIFT (19U)
#define | CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_MASK (0x200000U)
#define | CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_SHIFT (21U)
#define | CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG2_OK_MASK (0x400000U)
#define | CCM_ANALOG_MISC2_TOG_REG2_OK_SHIFT (22U)
#define | CCM_ANALOG_MISC2_TOG_REG2_OK(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_OK_MASK)
#define | CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_MASK (0x800000U)
#define | CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_SHIFT (23U)
#define | CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_MASK (0x3000000U)
#define | CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_SHIFT (24U)
#define | CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_MASK (0xC000000U)
#define | CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_SHIFT (26U)
#define | CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_MASK (0x30000000U)
#define | CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_SHIFT (28U)
#define | CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_MASK)
#define | CCM_ANALOG_MISC2_TOG_VIDEO_DIV_MASK (0xC0000000U)
#define | CCM_ANALOG_MISC2_TOG_VIDEO_DIV_SHIFT (30U)
#define | CCM_ANALOG_MISC2_TOG_VIDEO_DIV(x) (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_TOG_VIDEO_DIV_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ CCM_ANALOG_MISC0_CLKGATE_CTRL

#define CCM_ANALOG_MISC0_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 8724 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLKGATE_CTRL_MASK

#define CCM_ANALOG_MISC0_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 8718 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLKGATE_CTRL_SHIFT

#define CCM_ANALOG_MISC0_CLKGATE_CTRL_SHIFT (25U)

Definition at line 8719 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLKGATE_DELAY

#define CCM_ANALOG_MISC0_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 8737 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLKGATE_DELAY_MASK

#define CCM_ANALOG_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 8725 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLKGATE_DELAY_SHIFT

#define CCM_ANALOG_MISC0_CLKGATE_DELAY_SHIFT (26U)

Definition at line 8726 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL

#define CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 8908 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_MASK

#define CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 8902 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_SHIFT

#define CCM_ANALOG_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)

Definition at line 8903 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY

#define CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 8921 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_MASK

#define CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 8909 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_SHIFT

#define CCM_ANALOG_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)

Definition at line 8910 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS

#define CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 8886 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_MASK

#define CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 8880 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT

#define CCM_ANALOG_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 8881 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_I

#define CCM_ANALOG_MISC0_CLR_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_CLR_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 8895 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_I_MASK

#define CCM_ANALOG_MISC0_CLR_OSC_I_MASK (0x6000U)

Definition at line 8887 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_I_SHIFT

#define CCM_ANALOG_MISC0_CLR_OSC_I_SHIFT (13U)

Definition at line 8888 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_XTALOK

#define CCM_ANALOG_MISC0_CLR_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_CLR_OSC_XTALOK_MASK)

Definition at line 8898 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN

#define CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_MASK)

Definition at line 8901 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_MASK

#define CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 8899 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_SHIFT

#define CCM_ANALOG_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 8900 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_XTALOK_MASK

#define CCM_ANALOG_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)

Definition at line 8896 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_OSC_XTALOK_SHIFT

#define CCM_ANALOG_MISC0_CLR_OSC_XTALOK_SHIFT (15U)

Definition at line 8897 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_PWD

#define CCM_ANALOG_MISC0_CLR_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_PWD_MASK)

Definition at line 8846 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_PWD_MASK

#define CCM_ANALOG_MISC0_CLR_REFTOP_PWD_MASK (0x1U)

Definition at line 8844 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_PWD_SHIFT

#define CCM_ANALOG_MISC0_CLR_REFTOP_PWD_SHIFT (0U)

Definition at line 8845 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF

#define CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 8853 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_MASK

#define CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 8847 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT

#define CCM_ANALOG_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 8848 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ

#define CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 8866 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_MASK

#define CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 8854 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_SHIFT

#define CCM_ANALOG_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 8855 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP

#define CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_MASK)

Definition at line 8869 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_MASK

#define CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)

Definition at line 8867 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_SHIFT

#define CCM_ANALOG_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)

Definition at line 8868 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE

#define CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 8928 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_MASK

#define CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 8922 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT

#define CCM_ANALOG_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 8923 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG

#define CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except RTC powered down on stop mode assertion. 0b01..Beside RTC, analog bandgap, 1p1 and 2p5 regulators are also on. 0b10..Beside RTC, 1p1 and 2p5 regulators are also on, low-power bandgap is selected so that the normal analog bandgap together with the rest analog is powered down. 0b11..Beside RTC, low-power bandgap is selected and the rest analog is powered down.

Definition at line 8879 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_MASK

#define CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 8870 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_SHIFT

#define CCM_ANALOG_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 8871 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD

#define CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_MASK)

Definition at line 8931 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_MASK

#define CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 8929 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_SHIFT

#define CCM_ANALOG_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)

Definition at line 8930 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_DISCON_HIGH_SNVS

#define CCM_ANALOG_MISC0_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 8702 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_MASK

#define CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 8696 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_SHIFT

#define CCM_ANALOG_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 8697 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_I

#define CCM_ANALOG_MISC0_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 8711 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_I_MASK

#define CCM_ANALOG_MISC0_OSC_I_MASK (0x6000U)

Definition at line 8703 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_I_SHIFT

#define CCM_ANALOG_MISC0_OSC_I_SHIFT (13U)

Definition at line 8704 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_XTALOK

#define CCM_ANALOG_MISC0_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_OSC_XTALOK_MASK)

Definition at line 8714 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_XTALOK_EN

#define CCM_ANALOG_MISC0_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_OSC_XTALOK_EN_MASK)

Definition at line 8717 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_XTALOK_EN_MASK

#define CCM_ANALOG_MISC0_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 8715 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_XTALOK_EN_SHIFT

#define CCM_ANALOG_MISC0_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 8716 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_XTALOK_MASK

#define CCM_ANALOG_MISC0_OSC_XTALOK_MASK (0x8000U)

Definition at line 8712 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_OSC_XTALOK_SHIFT

#define CCM_ANALOG_MISC0_OSC_XTALOK_SHIFT (15U)

Definition at line 8713 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_PWD

#define CCM_ANALOG_MISC0_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_PWD_MASK)

Definition at line 8662 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_PWD_MASK

#define CCM_ANALOG_MISC0_REFTOP_PWD_MASK (0x1U)

Definition at line 8660 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_PWD_SHIFT

#define CCM_ANALOG_MISC0_REFTOP_PWD_SHIFT (0U)

Definition at line 8661 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF

#define CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 8669 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_MASK

#define CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 8663 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_SHIFT

#define CCM_ANALOG_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 8664 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_VBGADJ

#define CCM_ANALOG_MISC0_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 8682 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_VBGADJ_MASK

#define CCM_ANALOG_MISC0_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 8670 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_VBGADJ_SHIFT

#define CCM_ANALOG_MISC0_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 8671 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_VBGUP

#define CCM_ANALOG_MISC0_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_REFTOP_VBGUP_MASK)

Definition at line 8685 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_VBGUP_MASK

#define CCM_ANALOG_MISC0_REFTOP_VBGUP_MASK (0x80U)

Definition at line 8683 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_REFTOP_VBGUP_SHIFT

#define CCM_ANALOG_MISC0_REFTOP_VBGUP_SHIFT (7U)

Definition at line 8684 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_RTC_XTAL_SOURCE

#define CCM_ANALOG_MISC0_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 8744 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_MASK

#define CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 8738 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_SHIFT

#define CCM_ANALOG_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 8739 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_CLKGATE_CTRL

#define CCM_ANALOG_MISC0_SET_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 8816 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_MASK

#define CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 8810 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_SHIFT

#define CCM_ANALOG_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)

Definition at line 8811 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_CLKGATE_DELAY

#define CCM_ANALOG_MISC0_SET_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 8829 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_MASK

#define CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 8817 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_SHIFT

#define CCM_ANALOG_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)

Definition at line 8818 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS

#define CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 8794 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_MASK

#define CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 8788 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_SHIFT

#define CCM_ANALOG_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 8789 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_I

#define CCM_ANALOG_MISC0_SET_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_SET_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 8803 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_I_MASK

#define CCM_ANALOG_MISC0_SET_OSC_I_MASK (0x6000U)

Definition at line 8795 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_I_SHIFT

#define CCM_ANALOG_MISC0_SET_OSC_I_SHIFT (13U)

Definition at line 8796 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_XTALOK

#define CCM_ANALOG_MISC0_SET_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_SET_OSC_XTALOK_MASK)

Definition at line 8806 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN

#define CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_MASK)

Definition at line 8809 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_MASK

#define CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 8807 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_SHIFT

#define CCM_ANALOG_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 8808 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_XTALOK_MASK

#define CCM_ANALOG_MISC0_SET_OSC_XTALOK_MASK (0x8000U)

Definition at line 8804 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_OSC_XTALOK_SHIFT

#define CCM_ANALOG_MISC0_SET_OSC_XTALOK_SHIFT (15U)

Definition at line 8805 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_PWD

#define CCM_ANALOG_MISC0_SET_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_PWD_MASK)

Definition at line 8754 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_PWD_MASK

#define CCM_ANALOG_MISC0_SET_REFTOP_PWD_MASK (0x1U)

Definition at line 8752 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_PWD_SHIFT

#define CCM_ANALOG_MISC0_SET_REFTOP_PWD_SHIFT (0U)

Definition at line 8753 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF

#define CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 8761 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_MASK

#define CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 8755 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT

#define CCM_ANALOG_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 8756 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ

#define CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 8774 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_MASK

#define CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 8762 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_SHIFT

#define CCM_ANALOG_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 8763 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_VBGUP

#define CCM_ANALOG_MISC0_SET_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_MASK)

Definition at line 8777 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_MASK

#define CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)

Definition at line 8775 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_SHIFT

#define CCM_ANALOG_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)

Definition at line 8776 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE

#define CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 8836 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_MASK

#define CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 8830 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_SHIFT

#define CCM_ANALOG_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 8831 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG

#define CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except RTC powered down on stop mode assertion. 0b01..Beside RTC, analog bandgap, 1p1 and 2p5 regulators are also on. 0b10..Beside RTC, 1p1 and 2p5 regulators are also on, low-power bandgap is selected so that the normal analog bandgap together with the rest analog is powered down. 0b11..Beside RTC, low-power bandgap is selected and the rest analog is powered down.

Definition at line 8787 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_MASK

#define CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 8778 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_SHIFT

#define CCM_ANALOG_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 8779 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_XTAL_24M_PWD

#define CCM_ANALOG_MISC0_SET_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_MASK)

Definition at line 8839 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_MASK

#define CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 8837 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_SHIFT

#define CCM_ANALOG_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)

Definition at line 8838 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_STOP_MODE_CONFIG

#define CCM_ANALOG_MISC0_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except RTC powered down on stop mode assertion. 0b01..Beside RTC, analog bandgap, 1p1 and 2p5 regulators are also on. 0b10..Beside RTC, 1p1 and 2p5 regulators are also on, low-power bandgap is selected so that the normal analog bandgap together with the rest analog is powered down. 0b11..Beside RTC, low-power bandgap is selected and the rest analog is powered down.

Definition at line 8695 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_STOP_MODE_CONFIG_MASK

#define CCM_ANALOG_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 8686 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_STOP_MODE_CONFIG_SHIFT

#define CCM_ANALOG_MISC0_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 8687 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL

#define CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 9000 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_MASK

#define CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 8994 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_SHIFT

#define CCM_ANALOG_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)

Definition at line 8995 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY

#define CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 9013 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_MASK

#define CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 9001 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_SHIFT

#define CCM_ANALOG_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)

Definition at line 9002 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS

#define CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 8978 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_MASK

#define CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 8972 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT

#define CCM_ANALOG_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 8973 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_I

#define CCM_ANALOG_MISC0_TOG_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_OSC_I_SHIFT)) & CCM_ANALOG_MISC0_TOG_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 8987 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_I_MASK

#define CCM_ANALOG_MISC0_TOG_OSC_I_MASK (0x6000U)

Definition at line 8979 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_I_SHIFT

#define CCM_ANALOG_MISC0_TOG_OSC_I_SHIFT (13U)

Definition at line 8980 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_XTALOK

#define CCM_ANALOG_MISC0_TOG_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_OSC_XTALOK_SHIFT)) & CCM_ANALOG_MISC0_TOG_OSC_XTALOK_MASK)

Definition at line 8990 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN

#define CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_MASK)

Definition at line 8993 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_MASK

#define CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 8991 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_SHIFT

#define CCM_ANALOG_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 8992 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_XTALOK_MASK

#define CCM_ANALOG_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)

Definition at line 8988 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_OSC_XTALOK_SHIFT

#define CCM_ANALOG_MISC0_TOG_OSC_XTALOK_SHIFT (15U)

Definition at line 8989 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_PWD

#define CCM_ANALOG_MISC0_TOG_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_PWD_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_PWD_MASK)

Definition at line 8938 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_PWD_MASK

#define CCM_ANALOG_MISC0_TOG_REFTOP_PWD_MASK (0x1U)

Definition at line 8936 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_PWD_SHIFT

#define CCM_ANALOG_MISC0_TOG_REFTOP_PWD_SHIFT (0U)

Definition at line 8937 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF

#define CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 8945 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_MASK

#define CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 8939 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT

#define CCM_ANALOG_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 8940 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ

#define CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 8958 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_MASK

#define CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 8946 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_SHIFT

#define CCM_ANALOG_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 8947 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP

#define CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_MASK)

Definition at line 8961 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_MASK

#define CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)

Definition at line 8959 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_SHIFT

#define CCM_ANALOG_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)

Definition at line 8960 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE

#define CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 9020 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_MASK

#define CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 9014 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT

#define CCM_ANALOG_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 9015 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG

#define CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except RTC powered down on stop mode assertion. 0b01..Beside RTC, analog bandgap, 1p1 and 2p5 regulators are also on. 0b10..Beside RTC, 1p1 and 2p5 regulators are also on, low-power bandgap is selected so that the normal analog bandgap together with the rest analog is powered down. 0b11..Beside RTC, low-power bandgap is selected and the rest analog is powered down.

Definition at line 8971 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_MASK

#define CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 8962 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_SHIFT

#define CCM_ANALOG_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 8963 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD

#define CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_MASK)

Definition at line 9023 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_MASK

#define CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 9021 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_SHIFT

#define CCM_ANALOG_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)

Definition at line 9022 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_XTAL_24M_PWD

#define CCM_ANALOG_MISC0_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC0_XTAL_24M_PWD_SHIFT)) & CCM_ANALOG_MISC0_XTAL_24M_PWD_MASK)

Definition at line 8747 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_XTAL_24M_PWD_MASK

#define CCM_ANALOG_MISC0_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 8745 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC0_XTAL_24M_PWD_SHIFT

#define CCM_ANALOG_MISC0_XTAL_24M_PWD_SHIFT (30U)

Definition at line 8746 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO

#define CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_MASK)

Definition at line 9176 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_MASK

#define CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 9174 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_SHIFT

#define CCM_ANALOG_MISC1_CLR_IRQ_ANA_BO_SHIFT (30U)

Definition at line 9175 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO

#define CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_MASK)

Definition at line 9179 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_MASK

#define CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 9177 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_SHIFT

#define CCM_ANALOG_MISC1_CLR_IRQ_DIG_BO_SHIFT (31U)

Definition at line 9178 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_MASK)

Definition at line 9173 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_MASK

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 9171 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_SHIFT

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 9172 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_MASK)

Definition at line 9170 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_MASK

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 9168 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_SHIFT

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 9169 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_MASK)

Definition at line 9167 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_MASK

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 9165 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_SHIFT

#define CCM_ANALOG_MISC1_CLR_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 9166 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL

#define CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 9152 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_MASK

#define CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 9132 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_SHIFT

#define CCM_ANALOG_MISC1_CLR_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 9133 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN

#define CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_MASK)

Definition at line 9158 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_MASK

#define CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 9156 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_SHIFT

#define CCM_ANALOG_MISC1_CLR_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 9157 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN

#define CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_MASK)

Definition at line 9155 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_MASK

#define CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 9153 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_SHIFT

#define CCM_ANALOG_MISC1_CLR_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 9154 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN

#define CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK)

Definition at line 9161 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 9159 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 9160 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN

#define CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK)

Definition at line 9164 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 9162 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 9163 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_ANA_BO

#define CCM_ANALOG_MISC1_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_IRQ_ANA_BO_MASK)

Definition at line 9072 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_ANA_BO_MASK

#define CCM_ANALOG_MISC1_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 9070 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_ANA_BO_SHIFT

#define CCM_ANALOG_MISC1_IRQ_ANA_BO_SHIFT (30U)

Definition at line 9071 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_DIG_BO

#define CCM_ANALOG_MISC1_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_IRQ_DIG_BO_MASK)

Definition at line 9075 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_DIG_BO_MASK

#define CCM_ANALOG_MISC1_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 9073 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_DIG_BO_SHIFT

#define CCM_ANALOG_MISC1_IRQ_DIG_BO_SHIFT (31U)

Definition at line 9074 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPHIGH

#define CCM_ANALOG_MISC1_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_IRQ_TEMPHIGH_MASK)

Definition at line 9069 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPHIGH_MASK

#define CCM_ANALOG_MISC1_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 9067 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPHIGH_SHIFT

#define CCM_ANALOG_MISC1_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 9068 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPLOW

#define CCM_ANALOG_MISC1_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_IRQ_TEMPLOW_MASK)

Definition at line 9066 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPLOW_MASK

#define CCM_ANALOG_MISC1_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 9064 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPLOW_SHIFT

#define CCM_ANALOG_MISC1_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 9065 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPPANIC

#define CCM_ANALOG_MISC1_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_IRQ_TEMPPANIC_MASK)

Definition at line 9063 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPPANIC_MASK

#define CCM_ANALOG_MISC1_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 9061 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_IRQ_TEMPPANIC_SHIFT

#define CCM_ANALOG_MISC1_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 9062 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDS1_CLK_SEL

#define CCM_ANALOG_MISC1_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 9048 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDS1_CLK_SEL_MASK

#define CCM_ANALOG_MISC1_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 9028 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDS1_CLK_SEL_SHIFT

#define CCM_ANALOG_MISC1_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 9029 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDSCLK1_IBEN

#define CCM_ANALOG_MISC1_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_LVDSCLK1_IBEN_MASK)

Definition at line 9054 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDSCLK1_IBEN_MASK

#define CCM_ANALOG_MISC1_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 9052 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDSCLK1_IBEN_SHIFT

#define CCM_ANALOG_MISC1_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 9053 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDSCLK1_OBEN

#define CCM_ANALOG_MISC1_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_LVDSCLK1_OBEN_MASK)

Definition at line 9051 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDSCLK1_OBEN_MASK

#define CCM_ANALOG_MISC1_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 9049 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_LVDSCLK1_OBEN_SHIFT

#define CCM_ANALOG_MISC1_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 9050 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN

#define CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_MASK)

Definition at line 9057 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 9055 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 9056 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN

#define CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_MASK)

Definition at line 9060 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 9058 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 9059 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_ANA_BO

#define CCM_ANALOG_MISC1_SET_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_MASK)

Definition at line 9124 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_MASK

#define CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 9122 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_SHIFT

#define CCM_ANALOG_MISC1_SET_IRQ_ANA_BO_SHIFT (30U)

Definition at line 9123 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_DIG_BO

#define CCM_ANALOG_MISC1_SET_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_MASK)

Definition at line 9127 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_MASK

#define CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 9125 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_SHIFT

#define CCM_ANALOG_MISC1_SET_IRQ_DIG_BO_SHIFT (31U)

Definition at line 9126 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_MASK)

Definition at line 9121 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_MASK

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 9119 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_SHIFT

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 9120 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_MASK)

Definition at line 9118 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_MASK

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 9116 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_SHIFT

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 9117 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_MASK)

Definition at line 9115 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_MASK

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 9113 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_SHIFT

#define CCM_ANALOG_MISC1_SET_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 9114 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL

#define CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 9100 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_MASK

#define CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 9080 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_SHIFT

#define CCM_ANALOG_MISC1_SET_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 9081 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN

#define CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_MASK)

Definition at line 9106 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_MASK

#define CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 9104 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_SHIFT

#define CCM_ANALOG_MISC1_SET_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 9105 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN

#define CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_MASK)

Definition at line 9103 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_MASK

#define CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 9101 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_SHIFT

#define CCM_ANALOG_MISC1_SET_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 9102 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN

#define CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_MASK)

Definition at line 9109 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 9107 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 9108 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN

#define CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_MASK)

Definition at line 9112 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 9110 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 9111 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO

#define CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_MASK)

Definition at line 9228 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_MASK

#define CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 9226 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_SHIFT

#define CCM_ANALOG_MISC1_TOG_IRQ_ANA_BO_SHIFT (30U)

Definition at line 9227 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO

#define CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_MASK)

Definition at line 9231 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_MASK

#define CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 9229 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_SHIFT

#define CCM_ANALOG_MISC1_TOG_IRQ_DIG_BO_SHIFT (31U)

Definition at line 9230 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_MASK)

Definition at line 9225 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_MASK

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 9223 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_SHIFT

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 9224 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_MASK)

Definition at line 9222 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_MASK

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 9220 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_SHIFT

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 9221 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_SHIFT)) & CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_MASK)

Definition at line 9219 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_MASK

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 9217 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_SHIFT

#define CCM_ANALOG_MISC1_TOG_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 9218 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL

#define CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_SHIFT)) & CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 9204 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_MASK

#define CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 9184 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_SHIFT

#define CCM_ANALOG_MISC1_TOG_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 9185 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN

#define CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_SHIFT)) & CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_MASK)

Definition at line 9210 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_MASK

#define CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 9208 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_SHIFT

#define CCM_ANALOG_MISC1_TOG_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 9209 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN

#define CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_SHIFT)) & CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_MASK)

Definition at line 9207 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_MASK

#define CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 9205 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_SHIFT

#define CCM_ANALOG_MISC1_TOG_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 9206 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN

#define CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK)

Definition at line 9213 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 9211 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 9212 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN

#define CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT)) & CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK)

Definition at line 9216 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK

#define CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 9214 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT

#define CCM_ANALOG_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 9215 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_AUDIO_DIV_LSB

#define CCM_ANALOG_MISC2_AUDIO_DIV_LSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_AUDIO_DIV_LSB_MASK)

AUDIO_DIV_LSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9287 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_AUDIO_DIV_LSB_MASK

#define CCM_ANALOG_MISC2_AUDIO_DIV_LSB_MASK (0x8000U)

Definition at line 9281 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_AUDIO_DIV_LSB_SHIFT

#define CCM_ANALOG_MISC2_AUDIO_DIV_LSB_SHIFT (15U)

Definition at line 9282 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_AUDIO_DIV_MSB

#define CCM_ANALOG_MISC2_AUDIO_DIV_MSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_AUDIO_DIV_MSB_MASK)

AUDIO_DIV_MSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9310 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_AUDIO_DIV_MSB_MASK

#define CCM_ANALOG_MISC2_AUDIO_DIV_MSB_MASK (0x800000U)

Definition at line 9304 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_AUDIO_DIV_MSB_SHIFT

#define CCM_ANALOG_MISC2_AUDIO_DIV_MSB_SHIFT (23U)

Definition at line 9305 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB

#define CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_MASK)

AUDIO_DIV_LSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9517 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_MASK

#define CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_MASK (0x8000U)

Definition at line 9511 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_SHIFT

#define CCM_ANALOG_MISC2_CLR_AUDIO_DIV_LSB_SHIFT (15U)

Definition at line 9512 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB

#define CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_MASK)

AUDIO_DIV_MSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9540 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_MASK

#define CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_MASK (0x800000U)

Definition at line 9534 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_SHIFT

#define CCM_ANALOG_MISC2_CLR_AUDIO_DIV_MSB_SHIFT (23U)

Definition at line 9535 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_PLL3_DISABLE

#define CCM_ANALOG_MISC2_CLR_PLL3_DISABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_MASK)

PLL3_DISABLE 0b0..PLL3 is being used by peripherals and is enabled when SoC is not in any low power mode 0b1..PLL3 can be disabled when the SoC is not in any low power mode

Definition at line 9491 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_MASK

#define CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_MASK (0x80U)

Definition at line 9485 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_SHIFT

#define CCM_ANALOG_MISC2_CLR_PLL3_DISABLE_SHIFT (7U)

Definition at line 9486 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET

#define CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_MASK)

REG0_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9472 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_MASK (0x7U)

Definition at line 9466 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG0_BO_OFFSET_SHIFT (0U)

Definition at line 9467 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS

#define CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_MASK)

REG0_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9478 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_MASK (0x8U)

Definition at line 9473 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG0_BO_STATUS_SHIFT (3U)

Definition at line 9474 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO

#define CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_MASK)

Definition at line 9481 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_MASK (0x20U)

Definition at line 9479 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG0_ENABLE_BO_SHIFT (5U)

Definition at line 9480 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_OK

#define CCM_ANALOG_MISC2_CLR_REG0_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_OK_MASK)

Definition at line 9484 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_OK_MASK

#define CCM_ANALOG_MISC2_CLR_REG0_OK_MASK (0x40U)

Definition at line 9482 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_OK_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG0_OK_SHIFT (6U)

Definition at line 9483 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME

#define CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_MASK)

REG0_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9549 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_MASK (0x3000000U)

Definition at line 9541 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG0_STEP_TIME_SHIFT (24U)

Definition at line 9542 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET

#define CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_MASK)

REG1_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9498 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_MASK (0x700U)

Definition at line 9492 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG1_BO_OFFSET_SHIFT (8U)

Definition at line 9493 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS

#define CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_MASK)

REG1_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9504 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_MASK (0x800U)

Definition at line 9499 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG1_BO_STATUS_SHIFT (11U)

Definition at line 9500 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO

#define CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_MASK)

Definition at line 9507 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_MASK (0x2000U)

Definition at line 9505 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG1_ENABLE_BO_SHIFT (13U)

Definition at line 9506 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_OK

#define CCM_ANALOG_MISC2_CLR_REG1_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_OK_MASK)

Definition at line 9510 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_OK_MASK

#define CCM_ANALOG_MISC2_CLR_REG1_OK_MASK (0x4000U)

Definition at line 9508 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_OK_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG1_OK_SHIFT (14U)

Definition at line 9509 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME

#define CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_MASK)

REG1_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9558 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_MASK (0xC000000U)

Definition at line 9550 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG1_STEP_TIME_SHIFT (26U)

Definition at line 9551 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET

#define CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_MASK)

REG2_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9524 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_MASK (0x70000U)

Definition at line 9518 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG2_BO_OFFSET_SHIFT (16U)

Definition at line 9519 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS

#define CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_MASK)

Definition at line 9527 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_MASK (0x80000U)

Definition at line 9525 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG2_BO_STATUS_SHIFT (19U)

Definition at line 9526 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO

#define CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_MASK)

Definition at line 9530 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_MASK (0x200000U)

Definition at line 9528 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG2_ENABLE_BO_SHIFT (21U)

Definition at line 9529 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_OK

#define CCM_ANALOG_MISC2_CLR_REG2_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_OK_MASK)

Definition at line 9533 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_OK_MASK

#define CCM_ANALOG_MISC2_CLR_REG2_OK_MASK (0x400000U)

Definition at line 9531 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_OK_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG2_OK_SHIFT (22U)

Definition at line 9532 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME

#define CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_MASK)

REG2_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9567 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_MASK (0x30000000U)

Definition at line 9559 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_CLR_REG2_STEP_TIME_SHIFT (28U)

Definition at line 9560 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_VIDEO_DIV

#define CCM_ANALOG_MISC2_CLR_VIDEO_DIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_CLR_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_CLR_VIDEO_DIV_MASK)

VIDEO_DIV 0b00..divide by 1 (Default) 0b01..divide by 2 0b10..divide by 1 0b11..divide by 4

Definition at line 9576 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_VIDEO_DIV_MASK

#define CCM_ANALOG_MISC2_CLR_VIDEO_DIV_MASK (0xC0000000U)

Definition at line 9568 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_CLR_VIDEO_DIV_SHIFT

#define CCM_ANALOG_MISC2_CLR_VIDEO_DIV_SHIFT (30U)

Definition at line 9569 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_PLL3_DISABLE

#define CCM_ANALOG_MISC2_PLL3_DISABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_PLL3_DISABLE_MASK)

PLL3_DISABLE 0b0..PLL3 is being used by peripherals and is enabled when SoC is not in any low power mode 0b1..PLL3 can be disabled when the SoC is not in any low power mode

Definition at line 9261 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_PLL3_DISABLE_MASK

#define CCM_ANALOG_MISC2_PLL3_DISABLE_MASK (0x80U)

Definition at line 9255 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_PLL3_DISABLE_SHIFT

#define CCM_ANALOG_MISC2_PLL3_DISABLE_SHIFT (7U)

Definition at line 9256 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_BO_OFFSET

#define CCM_ANALOG_MISC2_REG0_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_REG0_BO_OFFSET_MASK)

REG0_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9242 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_REG0_BO_OFFSET_MASK (0x7U)

Definition at line 9236 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_REG0_BO_OFFSET_SHIFT (0U)

Definition at line 9237 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_BO_STATUS

#define CCM_ANALOG_MISC2_REG0_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_REG0_BO_STATUS_MASK)

REG0_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9248 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_REG0_BO_STATUS_MASK (0x8U)

Definition at line 9243 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_REG0_BO_STATUS_SHIFT (3U)

Definition at line 9244 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_ENABLE_BO

#define CCM_ANALOG_MISC2_REG0_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_REG0_ENABLE_BO_MASK)

Definition at line 9251 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_REG0_ENABLE_BO_MASK (0x20U)

Definition at line 9249 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_REG0_ENABLE_BO_SHIFT (5U)

Definition at line 9250 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_OK

#define CCM_ANALOG_MISC2_REG0_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_REG0_OK_MASK)

Definition at line 9254 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_OK_MASK

#define CCM_ANALOG_MISC2_REG0_OK_MASK (0x40U)

Definition at line 9252 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_OK_SHIFT

#define CCM_ANALOG_MISC2_REG0_OK_SHIFT (6U)

Definition at line 9253 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_STEP_TIME

#define CCM_ANALOG_MISC2_REG0_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_REG0_STEP_TIME_MASK)

REG0_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9319 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_REG0_STEP_TIME_MASK (0x3000000U)

Definition at line 9311 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG0_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_REG0_STEP_TIME_SHIFT (24U)

Definition at line 9312 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_BO_OFFSET

#define CCM_ANALOG_MISC2_REG1_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_REG1_BO_OFFSET_MASK)

REG1_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9268 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_REG1_BO_OFFSET_MASK (0x700U)

Definition at line 9262 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_REG1_BO_OFFSET_SHIFT (8U)

Definition at line 9263 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_BO_STATUS

#define CCM_ANALOG_MISC2_REG1_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_REG1_BO_STATUS_MASK)

REG1_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9274 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_REG1_BO_STATUS_MASK (0x800U)

Definition at line 9269 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_REG1_BO_STATUS_SHIFT (11U)

Definition at line 9270 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_ENABLE_BO

#define CCM_ANALOG_MISC2_REG1_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_REG1_ENABLE_BO_MASK)

Definition at line 9277 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_REG1_ENABLE_BO_MASK (0x2000U)

Definition at line 9275 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_REG1_ENABLE_BO_SHIFT (13U)

Definition at line 9276 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_OK

#define CCM_ANALOG_MISC2_REG1_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_REG1_OK_MASK)

Definition at line 9280 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_OK_MASK

#define CCM_ANALOG_MISC2_REG1_OK_MASK (0x4000U)

Definition at line 9278 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_OK_SHIFT

#define CCM_ANALOG_MISC2_REG1_OK_SHIFT (14U)

Definition at line 9279 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_STEP_TIME

#define CCM_ANALOG_MISC2_REG1_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_REG1_STEP_TIME_MASK)

REG1_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9328 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_REG1_STEP_TIME_MASK (0xC000000U)

Definition at line 9320 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG1_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_REG1_STEP_TIME_SHIFT (26U)

Definition at line 9321 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_BO_OFFSET

#define CCM_ANALOG_MISC2_REG2_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_REG2_BO_OFFSET_MASK)

REG2_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9294 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_REG2_BO_OFFSET_MASK (0x70000U)

Definition at line 9288 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_REG2_BO_OFFSET_SHIFT (16U)

Definition at line 9289 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_BO_STATUS

#define CCM_ANALOG_MISC2_REG2_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_REG2_BO_STATUS_MASK)

Definition at line 9297 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_REG2_BO_STATUS_MASK (0x80000U)

Definition at line 9295 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_REG2_BO_STATUS_SHIFT (19U)

Definition at line 9296 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_ENABLE_BO

#define CCM_ANALOG_MISC2_REG2_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_REG2_ENABLE_BO_MASK)

Definition at line 9300 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_REG2_ENABLE_BO_MASK (0x200000U)

Definition at line 9298 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_REG2_ENABLE_BO_SHIFT (21U)

Definition at line 9299 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_OK

#define CCM_ANALOG_MISC2_REG2_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_REG2_OK_MASK)

Definition at line 9303 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_OK_MASK

#define CCM_ANALOG_MISC2_REG2_OK_MASK (0x400000U)

Definition at line 9301 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_OK_SHIFT

#define CCM_ANALOG_MISC2_REG2_OK_SHIFT (22U)

Definition at line 9302 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_STEP_TIME

#define CCM_ANALOG_MISC2_REG2_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_REG2_STEP_TIME_MASK)

REG2_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9337 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_REG2_STEP_TIME_MASK (0x30000000U)

Definition at line 9329 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_REG2_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_REG2_STEP_TIME_SHIFT (28U)

Definition at line 9330 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB

#define CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_MASK)

AUDIO_DIV_LSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9402 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_MASK

#define CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_MASK (0x8000U)

Definition at line 9396 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_SHIFT

#define CCM_ANALOG_MISC2_SET_AUDIO_DIV_LSB_SHIFT (15U)

Definition at line 9397 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB

#define CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_MASK)

AUDIO_DIV_MSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9425 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_MASK

#define CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_MASK (0x800000U)

Definition at line 9419 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_SHIFT

#define CCM_ANALOG_MISC2_SET_AUDIO_DIV_MSB_SHIFT (23U)

Definition at line 9420 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_PLL3_DISABLE

#define CCM_ANALOG_MISC2_SET_PLL3_DISABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_SET_PLL3_DISABLE_MASK)

PLL3_DISABLE 0b0..PLL3 is being used by peripherals and is enabled when SoC is not in any low power mode 0b1..PLL3 can be disabled when the SoC is not in any low power mode

Definition at line 9376 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_PLL3_DISABLE_MASK

#define CCM_ANALOG_MISC2_SET_PLL3_DISABLE_MASK (0x80U)

Definition at line 9370 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_PLL3_DISABLE_SHIFT

#define CCM_ANALOG_MISC2_SET_PLL3_DISABLE_SHIFT (7U)

Definition at line 9371 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET

#define CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_MASK)

REG0_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9357 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_MASK (0x7U)

Definition at line 9351 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_SET_REG0_BO_OFFSET_SHIFT (0U)

Definition at line 9352 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_BO_STATUS

#define CCM_ANALOG_MISC2_SET_REG0_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_MASK)

REG0_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9363 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_MASK (0x8U)

Definition at line 9358 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_SET_REG0_BO_STATUS_SHIFT (3U)

Definition at line 9359 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO

#define CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_MASK)

Definition at line 9366 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_MASK (0x20U)

Definition at line 9364 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_SET_REG0_ENABLE_BO_SHIFT (5U)

Definition at line 9365 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_OK

#define CCM_ANALOG_MISC2_SET_REG0_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_OK_MASK)

Definition at line 9369 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_OK_MASK

#define CCM_ANALOG_MISC2_SET_REG0_OK_MASK (0x40U)

Definition at line 9367 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_OK_SHIFT

#define CCM_ANALOG_MISC2_SET_REG0_OK_SHIFT (6U)

Definition at line 9368 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_STEP_TIME

#define CCM_ANALOG_MISC2_SET_REG0_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_MASK)

REG0_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9434 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_MASK (0x3000000U)

Definition at line 9426 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_SET_REG0_STEP_TIME_SHIFT (24U)

Definition at line 9427 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET

#define CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_MASK)

REG1_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9383 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_MASK (0x700U)

Definition at line 9377 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_SET_REG1_BO_OFFSET_SHIFT (8U)

Definition at line 9378 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_BO_STATUS

#define CCM_ANALOG_MISC2_SET_REG1_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_MASK)

REG1_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9389 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_MASK (0x800U)

Definition at line 9384 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_SET_REG1_BO_STATUS_SHIFT (11U)

Definition at line 9385 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO

#define CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_MASK)

Definition at line 9392 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_MASK (0x2000U)

Definition at line 9390 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_SET_REG1_ENABLE_BO_SHIFT (13U)

Definition at line 9391 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_OK

#define CCM_ANALOG_MISC2_SET_REG1_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_OK_MASK)

Definition at line 9395 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_OK_MASK

#define CCM_ANALOG_MISC2_SET_REG1_OK_MASK (0x4000U)

Definition at line 9393 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_OK_SHIFT

#define CCM_ANALOG_MISC2_SET_REG1_OK_SHIFT (14U)

Definition at line 9394 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_STEP_TIME

#define CCM_ANALOG_MISC2_SET_REG1_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_MASK)

REG1_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9443 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_MASK (0xC000000U)

Definition at line 9435 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_SET_REG1_STEP_TIME_SHIFT (26U)

Definition at line 9436 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET

#define CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_MASK)

REG2_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9409 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_MASK (0x70000U)

Definition at line 9403 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_SET_REG2_BO_OFFSET_SHIFT (16U)

Definition at line 9404 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_BO_STATUS

#define CCM_ANALOG_MISC2_SET_REG2_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_MASK)

Definition at line 9412 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_MASK (0x80000U)

Definition at line 9410 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_SET_REG2_BO_STATUS_SHIFT (19U)

Definition at line 9411 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO

#define CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_MASK)

Definition at line 9415 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_MASK (0x200000U)

Definition at line 9413 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_SET_REG2_ENABLE_BO_SHIFT (21U)

Definition at line 9414 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_OK

#define CCM_ANALOG_MISC2_SET_REG2_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_OK_MASK)

Definition at line 9418 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_OK_MASK

#define CCM_ANALOG_MISC2_SET_REG2_OK_MASK (0x400000U)

Definition at line 9416 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_OK_SHIFT

#define CCM_ANALOG_MISC2_SET_REG2_OK_SHIFT (22U)

Definition at line 9417 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_STEP_TIME

#define CCM_ANALOG_MISC2_SET_REG2_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_MASK)

REG2_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9452 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_MASK (0x30000000U)

Definition at line 9444 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_SET_REG2_STEP_TIME_SHIFT (28U)

Definition at line 9445 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_VIDEO_DIV

#define CCM_ANALOG_MISC2_SET_VIDEO_DIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_SET_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_SET_VIDEO_DIV_MASK)

VIDEO_DIV 0b00..divide by 1 (Default) 0b01..divide by 2 0b10..divide by 1 0b11..divide by 4

Definition at line 9461 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_VIDEO_DIV_MASK

#define CCM_ANALOG_MISC2_SET_VIDEO_DIV_MASK (0xC0000000U)

Definition at line 9453 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_SET_VIDEO_DIV_SHIFT

#define CCM_ANALOG_MISC2_SET_VIDEO_DIV_SHIFT (30U)

Definition at line 9454 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB

#define CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_SHIFT)) & CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_MASK)

AUDIO_DIV_LSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9632 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_MASK

#define CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_MASK (0x8000U)

Definition at line 9626 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_SHIFT

#define CCM_ANALOG_MISC2_TOG_AUDIO_DIV_LSB_SHIFT (15U)

Definition at line 9627 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB

#define CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_SHIFT)) & CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_MASK)

AUDIO_DIV_MSB 0b0..divide by 1 (Default) 0b1..divide by 2

Definition at line 9655 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_MASK

#define CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_MASK (0x800000U)

Definition at line 9649 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_SHIFT

#define CCM_ANALOG_MISC2_TOG_AUDIO_DIV_MSB_SHIFT (23U)

Definition at line 9650 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_PLL3_DISABLE

#define CCM_ANALOG_MISC2_TOG_PLL3_DISABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_SHIFT)) & CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_MASK)

PLL3_DISABLE 0b0..PLL3 is being used by peripherals and is enabled when SoC is not in any low power mode 0b1..PLL3 can be disabled when the SoC is not in any low power mode

Definition at line 9606 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_MASK

#define CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_MASK (0x80U)

Definition at line 9600 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_SHIFT

#define CCM_ANALOG_MISC2_TOG_PLL3_DISABLE_SHIFT (7U)

Definition at line 9601 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET

#define CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_MASK)

REG0_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9587 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_MASK (0x7U)

Definition at line 9581 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG0_BO_OFFSET_SHIFT (0U)

Definition at line 9582 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS

#define CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_MASK)

REG0_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9593 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_MASK (0x8U)

Definition at line 9588 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG0_BO_STATUS_SHIFT (3U)

Definition at line 9589 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO

#define CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_MASK)

Definition at line 9596 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_MASK (0x20U)

Definition at line 9594 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG0_ENABLE_BO_SHIFT (5U)

Definition at line 9595 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_OK

#define CCM_ANALOG_MISC2_TOG_REG0_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_OK_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_OK_MASK)

Definition at line 9599 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_OK_MASK

#define CCM_ANALOG_MISC2_TOG_REG0_OK_MASK (0x40U)

Definition at line 9597 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_OK_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG0_OK_SHIFT (6U)

Definition at line 9598 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME

#define CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_MASK)

REG0_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9664 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_MASK (0x3000000U)

Definition at line 9656 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG0_STEP_TIME_SHIFT (24U)

Definition at line 9657 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET

#define CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_MASK)

REG1_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9613 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_MASK (0x700U)

Definition at line 9607 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG1_BO_OFFSET_SHIFT (8U)

Definition at line 9608 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS

#define CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_MASK)

REG1_BO_STATUS 0b1..Brownout, supply is below target minus brownout offset.

Definition at line 9619 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_MASK (0x800U)

Definition at line 9614 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG1_BO_STATUS_SHIFT (11U)

Definition at line 9615 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO

#define CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_MASK)

Definition at line 9622 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_MASK (0x2000U)

Definition at line 9620 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG1_ENABLE_BO_SHIFT (13U)

Definition at line 9621 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_OK

#define CCM_ANALOG_MISC2_TOG_REG1_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_OK_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_OK_MASK)

Definition at line 9625 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_OK_MASK

#define CCM_ANALOG_MISC2_TOG_REG1_OK_MASK (0x4000U)

Definition at line 9623 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_OK_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG1_OK_SHIFT (14U)

Definition at line 9624 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME

#define CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_MASK)

REG1_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9673 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_MASK (0xC000000U)

Definition at line 9665 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG1_STEP_TIME_SHIFT (26U)

Definition at line 9666 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET

#define CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_MASK)

REG2_BO_OFFSET 0b100..Brownout offset = 0.100V 0b111..Brownout offset = 0.175V

Definition at line 9639 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_MASK

#define CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_MASK (0x70000U)

Definition at line 9633 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG2_BO_OFFSET_SHIFT (16U)

Definition at line 9634 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS

#define CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_MASK)

Definition at line 9642 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_MASK

#define CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_MASK (0x80000U)

Definition at line 9640 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG2_BO_STATUS_SHIFT (19U)

Definition at line 9641 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO

#define CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_MASK)

Definition at line 9645 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_MASK

#define CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_MASK (0x200000U)

Definition at line 9643 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG2_ENABLE_BO_SHIFT (21U)

Definition at line 9644 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_OK

#define CCM_ANALOG_MISC2_TOG_REG2_OK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_OK_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_OK_MASK)

Definition at line 9648 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_OK_MASK

#define CCM_ANALOG_MISC2_TOG_REG2_OK_MASK (0x400000U)

Definition at line 9646 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_OK_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG2_OK_SHIFT (22U)

Definition at line 9647 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME

#define CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_SHIFT)) & CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_MASK)

REG2_STEP_TIME 0b00..64 0b01..128 0b10..256 0b11..512

Definition at line 9682 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_MASK

#define CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_MASK (0x30000000U)

Definition at line 9674 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_SHIFT

#define CCM_ANALOG_MISC2_TOG_REG2_STEP_TIME_SHIFT (28U)

Definition at line 9675 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_VIDEO_DIV

#define CCM_ANALOG_MISC2_TOG_VIDEO_DIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_TOG_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_TOG_VIDEO_DIV_MASK)

VIDEO_DIV 0b00..divide by 1 (Default) 0b01..divide by 2 0b10..divide by 1 0b11..divide by 4

Definition at line 9691 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_VIDEO_DIV_MASK

#define CCM_ANALOG_MISC2_TOG_VIDEO_DIV_MASK (0xC0000000U)

Definition at line 9683 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_TOG_VIDEO_DIV_SHIFT

#define CCM_ANALOG_MISC2_TOG_VIDEO_DIV_SHIFT (30U)

Definition at line 9684 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_VIDEO_DIV

#define CCM_ANALOG_MISC2_VIDEO_DIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_MISC2_VIDEO_DIV_SHIFT)) & CCM_ANALOG_MISC2_VIDEO_DIV_MASK)

VIDEO_DIV 0b00..divide by 1 (Default) 0b01..divide by 2 0b10..divide by 1 0b11..divide by 4

Definition at line 9346 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_VIDEO_DIV_MASK

#define CCM_ANALOG_MISC2_VIDEO_DIV_MASK (0xC0000000U)

Definition at line 9338 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_MISC2_VIDEO_DIV_SHIFT

#define CCM_ANALOG_MISC2_VIDEO_DIV_SHIFT (30U)

Definition at line 9339 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE

#define CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_MASK)

Definition at line 8428 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8426 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8427 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_FRAC

#define CCM_ANALOG_PFD_480_CLR_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_MASK)

Definition at line 8422 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_MASK (0x3FU)

Definition at line 8420 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD0_FRAC_SHIFT (0U)

Definition at line 8421 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_STABLE

#define CCM_ANALOG_PFD_480_CLR_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_MASK)

Definition at line 8425 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_MASK (0x40U)

Definition at line 8423 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD0_STABLE_SHIFT (6U)

Definition at line 8424 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE

#define CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_MASK)

Definition at line 8437 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8435 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8436 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_FRAC

#define CCM_ANALOG_PFD_480_CLR_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_MASK)

Definition at line 8431 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8429 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD1_FRAC_SHIFT (8U)

Definition at line 8430 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_STABLE

#define CCM_ANALOG_PFD_480_CLR_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_MASK)

Definition at line 8434 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_MASK (0x4000U)

Definition at line 8432 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD1_STABLE_SHIFT (14U)

Definition at line 8433 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE

#define CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_MASK)

Definition at line 8446 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8444 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8445 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_FRAC

#define CCM_ANALOG_PFD_480_CLR_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_MASK)

Definition at line 8440 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8438 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD2_FRAC_SHIFT (16U)

Definition at line 8439 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_STABLE

#define CCM_ANALOG_PFD_480_CLR_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_MASK)

Definition at line 8443 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_MASK (0x400000U)

Definition at line 8441 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD2_STABLE_SHIFT (22U)

Definition at line 8442 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE

#define CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_MASK)

Definition at line 8455 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8453 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8454 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_FRAC

#define CCM_ANALOG_PFD_480_CLR_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_MASK)

Definition at line 8449 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8447 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD3_FRAC_SHIFT (24U)

Definition at line 8448 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_STABLE

#define CCM_ANALOG_PFD_480_CLR_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_MASK)

Definition at line 8452 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8450 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_CLR_PFD3_STABLE_SHIFT (30U)

Definition at line 8451 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_CLKGATE

#define CCM_ANALOG_PFD_480_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD0_CLKGATE_MASK)

Definition at line 8348 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8346 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8347 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_FRAC

#define CCM_ANALOG_PFD_480_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD0_FRAC_MASK)

Definition at line 8342 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_480_PFD0_FRAC_MASK (0x3FU)

Definition at line 8340 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_PFD0_FRAC_SHIFT (0U)

Definition at line 8341 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_STABLE

#define CCM_ANALOG_PFD_480_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD0_STABLE_MASK)

Definition at line 8345 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_480_PFD0_STABLE_MASK (0x40U)

Definition at line 8343 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_PFD0_STABLE_SHIFT (6U)

Definition at line 8344 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_CLKGATE

#define CCM_ANALOG_PFD_480_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD1_CLKGATE_MASK)

Definition at line 8357 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8355 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8356 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_FRAC

#define CCM_ANALOG_PFD_480_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD1_FRAC_MASK)

Definition at line 8351 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_480_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8349 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_PFD1_FRAC_SHIFT (8U)

Definition at line 8350 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_STABLE

#define CCM_ANALOG_PFD_480_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD1_STABLE_MASK)

Definition at line 8354 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_480_PFD1_STABLE_MASK (0x4000U)

Definition at line 8352 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_PFD1_STABLE_SHIFT (14U)

Definition at line 8353 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_CLKGATE

#define CCM_ANALOG_PFD_480_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD2_CLKGATE_MASK)

Definition at line 8366 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8364 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8365 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_FRAC

#define CCM_ANALOG_PFD_480_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD2_FRAC_MASK)

Definition at line 8360 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_480_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8358 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_PFD2_FRAC_SHIFT (16U)

Definition at line 8359 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_STABLE

#define CCM_ANALOG_PFD_480_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD2_STABLE_MASK)

Definition at line 8363 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_480_PFD2_STABLE_MASK (0x400000U)

Definition at line 8361 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_PFD2_STABLE_SHIFT (22U)

Definition at line 8362 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_CLKGATE

#define CCM_ANALOG_PFD_480_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_PFD3_CLKGATE_MASK)

Definition at line 8375 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8373 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8374 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_FRAC

#define CCM_ANALOG_PFD_480_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_PFD3_FRAC_MASK)

Definition at line 8369 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_480_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8367 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_PFD3_FRAC_SHIFT (24U)

Definition at line 8368 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_STABLE

#define CCM_ANALOG_PFD_480_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_PFD3_STABLE_MASK)

Definition at line 8372 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_480_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8370 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_PFD3_STABLE_SHIFT (30U)

Definition at line 8371 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE

#define CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_MASK)

Definition at line 8388 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8386 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8387 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_FRAC

#define CCM_ANALOG_PFD_480_SET_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD0_FRAC_MASK)

Definition at line 8382 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_480_SET_PFD0_FRAC_MASK (0x3FU)

Definition at line 8380 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD0_FRAC_SHIFT (0U)

Definition at line 8381 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_STABLE

#define CCM_ANALOG_PFD_480_SET_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD0_STABLE_MASK)

Definition at line 8385 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD0_STABLE_MASK (0x40U)

Definition at line 8383 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD0_STABLE_SHIFT (6U)

Definition at line 8384 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE

#define CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_MASK)

Definition at line 8397 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8395 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8396 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_FRAC

#define CCM_ANALOG_PFD_480_SET_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD1_FRAC_MASK)

Definition at line 8391 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_480_SET_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8389 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD1_FRAC_SHIFT (8U)

Definition at line 8390 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_STABLE

#define CCM_ANALOG_PFD_480_SET_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD1_STABLE_MASK)

Definition at line 8394 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD1_STABLE_MASK (0x4000U)

Definition at line 8392 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD1_STABLE_SHIFT (14U)

Definition at line 8393 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE

#define CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_MASK)

Definition at line 8406 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8404 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8405 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_FRAC

#define CCM_ANALOG_PFD_480_SET_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD2_FRAC_MASK)

Definition at line 8400 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_480_SET_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8398 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD2_FRAC_SHIFT (16U)

Definition at line 8399 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_STABLE

#define CCM_ANALOG_PFD_480_SET_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD2_STABLE_MASK)

Definition at line 8403 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD2_STABLE_MASK (0x400000U)

Definition at line 8401 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD2_STABLE_SHIFT (22U)

Definition at line 8402 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE

#define CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_MASK)

Definition at line 8415 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8413 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8414 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_FRAC

#define CCM_ANALOG_PFD_480_SET_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD3_FRAC_MASK)

Definition at line 8409 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_480_SET_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8407 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD3_FRAC_SHIFT (24U)

Definition at line 8408 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_STABLE

#define CCM_ANALOG_PFD_480_SET_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_SET_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_SET_PFD3_STABLE_MASK)

Definition at line 8412 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_480_SET_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8410 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_SET_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_SET_PFD3_STABLE_SHIFT (30U)

Definition at line 8411 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE

#define CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_MASK)

Definition at line 8468 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8466 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8467 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_FRAC

#define CCM_ANALOG_PFD_480_TOG_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_MASK)

Definition at line 8462 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_MASK (0x3FU)

Definition at line 8460 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD0_FRAC_SHIFT (0U)

Definition at line 8461 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_STABLE

#define CCM_ANALOG_PFD_480_TOG_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_MASK)

Definition at line 8465 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_MASK (0x40U)

Definition at line 8463 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD0_STABLE_SHIFT (6U)

Definition at line 8464 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE

#define CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_MASK)

Definition at line 8477 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8475 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8476 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_FRAC

#define CCM_ANALOG_PFD_480_TOG_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_MASK)

Definition at line 8471 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8469 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD1_FRAC_SHIFT (8U)

Definition at line 8470 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_STABLE

#define CCM_ANALOG_PFD_480_TOG_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_MASK)

Definition at line 8474 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_MASK (0x4000U)

Definition at line 8472 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD1_STABLE_SHIFT (14U)

Definition at line 8473 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE

#define CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_MASK)

Definition at line 8486 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8484 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8485 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_FRAC

#define CCM_ANALOG_PFD_480_TOG_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_MASK)

Definition at line 8480 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8478 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD2_FRAC_SHIFT (16U)

Definition at line 8479 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_STABLE

#define CCM_ANALOG_PFD_480_TOG_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_MASK)

Definition at line 8483 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_MASK (0x400000U)

Definition at line 8481 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD2_STABLE_SHIFT (22U)

Definition at line 8482 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE

#define CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_MASK)

Definition at line 8495 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8493 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8494 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_FRAC

#define CCM_ANALOG_PFD_480_TOG_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_MASK)

Definition at line 8489 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8487 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD3_FRAC_SHIFT (24U)

Definition at line 8488 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_STABLE

#define CCM_ANALOG_PFD_480_TOG_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_MASK)

Definition at line 8492 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8490 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_480_TOG_PFD3_STABLE_SHIFT (30U)

Definition at line 8491 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE

#define CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_MASK)

Definition at line 8588 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8586 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8587 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_FRAC

#define CCM_ANALOG_PFD_528_CLR_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_MASK)

Definition at line 8582 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_MASK (0x3FU)

Definition at line 8580 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD0_FRAC_SHIFT (0U)

Definition at line 8581 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_STABLE

#define CCM_ANALOG_PFD_528_CLR_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_MASK)

Definition at line 8585 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_MASK (0x40U)

Definition at line 8583 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD0_STABLE_SHIFT (6U)

Definition at line 8584 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE

#define CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_MASK)

Definition at line 8597 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8595 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8596 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_FRAC

#define CCM_ANALOG_PFD_528_CLR_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_MASK)

Definition at line 8591 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8589 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD1_FRAC_SHIFT (8U)

Definition at line 8590 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_STABLE

#define CCM_ANALOG_PFD_528_CLR_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_MASK)

Definition at line 8594 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_MASK (0x4000U)

Definition at line 8592 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD1_STABLE_SHIFT (14U)

Definition at line 8593 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE

#define CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_MASK)

Definition at line 8606 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8604 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8605 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_FRAC

#define CCM_ANALOG_PFD_528_CLR_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_MASK)

Definition at line 8600 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8598 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD2_FRAC_SHIFT (16U)

Definition at line 8599 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_STABLE

#define CCM_ANALOG_PFD_528_CLR_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_MASK)

Definition at line 8603 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_MASK (0x400000U)

Definition at line 8601 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD2_STABLE_SHIFT (22U)

Definition at line 8602 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE

#define CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_MASK)

Definition at line 8615 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8613 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8614 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_FRAC

#define CCM_ANALOG_PFD_528_CLR_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_MASK)

Definition at line 8609 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8607 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD3_FRAC_SHIFT (24U)

Definition at line 8608 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_STABLE

#define CCM_ANALOG_PFD_528_CLR_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_MASK)

Definition at line 8612 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8610 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_CLR_PFD3_STABLE_SHIFT (30U)

Definition at line 8611 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_CLKGATE

#define CCM_ANALOG_PFD_528_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD0_CLKGATE_MASK)

Definition at line 8508 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8506 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8507 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_FRAC

#define CCM_ANALOG_PFD_528_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD0_FRAC_MASK)

Definition at line 8502 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_528_PFD0_FRAC_MASK (0x3FU)

Definition at line 8500 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_PFD0_FRAC_SHIFT (0U)

Definition at line 8501 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_STABLE

#define CCM_ANALOG_PFD_528_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD0_STABLE_MASK)

Definition at line 8505 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_528_PFD0_STABLE_MASK (0x40U)

Definition at line 8503 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_PFD0_STABLE_SHIFT (6U)

Definition at line 8504 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_CLKGATE

#define CCM_ANALOG_PFD_528_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD1_CLKGATE_MASK)

Definition at line 8517 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8515 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8516 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_FRAC

#define CCM_ANALOG_PFD_528_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD1_FRAC_MASK)

Definition at line 8511 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_528_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8509 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_PFD1_FRAC_SHIFT (8U)

Definition at line 8510 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_STABLE

#define CCM_ANALOG_PFD_528_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD1_STABLE_MASK)

Definition at line 8514 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_528_PFD1_STABLE_MASK (0x4000U)

Definition at line 8512 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_PFD1_STABLE_SHIFT (14U)

Definition at line 8513 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_CLKGATE

#define CCM_ANALOG_PFD_528_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD2_CLKGATE_MASK)

Definition at line 8526 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8524 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8525 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_FRAC

#define CCM_ANALOG_PFD_528_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD2_FRAC_MASK)

Definition at line 8520 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_528_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8518 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_PFD2_FRAC_SHIFT (16U)

Definition at line 8519 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_STABLE

#define CCM_ANALOG_PFD_528_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD2_STABLE_MASK)

Definition at line 8523 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_528_PFD2_STABLE_MASK (0x400000U)

Definition at line 8521 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_PFD2_STABLE_SHIFT (22U)

Definition at line 8522 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_CLKGATE

#define CCM_ANALOG_PFD_528_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_PFD3_CLKGATE_MASK)

Definition at line 8535 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8533 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8534 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_FRAC

#define CCM_ANALOG_PFD_528_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_PFD3_FRAC_MASK)

Definition at line 8529 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_528_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8527 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_PFD3_FRAC_SHIFT (24U)

Definition at line 8528 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_STABLE

#define CCM_ANALOG_PFD_528_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_PFD3_STABLE_MASK)

Definition at line 8532 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_528_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8530 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_PFD3_STABLE_SHIFT (30U)

Definition at line 8531 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE

#define CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_MASK)

Definition at line 8548 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8546 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8547 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_FRAC

#define CCM_ANALOG_PFD_528_SET_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD0_FRAC_MASK)

Definition at line 8542 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_528_SET_PFD0_FRAC_MASK (0x3FU)

Definition at line 8540 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD0_FRAC_SHIFT (0U)

Definition at line 8541 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_STABLE

#define CCM_ANALOG_PFD_528_SET_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD0_STABLE_MASK)

Definition at line 8545 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD0_STABLE_MASK (0x40U)

Definition at line 8543 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD0_STABLE_SHIFT (6U)

Definition at line 8544 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE

#define CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_MASK)

Definition at line 8557 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8555 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8556 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_FRAC

#define CCM_ANALOG_PFD_528_SET_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD1_FRAC_MASK)

Definition at line 8551 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_528_SET_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8549 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD1_FRAC_SHIFT (8U)

Definition at line 8550 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_STABLE

#define CCM_ANALOG_PFD_528_SET_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD1_STABLE_MASK)

Definition at line 8554 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD1_STABLE_MASK (0x4000U)

Definition at line 8552 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD1_STABLE_SHIFT (14U)

Definition at line 8553 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE

#define CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_MASK)

Definition at line 8566 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8564 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8565 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_FRAC

#define CCM_ANALOG_PFD_528_SET_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD2_FRAC_MASK)

Definition at line 8560 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_528_SET_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8558 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD2_FRAC_SHIFT (16U)

Definition at line 8559 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_STABLE

#define CCM_ANALOG_PFD_528_SET_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD2_STABLE_MASK)

Definition at line 8563 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD2_STABLE_MASK (0x400000U)

Definition at line 8561 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD2_STABLE_SHIFT (22U)

Definition at line 8562 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE

#define CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_MASK)

Definition at line 8575 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8573 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8574 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_FRAC

#define CCM_ANALOG_PFD_528_SET_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD3_FRAC_MASK)

Definition at line 8569 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_528_SET_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8567 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD3_FRAC_SHIFT (24U)

Definition at line 8568 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_STABLE

#define CCM_ANALOG_PFD_528_SET_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_SET_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_SET_PFD3_STABLE_MASK)

Definition at line 8572 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_528_SET_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8570 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_SET_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_SET_PFD3_STABLE_SHIFT (30U)

Definition at line 8571 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE

#define CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_MASK)

Definition at line 8628 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_MASK (0x80U)

Definition at line 8626 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD0_CLKGATE_SHIFT (7U)

Definition at line 8627 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_FRAC

#define CCM_ANALOG_PFD_528_TOG_PFD0_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_MASK)

Definition at line 8622 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_MASK (0x3FU)

Definition at line 8620 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD0_FRAC_SHIFT (0U)

Definition at line 8621 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_STABLE

#define CCM_ANALOG_PFD_528_TOG_PFD0_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_MASK)

Definition at line 8625 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_MASK (0x40U)

Definition at line 8623 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD0_STABLE_SHIFT (6U)

Definition at line 8624 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE

#define CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_MASK)

Definition at line 8637 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_MASK (0x8000U)

Definition at line 8635 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD1_CLKGATE_SHIFT (15U)

Definition at line 8636 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_FRAC

#define CCM_ANALOG_PFD_528_TOG_PFD1_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_MASK)

Definition at line 8631 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_MASK (0x3F00U)

Definition at line 8629 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD1_FRAC_SHIFT (8U)

Definition at line 8630 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_STABLE

#define CCM_ANALOG_PFD_528_TOG_PFD1_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_MASK)

Definition at line 8634 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_MASK (0x4000U)

Definition at line 8632 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD1_STABLE_SHIFT (14U)

Definition at line 8633 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE

#define CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_MASK)

Definition at line 8646 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_MASK (0x800000U)

Definition at line 8644 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD2_CLKGATE_SHIFT (23U)

Definition at line 8645 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_FRAC

#define CCM_ANALOG_PFD_528_TOG_PFD2_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_MASK)

Definition at line 8640 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_MASK (0x3F0000U)

Definition at line 8638 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD2_FRAC_SHIFT (16U)

Definition at line 8639 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_STABLE

#define CCM_ANALOG_PFD_528_TOG_PFD2_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_MASK)

Definition at line 8643 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_MASK (0x400000U)

Definition at line 8641 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD2_STABLE_SHIFT (22U)

Definition at line 8642 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE

#define CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_MASK)

Definition at line 8655 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_MASK (0x80000000U)

Definition at line 8653 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD3_CLKGATE_SHIFT (31U)

Definition at line 8654 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_FRAC

#define CCM_ANALOG_PFD_528_TOG_PFD3_FRAC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_MASK)

Definition at line 8649 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_MASK (0x3F000000U)

Definition at line 8647 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD3_FRAC_SHIFT (24U)

Definition at line 8648 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_STABLE

#define CCM_ANALOG_PFD_528_TOG_PFD3_STABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_SHIFT)) & CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_MASK)

Definition at line 8652 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_MASK

#define CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_MASK (0x40000000U)

Definition at line 8650 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_SHIFT

#define CCM_ANALOG_PFD_528_TOG_PFD3_STABLE_SHIFT (30U)

Definition at line 8651 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_BYPASS

#define CCM_ANALOG_PLL_ARM_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_BYPASS_MASK)

Definition at line 7349 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7346 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7338 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ARM_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7339 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_BYPASS_MASK

#define CCM_ANALOG_PLL_ARM_BYPASS_MASK (0x10000U)

Definition at line 7347 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ARM_BYPASS_SHIFT (16U)

Definition at line 7348 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_BYPASS

#define CCM_ANALOG_PLL_ARM_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_BYPASS_MASK)

Definition at line 7411 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7408 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7400 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ARM_CLR_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7401 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_BYPASS_MASK

#define CCM_ANALOG_PLL_ARM_CLR_BYPASS_MASK (0x10000U)

Definition at line 7409 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ARM_CLR_BYPASS_SHIFT (16U)

Definition at line 7410 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT

#define CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_MASK)

Definition at line 7393 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_MASK (0x7FU)

Definition at line 7391 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ARM_CLR_DIV_SELECT_SHIFT (0U)

Definition at line 7392 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_ENABLE

#define CCM_ANALOG_PLL_ARM_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_ENABLE_MASK)

Definition at line 7399 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_ENABLE_MASK

#define CCM_ANALOG_PLL_ARM_CLR_ENABLE_MASK (0x2000U)

Definition at line 7397 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ARM_CLR_ENABLE_SHIFT (13U)

Definition at line 7398 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_LOCK

#define CCM_ANALOG_PLL_ARM_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_LOCK_MASK)

Definition at line 7417 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_LOCK_MASK

#define CCM_ANALOG_PLL_ARM_CLR_LOCK_MASK (0x80000000U)

Definition at line 7415 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_LOCK_SHIFT

#define CCM_ANALOG_PLL_ARM_CLR_LOCK_SHIFT (31U)

Definition at line 7416 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_PLL_SEL

#define CCM_ANALOG_PLL_ARM_CLR_PLL_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_MASK)

Definition at line 7414 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_MASK

#define CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_MASK (0x80000U)

Definition at line 7412 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_SHIFT

#define CCM_ANALOG_PLL_ARM_CLR_PLL_SEL_SHIFT (19U)

Definition at line 7413 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_POWERDOWN

#define CCM_ANALOG_PLL_ARM_CLR_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_MASK)

Definition at line 7396 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_MASK (0x1000U)

Definition at line 7394 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ARM_CLR_POWERDOWN_SHIFT (12U)

Definition at line 7395 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_DIV_SELECT

#define CCM_ANALOG_PLL_ARM_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_DIV_SELECT_MASK)

Definition at line 7331 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ARM_DIV_SELECT_MASK (0x7FU)

Definition at line 7329 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ARM_DIV_SELECT_SHIFT (0U)

Definition at line 7330 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_ENABLE

#define CCM_ANALOG_PLL_ARM_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_ENABLE_MASK)

Definition at line 7337 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_ENABLE_MASK

#define CCM_ANALOG_PLL_ARM_ENABLE_MASK (0x2000U)

Definition at line 7335 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ARM_ENABLE_SHIFT (13U)

Definition at line 7336 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_LOCK

#define CCM_ANALOG_PLL_ARM_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_LOCK_MASK)

Definition at line 7355 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_LOCK_MASK

#define CCM_ANALOG_PLL_ARM_LOCK_MASK (0x80000000U)

Definition at line 7353 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_LOCK_SHIFT

#define CCM_ANALOG_PLL_ARM_LOCK_SHIFT (31U)

Definition at line 7354 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_PLL_SEL

#define CCM_ANALOG_PLL_ARM_PLL_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_PLL_SEL_MASK)

Definition at line 7352 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_PLL_SEL_MASK

#define CCM_ANALOG_PLL_ARM_PLL_SEL_MASK (0x80000U)

Definition at line 7350 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_PLL_SEL_SHIFT

#define CCM_ANALOG_PLL_ARM_PLL_SEL_SHIFT (19U)

Definition at line 7351 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_POWERDOWN

#define CCM_ANALOG_PLL_ARM_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_POWERDOWN_MASK)

Definition at line 7334 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ARM_POWERDOWN_MASK (0x1000U)

Definition at line 7332 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ARM_POWERDOWN_SHIFT (12U)

Definition at line 7333 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_BYPASS

#define CCM_ANALOG_PLL_ARM_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_BYPASS_MASK)

Definition at line 7380 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7377 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7369 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ARM_SET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7370 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_BYPASS_MASK

#define CCM_ANALOG_PLL_ARM_SET_BYPASS_MASK (0x10000U)

Definition at line 7378 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ARM_SET_BYPASS_SHIFT (16U)

Definition at line 7379 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_DIV_SELECT

#define CCM_ANALOG_PLL_ARM_SET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_MASK)

Definition at line 7362 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_MASK (0x7FU)

Definition at line 7360 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ARM_SET_DIV_SELECT_SHIFT (0U)

Definition at line 7361 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_ENABLE

#define CCM_ANALOG_PLL_ARM_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_ENABLE_MASK)

Definition at line 7368 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_ENABLE_MASK

#define CCM_ANALOG_PLL_ARM_SET_ENABLE_MASK (0x2000U)

Definition at line 7366 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ARM_SET_ENABLE_SHIFT (13U)

Definition at line 7367 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_LOCK

#define CCM_ANALOG_PLL_ARM_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_LOCK_MASK)

Definition at line 7386 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_LOCK_MASK

#define CCM_ANALOG_PLL_ARM_SET_LOCK_MASK (0x80000000U)

Definition at line 7384 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_LOCK_SHIFT

#define CCM_ANALOG_PLL_ARM_SET_LOCK_SHIFT (31U)

Definition at line 7385 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_PLL_SEL

#define CCM_ANALOG_PLL_ARM_SET_PLL_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_PLL_SEL_MASK)

Definition at line 7383 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_PLL_SEL_MASK

#define CCM_ANALOG_PLL_ARM_SET_PLL_SEL_MASK (0x80000U)

Definition at line 7381 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_PLL_SEL_SHIFT

#define CCM_ANALOG_PLL_ARM_SET_PLL_SEL_SHIFT (19U)

Definition at line 7382 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_POWERDOWN

#define CCM_ANALOG_PLL_ARM_SET_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_SET_POWERDOWN_MASK)

Definition at line 7365 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ARM_SET_POWERDOWN_MASK (0x1000U)

Definition at line 7363 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_SET_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ARM_SET_POWERDOWN_SHIFT (12U)

Definition at line 7364 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_BYPASS

#define CCM_ANALOG_PLL_ARM_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_BYPASS_MASK)

Definition at line 7442 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7439 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7431 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ARM_TOG_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7432 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_BYPASS_MASK

#define CCM_ANALOG_PLL_ARM_TOG_BYPASS_MASK (0x10000U)

Definition at line 7440 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ARM_TOG_BYPASS_SHIFT (16U)

Definition at line 7441 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT

#define CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_MASK)

Definition at line 7424 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_MASK (0x7FU)

Definition at line 7422 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ARM_TOG_DIV_SELECT_SHIFT (0U)

Definition at line 7423 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_ENABLE

#define CCM_ANALOG_PLL_ARM_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_ENABLE_MASK)

Definition at line 7430 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_ENABLE_MASK

#define CCM_ANALOG_PLL_ARM_TOG_ENABLE_MASK (0x2000U)

Definition at line 7428 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ARM_TOG_ENABLE_SHIFT (13U)

Definition at line 7429 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_LOCK

#define CCM_ANALOG_PLL_ARM_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_LOCK_MASK)

Definition at line 7448 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_LOCK_MASK

#define CCM_ANALOG_PLL_ARM_TOG_LOCK_MASK (0x80000000U)

Definition at line 7446 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_LOCK_SHIFT

#define CCM_ANALOG_PLL_ARM_TOG_LOCK_SHIFT (31U)

Definition at line 7447 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_PLL_SEL

#define CCM_ANALOG_PLL_ARM_TOG_PLL_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_MASK)

Definition at line 7445 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_MASK

#define CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_MASK (0x80000U)

Definition at line 7443 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_SHIFT

#define CCM_ANALOG_PLL_ARM_TOG_PLL_SEL_SHIFT (19U)

Definition at line 7444 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_POWERDOWN

#define CCM_ANALOG_PLL_ARM_TOG_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_MASK)

Definition at line 7427 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_MASK (0x1000U)

Definition at line 7425 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ARM_TOG_POWERDOWN_SHIFT (12U)

Definition at line 7426 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_BYPASS

#define CCM_ANALOG_PLL_AUDIO_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_BYPASS_MASK)

Definition at line 7864 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7861 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7853 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_AUDIO_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7854 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_BYPASS_MASK

#define CCM_ANALOG_PLL_AUDIO_BYPASS_MASK (0x10000U)

Definition at line 7862 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_BYPASS_SHIFT

#define CCM_ANALOG_PLL_AUDIO_BYPASS_SHIFT (16U)

Definition at line 7863 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_BYPASS

#define CCM_ANALOG_PLL_AUDIO_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_MASK)

Definition at line 7938 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7935 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7927 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7928 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_MASK

#define CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_MASK (0x10000U)

Definition at line 7936 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_SHIFT

#define CCM_ANALOG_PLL_AUDIO_CLR_BYPASS_SHIFT (16U)

Definition at line 7937 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_MASK)

Definition at line 7920 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_MASK (0x7FU)

Definition at line 7918 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_CLR_DIV_SELECT_SHIFT (0U)

Definition at line 7919 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_ENABLE

#define CCM_ANALOG_PLL_AUDIO_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_MASK)

Definition at line 7926 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_MASK

#define CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_MASK (0x2000U)

Definition at line 7924 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_SHIFT

#define CCM_ANALOG_PLL_AUDIO_CLR_ENABLE_SHIFT (13U)

Definition at line 7925 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_LOCK

#define CCM_ANALOG_PLL_AUDIO_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_LOCK_MASK)

Definition at line 7950 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_LOCK_MASK

#define CCM_ANALOG_PLL_AUDIO_CLR_LOCK_MASK (0x80000000U)

Definition at line 7948 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_LOCK_SHIFT

#define CCM_ANALOG_PLL_AUDIO_CLR_LOCK_SHIFT (31U)

Definition at line 7949 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 7947 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 7939 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_CLR_POST_DIV_SELECT_SHIFT (19U)

Definition at line 7940 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN

#define CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_MASK)

Definition at line 7923 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_MASK

#define CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_MASK (0x1000U)

Definition at line 7921 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_AUDIO_CLR_POWERDOWN_SHIFT (12U)

Definition at line 7922 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_DENOM_B

#define CCM_ANALOG_PLL_AUDIO_DENOM_B | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_DENOM_B_SHIFT)) & CCM_ANALOG_PLL_AUDIO_DENOM_B_MASK)

Definition at line 8001 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_DENOM_B_MASK

#define CCM_ANALOG_PLL_AUDIO_DENOM_B_MASK (0x3FFFFFFFU)

Definition at line 7999 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_DENOM_B_SHIFT

#define CCM_ANALOG_PLL_AUDIO_DENOM_B_SHIFT (0U)

Definition at line 8000 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_DIV_SELECT_MASK)

Definition at line 7846 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_DIV_SELECT_MASK (0x7FU)

Definition at line 7844 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_DIV_SELECT_SHIFT (0U)

Definition at line 7845 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_ENABLE

#define CCM_ANALOG_PLL_AUDIO_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_ENABLE_MASK)

Definition at line 7852 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_ENABLE_MASK

#define CCM_ANALOG_PLL_AUDIO_ENABLE_MASK (0x2000U)

Definition at line 7850 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_ENABLE_SHIFT

#define CCM_ANALOG_PLL_AUDIO_ENABLE_SHIFT (13U)

Definition at line 7851 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_LOCK

#define CCM_ANALOG_PLL_AUDIO_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_LOCK_MASK)

Definition at line 7876 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_LOCK_MASK

#define CCM_ANALOG_PLL_AUDIO_LOCK_MASK (0x80000000U)

Definition at line 7874 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_LOCK_SHIFT

#define CCM_ANALOG_PLL_AUDIO_LOCK_SHIFT (31U)

Definition at line 7875 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_NUM_A

#define CCM_ANALOG_PLL_AUDIO_NUM_A | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_NUM_A_SHIFT)) & CCM_ANALOG_PLL_AUDIO_NUM_A_MASK)

Definition at line 7994 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_NUM_A_MASK

#define CCM_ANALOG_PLL_AUDIO_NUM_A_MASK (0x3FFFFFFFU)

Definition at line 7992 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_NUM_A_SHIFT

#define CCM_ANALOG_PLL_AUDIO_NUM_A_SHIFT (0U)

Definition at line 7993 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 7873 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 7865 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_POST_DIV_SELECT_SHIFT (19U)

Definition at line 7866 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_POWERDOWN

#define CCM_ANALOG_PLL_AUDIO_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_POWERDOWN_MASK)

Definition at line 7849 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_POWERDOWN_MASK

#define CCM_ANALOG_PLL_AUDIO_POWERDOWN_MASK (0x1000U)

Definition at line 7847 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_AUDIO_POWERDOWN_SHIFT (12U)

Definition at line 7848 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_BYPASS

#define CCM_ANALOG_PLL_AUDIO_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_BYPASS_MASK)

Definition at line 7901 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7898 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7890 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_AUDIO_SET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7891 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_BYPASS_MASK

#define CCM_ANALOG_PLL_AUDIO_SET_BYPASS_MASK (0x10000U)

Definition at line 7899 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_AUDIO_SET_BYPASS_SHIFT (16U)

Definition at line 7900 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_MASK)

Definition at line 7883 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_MASK (0x7FU)

Definition at line 7881 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_SET_DIV_SELECT_SHIFT (0U)

Definition at line 7882 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_ENABLE

#define CCM_ANALOG_PLL_AUDIO_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_ENABLE_MASK)

Definition at line 7889 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_ENABLE_MASK

#define CCM_ANALOG_PLL_AUDIO_SET_ENABLE_MASK (0x2000U)

Definition at line 7887 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_AUDIO_SET_ENABLE_SHIFT (13U)

Definition at line 7888 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_LOCK

#define CCM_ANALOG_PLL_AUDIO_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_LOCK_MASK)

Definition at line 7913 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_LOCK_MASK

#define CCM_ANALOG_PLL_AUDIO_SET_LOCK_MASK (0x80000000U)

Definition at line 7911 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_LOCK_SHIFT

#define CCM_ANALOG_PLL_AUDIO_SET_LOCK_SHIFT (31U)

Definition at line 7912 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 7910 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 7902 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_SET_POST_DIV_SELECT_SHIFT (19U)

Definition at line 7903 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN

#define CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_MASK)

Definition at line 7886 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_MASK

#define CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_MASK (0x1000U)

Definition at line 7884 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_AUDIO_SET_POWERDOWN_SHIFT (12U)

Definition at line 7885 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_BYPASS

#define CCM_ANALOG_PLL_AUDIO_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_MASK)

Definition at line 7975 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7972 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7964 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7965 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_MASK

#define CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_MASK (0x10000U)

Definition at line 7973 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_SHIFT

#define CCM_ANALOG_PLL_AUDIO_TOG_BYPASS_SHIFT (16U)

Definition at line 7974 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_MASK)

Definition at line 7957 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_MASK (0x7FU)

Definition at line 7955 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_TOG_DIV_SELECT_SHIFT (0U)

Definition at line 7956 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_ENABLE

#define CCM_ANALOG_PLL_AUDIO_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_MASK)

Definition at line 7963 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_MASK

#define CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_MASK (0x2000U)

Definition at line 7961 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_SHIFT

#define CCM_ANALOG_PLL_AUDIO_TOG_ENABLE_SHIFT (13U)

Definition at line 7962 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_LOCK

#define CCM_ANALOG_PLL_AUDIO_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_LOCK_MASK)

Definition at line 7987 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_LOCK_MASK

#define CCM_ANALOG_PLL_AUDIO_TOG_LOCK_MASK (0x80000000U)

Definition at line 7985 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_LOCK_SHIFT

#define CCM_ANALOG_PLL_AUDIO_TOG_LOCK_SHIFT (31U)

Definition at line 7986 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT

#define CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 7984 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 7976 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_AUDIO_TOG_POST_DIV_SELECT_SHIFT (19U)

Definition at line 7977 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN

#define CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_MASK)

Definition at line 7960 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_MASK

#define CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_MASK (0x1000U)

Definition at line 7958 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_AUDIO_TOG_POWERDOWN_SHIFT (12U)

Definition at line 7959 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_BYPASS

#define CCM_ANALOG_PLL_ENET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_BYPASS_MASK)

Definition at line 8197 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8194 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8186 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ENET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8187 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_BYPASS_MASK

#define CCM_ANALOG_PLL_ENET_BYPASS_MASK (0x10000U)

Definition at line 8195 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ENET_BYPASS_SHIFT (16U)

Definition at line 8196 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_BYPASS

#define CCM_ANALOG_PLL_ENET_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_BYPASS_MASK)

Definition at line 8283 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8280 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8272 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8273 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_BYPASS_MASK

#define CCM_ANALOG_PLL_ENET_CLR_BYPASS_MASK (0x10000U)

Definition at line 8281 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_BYPASS_SHIFT (16U)

Definition at line 8282 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_MASK)

Definition at line 8256 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_MASK (0x3U)

Definition at line 8254 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_DIV_SELECT_SHIFT (0U)

Definition at line 8255 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENABLE

#define CCM_ANALOG_PLL_ENET_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENABLE_MASK)

Definition at line 8271 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENABLE_MASK

#define CCM_ANALOG_PLL_ENET_CLR_ENABLE_MASK (0x2000U)

Definition at line 8269 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_ENABLE_SHIFT (13U)

Definition at line 8270 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_MASK)

ENET2_DIV_SELECT 0b00..25MHz 0b01..50MHz 0b10..100MHz (not 50% duty cycle) 0b11..125MHz

Definition at line 8265 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_MASK (0xCU)

Definition at line 8257 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_ENET2_DIV_SELECT_SHIFT (2U)

Definition at line 8258 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN

#define CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_MASK)

Definition at line 8286 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_MASK (0x100000U)

Definition at line 8284 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_ENET2_REF_EN_SHIFT (20U)

Definition at line 8285 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN

#define CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_MASK)

Definition at line 8289 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_MASK (0x200000U)

Definition at line 8287 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_ENET_25M_REF_EN_SHIFT (21U)

Definition at line 8288 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_LOCK

#define CCM_ANALOG_PLL_ENET_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_LOCK_MASK)

Definition at line 8292 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_LOCK_MASK

#define CCM_ANALOG_PLL_ENET_CLR_LOCK_MASK (0x80000000U)

Definition at line 8290 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_LOCK_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_LOCK_SHIFT (31U)

Definition at line 8291 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_POWERDOWN

#define CCM_ANALOG_PLL_ENET_CLR_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_MASK)

Definition at line 8268 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_MASK (0x1000U)

Definition at line 8266 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ENET_CLR_POWERDOWN_SHIFT (12U)

Definition at line 8267 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_DIV_SELECT_MASK)

Definition at line 8170 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_DIV_SELECT_MASK (0x3U)

Definition at line 8168 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_DIV_SELECT_SHIFT (0U)

Definition at line 8169 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENABLE

#define CCM_ANALOG_PLL_ENET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_ENABLE_MASK)

Definition at line 8185 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENABLE_MASK

#define CCM_ANALOG_PLL_ENET_ENABLE_MASK (0x2000U)

Definition at line 8183 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ENET_ENABLE_SHIFT (13U)

Definition at line 8184 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_MASK)

ENET2_DIV_SELECT 0b00..25MHz 0b01..50MHz 0b10..100MHz (not 50% duty cycle) 0b11..125MHz

Definition at line 8179 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_MASK (0xCU)

Definition at line 8171 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_ENET2_DIV_SELECT_SHIFT (2U)

Definition at line 8172 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET2_REF_EN

#define CCM_ANALOG_PLL_ENET_ENET2_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_ENET2_REF_EN_MASK)

Definition at line 8200 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET2_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_ENET2_REF_EN_MASK (0x100000U)

Definition at line 8198 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET2_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_ENET2_REF_EN_SHIFT (20U)

Definition at line 8199 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN

#define CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_MASK)

Definition at line 8203 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_MASK (0x200000U)

Definition at line 8201 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_SHIFT (21U)

Definition at line 8202 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_LOCK

#define CCM_ANALOG_PLL_ENET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_LOCK_MASK)

Definition at line 8206 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_LOCK_MASK

#define CCM_ANALOG_PLL_ENET_LOCK_MASK (0x80000000U)

Definition at line 8204 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_LOCK_SHIFT

#define CCM_ANALOG_PLL_ENET_LOCK_SHIFT (31U)

Definition at line 8205 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_POWERDOWN

#define CCM_ANALOG_PLL_ENET_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_POWERDOWN_MASK)

Definition at line 8182 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ENET_POWERDOWN_MASK (0x1000U)

Definition at line 8180 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ENET_POWERDOWN_SHIFT (12U)

Definition at line 8181 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_BYPASS

#define CCM_ANALOG_PLL_ENET_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_BYPASS_MASK)

Definition at line 8240 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8237 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8229 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8230 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_BYPASS_MASK

#define CCM_ANALOG_PLL_ENET_SET_BYPASS_MASK (0x10000U)

Definition at line 8238 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_BYPASS_SHIFT (16U)

Definition at line 8239 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_SET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_MASK)

Definition at line 8213 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_MASK (0x3U)

Definition at line 8211 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_DIV_SELECT_SHIFT (0U)

Definition at line 8212 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENABLE

#define CCM_ANALOG_PLL_ENET_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENABLE_MASK)

Definition at line 8228 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENABLE_MASK

#define CCM_ANALOG_PLL_ENET_SET_ENABLE_MASK (0x2000U)

Definition at line 8226 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_ENABLE_SHIFT (13U)

Definition at line 8227 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_MASK)

ENET2_DIV_SELECT 0b00..25MHz 0b01..50MHz 0b10..100MHz (not 50% duty cycle) 0b11..125MHz

Definition at line 8222 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_MASK (0xCU)

Definition at line 8214 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_ENET2_DIV_SELECT_SHIFT (2U)

Definition at line 8215 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN

#define CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_MASK)

Definition at line 8243 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_MASK (0x100000U)

Definition at line 8241 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_ENET2_REF_EN_SHIFT (20U)

Definition at line 8242 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN

#define CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_MASK)

Definition at line 8246 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_MASK (0x200000U)

Definition at line 8244 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_ENET_25M_REF_EN_SHIFT (21U)

Definition at line 8245 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_LOCK

#define CCM_ANALOG_PLL_ENET_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_LOCK_MASK)

Definition at line 8249 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_LOCK_MASK

#define CCM_ANALOG_PLL_ENET_SET_LOCK_MASK (0x80000000U)

Definition at line 8247 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_LOCK_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_LOCK_SHIFT (31U)

Definition at line 8248 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_POWERDOWN

#define CCM_ANALOG_PLL_ENET_SET_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_SET_POWERDOWN_MASK)

Definition at line 8225 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ENET_SET_POWERDOWN_MASK (0x1000U)

Definition at line 8223 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_SET_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ENET_SET_POWERDOWN_SHIFT (12U)

Definition at line 8224 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_BYPASS

#define CCM_ANALOG_PLL_ENET_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_BYPASS_MASK)

Definition at line 8326 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8323 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8315 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8316 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_BYPASS_MASK

#define CCM_ANALOG_PLL_ENET_TOG_BYPASS_MASK (0x10000U)

Definition at line 8324 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_BYPASS_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_BYPASS_SHIFT (16U)

Definition at line 8325 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_MASK)

Definition at line 8299 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_MASK (0x3U)

Definition at line 8297 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_DIV_SELECT_SHIFT (0U)

Definition at line 8298 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENABLE

#define CCM_ANALOG_PLL_ENET_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENABLE_MASK)

Definition at line 8314 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENABLE_MASK

#define CCM_ANALOG_PLL_ENET_TOG_ENABLE_MASK (0x2000U)

Definition at line 8312 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENABLE_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_ENABLE_SHIFT (13U)

Definition at line 8313 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT

#define CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_MASK)

ENET2_DIV_SELECT 0b00..25MHz 0b01..50MHz 0b10..100MHz (not 50% duty cycle) 0b11..125MHz

Definition at line 8308 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_MASK (0xCU)

Definition at line 8300 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_ENET2_DIV_SELECT_SHIFT (2U)

Definition at line 8301 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN

#define CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_MASK)

Definition at line 8329 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_MASK (0x100000U)

Definition at line 8327 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_ENET2_REF_EN_SHIFT (20U)

Definition at line 8328 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN

#define CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_MASK)

Definition at line 8332 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_MASK

#define CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_MASK (0x200000U)

Definition at line 8330 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_ENET_25M_REF_EN_SHIFT (21U)

Definition at line 8331 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_LOCK

#define CCM_ANALOG_PLL_ENET_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_LOCK_MASK)

Definition at line 8335 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_LOCK_MASK

#define CCM_ANALOG_PLL_ENET_TOG_LOCK_MASK (0x80000000U)

Definition at line 8333 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_LOCK_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_LOCK_SHIFT (31U)

Definition at line 8334 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_POWERDOWN

#define CCM_ANALOG_PLL_ENET_TOG_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_MASK)

Definition at line 8311 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_MASK

#define CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_MASK (0x1000U)

Definition at line 8309 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_ENET_TOG_POWERDOWN_SHIFT (12U)

Definition at line 8310 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_BYPASS

#define CCM_ANALOG_PLL_SYS_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_BYPASS_MASK)

Definition at line 7727 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7724 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7718 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_SYS_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7719 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_BYPASS_MASK

#define CCM_ANALOG_PLL_SYS_BYPASS_MASK (0x10000U)

Definition at line 7725 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_BYPASS_SHIFT

#define CCM_ANALOG_PLL_SYS_BYPASS_SHIFT (16U)

Definition at line 7726 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_BYPASS

#define CCM_ANALOG_PLL_SYS_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_BYPASS_MASK)

Definition at line 7779 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7776 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7770 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_SYS_CLR_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7771 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_BYPASS_MASK

#define CCM_ANALOG_PLL_SYS_CLR_BYPASS_MASK (0x10000U)

Definition at line 7777 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_BYPASS_SHIFT

#define CCM_ANALOG_PLL_SYS_CLR_BYPASS_SHIFT (16U)

Definition at line 7778 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT

#define CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_MASK)

Definition at line 7763 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_MASK (0x1U)

Definition at line 7761 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_SYS_CLR_DIV_SELECT_SHIFT (0U)

Definition at line 7762 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_ENABLE

#define CCM_ANALOG_PLL_SYS_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_ENABLE_MASK)

Definition at line 7769 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_ENABLE_MASK

#define CCM_ANALOG_PLL_SYS_CLR_ENABLE_MASK (0x2000U)

Definition at line 7767 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_ENABLE_SHIFT

#define CCM_ANALOG_PLL_SYS_CLR_ENABLE_SHIFT (13U)

Definition at line 7768 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_LOCK

#define CCM_ANALOG_PLL_SYS_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_LOCK_MASK)

Definition at line 7782 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_LOCK_MASK

#define CCM_ANALOG_PLL_SYS_CLR_LOCK_MASK (0x80000000U)

Definition at line 7780 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_LOCK_SHIFT

#define CCM_ANALOG_PLL_SYS_CLR_LOCK_SHIFT (31U)

Definition at line 7781 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_POWERDOWN

#define CCM_ANALOG_PLL_SYS_CLR_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_MASK)

Definition at line 7766 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_MASK

#define CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_MASK (0x1000U)

Definition at line 7764 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_SYS_CLR_POWERDOWN_SHIFT (12U)

Definition at line 7765 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_DENOM_B

#define CCM_ANALOG_PLL_SYS_DENOM_B | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_DENOM_B_SHIFT)) & CCM_ANALOG_PLL_SYS_DENOM_B_MASK)

Definition at line 7839 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_DENOM_B_MASK

#define CCM_ANALOG_PLL_SYS_DENOM_B_MASK (0x3FFFFFFFU)

Definition at line 7837 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_DENOM_B_SHIFT

#define CCM_ANALOG_PLL_SYS_DENOM_B_SHIFT (0U)

Definition at line 7838 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_DIV_SELECT

#define CCM_ANALOG_PLL_SYS_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_DIV_SELECT_MASK)

Definition at line 7711 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_SYS_DIV_SELECT_MASK (0x1U)

Definition at line 7709 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_SYS_DIV_SELECT_SHIFT (0U)

Definition at line 7710 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_ENABLE

#define CCM_ANALOG_PLL_SYS_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_ENABLE_MASK)

Definition at line 7717 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_ENABLE_MASK

#define CCM_ANALOG_PLL_SYS_ENABLE_MASK (0x2000U)

Definition at line 7715 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_ENABLE_SHIFT

#define CCM_ANALOG_PLL_SYS_ENABLE_SHIFT (13U)

Definition at line 7716 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_LOCK

#define CCM_ANALOG_PLL_SYS_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_LOCK_MASK)

Definition at line 7730 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_LOCK_MASK

#define CCM_ANALOG_PLL_SYS_LOCK_MASK (0x80000000U)

Definition at line 7728 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_LOCK_SHIFT

#define CCM_ANALOG_PLL_SYS_LOCK_SHIFT (31U)

Definition at line 7729 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_NUM_A

#define CCM_ANALOG_PLL_SYS_NUM_A | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_NUM_A_SHIFT)) & CCM_ANALOG_PLL_SYS_NUM_A_MASK)

Definition at line 7832 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_NUM_A_MASK

#define CCM_ANALOG_PLL_SYS_NUM_A_MASK (0x3FFFFFFFU)

Definition at line 7830 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_NUM_A_SHIFT

#define CCM_ANALOG_PLL_SYS_NUM_A_SHIFT (0U)

Definition at line 7831 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_POWERDOWN

#define CCM_ANALOG_PLL_SYS_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_POWERDOWN_MASK)

Definition at line 7714 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_POWERDOWN_MASK

#define CCM_ANALOG_PLL_SYS_POWERDOWN_MASK (0x1000U)

Definition at line 7712 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_SYS_POWERDOWN_SHIFT (12U)

Definition at line 7713 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_BYPASS

#define CCM_ANALOG_PLL_SYS_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_BYPASS_MASK)

Definition at line 7753 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7750 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7744 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_SYS_SET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7745 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_BYPASS_MASK

#define CCM_ANALOG_PLL_SYS_SET_BYPASS_MASK (0x10000U)

Definition at line 7751 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_SYS_SET_BYPASS_SHIFT (16U)

Definition at line 7752 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_DIV_SELECT

#define CCM_ANALOG_PLL_SYS_SET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_MASK)

Definition at line 7737 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_MASK (0x1U)

Definition at line 7735 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_SYS_SET_DIV_SELECT_SHIFT (0U)

Definition at line 7736 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_ENABLE

#define CCM_ANALOG_PLL_SYS_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_ENABLE_MASK)

Definition at line 7743 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_ENABLE_MASK

#define CCM_ANALOG_PLL_SYS_SET_ENABLE_MASK (0x2000U)

Definition at line 7741 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_SYS_SET_ENABLE_SHIFT (13U)

Definition at line 7742 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_LOCK

#define CCM_ANALOG_PLL_SYS_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_LOCK_MASK)

Definition at line 7756 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_LOCK_MASK

#define CCM_ANALOG_PLL_SYS_SET_LOCK_MASK (0x80000000U)

Definition at line 7754 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_LOCK_SHIFT

#define CCM_ANALOG_PLL_SYS_SET_LOCK_SHIFT (31U)

Definition at line 7755 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_POWERDOWN

#define CCM_ANALOG_PLL_SYS_SET_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_SET_POWERDOWN_MASK)

Definition at line 7740 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_POWERDOWN_MASK

#define CCM_ANALOG_PLL_SYS_SET_POWERDOWN_MASK (0x1000U)

Definition at line 7738 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SET_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_SYS_SET_POWERDOWN_SHIFT (12U)

Definition at line 7739 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_ENABLE

#define CCM_ANALOG_PLL_SYS_SS_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SS_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_SS_ENABLE_MASK)

ENABLE - Enable bit 0b0..Spread spectrum modulation disabled 0b1..Soread spectrum modulation enabled

Definition at line 7822 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_ENABLE_MASK

#define CCM_ANALOG_PLL_SYS_SS_ENABLE_MASK (0x8000U)

Definition at line 7816 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_ENABLE_SHIFT

#define CCM_ANALOG_PLL_SYS_SS_ENABLE_SHIFT (15U)

Definition at line 7817 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_STEP

#define CCM_ANALOG_PLL_SYS_SS_STEP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SS_STEP_SHIFT)) & CCM_ANALOG_PLL_SYS_SS_STEP_MASK)

Definition at line 7815 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_STEP_MASK

#define CCM_ANALOG_PLL_SYS_SS_STEP_MASK (0x7FFFU)

Definition at line 7813 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_STEP_SHIFT

#define CCM_ANALOG_PLL_SYS_SS_STEP_SHIFT (0U)

Definition at line 7814 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_STOP

#define CCM_ANALOG_PLL_SYS_SS_STOP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_SS_STOP_SHIFT)) & CCM_ANALOG_PLL_SYS_SS_STOP_MASK)

Definition at line 7825 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_STOP_MASK

#define CCM_ANALOG_PLL_SYS_SS_STOP_MASK (0xFFFF0000U)

Definition at line 7823 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_SS_STOP_SHIFT

#define CCM_ANALOG_PLL_SYS_SS_STOP_SHIFT (16U)

Definition at line 7824 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_BYPASS

#define CCM_ANALOG_PLL_SYS_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_BYPASS_MASK)

Definition at line 7805 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7802 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7796 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_SYS_TOG_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7797 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_BYPASS_MASK

#define CCM_ANALOG_PLL_SYS_TOG_BYPASS_MASK (0x10000U)

Definition at line 7803 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_BYPASS_SHIFT

#define CCM_ANALOG_PLL_SYS_TOG_BYPASS_SHIFT (16U)

Definition at line 7804 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT

#define CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_MASK)

Definition at line 7789 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_MASK (0x1U)

Definition at line 7787 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_SYS_TOG_DIV_SELECT_SHIFT (0U)

Definition at line 7788 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_ENABLE

#define CCM_ANALOG_PLL_SYS_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_ENABLE_MASK)

Definition at line 7795 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_ENABLE_MASK

#define CCM_ANALOG_PLL_SYS_TOG_ENABLE_MASK (0x2000U)

Definition at line 7793 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_ENABLE_SHIFT

#define CCM_ANALOG_PLL_SYS_TOG_ENABLE_SHIFT (13U)

Definition at line 7794 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_LOCK

#define CCM_ANALOG_PLL_SYS_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_LOCK_MASK)

Definition at line 7808 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_LOCK_MASK

#define CCM_ANALOG_PLL_SYS_TOG_LOCK_MASK (0x80000000U)

Definition at line 7806 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_LOCK_SHIFT

#define CCM_ANALOG_PLL_SYS_TOG_LOCK_SHIFT (31U)

Definition at line 7807 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_POWERDOWN

#define CCM_ANALOG_PLL_SYS_TOG_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_MASK)

Definition at line 7792 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_MASK

#define CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_MASK (0x1000U)

Definition at line 7790 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_SYS_TOG_POWERDOWN_SHIFT (12U)

Definition at line 7791 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_BYPASS

#define CCM_ANALOG_PLL_USB1_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_BYPASS_MASK)

Definition at line 7478 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7475 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7469 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB1_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7470 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_BYPASS_MASK

#define CCM_ANALOG_PLL_USB1_BYPASS_MASK (0x10000U)

Definition at line 7476 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB1_BYPASS_SHIFT (16U)

Definition at line 7477 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_BYPASS

#define CCM_ANALOG_PLL_USB1_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_BYPASS_MASK)

Definition at line 7544 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7541 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7535 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB1_CLR_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7536 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_BYPASS_MASK

#define CCM_ANALOG_PLL_USB1_CLR_BYPASS_MASK (0x10000U)

Definition at line 7542 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB1_CLR_BYPASS_SHIFT (16U)

Definition at line 7543 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT

#define CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_MASK)

Definition at line 7521 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_MASK (0x2U)

Definition at line 7519 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB1_CLR_DIV_SELECT_SHIFT (1U)

Definition at line 7520 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_MASK)

EN_USB_CLKS 0b0..PLL outputs for USBPHYn off. 0b1..PLL outputs for USBPHYn on.

Definition at line 7528 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_MASK (0x40U)

Definition at line 7522 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB1_CLR_EN_USB_CLKS_SHIFT (6U)

Definition at line 7523 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_ENABLE

#define CCM_ANALOG_PLL_USB1_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_ENABLE_MASK)

Definition at line 7534 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_ENABLE_MASK

#define CCM_ANALOG_PLL_USB1_CLR_ENABLE_MASK (0x2000U)

Definition at line 7532 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB1_CLR_ENABLE_SHIFT (13U)

Definition at line 7533 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_LOCK

#define CCM_ANALOG_PLL_USB1_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_LOCK_MASK)

Definition at line 7547 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_LOCK_MASK

#define CCM_ANALOG_PLL_USB1_CLR_LOCK_MASK (0x80000000U)

Definition at line 7545 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB1_CLR_LOCK_SHIFT (31U)

Definition at line 7546 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_POWER

#define CCM_ANALOG_PLL_USB1_CLR_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_CLR_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_CLR_POWER_MASK)

Definition at line 7531 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_POWER_MASK

#define CCM_ANALOG_PLL_USB1_CLR_POWER_MASK (0x1000U)

Definition at line 7529 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_CLR_POWER_SHIFT

#define CCM_ANALOG_PLL_USB1_CLR_POWER_SHIFT (12U)

Definition at line 7530 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_DIV_SELECT

#define CCM_ANALOG_PLL_USB1_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_DIV_SELECT_MASK)

Definition at line 7455 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB1_DIV_SELECT_MASK (0x2U)

Definition at line 7453 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB1_DIV_SELECT_SHIFT (1U)

Definition at line 7454 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB1_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_EN_USB_CLKS_MASK)

EN_USB_CLKS 0b0..PLL outputs for USBPHYn off. 0b1..PLL outputs for USBPHYn on.

Definition at line 7462 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB1_EN_USB_CLKS_MASK (0x40U)

Definition at line 7456 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB1_EN_USB_CLKS_SHIFT (6U)

Definition at line 7457 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_ENABLE

#define CCM_ANALOG_PLL_USB1_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_ENABLE_MASK)

Definition at line 7468 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_ENABLE_MASK

#define CCM_ANALOG_PLL_USB1_ENABLE_MASK (0x2000U)

Definition at line 7466 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB1_ENABLE_SHIFT (13U)

Definition at line 7467 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_LOCK

#define CCM_ANALOG_PLL_USB1_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_LOCK_MASK)

Definition at line 7481 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_LOCK_MASK

#define CCM_ANALOG_PLL_USB1_LOCK_MASK (0x80000000U)

Definition at line 7479 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB1_LOCK_SHIFT (31U)

Definition at line 7480 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_POWER

#define CCM_ANALOG_PLL_USB1_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_POWER_MASK)

Definition at line 7465 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_POWER_MASK

#define CCM_ANALOG_PLL_USB1_POWER_MASK (0x1000U)

Definition at line 7463 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_POWER_SHIFT

#define CCM_ANALOG_PLL_USB1_POWER_SHIFT (12U)

Definition at line 7464 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_BYPASS

#define CCM_ANALOG_PLL_USB1_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_BYPASS_MASK)

Definition at line 7511 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7508 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7502 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB1_SET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7503 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_BYPASS_MASK

#define CCM_ANALOG_PLL_USB1_SET_BYPASS_MASK (0x10000U)

Definition at line 7509 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB1_SET_BYPASS_SHIFT (16U)

Definition at line 7510 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_DIV_SELECT

#define CCM_ANALOG_PLL_USB1_SET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_MASK)

Definition at line 7488 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_MASK (0x2U)

Definition at line 7486 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB1_SET_DIV_SELECT_SHIFT (1U)

Definition at line 7487 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_MASK)

EN_USB_CLKS 0b0..PLL outputs for USBPHYn off. 0b1..PLL outputs for USBPHYn on.

Definition at line 7495 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_MASK (0x40U)

Definition at line 7489 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB1_SET_EN_USB_CLKS_SHIFT (6U)

Definition at line 7490 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_ENABLE

#define CCM_ANALOG_PLL_USB1_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_ENABLE_MASK)

Definition at line 7501 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_ENABLE_MASK

#define CCM_ANALOG_PLL_USB1_SET_ENABLE_MASK (0x2000U)

Definition at line 7499 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB1_SET_ENABLE_SHIFT (13U)

Definition at line 7500 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_LOCK

#define CCM_ANALOG_PLL_USB1_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_LOCK_MASK)

Definition at line 7514 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_LOCK_MASK

#define CCM_ANALOG_PLL_USB1_SET_LOCK_MASK (0x80000000U)

Definition at line 7512 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB1_SET_LOCK_SHIFT (31U)

Definition at line 7513 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_POWER

#define CCM_ANALOG_PLL_USB1_SET_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_SET_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_SET_POWER_MASK)

Definition at line 7498 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_POWER_MASK

#define CCM_ANALOG_PLL_USB1_SET_POWER_MASK (0x1000U)

Definition at line 7496 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_SET_POWER_SHIFT

#define CCM_ANALOG_PLL_USB1_SET_POWER_SHIFT (12U)

Definition at line 7497 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_BYPASS

#define CCM_ANALOG_PLL_USB1_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_BYPASS_MASK)

Definition at line 7577 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source.

Definition at line 7574 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7568 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB1_TOG_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7569 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_BYPASS_MASK

#define CCM_ANALOG_PLL_USB1_TOG_BYPASS_MASK (0x10000U)

Definition at line 7575 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB1_TOG_BYPASS_SHIFT (16U)

Definition at line 7576 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT

#define CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_MASK)

Definition at line 7554 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_MASK (0x2U)

Definition at line 7552 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB1_TOG_DIV_SELECT_SHIFT (1U)

Definition at line 7553 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_MASK)

EN_USB_CLKS 0b0..PLL outputs for USBPHYn off. 0b1..PLL outputs for USBPHYn on.

Definition at line 7561 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_MASK (0x40U)

Definition at line 7555 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB1_TOG_EN_USB_CLKS_SHIFT (6U)

Definition at line 7556 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_ENABLE

#define CCM_ANALOG_PLL_USB1_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_ENABLE_MASK)

Definition at line 7567 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_ENABLE_MASK

#define CCM_ANALOG_PLL_USB1_TOG_ENABLE_MASK (0x2000U)

Definition at line 7565 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB1_TOG_ENABLE_SHIFT (13U)

Definition at line 7566 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_LOCK

#define CCM_ANALOG_PLL_USB1_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_LOCK_MASK)

Definition at line 7580 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_LOCK_MASK

#define CCM_ANALOG_PLL_USB1_TOG_LOCK_MASK (0x80000000U)

Definition at line 7578 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB1_TOG_LOCK_SHIFT (31U)

Definition at line 7579 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_POWER

#define CCM_ANALOG_PLL_USB1_TOG_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB1_TOG_POWER_SHIFT)) & CCM_ANALOG_PLL_USB1_TOG_POWER_MASK)

Definition at line 7564 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_POWER_MASK

#define CCM_ANALOG_PLL_USB1_TOG_POWER_MASK (0x1000U)

Definition at line 7562 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB1_TOG_POWER_SHIFT

#define CCM_ANALOG_PLL_USB1_TOG_POWER_SHIFT (12U)

Definition at line 7563 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_BYPASS

#define CCM_ANALOG_PLL_USB2_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_BYPASS_MASK)

Definition at line 7608 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7605 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7597 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB2_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7598 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_BYPASS_MASK

#define CCM_ANALOG_PLL_USB2_BYPASS_MASK (0x10000U)

Definition at line 7606 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB2_BYPASS_SHIFT (16U)

Definition at line 7607 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_BYPASS

#define CCM_ANALOG_PLL_USB2_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_BYPASS_MASK)

Definition at line 7670 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7667 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7659 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB2_CLR_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7660 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_BYPASS_MASK

#define CCM_ANALOG_PLL_USB2_CLR_BYPASS_MASK (0x10000U)

Definition at line 7668 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB2_CLR_BYPASS_SHIFT (16U)

Definition at line 7669 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT

#define CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_MASK)

Definition at line 7649 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_MASK (0x2U)

Definition at line 7647 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB2_CLR_DIV_SELECT_SHIFT (1U)

Definition at line 7648 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_MASK)

Definition at line 7652 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_MASK (0x40U)

Definition at line 7650 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB2_CLR_EN_USB_CLKS_SHIFT (6U)

Definition at line 7651 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_ENABLE

#define CCM_ANALOG_PLL_USB2_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_ENABLE_MASK)

Definition at line 7658 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_ENABLE_MASK

#define CCM_ANALOG_PLL_USB2_CLR_ENABLE_MASK (0x2000U)

Definition at line 7656 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB2_CLR_ENABLE_SHIFT (13U)

Definition at line 7657 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_LOCK

#define CCM_ANALOG_PLL_USB2_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_LOCK_MASK)

Definition at line 7673 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_LOCK_MASK

#define CCM_ANALOG_PLL_USB2_CLR_LOCK_MASK (0x80000000U)

Definition at line 7671 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB2_CLR_LOCK_SHIFT (31U)

Definition at line 7672 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_POWER

#define CCM_ANALOG_PLL_USB2_CLR_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_CLR_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_CLR_POWER_MASK)

Definition at line 7655 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_POWER_MASK

#define CCM_ANALOG_PLL_USB2_CLR_POWER_MASK (0x1000U)

Definition at line 7653 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_CLR_POWER_SHIFT

#define CCM_ANALOG_PLL_USB2_CLR_POWER_SHIFT (12U)

Definition at line 7654 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_DIV_SELECT

#define CCM_ANALOG_PLL_USB2_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_DIV_SELECT_MASK)

Definition at line 7587 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB2_DIV_SELECT_MASK (0x2U)

Definition at line 7585 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB2_DIV_SELECT_SHIFT (1U)

Definition at line 7586 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB2_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_EN_USB_CLKS_MASK)

Definition at line 7590 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB2_EN_USB_CLKS_MASK (0x40U)

Definition at line 7588 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB2_EN_USB_CLKS_SHIFT (6U)

Definition at line 7589 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_ENABLE

#define CCM_ANALOG_PLL_USB2_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_ENABLE_MASK)

Definition at line 7596 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_ENABLE_MASK

#define CCM_ANALOG_PLL_USB2_ENABLE_MASK (0x2000U)

Definition at line 7594 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB2_ENABLE_SHIFT (13U)

Definition at line 7595 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_LOCK

#define CCM_ANALOG_PLL_USB2_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_LOCK_MASK)

Definition at line 7611 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_LOCK_MASK

#define CCM_ANALOG_PLL_USB2_LOCK_MASK (0x80000000U)

Definition at line 7609 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB2_LOCK_SHIFT (31U)

Definition at line 7610 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_POWER

#define CCM_ANALOG_PLL_USB2_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_POWER_MASK)

Definition at line 7593 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_POWER_MASK

#define CCM_ANALOG_PLL_USB2_POWER_MASK (0x1000U)

Definition at line 7591 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_POWER_SHIFT

#define CCM_ANALOG_PLL_USB2_POWER_SHIFT (12U)

Definition at line 7592 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_BYPASS

#define CCM_ANALOG_PLL_USB2_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_BYPASS_MASK)

Definition at line 7639 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7636 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7628 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB2_SET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7629 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_BYPASS_MASK

#define CCM_ANALOG_PLL_USB2_SET_BYPASS_MASK (0x10000U)

Definition at line 7637 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB2_SET_BYPASS_SHIFT (16U)

Definition at line 7638 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_DIV_SELECT

#define CCM_ANALOG_PLL_USB2_SET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_MASK)

Definition at line 7618 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_MASK (0x2U)

Definition at line 7616 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB2_SET_DIV_SELECT_SHIFT (1U)

Definition at line 7617 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_MASK)

Definition at line 7621 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_MASK (0x40U)

Definition at line 7619 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB2_SET_EN_USB_CLKS_SHIFT (6U)

Definition at line 7620 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_ENABLE

#define CCM_ANALOG_PLL_USB2_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_ENABLE_MASK)

Definition at line 7627 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_ENABLE_MASK

#define CCM_ANALOG_PLL_USB2_SET_ENABLE_MASK (0x2000U)

Definition at line 7625 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB2_SET_ENABLE_SHIFT (13U)

Definition at line 7626 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_LOCK

#define CCM_ANALOG_PLL_USB2_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_LOCK_MASK)

Definition at line 7642 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_LOCK_MASK

#define CCM_ANALOG_PLL_USB2_SET_LOCK_MASK (0x80000000U)

Definition at line 7640 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB2_SET_LOCK_SHIFT (31U)

Definition at line 7641 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_POWER

#define CCM_ANALOG_PLL_USB2_SET_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_SET_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_SET_POWER_MASK)

Definition at line 7624 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_POWER_MASK

#define CCM_ANALOG_PLL_USB2_SET_POWER_MASK (0x1000U)

Definition at line 7622 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_SET_POWER_SHIFT

#define CCM_ANALOG_PLL_USB2_SET_POWER_SHIFT (12U)

Definition at line 7623 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_BYPASS

#define CCM_ANALOG_PLL_USB2_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_BYPASS_MASK)

Definition at line 7701 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 7698 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 7690 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_USB2_TOG_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 7691 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_BYPASS_MASK

#define CCM_ANALOG_PLL_USB2_TOG_BYPASS_MASK (0x10000U)

Definition at line 7699 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_BYPASS_SHIFT

#define CCM_ANALOG_PLL_USB2_TOG_BYPASS_SHIFT (16U)

Definition at line 7700 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT

#define CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_MASK)

Definition at line 7680 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_MASK (0x2U)

Definition at line 7678 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_USB2_TOG_DIV_SELECT_SHIFT (1U)

Definition at line 7679 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS

#define CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_MASK)

Definition at line 7683 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_MASK

#define CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_MASK (0x40U)

Definition at line 7681 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_SHIFT

#define CCM_ANALOG_PLL_USB2_TOG_EN_USB_CLKS_SHIFT (6U)

Definition at line 7682 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_ENABLE

#define CCM_ANALOG_PLL_USB2_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_ENABLE_MASK)

Definition at line 7689 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_ENABLE_MASK

#define CCM_ANALOG_PLL_USB2_TOG_ENABLE_MASK (0x2000U)

Definition at line 7687 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_ENABLE_SHIFT

#define CCM_ANALOG_PLL_USB2_TOG_ENABLE_SHIFT (13U)

Definition at line 7688 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_LOCK

#define CCM_ANALOG_PLL_USB2_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_LOCK_MASK)

Definition at line 7704 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_LOCK_MASK

#define CCM_ANALOG_PLL_USB2_TOG_LOCK_MASK (0x80000000U)

Definition at line 7702 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_LOCK_SHIFT

#define CCM_ANALOG_PLL_USB2_TOG_LOCK_SHIFT (31U)

Definition at line 7703 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_POWER

#define CCM_ANALOG_PLL_USB2_TOG_POWER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_USB2_TOG_POWER_SHIFT)) & CCM_ANALOG_PLL_USB2_TOG_POWER_MASK)

Definition at line 7686 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_POWER_MASK

#define CCM_ANALOG_PLL_USB2_TOG_POWER_MASK (0x1000U)

Definition at line 7684 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_USB2_TOG_POWER_SHIFT

#define CCM_ANALOG_PLL_USB2_TOG_POWER_SHIFT (12U)

Definition at line 7685 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_BYPASS

#define CCM_ANALOG_PLL_VIDEO_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_BYPASS_MASK)

Definition at line 8026 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8023 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8015 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_VIDEO_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8016 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_BYPASS_MASK

#define CCM_ANALOG_PLL_VIDEO_BYPASS_MASK (0x10000U)

Definition at line 8024 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_BYPASS_SHIFT

#define CCM_ANALOG_PLL_VIDEO_BYPASS_SHIFT (16U)

Definition at line 8025 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_BYPASS

#define CCM_ANALOG_PLL_VIDEO_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_MASK)

Definition at line 8100 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8097 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8089 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8090 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_MASK

#define CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_MASK (0x10000U)

Definition at line 8098 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_SHIFT

#define CCM_ANALOG_PLL_VIDEO_CLR_BYPASS_SHIFT (16U)

Definition at line 8099 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_MASK)

Definition at line 8082 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_MASK (0x7FU)

Definition at line 8080 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_CLR_DIV_SELECT_SHIFT (0U)

Definition at line 8081 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_ENABLE

#define CCM_ANALOG_PLL_VIDEO_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_MASK)

Definition at line 8088 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_MASK

#define CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_MASK (0x2000U)

Definition at line 8086 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_SHIFT

#define CCM_ANALOG_PLL_VIDEO_CLR_ENABLE_SHIFT (13U)

Definition at line 8087 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_LOCK

#define CCM_ANALOG_PLL_VIDEO_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_LOCK_MASK)

Definition at line 8112 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_LOCK_MASK

#define CCM_ANALOG_PLL_VIDEO_CLR_LOCK_MASK (0x80000000U)

Definition at line 8110 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_LOCK_SHIFT

#define CCM_ANALOG_PLL_VIDEO_CLR_LOCK_SHIFT (31U)

Definition at line 8111 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 8109 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 8101 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_CLR_POST_DIV_SELECT_SHIFT (19U)

Definition at line 8102 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN

#define CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_MASK)

Definition at line 8085 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_MASK

#define CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_MASK (0x1000U)

Definition at line 8083 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_VIDEO_CLR_POWERDOWN_SHIFT (12U)

Definition at line 8084 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_DENOM_B

#define CCM_ANALOG_PLL_VIDEO_DENOM_B | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_DENOM_B_SHIFT)) & CCM_ANALOG_PLL_VIDEO_DENOM_B_MASK)

Definition at line 8163 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_DENOM_B_MASK

#define CCM_ANALOG_PLL_VIDEO_DENOM_B_MASK (0x3FFFFFFFU)

Definition at line 8161 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_DENOM_B_SHIFT

#define CCM_ANALOG_PLL_VIDEO_DENOM_B_SHIFT (0U)

Definition at line 8162 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_DIV_SELECT_MASK)

Definition at line 8008 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_DIV_SELECT_MASK (0x7FU)

Definition at line 8006 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_DIV_SELECT_SHIFT (0U)

Definition at line 8007 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_ENABLE

#define CCM_ANALOG_PLL_VIDEO_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_ENABLE_MASK)

Definition at line 8014 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_ENABLE_MASK

#define CCM_ANALOG_PLL_VIDEO_ENABLE_MASK (0x2000U)

Definition at line 8012 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_ENABLE_SHIFT

#define CCM_ANALOG_PLL_VIDEO_ENABLE_SHIFT (13U)

Definition at line 8013 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_LOCK

#define CCM_ANALOG_PLL_VIDEO_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_LOCK_MASK)

Definition at line 8038 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_LOCK_MASK

#define CCM_ANALOG_PLL_VIDEO_LOCK_MASK (0x80000000U)

Definition at line 8036 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_LOCK_SHIFT

#define CCM_ANALOG_PLL_VIDEO_LOCK_SHIFT (31U)

Definition at line 8037 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_NUM_A

#define CCM_ANALOG_PLL_VIDEO_NUM_A | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_NUM_A_SHIFT)) & CCM_ANALOG_PLL_VIDEO_NUM_A_MASK)

Definition at line 8156 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_NUM_A_MASK

#define CCM_ANALOG_PLL_VIDEO_NUM_A_MASK (0x3FFFFFFFU)

Definition at line 8154 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_NUM_A_SHIFT

#define CCM_ANALOG_PLL_VIDEO_NUM_A_SHIFT (0U)

Definition at line 8155 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 8035 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 8027 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_POST_DIV_SELECT_SHIFT (19U)

Definition at line 8028 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_POWERDOWN

#define CCM_ANALOG_PLL_VIDEO_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_POWERDOWN_MASK)

Definition at line 8011 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_POWERDOWN_MASK

#define CCM_ANALOG_PLL_VIDEO_POWERDOWN_MASK (0x1000U)

Definition at line 8009 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_VIDEO_POWERDOWN_SHIFT (12U)

Definition at line 8010 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_BYPASS

#define CCM_ANALOG_PLL_VIDEO_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_BYPASS_MASK)

Definition at line 8063 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8060 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8052 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_VIDEO_SET_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8053 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_BYPASS_MASK

#define CCM_ANALOG_PLL_VIDEO_SET_BYPASS_MASK (0x10000U)

Definition at line 8061 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_BYPASS_SHIFT

#define CCM_ANALOG_PLL_VIDEO_SET_BYPASS_SHIFT (16U)

Definition at line 8062 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_MASK)

Definition at line 8045 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_MASK (0x7FU)

Definition at line 8043 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_SET_DIV_SELECT_SHIFT (0U)

Definition at line 8044 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_ENABLE

#define CCM_ANALOG_PLL_VIDEO_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_ENABLE_MASK)

Definition at line 8051 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_ENABLE_MASK

#define CCM_ANALOG_PLL_VIDEO_SET_ENABLE_MASK (0x2000U)

Definition at line 8049 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_ENABLE_SHIFT

#define CCM_ANALOG_PLL_VIDEO_SET_ENABLE_SHIFT (13U)

Definition at line 8050 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_LOCK

#define CCM_ANALOG_PLL_VIDEO_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_LOCK_MASK)

Definition at line 8075 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_LOCK_MASK

#define CCM_ANALOG_PLL_VIDEO_SET_LOCK_MASK (0x80000000U)

Definition at line 8073 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_LOCK_SHIFT

#define CCM_ANALOG_PLL_VIDEO_SET_LOCK_SHIFT (31U)

Definition at line 8074 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 8072 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 8064 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_SET_POST_DIV_SELECT_SHIFT (19U)

Definition at line 8065 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN

#define CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_MASK)

Definition at line 8048 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_MASK

#define CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_MASK (0x1000U)

Definition at line 8046 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_VIDEO_SET_POWERDOWN_SHIFT (12U)

Definition at line 8047 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_BYPASS

#define CCM_ANALOG_PLL_VIDEO_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_MASK)

Definition at line 8137 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC

#define CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_MASK)

BYPASS_CLK_SRC 0b00..Select the 24MHz oscillator as source. 0b01..Select the CLK1_N / CLK1_P as source. 0b10..Reserved1 0b11..Reserved2

Definition at line 8134 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_MASK

#define CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_MASK (0xC000U)

Definition at line 8126 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_SHIFT

#define CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_CLK_SRC_SHIFT (14U)

Definition at line 8127 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_MASK

#define CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_MASK (0x10000U)

Definition at line 8135 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_SHIFT

#define CCM_ANALOG_PLL_VIDEO_TOG_BYPASS_SHIFT (16U)

Definition at line 8136 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_MASK)

Definition at line 8119 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_MASK (0x7FU)

Definition at line 8117 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_TOG_DIV_SELECT_SHIFT (0U)

Definition at line 8118 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_ENABLE

#define CCM_ANALOG_PLL_VIDEO_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_MASK)

Definition at line 8125 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_MASK

#define CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_MASK (0x2000U)

Definition at line 8123 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_SHIFT

#define CCM_ANALOG_PLL_VIDEO_TOG_ENABLE_SHIFT (13U)

Definition at line 8124 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_LOCK

#define CCM_ANALOG_PLL_VIDEO_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_LOCK_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_LOCK_MASK)

Definition at line 8149 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_LOCK_MASK

#define CCM_ANALOG_PLL_VIDEO_TOG_LOCK_MASK (0x80000000U)

Definition at line 8147 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_LOCK_SHIFT

#define CCM_ANALOG_PLL_VIDEO_TOG_LOCK_SHIFT (31U)

Definition at line 8148 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT

#define CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_MASK)

POST_DIV_SELECT 0b00..Divide by 4. 0b01..Divide by 2. 0b10..Divide by 1. 0b11..Reserved

Definition at line 8146 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_MASK

#define CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_MASK (0x180000U)

Definition at line 8138 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_SHIFT

#define CCM_ANALOG_PLL_VIDEO_TOG_POST_DIV_SELECT_SHIFT (19U)

Definition at line 8139 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN

#define CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_SHIFT)) & CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_MASK)

Definition at line 8122 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_MASK

#define CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_MASK (0x1000U)

Definition at line 8120 of file MIMXRT1062.h.

## ◆ CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_SHIFT

#define CCM_ANALOG_PLL_VIDEO_TOG_POWERDOWN_SHIFT (12U)

Definition at line 8121 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLKGATE_CTRL

#define PMU_MISC0_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 31946 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLKGATE_CTRL_MASK

#define PMU_MISC0_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 31940 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLKGATE_CTRL_SHIFT

#define PMU_MISC0_CLKGATE_CTRL_SHIFT (25U)

Definition at line 31941 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLKGATE_DELAY

#define PMU_MISC0_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 31959 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLKGATE_DELAY_MASK

#define PMU_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 31947 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLKGATE_DELAY_SHIFT

#define PMU_MISC0_CLKGATE_DELAY_SHIFT (26U)

Definition at line 31948 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_CLKGATE_CTRL

#define PMU_MISC0_CLR_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_CLR_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 32142 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_CLKGATE_CTRL_MASK

#define PMU_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 32136 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_CLKGATE_CTRL_SHIFT

#define PMU_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)

Definition at line 32137 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_CLKGATE_DELAY

#define PMU_MISC0_CLR_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_CLR_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 32155 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_CLKGATE_DELAY_MASK

#define PMU_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 32143 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_CLKGATE_DELAY_SHIFT

#define PMU_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)

Definition at line 32144 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_DISCON_HIGH_SNVS

#define PMU_MISC0_CLR_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_CLR_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 32120 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_DISCON_HIGH_SNVS_MASK

#define PMU_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 32114 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT

#define PMU_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 32115 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_I

#define PMU_MISC0_CLR_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_OSC_I_SHIFT)) & PMU_MISC0_CLR_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 32129 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_I_MASK

#define PMU_MISC0_CLR_OSC_I_MASK (0x6000U)

Definition at line 32121 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_I_SHIFT

#define PMU_MISC0_CLR_OSC_I_SHIFT (13U)

Definition at line 32122 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_XTALOK

#define PMU_MISC0_CLR_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_OSC_XTALOK_SHIFT)) & PMU_MISC0_CLR_OSC_XTALOK_MASK)

Definition at line 32132 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_XTALOK_EN

#define PMU_MISC0_CLR_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_CLR_OSC_XTALOK_EN_MASK)

Definition at line 32135 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_XTALOK_EN_MASK

#define PMU_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 32133 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_XTALOK_EN_SHIFT

#define PMU_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 32134 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_XTALOK_MASK

#define PMU_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)

Definition at line 32130 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_OSC_XTALOK_SHIFT

#define PMU_MISC0_CLR_OSC_XTALOK_SHIFT (15U)

Definition at line 32131 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_PWD

#define PMU_MISC0_CLR_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_PWD_SHIFT)) & PMU_MISC0_CLR_REFTOP_PWD_MASK)

Definition at line 32081 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_PWD_MASK

#define PMU_MISC0_CLR_REFTOP_PWD_MASK (0x1U)

Definition at line 32079 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_PWD_SHIFT

#define PMU_MISC0_CLR_REFTOP_PWD_SHIFT (0U)

Definition at line 32080 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_SELFBIASOFF

#define PMU_MISC0_CLR_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 32088 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_SELFBIASOFF_MASK

#define PMU_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 32082 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT

#define PMU_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 32083 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_VBGADJ

#define PMU_MISC0_CLR_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_CLR_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 32101 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_VBGADJ_MASK

#define PMU_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 32089 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_VBGADJ_SHIFT

#define PMU_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 32090 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_VBGUP

#define PMU_MISC0_CLR_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_CLR_REFTOP_VBGUP_MASK)

Definition at line 32104 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_VBGUP_MASK

#define PMU_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)

Definition at line 32102 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_REFTOP_VBGUP_SHIFT

#define PMU_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)

Definition at line 32103 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_RTC_XTAL_SOURCE

#define PMU_MISC0_CLR_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_CLR_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 32162 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_RTC_XTAL_SOURCE_MASK

#define PMU_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 32156 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT

#define PMU_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 32157 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_STOP_MODE_CONFIG

#define PMU_MISC0_CLR_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_CLR_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..SUSPEND (DSM) 0b01..Analog regulators are ON. 0b10..STOP (lower power) 0b11..STOP (very lower power)

Definition at line 32113 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_STOP_MODE_CONFIG_MASK

#define PMU_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 32105 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_STOP_MODE_CONFIG_SHIFT

#define PMU_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 32106 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_VID_PLL_PREDIV

#define PMU_MISC0_CLR_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_CLR_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 32172 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_VID_PLL_PREDIV_MASK

#define PMU_MISC0_CLR_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 32166 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_VID_PLL_PREDIV_SHIFT

#define PMU_MISC0_CLR_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 32167 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_XTAL_24M_PWD

#define PMU_MISC0_CLR_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_CLR_XTAL_24M_PWD_MASK)

Definition at line 32165 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_XTAL_24M_PWD_MASK

#define PMU_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 32163 of file MIMXRT1062.h.

## ◆ PMU_MISC0_CLR_XTAL_24M_PWD_SHIFT

#define PMU_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)

Definition at line 32164 of file MIMXRT1062.h.

## ◆ PMU_MISC0_DISCON_HIGH_SNVS

#define PMU_MISC0_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 31924 of file MIMXRT1062.h.

## ◆ PMU_MISC0_DISCON_HIGH_SNVS_MASK

#define PMU_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 31918 of file MIMXRT1062.h.

## ◆ PMU_MISC0_DISCON_HIGH_SNVS_SHIFT

#define PMU_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 31919 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_I

#define PMU_MISC0_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_OSC_I_SHIFT)) & PMU_MISC0_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 31933 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_I_MASK

#define PMU_MISC0_OSC_I_MASK (0x6000U)

Definition at line 31925 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_I_SHIFT

#define PMU_MISC0_OSC_I_SHIFT (13U)

Definition at line 31926 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_XTALOK

#define PMU_MISC0_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_OSC_XTALOK_SHIFT)) & PMU_MISC0_OSC_XTALOK_MASK)

Definition at line 31936 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_XTALOK_EN

#define PMU_MISC0_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_OSC_XTALOK_EN_MASK)

Definition at line 31939 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_XTALOK_EN_MASK

#define PMU_MISC0_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 31937 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_XTALOK_EN_SHIFT

#define PMU_MISC0_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 31938 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_XTALOK_MASK

#define PMU_MISC0_OSC_XTALOK_MASK (0x8000U)

Definition at line 31934 of file MIMXRT1062.h.

## ◆ PMU_MISC0_OSC_XTALOK_SHIFT

#define PMU_MISC0_OSC_XTALOK_SHIFT (15U)

Definition at line 31935 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_PWD

#define PMU_MISC0_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_PWD_SHIFT)) & PMU_MISC0_REFTOP_PWD_MASK)

Definition at line 31885 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_PWD_MASK

#define PMU_MISC0_REFTOP_PWD_MASK (0x1U)

Definition at line 31883 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_PWD_SHIFT

#define PMU_MISC0_REFTOP_PWD_SHIFT (0U)

Definition at line 31884 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_SELFBIASOFF

#define PMU_MISC0_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 31892 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_SELFBIASOFF_MASK

#define PMU_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 31886 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_SELFBIASOFF_SHIFT

#define PMU_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 31887 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_VBGADJ

#define PMU_MISC0_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 31905 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_VBGADJ_MASK

#define PMU_MISC0_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 31893 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_VBGADJ_SHIFT

#define PMU_MISC0_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 31894 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_VBGUP

#define PMU_MISC0_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_REFTOP_VBGUP_MASK)

Definition at line 31908 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_VBGUP_MASK

#define PMU_MISC0_REFTOP_VBGUP_MASK (0x80U)

Definition at line 31906 of file MIMXRT1062.h.

## ◆ PMU_MISC0_REFTOP_VBGUP_SHIFT

#define PMU_MISC0_REFTOP_VBGUP_SHIFT (7U)

Definition at line 31907 of file MIMXRT1062.h.

## ◆ PMU_MISC0_RTC_XTAL_SOURCE

#define PMU_MISC0_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 31966 of file MIMXRT1062.h.

## ◆ PMU_MISC0_RTC_XTAL_SOURCE_MASK

#define PMU_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 31960 of file MIMXRT1062.h.

## ◆ PMU_MISC0_RTC_XTAL_SOURCE_SHIFT

#define PMU_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 31961 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_CLKGATE_CTRL

#define PMU_MISC0_SET_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_SET_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 32044 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_CLKGATE_CTRL_MASK

#define PMU_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 32038 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_CLKGATE_CTRL_SHIFT

#define PMU_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)

Definition at line 32039 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_CLKGATE_DELAY

#define PMU_MISC0_SET_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_SET_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 32057 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_CLKGATE_DELAY_MASK

#define PMU_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 32045 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_CLKGATE_DELAY_SHIFT

#define PMU_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)

Definition at line 32046 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_DISCON_HIGH_SNVS

#define PMU_MISC0_SET_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_SET_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 32022 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_DISCON_HIGH_SNVS_MASK

#define PMU_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 32016 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_DISCON_HIGH_SNVS_SHIFT

#define PMU_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 32017 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_I

#define PMU_MISC0_SET_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_OSC_I_SHIFT)) & PMU_MISC0_SET_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 32031 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_I_MASK

#define PMU_MISC0_SET_OSC_I_MASK (0x6000U)

Definition at line 32023 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_I_SHIFT

#define PMU_MISC0_SET_OSC_I_SHIFT (13U)

Definition at line 32024 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_XTALOK

#define PMU_MISC0_SET_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_OSC_XTALOK_SHIFT)) & PMU_MISC0_SET_OSC_XTALOK_MASK)

Definition at line 32034 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_XTALOK_EN

#define PMU_MISC0_SET_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_SET_OSC_XTALOK_EN_MASK)

Definition at line 32037 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_XTALOK_EN_MASK

#define PMU_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 32035 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_XTALOK_EN_SHIFT

#define PMU_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 32036 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_XTALOK_MASK

#define PMU_MISC0_SET_OSC_XTALOK_MASK (0x8000U)

Definition at line 32032 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_OSC_XTALOK_SHIFT

#define PMU_MISC0_SET_OSC_XTALOK_SHIFT (15U)

Definition at line 32033 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_PWD

#define PMU_MISC0_SET_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_PWD_SHIFT)) & PMU_MISC0_SET_REFTOP_PWD_MASK)

Definition at line 31983 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_PWD_MASK

#define PMU_MISC0_SET_REFTOP_PWD_MASK (0x1U)

Definition at line 31981 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_PWD_SHIFT

#define PMU_MISC0_SET_REFTOP_PWD_SHIFT (0U)

Definition at line 31982 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_SELFBIASOFF

#define PMU_MISC0_SET_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_SET_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 31990 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_SELFBIASOFF_MASK

#define PMU_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 31984 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT

#define PMU_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 31985 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_VBGADJ

#define PMU_MISC0_SET_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_SET_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 32003 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_VBGADJ_MASK

#define PMU_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 31991 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_VBGADJ_SHIFT

#define PMU_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 31992 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_VBGUP

#define PMU_MISC0_SET_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_SET_REFTOP_VBGUP_MASK)

Definition at line 32006 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_VBGUP_MASK

#define PMU_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)

Definition at line 32004 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_REFTOP_VBGUP_SHIFT

#define PMU_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)

Definition at line 32005 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_RTC_XTAL_SOURCE

#define PMU_MISC0_SET_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_SET_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 32064 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_RTC_XTAL_SOURCE_MASK

#define PMU_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 32058 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_RTC_XTAL_SOURCE_SHIFT

#define PMU_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 32059 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_STOP_MODE_CONFIG

#define PMU_MISC0_SET_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_SET_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..SUSPEND (DSM) 0b01..Analog regulators are ON. 0b10..STOP (lower power) 0b11..STOP (very lower power)

Definition at line 32015 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_STOP_MODE_CONFIG_MASK

#define PMU_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 32007 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_STOP_MODE_CONFIG_SHIFT

#define PMU_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 32008 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_VID_PLL_PREDIV

#define PMU_MISC0_SET_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_SET_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 32074 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_VID_PLL_PREDIV_MASK

#define PMU_MISC0_SET_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 32068 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_VID_PLL_PREDIV_SHIFT

#define PMU_MISC0_SET_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 32069 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_XTAL_24M_PWD

#define PMU_MISC0_SET_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_SET_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_SET_XTAL_24M_PWD_MASK)

Definition at line 32067 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_XTAL_24M_PWD_MASK

#define PMU_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 32065 of file MIMXRT1062.h.

## ◆ PMU_MISC0_SET_XTAL_24M_PWD_SHIFT

#define PMU_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)

Definition at line 32066 of file MIMXRT1062.h.

## ◆ PMU_MISC0_STOP_MODE_CONFIG

#define PMU_MISC0_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..SUSPEND (DSM) 0b01..Analog regulators are ON. 0b10..STOP (lower power) 0b11..STOP (very lower power)

Definition at line 31917 of file MIMXRT1062.h.

## ◆ PMU_MISC0_STOP_MODE_CONFIG_MASK

#define PMU_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 31909 of file MIMXRT1062.h.

## ◆ PMU_MISC0_STOP_MODE_CONFIG_SHIFT

#define PMU_MISC0_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 31910 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_CLKGATE_CTRL

#define PMU_MISC0_TOG_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & PMU_MISC0_TOG_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 32240 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_CLKGATE_CTRL_MASK

#define PMU_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 32234 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_CLKGATE_CTRL_SHIFT

#define PMU_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)

Definition at line 32235 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_CLKGATE_DELAY

#define PMU_MISC0_TOG_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & PMU_MISC0_TOG_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 32253 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_CLKGATE_DELAY_MASK

#define PMU_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 32241 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_CLKGATE_DELAY_SHIFT

#define PMU_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)

Definition at line 32242 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_DISCON_HIGH_SNVS

#define PMU_MISC0_TOG_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & PMU_MISC0_TOG_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 32218 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_DISCON_HIGH_SNVS_MASK

#define PMU_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 32212 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT

#define PMU_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 32213 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_I

#define PMU_MISC0_TOG_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_OSC_I_SHIFT)) & PMU_MISC0_TOG_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 32227 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_I_MASK

#define PMU_MISC0_TOG_OSC_I_MASK (0x6000U)

Definition at line 32219 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_I_SHIFT

#define PMU_MISC0_TOG_OSC_I_SHIFT (13U)

Definition at line 32220 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_XTALOK

#define PMU_MISC0_TOG_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_OSC_XTALOK_SHIFT)) & PMU_MISC0_TOG_OSC_XTALOK_MASK)

Definition at line 32230 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_XTALOK_EN

#define PMU_MISC0_TOG_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & PMU_MISC0_TOG_OSC_XTALOK_EN_MASK)

Definition at line 32233 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_XTALOK_EN_MASK

#define PMU_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 32231 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_XTALOK_EN_SHIFT

#define PMU_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 32232 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_XTALOK_MASK

#define PMU_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)

Definition at line 32228 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_OSC_XTALOK_SHIFT

#define PMU_MISC0_TOG_OSC_XTALOK_SHIFT (15U)

Definition at line 32229 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_PWD

#define PMU_MISC0_TOG_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_PWD_SHIFT)) & PMU_MISC0_TOG_REFTOP_PWD_MASK)

Definition at line 32179 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_PWD_MASK

#define PMU_MISC0_TOG_REFTOP_PWD_MASK (0x1U)

Definition at line 32177 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_PWD_SHIFT

#define PMU_MISC0_TOG_REFTOP_PWD_SHIFT (0U)

Definition at line 32178 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_SELFBIASOFF

#define PMU_MISC0_TOG_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & PMU_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 32186 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_SELFBIASOFF_MASK

#define PMU_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 32180 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT

#define PMU_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 32181 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_VBGADJ

#define PMU_MISC0_TOG_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & PMU_MISC0_TOG_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 32199 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_VBGADJ_MASK

#define PMU_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 32187 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_VBGADJ_SHIFT

#define PMU_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 32188 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_VBGUP

#define PMU_MISC0_TOG_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & PMU_MISC0_TOG_REFTOP_VBGUP_MASK)

Definition at line 32202 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_VBGUP_MASK

#define PMU_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)

Definition at line 32200 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_REFTOP_VBGUP_SHIFT

#define PMU_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)

Definition at line 32201 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_RTC_XTAL_SOURCE

#define PMU_MISC0_TOG_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & PMU_MISC0_TOG_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 32260 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_RTC_XTAL_SOURCE_MASK

#define PMU_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 32254 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT

#define PMU_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 32255 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_STOP_MODE_CONFIG

#define PMU_MISC0_TOG_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & PMU_MISC0_TOG_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..SUSPEND (DSM) 0b01..Analog regulators are ON. 0b10..STOP (lower power) 0b11..STOP (very lower power)

Definition at line 32211 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_STOP_MODE_CONFIG_MASK

#define PMU_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 32203 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_STOP_MODE_CONFIG_SHIFT

#define PMU_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 32204 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_VID_PLL_PREDIV

#define PMU_MISC0_TOG_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_TOG_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 32270 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_VID_PLL_PREDIV_MASK

#define PMU_MISC0_TOG_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 32264 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_VID_PLL_PREDIV_SHIFT

#define PMU_MISC0_TOG_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 32265 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_XTAL_24M_PWD

#define PMU_MISC0_TOG_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_TOG_XTAL_24M_PWD_MASK)

Definition at line 32263 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_XTAL_24M_PWD_MASK

#define PMU_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 32261 of file MIMXRT1062.h.

## ◆ PMU_MISC0_TOG_XTAL_24M_PWD_SHIFT

#define PMU_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)

Definition at line 32262 of file MIMXRT1062.h.

## ◆ PMU_MISC0_VID_PLL_PREDIV

#define PMU_MISC0_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_VID_PLL_PREDIV_SHIFT)) & PMU_MISC0_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 31976 of file MIMXRT1062.h.

## ◆ PMU_MISC0_VID_PLL_PREDIV_MASK

#define PMU_MISC0_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 31970 of file MIMXRT1062.h.

## ◆ PMU_MISC0_VID_PLL_PREDIV_SHIFT

#define PMU_MISC0_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 31971 of file MIMXRT1062.h.

## ◆ PMU_MISC0_XTAL_24M_PWD

#define PMU_MISC0_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC0_XTAL_24M_PWD_SHIFT)) & PMU_MISC0_XTAL_24M_PWD_MASK)

Definition at line 31969 of file MIMXRT1062.h.

## ◆ PMU_MISC0_XTAL_24M_PWD_MASK

#define PMU_MISC0_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 31967 of file MIMXRT1062.h.

## ◆ PMU_MISC0_XTAL_24M_PWD_SHIFT

#define PMU_MISC0_XTAL_24M_PWD_SHIFT (30U)

Definition at line 31968 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_ANA_BO

#define PMU_MISC1_CLR_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_CLR_IRQ_ANA_BO_MASK)

Definition at line 32519 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_ANA_BO_MASK

#define PMU_MISC1_CLR_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 32517 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_ANA_BO_SHIFT

#define PMU_MISC1_CLR_IRQ_ANA_BO_SHIFT (30U)

Definition at line 32518 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_DIG_BO

#define PMU_MISC1_CLR_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_CLR_IRQ_DIG_BO_MASK)

Definition at line 32522 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_DIG_BO_MASK

#define PMU_MISC1_CLR_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 32520 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_DIG_BO_SHIFT

#define PMU_MISC1_CLR_IRQ_DIG_BO_SHIFT (31U)

Definition at line 32521 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPHIGH

#define PMU_MISC1_CLR_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_CLR_IRQ_TEMPHIGH_MASK)

Definition at line 32516 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPHIGH_MASK

#define PMU_MISC1_CLR_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 32514 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPHIGH_SHIFT

#define PMU_MISC1_CLR_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 32515 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPLOW

#define PMU_MISC1_CLR_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_CLR_IRQ_TEMPLOW_MASK)

Definition at line 32513 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPLOW_MASK

#define PMU_MISC1_CLR_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 32511 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPLOW_SHIFT

#define PMU_MISC1_CLR_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 32512 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPPANIC

#define PMU_MISC1_CLR_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_CLR_IRQ_TEMPPANIC_MASK)

Definition at line 32510 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPPANIC_MASK

#define PMU_MISC1_CLR_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 32508 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_IRQ_TEMPPANIC_SHIFT

#define PMU_MISC1_CLR_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 32509 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDS1_CLK_SEL

#define PMU_MISC1_CLR_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_CLR_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 32463 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDS1_CLK_SEL_MASK

#define PMU_MISC1_CLR_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 32443 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDS1_CLK_SEL_SHIFT

#define PMU_MISC1_CLR_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 32444 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDS2_CLK_SEL

#define PMU_MISC1_CLR_LVDS2_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_CLR_LVDS2_CLK_SEL_MASK)

LVDS2_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01000..MLB PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01010..PCIe ref clock (125M) 0b01011..SATA ref clock (100M) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M) 0b10011..LVDS1 (loopback) 0b10100..LVDS2 (not useful)

Definition at line 32489 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDS2_CLK_SEL_MASK

#define PMU_MISC1_CLR_LVDS2_CLK_SEL_MASK (0x3E0U)

Definition at line 32464 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDS2_CLK_SEL_SHIFT

#define PMU_MISC1_CLR_LVDS2_CLK_SEL_SHIFT (5U)

Definition at line 32465 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK1_IBEN

#define PMU_MISC1_CLR_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK1_IBEN_MASK)

Definition at line 32498 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK1_IBEN_MASK

#define PMU_MISC1_CLR_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 32496 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK1_IBEN_SHIFT

#define PMU_MISC1_CLR_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 32497 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK1_OBEN

#define PMU_MISC1_CLR_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK1_OBEN_MASK)

Definition at line 32492 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK1_OBEN_MASK

#define PMU_MISC1_CLR_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 32490 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK1_OBEN_SHIFT

#define PMU_MISC1_CLR_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 32491 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK2_IBEN

#define PMU_MISC1_CLR_LVDSCLK2_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK2_IBEN_MASK)

Definition at line 32501 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK2_IBEN_MASK

#define PMU_MISC1_CLR_LVDSCLK2_IBEN_MASK (0x2000U)

Definition at line 32499 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK2_IBEN_SHIFT

#define PMU_MISC1_CLR_LVDSCLK2_IBEN_SHIFT (13U)

Definition at line 32500 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK2_OBEN

#define PMU_MISC1_CLR_LVDSCLK2_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_CLR_LVDSCLK2_OBEN_MASK)

Definition at line 32495 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK2_OBEN_MASK

#define PMU_MISC1_CLR_LVDSCLK2_OBEN_MASK (0x800U)

Definition at line 32493 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_LVDSCLK2_OBEN_SHIFT

#define PMU_MISC1_CLR_LVDSCLK2_OBEN_SHIFT (11U)

Definition at line 32494 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_PFD_480_AUTOGATE_EN

#define PMU_MISC1_CLR_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK)

Definition at line 32504 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK

#define PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 32502 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT

#define PMU_MISC1_CLR_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 32503 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_PFD_528_AUTOGATE_EN

#define PMU_MISC1_CLR_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK)

Definition at line 32507 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK

#define PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 32505 of file MIMXRT1062.h.

## ◆ PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT

#define PMU_MISC1_CLR_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 32506 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_ANA_BO

#define PMU_MISC1_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_IRQ_ANA_BO_MASK)

Definition at line 32351 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_ANA_BO_MASK

#define PMU_MISC1_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 32349 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_ANA_BO_SHIFT

#define PMU_MISC1_IRQ_ANA_BO_SHIFT (30U)

Definition at line 32350 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_DIG_BO

#define PMU_MISC1_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_IRQ_DIG_BO_MASK)

Definition at line 32354 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_DIG_BO_MASK

#define PMU_MISC1_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 32352 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_DIG_BO_SHIFT

#define PMU_MISC1_IRQ_DIG_BO_SHIFT (31U)

Definition at line 32353 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPHIGH

#define PMU_MISC1_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_IRQ_TEMPHIGH_MASK)

Definition at line 32348 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPHIGH_MASK

#define PMU_MISC1_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 32346 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPHIGH_SHIFT

#define PMU_MISC1_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 32347 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPLOW

#define PMU_MISC1_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_IRQ_TEMPLOW_MASK)

Definition at line 32345 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPLOW_MASK

#define PMU_MISC1_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 32343 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPLOW_SHIFT

#define PMU_MISC1_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 32344 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPPANIC

#define PMU_MISC1_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_IRQ_TEMPPANIC_MASK)

Definition at line 32342 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPPANIC_MASK

#define PMU_MISC1_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 32340 of file MIMXRT1062.h.

## ◆ PMU_MISC1_IRQ_TEMPPANIC_SHIFT

#define PMU_MISC1_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 32341 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDS1_CLK_SEL

#define PMU_MISC1_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 32295 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDS1_CLK_SEL_MASK

#define PMU_MISC1_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 32275 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDS1_CLK_SEL_SHIFT

#define PMU_MISC1_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 32276 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDS2_CLK_SEL

#define PMU_MISC1_LVDS2_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_LVDS2_CLK_SEL_MASK)

LVDS2_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01000..MLB PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01010..PCIe ref clock (125M) 0b01011..SATA ref clock (100M) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M) 0b10011..LVDS1 (loopback) 0b10100..LVDS2 (not useful)

Definition at line 32321 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDS2_CLK_SEL_MASK

#define PMU_MISC1_LVDS2_CLK_SEL_MASK (0x3E0U)

Definition at line 32296 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDS2_CLK_SEL_SHIFT

#define PMU_MISC1_LVDS2_CLK_SEL_SHIFT (5U)

Definition at line 32297 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK1_IBEN

#define PMU_MISC1_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_LVDSCLK1_IBEN_MASK)

Definition at line 32330 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK1_IBEN_MASK

#define PMU_MISC1_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 32328 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK1_IBEN_SHIFT

#define PMU_MISC1_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 32329 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK1_OBEN

#define PMU_MISC1_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_LVDSCLK1_OBEN_MASK)

Definition at line 32324 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK1_OBEN_MASK

#define PMU_MISC1_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 32322 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK1_OBEN_SHIFT

#define PMU_MISC1_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 32323 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK2_IBEN

#define PMU_MISC1_LVDSCLK2_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_LVDSCLK2_IBEN_MASK)

Definition at line 32333 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK2_IBEN_MASK

#define PMU_MISC1_LVDSCLK2_IBEN_MASK (0x2000U)

Definition at line 32331 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK2_IBEN_SHIFT

#define PMU_MISC1_LVDSCLK2_IBEN_SHIFT (13U)

Definition at line 32332 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK2_OBEN

#define PMU_MISC1_LVDSCLK2_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_LVDSCLK2_OBEN_MASK)

Definition at line 32327 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK2_OBEN_MASK

#define PMU_MISC1_LVDSCLK2_OBEN_MASK (0x800U)

Definition at line 32325 of file MIMXRT1062.h.

## ◆ PMU_MISC1_LVDSCLK2_OBEN_SHIFT

#define PMU_MISC1_LVDSCLK2_OBEN_SHIFT (11U)

Definition at line 32326 of file MIMXRT1062.h.

## ◆ PMU_MISC1_PFD_480_AUTOGATE_EN

#define PMU_MISC1_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_PFD_480_AUTOGATE_EN_MASK)

Definition at line 32336 of file MIMXRT1062.h.

## ◆ PMU_MISC1_PFD_480_AUTOGATE_EN_MASK

#define PMU_MISC1_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 32334 of file MIMXRT1062.h.

## ◆ PMU_MISC1_PFD_480_AUTOGATE_EN_SHIFT

#define PMU_MISC1_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 32335 of file MIMXRT1062.h.

## ◆ PMU_MISC1_PFD_528_AUTOGATE_EN

#define PMU_MISC1_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_PFD_528_AUTOGATE_EN_MASK)

Definition at line 32339 of file MIMXRT1062.h.

## ◆ PMU_MISC1_PFD_528_AUTOGATE_EN_MASK

#define PMU_MISC1_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 32337 of file MIMXRT1062.h.

## ◆ PMU_MISC1_PFD_528_AUTOGATE_EN_SHIFT

#define PMU_MISC1_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 32338 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_ANA_BO

#define PMU_MISC1_SET_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_SET_IRQ_ANA_BO_MASK)

Definition at line 32435 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_ANA_BO_MASK

#define PMU_MISC1_SET_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 32433 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_ANA_BO_SHIFT

#define PMU_MISC1_SET_IRQ_ANA_BO_SHIFT (30U)

Definition at line 32434 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_DIG_BO

#define PMU_MISC1_SET_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_SET_IRQ_DIG_BO_MASK)

Definition at line 32438 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_DIG_BO_MASK

#define PMU_MISC1_SET_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 32436 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_DIG_BO_SHIFT

#define PMU_MISC1_SET_IRQ_DIG_BO_SHIFT (31U)

Definition at line 32437 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPHIGH

#define PMU_MISC1_SET_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_SET_IRQ_TEMPHIGH_MASK)

Definition at line 32432 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPHIGH_MASK

#define PMU_MISC1_SET_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 32430 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPHIGH_SHIFT

#define PMU_MISC1_SET_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 32431 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPLOW

#define PMU_MISC1_SET_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_SET_IRQ_TEMPLOW_MASK)

Definition at line 32429 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPLOW_MASK

#define PMU_MISC1_SET_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 32427 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPLOW_SHIFT

#define PMU_MISC1_SET_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 32428 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPPANIC

#define PMU_MISC1_SET_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_SET_IRQ_TEMPPANIC_MASK)

Definition at line 32426 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPPANIC_MASK

#define PMU_MISC1_SET_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 32424 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_IRQ_TEMPPANIC_SHIFT

#define PMU_MISC1_SET_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 32425 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDS1_CLK_SEL

#define PMU_MISC1_SET_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_SET_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 32379 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDS1_CLK_SEL_MASK

#define PMU_MISC1_SET_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 32359 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDS1_CLK_SEL_SHIFT

#define PMU_MISC1_SET_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 32360 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDS2_CLK_SEL

#define PMU_MISC1_SET_LVDS2_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_SET_LVDS2_CLK_SEL_MASK)

LVDS2_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01000..MLB PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01010..PCIe ref clock (125M) 0b01011..SATA ref clock (100M) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M) 0b10011..LVDS1 (loopback) 0b10100..LVDS2 (not useful)

Definition at line 32405 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDS2_CLK_SEL_MASK

#define PMU_MISC1_SET_LVDS2_CLK_SEL_MASK (0x3E0U)

Definition at line 32380 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDS2_CLK_SEL_SHIFT

#define PMU_MISC1_SET_LVDS2_CLK_SEL_SHIFT (5U)

Definition at line 32381 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK1_IBEN

#define PMU_MISC1_SET_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK1_IBEN_MASK)

Definition at line 32414 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK1_IBEN_MASK

#define PMU_MISC1_SET_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 32412 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK1_IBEN_SHIFT

#define PMU_MISC1_SET_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 32413 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK1_OBEN

#define PMU_MISC1_SET_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK1_OBEN_MASK)

Definition at line 32408 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK1_OBEN_MASK

#define PMU_MISC1_SET_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 32406 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK1_OBEN_SHIFT

#define PMU_MISC1_SET_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 32407 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK2_IBEN

#define PMU_MISC1_SET_LVDSCLK2_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK2_IBEN_MASK)

Definition at line 32417 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK2_IBEN_MASK

#define PMU_MISC1_SET_LVDSCLK2_IBEN_MASK (0x2000U)

Definition at line 32415 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK2_IBEN_SHIFT

#define PMU_MISC1_SET_LVDSCLK2_IBEN_SHIFT (13U)

Definition at line 32416 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK2_OBEN

#define PMU_MISC1_SET_LVDSCLK2_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_SET_LVDSCLK2_OBEN_MASK)

Definition at line 32411 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK2_OBEN_MASK

#define PMU_MISC1_SET_LVDSCLK2_OBEN_MASK (0x800U)

Definition at line 32409 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_LVDSCLK2_OBEN_SHIFT

#define PMU_MISC1_SET_LVDSCLK2_OBEN_SHIFT (11U)

Definition at line 32410 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_PFD_480_AUTOGATE_EN

#define PMU_MISC1_SET_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_SET_PFD_480_AUTOGATE_EN_MASK)

Definition at line 32420 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_PFD_480_AUTOGATE_EN_MASK

#define PMU_MISC1_SET_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 32418 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT

#define PMU_MISC1_SET_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 32419 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_PFD_528_AUTOGATE_EN

#define PMU_MISC1_SET_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_SET_PFD_528_AUTOGATE_EN_MASK)

Definition at line 32423 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_PFD_528_AUTOGATE_EN_MASK

#define PMU_MISC1_SET_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 32421 of file MIMXRT1062.h.

## ◆ PMU_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT

#define PMU_MISC1_SET_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 32422 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_ANA_BO

#define PMU_MISC1_TOG_IRQ_ANA_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_ANA_BO_SHIFT)) & PMU_MISC1_TOG_IRQ_ANA_BO_MASK)

Definition at line 32603 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_ANA_BO_MASK

#define PMU_MISC1_TOG_IRQ_ANA_BO_MASK (0x40000000U)

Definition at line 32601 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_ANA_BO_SHIFT

#define PMU_MISC1_TOG_IRQ_ANA_BO_SHIFT (30U)

Definition at line 32602 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_DIG_BO

#define PMU_MISC1_TOG_IRQ_DIG_BO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_DIG_BO_SHIFT)) & PMU_MISC1_TOG_IRQ_DIG_BO_MASK)

Definition at line 32606 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_DIG_BO_MASK

#define PMU_MISC1_TOG_IRQ_DIG_BO_MASK (0x80000000U)

Definition at line 32604 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_DIG_BO_SHIFT

#define PMU_MISC1_TOG_IRQ_DIG_BO_SHIFT (31U)

Definition at line 32605 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPHIGH

#define PMU_MISC1_TOG_IRQ_TEMPHIGH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_TEMPHIGH_SHIFT)) & PMU_MISC1_TOG_IRQ_TEMPHIGH_MASK)

Definition at line 32600 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPHIGH_MASK

#define PMU_MISC1_TOG_IRQ_TEMPHIGH_MASK (0x20000000U)

Definition at line 32598 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPHIGH_SHIFT

#define PMU_MISC1_TOG_IRQ_TEMPHIGH_SHIFT (29U)

Definition at line 32599 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPLOW

#define PMU_MISC1_TOG_IRQ_TEMPLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_TEMPLOW_SHIFT)) & PMU_MISC1_TOG_IRQ_TEMPLOW_MASK)

Definition at line 32597 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPLOW_MASK

#define PMU_MISC1_TOG_IRQ_TEMPLOW_MASK (0x10000000U)

Definition at line 32595 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPLOW_SHIFT

#define PMU_MISC1_TOG_IRQ_TEMPLOW_SHIFT (28U)

Definition at line 32596 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPPANIC

#define PMU_MISC1_TOG_IRQ_TEMPPANIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_IRQ_TEMPPANIC_SHIFT)) & PMU_MISC1_TOG_IRQ_TEMPPANIC_MASK)

Definition at line 32594 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPPANIC_MASK

#define PMU_MISC1_TOG_IRQ_TEMPPANIC_MASK (0x8000000U)

Definition at line 32592 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_IRQ_TEMPPANIC_SHIFT

#define PMU_MISC1_TOG_IRQ_TEMPPANIC_SHIFT (27U)

Definition at line 32593 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDS1_CLK_SEL

#define PMU_MISC1_TOG_LVDS1_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDS1_CLK_SEL_SHIFT)) & PMU_MISC1_TOG_LVDS1_CLK_SEL_MASK)

LVDS1_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M)

Definition at line 32547 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDS1_CLK_SEL_MASK

#define PMU_MISC1_TOG_LVDS1_CLK_SEL_MASK (0x1FU)

Definition at line 32527 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDS1_CLK_SEL_SHIFT

#define PMU_MISC1_TOG_LVDS1_CLK_SEL_SHIFT (0U)

Definition at line 32528 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDS2_CLK_SEL

#define PMU_MISC1_TOG_LVDS2_CLK_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDS2_CLK_SEL_SHIFT)) & PMU_MISC1_TOG_LVDS2_CLK_SEL_MASK)

LVDS2_CLK_SEL 0b00000..Arm PLL 0b00001..System PLL 0b00010..ref_pfd4_clk == pll2_pfd0_clk 0b00011..ref_pfd5_clk == pll2_pfd1_clk 0b00100..ref_pfd6_clk == pll2_pfd2_clk 0b00101..ref_pfd7_clk == pll2_pfd3_clk 0b00110..Audio PLL 0b00111..Video PLL 0b01000..MLB PLL 0b01001..ethernet ref clock (ENET_PLL) 0b01010..PCIe ref clock (125M) 0b01011..SATA ref clock (100M) 0b01100..USB1 PLL clock 0b01101..USB2 PLL clock 0b01110..ref_pfd0_clk == pll3_pfd0_clk 0b01111..ref_pfd1_clk == pll3_pfd1_clk 0b10000..ref_pfd2_clk == pll3_pfd2_clk 0b10001..ref_pfd3_clk == pll3_pfd3_clk 0b10010..xtal (24M) 0b10011..LVDS1 (loopback) 0b10100..LVDS2 (not useful)

Definition at line 32573 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDS2_CLK_SEL_MASK

#define PMU_MISC1_TOG_LVDS2_CLK_SEL_MASK (0x3E0U)

Definition at line 32548 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDS2_CLK_SEL_SHIFT

#define PMU_MISC1_TOG_LVDS2_CLK_SEL_SHIFT (5U)

Definition at line 32549 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK1_IBEN

#define PMU_MISC1_TOG_LVDSCLK1_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK1_IBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK1_IBEN_MASK)

Definition at line 32582 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK1_IBEN_MASK

#define PMU_MISC1_TOG_LVDSCLK1_IBEN_MASK (0x1000U)

Definition at line 32580 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK1_IBEN_SHIFT

#define PMU_MISC1_TOG_LVDSCLK1_IBEN_SHIFT (12U)

Definition at line 32581 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK1_OBEN

#define PMU_MISC1_TOG_LVDSCLK1_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK1_OBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK1_OBEN_MASK)

Definition at line 32576 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK1_OBEN_MASK

#define PMU_MISC1_TOG_LVDSCLK1_OBEN_MASK (0x400U)

Definition at line 32574 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK1_OBEN_SHIFT

#define PMU_MISC1_TOG_LVDSCLK1_OBEN_SHIFT (10U)

Definition at line 32575 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK2_IBEN

#define PMU_MISC1_TOG_LVDSCLK2_IBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK2_IBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK2_IBEN_MASK)

Definition at line 32585 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK2_IBEN_MASK

#define PMU_MISC1_TOG_LVDSCLK2_IBEN_MASK (0x2000U)

Definition at line 32583 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK2_IBEN_SHIFT

#define PMU_MISC1_TOG_LVDSCLK2_IBEN_SHIFT (13U)

Definition at line 32584 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK2_OBEN

#define PMU_MISC1_TOG_LVDSCLK2_OBEN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_LVDSCLK2_OBEN_SHIFT)) & PMU_MISC1_TOG_LVDSCLK2_OBEN_MASK)

Definition at line 32579 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK2_OBEN_MASK

#define PMU_MISC1_TOG_LVDSCLK2_OBEN_MASK (0x800U)

Definition at line 32577 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_LVDSCLK2_OBEN_SHIFT

#define PMU_MISC1_TOG_LVDSCLK2_OBEN_SHIFT (11U)

Definition at line 32578 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_PFD_480_AUTOGATE_EN

#define PMU_MISC1_TOG_PFD_480_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT)) & PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK)

Definition at line 32588 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK

#define PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_MASK (0x10000U)

Definition at line 32586 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT

#define PMU_MISC1_TOG_PFD_480_AUTOGATE_EN_SHIFT (16U)

Definition at line 32587 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_PFD_528_AUTOGATE_EN

#define PMU_MISC1_TOG_PFD_528_AUTOGATE_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT)) & PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK)

Definition at line 32591 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK

#define PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_MASK (0x20000U)

Definition at line 32589 of file MIMXRT1062.h.

## ◆ PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT

#define PMU_MISC1_TOG_PFD_528_AUTOGATE_EN_SHIFT (17U)

Definition at line 32590 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_CTRL

#define XTALOSC24M_MISC0_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47653 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47647 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47648 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_DELAY

#define XTALOSC24M_MISC0_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47666 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47654 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47655 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_CTRL

#define XTALOSC24M_MISC0_CLR_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47849 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47843 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47844 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_DELAY

#define XTALOSC24M_MISC0_CLR_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47862 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47850 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47851 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47827 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47821 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47822 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_I

#define XTALOSC24M_MISC0_CLR_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_I_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47836 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_I_MASK

#define XTALOSC24M_MISC0_CLR_OSC_I_MASK (0x6000U)

Definition at line 47828 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_I_SHIFT

#define XTALOSC24M_MISC0_CLR_OSC_I_SHIFT (13U)

Definition at line 47829 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK)

Definition at line 47839 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK)

Definition at line 47842 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47840 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47841 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)

Definition at line 47837 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT (15U)

Definition at line 47838 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_PWD

#define XTALOSC24M_MISC0_CLR_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK)

Definition at line 47788 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK (0x1U)

Definition at line 47786 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT (0U)

Definition at line 47787 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47795 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47789 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47790 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47808 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47796 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47797 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGUP

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK)

Definition at line 47811 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47809 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47810 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47869 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47863 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47864 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47820 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47812 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47813 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47879 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47873 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47874 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_XTAL_24M_PWD

#define XTALOSC24M_MISC0_CLR_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK)

Definition at line 47872 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47870 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47871 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47631 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47625 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47626 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_I

#define XTALOSC24M_MISC0_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_I_SHIFT)) & XTALOSC24M_MISC0_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47640 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_I_MASK

#define XTALOSC24M_MISC0_OSC_I_MASK (0x6000U)

Definition at line 47632 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_I_SHIFT

#define XTALOSC24M_MISC0_OSC_I_SHIFT (13U)

Definition at line 47633 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK

#define XTALOSC24M_MISC0_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_MASK)

Definition at line 47643 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK)

Definition at line 47646 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47644 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47645 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_OSC_XTALOK_MASK (0x8000U)

Definition at line 47641 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_OSC_XTALOK_SHIFT (15U)

Definition at line 47642 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_PWD

#define XTALOSC24M_MISC0_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_REFTOP_PWD_MASK)

Definition at line 47592 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_REFTOP_PWD_MASK (0x1U)

Definition at line 47590 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_REFTOP_PWD_SHIFT (0U)

Definition at line 47591 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47599 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47593 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47594 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47612 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47600 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47601 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGUP

#define XTALOSC24M_MISC0_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGUP_MASK)

Definition at line 47615 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47613 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47614 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47673 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47667 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47668 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_CTRL

#define XTALOSC24M_MISC0_SET_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47751 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47745 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47746 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_DELAY

#define XTALOSC24M_MISC0_SET_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47764 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47752 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47753 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47729 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47723 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47724 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_I

#define XTALOSC24M_MISC0_SET_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_I_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47738 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_I_MASK

#define XTALOSC24M_MISC0_SET_OSC_I_MASK (0x6000U)

Definition at line 47730 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_I_SHIFT

#define XTALOSC24M_MISC0_SET_OSC_I_SHIFT (13U)

Definition at line 47731 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK

#define XTALOSC24M_MISC0_SET_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK)

Definition at line 47741 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK)

Definition at line 47744 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47742 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47743 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK (0x8000U)

Definition at line 47739 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT (15U)

Definition at line 47740 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_PWD

#define XTALOSC24M_MISC0_SET_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK)

Definition at line 47690 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK (0x1U)

Definition at line 47688 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT (0U)

Definition at line 47689 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47697 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47691 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47692 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_SET_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47710 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47698 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47699 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGUP

#define XTALOSC24M_MISC0_SET_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK)

Definition at line 47713 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47711 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47712 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47771 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47765 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47766 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47722 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47714 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47715 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_SET_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47781 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47775 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47776 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_XTAL_24M_PWD

#define XTALOSC24M_MISC0_SET_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK)

Definition at line 47774 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47772 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47773 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47624 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47616 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47617 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_CTRL

#define XTALOSC24M_MISC0_TOG_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47947 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47941 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47942 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_DELAY

#define XTALOSC24M_MISC0_TOG_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47960 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47948 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47949 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47925 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47919 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47920 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_I

#define XTALOSC24M_MISC0_TOG_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_I_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47934 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_I_MASK

#define XTALOSC24M_MISC0_TOG_OSC_I_MASK (0x6000U)

Definition at line 47926 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_I_SHIFT

#define XTALOSC24M_MISC0_TOG_OSC_I_SHIFT (13U)

Definition at line 47927 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK)

Definition at line 47937 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK)

Definition at line 47940 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47938 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47939 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)

Definition at line 47935 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT (15U)

Definition at line 47936 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_PWD

#define XTALOSC24M_MISC0_TOG_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK)

Definition at line 47886 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK (0x1U)

Definition at line 47884 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT (0U)

Definition at line 47885 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47893 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47887 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47888 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47906 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47894 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47895 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGUP

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK)

Definition at line 47909 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47907 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47908 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47967 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47961 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47962 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47918 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47910 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47911 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47977 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47971 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47972 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_XTAL_24M_PWD

#define XTALOSC24M_MISC0_TOG_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK)

Definition at line 47970 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47968 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47969 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47683 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47677 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47678 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_XTAL_24M_PWD

#define XTALOSC24M_MISC0_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_XTAL_24M_PWD_MASK)

Definition at line 47676 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47674 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47675 of file MIMXRT1062.h.