Callisto4Bootloader: CMP Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
CMP Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| CMP Register Masks

## Data Structures

struct | CMP_Type

## Macros

#define | CMP1_BASE (0x40094000u)
#define | CMP1 ((CMP_Type *)CMP1_BASE)
#define | CMP2_BASE (0x40094008u)
#define | CMP2 ((CMP_Type *)CMP2_BASE)
#define | CMP3_BASE (0x40094010u)
#define | CMP3 ((CMP_Type *)CMP3_BASE)
#define | CMP4_BASE (0x40094018u)
#define | CMP4 ((CMP_Type *)CMP4_BASE)
#define | CMP_BASE_ADDRS { 0u, CMP1_BASE, CMP2_BASE, CMP3_BASE, CMP4_BASE }
#define | CMP_BASE_PTRS { (CMP_Type *)0u, CMP1, CMP2, CMP3, CMP4 }
#define | CMP_IRQS { NotAvail_IRQn, ACMP1_IRQn, ACMP2_IRQn, ACMP3_IRQn, ACMP4_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ CMP1

#define CMP1 ((CMP_Type *)CMP1_BASE)

Peripheral CMP1 base pointer

Definition at line 9940 of file MIMXRT1062.h.

## ◆ CMP1_BASE

#define CMP1_BASE (0x40094000u)

Peripheral CMP1 base address

Definition at line 9938 of file MIMXRT1062.h.

## ◆ CMP2

#define CMP2 ((CMP_Type *)CMP2_BASE)

Peripheral CMP2 base pointer

Definition at line 9944 of file MIMXRT1062.h.

## ◆ CMP2_BASE

#define CMP2_BASE (0x40094008u)

Peripheral CMP2 base address

Definition at line 9942 of file MIMXRT1062.h.

## ◆ CMP3

#define CMP3 ((CMP_Type *)CMP3_BASE)

Peripheral CMP3 base pointer

Definition at line 9948 of file MIMXRT1062.h.

## ◆ CMP3_BASE

#define CMP3_BASE (0x40094010u)

Peripheral CMP3 base address

Definition at line 9946 of file MIMXRT1062.h.

## ◆ CMP4

#define CMP4 ((CMP_Type *)CMP4_BASE)

Peripheral CMP4 base pointer

Definition at line 9952 of file MIMXRT1062.h.

## ◆ CMP4_BASE

#define CMP4_BASE (0x40094018u)

Peripheral CMP4 base address

Definition at line 9950 of file MIMXRT1062.h.

## ◆ CMP_BASE_ADDRS

#define CMP_BASE_ADDRS { 0u, CMP1_BASE, CMP2_BASE, CMP3_BASE, CMP4_BASE }

Array initializer of CMP peripheral base addresses

Definition at line 9954 of file MIMXRT1062.h.

## ◆ CMP_BASE_PTRS

#define CMP_BASE_PTRS { (CMP_Type *)0u, CMP1, CMP2, CMP3, CMP4 }

Array initializer of CMP peripheral base pointers

Definition at line 9956 of file MIMXRT1062.h.

## ◆ CMP_IRQS

#define CMP_IRQS { NotAvail_IRQn, ACMP1_IRQn, ACMP2_IRQn, ACMP3_IRQn, ACMP4_IRQn }

Interrupt vectors for the CMP peripheral type

Definition at line 9958 of file MIMXRT1062.h.