Callisto4Bootloader: USB_ANALOG_Type Struct Reference

Callisto4Bootloader

Data Fields
USB_ANALOG_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » USB_ANALOG Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

uint8_t | RESERVED_0 [416]
struct {
__IO uint32_t USB_ANALOG_Type::VBUS_DETECT
__IO uint32_t USB_ANALOG_Type::VBUS_DETECT_SET
__IO uint32_t USB_ANALOG_Type::VBUS_DETECT_CLR
__IO uint32_t USB_ANALOG_Type::VBUS_DETECT_TOG
__IO uint32_t USB_ANALOG_Type::CHRG_DETECT
__IO uint32_t USB_ANALOG_Type::CHRG_DETECT_SET
__IO uint32_t USB_ANALOG_Type::CHRG_DETECT_CLR
__IO uint32_t USB_ANALOG_Type::CHRG_DETECT_TOG
__I uint32_t USB_ANALOG_Type::VBUS_DETECT_STAT
uint8_t USB_ANALOG_Type::RESERVED_0 [12]
__I uint32_t USB_ANALOG_Type::CHRG_DETECT_STAT
uint8_t USB_ANALOG_Type::RESERVED_1 [12]
__IO uint32_t USB_ANALOG_Type::LOOPBACK
__IO uint32_t USB_ANALOG_Type::LOOPBACK_SET
__IO uint32_t USB_ANALOG_Type::LOOPBACK_CLR
__IO uint32_t USB_ANALOG_Type::LOOPBACK_TOG
__IO uint32_t USB_ANALOG_Type::MISC
__IO uint32_t USB_ANALOG_Type::MISC_SET
__IO uint32_t USB_ANALOG_Type::MISC_CLR
__IO uint32_t USB_ANALOG_Type::MISC_TOG
} | INSTANCE [2]
__I uint32_t | DIGPROG

## Detailed Description

USB_ANALOG - Register Layout Typedef

Definition at line 44183 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h