Callisto4Bootloader: TPI_Type Struct Reference

Callisto4Bootloader

Data Fields
TPI_Type Struct Reference
Defines and Type Definitions » Status and Control Registers » Nested Vectored Interrupt Controller (NVIC) » System Control Block (SCB) » System Controls not in SCB (SCnSCB) » System Tick Timer (SysTick) » Instrumentation Trace Macrocell (ITM) » Data Watchpoint and Trace (DWT) » Trace Port Interface (TPI)

Structure type to access the Trace Port Interface Register (TPI). More...

`#include <core_armv81mml.h>`

## Data Fields

__IM uint32_t | SSPSR
__IOM uint32_t | CSPSR
uint32_t | RESERVED0 [2U]
__IOM uint32_t | ACPR
uint32_t | RESERVED1 [55U]
__IOM uint32_t | SPPR
uint32_t | RESERVED2 [131U]
__IM uint32_t | FFSR
__IOM uint32_t | FFCR
__IM uint32_t | FSCR
uint32_t | RESERVED3 [759U]
__IM uint32_t | TRIGGER
__IM uint32_t | FIFO0
__IM uint32_t | ITATBCTR2
uint32_t | RESERVED4 [1U]
__IM uint32_t | ITATBCTR0
__IM uint32_t | FIFO1
__IOM uint32_t | ITCTRL
uint32_t | RESERVED5 [39U]
__IOM uint32_t | CLAIMSET
__IOM uint32_t | CLAIMCLR
uint32_t | RESERVED7 [8U]
__IM uint32_t | DEVID
__IM uint32_t | DEVTYPE
__IOM uint32_t | PSCR
__OM uint32_t | LAR
__IM uint32_t | LSR
__IM uint32_t | TYPE

## Detailed Description

Structure type to access the Trace Port Interface Register (TPI).

Definition at line 1387 of file core_armv81mml.h.

The documentation for this struct was generated from the following files:

- CMSIS/core_armv81mml.h
- CMSIS/core_armv8mbl.h
- CMSIS/core_armv8mml.h
- CMSIS/core_cm7.h