Callisto4Bootloader: SPDIF Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
SPDIF Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| SPDIF Register Masks

## Data Structures

struct | SPDIF_Type

## Macros

#define | SPDIF_BASE (0x40380000u)
#define | SPDIF ((SPDIF_Type *)SPDIF_BASE)
#define | SPDIF_BASE_ADDRS { SPDIF_BASE }
#define | SPDIF_BASE_PTRS { SPDIF }
#define | SPDIF_IRQS { SPDIF_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ SPDIF

#define SPDIF ((SPDIF_Type *)SPDIF_BASE)

Peripheral SPDIF base pointer

Definition at line 39263 of file MIMXRT1062.h.

## ◆ SPDIF_BASE

#define SPDIF_BASE (0x40380000u)

Peripheral SPDIF base address

Definition at line 39261 of file MIMXRT1062.h.

## ◆ SPDIF_BASE_ADDRS

#define SPDIF_BASE_ADDRS { SPDIF_BASE }

Array initializer of SPDIF peripheral base addresses

Definition at line 39265 of file MIMXRT1062.h.

## ◆ SPDIF_BASE_PTRS

#define SPDIF_BASE_PTRS { SPDIF }

Array initializer of SPDIF peripheral base pointers

Definition at line 39267 of file MIMXRT1062.h.

## ◆ SPDIF_IRQS

#define SPDIF_IRQS { SPDIF_IRQn }

Interrupt vectors for the SPDIF peripheral type

Definition at line 39269 of file MIMXRT1062.h.