Callisto4Bootloader: DMA Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
DMA Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| DMA Register Masks

## Data Structures

struct | DMA_Type

## Macros

#define | DMA0_BASE (0x400E8000u)
#define | DMA0 ((DMA_Type *)DMA0_BASE)
#define | DMA_BASE_ADDRS { DMA0_BASE }
#define | DMA_BASE_PTRS { DMA0 }
#define | DMA_CHN_IRQS { { DMA0_DMA16_IRQn, DMA1_DMA17_IRQn, DMA2_DMA18_IRQn, DMA3_DMA19_IRQn, DMA4_DMA20_IRQn, DMA5_DMA21_IRQn, DMA6_DMA22_IRQn, DMA7_DMA23_IRQn, DMA8_DMA24_IRQn, DMA9_DMA25_IRQn, DMA10_DMA26_IRQn, DMA11_DMA27_IRQn, DMA12_DMA28_IRQn, DMA13_DMA29_IRQn, DMA14_DMA30_IRQn, DMA15_DMA31_IRQn, DMA0_DMA16_IRQn, DMA1_DMA17_IRQn, DMA2_DMA18_IRQn, DMA3_DMA19_IRQn, DMA4_DMA20_IRQn, DMA5_DMA21_IRQn, DMA6_DMA22_IRQn, DMA7_DMA23_IRQn, DMA8_DMA24_IRQn, DMA9_DMA25_IRQn, DMA10_DMA26_IRQn, DMA11_DMA27_IRQn, DMA12_DMA28_IRQn, DMA13_DMA29_IRQn, DMA14_DMA30_IRQn, DMA15_DMA31_IRQn } }
#define | DMA_ERROR_IRQS { DMA_ERROR_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ DMA0

#define DMA0 ((DMA_Type *)DMA0_BASE)

Peripheral DMA0 base pointer

Definition at line 16220 of file MIMXRT1062.h.

## ◆ DMA0_BASE

#define DMA0_BASE (0x400E8000u)

Peripheral DMA0 base address

Definition at line 16218 of file MIMXRT1062.h.

## ◆ DMA_BASE_ADDRS

#define DMA_BASE_ADDRS { DMA0_BASE }

Array initializer of DMA peripheral base addresses

Definition at line 16222 of file MIMXRT1062.h.

## ◆ DMA_BASE_PTRS

#define DMA_BASE_PTRS { DMA0 }

Array initializer of DMA peripheral base pointers

Definition at line 16224 of file MIMXRT1062.h.

## ◆ DMA_CHN_IRQS

#define DMA_CHN_IRQS { { DMA0_DMA16_IRQn, DMA1_DMA17_IRQn, DMA2_DMA18_IRQn, DMA3_DMA19_IRQn, DMA4_DMA20_IRQn, DMA5_DMA21_IRQn, DMA6_DMA22_IRQn, DMA7_DMA23_IRQn, DMA8_DMA24_IRQn, DMA9_DMA25_IRQn, DMA10_DMA26_IRQn, DMA11_DMA27_IRQn, DMA12_DMA28_IRQn, DMA13_DMA29_IRQn, DMA14_DMA30_IRQn, DMA15_DMA31_IRQn, DMA0_DMA16_IRQn, DMA1_DMA17_IRQn, DMA2_DMA18_IRQn, DMA3_DMA19_IRQn, DMA4_DMA20_IRQn, DMA5_DMA21_IRQn, DMA6_DMA22_IRQn, DMA7_DMA23_IRQn, DMA8_DMA24_IRQn, DMA9_DMA25_IRQn, DMA10_DMA26_IRQn, DMA11_DMA27_IRQn, DMA12_DMA28_IRQn, DMA13_DMA29_IRQn, DMA14_DMA30_IRQn, DMA15_DMA31_IRQn } }

Interrupt vectors for the DMA peripheral type

Definition at line 16226 of file MIMXRT1062.h.

## ◆ DMA_ERROR_IRQS

#define DMA_ERROR_IRQS { DMA_ERROR_IRQn }

Definition at line 16227 of file MIMXRT1062.h.