Callisto4Bootloader: AIPSTZ Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
AIPSTZ Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| AIPSTZ Register Masks

## Data Structures

struct | AIPSTZ_Type

## Macros

#define | AIPSTZ1_BASE (0x4007C000u)
#define | AIPSTZ1 ((AIPSTZ_Type *)AIPSTZ1_BASE)
#define | AIPSTZ2_BASE (0x4017C000u)
#define | AIPSTZ2 ((AIPSTZ_Type *)AIPSTZ2_BASE)
#define | AIPSTZ3_BASE (0x4027C000u)
#define | AIPSTZ3 ((AIPSTZ_Type *)AIPSTZ3_BASE)
#define | AIPSTZ4_BASE (0x4037C000u)
#define | AIPSTZ4 ((AIPSTZ_Type *)AIPSTZ4_BASE)
#define | AIPSTZ_BASE_ADDRS { 0u, AIPSTZ1_BASE, AIPSTZ2_BASE, AIPSTZ3_BASE, AIPSTZ4_BASE }
#define | AIPSTZ_BASE_PTRS { (AIPSTZ_Type *)0u, AIPSTZ1, AIPSTZ2, AIPSTZ3, AIPSTZ4 }

## Detailed Description

## Macro Definition Documentation

## ◆ AIPSTZ1

#define AIPSTZ1 ((AIPSTZ_Type *)AIPSTZ1_BASE)

Peripheral AIPSTZ1 base pointer

Definition at line 2894 of file MIMXRT1062.h.

## ◆ AIPSTZ1_BASE

#define AIPSTZ1_BASE (0x4007C000u)

Peripheral AIPSTZ1 base address

Definition at line 2892 of file MIMXRT1062.h.

## ◆ AIPSTZ2

#define AIPSTZ2 ((AIPSTZ_Type *)AIPSTZ2_BASE)

Peripheral AIPSTZ2 base pointer

Definition at line 2898 of file MIMXRT1062.h.

## ◆ AIPSTZ2_BASE

#define AIPSTZ2_BASE (0x4017C000u)

Peripheral AIPSTZ2 base address

Definition at line 2896 of file MIMXRT1062.h.

## ◆ AIPSTZ3

#define AIPSTZ3 ((AIPSTZ_Type *)AIPSTZ3_BASE)

Peripheral AIPSTZ3 base pointer

Definition at line 2902 of file MIMXRT1062.h.

## ◆ AIPSTZ3_BASE

#define AIPSTZ3_BASE (0x4027C000u)

Peripheral AIPSTZ3 base address

Definition at line 2900 of file MIMXRT1062.h.

## ◆ AIPSTZ4

#define AIPSTZ4 ((AIPSTZ_Type *)AIPSTZ4_BASE)

Peripheral AIPSTZ4 base pointer

Definition at line 2906 of file MIMXRT1062.h.

## ◆ AIPSTZ4_BASE

#define AIPSTZ4_BASE (0x4037C000u)

Peripheral AIPSTZ4 base address

Definition at line 2904 of file MIMXRT1062.h.

## ◆ AIPSTZ_BASE_ADDRS

#define AIPSTZ_BASE_ADDRS { 0u, AIPSTZ1_BASE, AIPSTZ2_BASE, AIPSTZ3_BASE, AIPSTZ4_BASE }

Array initializer of AIPSTZ peripheral base addresses

Definition at line 2908 of file MIMXRT1062.h.

## ◆ AIPSTZ_BASE_PTRS

#define AIPSTZ_BASE_PTRS { (AIPSTZ_Type *)0u, AIPSTZ1, AIPSTZ2, AIPSTZ3, AIPSTZ4 }

Array initializer of AIPSTZ peripheral base pointers

Definition at line 2910 of file MIMXRT1062.h.