Callisto4Bootloader: USB_ANALOG Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
USB_ANALOG Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| USB_ANALOG Register Masks

## Data Structures

struct | USB_ANALOG_Type

## Macros

#define | USB_ANALOG_BASE (0x400D8000u)
#define | USB_ANALOG ((USB_ANALOG_Type *)USB_ANALOG_BASE)
#define | USB_ANALOG_BASE_ADDRS { USB_ANALOG_BASE }
#define | USB_ANALOG_BASE_PTRS { USB_ANALOG }

## Detailed Description

## Macro Definition Documentation

## ◆ USB_ANALOG

#define USB_ANALOG ((USB_ANALOG_Type *)USB_ANALOG_BASE)

Peripheral USB_ANALOG base pointer

Definition at line 44617 of file MIMXRT1062.h.

## ◆ USB_ANALOG_BASE

#define USB_ANALOG_BASE (0x400D8000u)

Peripheral USB_ANALOG base address

Definition at line 44615 of file MIMXRT1062.h.

## ◆ USB_ANALOG_BASE_ADDRS

#define USB_ANALOG_BASE_ADDRS { USB_ANALOG_BASE }

Array initializer of USB_ANALOG peripheral base addresses

Definition at line 44619 of file MIMXRT1062.h.

## ◆ USB_ANALOG_BASE_PTRS

#define USB_ANALOG_BASE_PTRS { USB_ANALOG }

Array initializer of USB_ANALOG peripheral base pointers

Definition at line 44621 of file MIMXRT1062.h.