Callisto4Bootloader: CCM_Type Struct Reference

Callisto4Bootloader

Data Fields
CCM_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » CCM Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | CCR
uint8_t | RESERVED_0 [4]
__I uint32_t | CSR
__IO uint32_t | CCSR
__IO uint32_t | CACRR
__IO uint32_t | CBCDR
__IO uint32_t | CBCMR
__IO uint32_t | CSCMR1
__IO uint32_t | CSCMR2
__IO uint32_t | CSCDR1
__IO uint32_t | CS1CDR
__IO uint32_t | CS2CDR
__IO uint32_t | CDCDR
uint8_t | RESERVED_1 [4]
__IO uint32_t | CSCDR2
__IO uint32_t | CSCDR3
uint8_t | RESERVED_2 [8]
__I uint32_t | CDHIPR
uint8_t | RESERVED_3 [8]
__IO uint32_t | CLPCR
__IO uint32_t | CISR
__IO uint32_t | CIMR
__IO uint32_t | CCOSR
__IO uint32_t | CGPR
__IO uint32_t | CCGR0
__IO uint32_t | CCGR1
__IO uint32_t | CCGR2
__IO uint32_t | CCGR3
__IO uint32_t | CCGR4
__IO uint32_t | CCGR5
__IO uint32_t | CCGR6
__IO uint32_t | CCGR7
__IO uint32_t | CMEOR

## Detailed Description

CCM - Register Layout Typedef

Definition at line 5279 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h