Callisto4Bootloader: USBPHY Register Masks

Callisto4Bootloader

USBPHY Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » USBPHY Peripheral Access Layer

## PWD - USB PHY Power-Down Register

#define | USBPHY_PWD_RSVD0_MASK (0x3FFU)
#define | USBPHY_PWD_RSVD0_SHIFT (0U)
#define | USBPHY_PWD_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RSVD0_SHIFT)) & USBPHY_PWD_RSVD0_MASK)
#define | USBPHY_PWD_TXPWDFS_MASK (0x400U)
#define | USBPHY_PWD_TXPWDFS_SHIFT (10U)
#define | USBPHY_PWD_TXPWDFS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TXPWDFS_SHIFT)) & USBPHY_PWD_TXPWDFS_MASK)
#define | USBPHY_PWD_TXPWDIBIAS_MASK (0x800U)
#define | USBPHY_PWD_TXPWDIBIAS_SHIFT (11U)
#define | USBPHY_PWD_TXPWDIBIAS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_TXPWDIBIAS_MASK)
#define | USBPHY_PWD_TXPWDV2I_MASK (0x1000U)
#define | USBPHY_PWD_TXPWDV2I_SHIFT (12U)
#define | USBPHY_PWD_TXPWDV2I(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TXPWDV2I_SHIFT)) & USBPHY_PWD_TXPWDV2I_MASK)
#define | USBPHY_PWD_RSVD1_MASK (0x1E000U)
#define | USBPHY_PWD_RSVD1_SHIFT (13U)
#define | USBPHY_PWD_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RSVD1_SHIFT)) & USBPHY_PWD_RSVD1_MASK)
#define | USBPHY_PWD_RXPWDENV_MASK (0x20000U)
#define | USBPHY_PWD_RXPWDENV_SHIFT (17U)
#define | USBPHY_PWD_RXPWDENV(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWDENV_SHIFT)) & USBPHY_PWD_RXPWDENV_MASK)
#define | USBPHY_PWD_RXPWD1PT1_MASK (0x40000U)
#define | USBPHY_PWD_RXPWD1PT1_SHIFT (18U)
#define | USBPHY_PWD_RXPWD1PT1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWD1PT1_SHIFT)) & USBPHY_PWD_RXPWD1PT1_MASK)
#define | USBPHY_PWD_RXPWDDIFF_MASK (0x80000U)
#define | USBPHY_PWD_RXPWDDIFF_SHIFT (19U)
#define | USBPHY_PWD_RXPWDDIFF(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWDDIFF_SHIFT)) & USBPHY_PWD_RXPWDDIFF_MASK)
#define | USBPHY_PWD_RXPWDRX_MASK (0x100000U)
#define | USBPHY_PWD_RXPWDRX_SHIFT (20U)
#define | USBPHY_PWD_RXPWDRX(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWDRX_SHIFT)) & USBPHY_PWD_RXPWDRX_MASK)
#define | USBPHY_PWD_RSVD2_MASK (0xFFE00000U)
#define | USBPHY_PWD_RSVD2_SHIFT (21U)
#define | USBPHY_PWD_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RSVD2_SHIFT)) & USBPHY_PWD_RSVD2_MASK)

## PWD_SET - USB PHY Power-Down Register

#define | USBPHY_PWD_SET_RSVD0_MASK (0x3FFU)
#define | USBPHY_PWD_SET_RSVD0_SHIFT (0U)
#define | USBPHY_PWD_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RSVD0_SHIFT)) & USBPHY_PWD_SET_RSVD0_MASK)
#define | USBPHY_PWD_SET_TXPWDFS_MASK (0x400U)
#define | USBPHY_PWD_SET_TXPWDFS_SHIFT (10U)
#define | USBPHY_PWD_SET_TXPWDFS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_TXPWDFS_SHIFT)) & USBPHY_PWD_SET_TXPWDFS_MASK)
#define | USBPHY_PWD_SET_TXPWDIBIAS_MASK (0x800U)
#define | USBPHY_PWD_SET_TXPWDIBIAS_SHIFT (11U)
#define | USBPHY_PWD_SET_TXPWDIBIAS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_SET_TXPWDIBIAS_MASK)
#define | USBPHY_PWD_SET_TXPWDV2I_MASK (0x1000U)
#define | USBPHY_PWD_SET_TXPWDV2I_SHIFT (12U)
#define | USBPHY_PWD_SET_TXPWDV2I(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_TXPWDV2I_SHIFT)) & USBPHY_PWD_SET_TXPWDV2I_MASK)
#define | USBPHY_PWD_SET_RSVD1_MASK (0x1E000U)
#define | USBPHY_PWD_SET_RSVD1_SHIFT (13U)
#define | USBPHY_PWD_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RSVD1_SHIFT)) & USBPHY_PWD_SET_RSVD1_MASK)
#define | USBPHY_PWD_SET_RXPWDENV_MASK (0x20000U)
#define | USBPHY_PWD_SET_RXPWDENV_SHIFT (17U)
#define | USBPHY_PWD_SET_RXPWDENV(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWDENV_SHIFT)) & USBPHY_PWD_SET_RXPWDENV_MASK)
#define | USBPHY_PWD_SET_RXPWD1PT1_MASK (0x40000U)
#define | USBPHY_PWD_SET_RXPWD1PT1_SHIFT (18U)
#define | USBPHY_PWD_SET_RXPWD1PT1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWD1PT1_SHIFT)) & USBPHY_PWD_SET_RXPWD1PT1_MASK)
#define | USBPHY_PWD_SET_RXPWDDIFF_MASK (0x80000U)
#define | USBPHY_PWD_SET_RXPWDDIFF_SHIFT (19U)
#define | USBPHY_PWD_SET_RXPWDDIFF(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWDDIFF_SHIFT)) & USBPHY_PWD_SET_RXPWDDIFF_MASK)
#define | USBPHY_PWD_SET_RXPWDRX_MASK (0x100000U)
#define | USBPHY_PWD_SET_RXPWDRX_SHIFT (20U)
#define | USBPHY_PWD_SET_RXPWDRX(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWDRX_SHIFT)) & USBPHY_PWD_SET_RXPWDRX_MASK)
#define | USBPHY_PWD_SET_RSVD2_MASK (0xFFE00000U)
#define | USBPHY_PWD_SET_RSVD2_SHIFT (21U)
#define | USBPHY_PWD_SET_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RSVD2_SHIFT)) & USBPHY_PWD_SET_RSVD2_MASK)

## PWD_CLR - USB PHY Power-Down Register

#define | USBPHY_PWD_CLR_RSVD0_MASK (0x3FFU)
#define | USBPHY_PWD_CLR_RSVD0_SHIFT (0U)
#define | USBPHY_PWD_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RSVD0_SHIFT)) & USBPHY_PWD_CLR_RSVD0_MASK)
#define | USBPHY_PWD_CLR_TXPWDFS_MASK (0x400U)
#define | USBPHY_PWD_CLR_TXPWDFS_SHIFT (10U)
#define | USBPHY_PWD_CLR_TXPWDFS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_TXPWDFS_SHIFT)) & USBPHY_PWD_CLR_TXPWDFS_MASK)
#define | USBPHY_PWD_CLR_TXPWDIBIAS_MASK (0x800U)
#define | USBPHY_PWD_CLR_TXPWDIBIAS_SHIFT (11U)
#define | USBPHY_PWD_CLR_TXPWDIBIAS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_CLR_TXPWDIBIAS_MASK)
#define | USBPHY_PWD_CLR_TXPWDV2I_MASK (0x1000U)
#define | USBPHY_PWD_CLR_TXPWDV2I_SHIFT (12U)
#define | USBPHY_PWD_CLR_TXPWDV2I(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_TXPWDV2I_SHIFT)) & USBPHY_PWD_CLR_TXPWDV2I_MASK)
#define | USBPHY_PWD_CLR_RSVD1_MASK (0x1E000U)
#define | USBPHY_PWD_CLR_RSVD1_SHIFT (13U)
#define | USBPHY_PWD_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RSVD1_SHIFT)) & USBPHY_PWD_CLR_RSVD1_MASK)
#define | USBPHY_PWD_CLR_RXPWDENV_MASK (0x20000U)
#define | USBPHY_PWD_CLR_RXPWDENV_SHIFT (17U)
#define | USBPHY_PWD_CLR_RXPWDENV(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWDENV_SHIFT)) & USBPHY_PWD_CLR_RXPWDENV_MASK)
#define | USBPHY_PWD_CLR_RXPWD1PT1_MASK (0x40000U)
#define | USBPHY_PWD_CLR_RXPWD1PT1_SHIFT (18U)
#define | USBPHY_PWD_CLR_RXPWD1PT1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWD1PT1_SHIFT)) & USBPHY_PWD_CLR_RXPWD1PT1_MASK)
#define | USBPHY_PWD_CLR_RXPWDDIFF_MASK (0x80000U)
#define | USBPHY_PWD_CLR_RXPWDDIFF_SHIFT (19U)
#define | USBPHY_PWD_CLR_RXPWDDIFF(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWDDIFF_SHIFT)) & USBPHY_PWD_CLR_RXPWDDIFF_MASK)
#define | USBPHY_PWD_CLR_RXPWDRX_MASK (0x100000U)
#define | USBPHY_PWD_CLR_RXPWDRX_SHIFT (20U)
#define | USBPHY_PWD_CLR_RXPWDRX(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWDRX_SHIFT)) & USBPHY_PWD_CLR_RXPWDRX_MASK)
#define | USBPHY_PWD_CLR_RSVD2_MASK (0xFFE00000U)
#define | USBPHY_PWD_CLR_RSVD2_SHIFT (21U)
#define | USBPHY_PWD_CLR_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RSVD2_SHIFT)) & USBPHY_PWD_CLR_RSVD2_MASK)

## PWD_TOG - USB PHY Power-Down Register

#define | USBPHY_PWD_TOG_RSVD0_MASK (0x3FFU)
#define | USBPHY_PWD_TOG_RSVD0_SHIFT (0U)
#define | USBPHY_PWD_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RSVD0_SHIFT)) & USBPHY_PWD_TOG_RSVD0_MASK)
#define | USBPHY_PWD_TOG_TXPWDFS_MASK (0x400U)
#define | USBPHY_PWD_TOG_TXPWDFS_SHIFT (10U)
#define | USBPHY_PWD_TOG_TXPWDFS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_TXPWDFS_SHIFT)) & USBPHY_PWD_TOG_TXPWDFS_MASK)
#define | USBPHY_PWD_TOG_TXPWDIBIAS_MASK (0x800U)
#define | USBPHY_PWD_TOG_TXPWDIBIAS_SHIFT (11U)
#define | USBPHY_PWD_TOG_TXPWDIBIAS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_TOG_TXPWDIBIAS_MASK)
#define | USBPHY_PWD_TOG_TXPWDV2I_MASK (0x1000U)
#define | USBPHY_PWD_TOG_TXPWDV2I_SHIFT (12U)
#define | USBPHY_PWD_TOG_TXPWDV2I(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_TXPWDV2I_SHIFT)) & USBPHY_PWD_TOG_TXPWDV2I_MASK)
#define | USBPHY_PWD_TOG_RSVD1_MASK (0x1E000U)
#define | USBPHY_PWD_TOG_RSVD1_SHIFT (13U)
#define | USBPHY_PWD_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RSVD1_SHIFT)) & USBPHY_PWD_TOG_RSVD1_MASK)
#define | USBPHY_PWD_TOG_RXPWDENV_MASK (0x20000U)
#define | USBPHY_PWD_TOG_RXPWDENV_SHIFT (17U)
#define | USBPHY_PWD_TOG_RXPWDENV(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWDENV_SHIFT)) & USBPHY_PWD_TOG_RXPWDENV_MASK)
#define | USBPHY_PWD_TOG_RXPWD1PT1_MASK (0x40000U)
#define | USBPHY_PWD_TOG_RXPWD1PT1_SHIFT (18U)
#define | USBPHY_PWD_TOG_RXPWD1PT1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWD1PT1_SHIFT)) & USBPHY_PWD_TOG_RXPWD1PT1_MASK)
#define | USBPHY_PWD_TOG_RXPWDDIFF_MASK (0x80000U)
#define | USBPHY_PWD_TOG_RXPWDDIFF_SHIFT (19U)
#define | USBPHY_PWD_TOG_RXPWDDIFF(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWDDIFF_SHIFT)) & USBPHY_PWD_TOG_RXPWDDIFF_MASK)
#define | USBPHY_PWD_TOG_RXPWDRX_MASK (0x100000U)
#define | USBPHY_PWD_TOG_RXPWDRX_SHIFT (20U)
#define | USBPHY_PWD_TOG_RXPWDRX(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWDRX_SHIFT)) & USBPHY_PWD_TOG_RXPWDRX_MASK)
#define | USBPHY_PWD_TOG_RSVD2_MASK (0xFFE00000U)
#define | USBPHY_PWD_TOG_RSVD2_SHIFT (21U)
#define | USBPHY_PWD_TOG_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RSVD2_SHIFT)) & USBPHY_PWD_TOG_RSVD2_MASK)

## TX - USB PHY Transmitter Control Register

#define | USBPHY_TX_D_CAL_MASK (0xFU)
#define | USBPHY_TX_D_CAL_SHIFT (0U)
#define | USBPHY_TX_D_CAL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_D_CAL_SHIFT)) & USBPHY_TX_D_CAL_MASK)
#define | USBPHY_TX_RSVD0_MASK (0xF0U)
#define | USBPHY_TX_RSVD0_SHIFT (4U)
#define | USBPHY_TX_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD0_SHIFT)) & USBPHY_TX_RSVD0_MASK)
#define | USBPHY_TX_TXCAL45DN_MASK (0xF00U)
#define | USBPHY_TX_TXCAL45DN_SHIFT (8U)
#define | USBPHY_TX_TXCAL45DN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TXCAL45DN_SHIFT)) & USBPHY_TX_TXCAL45DN_MASK)
#define | USBPHY_TX_RSVD1_MASK (0xF000U)
#define | USBPHY_TX_RSVD1_SHIFT (12U)
#define | USBPHY_TX_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD1_SHIFT)) & USBPHY_TX_RSVD1_MASK)
#define | USBPHY_TX_TXCAL45DP_MASK (0xF0000U)
#define | USBPHY_TX_TXCAL45DP_SHIFT (16U)
#define | USBPHY_TX_TXCAL45DP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TXCAL45DP_SHIFT)) & USBPHY_TX_TXCAL45DP_MASK)
#define | USBPHY_TX_RSVD2_MASK (0x3F00000U)
#define | USBPHY_TX_RSVD2_SHIFT (20U)
#define | USBPHY_TX_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD2_SHIFT)) & USBPHY_TX_RSVD2_MASK)
#define | USBPHY_TX_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)
#define | USBPHY_TX_USBPHY_TX_EDGECTRL_SHIFT (26U)
#define | USBPHY_TX_USBPHY_TX_EDGECTRL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_USBPHY_TX_EDGECTRL_MASK)
#define | USBPHY_TX_RSVD5_MASK (0xE0000000U)
#define | USBPHY_TX_RSVD5_SHIFT (29U)
#define | USBPHY_TX_RSVD5(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD5_SHIFT)) & USBPHY_TX_RSVD5_MASK)

## TX_SET - USB PHY Transmitter Control Register

#define | USBPHY_TX_SET_D_CAL_MASK (0xFU)
#define | USBPHY_TX_SET_D_CAL_SHIFT (0U)
#define | USBPHY_TX_SET_D_CAL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_D_CAL_SHIFT)) & USBPHY_TX_SET_D_CAL_MASK)
#define | USBPHY_TX_SET_RSVD0_MASK (0xF0U)
#define | USBPHY_TX_SET_RSVD0_SHIFT (4U)
#define | USBPHY_TX_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD0_SHIFT)) & USBPHY_TX_SET_RSVD0_MASK)
#define | USBPHY_TX_SET_TXCAL45DN_MASK (0xF00U)
#define | USBPHY_TX_SET_TXCAL45DN_SHIFT (8U)
#define | USBPHY_TX_SET_TXCAL45DN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_TXCAL45DN_SHIFT)) & USBPHY_TX_SET_TXCAL45DN_MASK)
#define | USBPHY_TX_SET_RSVD1_MASK (0xF000U)
#define | USBPHY_TX_SET_RSVD1_SHIFT (12U)
#define | USBPHY_TX_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD1_SHIFT)) & USBPHY_TX_SET_RSVD1_MASK)
#define | USBPHY_TX_SET_TXCAL45DP_MASK (0xF0000U)
#define | USBPHY_TX_SET_TXCAL45DP_SHIFT (16U)
#define | USBPHY_TX_SET_TXCAL45DP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_TXCAL45DP_SHIFT)) & USBPHY_TX_SET_TXCAL45DP_MASK)
#define | USBPHY_TX_SET_RSVD2_MASK (0x3F00000U)
#define | USBPHY_TX_SET_RSVD2_SHIFT (20U)
#define | USBPHY_TX_SET_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD2_SHIFT)) & USBPHY_TX_SET_RSVD2_MASK)
#define | USBPHY_TX_SET_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)
#define | USBPHY_TX_SET_USBPHY_TX_EDGECTRL_SHIFT (26U)
#define | USBPHY_TX_SET_USBPHY_TX_EDGECTRL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_SET_USBPHY_TX_EDGECTRL_MASK)
#define | USBPHY_TX_SET_RSVD5_MASK (0xE0000000U)
#define | USBPHY_TX_SET_RSVD5_SHIFT (29U)
#define | USBPHY_TX_SET_RSVD5(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD5_SHIFT)) & USBPHY_TX_SET_RSVD5_MASK)

## TX_CLR - USB PHY Transmitter Control Register

#define | USBPHY_TX_CLR_D_CAL_MASK (0xFU)
#define | USBPHY_TX_CLR_D_CAL_SHIFT (0U)
#define | USBPHY_TX_CLR_D_CAL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_D_CAL_SHIFT)) & USBPHY_TX_CLR_D_CAL_MASK)
#define | USBPHY_TX_CLR_RSVD0_MASK (0xF0U)
#define | USBPHY_TX_CLR_RSVD0_SHIFT (4U)
#define | USBPHY_TX_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD0_SHIFT)) & USBPHY_TX_CLR_RSVD0_MASK)
#define | USBPHY_TX_CLR_TXCAL45DN_MASK (0xF00U)
#define | USBPHY_TX_CLR_TXCAL45DN_SHIFT (8U)
#define | USBPHY_TX_CLR_TXCAL45DN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_TXCAL45DN_SHIFT)) & USBPHY_TX_CLR_TXCAL45DN_MASK)
#define | USBPHY_TX_CLR_RSVD1_MASK (0xF000U)
#define | USBPHY_TX_CLR_RSVD1_SHIFT (12U)
#define | USBPHY_TX_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD1_SHIFT)) & USBPHY_TX_CLR_RSVD1_MASK)
#define | USBPHY_TX_CLR_TXCAL45DP_MASK (0xF0000U)
#define | USBPHY_TX_CLR_TXCAL45DP_SHIFT (16U)
#define | USBPHY_TX_CLR_TXCAL45DP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_TXCAL45DP_SHIFT)) & USBPHY_TX_CLR_TXCAL45DP_MASK)
#define | USBPHY_TX_CLR_RSVD2_MASK (0x3F00000U)
#define | USBPHY_TX_CLR_RSVD2_SHIFT (20U)
#define | USBPHY_TX_CLR_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD2_SHIFT)) & USBPHY_TX_CLR_RSVD2_MASK)
#define | USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)
#define | USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_SHIFT (26U)
#define | USBPHY_TX_CLR_USBPHY_TX_EDGECTRL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_MASK)
#define | USBPHY_TX_CLR_RSVD5_MASK (0xE0000000U)
#define | USBPHY_TX_CLR_RSVD5_SHIFT (29U)
#define | USBPHY_TX_CLR_RSVD5(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD5_SHIFT)) & USBPHY_TX_CLR_RSVD5_MASK)

## TX_TOG - USB PHY Transmitter Control Register

#define | USBPHY_TX_TOG_D_CAL_MASK (0xFU)
#define | USBPHY_TX_TOG_D_CAL_SHIFT (0U)
#define | USBPHY_TX_TOG_D_CAL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_D_CAL_SHIFT)) & USBPHY_TX_TOG_D_CAL_MASK)
#define | USBPHY_TX_TOG_RSVD0_MASK (0xF0U)
#define | USBPHY_TX_TOG_RSVD0_SHIFT (4U)
#define | USBPHY_TX_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD0_SHIFT)) & USBPHY_TX_TOG_RSVD0_MASK)
#define | USBPHY_TX_TOG_TXCAL45DN_MASK (0xF00U)
#define | USBPHY_TX_TOG_TXCAL45DN_SHIFT (8U)
#define | USBPHY_TX_TOG_TXCAL45DN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_TXCAL45DN_SHIFT)) & USBPHY_TX_TOG_TXCAL45DN_MASK)
#define | USBPHY_TX_TOG_RSVD1_MASK (0xF000U)
#define | USBPHY_TX_TOG_RSVD1_SHIFT (12U)
#define | USBPHY_TX_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD1_SHIFT)) & USBPHY_TX_TOG_RSVD1_MASK)
#define | USBPHY_TX_TOG_TXCAL45DP_MASK (0xF0000U)
#define | USBPHY_TX_TOG_TXCAL45DP_SHIFT (16U)
#define | USBPHY_TX_TOG_TXCAL45DP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_TXCAL45DP_SHIFT)) & USBPHY_TX_TOG_TXCAL45DP_MASK)
#define | USBPHY_TX_TOG_RSVD2_MASK (0x3F00000U)
#define | USBPHY_TX_TOG_RSVD2_SHIFT (20U)
#define | USBPHY_TX_TOG_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD2_SHIFT)) & USBPHY_TX_TOG_RSVD2_MASK)
#define | USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)
#define | USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_SHIFT (26U)
#define | USBPHY_TX_TOG_USBPHY_TX_EDGECTRL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_MASK)
#define | USBPHY_TX_TOG_RSVD5_MASK (0xE0000000U)
#define | USBPHY_TX_TOG_RSVD5_SHIFT (29U)
#define | USBPHY_TX_TOG_RSVD5(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD5_SHIFT)) & USBPHY_TX_TOG_RSVD5_MASK)

## RX - USB PHY Receiver Control Register

#define | USBPHY_RX_ENVADJ_MASK (0x7U)
#define | USBPHY_RX_ENVADJ_SHIFT (0U)
#define | USBPHY_RX_ENVADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_ENVADJ_SHIFT)) & USBPHY_RX_ENVADJ_MASK)
#define | USBPHY_RX_RSVD0_MASK (0x8U)
#define | USBPHY_RX_RSVD0_SHIFT (3U)
#define | USBPHY_RX_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RSVD0_SHIFT)) & USBPHY_RX_RSVD0_MASK)
#define | USBPHY_RX_DISCONADJ_MASK (0x70U)
#define | USBPHY_RX_DISCONADJ_SHIFT (4U)
#define | USBPHY_RX_DISCONADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_DISCONADJ_SHIFT)) & USBPHY_RX_DISCONADJ_MASK)
#define | USBPHY_RX_RSVD1_MASK (0x3FFF80U)
#define | USBPHY_RX_RSVD1_SHIFT (7U)
#define | USBPHY_RX_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RSVD1_SHIFT)) & USBPHY_RX_RSVD1_MASK)
#define | USBPHY_RX_RXDBYPASS_MASK (0x400000U)
#define | USBPHY_RX_RXDBYPASS_SHIFT (22U)
#define | USBPHY_RX_RXDBYPASS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RXDBYPASS_SHIFT)) & USBPHY_RX_RXDBYPASS_MASK)
#define | USBPHY_RX_RSVD2_MASK (0xFF800000U)
#define | USBPHY_RX_RSVD2_SHIFT (23U)
#define | USBPHY_RX_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RSVD2_SHIFT)) & USBPHY_RX_RSVD2_MASK)

## RX_SET - USB PHY Receiver Control Register

#define | USBPHY_RX_SET_ENVADJ_MASK (0x7U)
#define | USBPHY_RX_SET_ENVADJ_SHIFT (0U)
#define | USBPHY_RX_SET_ENVADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_ENVADJ_SHIFT)) & USBPHY_RX_SET_ENVADJ_MASK)
#define | USBPHY_RX_SET_RSVD0_MASK (0x8U)
#define | USBPHY_RX_SET_RSVD0_SHIFT (3U)
#define | USBPHY_RX_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RSVD0_SHIFT)) & USBPHY_RX_SET_RSVD0_MASK)
#define | USBPHY_RX_SET_DISCONADJ_MASK (0x70U)
#define | USBPHY_RX_SET_DISCONADJ_SHIFT (4U)
#define | USBPHY_RX_SET_DISCONADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_DISCONADJ_SHIFT)) & USBPHY_RX_SET_DISCONADJ_MASK)
#define | USBPHY_RX_SET_RSVD1_MASK (0x3FFF80U)
#define | USBPHY_RX_SET_RSVD1_SHIFT (7U)
#define | USBPHY_RX_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RSVD1_SHIFT)) & USBPHY_RX_SET_RSVD1_MASK)
#define | USBPHY_RX_SET_RXDBYPASS_MASK (0x400000U)
#define | USBPHY_RX_SET_RXDBYPASS_SHIFT (22U)
#define | USBPHY_RX_SET_RXDBYPASS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RXDBYPASS_SHIFT)) & USBPHY_RX_SET_RXDBYPASS_MASK)
#define | USBPHY_RX_SET_RSVD2_MASK (0xFF800000U)
#define | USBPHY_RX_SET_RSVD2_SHIFT (23U)
#define | USBPHY_RX_SET_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RSVD2_SHIFT)) & USBPHY_RX_SET_RSVD2_MASK)

## RX_CLR - USB PHY Receiver Control Register

#define | USBPHY_RX_CLR_ENVADJ_MASK (0x7U)
#define | USBPHY_RX_CLR_ENVADJ_SHIFT (0U)
#define | USBPHY_RX_CLR_ENVADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_ENVADJ_SHIFT)) & USBPHY_RX_CLR_ENVADJ_MASK)
#define | USBPHY_RX_CLR_RSVD0_MASK (0x8U)
#define | USBPHY_RX_CLR_RSVD0_SHIFT (3U)
#define | USBPHY_RX_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RSVD0_SHIFT)) & USBPHY_RX_CLR_RSVD0_MASK)
#define | USBPHY_RX_CLR_DISCONADJ_MASK (0x70U)
#define | USBPHY_RX_CLR_DISCONADJ_SHIFT (4U)
#define | USBPHY_RX_CLR_DISCONADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_DISCONADJ_SHIFT)) & USBPHY_RX_CLR_DISCONADJ_MASK)
#define | USBPHY_RX_CLR_RSVD1_MASK (0x3FFF80U)
#define | USBPHY_RX_CLR_RSVD1_SHIFT (7U)
#define | USBPHY_RX_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RSVD1_SHIFT)) & USBPHY_RX_CLR_RSVD1_MASK)
#define | USBPHY_RX_CLR_RXDBYPASS_MASK (0x400000U)
#define | USBPHY_RX_CLR_RXDBYPASS_SHIFT (22U)
#define | USBPHY_RX_CLR_RXDBYPASS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RXDBYPASS_SHIFT)) & USBPHY_RX_CLR_RXDBYPASS_MASK)
#define | USBPHY_RX_CLR_RSVD2_MASK (0xFF800000U)
#define | USBPHY_RX_CLR_RSVD2_SHIFT (23U)
#define | USBPHY_RX_CLR_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RSVD2_SHIFT)) & USBPHY_RX_CLR_RSVD2_MASK)

## RX_TOG - USB PHY Receiver Control Register

#define | USBPHY_RX_TOG_ENVADJ_MASK (0x7U)
#define | USBPHY_RX_TOG_ENVADJ_SHIFT (0U)
#define | USBPHY_RX_TOG_ENVADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_ENVADJ_SHIFT)) & USBPHY_RX_TOG_ENVADJ_MASK)
#define | USBPHY_RX_TOG_RSVD0_MASK (0x8U)
#define | USBPHY_RX_TOG_RSVD0_SHIFT (3U)
#define | USBPHY_RX_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RSVD0_SHIFT)) & USBPHY_RX_TOG_RSVD0_MASK)
#define | USBPHY_RX_TOG_DISCONADJ_MASK (0x70U)
#define | USBPHY_RX_TOG_DISCONADJ_SHIFT (4U)
#define | USBPHY_RX_TOG_DISCONADJ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_DISCONADJ_SHIFT)) & USBPHY_RX_TOG_DISCONADJ_MASK)
#define | USBPHY_RX_TOG_RSVD1_MASK (0x3FFF80U)
#define | USBPHY_RX_TOG_RSVD1_SHIFT (7U)
#define | USBPHY_RX_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RSVD1_SHIFT)) & USBPHY_RX_TOG_RSVD1_MASK)
#define | USBPHY_RX_TOG_RXDBYPASS_MASK (0x400000U)
#define | USBPHY_RX_TOG_RXDBYPASS_SHIFT (22U)
#define | USBPHY_RX_TOG_RXDBYPASS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RXDBYPASS_SHIFT)) & USBPHY_RX_TOG_RXDBYPASS_MASK)
#define | USBPHY_RX_TOG_RSVD2_MASK (0xFF800000U)
#define | USBPHY_RX_TOG_RSVD2_SHIFT (23U)
#define | USBPHY_RX_TOG_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RSVD2_SHIFT)) & USBPHY_RX_TOG_RSVD2_MASK)

## CTRL - USB PHY General Control Register

#define | USBPHY_CTRL_ENOTG_ID_CHG_IRQ_MASK (0x1U)
#define | USBPHY_CTRL_ENOTG_ID_CHG_IRQ_SHIFT (0U)
#define | USBPHY_CTRL_ENOTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_ENOTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_ENHOSTDISCONDETECT_MASK (0x2U)
#define | USBPHY_CTRL_ENHOSTDISCONDETECT_SHIFT (1U)
#define | USBPHY_CTRL_ENHOSTDISCONDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_ENHOSTDISCONDETECT_MASK)
#define | USBPHY_CTRL_ENIRQHOSTDISCON_MASK (0x4U)
#define | USBPHY_CTRL_ENIRQHOSTDISCON_SHIFT (2U)
#define | USBPHY_CTRL_ENIRQHOSTDISCON(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_ENIRQHOSTDISCON_MASK)
#define | USBPHY_CTRL_HOSTDISCONDETECT_IRQ_MASK (0x8U)
#define | USBPHY_CTRL_HOSTDISCONDETECT_IRQ_SHIFT (3U)
#define | USBPHY_CTRL_HOSTDISCONDETECT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_HOSTDISCONDETECT_IRQ_MASK)
#define | USBPHY_CTRL_ENDEVPLUGINDETECT_MASK (0x10U)
#define | USBPHY_CTRL_ENDEVPLUGINDETECT_SHIFT (4U)
#define | USBPHY_CTRL_ENDEVPLUGINDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_ENDEVPLUGINDETECT_MASK)
#define | USBPHY_CTRL_DEVPLUGIN_POLARITY_MASK (0x20U)
#define | USBPHY_CTRL_DEVPLUGIN_POLARITY_SHIFT (5U)
#define | USBPHY_CTRL_DEVPLUGIN_POLARITY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_DEVPLUGIN_POLARITY_MASK)
#define | USBPHY_CTRL_OTG_ID_CHG_IRQ_MASK (0x40U)
#define | USBPHY_CTRL_OTG_ID_CHG_IRQ_SHIFT (6U)
#define | USBPHY_CTRL_OTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_OTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_ENOTGIDDETECT_MASK (0x80U)
#define | USBPHY_CTRL_ENOTGIDDETECT_SHIFT (7U)
#define | USBPHY_CTRL_ENOTGIDDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_ENOTGIDDETECT_MASK)
#define | USBPHY_CTRL_RESUMEIRQSTICKY_MASK (0x100U)
#define | USBPHY_CTRL_RESUMEIRQSTICKY_SHIFT (8U)
#define | USBPHY_CTRL_RESUMEIRQSTICKY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_RESUMEIRQSTICKY_MASK)
#define | USBPHY_CTRL_ENIRQRESUMEDETECT_MASK (0x200U)
#define | USBPHY_CTRL_ENIRQRESUMEDETECT_SHIFT (9U)
#define | USBPHY_CTRL_ENIRQRESUMEDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_ENIRQRESUMEDETECT_MASK)
#define | USBPHY_CTRL_RESUME_IRQ_MASK (0x400U)
#define | USBPHY_CTRL_RESUME_IRQ_SHIFT (10U)
#define | USBPHY_CTRL_RESUME_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_RESUME_IRQ_MASK)
#define | USBPHY_CTRL_ENIRQDEVPLUGIN_MASK (0x800U)
#define | USBPHY_CTRL_ENIRQDEVPLUGIN_SHIFT (11U)
#define | USBPHY_CTRL_ENIRQDEVPLUGIN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_ENIRQDEVPLUGIN_MASK)
#define | USBPHY_CTRL_DEVPLUGIN_IRQ_MASK (0x1000U)
#define | USBPHY_CTRL_DEVPLUGIN_IRQ_SHIFT (12U)
#define | USBPHY_CTRL_DEVPLUGIN_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_DEVPLUGIN_IRQ_MASK)
#define | USBPHY_CTRL_DATA_ON_LRADC_MASK (0x2000U)
#define | USBPHY_CTRL_DATA_ON_LRADC_SHIFT (13U)
#define | USBPHY_CTRL_DATA_ON_LRADC(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_DATA_ON_LRADC_MASK)
#define | USBPHY_CTRL_ENUTMILEVEL2_MASK (0x4000U)
#define | USBPHY_CTRL_ENUTMILEVEL2_SHIFT (14U)
#define | USBPHY_CTRL_ENUTMILEVEL2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_ENUTMILEVEL2_MASK)
#define | USBPHY_CTRL_ENUTMILEVEL3_MASK (0x8000U)
#define | USBPHY_CTRL_ENUTMILEVEL3_SHIFT (15U)
#define | USBPHY_CTRL_ENUTMILEVEL3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_ENUTMILEVEL3_MASK)
#define | USBPHY_CTRL_ENIRQWAKEUP_MASK (0x10000U)
#define | USBPHY_CTRL_ENIRQWAKEUP_SHIFT (16U)
#define | USBPHY_CTRL_ENIRQWAKEUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_ENIRQWAKEUP_MASK)
#define | USBPHY_CTRL_WAKEUP_IRQ_MASK (0x20000U)
#define | USBPHY_CTRL_WAKEUP_IRQ_SHIFT (17U)
#define | USBPHY_CTRL_WAKEUP_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_WAKEUP_IRQ_MASK)
#define | USBPHY_CTRL_ENAUTO_PWRON_PLL_MASK (0x40000U)
#define | USBPHY_CTRL_ENAUTO_PWRON_PLL_SHIFT (18U)
#define | USBPHY_CTRL_ENAUTO_PWRON_PLL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_ENAUTO_PWRON_PLL_MASK)
#define | USBPHY_CTRL_ENAUTOCLR_CLKGATE_MASK (0x80000U)
#define | USBPHY_CTRL_ENAUTOCLR_CLKGATE_SHIFT (19U)
#define | USBPHY_CTRL_ENAUTOCLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_ENAUTOCLR_CLKGATE_MASK)
#define | USBPHY_CTRL_ENAUTOCLR_PHY_PWD_MASK (0x100000U)
#define | USBPHY_CTRL_ENAUTOCLR_PHY_PWD_SHIFT (20U)
#define | USBPHY_CTRL_ENAUTOCLR_PHY_PWD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_ENAUTOCLR_PHY_PWD_MASK)
#define | USBPHY_CTRL_ENDPDMCHG_WKUP_MASK (0x200000U)
#define | USBPHY_CTRL_ENDPDMCHG_WKUP_SHIFT (21U)
#define | USBPHY_CTRL_ENDPDMCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_ENDPDMCHG_WKUP_MASK)
#define | USBPHY_CTRL_ENIDCHG_WKUP_MASK (0x400000U)
#define | USBPHY_CTRL_ENIDCHG_WKUP_SHIFT (22U)
#define | USBPHY_CTRL_ENIDCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_ENIDCHG_WKUP_MASK)
#define | USBPHY_CTRL_ENVBUSCHG_WKUP_MASK (0x800000U)
#define | USBPHY_CTRL_ENVBUSCHG_WKUP_SHIFT (23U)
#define | USBPHY_CTRL_ENVBUSCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_ENVBUSCHG_WKUP_MASK)
#define | USBPHY_CTRL_FSDLL_RST_EN_MASK (0x1000000U)
#define | USBPHY_CTRL_FSDLL_RST_EN_SHIFT (24U)
#define | USBPHY_CTRL_FSDLL_RST_EN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_FSDLL_RST_EN_MASK)
#define | USBPHY_CTRL_RSVD1_MASK (0x6000000U)
#define | USBPHY_CTRL_RSVD1_SHIFT (25U)
#define | USBPHY_CTRL_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_RSVD1_SHIFT)) & USBPHY_CTRL_RSVD1_MASK)
#define | USBPHY_CTRL_OTG_ID_VALUE_MASK (0x8000000U)
#define | USBPHY_CTRL_OTG_ID_VALUE_SHIFT (27U)
#define | USBPHY_CTRL_OTG_ID_VALUE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_OTG_ID_VALUE_MASK)
#define | USBPHY_CTRL_HOST_FORCE_LS_SE0_MASK (0x10000000U)
#define | USBPHY_CTRL_HOST_FORCE_LS_SE0_SHIFT (28U)
#define | USBPHY_CTRL_HOST_FORCE_LS_SE0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_HOST_FORCE_LS_SE0_MASK)
#define | USBPHY_CTRL_UTMI_SUSPENDM_MASK (0x20000000U)
#define | USBPHY_CTRL_UTMI_SUSPENDM_SHIFT (29U)
#define | USBPHY_CTRL_UTMI_SUSPENDM(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_UTMI_SUSPENDM_MASK)
#define | USBPHY_CTRL_CLKGATE_MASK (0x40000000U)
#define | USBPHY_CTRL_CLKGATE_SHIFT (30U)
#define | USBPHY_CTRL_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLKGATE_SHIFT)) & USBPHY_CTRL_CLKGATE_MASK)
#define | USBPHY_CTRL_SFTRST_MASK (0x80000000U)
#define | USBPHY_CTRL_SFTRST_SHIFT (31U)
#define | USBPHY_CTRL_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SFTRST_SHIFT)) & USBPHY_CTRL_SFTRST_MASK)

## CTRL_SET - USB PHY General Control Register

#define | USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_MASK (0x1U)
#define | USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_SHIFT (0U)
#define | USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_SET_ENHOSTDISCONDETECT_MASK (0x2U)
#define | USBPHY_CTRL_SET_ENHOSTDISCONDETECT_SHIFT (1U)
#define | USBPHY_CTRL_SET_ENHOSTDISCONDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_SET_ENHOSTDISCONDETECT_MASK)
#define | USBPHY_CTRL_SET_ENIRQHOSTDISCON_MASK (0x4U)
#define | USBPHY_CTRL_SET_ENIRQHOSTDISCON_SHIFT (2U)
#define | USBPHY_CTRL_SET_ENIRQHOSTDISCON(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_SET_ENIRQHOSTDISCON_MASK)
#define | USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_MASK (0x8U)
#define | USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_SHIFT (3U)
#define | USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_MASK)
#define | USBPHY_CTRL_SET_ENDEVPLUGINDETECT_MASK (0x10U)
#define | USBPHY_CTRL_SET_ENDEVPLUGINDETECT_SHIFT (4U)
#define | USBPHY_CTRL_SET_ENDEVPLUGINDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_SET_ENDEVPLUGINDETECT_MASK)
#define | USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_MASK (0x20U)
#define | USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_SHIFT (5U)
#define | USBPHY_CTRL_SET_DEVPLUGIN_POLARITY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_MASK)
#define | USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_MASK (0x40U)
#define | USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_SHIFT (6U)
#define | USBPHY_CTRL_SET_OTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_SET_ENOTGIDDETECT_MASK (0x80U)
#define | USBPHY_CTRL_SET_ENOTGIDDETECT_SHIFT (7U)
#define | USBPHY_CTRL_SET_ENOTGIDDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_SET_ENOTGIDDETECT_MASK)
#define | USBPHY_CTRL_SET_RESUMEIRQSTICKY_MASK (0x100U)
#define | USBPHY_CTRL_SET_RESUMEIRQSTICKY_SHIFT (8U)
#define | USBPHY_CTRL_SET_RESUMEIRQSTICKY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_SET_RESUMEIRQSTICKY_MASK)
#define | USBPHY_CTRL_SET_ENIRQRESUMEDETECT_MASK (0x200U)
#define | USBPHY_CTRL_SET_ENIRQRESUMEDETECT_SHIFT (9U)
#define | USBPHY_CTRL_SET_ENIRQRESUMEDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_SET_ENIRQRESUMEDETECT_MASK)
#define | USBPHY_CTRL_SET_RESUME_IRQ_MASK (0x400U)
#define | USBPHY_CTRL_SET_RESUME_IRQ_SHIFT (10U)
#define | USBPHY_CTRL_SET_RESUME_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_SET_RESUME_IRQ_MASK)
#define | USBPHY_CTRL_SET_ENIRQDEVPLUGIN_MASK (0x800U)
#define | USBPHY_CTRL_SET_ENIRQDEVPLUGIN_SHIFT (11U)
#define | USBPHY_CTRL_SET_ENIRQDEVPLUGIN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_SET_ENIRQDEVPLUGIN_MASK)
#define | USBPHY_CTRL_SET_DEVPLUGIN_IRQ_MASK (0x1000U)
#define | USBPHY_CTRL_SET_DEVPLUGIN_IRQ_SHIFT (12U)
#define | USBPHY_CTRL_SET_DEVPLUGIN_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_SET_DEVPLUGIN_IRQ_MASK)
#define | USBPHY_CTRL_SET_DATA_ON_LRADC_MASK (0x2000U)
#define | USBPHY_CTRL_SET_DATA_ON_LRADC_SHIFT (13U)
#define | USBPHY_CTRL_SET_DATA_ON_LRADC(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_SET_DATA_ON_LRADC_MASK)
#define | USBPHY_CTRL_SET_ENUTMILEVEL2_MASK (0x4000U)
#define | USBPHY_CTRL_SET_ENUTMILEVEL2_SHIFT (14U)
#define | USBPHY_CTRL_SET_ENUTMILEVEL2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_SET_ENUTMILEVEL2_MASK)
#define | USBPHY_CTRL_SET_ENUTMILEVEL3_MASK (0x8000U)
#define | USBPHY_CTRL_SET_ENUTMILEVEL3_SHIFT (15U)
#define | USBPHY_CTRL_SET_ENUTMILEVEL3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_SET_ENUTMILEVEL3_MASK)
#define | USBPHY_CTRL_SET_ENIRQWAKEUP_MASK (0x10000U)
#define | USBPHY_CTRL_SET_ENIRQWAKEUP_SHIFT (16U)
#define | USBPHY_CTRL_SET_ENIRQWAKEUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_SET_ENIRQWAKEUP_MASK)
#define | USBPHY_CTRL_SET_WAKEUP_IRQ_MASK (0x20000U)
#define | USBPHY_CTRL_SET_WAKEUP_IRQ_SHIFT (17U)
#define | USBPHY_CTRL_SET_WAKEUP_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_SET_WAKEUP_IRQ_MASK)
#define | USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_MASK (0x40000U)
#define | USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_SHIFT (18U)
#define | USBPHY_CTRL_SET_ENAUTO_PWRON_PLL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_MASK)
#define | USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_MASK (0x80000U)
#define | USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_SHIFT (19U)
#define | USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_MASK)
#define | USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_MASK (0x100000U)
#define | USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_SHIFT (20U)
#define | USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_MASK)
#define | USBPHY_CTRL_SET_ENDPDMCHG_WKUP_MASK (0x200000U)
#define | USBPHY_CTRL_SET_ENDPDMCHG_WKUP_SHIFT (21U)
#define | USBPHY_CTRL_SET_ENDPDMCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_SET_ENDPDMCHG_WKUP_MASK)
#define | USBPHY_CTRL_SET_ENIDCHG_WKUP_MASK (0x400000U)
#define | USBPHY_CTRL_SET_ENIDCHG_WKUP_SHIFT (22U)
#define | USBPHY_CTRL_SET_ENIDCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_SET_ENIDCHG_WKUP_MASK)
#define | USBPHY_CTRL_SET_ENVBUSCHG_WKUP_MASK (0x800000U)
#define | USBPHY_CTRL_SET_ENVBUSCHG_WKUP_SHIFT (23U)
#define | USBPHY_CTRL_SET_ENVBUSCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_SET_ENVBUSCHG_WKUP_MASK)
#define | USBPHY_CTRL_SET_FSDLL_RST_EN_MASK (0x1000000U)
#define | USBPHY_CTRL_SET_FSDLL_RST_EN_SHIFT (24U)
#define | USBPHY_CTRL_SET_FSDLL_RST_EN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_SET_FSDLL_RST_EN_MASK)
#define | USBPHY_CTRL_SET_RSVD1_MASK (0x6000000U)
#define | USBPHY_CTRL_SET_RSVD1_SHIFT (25U)
#define | USBPHY_CTRL_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_RSVD1_SHIFT)) & USBPHY_CTRL_SET_RSVD1_MASK)
#define | USBPHY_CTRL_SET_OTG_ID_VALUE_MASK (0x8000000U)
#define | USBPHY_CTRL_SET_OTG_ID_VALUE_SHIFT (27U)
#define | USBPHY_CTRL_SET_OTG_ID_VALUE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_SET_OTG_ID_VALUE_MASK)
#define | USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_MASK (0x10000000U)
#define | USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_SHIFT (28U)
#define | USBPHY_CTRL_SET_HOST_FORCE_LS_SE0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_MASK)
#define | USBPHY_CTRL_SET_UTMI_SUSPENDM_MASK (0x20000000U)
#define | USBPHY_CTRL_SET_UTMI_SUSPENDM_SHIFT (29U)
#define | USBPHY_CTRL_SET_UTMI_SUSPENDM(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_SET_UTMI_SUSPENDM_MASK)
#define | USBPHY_CTRL_SET_CLKGATE_MASK (0x40000000U)
#define | USBPHY_CTRL_SET_CLKGATE_SHIFT (30U)
#define | USBPHY_CTRL_SET_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_CLKGATE_SHIFT)) & USBPHY_CTRL_SET_CLKGATE_MASK)
#define | USBPHY_CTRL_SET_SFTRST_MASK (0x80000000U)
#define | USBPHY_CTRL_SET_SFTRST_SHIFT (31U)
#define | USBPHY_CTRL_SET_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_SFTRST_SHIFT)) & USBPHY_CTRL_SET_SFTRST_MASK)

## CTRL_CLR - USB PHY General Control Register

#define | USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_MASK (0x1U)
#define | USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_SHIFT (0U)
#define | USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_MASK (0x2U)
#define | USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_SHIFT (1U)
#define | USBPHY_CTRL_CLR_ENHOSTDISCONDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_MASK)
#define | USBPHY_CTRL_CLR_ENIRQHOSTDISCON_MASK (0x4U)
#define | USBPHY_CTRL_CLR_ENIRQHOSTDISCON_SHIFT (2U)
#define | USBPHY_CTRL_CLR_ENIRQHOSTDISCON(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_CLR_ENIRQHOSTDISCON_MASK)
#define | USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_MASK (0x8U)
#define | USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_SHIFT (3U)
#define | USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_MASK)
#define | USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_MASK (0x10U)
#define | USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_SHIFT (4U)
#define | USBPHY_CTRL_CLR_ENDEVPLUGINDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_MASK)
#define | USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_MASK (0x20U)
#define | USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_SHIFT (5U)
#define | USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_MASK)
#define | USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_MASK (0x40U)
#define | USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_SHIFT (6U)
#define | USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_CLR_ENOTGIDDETECT_MASK (0x80U)
#define | USBPHY_CTRL_CLR_ENOTGIDDETECT_SHIFT (7U)
#define | USBPHY_CTRL_CLR_ENOTGIDDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENOTGIDDETECT_MASK)
#define | USBPHY_CTRL_CLR_RESUMEIRQSTICKY_MASK (0x100U)
#define | USBPHY_CTRL_CLR_RESUMEIRQSTICKY_SHIFT (8U)
#define | USBPHY_CTRL_CLR_RESUMEIRQSTICKY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_CLR_RESUMEIRQSTICKY_MASK)
#define | USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_MASK (0x200U)
#define | USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_SHIFT (9U)
#define | USBPHY_CTRL_CLR_ENIRQRESUMEDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_MASK)
#define | USBPHY_CTRL_CLR_RESUME_IRQ_MASK (0x400U)
#define | USBPHY_CTRL_CLR_RESUME_IRQ_SHIFT (10U)
#define | USBPHY_CTRL_CLR_RESUME_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_CLR_RESUME_IRQ_MASK)
#define | USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_MASK (0x800U)
#define | USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_SHIFT (11U)
#define | USBPHY_CTRL_CLR_ENIRQDEVPLUGIN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_MASK)
#define | USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_MASK (0x1000U)
#define | USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_SHIFT (12U)
#define | USBPHY_CTRL_CLR_DEVPLUGIN_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_MASK)
#define | USBPHY_CTRL_CLR_DATA_ON_LRADC_MASK (0x2000U)
#define | USBPHY_CTRL_CLR_DATA_ON_LRADC_SHIFT (13U)
#define | USBPHY_CTRL_CLR_DATA_ON_LRADC(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_CLR_DATA_ON_LRADC_MASK)
#define | USBPHY_CTRL_CLR_ENUTMILEVEL2_MASK (0x4000U)
#define | USBPHY_CTRL_CLR_ENUTMILEVEL2_SHIFT (14U)
#define | USBPHY_CTRL_CLR_ENUTMILEVEL2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_CLR_ENUTMILEVEL2_MASK)
#define | USBPHY_CTRL_CLR_ENUTMILEVEL3_MASK (0x8000U)
#define | USBPHY_CTRL_CLR_ENUTMILEVEL3_SHIFT (15U)
#define | USBPHY_CTRL_CLR_ENUTMILEVEL3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_CLR_ENUTMILEVEL3_MASK)
#define | USBPHY_CTRL_CLR_ENIRQWAKEUP_MASK (0x10000U)
#define | USBPHY_CTRL_CLR_ENIRQWAKEUP_SHIFT (16U)
#define | USBPHY_CTRL_CLR_ENIRQWAKEUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_CLR_ENIRQWAKEUP_MASK)
#define | USBPHY_CTRL_CLR_WAKEUP_IRQ_MASK (0x20000U)
#define | USBPHY_CTRL_CLR_WAKEUP_IRQ_SHIFT (17U)
#define | USBPHY_CTRL_CLR_WAKEUP_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_CLR_WAKEUP_IRQ_MASK)
#define | USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_MASK (0x40000U)
#define | USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_SHIFT (18U)
#define | USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_MASK)
#define | USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_MASK (0x80000U)
#define | USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_SHIFT (19U)
#define | USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_MASK)
#define | USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_MASK (0x100000U)
#define | USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_SHIFT (20U)
#define | USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_MASK)
#define | USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_MASK (0x200000U)
#define | USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_SHIFT (21U)
#define | USBPHY_CTRL_CLR_ENDPDMCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_MASK)
#define | USBPHY_CTRL_CLR_ENIDCHG_WKUP_MASK (0x400000U)
#define | USBPHY_CTRL_CLR_ENIDCHG_WKUP_SHIFT (22U)
#define | USBPHY_CTRL_CLR_ENIDCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_CLR_ENIDCHG_WKUP_MASK)
#define | USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_MASK (0x800000U)
#define | USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_SHIFT (23U)
#define | USBPHY_CTRL_CLR_ENVBUSCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_MASK)
#define | USBPHY_CTRL_CLR_FSDLL_RST_EN_MASK (0x1000000U)
#define | USBPHY_CTRL_CLR_FSDLL_RST_EN_SHIFT (24U)
#define | USBPHY_CTRL_CLR_FSDLL_RST_EN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_CLR_FSDLL_RST_EN_MASK)
#define | USBPHY_CTRL_CLR_RSVD1_MASK (0x6000000U)
#define | USBPHY_CTRL_CLR_RSVD1_SHIFT (25U)
#define | USBPHY_CTRL_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_RSVD1_SHIFT)) & USBPHY_CTRL_CLR_RSVD1_MASK)
#define | USBPHY_CTRL_CLR_OTG_ID_VALUE_MASK (0x8000000U)
#define | USBPHY_CTRL_CLR_OTG_ID_VALUE_SHIFT (27U)
#define | USBPHY_CTRL_CLR_OTG_ID_VALUE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_CLR_OTG_ID_VALUE_MASK)
#define | USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_MASK (0x10000000U)
#define | USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_SHIFT (28U)
#define | USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_MASK)
#define | USBPHY_CTRL_CLR_UTMI_SUSPENDM_MASK (0x20000000U)
#define | USBPHY_CTRL_CLR_UTMI_SUSPENDM_SHIFT (29U)
#define | USBPHY_CTRL_CLR_UTMI_SUSPENDM(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_CLR_UTMI_SUSPENDM_MASK)
#define | USBPHY_CTRL_CLR_CLKGATE_MASK (0x40000000U)
#define | USBPHY_CTRL_CLR_CLKGATE_SHIFT (30U)
#define | USBPHY_CTRL_CLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_CLKGATE_SHIFT)) & USBPHY_CTRL_CLR_CLKGATE_MASK)
#define | USBPHY_CTRL_CLR_SFTRST_MASK (0x80000000U)
#define | USBPHY_CTRL_CLR_SFTRST_SHIFT (31U)
#define | USBPHY_CTRL_CLR_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_SFTRST_SHIFT)) & USBPHY_CTRL_CLR_SFTRST_MASK)

## CTRL_TOG - USB PHY General Control Register

#define | USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_MASK (0x1U)
#define | USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_SHIFT (0U)
#define | USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_MASK (0x2U)
#define | USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_SHIFT (1U)
#define | USBPHY_CTRL_TOG_ENHOSTDISCONDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_MASK)
#define | USBPHY_CTRL_TOG_ENIRQHOSTDISCON_MASK (0x4U)
#define | USBPHY_CTRL_TOG_ENIRQHOSTDISCON_SHIFT (2U)
#define | USBPHY_CTRL_TOG_ENIRQHOSTDISCON(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_TOG_ENIRQHOSTDISCON_MASK)
#define | USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_MASK (0x8U)
#define | USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_SHIFT (3U)
#define | USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_MASK)
#define | USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_MASK (0x10U)
#define | USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_SHIFT (4U)
#define | USBPHY_CTRL_TOG_ENDEVPLUGINDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_MASK)
#define | USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_MASK (0x20U)
#define | USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_SHIFT (5U)
#define | USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_MASK)
#define | USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_MASK (0x40U)
#define | USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_SHIFT (6U)
#define | USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_MASK)
#define | USBPHY_CTRL_TOG_ENOTGIDDETECT_MASK (0x80U)
#define | USBPHY_CTRL_TOG_ENOTGIDDETECT_SHIFT (7U)
#define | USBPHY_CTRL_TOG_ENOTGIDDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENOTGIDDETECT_MASK)
#define | USBPHY_CTRL_TOG_RESUMEIRQSTICKY_MASK (0x100U)
#define | USBPHY_CTRL_TOG_RESUMEIRQSTICKY_SHIFT (8U)
#define | USBPHY_CTRL_TOG_RESUMEIRQSTICKY(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_TOG_RESUMEIRQSTICKY_MASK)
#define | USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_MASK (0x200U)
#define | USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_SHIFT (9U)
#define | USBPHY_CTRL_TOG_ENIRQRESUMEDETECT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_MASK)
#define | USBPHY_CTRL_TOG_RESUME_IRQ_MASK (0x400U)
#define | USBPHY_CTRL_TOG_RESUME_IRQ_SHIFT (10U)
#define | USBPHY_CTRL_TOG_RESUME_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_TOG_RESUME_IRQ_MASK)
#define | USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_MASK (0x800U)
#define | USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_SHIFT (11U)
#define | USBPHY_CTRL_TOG_ENIRQDEVPLUGIN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_MASK)
#define | USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_MASK (0x1000U)
#define | USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_SHIFT (12U)
#define | USBPHY_CTRL_TOG_DEVPLUGIN_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_MASK)
#define | USBPHY_CTRL_TOG_DATA_ON_LRADC_MASK (0x2000U)
#define | USBPHY_CTRL_TOG_DATA_ON_LRADC_SHIFT (13U)
#define | USBPHY_CTRL_TOG_DATA_ON_LRADC(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_TOG_DATA_ON_LRADC_MASK)
#define | USBPHY_CTRL_TOG_ENUTMILEVEL2_MASK (0x4000U)
#define | USBPHY_CTRL_TOG_ENUTMILEVEL2_SHIFT (14U)
#define | USBPHY_CTRL_TOG_ENUTMILEVEL2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_TOG_ENUTMILEVEL2_MASK)
#define | USBPHY_CTRL_TOG_ENUTMILEVEL3_MASK (0x8000U)
#define | USBPHY_CTRL_TOG_ENUTMILEVEL3_SHIFT (15U)
#define | USBPHY_CTRL_TOG_ENUTMILEVEL3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_TOG_ENUTMILEVEL3_MASK)
#define | USBPHY_CTRL_TOG_ENIRQWAKEUP_MASK (0x10000U)
#define | USBPHY_CTRL_TOG_ENIRQWAKEUP_SHIFT (16U)
#define | USBPHY_CTRL_TOG_ENIRQWAKEUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_TOG_ENIRQWAKEUP_MASK)
#define | USBPHY_CTRL_TOG_WAKEUP_IRQ_MASK (0x20000U)
#define | USBPHY_CTRL_TOG_WAKEUP_IRQ_SHIFT (17U)
#define | USBPHY_CTRL_TOG_WAKEUP_IRQ(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_TOG_WAKEUP_IRQ_MASK)
#define | USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_MASK (0x40000U)
#define | USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_SHIFT (18U)
#define | USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_MASK)
#define | USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_MASK (0x80000U)
#define | USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_SHIFT (19U)
#define | USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_MASK)
#define | USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_MASK (0x100000U)
#define | USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_SHIFT (20U)
#define | USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_MASK)
#define | USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_MASK (0x200000U)
#define | USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_SHIFT (21U)
#define | USBPHY_CTRL_TOG_ENDPDMCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_MASK)
#define | USBPHY_CTRL_TOG_ENIDCHG_WKUP_MASK (0x400000U)
#define | USBPHY_CTRL_TOG_ENIDCHG_WKUP_SHIFT (22U)
#define | USBPHY_CTRL_TOG_ENIDCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_TOG_ENIDCHG_WKUP_MASK)
#define | USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_MASK (0x800000U)
#define | USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_SHIFT (23U)
#define | USBPHY_CTRL_TOG_ENVBUSCHG_WKUP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_MASK)
#define | USBPHY_CTRL_TOG_FSDLL_RST_EN_MASK (0x1000000U)
#define | USBPHY_CTRL_TOG_FSDLL_RST_EN_SHIFT (24U)
#define | USBPHY_CTRL_TOG_FSDLL_RST_EN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_TOG_FSDLL_RST_EN_MASK)
#define | USBPHY_CTRL_TOG_RSVD1_MASK (0x6000000U)
#define | USBPHY_CTRL_TOG_RSVD1_SHIFT (25U)
#define | USBPHY_CTRL_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_RSVD1_SHIFT)) & USBPHY_CTRL_TOG_RSVD1_MASK)
#define | USBPHY_CTRL_TOG_OTG_ID_VALUE_MASK (0x8000000U)
#define | USBPHY_CTRL_TOG_OTG_ID_VALUE_SHIFT (27U)
#define | USBPHY_CTRL_TOG_OTG_ID_VALUE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_TOG_OTG_ID_VALUE_MASK)
#define | USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_MASK (0x10000000U)
#define | USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_SHIFT (28U)
#define | USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_MASK)
#define | USBPHY_CTRL_TOG_UTMI_SUSPENDM_MASK (0x20000000U)
#define | USBPHY_CTRL_TOG_UTMI_SUSPENDM_SHIFT (29U)
#define | USBPHY_CTRL_TOG_UTMI_SUSPENDM(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_TOG_UTMI_SUSPENDM_MASK)
#define | USBPHY_CTRL_TOG_CLKGATE_MASK (0x40000000U)
#define | USBPHY_CTRL_TOG_CLKGATE_SHIFT (30U)
#define | USBPHY_CTRL_TOG_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_CLKGATE_SHIFT)) & USBPHY_CTRL_TOG_CLKGATE_MASK)
#define | USBPHY_CTRL_TOG_SFTRST_MASK (0x80000000U)
#define | USBPHY_CTRL_TOG_SFTRST_SHIFT (31U)
#define | USBPHY_CTRL_TOG_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_SFTRST_SHIFT)) & USBPHY_CTRL_TOG_SFTRST_MASK)

## STATUS - USB PHY Status Register

#define | USBPHY_STATUS_RSVD0_MASK (0x7U)
#define | USBPHY_STATUS_RSVD0_SHIFT (0U)
#define | USBPHY_STATUS_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD0_SHIFT)) & USBPHY_STATUS_RSVD0_MASK)
#define | USBPHY_STATUS_HOSTDISCONDETECT_STATUS_MASK (0x8U)
#define | USBPHY_STATUS_HOSTDISCONDETECT_STATUS_SHIFT (3U)
#define | USBPHY_STATUS_HOSTDISCONDETECT_STATUS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_HOSTDISCONDETECT_STATUS_SHIFT)) & USBPHY_STATUS_HOSTDISCONDETECT_STATUS_MASK)
#define | USBPHY_STATUS_RSVD1_MASK (0x30U)
#define | USBPHY_STATUS_RSVD1_SHIFT (4U)
#define | USBPHY_STATUS_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD1_SHIFT)) & USBPHY_STATUS_RSVD1_MASK)
#define | USBPHY_STATUS_DEVPLUGIN_STATUS_MASK (0x40U)
#define | USBPHY_STATUS_DEVPLUGIN_STATUS_SHIFT (6U)
#define | USBPHY_STATUS_DEVPLUGIN_STATUS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_DEVPLUGIN_STATUS_SHIFT)) & USBPHY_STATUS_DEVPLUGIN_STATUS_MASK)
#define | USBPHY_STATUS_RSVD2_MASK (0x80U)
#define | USBPHY_STATUS_RSVD2_SHIFT (7U)
#define | USBPHY_STATUS_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD2_SHIFT)) & USBPHY_STATUS_RSVD2_MASK)
#define | USBPHY_STATUS_OTGID_STATUS_MASK (0x100U)
#define | USBPHY_STATUS_OTGID_STATUS_SHIFT (8U)
#define | USBPHY_STATUS_OTGID_STATUS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_OTGID_STATUS_SHIFT)) & USBPHY_STATUS_OTGID_STATUS_MASK)
#define | USBPHY_STATUS_RSVD3_MASK (0x200U)
#define | USBPHY_STATUS_RSVD3_SHIFT (9U)
#define | USBPHY_STATUS_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD3_SHIFT)) & USBPHY_STATUS_RSVD3_MASK)
#define | USBPHY_STATUS_RESUME_STATUS_MASK (0x400U)
#define | USBPHY_STATUS_RESUME_STATUS_SHIFT (10U)
#define | USBPHY_STATUS_RESUME_STATUS(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RESUME_STATUS_SHIFT)) & USBPHY_STATUS_RESUME_STATUS_MASK)
#define | USBPHY_STATUS_RSVD4_MASK (0xFFFFF800U)
#define | USBPHY_STATUS_RSVD4_SHIFT (11U)
#define | USBPHY_STATUS_RSVD4(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD4_SHIFT)) & USBPHY_STATUS_RSVD4_MASK)

## DEBUG - USB PHY Debug Register

#define | USBPHY_DEBUG_OTGIDPIOLOCK_MASK (0x1U)
#define | USBPHY_DEBUG_OTGIDPIOLOCK_SHIFT (0U)
#define | USBPHY_DEBUG_OTGIDPIOLOCK(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_OTGIDPIOLOCK_MASK)
#define | USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_MASK (0x2U)
#define | USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_SHIFT (1U)
#define | USBPHY_DEBUG_DEBUG_INTERFACE_HOLD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_MASK)
#define | USBPHY_DEBUG_HSTPULLDOWN_MASK (0xCU)
#define | USBPHY_DEBUG_HSTPULLDOWN_SHIFT (2U)
#define | USBPHY_DEBUG_HSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_HSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_ENHSTPULLDOWN_MASK (0x30U)
#define | USBPHY_DEBUG_ENHSTPULLDOWN_SHIFT (4U)
#define | USBPHY_DEBUG_ENHSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_ENHSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_RSVD0_MASK (0xC0U)
#define | USBPHY_DEBUG_RSVD0_SHIFT (6U)
#define | USBPHY_DEBUG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD0_SHIFT)) & USBPHY_DEBUG_RSVD0_MASK)
#define | USBPHY_DEBUG_TX2RXCOUNT_MASK (0xF00U)
#define | USBPHY_DEBUG_TX2RXCOUNT_SHIFT (8U)
#define | USBPHY_DEBUG_TX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_TX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_ENTX2RXCOUNT_MASK (0x1000U)
#define | USBPHY_DEBUG_ENTX2RXCOUNT_SHIFT (12U)
#define | USBPHY_DEBUG_ENTX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_ENTX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_RSVD1_MASK (0xE000U)
#define | USBPHY_DEBUG_RSVD1_SHIFT (13U)
#define | USBPHY_DEBUG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD1_SHIFT)) & USBPHY_DEBUG_RSVD1_MASK)
#define | USBPHY_DEBUG_SQUELCHRESETCOUNT_MASK (0x1F0000U)
#define | USBPHY_DEBUG_SQUELCHRESETCOUNT_SHIFT (16U)
#define | USBPHY_DEBUG_SQUELCHRESETCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_SQUELCHRESETCOUNT_MASK)
#define | USBPHY_DEBUG_RSVD2_MASK (0xE00000U)
#define | USBPHY_DEBUG_RSVD2_SHIFT (21U)
#define | USBPHY_DEBUG_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD2_SHIFT)) & USBPHY_DEBUG_RSVD2_MASK)
#define | USBPHY_DEBUG_ENSQUELCHRESET_MASK (0x1000000U)
#define | USBPHY_DEBUG_ENSQUELCHRESET_SHIFT (24U)
#define | USBPHY_DEBUG_ENSQUELCHRESET(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_ENSQUELCHRESET_MASK)
#define | USBPHY_DEBUG_SQUELCHRESETLENGTH_MASK (0x1E000000U)
#define | USBPHY_DEBUG_SQUELCHRESETLENGTH_SHIFT (25U)
#define | USBPHY_DEBUG_SQUELCHRESETLENGTH(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_SQUELCHRESETLENGTH_MASK)
#define | USBPHY_DEBUG_HOST_RESUME_DEBUG_MASK (0x20000000U)
#define | USBPHY_DEBUG_HOST_RESUME_DEBUG_SHIFT (29U)
#define | USBPHY_DEBUG_HOST_RESUME_DEBUG(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_HOST_RESUME_DEBUG_MASK)
#define | USBPHY_DEBUG_CLKGATE_MASK (0x40000000U)
#define | USBPHY_DEBUG_CLKGATE_SHIFT (30U)
#define | USBPHY_DEBUG_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLKGATE_SHIFT)) & USBPHY_DEBUG_CLKGATE_MASK)
#define | USBPHY_DEBUG_RSVD3_MASK (0x80000000U)
#define | USBPHY_DEBUG_RSVD3_SHIFT (31U)
#define | USBPHY_DEBUG_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD3_SHIFT)) & USBPHY_DEBUG_RSVD3_MASK)

## DEBUG_SET - USB PHY Debug Register

#define | USBPHY_DEBUG_SET_OTGIDPIOLOCK_MASK (0x1U)
#define | USBPHY_DEBUG_SET_OTGIDPIOLOCK_SHIFT (0U)
#define | USBPHY_DEBUG_SET_OTGIDPIOLOCK(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_SET_OTGIDPIOLOCK_MASK)
#define | USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_MASK (0x2U)
#define | USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_SHIFT (1U)
#define | USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_MASK)
#define | USBPHY_DEBUG_SET_HSTPULLDOWN_MASK (0xCU)
#define | USBPHY_DEBUG_SET_HSTPULLDOWN_SHIFT (2U)
#define | USBPHY_DEBUG_SET_HSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_SET_HSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_SET_ENHSTPULLDOWN_MASK (0x30U)
#define | USBPHY_DEBUG_SET_ENHSTPULLDOWN_SHIFT (4U)
#define | USBPHY_DEBUG_SET_ENHSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_SET_ENHSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_SET_RSVD0_MASK (0xC0U)
#define | USBPHY_DEBUG_SET_RSVD0_SHIFT (6U)
#define | USBPHY_DEBUG_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD0_SHIFT)) & USBPHY_DEBUG_SET_RSVD0_MASK)
#define | USBPHY_DEBUG_SET_TX2RXCOUNT_MASK (0xF00U)
#define | USBPHY_DEBUG_SET_TX2RXCOUNT_SHIFT (8U)
#define | USBPHY_DEBUG_SET_TX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_SET_TX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_SET_ENTX2RXCOUNT_MASK (0x1000U)
#define | USBPHY_DEBUG_SET_ENTX2RXCOUNT_SHIFT (12U)
#define | USBPHY_DEBUG_SET_ENTX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_SET_ENTX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_SET_RSVD1_MASK (0xE000U)
#define | USBPHY_DEBUG_SET_RSVD1_SHIFT (13U)
#define | USBPHY_DEBUG_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD1_SHIFT)) & USBPHY_DEBUG_SET_RSVD1_MASK)
#define | USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_MASK (0x1F0000U)
#define | USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_SHIFT (16U)
#define | USBPHY_DEBUG_SET_SQUELCHRESETCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_MASK)
#define | USBPHY_DEBUG_SET_RSVD2_MASK (0xE00000U)
#define | USBPHY_DEBUG_SET_RSVD2_SHIFT (21U)
#define | USBPHY_DEBUG_SET_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD2_SHIFT)) & USBPHY_DEBUG_SET_RSVD2_MASK)
#define | USBPHY_DEBUG_SET_ENSQUELCHRESET_MASK (0x1000000U)
#define | USBPHY_DEBUG_SET_ENSQUELCHRESET_SHIFT (24U)
#define | USBPHY_DEBUG_SET_ENSQUELCHRESET(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_SET_ENSQUELCHRESET_MASK)
#define | USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_MASK (0x1E000000U)
#define | USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_SHIFT (25U)
#define | USBPHY_DEBUG_SET_SQUELCHRESETLENGTH(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_MASK)
#define | USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_MASK (0x20000000U)
#define | USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_SHIFT (29U)
#define | USBPHY_DEBUG_SET_HOST_RESUME_DEBUG(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_MASK)
#define | USBPHY_DEBUG_SET_CLKGATE_MASK (0x40000000U)
#define | USBPHY_DEBUG_SET_CLKGATE_SHIFT (30U)
#define | USBPHY_DEBUG_SET_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_CLKGATE_SHIFT)) & USBPHY_DEBUG_SET_CLKGATE_MASK)
#define | USBPHY_DEBUG_SET_RSVD3_MASK (0x80000000U)
#define | USBPHY_DEBUG_SET_RSVD3_SHIFT (31U)
#define | USBPHY_DEBUG_SET_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD3_SHIFT)) & USBPHY_DEBUG_SET_RSVD3_MASK)

## DEBUG_CLR - USB PHY Debug Register

#define | USBPHY_DEBUG_CLR_OTGIDPIOLOCK_MASK (0x1U)
#define | USBPHY_DEBUG_CLR_OTGIDPIOLOCK_SHIFT (0U)
#define | USBPHY_DEBUG_CLR_OTGIDPIOLOCK(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_CLR_OTGIDPIOLOCK_MASK)
#define | USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_MASK (0x2U)
#define | USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_SHIFT (1U)
#define | USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_MASK)
#define | USBPHY_DEBUG_CLR_HSTPULLDOWN_MASK (0xCU)
#define | USBPHY_DEBUG_CLR_HSTPULLDOWN_SHIFT (2U)
#define | USBPHY_DEBUG_CLR_HSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_CLR_HSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_CLR_ENHSTPULLDOWN_MASK (0x30U)
#define | USBPHY_DEBUG_CLR_ENHSTPULLDOWN_SHIFT (4U)
#define | USBPHY_DEBUG_CLR_ENHSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_CLR_ENHSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_CLR_RSVD0_MASK (0xC0U)
#define | USBPHY_DEBUG_CLR_RSVD0_SHIFT (6U)
#define | USBPHY_DEBUG_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD0_SHIFT)) & USBPHY_DEBUG_CLR_RSVD0_MASK)
#define | USBPHY_DEBUG_CLR_TX2RXCOUNT_MASK (0xF00U)
#define | USBPHY_DEBUG_CLR_TX2RXCOUNT_SHIFT (8U)
#define | USBPHY_DEBUG_CLR_TX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_CLR_TX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_CLR_ENTX2RXCOUNT_MASK (0x1000U)
#define | USBPHY_DEBUG_CLR_ENTX2RXCOUNT_SHIFT (12U)
#define | USBPHY_DEBUG_CLR_ENTX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_CLR_ENTX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_CLR_RSVD1_MASK (0xE000U)
#define | USBPHY_DEBUG_CLR_RSVD1_SHIFT (13U)
#define | USBPHY_DEBUG_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD1_SHIFT)) & USBPHY_DEBUG_CLR_RSVD1_MASK)
#define | USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_MASK (0x1F0000U)
#define | USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_SHIFT (16U)
#define | USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_MASK)
#define | USBPHY_DEBUG_CLR_RSVD2_MASK (0xE00000U)
#define | USBPHY_DEBUG_CLR_RSVD2_SHIFT (21U)
#define | USBPHY_DEBUG_CLR_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD2_SHIFT)) & USBPHY_DEBUG_CLR_RSVD2_MASK)
#define | USBPHY_DEBUG_CLR_ENSQUELCHRESET_MASK (0x1000000U)
#define | USBPHY_DEBUG_CLR_ENSQUELCHRESET_SHIFT (24U)
#define | USBPHY_DEBUG_CLR_ENSQUELCHRESET(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_CLR_ENSQUELCHRESET_MASK)
#define | USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_MASK (0x1E000000U)
#define | USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_SHIFT (25U)
#define | USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_MASK)
#define | USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_MASK (0x20000000U)
#define | USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_SHIFT (29U)
#define | USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_MASK)
#define | USBPHY_DEBUG_CLR_CLKGATE_MASK (0x40000000U)
#define | USBPHY_DEBUG_CLR_CLKGATE_SHIFT (30U)
#define | USBPHY_DEBUG_CLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_CLKGATE_SHIFT)) & USBPHY_DEBUG_CLR_CLKGATE_MASK)
#define | USBPHY_DEBUG_CLR_RSVD3_MASK (0x80000000U)
#define | USBPHY_DEBUG_CLR_RSVD3_SHIFT (31U)
#define | USBPHY_DEBUG_CLR_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD3_SHIFT)) & USBPHY_DEBUG_CLR_RSVD3_MASK)

## DEBUG_TOG - USB PHY Debug Register

#define | USBPHY_DEBUG_TOG_OTGIDPIOLOCK_MASK (0x1U)
#define | USBPHY_DEBUG_TOG_OTGIDPIOLOCK_SHIFT (0U)
#define | USBPHY_DEBUG_TOG_OTGIDPIOLOCK(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_TOG_OTGIDPIOLOCK_MASK)
#define | USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_MASK (0x2U)
#define | USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_SHIFT (1U)
#define | USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_MASK)
#define | USBPHY_DEBUG_TOG_HSTPULLDOWN_MASK (0xCU)
#define | USBPHY_DEBUG_TOG_HSTPULLDOWN_SHIFT (2U)
#define | USBPHY_DEBUG_TOG_HSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_TOG_HSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_TOG_ENHSTPULLDOWN_MASK (0x30U)
#define | USBPHY_DEBUG_TOG_ENHSTPULLDOWN_SHIFT (4U)
#define | USBPHY_DEBUG_TOG_ENHSTPULLDOWN(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_TOG_ENHSTPULLDOWN_MASK)
#define | USBPHY_DEBUG_TOG_RSVD0_MASK (0xC0U)
#define | USBPHY_DEBUG_TOG_RSVD0_SHIFT (6U)
#define | USBPHY_DEBUG_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD0_SHIFT)) & USBPHY_DEBUG_TOG_RSVD0_MASK)
#define | USBPHY_DEBUG_TOG_TX2RXCOUNT_MASK (0xF00U)
#define | USBPHY_DEBUG_TOG_TX2RXCOUNT_SHIFT (8U)
#define | USBPHY_DEBUG_TOG_TX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_TOG_TX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_TOG_ENTX2RXCOUNT_MASK (0x1000U)
#define | USBPHY_DEBUG_TOG_ENTX2RXCOUNT_SHIFT (12U)
#define | USBPHY_DEBUG_TOG_ENTX2RXCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_TOG_ENTX2RXCOUNT_MASK)
#define | USBPHY_DEBUG_TOG_RSVD1_MASK (0xE000U)
#define | USBPHY_DEBUG_TOG_RSVD1_SHIFT (13U)
#define | USBPHY_DEBUG_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD1_SHIFT)) & USBPHY_DEBUG_TOG_RSVD1_MASK)
#define | USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_MASK (0x1F0000U)
#define | USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_SHIFT (16U)
#define | USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_MASK)
#define | USBPHY_DEBUG_TOG_RSVD2_MASK (0xE00000U)
#define | USBPHY_DEBUG_TOG_RSVD2_SHIFT (21U)
#define | USBPHY_DEBUG_TOG_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD2_SHIFT)) & USBPHY_DEBUG_TOG_RSVD2_MASK)
#define | USBPHY_DEBUG_TOG_ENSQUELCHRESET_MASK (0x1000000U)
#define | USBPHY_DEBUG_TOG_ENSQUELCHRESET_SHIFT (24U)
#define | USBPHY_DEBUG_TOG_ENSQUELCHRESET(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_TOG_ENSQUELCHRESET_MASK)
#define | USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_MASK (0x1E000000U)
#define | USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_SHIFT (25U)
#define | USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_MASK)
#define | USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_MASK (0x20000000U)
#define | USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_SHIFT (29U)
#define | USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_MASK)
#define | USBPHY_DEBUG_TOG_CLKGATE_MASK (0x40000000U)
#define | USBPHY_DEBUG_TOG_CLKGATE_SHIFT (30U)
#define | USBPHY_DEBUG_TOG_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_CLKGATE_SHIFT)) & USBPHY_DEBUG_TOG_CLKGATE_MASK)
#define | USBPHY_DEBUG_TOG_RSVD3_MASK (0x80000000U)
#define | USBPHY_DEBUG_TOG_RSVD3_SHIFT (31U)
#define | USBPHY_DEBUG_TOG_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD3_SHIFT)) & USBPHY_DEBUG_TOG_RSVD3_MASK)

## DEBUG0_STATUS - UTMI Debug Status Register 0

#define | USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_MASK (0xFFFFU)
#define | USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_SHIFT (0U)
#define | USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_SHIFT)) & USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_MASK)
#define | USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_MASK (0x3FF0000U)
#define | USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_SHIFT (16U)
#define | USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_SHIFT)) & USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_MASK)
#define | USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_MASK (0xFC000000U)
#define | USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_SHIFT (26U)
#define | USBPHY_DEBUG0_STATUS_SQUELCH_COUNT(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_SHIFT)) & USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_MASK)

## DEBUG1 - UTMI Debug Status Register 1

#define | USBPHY_DEBUG1_RSVD0_MASK (0x1FFFU)
#define | USBPHY_DEBUG1_RSVD0_SHIFT (0U)
#define | USBPHY_DEBUG1_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_RSVD0_SHIFT)) & USBPHY_DEBUG1_RSVD0_MASK)
#define | USBPHY_DEBUG1_ENTAILADJVD_MASK (0x6000U)
#define | USBPHY_DEBUG1_ENTAILADJVD_SHIFT (13U)
#define | USBPHY_DEBUG1_ENTAILADJVD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_ENTAILADJVD_MASK)
#define | USBPHY_DEBUG1_RSVD1_MASK (0xFFFF8000U)
#define | USBPHY_DEBUG1_RSVD1_SHIFT (15U)
#define | USBPHY_DEBUG1_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_RSVD1_SHIFT)) & USBPHY_DEBUG1_RSVD1_MASK)

## DEBUG1_SET - UTMI Debug Status Register 1

#define | USBPHY_DEBUG1_SET_RSVD0_MASK (0x1FFFU)
#define | USBPHY_DEBUG1_SET_RSVD0_SHIFT (0U)
#define | USBPHY_DEBUG1_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_SET_RSVD0_SHIFT)) & USBPHY_DEBUG1_SET_RSVD0_MASK)
#define | USBPHY_DEBUG1_SET_ENTAILADJVD_MASK (0x6000U)
#define | USBPHY_DEBUG1_SET_ENTAILADJVD_SHIFT (13U)
#define | USBPHY_DEBUG1_SET_ENTAILADJVD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_SET_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_SET_ENTAILADJVD_MASK)
#define | USBPHY_DEBUG1_SET_RSVD1_MASK (0xFFFF8000U)
#define | USBPHY_DEBUG1_SET_RSVD1_SHIFT (15U)
#define | USBPHY_DEBUG1_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_SET_RSVD1_SHIFT)) & USBPHY_DEBUG1_SET_RSVD1_MASK)

## DEBUG1_CLR - UTMI Debug Status Register 1

#define | USBPHY_DEBUG1_CLR_RSVD0_MASK (0x1FFFU)
#define | USBPHY_DEBUG1_CLR_RSVD0_SHIFT (0U)
#define | USBPHY_DEBUG1_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_CLR_RSVD0_SHIFT)) & USBPHY_DEBUG1_CLR_RSVD0_MASK)
#define | USBPHY_DEBUG1_CLR_ENTAILADJVD_MASK (0x6000U)
#define | USBPHY_DEBUG1_CLR_ENTAILADJVD_SHIFT (13U)
#define | USBPHY_DEBUG1_CLR_ENTAILADJVD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_CLR_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_CLR_ENTAILADJVD_MASK)
#define | USBPHY_DEBUG1_CLR_RSVD1_MASK (0xFFFF8000U)
#define | USBPHY_DEBUG1_CLR_RSVD1_SHIFT (15U)
#define | USBPHY_DEBUG1_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_CLR_RSVD1_SHIFT)) & USBPHY_DEBUG1_CLR_RSVD1_MASK)

## DEBUG1_TOG - UTMI Debug Status Register 1

#define | USBPHY_DEBUG1_TOG_RSVD0_MASK (0x1FFFU)
#define | USBPHY_DEBUG1_TOG_RSVD0_SHIFT (0U)
#define | USBPHY_DEBUG1_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_TOG_RSVD0_SHIFT)) & USBPHY_DEBUG1_TOG_RSVD0_MASK)
#define | USBPHY_DEBUG1_TOG_ENTAILADJVD_MASK (0x6000U)
#define | USBPHY_DEBUG1_TOG_ENTAILADJVD_SHIFT (13U)
#define | USBPHY_DEBUG1_TOG_ENTAILADJVD(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_TOG_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_TOG_ENTAILADJVD_MASK)
#define | USBPHY_DEBUG1_TOG_RSVD1_MASK (0xFFFF8000U)
#define | USBPHY_DEBUG1_TOG_RSVD1_SHIFT (15U)
#define | USBPHY_DEBUG1_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_TOG_RSVD1_SHIFT)) & USBPHY_DEBUG1_TOG_RSVD1_MASK)

## VERSION - UTMI RTL Version

#define | USBPHY_VERSION_STEP_MASK (0xFFFFU)
#define | USBPHY_VERSION_STEP_SHIFT (0U)
#define | USBPHY_VERSION_STEP(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_VERSION_STEP_SHIFT)) & USBPHY_VERSION_STEP_MASK)
#define | USBPHY_VERSION_MINOR_MASK (0xFF0000U)
#define | USBPHY_VERSION_MINOR_SHIFT (16U)
#define | USBPHY_VERSION_MINOR(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_VERSION_MINOR_SHIFT)) & USBPHY_VERSION_MINOR_MASK)
#define | USBPHY_VERSION_MAJOR_MASK (0xFF000000U)
#define | USBPHY_VERSION_MAJOR_SHIFT (24U)
#define | USBPHY_VERSION_MAJOR(x) (((uint32_t)(((uint32_t)(x)) << USBPHY_VERSION_MAJOR_SHIFT)) & USBPHY_VERSION_MAJOR_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ USBPHY_CTRL_CLKGATE

#define USBPHY_CTRL_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLKGATE_SHIFT)) & USBPHY_CTRL_CLKGATE_MASK)

Definition at line 43536 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLKGATE_MASK

#define USBPHY_CTRL_CLKGATE_MASK (0x40000000U)

Definition at line 43534 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLKGATE_SHIFT

#define USBPHY_CTRL_CLKGATE_SHIFT (30U)

Definition at line 43535 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_CLKGATE

#define USBPHY_CTRL_CLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_CLKGATE_SHIFT)) & USBPHY_CTRL_CLR_CLKGATE_MASK)

Definition at line 43730 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_CLKGATE_MASK

#define USBPHY_CTRL_CLR_CLKGATE_MASK (0x40000000U)

Definition at line 43728 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_CLKGATE_SHIFT

#define USBPHY_CTRL_CLR_CLKGATE_SHIFT (30U)

Definition at line 43729 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DATA_ON_LRADC

#define USBPHY_CTRL_CLR_DATA_ON_LRADC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_CLR_DATA_ON_LRADC_MASK)

Definition at line 43682 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DATA_ON_LRADC_MASK

#define USBPHY_CTRL_CLR_DATA_ON_LRADC_MASK (0x2000U)

Definition at line 43680 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DATA_ON_LRADC_SHIFT

#define USBPHY_CTRL_CLR_DATA_ON_LRADC_SHIFT (13U)

Definition at line 43681 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DEVPLUGIN_IRQ

#define USBPHY_CTRL_CLR_DEVPLUGIN_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_MASK)

Definition at line 43679 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_MASK

#define USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_MASK (0x1000U)

Definition at line 43677 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_SHIFT

#define USBPHY_CTRL_CLR_DEVPLUGIN_IRQ_SHIFT (12U)

Definition at line 43678 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY

#define USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_MASK)

Definition at line 43658 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_MASK

#define USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_MASK (0x20U)

Definition at line 43656 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_SHIFT

#define USBPHY_CTRL_CLR_DEVPLUGIN_POLARITY_SHIFT (5U)

Definition at line 43657 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL

#define USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_MASK)

Definition at line 43697 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_MASK

#define USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_MASK (0x40000U)

Definition at line 43695 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_SHIFT

#define USBPHY_CTRL_CLR_ENAUTO_PWRON_PLL_SHIFT (18U)

Definition at line 43696 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE

#define USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_MASK)

Definition at line 43700 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_MASK

#define USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_MASK (0x80000U)

Definition at line 43698 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_SHIFT

#define USBPHY_CTRL_CLR_ENAUTOCLR_CLKGATE_SHIFT (19U)

Definition at line 43699 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD

#define USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_MASK)

Definition at line 43703 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_MASK

#define USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_MASK (0x100000U)

Definition at line 43701 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_SHIFT

#define USBPHY_CTRL_CLR_ENAUTOCLR_PHY_PWD_SHIFT (20U)

Definition at line 43702 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENDEVPLUGINDETECT

#define USBPHY_CTRL_CLR_ENDEVPLUGINDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_MASK)

Definition at line 43655 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_MASK

#define USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_MASK (0x10U)

Definition at line 43653 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_SHIFT

#define USBPHY_CTRL_CLR_ENDEVPLUGINDETECT_SHIFT (4U)

Definition at line 43654 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENDPDMCHG_WKUP

#define USBPHY_CTRL_CLR_ENDPDMCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_MASK)

Definition at line 43706 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_MASK

#define USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_MASK (0x200000U)

Definition at line 43704 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_SHIFT

#define USBPHY_CTRL_CLR_ENDPDMCHG_WKUP_SHIFT (21U)

Definition at line 43705 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENHOSTDISCONDETECT

#define USBPHY_CTRL_CLR_ENHOSTDISCONDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_MASK)

Definition at line 43646 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_MASK

#define USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_MASK (0x2U)

Definition at line 43644 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_SHIFT

#define USBPHY_CTRL_CLR_ENHOSTDISCONDETECT_SHIFT (1U)

Definition at line 43645 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIDCHG_WKUP

#define USBPHY_CTRL_CLR_ENIDCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_CLR_ENIDCHG_WKUP_MASK)

Definition at line 43709 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIDCHG_WKUP_MASK

#define USBPHY_CTRL_CLR_ENIDCHG_WKUP_MASK (0x400000U)

Definition at line 43707 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIDCHG_WKUP_SHIFT

#define USBPHY_CTRL_CLR_ENIDCHG_WKUP_SHIFT (22U)

Definition at line 43708 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQDEVPLUGIN

#define USBPHY_CTRL_CLR_ENIRQDEVPLUGIN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_MASK)

Definition at line 43676 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_MASK

#define USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_MASK (0x800U)

Definition at line 43674 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_SHIFT

#define USBPHY_CTRL_CLR_ENIRQDEVPLUGIN_SHIFT (11U)

Definition at line 43675 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQHOSTDISCON

#define USBPHY_CTRL_CLR_ENIRQHOSTDISCON | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_CLR_ENIRQHOSTDISCON_MASK)

Definition at line 43649 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQHOSTDISCON_MASK

#define USBPHY_CTRL_CLR_ENIRQHOSTDISCON_MASK (0x4U)

Definition at line 43647 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQHOSTDISCON_SHIFT

#define USBPHY_CTRL_CLR_ENIRQHOSTDISCON_SHIFT (2U)

Definition at line 43648 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQRESUMEDETECT

#define USBPHY_CTRL_CLR_ENIRQRESUMEDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_MASK)

Definition at line 43670 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_MASK

#define USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_MASK (0x200U)

Definition at line 43668 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_SHIFT

#define USBPHY_CTRL_CLR_ENIRQRESUMEDETECT_SHIFT (9U)

Definition at line 43669 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQWAKEUP

#define USBPHY_CTRL_CLR_ENIRQWAKEUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_CLR_ENIRQWAKEUP_MASK)

Definition at line 43691 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQWAKEUP_MASK

#define USBPHY_CTRL_CLR_ENIRQWAKEUP_MASK (0x10000U)

Definition at line 43689 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENIRQWAKEUP_SHIFT

#define USBPHY_CTRL_CLR_ENIRQWAKEUP_SHIFT (16U)

Definition at line 43690 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ

#define USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_MASK)

Definition at line 43643 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_MASK (0x1U)

Definition at line 43641 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_CLR_ENOTG_ID_CHG_IRQ_SHIFT (0U)

Definition at line 43642 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENOTGIDDETECT

#define USBPHY_CTRL_CLR_ENOTGIDDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_CLR_ENOTGIDDETECT_MASK)

Definition at line 43664 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENOTGIDDETECT_MASK

#define USBPHY_CTRL_CLR_ENOTGIDDETECT_MASK (0x80U)

Definition at line 43662 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENOTGIDDETECT_SHIFT

#define USBPHY_CTRL_CLR_ENOTGIDDETECT_SHIFT (7U)

Definition at line 43663 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENUTMILEVEL2

#define USBPHY_CTRL_CLR_ENUTMILEVEL2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_CLR_ENUTMILEVEL2_MASK)

Definition at line 43685 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENUTMILEVEL2_MASK

#define USBPHY_CTRL_CLR_ENUTMILEVEL2_MASK (0x4000U)

Definition at line 43683 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENUTMILEVEL2_SHIFT

#define USBPHY_CTRL_CLR_ENUTMILEVEL2_SHIFT (14U)

Definition at line 43684 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENUTMILEVEL3

#define USBPHY_CTRL_CLR_ENUTMILEVEL3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_CLR_ENUTMILEVEL3_MASK)

Definition at line 43688 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENUTMILEVEL3_MASK

#define USBPHY_CTRL_CLR_ENUTMILEVEL3_MASK (0x8000U)

Definition at line 43686 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENUTMILEVEL3_SHIFT

#define USBPHY_CTRL_CLR_ENUTMILEVEL3_SHIFT (15U)

Definition at line 43687 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENVBUSCHG_WKUP

#define USBPHY_CTRL_CLR_ENVBUSCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_MASK)

Definition at line 43712 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_MASK

#define USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_MASK (0x800000U)

Definition at line 43710 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_SHIFT

#define USBPHY_CTRL_CLR_ENVBUSCHG_WKUP_SHIFT (23U)

Definition at line 43711 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_FSDLL_RST_EN

#define USBPHY_CTRL_CLR_FSDLL_RST_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_CLR_FSDLL_RST_EN_MASK)

Definition at line 43715 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_FSDLL_RST_EN_MASK

#define USBPHY_CTRL_CLR_FSDLL_RST_EN_MASK (0x1000000U)

Definition at line 43713 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_FSDLL_RST_EN_SHIFT

#define USBPHY_CTRL_CLR_FSDLL_RST_EN_SHIFT (24U)

Definition at line 43714 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0

#define USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_MASK)

Definition at line 43724 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_MASK

#define USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_MASK (0x10000000U)

Definition at line 43722 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_SHIFT

#define USBPHY_CTRL_CLR_HOST_FORCE_LS_SE0_SHIFT (28U)

Definition at line 43723 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ

#define USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_MASK)

Definition at line 43652 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_MASK

#define USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_MASK (0x8U)

Definition at line 43650 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_SHIFT

#define USBPHY_CTRL_CLR_HOSTDISCONDETECT_IRQ_SHIFT (3U)

Definition at line 43651 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ

#define USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_MASK)

Definition at line 43661 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_MASK (0x40U)

Definition at line 43659 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_CLR_OTG_ID_CHG_IRQ_SHIFT (6U)

Definition at line 43660 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_OTG_ID_VALUE

#define USBPHY_CTRL_CLR_OTG_ID_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_CLR_OTG_ID_VALUE_MASK)

Definition at line 43721 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_OTG_ID_VALUE_MASK

#define USBPHY_CTRL_CLR_OTG_ID_VALUE_MASK (0x8000000U)

Definition at line 43719 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_OTG_ID_VALUE_SHIFT

#define USBPHY_CTRL_CLR_OTG_ID_VALUE_SHIFT (27U)

Definition at line 43720 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RESUME_IRQ

#define USBPHY_CTRL_CLR_RESUME_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_CLR_RESUME_IRQ_MASK)

Definition at line 43673 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RESUME_IRQ_MASK

#define USBPHY_CTRL_CLR_RESUME_IRQ_MASK (0x400U)

Definition at line 43671 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RESUME_IRQ_SHIFT

#define USBPHY_CTRL_CLR_RESUME_IRQ_SHIFT (10U)

Definition at line 43672 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RESUMEIRQSTICKY

#define USBPHY_CTRL_CLR_RESUMEIRQSTICKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_CLR_RESUMEIRQSTICKY_MASK)

Definition at line 43667 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RESUMEIRQSTICKY_MASK

#define USBPHY_CTRL_CLR_RESUMEIRQSTICKY_MASK (0x100U)

Definition at line 43665 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RESUMEIRQSTICKY_SHIFT

#define USBPHY_CTRL_CLR_RESUMEIRQSTICKY_SHIFT (8U)

Definition at line 43666 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RSVD1

#define USBPHY_CTRL_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_RSVD1_SHIFT)) & USBPHY_CTRL_CLR_RSVD1_MASK)

Definition at line 43718 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RSVD1_MASK

#define USBPHY_CTRL_CLR_RSVD1_MASK (0x6000000U)

Definition at line 43716 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_RSVD1_SHIFT

#define USBPHY_CTRL_CLR_RSVD1_SHIFT (25U)

Definition at line 43717 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_SFTRST

#define USBPHY_CTRL_CLR_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_SFTRST_SHIFT)) & USBPHY_CTRL_CLR_SFTRST_MASK)

Definition at line 43733 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_SFTRST_MASK

#define USBPHY_CTRL_CLR_SFTRST_MASK (0x80000000U)

Definition at line 43731 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_SFTRST_SHIFT

#define USBPHY_CTRL_CLR_SFTRST_SHIFT (31U)

Definition at line 43732 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_UTMI_SUSPENDM

#define USBPHY_CTRL_CLR_UTMI_SUSPENDM | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_CLR_UTMI_SUSPENDM_MASK)

Definition at line 43727 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_UTMI_SUSPENDM_MASK

#define USBPHY_CTRL_CLR_UTMI_SUSPENDM_MASK (0x20000000U)

Definition at line 43725 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_UTMI_SUSPENDM_SHIFT

#define USBPHY_CTRL_CLR_UTMI_SUSPENDM_SHIFT (29U)

Definition at line 43726 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_WAKEUP_IRQ

#define USBPHY_CTRL_CLR_WAKEUP_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_CLR_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_CLR_WAKEUP_IRQ_MASK)

Definition at line 43694 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_WAKEUP_IRQ_MASK

#define USBPHY_CTRL_CLR_WAKEUP_IRQ_MASK (0x20000U)

Definition at line 43692 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_CLR_WAKEUP_IRQ_SHIFT

#define USBPHY_CTRL_CLR_WAKEUP_IRQ_SHIFT (17U)

Definition at line 43693 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DATA_ON_LRADC

#define USBPHY_CTRL_DATA_ON_LRADC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_DATA_ON_LRADC_MASK)

Definition at line 43488 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DATA_ON_LRADC_MASK

#define USBPHY_CTRL_DATA_ON_LRADC_MASK (0x2000U)

Definition at line 43486 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DATA_ON_LRADC_SHIFT

#define USBPHY_CTRL_DATA_ON_LRADC_SHIFT (13U)

Definition at line 43487 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DEVPLUGIN_IRQ

#define USBPHY_CTRL_DEVPLUGIN_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_DEVPLUGIN_IRQ_MASK)

Definition at line 43485 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DEVPLUGIN_IRQ_MASK

#define USBPHY_CTRL_DEVPLUGIN_IRQ_MASK (0x1000U)

Definition at line 43483 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DEVPLUGIN_IRQ_SHIFT

#define USBPHY_CTRL_DEVPLUGIN_IRQ_SHIFT (12U)

Definition at line 43484 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DEVPLUGIN_POLARITY

#define USBPHY_CTRL_DEVPLUGIN_POLARITY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_DEVPLUGIN_POLARITY_MASK)

Definition at line 43464 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DEVPLUGIN_POLARITY_MASK

#define USBPHY_CTRL_DEVPLUGIN_POLARITY_MASK (0x20U)

Definition at line 43462 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_DEVPLUGIN_POLARITY_SHIFT

#define USBPHY_CTRL_DEVPLUGIN_POLARITY_SHIFT (5U)

Definition at line 43463 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTO_PWRON_PLL

#define USBPHY_CTRL_ENAUTO_PWRON_PLL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_ENAUTO_PWRON_PLL_MASK)

Definition at line 43503 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTO_PWRON_PLL_MASK

#define USBPHY_CTRL_ENAUTO_PWRON_PLL_MASK (0x40000U)

Definition at line 43501 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTO_PWRON_PLL_SHIFT

#define USBPHY_CTRL_ENAUTO_PWRON_PLL_SHIFT (18U)

Definition at line 43502 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTOCLR_CLKGATE

#define USBPHY_CTRL_ENAUTOCLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_ENAUTOCLR_CLKGATE_MASK)

Definition at line 43506 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTOCLR_CLKGATE_MASK

#define USBPHY_CTRL_ENAUTOCLR_CLKGATE_MASK (0x80000U)

Definition at line 43504 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTOCLR_CLKGATE_SHIFT

#define USBPHY_CTRL_ENAUTOCLR_CLKGATE_SHIFT (19U)

Definition at line 43505 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTOCLR_PHY_PWD

#define USBPHY_CTRL_ENAUTOCLR_PHY_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_ENAUTOCLR_PHY_PWD_MASK)

Definition at line 43509 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTOCLR_PHY_PWD_MASK

#define USBPHY_CTRL_ENAUTOCLR_PHY_PWD_MASK (0x100000U)

Definition at line 43507 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENAUTOCLR_PHY_PWD_SHIFT

#define USBPHY_CTRL_ENAUTOCLR_PHY_PWD_SHIFT (20U)

Definition at line 43508 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDEVPLUGINDETECT

#define USBPHY_CTRL_ENDEVPLUGINDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_ENDEVPLUGINDETECT_MASK)

Definition at line 43461 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDEVPLUGINDETECT_MASK

#define USBPHY_CTRL_ENDEVPLUGINDETECT_MASK (0x10U)

Definition at line 43459 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDEVPLUGINDETECT_SHIFT

#define USBPHY_CTRL_ENDEVPLUGINDETECT_SHIFT (4U)

Definition at line 43460 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDPDMCHG_WKUP

#define USBPHY_CTRL_ENDPDMCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_ENDPDMCHG_WKUP_MASK)

Definition at line 43512 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDPDMCHG_WKUP_MASK

#define USBPHY_CTRL_ENDPDMCHG_WKUP_MASK (0x200000U)

Definition at line 43510 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDPDMCHG_WKUP_SHIFT

#define USBPHY_CTRL_ENDPDMCHG_WKUP_SHIFT (21U)

Definition at line 43511 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENHOSTDISCONDETECT

#define USBPHY_CTRL_ENHOSTDISCONDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_ENHOSTDISCONDETECT_MASK)

Definition at line 43452 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENHOSTDISCONDETECT_MASK

#define USBPHY_CTRL_ENHOSTDISCONDETECT_MASK (0x2U)

Definition at line 43450 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENHOSTDISCONDETECT_SHIFT

#define USBPHY_CTRL_ENHOSTDISCONDETECT_SHIFT (1U)

Definition at line 43451 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIDCHG_WKUP

#define USBPHY_CTRL_ENIDCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_ENIDCHG_WKUP_MASK)

Definition at line 43515 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIDCHG_WKUP_MASK

#define USBPHY_CTRL_ENIDCHG_WKUP_MASK (0x400000U)

Definition at line 43513 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIDCHG_WKUP_SHIFT

#define USBPHY_CTRL_ENIDCHG_WKUP_SHIFT (22U)

Definition at line 43514 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQDEVPLUGIN

#define USBPHY_CTRL_ENIRQDEVPLUGIN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_ENIRQDEVPLUGIN_MASK)

Definition at line 43482 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQDEVPLUGIN_MASK

#define USBPHY_CTRL_ENIRQDEVPLUGIN_MASK (0x800U)

Definition at line 43480 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQDEVPLUGIN_SHIFT

#define USBPHY_CTRL_ENIRQDEVPLUGIN_SHIFT (11U)

Definition at line 43481 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQHOSTDISCON

#define USBPHY_CTRL_ENIRQHOSTDISCON | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_ENIRQHOSTDISCON_MASK)

Definition at line 43455 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQHOSTDISCON_MASK

#define USBPHY_CTRL_ENIRQHOSTDISCON_MASK (0x4U)

Definition at line 43453 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQHOSTDISCON_SHIFT

#define USBPHY_CTRL_ENIRQHOSTDISCON_SHIFT (2U)

Definition at line 43454 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQRESUMEDETECT

#define USBPHY_CTRL_ENIRQRESUMEDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_ENIRQRESUMEDETECT_MASK)

Definition at line 43476 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQRESUMEDETECT_MASK

#define USBPHY_CTRL_ENIRQRESUMEDETECT_MASK (0x200U)

Definition at line 43474 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQRESUMEDETECT_SHIFT

#define USBPHY_CTRL_ENIRQRESUMEDETECT_SHIFT (9U)

Definition at line 43475 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQWAKEUP

#define USBPHY_CTRL_ENIRQWAKEUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_ENIRQWAKEUP_MASK)

Definition at line 43497 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQWAKEUP_MASK

#define USBPHY_CTRL_ENIRQWAKEUP_MASK (0x10000U)

Definition at line 43495 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENIRQWAKEUP_SHIFT

#define USBPHY_CTRL_ENIRQWAKEUP_SHIFT (16U)

Definition at line 43496 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENOTG_ID_CHG_IRQ

#define USBPHY_CTRL_ENOTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_ENOTG_ID_CHG_IRQ_MASK)

Definition at line 43449 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENOTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_ENOTG_ID_CHG_IRQ_MASK (0x1U)

Definition at line 43447 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENOTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_ENOTG_ID_CHG_IRQ_SHIFT (0U)

Definition at line 43448 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENOTGIDDETECT

#define USBPHY_CTRL_ENOTGIDDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_ENOTGIDDETECT_MASK)

Definition at line 43470 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENOTGIDDETECT_MASK

#define USBPHY_CTRL_ENOTGIDDETECT_MASK (0x80U)

Definition at line 43468 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENOTGIDDETECT_SHIFT

#define USBPHY_CTRL_ENOTGIDDETECT_SHIFT (7U)

Definition at line 43469 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENUTMILEVEL2

#define USBPHY_CTRL_ENUTMILEVEL2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_ENUTMILEVEL2_MASK)

Definition at line 43491 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENUTMILEVEL2_MASK

#define USBPHY_CTRL_ENUTMILEVEL2_MASK (0x4000U)

Definition at line 43489 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENUTMILEVEL2_SHIFT

#define USBPHY_CTRL_ENUTMILEVEL2_SHIFT (14U)

Definition at line 43490 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENUTMILEVEL3

#define USBPHY_CTRL_ENUTMILEVEL3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_ENUTMILEVEL3_MASK)

Definition at line 43494 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENUTMILEVEL3_MASK

#define USBPHY_CTRL_ENUTMILEVEL3_MASK (0x8000U)

Definition at line 43492 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENUTMILEVEL3_SHIFT

#define USBPHY_CTRL_ENUTMILEVEL3_SHIFT (15U)

Definition at line 43493 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENVBUSCHG_WKUP

#define USBPHY_CTRL_ENVBUSCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_ENVBUSCHG_WKUP_MASK)

Definition at line 43518 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENVBUSCHG_WKUP_MASK

#define USBPHY_CTRL_ENVBUSCHG_WKUP_MASK (0x800000U)

Definition at line 43516 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENVBUSCHG_WKUP_SHIFT

#define USBPHY_CTRL_ENVBUSCHG_WKUP_SHIFT (23U)

Definition at line 43517 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_FSDLL_RST_EN

#define USBPHY_CTRL_FSDLL_RST_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_FSDLL_RST_EN_MASK)

Definition at line 43521 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_FSDLL_RST_EN_MASK

#define USBPHY_CTRL_FSDLL_RST_EN_MASK (0x1000000U)

Definition at line 43519 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_FSDLL_RST_EN_SHIFT

#define USBPHY_CTRL_FSDLL_RST_EN_SHIFT (24U)

Definition at line 43520 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_HOST_FORCE_LS_SE0

#define USBPHY_CTRL_HOST_FORCE_LS_SE0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_HOST_FORCE_LS_SE0_MASK)

Definition at line 43530 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_HOST_FORCE_LS_SE0_MASK

#define USBPHY_CTRL_HOST_FORCE_LS_SE0_MASK (0x10000000U)

Definition at line 43528 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_HOST_FORCE_LS_SE0_SHIFT

#define USBPHY_CTRL_HOST_FORCE_LS_SE0_SHIFT (28U)

Definition at line 43529 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_HOSTDISCONDETECT_IRQ

#define USBPHY_CTRL_HOSTDISCONDETECT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_HOSTDISCONDETECT_IRQ_MASK)

Definition at line 43458 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_HOSTDISCONDETECT_IRQ_MASK

#define USBPHY_CTRL_HOSTDISCONDETECT_IRQ_MASK (0x8U)

Definition at line 43456 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_HOSTDISCONDETECT_IRQ_SHIFT

#define USBPHY_CTRL_HOSTDISCONDETECT_IRQ_SHIFT (3U)

Definition at line 43457 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_OTG_ID_CHG_IRQ

#define USBPHY_CTRL_OTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_OTG_ID_CHG_IRQ_MASK)

Definition at line 43467 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_OTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_OTG_ID_CHG_IRQ_MASK (0x40U)

Definition at line 43465 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_OTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_OTG_ID_CHG_IRQ_SHIFT (6U)

Definition at line 43466 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_OTG_ID_VALUE

#define USBPHY_CTRL_OTG_ID_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_OTG_ID_VALUE_MASK)

Definition at line 43527 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_OTG_ID_VALUE_MASK

#define USBPHY_CTRL_OTG_ID_VALUE_MASK (0x8000000U)

Definition at line 43525 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_OTG_ID_VALUE_SHIFT

#define USBPHY_CTRL_OTG_ID_VALUE_SHIFT (27U)

Definition at line 43526 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RESUME_IRQ

#define USBPHY_CTRL_RESUME_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_RESUME_IRQ_MASK)

Definition at line 43479 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RESUME_IRQ_MASK

#define USBPHY_CTRL_RESUME_IRQ_MASK (0x400U)

Definition at line 43477 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RESUME_IRQ_SHIFT

#define USBPHY_CTRL_RESUME_IRQ_SHIFT (10U)

Definition at line 43478 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RESUMEIRQSTICKY

#define USBPHY_CTRL_RESUMEIRQSTICKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_RESUMEIRQSTICKY_MASK)

Definition at line 43473 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RESUMEIRQSTICKY_MASK

#define USBPHY_CTRL_RESUMEIRQSTICKY_MASK (0x100U)

Definition at line 43471 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RESUMEIRQSTICKY_SHIFT

#define USBPHY_CTRL_RESUMEIRQSTICKY_SHIFT (8U)

Definition at line 43472 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RSVD1

#define USBPHY_CTRL_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_RSVD1_SHIFT)) & USBPHY_CTRL_RSVD1_MASK)

Definition at line 43524 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RSVD1_MASK

#define USBPHY_CTRL_RSVD1_MASK (0x6000000U)

Definition at line 43522 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_RSVD1_SHIFT

#define USBPHY_CTRL_RSVD1_SHIFT (25U)

Definition at line 43523 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_CLKGATE

#define USBPHY_CTRL_SET_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_CLKGATE_SHIFT)) & USBPHY_CTRL_SET_CLKGATE_MASK)

Definition at line 43633 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_CLKGATE_MASK

#define USBPHY_CTRL_SET_CLKGATE_MASK (0x40000000U)

Definition at line 43631 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_CLKGATE_SHIFT

#define USBPHY_CTRL_SET_CLKGATE_SHIFT (30U)

Definition at line 43632 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DATA_ON_LRADC

#define USBPHY_CTRL_SET_DATA_ON_LRADC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_SET_DATA_ON_LRADC_MASK)

Definition at line 43585 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DATA_ON_LRADC_MASK

#define USBPHY_CTRL_SET_DATA_ON_LRADC_MASK (0x2000U)

Definition at line 43583 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DATA_ON_LRADC_SHIFT

#define USBPHY_CTRL_SET_DATA_ON_LRADC_SHIFT (13U)

Definition at line 43584 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DEVPLUGIN_IRQ

#define USBPHY_CTRL_SET_DEVPLUGIN_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_SET_DEVPLUGIN_IRQ_MASK)

Definition at line 43582 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DEVPLUGIN_IRQ_MASK

#define USBPHY_CTRL_SET_DEVPLUGIN_IRQ_MASK (0x1000U)

Definition at line 43580 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DEVPLUGIN_IRQ_SHIFT

#define USBPHY_CTRL_SET_DEVPLUGIN_IRQ_SHIFT (12U)

Definition at line 43581 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DEVPLUGIN_POLARITY

#define USBPHY_CTRL_SET_DEVPLUGIN_POLARITY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_MASK)

Definition at line 43561 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_MASK

#define USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_MASK (0x20U)

Definition at line 43559 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_SHIFT

#define USBPHY_CTRL_SET_DEVPLUGIN_POLARITY_SHIFT (5U)

Definition at line 43560 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTO_PWRON_PLL

#define USBPHY_CTRL_SET_ENAUTO_PWRON_PLL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_MASK)

Definition at line 43600 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_MASK

#define USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_MASK (0x40000U)

Definition at line 43598 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_SHIFT

#define USBPHY_CTRL_SET_ENAUTO_PWRON_PLL_SHIFT (18U)

Definition at line 43599 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE

#define USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_MASK)

Definition at line 43603 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_MASK

#define USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_MASK (0x80000U)

Definition at line 43601 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_SHIFT

#define USBPHY_CTRL_SET_ENAUTOCLR_CLKGATE_SHIFT (19U)

Definition at line 43602 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD

#define USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_MASK)

Definition at line 43606 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_MASK

#define USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_MASK (0x100000U)

Definition at line 43604 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_SHIFT

#define USBPHY_CTRL_SET_ENAUTOCLR_PHY_PWD_SHIFT (20U)

Definition at line 43605 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENDEVPLUGINDETECT

#define USBPHY_CTRL_SET_ENDEVPLUGINDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_SET_ENDEVPLUGINDETECT_MASK)

Definition at line 43558 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENDEVPLUGINDETECT_MASK

#define USBPHY_CTRL_SET_ENDEVPLUGINDETECT_MASK (0x10U)

Definition at line 43556 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENDEVPLUGINDETECT_SHIFT

#define USBPHY_CTRL_SET_ENDEVPLUGINDETECT_SHIFT (4U)

Definition at line 43557 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENDPDMCHG_WKUP

#define USBPHY_CTRL_SET_ENDPDMCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_SET_ENDPDMCHG_WKUP_MASK)

Definition at line 43609 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENDPDMCHG_WKUP_MASK

#define USBPHY_CTRL_SET_ENDPDMCHG_WKUP_MASK (0x200000U)

Definition at line 43607 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENDPDMCHG_WKUP_SHIFT

#define USBPHY_CTRL_SET_ENDPDMCHG_WKUP_SHIFT (21U)

Definition at line 43608 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENHOSTDISCONDETECT

#define USBPHY_CTRL_SET_ENHOSTDISCONDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_SET_ENHOSTDISCONDETECT_MASK)

Definition at line 43549 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENHOSTDISCONDETECT_MASK

#define USBPHY_CTRL_SET_ENHOSTDISCONDETECT_MASK (0x2U)

Definition at line 43547 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENHOSTDISCONDETECT_SHIFT

#define USBPHY_CTRL_SET_ENHOSTDISCONDETECT_SHIFT (1U)

Definition at line 43548 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIDCHG_WKUP

#define USBPHY_CTRL_SET_ENIDCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_SET_ENIDCHG_WKUP_MASK)

Definition at line 43612 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIDCHG_WKUP_MASK

#define USBPHY_CTRL_SET_ENIDCHG_WKUP_MASK (0x400000U)

Definition at line 43610 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIDCHG_WKUP_SHIFT

#define USBPHY_CTRL_SET_ENIDCHG_WKUP_SHIFT (22U)

Definition at line 43611 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQDEVPLUGIN

#define USBPHY_CTRL_SET_ENIRQDEVPLUGIN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_SET_ENIRQDEVPLUGIN_MASK)

Definition at line 43579 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQDEVPLUGIN_MASK

#define USBPHY_CTRL_SET_ENIRQDEVPLUGIN_MASK (0x800U)

Definition at line 43577 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQDEVPLUGIN_SHIFT

#define USBPHY_CTRL_SET_ENIRQDEVPLUGIN_SHIFT (11U)

Definition at line 43578 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQHOSTDISCON

#define USBPHY_CTRL_SET_ENIRQHOSTDISCON | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_SET_ENIRQHOSTDISCON_MASK)

Definition at line 43552 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQHOSTDISCON_MASK

#define USBPHY_CTRL_SET_ENIRQHOSTDISCON_MASK (0x4U)

Definition at line 43550 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQHOSTDISCON_SHIFT

#define USBPHY_CTRL_SET_ENIRQHOSTDISCON_SHIFT (2U)

Definition at line 43551 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQRESUMEDETECT

#define USBPHY_CTRL_SET_ENIRQRESUMEDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_SET_ENIRQRESUMEDETECT_MASK)

Definition at line 43573 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQRESUMEDETECT_MASK

#define USBPHY_CTRL_SET_ENIRQRESUMEDETECT_MASK (0x200U)

Definition at line 43571 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQRESUMEDETECT_SHIFT

#define USBPHY_CTRL_SET_ENIRQRESUMEDETECT_SHIFT (9U)

Definition at line 43572 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQWAKEUP

#define USBPHY_CTRL_SET_ENIRQWAKEUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_SET_ENIRQWAKEUP_MASK)

Definition at line 43594 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQWAKEUP_MASK

#define USBPHY_CTRL_SET_ENIRQWAKEUP_MASK (0x10000U)

Definition at line 43592 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENIRQWAKEUP_SHIFT

#define USBPHY_CTRL_SET_ENIRQWAKEUP_SHIFT (16U)

Definition at line 43593 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ

#define USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_MASK)

Definition at line 43546 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_MASK (0x1U)

Definition at line 43544 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_SET_ENOTG_ID_CHG_IRQ_SHIFT (0U)

Definition at line 43545 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENOTGIDDETECT

#define USBPHY_CTRL_SET_ENOTGIDDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_SET_ENOTGIDDETECT_MASK)

Definition at line 43567 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENOTGIDDETECT_MASK

#define USBPHY_CTRL_SET_ENOTGIDDETECT_MASK (0x80U)

Definition at line 43565 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENOTGIDDETECT_SHIFT

#define USBPHY_CTRL_SET_ENOTGIDDETECT_SHIFT (7U)

Definition at line 43566 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENUTMILEVEL2

#define USBPHY_CTRL_SET_ENUTMILEVEL2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_SET_ENUTMILEVEL2_MASK)

Definition at line 43588 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENUTMILEVEL2_MASK

#define USBPHY_CTRL_SET_ENUTMILEVEL2_MASK (0x4000U)

Definition at line 43586 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENUTMILEVEL2_SHIFT

#define USBPHY_CTRL_SET_ENUTMILEVEL2_SHIFT (14U)

Definition at line 43587 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENUTMILEVEL3

#define USBPHY_CTRL_SET_ENUTMILEVEL3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_SET_ENUTMILEVEL3_MASK)

Definition at line 43591 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENUTMILEVEL3_MASK

#define USBPHY_CTRL_SET_ENUTMILEVEL3_MASK (0x8000U)

Definition at line 43589 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENUTMILEVEL3_SHIFT

#define USBPHY_CTRL_SET_ENUTMILEVEL3_SHIFT (15U)

Definition at line 43590 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENVBUSCHG_WKUP

#define USBPHY_CTRL_SET_ENVBUSCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_SET_ENVBUSCHG_WKUP_MASK)

Definition at line 43615 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENVBUSCHG_WKUP_MASK

#define USBPHY_CTRL_SET_ENVBUSCHG_WKUP_MASK (0x800000U)

Definition at line 43613 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_ENVBUSCHG_WKUP_SHIFT

#define USBPHY_CTRL_SET_ENVBUSCHG_WKUP_SHIFT (23U)

Definition at line 43614 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_FSDLL_RST_EN

#define USBPHY_CTRL_SET_FSDLL_RST_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_SET_FSDLL_RST_EN_MASK)

Definition at line 43618 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_FSDLL_RST_EN_MASK

#define USBPHY_CTRL_SET_FSDLL_RST_EN_MASK (0x1000000U)

Definition at line 43616 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_FSDLL_RST_EN_SHIFT

#define USBPHY_CTRL_SET_FSDLL_RST_EN_SHIFT (24U)

Definition at line 43617 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_HOST_FORCE_LS_SE0

#define USBPHY_CTRL_SET_HOST_FORCE_LS_SE0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_MASK)

Definition at line 43627 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_MASK

#define USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_MASK (0x10000000U)

Definition at line 43625 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_SHIFT

#define USBPHY_CTRL_SET_HOST_FORCE_LS_SE0_SHIFT (28U)

Definition at line 43626 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ

#define USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_MASK)

Definition at line 43555 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_MASK

#define USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_MASK (0x8U)

Definition at line 43553 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_SHIFT

#define USBPHY_CTRL_SET_HOSTDISCONDETECT_IRQ_SHIFT (3U)

Definition at line 43554 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_OTG_ID_CHG_IRQ

#define USBPHY_CTRL_SET_OTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_MASK)

Definition at line 43564 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_MASK (0x40U)

Definition at line 43562 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_SET_OTG_ID_CHG_IRQ_SHIFT (6U)

Definition at line 43563 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_OTG_ID_VALUE

#define USBPHY_CTRL_SET_OTG_ID_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_SET_OTG_ID_VALUE_MASK)

Definition at line 43624 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_OTG_ID_VALUE_MASK

#define USBPHY_CTRL_SET_OTG_ID_VALUE_MASK (0x8000000U)

Definition at line 43622 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_OTG_ID_VALUE_SHIFT

#define USBPHY_CTRL_SET_OTG_ID_VALUE_SHIFT (27U)

Definition at line 43623 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RESUME_IRQ

#define USBPHY_CTRL_SET_RESUME_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_SET_RESUME_IRQ_MASK)

Definition at line 43576 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RESUME_IRQ_MASK

#define USBPHY_CTRL_SET_RESUME_IRQ_MASK (0x400U)

Definition at line 43574 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RESUME_IRQ_SHIFT

#define USBPHY_CTRL_SET_RESUME_IRQ_SHIFT (10U)

Definition at line 43575 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RESUMEIRQSTICKY

#define USBPHY_CTRL_SET_RESUMEIRQSTICKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_SET_RESUMEIRQSTICKY_MASK)

Definition at line 43570 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RESUMEIRQSTICKY_MASK

#define USBPHY_CTRL_SET_RESUMEIRQSTICKY_MASK (0x100U)

Definition at line 43568 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RESUMEIRQSTICKY_SHIFT

#define USBPHY_CTRL_SET_RESUMEIRQSTICKY_SHIFT (8U)

Definition at line 43569 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RSVD1

#define USBPHY_CTRL_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_RSVD1_SHIFT)) & USBPHY_CTRL_SET_RSVD1_MASK)

Definition at line 43621 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RSVD1_MASK

#define USBPHY_CTRL_SET_RSVD1_MASK (0x6000000U)

Definition at line 43619 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_RSVD1_SHIFT

#define USBPHY_CTRL_SET_RSVD1_SHIFT (25U)

Definition at line 43620 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_SFTRST

#define USBPHY_CTRL_SET_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_SFTRST_SHIFT)) & USBPHY_CTRL_SET_SFTRST_MASK)

Definition at line 43636 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_SFTRST_MASK

#define USBPHY_CTRL_SET_SFTRST_MASK (0x80000000U)

Definition at line 43634 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_SFTRST_SHIFT

#define USBPHY_CTRL_SET_SFTRST_SHIFT (31U)

Definition at line 43635 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_UTMI_SUSPENDM

#define USBPHY_CTRL_SET_UTMI_SUSPENDM | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_SET_UTMI_SUSPENDM_MASK)

Definition at line 43630 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_UTMI_SUSPENDM_MASK

#define USBPHY_CTRL_SET_UTMI_SUSPENDM_MASK (0x20000000U)

Definition at line 43628 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_UTMI_SUSPENDM_SHIFT

#define USBPHY_CTRL_SET_UTMI_SUSPENDM_SHIFT (29U)

Definition at line 43629 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_WAKEUP_IRQ

#define USBPHY_CTRL_SET_WAKEUP_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SET_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_SET_WAKEUP_IRQ_MASK)

Definition at line 43597 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_WAKEUP_IRQ_MASK

#define USBPHY_CTRL_SET_WAKEUP_IRQ_MASK (0x20000U)

Definition at line 43595 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SET_WAKEUP_IRQ_SHIFT

#define USBPHY_CTRL_SET_WAKEUP_IRQ_SHIFT (17U)

Definition at line 43596 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SFTRST

#define USBPHY_CTRL_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_SFTRST_SHIFT)) & USBPHY_CTRL_SFTRST_MASK)

Definition at line 43539 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SFTRST_MASK

#define USBPHY_CTRL_SFTRST_MASK (0x80000000U)

Definition at line 43537 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_SFTRST_SHIFT

#define USBPHY_CTRL_SFTRST_SHIFT (31U)

Definition at line 43538 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_CLKGATE

#define USBPHY_CTRL_TOG_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_CLKGATE_SHIFT)) & USBPHY_CTRL_TOG_CLKGATE_MASK)

Definition at line 43827 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_CLKGATE_MASK

#define USBPHY_CTRL_TOG_CLKGATE_MASK (0x40000000U)

Definition at line 43825 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_CLKGATE_SHIFT

#define USBPHY_CTRL_TOG_CLKGATE_SHIFT (30U)

Definition at line 43826 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DATA_ON_LRADC

#define USBPHY_CTRL_TOG_DATA_ON_LRADC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_DATA_ON_LRADC_SHIFT)) & USBPHY_CTRL_TOG_DATA_ON_LRADC_MASK)

Definition at line 43779 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DATA_ON_LRADC_MASK

#define USBPHY_CTRL_TOG_DATA_ON_LRADC_MASK (0x2000U)

Definition at line 43777 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DATA_ON_LRADC_SHIFT

#define USBPHY_CTRL_TOG_DATA_ON_LRADC_SHIFT (13U)

Definition at line 43778 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DEVPLUGIN_IRQ

#define USBPHY_CTRL_TOG_DEVPLUGIN_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_SHIFT)) & USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_MASK)

Definition at line 43776 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_MASK

#define USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_MASK (0x1000U)

Definition at line 43774 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_SHIFT

#define USBPHY_CTRL_TOG_DEVPLUGIN_IRQ_SHIFT (12U)

Definition at line 43775 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY

#define USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_SHIFT)) & USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_MASK)

Definition at line 43755 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_MASK

#define USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_MASK (0x20U)

Definition at line 43753 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_SHIFT

#define USBPHY_CTRL_TOG_DEVPLUGIN_POLARITY_SHIFT (5U)

Definition at line 43754 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL

#define USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_SHIFT)) & USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_MASK)

Definition at line 43794 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_MASK

#define USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_MASK (0x40000U)

Definition at line 43792 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_SHIFT

#define USBPHY_CTRL_TOG_ENAUTO_PWRON_PLL_SHIFT (18U)

Definition at line 43793 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE

#define USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_SHIFT)) & USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_MASK)

Definition at line 43797 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_MASK

#define USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_MASK (0x80000U)

Definition at line 43795 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_SHIFT

#define USBPHY_CTRL_TOG_ENAUTOCLR_CLKGATE_SHIFT (19U)

Definition at line 43796 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD

#define USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_SHIFT)) & USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_MASK)

Definition at line 43800 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_MASK

#define USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_MASK (0x100000U)

Definition at line 43798 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_SHIFT

#define USBPHY_CTRL_TOG_ENAUTOCLR_PHY_PWD_SHIFT (20U)

Definition at line 43799 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENDEVPLUGINDETECT

#define USBPHY_CTRL_TOG_ENDEVPLUGINDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_MASK)

Definition at line 43752 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_MASK

#define USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_MASK (0x10U)

Definition at line 43750 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_SHIFT

#define USBPHY_CTRL_TOG_ENDEVPLUGINDETECT_SHIFT (4U)

Definition at line 43751 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENDPDMCHG_WKUP

#define USBPHY_CTRL_TOG_ENDPDMCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_SHIFT)) & USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_MASK)

Definition at line 43803 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_MASK

#define USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_MASK (0x200000U)

Definition at line 43801 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_SHIFT

#define USBPHY_CTRL_TOG_ENDPDMCHG_WKUP_SHIFT (21U)

Definition at line 43802 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENHOSTDISCONDETECT

#define USBPHY_CTRL_TOG_ENHOSTDISCONDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_MASK)

Definition at line 43743 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_MASK

#define USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_MASK (0x2U)

Definition at line 43741 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_SHIFT

#define USBPHY_CTRL_TOG_ENHOSTDISCONDETECT_SHIFT (1U)

Definition at line 43742 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIDCHG_WKUP

#define USBPHY_CTRL_TOG_ENIDCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIDCHG_WKUP_SHIFT)) & USBPHY_CTRL_TOG_ENIDCHG_WKUP_MASK)

Definition at line 43806 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIDCHG_WKUP_MASK

#define USBPHY_CTRL_TOG_ENIDCHG_WKUP_MASK (0x400000U)

Definition at line 43804 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIDCHG_WKUP_SHIFT

#define USBPHY_CTRL_TOG_ENIDCHG_WKUP_SHIFT (22U)

Definition at line 43805 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQDEVPLUGIN

#define USBPHY_CTRL_TOG_ENIRQDEVPLUGIN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_SHIFT)) & USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_MASK)

Definition at line 43773 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_MASK

#define USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_MASK (0x800U)

Definition at line 43771 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_SHIFT

#define USBPHY_CTRL_TOG_ENIRQDEVPLUGIN_SHIFT (11U)

Definition at line 43772 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQHOSTDISCON

#define USBPHY_CTRL_TOG_ENIRQHOSTDISCON | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQHOSTDISCON_SHIFT)) & USBPHY_CTRL_TOG_ENIRQHOSTDISCON_MASK)

Definition at line 43746 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQHOSTDISCON_MASK

#define USBPHY_CTRL_TOG_ENIRQHOSTDISCON_MASK (0x4U)

Definition at line 43744 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQHOSTDISCON_SHIFT

#define USBPHY_CTRL_TOG_ENIRQHOSTDISCON_SHIFT (2U)

Definition at line 43745 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQRESUMEDETECT

#define USBPHY_CTRL_TOG_ENIRQRESUMEDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_MASK)

Definition at line 43767 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_MASK

#define USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_MASK (0x200U)

Definition at line 43765 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_SHIFT

#define USBPHY_CTRL_TOG_ENIRQRESUMEDETECT_SHIFT (9U)

Definition at line 43766 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQWAKEUP

#define USBPHY_CTRL_TOG_ENIRQWAKEUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENIRQWAKEUP_SHIFT)) & USBPHY_CTRL_TOG_ENIRQWAKEUP_MASK)

Definition at line 43788 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQWAKEUP_MASK

#define USBPHY_CTRL_TOG_ENIRQWAKEUP_MASK (0x10000U)

Definition at line 43786 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENIRQWAKEUP_SHIFT

#define USBPHY_CTRL_TOG_ENIRQWAKEUP_SHIFT (16U)

Definition at line 43787 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ

#define USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_MASK)

Definition at line 43740 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_MASK (0x1U)

Definition at line 43738 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_TOG_ENOTG_ID_CHG_IRQ_SHIFT (0U)

Definition at line 43739 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENOTGIDDETECT

#define USBPHY_CTRL_TOG_ENOTGIDDETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENOTGIDDETECT_SHIFT)) & USBPHY_CTRL_TOG_ENOTGIDDETECT_MASK)

Definition at line 43761 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENOTGIDDETECT_MASK

#define USBPHY_CTRL_TOG_ENOTGIDDETECT_MASK (0x80U)

Definition at line 43759 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENOTGIDDETECT_SHIFT

#define USBPHY_CTRL_TOG_ENOTGIDDETECT_SHIFT (7U)

Definition at line 43760 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENUTMILEVEL2

#define USBPHY_CTRL_TOG_ENUTMILEVEL2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENUTMILEVEL2_SHIFT)) & USBPHY_CTRL_TOG_ENUTMILEVEL2_MASK)

Definition at line 43782 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENUTMILEVEL2_MASK

#define USBPHY_CTRL_TOG_ENUTMILEVEL2_MASK (0x4000U)

Definition at line 43780 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENUTMILEVEL2_SHIFT

#define USBPHY_CTRL_TOG_ENUTMILEVEL2_SHIFT (14U)

Definition at line 43781 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENUTMILEVEL3

#define USBPHY_CTRL_TOG_ENUTMILEVEL3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENUTMILEVEL3_SHIFT)) & USBPHY_CTRL_TOG_ENUTMILEVEL3_MASK)

Definition at line 43785 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENUTMILEVEL3_MASK

#define USBPHY_CTRL_TOG_ENUTMILEVEL3_MASK (0x8000U)

Definition at line 43783 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENUTMILEVEL3_SHIFT

#define USBPHY_CTRL_TOG_ENUTMILEVEL3_SHIFT (15U)

Definition at line 43784 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENVBUSCHG_WKUP

#define USBPHY_CTRL_TOG_ENVBUSCHG_WKUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_SHIFT)) & USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_MASK)

Definition at line 43809 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_MASK

#define USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_MASK (0x800000U)

Definition at line 43807 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_SHIFT

#define USBPHY_CTRL_TOG_ENVBUSCHG_WKUP_SHIFT (23U)

Definition at line 43808 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_FSDLL_RST_EN

#define USBPHY_CTRL_TOG_FSDLL_RST_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_FSDLL_RST_EN_SHIFT)) & USBPHY_CTRL_TOG_FSDLL_RST_EN_MASK)

Definition at line 43812 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_FSDLL_RST_EN_MASK

#define USBPHY_CTRL_TOG_FSDLL_RST_EN_MASK (0x1000000U)

Definition at line 43810 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_FSDLL_RST_EN_SHIFT

#define USBPHY_CTRL_TOG_FSDLL_RST_EN_SHIFT (24U)

Definition at line 43811 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0

#define USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_SHIFT)) & USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_MASK)

Definition at line 43821 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_MASK

#define USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_MASK (0x10000000U)

Definition at line 43819 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_SHIFT

#define USBPHY_CTRL_TOG_HOST_FORCE_LS_SE0_SHIFT (28U)

Definition at line 43820 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ

#define USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_SHIFT)) & USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_MASK)

Definition at line 43749 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_MASK

#define USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_MASK (0x8U)

Definition at line 43747 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_SHIFT

#define USBPHY_CTRL_TOG_HOSTDISCONDETECT_IRQ_SHIFT (3U)

Definition at line 43748 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ

#define USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_SHIFT)) & USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_MASK)

Definition at line 43758 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_MASK

#define USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_MASK (0x40U)

Definition at line 43756 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_SHIFT

#define USBPHY_CTRL_TOG_OTG_ID_CHG_IRQ_SHIFT (6U)

Definition at line 43757 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_OTG_ID_VALUE

#define USBPHY_CTRL_TOG_OTG_ID_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_OTG_ID_VALUE_SHIFT)) & USBPHY_CTRL_TOG_OTG_ID_VALUE_MASK)

Definition at line 43818 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_OTG_ID_VALUE_MASK

#define USBPHY_CTRL_TOG_OTG_ID_VALUE_MASK (0x8000000U)

Definition at line 43816 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_OTG_ID_VALUE_SHIFT

#define USBPHY_CTRL_TOG_OTG_ID_VALUE_SHIFT (27U)

Definition at line 43817 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RESUME_IRQ

#define USBPHY_CTRL_TOG_RESUME_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_RESUME_IRQ_SHIFT)) & USBPHY_CTRL_TOG_RESUME_IRQ_MASK)

Definition at line 43770 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RESUME_IRQ_MASK

#define USBPHY_CTRL_TOG_RESUME_IRQ_MASK (0x400U)

Definition at line 43768 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RESUME_IRQ_SHIFT

#define USBPHY_CTRL_TOG_RESUME_IRQ_SHIFT (10U)

Definition at line 43769 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RESUMEIRQSTICKY

#define USBPHY_CTRL_TOG_RESUMEIRQSTICKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_RESUMEIRQSTICKY_SHIFT)) & USBPHY_CTRL_TOG_RESUMEIRQSTICKY_MASK)

Definition at line 43764 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RESUMEIRQSTICKY_MASK

#define USBPHY_CTRL_TOG_RESUMEIRQSTICKY_MASK (0x100U)

Definition at line 43762 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RESUMEIRQSTICKY_SHIFT

#define USBPHY_CTRL_TOG_RESUMEIRQSTICKY_SHIFT (8U)

Definition at line 43763 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RSVD1

#define USBPHY_CTRL_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_RSVD1_SHIFT)) & USBPHY_CTRL_TOG_RSVD1_MASK)

Definition at line 43815 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RSVD1_MASK

#define USBPHY_CTRL_TOG_RSVD1_MASK (0x6000000U)

Definition at line 43813 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_RSVD1_SHIFT

#define USBPHY_CTRL_TOG_RSVD1_SHIFT (25U)

Definition at line 43814 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_SFTRST

#define USBPHY_CTRL_TOG_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_SFTRST_SHIFT)) & USBPHY_CTRL_TOG_SFTRST_MASK)

Definition at line 43830 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_SFTRST_MASK

#define USBPHY_CTRL_TOG_SFTRST_MASK (0x80000000U)

Definition at line 43828 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_SFTRST_SHIFT

#define USBPHY_CTRL_TOG_SFTRST_SHIFT (31U)

Definition at line 43829 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_UTMI_SUSPENDM

#define USBPHY_CTRL_TOG_UTMI_SUSPENDM | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_TOG_UTMI_SUSPENDM_MASK)

Definition at line 43824 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_UTMI_SUSPENDM_MASK

#define USBPHY_CTRL_TOG_UTMI_SUSPENDM_MASK (0x20000000U)

Definition at line 43822 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_UTMI_SUSPENDM_SHIFT

#define USBPHY_CTRL_TOG_UTMI_SUSPENDM_SHIFT (29U)

Definition at line 43823 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_WAKEUP_IRQ

#define USBPHY_CTRL_TOG_WAKEUP_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_TOG_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_TOG_WAKEUP_IRQ_MASK)

Definition at line 43791 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_WAKEUP_IRQ_MASK

#define USBPHY_CTRL_TOG_WAKEUP_IRQ_MASK (0x20000U)

Definition at line 43789 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_TOG_WAKEUP_IRQ_SHIFT

#define USBPHY_CTRL_TOG_WAKEUP_IRQ_SHIFT (17U)

Definition at line 43790 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_UTMI_SUSPENDM

#define USBPHY_CTRL_UTMI_SUSPENDM | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_UTMI_SUSPENDM_SHIFT)) & USBPHY_CTRL_UTMI_SUSPENDM_MASK)

Definition at line 43533 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_UTMI_SUSPENDM_MASK

#define USBPHY_CTRL_UTMI_SUSPENDM_MASK (0x20000000U)

Definition at line 43531 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_UTMI_SUSPENDM_SHIFT

#define USBPHY_CTRL_UTMI_SUSPENDM_SHIFT (29U)

Definition at line 43532 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_WAKEUP_IRQ

#define USBPHY_CTRL_WAKEUP_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_CTRL_WAKEUP_IRQ_SHIFT)) & USBPHY_CTRL_WAKEUP_IRQ_MASK)

Definition at line 43500 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_WAKEUP_IRQ_MASK

#define USBPHY_CTRL_WAKEUP_IRQ_MASK (0x20000U)

Definition at line 43498 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_WAKEUP_IRQ_SHIFT

#define USBPHY_CTRL_WAKEUP_IRQ_SHIFT (17U)

Definition at line 43499 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT

#define USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_SHIFT)) & USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_MASK)

Definition at line 44064 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_MASK

#define USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_MASK (0xFFFFU)

Definition at line 44062 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_SHIFT

#define USBPHY_DEBUG0_STATUS_LOOP_BACK_FAIL_COUNT_SHIFT (0U)

Definition at line 44063 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_SQUELCH_COUNT

#define USBPHY_DEBUG0_STATUS_SQUELCH_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_SHIFT)) & USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_MASK)

Definition at line 44070 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_MASK

#define USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_MASK (0xFC000000U)

Definition at line 44068 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_SHIFT

#define USBPHY_DEBUG0_STATUS_SQUELCH_COUNT_SHIFT (26U)

Definition at line 44069 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT

#define USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_SHIFT)) & USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_MASK)

Definition at line 44067 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_MASK

#define USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_MASK (0x3FF0000U)

Definition at line 44065 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_SHIFT

#define USBPHY_DEBUG0_STATUS_UTMI_RXERROR_FAIL_COUNT_SHIFT (16U)

Definition at line 44066 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_ENTAILADJVD

#define USBPHY_DEBUG1_CLR_ENTAILADJVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_CLR_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_CLR_ENTAILADJVD_MASK)

Definition at line 44106 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_ENTAILADJVD_MASK

#define USBPHY_DEBUG1_CLR_ENTAILADJVD_MASK (0x6000U)

Definition at line 44104 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_ENTAILADJVD_SHIFT

#define USBPHY_DEBUG1_CLR_ENTAILADJVD_SHIFT (13U)

Definition at line 44105 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_RSVD0

#define USBPHY_DEBUG1_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_CLR_RSVD0_SHIFT)) & USBPHY_DEBUG1_CLR_RSVD0_MASK)

Definition at line 44103 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_RSVD0_MASK

#define USBPHY_DEBUG1_CLR_RSVD0_MASK (0x1FFFU)

Definition at line 44101 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_RSVD0_SHIFT

#define USBPHY_DEBUG1_CLR_RSVD0_SHIFT (0U)

Definition at line 44102 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_RSVD1

#define USBPHY_DEBUG1_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_CLR_RSVD1_SHIFT)) & USBPHY_DEBUG1_CLR_RSVD1_MASK)

Definition at line 44109 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_RSVD1_MASK

#define USBPHY_DEBUG1_CLR_RSVD1_MASK (0xFFFF8000U)

Definition at line 44107 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_CLR_RSVD1_SHIFT

#define USBPHY_DEBUG1_CLR_RSVD1_SHIFT (15U)

Definition at line 44108 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_ENTAILADJVD

#define USBPHY_DEBUG1_ENTAILADJVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_ENTAILADJVD_MASK)

Definition at line 44080 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_ENTAILADJVD_MASK

#define USBPHY_DEBUG1_ENTAILADJVD_MASK (0x6000U)

Definition at line 44078 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_ENTAILADJVD_SHIFT

#define USBPHY_DEBUG1_ENTAILADJVD_SHIFT (13U)

Definition at line 44079 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_RSVD0

#define USBPHY_DEBUG1_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_RSVD0_SHIFT)) & USBPHY_DEBUG1_RSVD0_MASK)

Definition at line 44077 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_RSVD0_MASK

#define USBPHY_DEBUG1_RSVD0_MASK (0x1FFFU)

Definition at line 44075 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_RSVD0_SHIFT

#define USBPHY_DEBUG1_RSVD0_SHIFT (0U)

Definition at line 44076 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_RSVD1

#define USBPHY_DEBUG1_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_RSVD1_SHIFT)) & USBPHY_DEBUG1_RSVD1_MASK)

Definition at line 44083 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_RSVD1_MASK

#define USBPHY_DEBUG1_RSVD1_MASK (0xFFFF8000U)

Definition at line 44081 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_RSVD1_SHIFT

#define USBPHY_DEBUG1_RSVD1_SHIFT (15U)

Definition at line 44082 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_ENTAILADJVD

#define USBPHY_DEBUG1_SET_ENTAILADJVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_SET_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_SET_ENTAILADJVD_MASK)

Definition at line 44093 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_ENTAILADJVD_MASK

#define USBPHY_DEBUG1_SET_ENTAILADJVD_MASK (0x6000U)

Definition at line 44091 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_ENTAILADJVD_SHIFT

#define USBPHY_DEBUG1_SET_ENTAILADJVD_SHIFT (13U)

Definition at line 44092 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_RSVD0

#define USBPHY_DEBUG1_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_SET_RSVD0_SHIFT)) & USBPHY_DEBUG1_SET_RSVD0_MASK)

Definition at line 44090 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_RSVD0_MASK

#define USBPHY_DEBUG1_SET_RSVD0_MASK (0x1FFFU)

Definition at line 44088 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_RSVD0_SHIFT

#define USBPHY_DEBUG1_SET_RSVD0_SHIFT (0U)

Definition at line 44089 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_RSVD1

#define USBPHY_DEBUG1_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_SET_RSVD1_SHIFT)) & USBPHY_DEBUG1_SET_RSVD1_MASK)

Definition at line 44096 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_RSVD1_MASK

#define USBPHY_DEBUG1_SET_RSVD1_MASK (0xFFFF8000U)

Definition at line 44094 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_SET_RSVD1_SHIFT

#define USBPHY_DEBUG1_SET_RSVD1_SHIFT (15U)

Definition at line 44095 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_ENTAILADJVD

#define USBPHY_DEBUG1_TOG_ENTAILADJVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_TOG_ENTAILADJVD_SHIFT)) & USBPHY_DEBUG1_TOG_ENTAILADJVD_MASK)

Definition at line 44119 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_ENTAILADJVD_MASK

#define USBPHY_DEBUG1_TOG_ENTAILADJVD_MASK (0x6000U)

Definition at line 44117 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_ENTAILADJVD_SHIFT

#define USBPHY_DEBUG1_TOG_ENTAILADJVD_SHIFT (13U)

Definition at line 44118 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_RSVD0

#define USBPHY_DEBUG1_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_TOG_RSVD0_SHIFT)) & USBPHY_DEBUG1_TOG_RSVD0_MASK)

Definition at line 44116 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_RSVD0_MASK

#define USBPHY_DEBUG1_TOG_RSVD0_MASK (0x1FFFU)

Definition at line 44114 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_RSVD0_SHIFT

#define USBPHY_DEBUG1_TOG_RSVD0_SHIFT (0U)

Definition at line 44115 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_RSVD1

#define USBPHY_DEBUG1_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG1_TOG_RSVD1_SHIFT)) & USBPHY_DEBUG1_TOG_RSVD1_MASK)

Definition at line 44122 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_RSVD1_MASK

#define USBPHY_DEBUG1_TOG_RSVD1_MASK (0xFFFF8000U)

Definition at line 44120 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG1_TOG_RSVD1_SHIFT

#define USBPHY_DEBUG1_TOG_RSVD1_SHIFT (15U)

Definition at line 44121 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLKGATE

#define USBPHY_DEBUG_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLKGATE_SHIFT)) & USBPHY_DEBUG_CLKGATE_MASK)

Definition at line 43907 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLKGATE_MASK

#define USBPHY_DEBUG_CLKGATE_MASK (0x40000000U)

Definition at line 43905 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLKGATE_SHIFT

#define USBPHY_DEBUG_CLKGATE_SHIFT (30U)

Definition at line 43906 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_CLKGATE

#define USBPHY_DEBUG_CLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_CLKGATE_SHIFT)) & USBPHY_DEBUG_CLR_CLKGATE_MASK)

Definition at line 44005 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_CLKGATE_MASK

#define USBPHY_DEBUG_CLR_CLKGATE_MASK (0x40000000U)

Definition at line 44003 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_CLKGATE_SHIFT

#define USBPHY_DEBUG_CLR_CLKGATE_SHIFT (30U)

Definition at line 44004 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD

#define USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_MASK)

Definition at line 43969 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_MASK

#define USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_MASK (0x2U)

Definition at line 43967 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_SHIFT

#define USBPHY_DEBUG_CLR_DEBUG_INTERFACE_HOLD_SHIFT (1U)

Definition at line 43968 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENHSTPULLDOWN

#define USBPHY_DEBUG_CLR_ENHSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_CLR_ENHSTPULLDOWN_MASK)

Definition at line 43975 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENHSTPULLDOWN_MASK

#define USBPHY_DEBUG_CLR_ENHSTPULLDOWN_MASK (0x30U)

Definition at line 43973 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENHSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_CLR_ENHSTPULLDOWN_SHIFT (4U)

Definition at line 43974 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENSQUELCHRESET

#define USBPHY_DEBUG_CLR_ENSQUELCHRESET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_CLR_ENSQUELCHRESET_MASK)

Definition at line 43996 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENSQUELCHRESET_MASK

#define USBPHY_DEBUG_CLR_ENSQUELCHRESET_MASK (0x1000000U)

Definition at line 43994 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENSQUELCHRESET_SHIFT

#define USBPHY_DEBUG_CLR_ENSQUELCHRESET_SHIFT (24U)

Definition at line 43995 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENTX2RXCOUNT

#define USBPHY_DEBUG_CLR_ENTX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_CLR_ENTX2RXCOUNT_MASK)

Definition at line 43984 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENTX2RXCOUNT_MASK

#define USBPHY_DEBUG_CLR_ENTX2RXCOUNT_MASK (0x1000U)

Definition at line 43982 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_ENTX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_CLR_ENTX2RXCOUNT_SHIFT (12U)

Definition at line 43983 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG

#define USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_MASK)

Definition at line 44002 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_MASK

#define USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_MASK (0x20000000U)

Definition at line 44000 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_SHIFT

#define USBPHY_DEBUG_CLR_HOST_RESUME_DEBUG_SHIFT (29U)

Definition at line 44001 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_HSTPULLDOWN

#define USBPHY_DEBUG_CLR_HSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_CLR_HSTPULLDOWN_MASK)

Definition at line 43972 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_HSTPULLDOWN_MASK

#define USBPHY_DEBUG_CLR_HSTPULLDOWN_MASK (0xCU)

Definition at line 43970 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_HSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_CLR_HSTPULLDOWN_SHIFT (2U)

Definition at line 43971 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_OTGIDPIOLOCK

#define USBPHY_DEBUG_CLR_OTGIDPIOLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_CLR_OTGIDPIOLOCK_MASK)

Definition at line 43966 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_OTGIDPIOLOCK_MASK

#define USBPHY_DEBUG_CLR_OTGIDPIOLOCK_MASK (0x1U)

Definition at line 43964 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_OTGIDPIOLOCK_SHIFT

#define USBPHY_DEBUG_CLR_OTGIDPIOLOCK_SHIFT (0U)

Definition at line 43965 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD0

#define USBPHY_DEBUG_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD0_SHIFT)) & USBPHY_DEBUG_CLR_RSVD0_MASK)

Definition at line 43978 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD0_MASK

#define USBPHY_DEBUG_CLR_RSVD0_MASK (0xC0U)

Definition at line 43976 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD0_SHIFT

#define USBPHY_DEBUG_CLR_RSVD0_SHIFT (6U)

Definition at line 43977 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD1

#define USBPHY_DEBUG_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD1_SHIFT)) & USBPHY_DEBUG_CLR_RSVD1_MASK)

Definition at line 43987 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD1_MASK

#define USBPHY_DEBUG_CLR_RSVD1_MASK (0xE000U)

Definition at line 43985 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD1_SHIFT

#define USBPHY_DEBUG_CLR_RSVD1_SHIFT (13U)

Definition at line 43986 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD2

#define USBPHY_DEBUG_CLR_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD2_SHIFT)) & USBPHY_DEBUG_CLR_RSVD2_MASK)

Definition at line 43993 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD2_MASK

#define USBPHY_DEBUG_CLR_RSVD2_MASK (0xE00000U)

Definition at line 43991 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD2_SHIFT

#define USBPHY_DEBUG_CLR_RSVD2_SHIFT (21U)

Definition at line 43992 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD3

#define USBPHY_DEBUG_CLR_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_RSVD3_SHIFT)) & USBPHY_DEBUG_CLR_RSVD3_MASK)

Definition at line 44008 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD3_MASK

#define USBPHY_DEBUG_CLR_RSVD3_MASK (0x80000000U)

Definition at line 44006 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_RSVD3_SHIFT

#define USBPHY_DEBUG_CLR_RSVD3_SHIFT (31U)

Definition at line 44007 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT

#define USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_MASK)

Definition at line 43990 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_MASK

#define USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_MASK (0x1F0000U)

Definition at line 43988 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_SHIFT

#define USBPHY_DEBUG_CLR_SQUELCHRESETCOUNT_SHIFT (16U)

Definition at line 43989 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH

#define USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_MASK)

Definition at line 43999 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_MASK

#define USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_MASK (0x1E000000U)

Definition at line 43997 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_SHIFT

#define USBPHY_DEBUG_CLR_SQUELCHRESETLENGTH_SHIFT (25U)

Definition at line 43998 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_TX2RXCOUNT

#define USBPHY_DEBUG_CLR_TX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_CLR_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_CLR_TX2RXCOUNT_MASK)

Definition at line 43981 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_TX2RXCOUNT_MASK

#define USBPHY_DEBUG_CLR_TX2RXCOUNT_MASK (0xF00U)

Definition at line 43979 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_CLR_TX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_CLR_TX2RXCOUNT_SHIFT (8U)

Definition at line 43980 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_DEBUG_INTERFACE_HOLD

#define USBPHY_DEBUG_DEBUG_INTERFACE_HOLD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_MASK)

Definition at line 43871 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_MASK

#define USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_MASK (0x2U)

Definition at line 43869 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_SHIFT

#define USBPHY_DEBUG_DEBUG_INTERFACE_HOLD_SHIFT (1U)

Definition at line 43870 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENHSTPULLDOWN

#define USBPHY_DEBUG_ENHSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_ENHSTPULLDOWN_MASK)

Definition at line 43877 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENHSTPULLDOWN_MASK

#define USBPHY_DEBUG_ENHSTPULLDOWN_MASK (0x30U)

Definition at line 43875 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENHSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_ENHSTPULLDOWN_SHIFT (4U)

Definition at line 43876 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENSQUELCHRESET

#define USBPHY_DEBUG_ENSQUELCHRESET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_ENSQUELCHRESET_MASK)

Definition at line 43898 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENSQUELCHRESET_MASK

#define USBPHY_DEBUG_ENSQUELCHRESET_MASK (0x1000000U)

Definition at line 43896 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENSQUELCHRESET_SHIFT

#define USBPHY_DEBUG_ENSQUELCHRESET_SHIFT (24U)

Definition at line 43897 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENTX2RXCOUNT

#define USBPHY_DEBUG_ENTX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_ENTX2RXCOUNT_MASK)

Definition at line 43886 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENTX2RXCOUNT_MASK

#define USBPHY_DEBUG_ENTX2RXCOUNT_MASK (0x1000U)

Definition at line 43884 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_ENTX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_ENTX2RXCOUNT_SHIFT (12U)

Definition at line 43885 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_HOST_RESUME_DEBUG

#define USBPHY_DEBUG_HOST_RESUME_DEBUG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_HOST_RESUME_DEBUG_MASK)

Definition at line 43904 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_HOST_RESUME_DEBUG_MASK

#define USBPHY_DEBUG_HOST_RESUME_DEBUG_MASK (0x20000000U)

Definition at line 43902 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_HOST_RESUME_DEBUG_SHIFT

#define USBPHY_DEBUG_HOST_RESUME_DEBUG_SHIFT (29U)

Definition at line 43903 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_HSTPULLDOWN

#define USBPHY_DEBUG_HSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_HSTPULLDOWN_MASK)

Definition at line 43874 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_HSTPULLDOWN_MASK

#define USBPHY_DEBUG_HSTPULLDOWN_MASK (0xCU)

Definition at line 43872 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_HSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_HSTPULLDOWN_SHIFT (2U)

Definition at line 43873 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_OTGIDPIOLOCK

#define USBPHY_DEBUG_OTGIDPIOLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_OTGIDPIOLOCK_MASK)

Definition at line 43868 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_OTGIDPIOLOCK_MASK

#define USBPHY_DEBUG_OTGIDPIOLOCK_MASK (0x1U)

Definition at line 43866 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_OTGIDPIOLOCK_SHIFT

#define USBPHY_DEBUG_OTGIDPIOLOCK_SHIFT (0U)

Definition at line 43867 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD0

#define USBPHY_DEBUG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD0_SHIFT)) & USBPHY_DEBUG_RSVD0_MASK)

Definition at line 43880 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD0_MASK

#define USBPHY_DEBUG_RSVD0_MASK (0xC0U)

Definition at line 43878 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD0_SHIFT

#define USBPHY_DEBUG_RSVD0_SHIFT (6U)

Definition at line 43879 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD1

#define USBPHY_DEBUG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD1_SHIFT)) & USBPHY_DEBUG_RSVD1_MASK)

Definition at line 43889 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD1_MASK

#define USBPHY_DEBUG_RSVD1_MASK (0xE000U)

Definition at line 43887 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD1_SHIFT

#define USBPHY_DEBUG_RSVD1_SHIFT (13U)

Definition at line 43888 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD2

#define USBPHY_DEBUG_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD2_SHIFT)) & USBPHY_DEBUG_RSVD2_MASK)

Definition at line 43895 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD2_MASK

#define USBPHY_DEBUG_RSVD2_MASK (0xE00000U)

Definition at line 43893 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD2_SHIFT

#define USBPHY_DEBUG_RSVD2_SHIFT (21U)

Definition at line 43894 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD3

#define USBPHY_DEBUG_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_RSVD3_SHIFT)) & USBPHY_DEBUG_RSVD3_MASK)

Definition at line 43910 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD3_MASK

#define USBPHY_DEBUG_RSVD3_MASK (0x80000000U)

Definition at line 43908 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_RSVD3_SHIFT

#define USBPHY_DEBUG_RSVD3_SHIFT (31U)

Definition at line 43909 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_CLKGATE

#define USBPHY_DEBUG_SET_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_CLKGATE_SHIFT)) & USBPHY_DEBUG_SET_CLKGATE_MASK)

Definition at line 43956 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_CLKGATE_MASK

#define USBPHY_DEBUG_SET_CLKGATE_MASK (0x40000000U)

Definition at line 43954 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_CLKGATE_SHIFT

#define USBPHY_DEBUG_SET_CLKGATE_SHIFT (30U)

Definition at line 43955 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD

#define USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_MASK)

Definition at line 43920 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_MASK

#define USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_MASK (0x2U)

Definition at line 43918 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_SHIFT

#define USBPHY_DEBUG_SET_DEBUG_INTERFACE_HOLD_SHIFT (1U)

Definition at line 43919 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENHSTPULLDOWN

#define USBPHY_DEBUG_SET_ENHSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_SET_ENHSTPULLDOWN_MASK)

Definition at line 43926 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENHSTPULLDOWN_MASK

#define USBPHY_DEBUG_SET_ENHSTPULLDOWN_MASK (0x30U)

Definition at line 43924 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENHSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_SET_ENHSTPULLDOWN_SHIFT (4U)

Definition at line 43925 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENSQUELCHRESET

#define USBPHY_DEBUG_SET_ENSQUELCHRESET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_SET_ENSQUELCHRESET_MASK)

Definition at line 43947 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENSQUELCHRESET_MASK

#define USBPHY_DEBUG_SET_ENSQUELCHRESET_MASK (0x1000000U)

Definition at line 43945 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENSQUELCHRESET_SHIFT

#define USBPHY_DEBUG_SET_ENSQUELCHRESET_SHIFT (24U)

Definition at line 43946 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENTX2RXCOUNT

#define USBPHY_DEBUG_SET_ENTX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_SET_ENTX2RXCOUNT_MASK)

Definition at line 43935 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENTX2RXCOUNT_MASK

#define USBPHY_DEBUG_SET_ENTX2RXCOUNT_MASK (0x1000U)

Definition at line 43933 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_ENTX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_SET_ENTX2RXCOUNT_SHIFT (12U)

Definition at line 43934 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_HOST_RESUME_DEBUG

#define USBPHY_DEBUG_SET_HOST_RESUME_DEBUG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_MASK)

Definition at line 43953 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_MASK

#define USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_MASK (0x20000000U)

Definition at line 43951 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_SHIFT

#define USBPHY_DEBUG_SET_HOST_RESUME_DEBUG_SHIFT (29U)

Definition at line 43952 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_HSTPULLDOWN

#define USBPHY_DEBUG_SET_HSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_SET_HSTPULLDOWN_MASK)

Definition at line 43923 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_HSTPULLDOWN_MASK

#define USBPHY_DEBUG_SET_HSTPULLDOWN_MASK (0xCU)

Definition at line 43921 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_HSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_SET_HSTPULLDOWN_SHIFT (2U)

Definition at line 43922 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_OTGIDPIOLOCK

#define USBPHY_DEBUG_SET_OTGIDPIOLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_SET_OTGIDPIOLOCK_MASK)

Definition at line 43917 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_OTGIDPIOLOCK_MASK

#define USBPHY_DEBUG_SET_OTGIDPIOLOCK_MASK (0x1U)

Definition at line 43915 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_OTGIDPIOLOCK_SHIFT

#define USBPHY_DEBUG_SET_OTGIDPIOLOCK_SHIFT (0U)

Definition at line 43916 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD0

#define USBPHY_DEBUG_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD0_SHIFT)) & USBPHY_DEBUG_SET_RSVD0_MASK)

Definition at line 43929 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD0_MASK

#define USBPHY_DEBUG_SET_RSVD0_MASK (0xC0U)

Definition at line 43927 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD0_SHIFT

#define USBPHY_DEBUG_SET_RSVD0_SHIFT (6U)

Definition at line 43928 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD1

#define USBPHY_DEBUG_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD1_SHIFT)) & USBPHY_DEBUG_SET_RSVD1_MASK)

Definition at line 43938 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD1_MASK

#define USBPHY_DEBUG_SET_RSVD1_MASK (0xE000U)

Definition at line 43936 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD1_SHIFT

#define USBPHY_DEBUG_SET_RSVD1_SHIFT (13U)

Definition at line 43937 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD2

#define USBPHY_DEBUG_SET_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD2_SHIFT)) & USBPHY_DEBUG_SET_RSVD2_MASK)

Definition at line 43944 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD2_MASK

#define USBPHY_DEBUG_SET_RSVD2_MASK (0xE00000U)

Definition at line 43942 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD2_SHIFT

#define USBPHY_DEBUG_SET_RSVD2_SHIFT (21U)

Definition at line 43943 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD3

#define USBPHY_DEBUG_SET_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_RSVD3_SHIFT)) & USBPHY_DEBUG_SET_RSVD3_MASK)

Definition at line 43959 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD3_MASK

#define USBPHY_DEBUG_SET_RSVD3_MASK (0x80000000U)

Definition at line 43957 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_RSVD3_SHIFT

#define USBPHY_DEBUG_SET_RSVD3_SHIFT (31U)

Definition at line 43958 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_SQUELCHRESETCOUNT

#define USBPHY_DEBUG_SET_SQUELCHRESETCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_MASK)

Definition at line 43941 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_MASK

#define USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_MASK (0x1F0000U)

Definition at line 43939 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_SHIFT

#define USBPHY_DEBUG_SET_SQUELCHRESETCOUNT_SHIFT (16U)

Definition at line 43940 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_SQUELCHRESETLENGTH

#define USBPHY_DEBUG_SET_SQUELCHRESETLENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_MASK)

Definition at line 43950 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_MASK

#define USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_MASK (0x1E000000U)

Definition at line 43948 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_SHIFT

#define USBPHY_DEBUG_SET_SQUELCHRESETLENGTH_SHIFT (25U)

Definition at line 43949 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_TX2RXCOUNT

#define USBPHY_DEBUG_SET_TX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SET_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_SET_TX2RXCOUNT_MASK)

Definition at line 43932 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_TX2RXCOUNT_MASK

#define USBPHY_DEBUG_SET_TX2RXCOUNT_MASK (0xF00U)

Definition at line 43930 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SET_TX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_SET_TX2RXCOUNT_SHIFT (8U)

Definition at line 43931 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SQUELCHRESETCOUNT

#define USBPHY_DEBUG_SQUELCHRESETCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_SQUELCHRESETCOUNT_MASK)

Definition at line 43892 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SQUELCHRESETCOUNT_MASK

#define USBPHY_DEBUG_SQUELCHRESETCOUNT_MASK (0x1F0000U)

Definition at line 43890 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SQUELCHRESETCOUNT_SHIFT

#define USBPHY_DEBUG_SQUELCHRESETCOUNT_SHIFT (16U)

Definition at line 43891 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SQUELCHRESETLENGTH

#define USBPHY_DEBUG_SQUELCHRESETLENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_SQUELCHRESETLENGTH_MASK)

Definition at line 43901 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SQUELCHRESETLENGTH_MASK

#define USBPHY_DEBUG_SQUELCHRESETLENGTH_MASK (0x1E000000U)

Definition at line 43899 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_SQUELCHRESETLENGTH_SHIFT

#define USBPHY_DEBUG_SQUELCHRESETLENGTH_SHIFT (25U)

Definition at line 43900 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_CLKGATE

#define USBPHY_DEBUG_TOG_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_CLKGATE_SHIFT)) & USBPHY_DEBUG_TOG_CLKGATE_MASK)

Definition at line 44054 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_CLKGATE_MASK

#define USBPHY_DEBUG_TOG_CLKGATE_MASK (0x40000000U)

Definition at line 44052 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_CLKGATE_SHIFT

#define USBPHY_DEBUG_TOG_CLKGATE_SHIFT (30U)

Definition at line 44053 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD

#define USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_SHIFT)) & USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_MASK)

Definition at line 44018 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_MASK

#define USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_MASK (0x2U)

Definition at line 44016 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_SHIFT

#define USBPHY_DEBUG_TOG_DEBUG_INTERFACE_HOLD_SHIFT (1U)

Definition at line 44017 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENHSTPULLDOWN

#define USBPHY_DEBUG_TOG_ENHSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_ENHSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_TOG_ENHSTPULLDOWN_MASK)

Definition at line 44024 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENHSTPULLDOWN_MASK

#define USBPHY_DEBUG_TOG_ENHSTPULLDOWN_MASK (0x30U)

Definition at line 44022 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENHSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_TOG_ENHSTPULLDOWN_SHIFT (4U)

Definition at line 44023 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENSQUELCHRESET

#define USBPHY_DEBUG_TOG_ENSQUELCHRESET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_ENSQUELCHRESET_SHIFT)) & USBPHY_DEBUG_TOG_ENSQUELCHRESET_MASK)

Definition at line 44045 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENSQUELCHRESET_MASK

#define USBPHY_DEBUG_TOG_ENSQUELCHRESET_MASK (0x1000000U)

Definition at line 44043 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENSQUELCHRESET_SHIFT

#define USBPHY_DEBUG_TOG_ENSQUELCHRESET_SHIFT (24U)

Definition at line 44044 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENTX2RXCOUNT

#define USBPHY_DEBUG_TOG_ENTX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_ENTX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_TOG_ENTX2RXCOUNT_MASK)

Definition at line 44033 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENTX2RXCOUNT_MASK

#define USBPHY_DEBUG_TOG_ENTX2RXCOUNT_MASK (0x1000U)

Definition at line 44031 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_ENTX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_TOG_ENTX2RXCOUNT_SHIFT (12U)

Definition at line 44032 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG

#define USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_SHIFT)) & USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_MASK)

Definition at line 44051 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_MASK

#define USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_MASK (0x20000000U)

Definition at line 44049 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_SHIFT

#define USBPHY_DEBUG_TOG_HOST_RESUME_DEBUG_SHIFT (29U)

Definition at line 44050 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_HSTPULLDOWN

#define USBPHY_DEBUG_TOG_HSTPULLDOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_HSTPULLDOWN_SHIFT)) & USBPHY_DEBUG_TOG_HSTPULLDOWN_MASK)

Definition at line 44021 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_HSTPULLDOWN_MASK

#define USBPHY_DEBUG_TOG_HSTPULLDOWN_MASK (0xCU)

Definition at line 44019 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_HSTPULLDOWN_SHIFT

#define USBPHY_DEBUG_TOG_HSTPULLDOWN_SHIFT (2U)

Definition at line 44020 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_OTGIDPIOLOCK

#define USBPHY_DEBUG_TOG_OTGIDPIOLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_OTGIDPIOLOCK_SHIFT)) & USBPHY_DEBUG_TOG_OTGIDPIOLOCK_MASK)

Definition at line 44015 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_OTGIDPIOLOCK_MASK

#define USBPHY_DEBUG_TOG_OTGIDPIOLOCK_MASK (0x1U)

Definition at line 44013 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_OTGIDPIOLOCK_SHIFT

#define USBPHY_DEBUG_TOG_OTGIDPIOLOCK_SHIFT (0U)

Definition at line 44014 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD0

#define USBPHY_DEBUG_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD0_SHIFT)) & USBPHY_DEBUG_TOG_RSVD0_MASK)

Definition at line 44027 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD0_MASK

#define USBPHY_DEBUG_TOG_RSVD0_MASK (0xC0U)

Definition at line 44025 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD0_SHIFT

#define USBPHY_DEBUG_TOG_RSVD0_SHIFT (6U)

Definition at line 44026 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD1

#define USBPHY_DEBUG_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD1_SHIFT)) & USBPHY_DEBUG_TOG_RSVD1_MASK)

Definition at line 44036 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD1_MASK

#define USBPHY_DEBUG_TOG_RSVD1_MASK (0xE000U)

Definition at line 44034 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD1_SHIFT

#define USBPHY_DEBUG_TOG_RSVD1_SHIFT (13U)

Definition at line 44035 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD2

#define USBPHY_DEBUG_TOG_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD2_SHIFT)) & USBPHY_DEBUG_TOG_RSVD2_MASK)

Definition at line 44042 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD2_MASK

#define USBPHY_DEBUG_TOG_RSVD2_MASK (0xE00000U)

Definition at line 44040 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD2_SHIFT

#define USBPHY_DEBUG_TOG_RSVD2_SHIFT (21U)

Definition at line 44041 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD3

#define USBPHY_DEBUG_TOG_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_RSVD3_SHIFT)) & USBPHY_DEBUG_TOG_RSVD3_MASK)

Definition at line 44057 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD3_MASK

#define USBPHY_DEBUG_TOG_RSVD3_MASK (0x80000000U)

Definition at line 44055 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_RSVD3_SHIFT

#define USBPHY_DEBUG_TOG_RSVD3_SHIFT (31U)

Definition at line 44056 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT

#define USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_SHIFT)) & USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_MASK)

Definition at line 44039 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_MASK

#define USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_MASK (0x1F0000U)

Definition at line 44037 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_SHIFT

#define USBPHY_DEBUG_TOG_SQUELCHRESETCOUNT_SHIFT (16U)

Definition at line 44038 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH

#define USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_SHIFT)) & USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_MASK)

Definition at line 44048 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_MASK

#define USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_MASK (0x1E000000U)

Definition at line 44046 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_SHIFT

#define USBPHY_DEBUG_TOG_SQUELCHRESETLENGTH_SHIFT (25U)

Definition at line 44047 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_TX2RXCOUNT

#define USBPHY_DEBUG_TOG_TX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TOG_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_TOG_TX2RXCOUNT_MASK)

Definition at line 44030 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_TX2RXCOUNT_MASK

#define USBPHY_DEBUG_TOG_TX2RXCOUNT_MASK (0xF00U)

Definition at line 44028 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TOG_TX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_TOG_TX2RXCOUNT_SHIFT (8U)

Definition at line 44029 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TX2RXCOUNT

#define USBPHY_DEBUG_TX2RXCOUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_DEBUG_TX2RXCOUNT_SHIFT)) & USBPHY_DEBUG_TX2RXCOUNT_MASK)

Definition at line 43883 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TX2RXCOUNT_MASK

#define USBPHY_DEBUG_TX2RXCOUNT_MASK (0xF00U)

Definition at line 43881 of file MIMXRT1062.h.

## ◆ USBPHY_DEBUG_TX2RXCOUNT_SHIFT

#define USBPHY_DEBUG_TX2RXCOUNT_SHIFT (8U)

Definition at line 43882 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD0

#define USBPHY_PWD_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RSVD0_SHIFT)) & USBPHY_PWD_CLR_RSVD0_MASK)

Definition at line 43181 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD0_MASK

#define USBPHY_PWD_CLR_RSVD0_MASK (0x3FFU)

Definition at line 43179 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD0_SHIFT

#define USBPHY_PWD_CLR_RSVD0_SHIFT (0U)

Definition at line 43180 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD1

#define USBPHY_PWD_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RSVD1_SHIFT)) & USBPHY_PWD_CLR_RSVD1_MASK)

Definition at line 43193 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD1_MASK

#define USBPHY_PWD_CLR_RSVD1_MASK (0x1E000U)

Definition at line 43191 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD1_SHIFT

#define USBPHY_PWD_CLR_RSVD1_SHIFT (13U)

Definition at line 43192 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD2

#define USBPHY_PWD_CLR_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RSVD2_SHIFT)) & USBPHY_PWD_CLR_RSVD2_MASK)

Definition at line 43208 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD2_MASK

#define USBPHY_PWD_CLR_RSVD2_MASK (0xFFE00000U)

Definition at line 43206 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RSVD2_SHIFT

#define USBPHY_PWD_CLR_RSVD2_SHIFT (21U)

Definition at line 43207 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWD1PT1

#define USBPHY_PWD_CLR_RXPWD1PT1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWD1PT1_SHIFT)) & USBPHY_PWD_CLR_RXPWD1PT1_MASK)

Definition at line 43199 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWD1PT1_MASK

#define USBPHY_PWD_CLR_RXPWD1PT1_MASK (0x40000U)

Definition at line 43197 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWD1PT1_SHIFT

#define USBPHY_PWD_CLR_RXPWD1PT1_SHIFT (18U)

Definition at line 43198 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDDIFF

#define USBPHY_PWD_CLR_RXPWDDIFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWDDIFF_SHIFT)) & USBPHY_PWD_CLR_RXPWDDIFF_MASK)

Definition at line 43202 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDDIFF_MASK

#define USBPHY_PWD_CLR_RXPWDDIFF_MASK (0x80000U)

Definition at line 43200 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDDIFF_SHIFT

#define USBPHY_PWD_CLR_RXPWDDIFF_SHIFT (19U)

Definition at line 43201 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDENV

#define USBPHY_PWD_CLR_RXPWDENV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWDENV_SHIFT)) & USBPHY_PWD_CLR_RXPWDENV_MASK)

Definition at line 43196 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDENV_MASK

#define USBPHY_PWD_CLR_RXPWDENV_MASK (0x20000U)

Definition at line 43194 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDENV_SHIFT

#define USBPHY_PWD_CLR_RXPWDENV_SHIFT (17U)

Definition at line 43195 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDRX

#define USBPHY_PWD_CLR_RXPWDRX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_RXPWDRX_SHIFT)) & USBPHY_PWD_CLR_RXPWDRX_MASK)

Definition at line 43205 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDRX_MASK

#define USBPHY_PWD_CLR_RXPWDRX_MASK (0x100000U)

Definition at line 43203 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_RXPWDRX_SHIFT

#define USBPHY_PWD_CLR_RXPWDRX_SHIFT (20U)

Definition at line 43204 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDFS

#define USBPHY_PWD_CLR_TXPWDFS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_TXPWDFS_SHIFT)) & USBPHY_PWD_CLR_TXPWDFS_MASK)

Definition at line 43184 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDFS_MASK

#define USBPHY_PWD_CLR_TXPWDFS_MASK (0x400U)

Definition at line 43182 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDFS_SHIFT

#define USBPHY_PWD_CLR_TXPWDFS_SHIFT (10U)

Definition at line 43183 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDIBIAS

#define USBPHY_PWD_CLR_TXPWDIBIAS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_CLR_TXPWDIBIAS_MASK)

Definition at line 43187 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDIBIAS_MASK

#define USBPHY_PWD_CLR_TXPWDIBIAS_MASK (0x800U)

Definition at line 43185 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDIBIAS_SHIFT

#define USBPHY_PWD_CLR_TXPWDIBIAS_SHIFT (11U)

Definition at line 43186 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDV2I

#define USBPHY_PWD_CLR_TXPWDV2I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_CLR_TXPWDV2I_SHIFT)) & USBPHY_PWD_CLR_TXPWDV2I_MASK)

Definition at line 43190 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDV2I_MASK

#define USBPHY_PWD_CLR_TXPWDV2I_MASK (0x1000U)

Definition at line 43188 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_CLR_TXPWDV2I_SHIFT

#define USBPHY_PWD_CLR_TXPWDV2I_SHIFT (12U)

Definition at line 43189 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD0

#define USBPHY_PWD_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RSVD0_SHIFT)) & USBPHY_PWD_RSVD0_MASK)

Definition at line 43113 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD0_MASK

#define USBPHY_PWD_RSVD0_MASK (0x3FFU)

Definition at line 43111 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD0_SHIFT

#define USBPHY_PWD_RSVD0_SHIFT (0U)

Definition at line 43112 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD1

#define USBPHY_PWD_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RSVD1_SHIFT)) & USBPHY_PWD_RSVD1_MASK)

Definition at line 43125 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD1_MASK

#define USBPHY_PWD_RSVD1_MASK (0x1E000U)

Definition at line 43123 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD1_SHIFT

#define USBPHY_PWD_RSVD1_SHIFT (13U)

Definition at line 43124 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD2

#define USBPHY_PWD_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RSVD2_SHIFT)) & USBPHY_PWD_RSVD2_MASK)

Definition at line 43140 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD2_MASK

#define USBPHY_PWD_RSVD2_MASK (0xFFE00000U)

Definition at line 43138 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RSVD2_SHIFT

#define USBPHY_PWD_RSVD2_SHIFT (21U)

Definition at line 43139 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWD1PT1

#define USBPHY_PWD_RXPWD1PT1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWD1PT1_SHIFT)) & USBPHY_PWD_RXPWD1PT1_MASK)

Definition at line 43131 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWD1PT1_MASK

#define USBPHY_PWD_RXPWD1PT1_MASK (0x40000U)

Definition at line 43129 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWD1PT1_SHIFT

#define USBPHY_PWD_RXPWD1PT1_SHIFT (18U)

Definition at line 43130 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDDIFF

#define USBPHY_PWD_RXPWDDIFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWDDIFF_SHIFT)) & USBPHY_PWD_RXPWDDIFF_MASK)

Definition at line 43134 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDDIFF_MASK

#define USBPHY_PWD_RXPWDDIFF_MASK (0x80000U)

Definition at line 43132 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDDIFF_SHIFT

#define USBPHY_PWD_RXPWDDIFF_SHIFT (19U)

Definition at line 43133 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDENV

#define USBPHY_PWD_RXPWDENV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWDENV_SHIFT)) & USBPHY_PWD_RXPWDENV_MASK)

Definition at line 43128 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDENV_MASK

#define USBPHY_PWD_RXPWDENV_MASK (0x20000U)

Definition at line 43126 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDENV_SHIFT

#define USBPHY_PWD_RXPWDENV_SHIFT (17U)

Definition at line 43127 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDRX

#define USBPHY_PWD_RXPWDRX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_RXPWDRX_SHIFT)) & USBPHY_PWD_RXPWDRX_MASK)

Definition at line 43137 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDRX_MASK

#define USBPHY_PWD_RXPWDRX_MASK (0x100000U)

Definition at line 43135 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_RXPWDRX_SHIFT

#define USBPHY_PWD_RXPWDRX_SHIFT (20U)

Definition at line 43136 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD0

#define USBPHY_PWD_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RSVD0_SHIFT)) & USBPHY_PWD_SET_RSVD0_MASK)

Definition at line 43147 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD0_MASK

#define USBPHY_PWD_SET_RSVD0_MASK (0x3FFU)

Definition at line 43145 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD0_SHIFT

#define USBPHY_PWD_SET_RSVD0_SHIFT (0U)

Definition at line 43146 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD1

#define USBPHY_PWD_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RSVD1_SHIFT)) & USBPHY_PWD_SET_RSVD1_MASK)

Definition at line 43159 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD1_MASK

#define USBPHY_PWD_SET_RSVD1_MASK (0x1E000U)

Definition at line 43157 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD1_SHIFT

#define USBPHY_PWD_SET_RSVD1_SHIFT (13U)

Definition at line 43158 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD2

#define USBPHY_PWD_SET_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RSVD2_SHIFT)) & USBPHY_PWD_SET_RSVD2_MASK)

Definition at line 43174 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD2_MASK

#define USBPHY_PWD_SET_RSVD2_MASK (0xFFE00000U)

Definition at line 43172 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RSVD2_SHIFT

#define USBPHY_PWD_SET_RSVD2_SHIFT (21U)

Definition at line 43173 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWD1PT1

#define USBPHY_PWD_SET_RXPWD1PT1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWD1PT1_SHIFT)) & USBPHY_PWD_SET_RXPWD1PT1_MASK)

Definition at line 43165 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWD1PT1_MASK

#define USBPHY_PWD_SET_RXPWD1PT1_MASK (0x40000U)

Definition at line 43163 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWD1PT1_SHIFT

#define USBPHY_PWD_SET_RXPWD1PT1_SHIFT (18U)

Definition at line 43164 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDDIFF

#define USBPHY_PWD_SET_RXPWDDIFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWDDIFF_SHIFT)) & USBPHY_PWD_SET_RXPWDDIFF_MASK)

Definition at line 43168 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDDIFF_MASK

#define USBPHY_PWD_SET_RXPWDDIFF_MASK (0x80000U)

Definition at line 43166 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDDIFF_SHIFT

#define USBPHY_PWD_SET_RXPWDDIFF_SHIFT (19U)

Definition at line 43167 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDENV

#define USBPHY_PWD_SET_RXPWDENV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWDENV_SHIFT)) & USBPHY_PWD_SET_RXPWDENV_MASK)

Definition at line 43162 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDENV_MASK

#define USBPHY_PWD_SET_RXPWDENV_MASK (0x20000U)

Definition at line 43160 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDENV_SHIFT

#define USBPHY_PWD_SET_RXPWDENV_SHIFT (17U)

Definition at line 43161 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDRX

#define USBPHY_PWD_SET_RXPWDRX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_RXPWDRX_SHIFT)) & USBPHY_PWD_SET_RXPWDRX_MASK)

Definition at line 43171 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDRX_MASK

#define USBPHY_PWD_SET_RXPWDRX_MASK (0x100000U)

Definition at line 43169 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_RXPWDRX_SHIFT

#define USBPHY_PWD_SET_RXPWDRX_SHIFT (20U)

Definition at line 43170 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDFS

#define USBPHY_PWD_SET_TXPWDFS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_TXPWDFS_SHIFT)) & USBPHY_PWD_SET_TXPWDFS_MASK)

Definition at line 43150 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDFS_MASK

#define USBPHY_PWD_SET_TXPWDFS_MASK (0x400U)

Definition at line 43148 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDFS_SHIFT

#define USBPHY_PWD_SET_TXPWDFS_SHIFT (10U)

Definition at line 43149 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDIBIAS

#define USBPHY_PWD_SET_TXPWDIBIAS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_SET_TXPWDIBIAS_MASK)

Definition at line 43153 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDIBIAS_MASK

#define USBPHY_PWD_SET_TXPWDIBIAS_MASK (0x800U)

Definition at line 43151 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDIBIAS_SHIFT

#define USBPHY_PWD_SET_TXPWDIBIAS_SHIFT (11U)

Definition at line 43152 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDV2I

#define USBPHY_PWD_SET_TXPWDV2I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_SET_TXPWDV2I_SHIFT)) & USBPHY_PWD_SET_TXPWDV2I_MASK)

Definition at line 43156 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDV2I_MASK

#define USBPHY_PWD_SET_TXPWDV2I_MASK (0x1000U)

Definition at line 43154 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_SET_TXPWDV2I_SHIFT

#define USBPHY_PWD_SET_TXPWDV2I_SHIFT (12U)

Definition at line 43155 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD0

#define USBPHY_PWD_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RSVD0_SHIFT)) & USBPHY_PWD_TOG_RSVD0_MASK)

Definition at line 43215 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD0_MASK

#define USBPHY_PWD_TOG_RSVD0_MASK (0x3FFU)

Definition at line 43213 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD0_SHIFT

#define USBPHY_PWD_TOG_RSVD0_SHIFT (0U)

Definition at line 43214 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD1

#define USBPHY_PWD_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RSVD1_SHIFT)) & USBPHY_PWD_TOG_RSVD1_MASK)

Definition at line 43227 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD1_MASK

#define USBPHY_PWD_TOG_RSVD1_MASK (0x1E000U)

Definition at line 43225 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD1_SHIFT

#define USBPHY_PWD_TOG_RSVD1_SHIFT (13U)

Definition at line 43226 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD2

#define USBPHY_PWD_TOG_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RSVD2_SHIFT)) & USBPHY_PWD_TOG_RSVD2_MASK)

Definition at line 43242 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD2_MASK

#define USBPHY_PWD_TOG_RSVD2_MASK (0xFFE00000U)

Definition at line 43240 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RSVD2_SHIFT

#define USBPHY_PWD_TOG_RSVD2_SHIFT (21U)

Definition at line 43241 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWD1PT1

#define USBPHY_PWD_TOG_RXPWD1PT1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWD1PT1_SHIFT)) & USBPHY_PWD_TOG_RXPWD1PT1_MASK)

Definition at line 43233 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWD1PT1_MASK

#define USBPHY_PWD_TOG_RXPWD1PT1_MASK (0x40000U)

Definition at line 43231 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWD1PT1_SHIFT

#define USBPHY_PWD_TOG_RXPWD1PT1_SHIFT (18U)

Definition at line 43232 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDDIFF

#define USBPHY_PWD_TOG_RXPWDDIFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWDDIFF_SHIFT)) & USBPHY_PWD_TOG_RXPWDDIFF_MASK)

Definition at line 43236 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDDIFF_MASK

#define USBPHY_PWD_TOG_RXPWDDIFF_MASK (0x80000U)

Definition at line 43234 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDDIFF_SHIFT

#define USBPHY_PWD_TOG_RXPWDDIFF_SHIFT (19U)

Definition at line 43235 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDENV

#define USBPHY_PWD_TOG_RXPWDENV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWDENV_SHIFT)) & USBPHY_PWD_TOG_RXPWDENV_MASK)

Definition at line 43230 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDENV_MASK

#define USBPHY_PWD_TOG_RXPWDENV_MASK (0x20000U)

Definition at line 43228 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDENV_SHIFT

#define USBPHY_PWD_TOG_RXPWDENV_SHIFT (17U)

Definition at line 43229 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDRX

#define USBPHY_PWD_TOG_RXPWDRX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_RXPWDRX_SHIFT)) & USBPHY_PWD_TOG_RXPWDRX_MASK)

Definition at line 43239 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDRX_MASK

#define USBPHY_PWD_TOG_RXPWDRX_MASK (0x100000U)

Definition at line 43237 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_RXPWDRX_SHIFT

#define USBPHY_PWD_TOG_RXPWDRX_SHIFT (20U)

Definition at line 43238 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDFS

#define USBPHY_PWD_TOG_TXPWDFS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_TXPWDFS_SHIFT)) & USBPHY_PWD_TOG_TXPWDFS_MASK)

Definition at line 43218 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDFS_MASK

#define USBPHY_PWD_TOG_TXPWDFS_MASK (0x400U)

Definition at line 43216 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDFS_SHIFT

#define USBPHY_PWD_TOG_TXPWDFS_SHIFT (10U)

Definition at line 43217 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDIBIAS

#define USBPHY_PWD_TOG_TXPWDIBIAS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_TOG_TXPWDIBIAS_MASK)

Definition at line 43221 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDIBIAS_MASK

#define USBPHY_PWD_TOG_TXPWDIBIAS_MASK (0x800U)

Definition at line 43219 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDIBIAS_SHIFT

#define USBPHY_PWD_TOG_TXPWDIBIAS_SHIFT (11U)

Definition at line 43220 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDV2I

#define USBPHY_PWD_TOG_TXPWDV2I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TOG_TXPWDV2I_SHIFT)) & USBPHY_PWD_TOG_TXPWDV2I_MASK)

Definition at line 43224 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDV2I_MASK

#define USBPHY_PWD_TOG_TXPWDV2I_MASK (0x1000U)

Definition at line 43222 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TOG_TXPWDV2I_SHIFT

#define USBPHY_PWD_TOG_TXPWDV2I_SHIFT (12U)

Definition at line 43223 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDFS

#define USBPHY_PWD_TXPWDFS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TXPWDFS_SHIFT)) & USBPHY_PWD_TXPWDFS_MASK)

Definition at line 43116 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDFS_MASK

#define USBPHY_PWD_TXPWDFS_MASK (0x400U)

Definition at line 43114 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDFS_SHIFT

#define USBPHY_PWD_TXPWDFS_SHIFT (10U)

Definition at line 43115 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDIBIAS

#define USBPHY_PWD_TXPWDIBIAS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TXPWDIBIAS_SHIFT)) & USBPHY_PWD_TXPWDIBIAS_MASK)

Definition at line 43119 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDIBIAS_MASK

#define USBPHY_PWD_TXPWDIBIAS_MASK (0x800U)

Definition at line 43117 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDIBIAS_SHIFT

#define USBPHY_PWD_TXPWDIBIAS_SHIFT (11U)

Definition at line 43118 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDV2I

#define USBPHY_PWD_TXPWDV2I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_PWD_TXPWDV2I_SHIFT)) & USBPHY_PWD_TXPWDV2I_MASK)

Definition at line 43122 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDV2I_MASK

#define USBPHY_PWD_TXPWDV2I_MASK (0x1000U)

Definition at line 43120 of file MIMXRT1062.h.

## ◆ USBPHY_PWD_TXPWDV2I_SHIFT

#define USBPHY_PWD_TXPWDV2I_SHIFT (12U)

Definition at line 43121 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_DISCONADJ

#define USBPHY_RX_CLR_DISCONADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_DISCONADJ_SHIFT)) & USBPHY_RX_CLR_DISCONADJ_MASK)

Definition at line 43411 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_DISCONADJ_MASK

#define USBPHY_RX_CLR_DISCONADJ_MASK (0x70U)

Definition at line 43409 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_DISCONADJ_SHIFT

#define USBPHY_RX_CLR_DISCONADJ_SHIFT (4U)

Definition at line 43410 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_ENVADJ

#define USBPHY_RX_CLR_ENVADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_ENVADJ_SHIFT)) & USBPHY_RX_CLR_ENVADJ_MASK)

Definition at line 43405 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_ENVADJ_MASK

#define USBPHY_RX_CLR_ENVADJ_MASK (0x7U)

Definition at line 43403 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_ENVADJ_SHIFT

#define USBPHY_RX_CLR_ENVADJ_SHIFT (0U)

Definition at line 43404 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD0

#define USBPHY_RX_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RSVD0_SHIFT)) & USBPHY_RX_CLR_RSVD0_MASK)

Definition at line 43408 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD0_MASK

#define USBPHY_RX_CLR_RSVD0_MASK (0x8U)

Definition at line 43406 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD0_SHIFT

#define USBPHY_RX_CLR_RSVD0_SHIFT (3U)

Definition at line 43407 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD1

#define USBPHY_RX_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RSVD1_SHIFT)) & USBPHY_RX_CLR_RSVD1_MASK)

Definition at line 43414 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD1_MASK

#define USBPHY_RX_CLR_RSVD1_MASK (0x3FFF80U)

Definition at line 43412 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD1_SHIFT

#define USBPHY_RX_CLR_RSVD1_SHIFT (7U)

Definition at line 43413 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD2

#define USBPHY_RX_CLR_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RSVD2_SHIFT)) & USBPHY_RX_CLR_RSVD2_MASK)

Definition at line 43420 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD2_MASK

#define USBPHY_RX_CLR_RSVD2_MASK (0xFF800000U)

Definition at line 43418 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RSVD2_SHIFT

#define USBPHY_RX_CLR_RSVD2_SHIFT (23U)

Definition at line 43419 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RXDBYPASS

#define USBPHY_RX_CLR_RXDBYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_CLR_RXDBYPASS_SHIFT)) & USBPHY_RX_CLR_RXDBYPASS_MASK)

Definition at line 43417 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RXDBYPASS_MASK

#define USBPHY_RX_CLR_RXDBYPASS_MASK (0x400000U)

Definition at line 43415 of file MIMXRT1062.h.

## ◆ USBPHY_RX_CLR_RXDBYPASS_SHIFT

#define USBPHY_RX_CLR_RXDBYPASS_SHIFT (22U)

Definition at line 43416 of file MIMXRT1062.h.

## ◆ USBPHY_RX_DISCONADJ

#define USBPHY_RX_DISCONADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_DISCONADJ_SHIFT)) & USBPHY_RX_DISCONADJ_MASK)

Definition at line 43367 of file MIMXRT1062.h.

## ◆ USBPHY_RX_DISCONADJ_MASK

#define USBPHY_RX_DISCONADJ_MASK (0x70U)

Definition at line 43365 of file MIMXRT1062.h.

## ◆ USBPHY_RX_DISCONADJ_SHIFT

#define USBPHY_RX_DISCONADJ_SHIFT (4U)

Definition at line 43366 of file MIMXRT1062.h.

## ◆ USBPHY_RX_ENVADJ

#define USBPHY_RX_ENVADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_ENVADJ_SHIFT)) & USBPHY_RX_ENVADJ_MASK)

Definition at line 43361 of file MIMXRT1062.h.

## ◆ USBPHY_RX_ENVADJ_MASK

#define USBPHY_RX_ENVADJ_MASK (0x7U)

Definition at line 43359 of file MIMXRT1062.h.

## ◆ USBPHY_RX_ENVADJ_SHIFT

#define USBPHY_RX_ENVADJ_SHIFT (0U)

Definition at line 43360 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD0

#define USBPHY_RX_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RSVD0_SHIFT)) & USBPHY_RX_RSVD0_MASK)

Definition at line 43364 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD0_MASK

#define USBPHY_RX_RSVD0_MASK (0x8U)

Definition at line 43362 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD0_SHIFT

#define USBPHY_RX_RSVD0_SHIFT (3U)

Definition at line 43363 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD1

#define USBPHY_RX_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RSVD1_SHIFT)) & USBPHY_RX_RSVD1_MASK)

Definition at line 43370 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD1_MASK

#define USBPHY_RX_RSVD1_MASK (0x3FFF80U)

Definition at line 43368 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD1_SHIFT

#define USBPHY_RX_RSVD1_SHIFT (7U)

Definition at line 43369 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD2

#define USBPHY_RX_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RSVD2_SHIFT)) & USBPHY_RX_RSVD2_MASK)

Definition at line 43376 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD2_MASK

#define USBPHY_RX_RSVD2_MASK (0xFF800000U)

Definition at line 43374 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RSVD2_SHIFT

#define USBPHY_RX_RSVD2_SHIFT (23U)

Definition at line 43375 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RXDBYPASS

#define USBPHY_RX_RXDBYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_RXDBYPASS_SHIFT)) & USBPHY_RX_RXDBYPASS_MASK)

Definition at line 43373 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RXDBYPASS_MASK

#define USBPHY_RX_RXDBYPASS_MASK (0x400000U)

Definition at line 43371 of file MIMXRT1062.h.

## ◆ USBPHY_RX_RXDBYPASS_SHIFT

#define USBPHY_RX_RXDBYPASS_SHIFT (22U)

Definition at line 43372 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_DISCONADJ

#define USBPHY_RX_SET_DISCONADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_DISCONADJ_SHIFT)) & USBPHY_RX_SET_DISCONADJ_MASK)

Definition at line 43389 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_DISCONADJ_MASK

#define USBPHY_RX_SET_DISCONADJ_MASK (0x70U)

Definition at line 43387 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_DISCONADJ_SHIFT

#define USBPHY_RX_SET_DISCONADJ_SHIFT (4U)

Definition at line 43388 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_ENVADJ

#define USBPHY_RX_SET_ENVADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_ENVADJ_SHIFT)) & USBPHY_RX_SET_ENVADJ_MASK)

Definition at line 43383 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_ENVADJ_MASK

#define USBPHY_RX_SET_ENVADJ_MASK (0x7U)

Definition at line 43381 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_ENVADJ_SHIFT

#define USBPHY_RX_SET_ENVADJ_SHIFT (0U)

Definition at line 43382 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD0

#define USBPHY_RX_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RSVD0_SHIFT)) & USBPHY_RX_SET_RSVD0_MASK)

Definition at line 43386 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD0_MASK

#define USBPHY_RX_SET_RSVD0_MASK (0x8U)

Definition at line 43384 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD0_SHIFT

#define USBPHY_RX_SET_RSVD0_SHIFT (3U)

Definition at line 43385 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD1

#define USBPHY_RX_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RSVD1_SHIFT)) & USBPHY_RX_SET_RSVD1_MASK)

Definition at line 43392 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD1_MASK

#define USBPHY_RX_SET_RSVD1_MASK (0x3FFF80U)

Definition at line 43390 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD1_SHIFT

#define USBPHY_RX_SET_RSVD1_SHIFT (7U)

Definition at line 43391 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD2

#define USBPHY_RX_SET_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RSVD2_SHIFT)) & USBPHY_RX_SET_RSVD2_MASK)

Definition at line 43398 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD2_MASK

#define USBPHY_RX_SET_RSVD2_MASK (0xFF800000U)

Definition at line 43396 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RSVD2_SHIFT

#define USBPHY_RX_SET_RSVD2_SHIFT (23U)

Definition at line 43397 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RXDBYPASS

#define USBPHY_RX_SET_RXDBYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_SET_RXDBYPASS_SHIFT)) & USBPHY_RX_SET_RXDBYPASS_MASK)

Definition at line 43395 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RXDBYPASS_MASK

#define USBPHY_RX_SET_RXDBYPASS_MASK (0x400000U)

Definition at line 43393 of file MIMXRT1062.h.

## ◆ USBPHY_RX_SET_RXDBYPASS_SHIFT

#define USBPHY_RX_SET_RXDBYPASS_SHIFT (22U)

Definition at line 43394 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_DISCONADJ

#define USBPHY_RX_TOG_DISCONADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_DISCONADJ_SHIFT)) & USBPHY_RX_TOG_DISCONADJ_MASK)

Definition at line 43433 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_DISCONADJ_MASK

#define USBPHY_RX_TOG_DISCONADJ_MASK (0x70U)

Definition at line 43431 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_DISCONADJ_SHIFT

#define USBPHY_RX_TOG_DISCONADJ_SHIFT (4U)

Definition at line 43432 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_ENVADJ

#define USBPHY_RX_TOG_ENVADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_ENVADJ_SHIFT)) & USBPHY_RX_TOG_ENVADJ_MASK)

Definition at line 43427 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_ENVADJ_MASK

#define USBPHY_RX_TOG_ENVADJ_MASK (0x7U)

Definition at line 43425 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_ENVADJ_SHIFT

#define USBPHY_RX_TOG_ENVADJ_SHIFT (0U)

Definition at line 43426 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD0

#define USBPHY_RX_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RSVD0_SHIFT)) & USBPHY_RX_TOG_RSVD0_MASK)

Definition at line 43430 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD0_MASK

#define USBPHY_RX_TOG_RSVD0_MASK (0x8U)

Definition at line 43428 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD0_SHIFT

#define USBPHY_RX_TOG_RSVD0_SHIFT (3U)

Definition at line 43429 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD1

#define USBPHY_RX_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RSVD1_SHIFT)) & USBPHY_RX_TOG_RSVD1_MASK)

Definition at line 43436 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD1_MASK

#define USBPHY_RX_TOG_RSVD1_MASK (0x3FFF80U)

Definition at line 43434 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD1_SHIFT

#define USBPHY_RX_TOG_RSVD1_SHIFT (7U)

Definition at line 43435 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD2

#define USBPHY_RX_TOG_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RSVD2_SHIFT)) & USBPHY_RX_TOG_RSVD2_MASK)

Definition at line 43442 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD2_MASK

#define USBPHY_RX_TOG_RSVD2_MASK (0xFF800000U)

Definition at line 43440 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RSVD2_SHIFT

#define USBPHY_RX_TOG_RSVD2_SHIFT (23U)

Definition at line 43441 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RXDBYPASS

#define USBPHY_RX_TOG_RXDBYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_RX_TOG_RXDBYPASS_SHIFT)) & USBPHY_RX_TOG_RXDBYPASS_MASK)

Definition at line 43439 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RXDBYPASS_MASK

#define USBPHY_RX_TOG_RXDBYPASS_MASK (0x400000U)

Definition at line 43437 of file MIMXRT1062.h.

## ◆ USBPHY_RX_TOG_RXDBYPASS_SHIFT

#define USBPHY_RX_TOG_RXDBYPASS_SHIFT (22U)

Definition at line 43438 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_DEVPLUGIN_STATUS

#define USBPHY_STATUS_DEVPLUGIN_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_DEVPLUGIN_STATUS_SHIFT)) & USBPHY_STATUS_DEVPLUGIN_STATUS_MASK)

Definition at line 43846 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_DEVPLUGIN_STATUS_MASK

#define USBPHY_STATUS_DEVPLUGIN_STATUS_MASK (0x40U)

Definition at line 43844 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_DEVPLUGIN_STATUS_SHIFT

#define USBPHY_STATUS_DEVPLUGIN_STATUS_SHIFT (6U)

Definition at line 43845 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_HOSTDISCONDETECT_STATUS

#define USBPHY_STATUS_HOSTDISCONDETECT_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_HOSTDISCONDETECT_STATUS_SHIFT)) & USBPHY_STATUS_HOSTDISCONDETECT_STATUS_MASK)

Definition at line 43840 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_HOSTDISCONDETECT_STATUS_MASK

#define USBPHY_STATUS_HOSTDISCONDETECT_STATUS_MASK (0x8U)

Definition at line 43838 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_HOSTDISCONDETECT_STATUS_SHIFT

#define USBPHY_STATUS_HOSTDISCONDETECT_STATUS_SHIFT (3U)

Definition at line 43839 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_OTGID_STATUS

#define USBPHY_STATUS_OTGID_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_OTGID_STATUS_SHIFT)) & USBPHY_STATUS_OTGID_STATUS_MASK)

Definition at line 43852 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_OTGID_STATUS_MASK

#define USBPHY_STATUS_OTGID_STATUS_MASK (0x100U)

Definition at line 43850 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_OTGID_STATUS_SHIFT

#define USBPHY_STATUS_OTGID_STATUS_SHIFT (8U)

Definition at line 43851 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RESUME_STATUS

#define USBPHY_STATUS_RESUME_STATUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RESUME_STATUS_SHIFT)) & USBPHY_STATUS_RESUME_STATUS_MASK)

Definition at line 43858 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RESUME_STATUS_MASK

#define USBPHY_STATUS_RESUME_STATUS_MASK (0x400U)

Definition at line 43856 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RESUME_STATUS_SHIFT

#define USBPHY_STATUS_RESUME_STATUS_SHIFT (10U)

Definition at line 43857 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD0

#define USBPHY_STATUS_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD0_SHIFT)) & USBPHY_STATUS_RSVD0_MASK)

Definition at line 43837 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD0_MASK

#define USBPHY_STATUS_RSVD0_MASK (0x7U)

Definition at line 43835 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD0_SHIFT

#define USBPHY_STATUS_RSVD0_SHIFT (0U)

Definition at line 43836 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD1

#define USBPHY_STATUS_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD1_SHIFT)) & USBPHY_STATUS_RSVD1_MASK)

Definition at line 43843 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD1_MASK

#define USBPHY_STATUS_RSVD1_MASK (0x30U)

Definition at line 43841 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD1_SHIFT

#define USBPHY_STATUS_RSVD1_SHIFT (4U)

Definition at line 43842 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD2

#define USBPHY_STATUS_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD2_SHIFT)) & USBPHY_STATUS_RSVD2_MASK)

Definition at line 43849 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD2_MASK

#define USBPHY_STATUS_RSVD2_MASK (0x80U)

Definition at line 43847 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD2_SHIFT

#define USBPHY_STATUS_RSVD2_SHIFT (7U)

Definition at line 43848 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD3

#define USBPHY_STATUS_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD3_SHIFT)) & USBPHY_STATUS_RSVD3_MASK)

Definition at line 43855 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD3_MASK

#define USBPHY_STATUS_RSVD3_MASK (0x200U)

Definition at line 43853 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD3_SHIFT

#define USBPHY_STATUS_RSVD3_SHIFT (9U)

Definition at line 43854 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD4

#define USBPHY_STATUS_RSVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_STATUS_RSVD4_SHIFT)) & USBPHY_STATUS_RSVD4_MASK)

Definition at line 43861 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD4_MASK

#define USBPHY_STATUS_RSVD4_MASK (0xFFFFF800U)

Definition at line 43859 of file MIMXRT1062.h.

## ◆ USBPHY_STATUS_RSVD4_SHIFT

#define USBPHY_STATUS_RSVD4_SHIFT (11U)

Definition at line 43860 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_D_CAL

#define USBPHY_TX_CLR_D_CAL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_D_CAL_SHIFT)) & USBPHY_TX_CLR_D_CAL_MASK)

Definition at line 43305 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_D_CAL_MASK

#define USBPHY_TX_CLR_D_CAL_MASK (0xFU)

Definition at line 43303 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_D_CAL_SHIFT

#define USBPHY_TX_CLR_D_CAL_SHIFT (0U)

Definition at line 43304 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD0

#define USBPHY_TX_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD0_SHIFT)) & USBPHY_TX_CLR_RSVD0_MASK)

Definition at line 43308 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD0_MASK

#define USBPHY_TX_CLR_RSVD0_MASK (0xF0U)

Definition at line 43306 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD0_SHIFT

#define USBPHY_TX_CLR_RSVD0_SHIFT (4U)

Definition at line 43307 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD1

#define USBPHY_TX_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD1_SHIFT)) & USBPHY_TX_CLR_RSVD1_MASK)

Definition at line 43314 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD1_MASK

#define USBPHY_TX_CLR_RSVD1_MASK (0xF000U)

Definition at line 43312 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD1_SHIFT

#define USBPHY_TX_CLR_RSVD1_SHIFT (12U)

Definition at line 43313 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD2

#define USBPHY_TX_CLR_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD2_SHIFT)) & USBPHY_TX_CLR_RSVD2_MASK)

Definition at line 43320 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD2_MASK

#define USBPHY_TX_CLR_RSVD2_MASK (0x3F00000U)

Definition at line 43318 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD2_SHIFT

#define USBPHY_TX_CLR_RSVD2_SHIFT (20U)

Definition at line 43319 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD5

#define USBPHY_TX_CLR_RSVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_RSVD5_SHIFT)) & USBPHY_TX_CLR_RSVD5_MASK)

Definition at line 43326 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD5_MASK

#define USBPHY_TX_CLR_RSVD5_MASK (0xE0000000U)

Definition at line 43324 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_RSVD5_SHIFT

#define USBPHY_TX_CLR_RSVD5_SHIFT (29U)

Definition at line 43325 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_TXCAL45DN

#define USBPHY_TX_CLR_TXCAL45DN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_TXCAL45DN_SHIFT)) & USBPHY_TX_CLR_TXCAL45DN_MASK)

Definition at line 43311 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_TXCAL45DN_MASK

#define USBPHY_TX_CLR_TXCAL45DN_MASK (0xF00U)

Definition at line 43309 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_TXCAL45DN_SHIFT

#define USBPHY_TX_CLR_TXCAL45DN_SHIFT (8U)

Definition at line 43310 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_TXCAL45DP

#define USBPHY_TX_CLR_TXCAL45DP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_TXCAL45DP_SHIFT)) & USBPHY_TX_CLR_TXCAL45DP_MASK)

Definition at line 43317 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_TXCAL45DP_MASK

#define USBPHY_TX_CLR_TXCAL45DP_MASK (0xF0000U)

Definition at line 43315 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_TXCAL45DP_SHIFT

#define USBPHY_TX_CLR_TXCAL45DP_SHIFT (16U)

Definition at line 43316 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_USBPHY_TX_EDGECTRL

#define USBPHY_TX_CLR_USBPHY_TX_EDGECTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_MASK)

Definition at line 43323 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_MASK

#define USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)

Definition at line 43321 of file MIMXRT1062.h.

## ◆ USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_SHIFT

#define USBPHY_TX_CLR_USBPHY_TX_EDGECTRL_SHIFT (26U)

Definition at line 43322 of file MIMXRT1062.h.

## ◆ USBPHY_TX_D_CAL

#define USBPHY_TX_D_CAL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_D_CAL_SHIFT)) & USBPHY_TX_D_CAL_MASK)

Definition at line 43249 of file MIMXRT1062.h.

## ◆ USBPHY_TX_D_CAL_MASK

#define USBPHY_TX_D_CAL_MASK (0xFU)

Definition at line 43247 of file MIMXRT1062.h.

## ◆ USBPHY_TX_D_CAL_SHIFT

#define USBPHY_TX_D_CAL_SHIFT (0U)

Definition at line 43248 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD0

#define USBPHY_TX_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD0_SHIFT)) & USBPHY_TX_RSVD0_MASK)

Definition at line 43252 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD0_MASK

#define USBPHY_TX_RSVD0_MASK (0xF0U)

Definition at line 43250 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD0_SHIFT

#define USBPHY_TX_RSVD0_SHIFT (4U)

Definition at line 43251 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD1

#define USBPHY_TX_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD1_SHIFT)) & USBPHY_TX_RSVD1_MASK)

Definition at line 43258 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD1_MASK

#define USBPHY_TX_RSVD1_MASK (0xF000U)

Definition at line 43256 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD1_SHIFT

#define USBPHY_TX_RSVD1_SHIFT (12U)

Definition at line 43257 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD2

#define USBPHY_TX_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD2_SHIFT)) & USBPHY_TX_RSVD2_MASK)

Definition at line 43264 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD2_MASK

#define USBPHY_TX_RSVD2_MASK (0x3F00000U)

Definition at line 43262 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD2_SHIFT

#define USBPHY_TX_RSVD2_SHIFT (20U)

Definition at line 43263 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD5

#define USBPHY_TX_RSVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_RSVD5_SHIFT)) & USBPHY_TX_RSVD5_MASK)

Definition at line 43270 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD5_MASK

#define USBPHY_TX_RSVD5_MASK (0xE0000000U)

Definition at line 43268 of file MIMXRT1062.h.

## ◆ USBPHY_TX_RSVD5_SHIFT

#define USBPHY_TX_RSVD5_SHIFT (29U)

Definition at line 43269 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_D_CAL

#define USBPHY_TX_SET_D_CAL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_D_CAL_SHIFT)) & USBPHY_TX_SET_D_CAL_MASK)

Definition at line 43277 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_D_CAL_MASK

#define USBPHY_TX_SET_D_CAL_MASK (0xFU)

Definition at line 43275 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_D_CAL_SHIFT

#define USBPHY_TX_SET_D_CAL_SHIFT (0U)

Definition at line 43276 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD0

#define USBPHY_TX_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD0_SHIFT)) & USBPHY_TX_SET_RSVD0_MASK)

Definition at line 43280 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD0_MASK

#define USBPHY_TX_SET_RSVD0_MASK (0xF0U)

Definition at line 43278 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD0_SHIFT

#define USBPHY_TX_SET_RSVD0_SHIFT (4U)

Definition at line 43279 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD1

#define USBPHY_TX_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD1_SHIFT)) & USBPHY_TX_SET_RSVD1_MASK)

Definition at line 43286 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD1_MASK

#define USBPHY_TX_SET_RSVD1_MASK (0xF000U)

Definition at line 43284 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD1_SHIFT

#define USBPHY_TX_SET_RSVD1_SHIFT (12U)

Definition at line 43285 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD2

#define USBPHY_TX_SET_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD2_SHIFT)) & USBPHY_TX_SET_RSVD2_MASK)

Definition at line 43292 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD2_MASK

#define USBPHY_TX_SET_RSVD2_MASK (0x3F00000U)

Definition at line 43290 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD2_SHIFT

#define USBPHY_TX_SET_RSVD2_SHIFT (20U)

Definition at line 43291 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD5

#define USBPHY_TX_SET_RSVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_RSVD5_SHIFT)) & USBPHY_TX_SET_RSVD5_MASK)

Definition at line 43298 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD5_MASK

#define USBPHY_TX_SET_RSVD5_MASK (0xE0000000U)

Definition at line 43296 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_RSVD5_SHIFT

#define USBPHY_TX_SET_RSVD5_SHIFT (29U)

Definition at line 43297 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_TXCAL45DN

#define USBPHY_TX_SET_TXCAL45DN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_TXCAL45DN_SHIFT)) & USBPHY_TX_SET_TXCAL45DN_MASK)

Definition at line 43283 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_TXCAL45DN_MASK

#define USBPHY_TX_SET_TXCAL45DN_MASK (0xF00U)

Definition at line 43281 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_TXCAL45DN_SHIFT

#define USBPHY_TX_SET_TXCAL45DN_SHIFT (8U)

Definition at line 43282 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_TXCAL45DP

#define USBPHY_TX_SET_TXCAL45DP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_TXCAL45DP_SHIFT)) & USBPHY_TX_SET_TXCAL45DP_MASK)

Definition at line 43289 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_TXCAL45DP_MASK

#define USBPHY_TX_SET_TXCAL45DP_MASK (0xF0000U)

Definition at line 43287 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_TXCAL45DP_SHIFT

#define USBPHY_TX_SET_TXCAL45DP_SHIFT (16U)

Definition at line 43288 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_USBPHY_TX_EDGECTRL

#define USBPHY_TX_SET_USBPHY_TX_EDGECTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_SET_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_SET_USBPHY_TX_EDGECTRL_MASK)

Definition at line 43295 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_USBPHY_TX_EDGECTRL_MASK

#define USBPHY_TX_SET_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)

Definition at line 43293 of file MIMXRT1062.h.

## ◆ USBPHY_TX_SET_USBPHY_TX_EDGECTRL_SHIFT

#define USBPHY_TX_SET_USBPHY_TX_EDGECTRL_SHIFT (26U)

Definition at line 43294 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_D_CAL

#define USBPHY_TX_TOG_D_CAL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_D_CAL_SHIFT)) & USBPHY_TX_TOG_D_CAL_MASK)

Definition at line 43333 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_D_CAL_MASK

#define USBPHY_TX_TOG_D_CAL_MASK (0xFU)

Definition at line 43331 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_D_CAL_SHIFT

#define USBPHY_TX_TOG_D_CAL_SHIFT (0U)

Definition at line 43332 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD0

#define USBPHY_TX_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD0_SHIFT)) & USBPHY_TX_TOG_RSVD0_MASK)

Definition at line 43336 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD0_MASK

#define USBPHY_TX_TOG_RSVD0_MASK (0xF0U)

Definition at line 43334 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD0_SHIFT

#define USBPHY_TX_TOG_RSVD0_SHIFT (4U)

Definition at line 43335 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD1

#define USBPHY_TX_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD1_SHIFT)) & USBPHY_TX_TOG_RSVD1_MASK)

Definition at line 43342 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD1_MASK

#define USBPHY_TX_TOG_RSVD1_MASK (0xF000U)

Definition at line 43340 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD1_SHIFT

#define USBPHY_TX_TOG_RSVD1_SHIFT (12U)

Definition at line 43341 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD2

#define USBPHY_TX_TOG_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD2_SHIFT)) & USBPHY_TX_TOG_RSVD2_MASK)

Definition at line 43348 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD2_MASK

#define USBPHY_TX_TOG_RSVD2_MASK (0x3F00000U)

Definition at line 43346 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD2_SHIFT

#define USBPHY_TX_TOG_RSVD2_SHIFT (20U)

Definition at line 43347 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD5

#define USBPHY_TX_TOG_RSVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_RSVD5_SHIFT)) & USBPHY_TX_TOG_RSVD5_MASK)

Definition at line 43354 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD5_MASK

#define USBPHY_TX_TOG_RSVD5_MASK (0xE0000000U)

Definition at line 43352 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_RSVD5_SHIFT

#define USBPHY_TX_TOG_RSVD5_SHIFT (29U)

Definition at line 43353 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_TXCAL45DN

#define USBPHY_TX_TOG_TXCAL45DN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_TXCAL45DN_SHIFT)) & USBPHY_TX_TOG_TXCAL45DN_MASK)

Definition at line 43339 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_TXCAL45DN_MASK

#define USBPHY_TX_TOG_TXCAL45DN_MASK (0xF00U)

Definition at line 43337 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_TXCAL45DN_SHIFT

#define USBPHY_TX_TOG_TXCAL45DN_SHIFT (8U)

Definition at line 43338 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_TXCAL45DP

#define USBPHY_TX_TOG_TXCAL45DP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_TXCAL45DP_SHIFT)) & USBPHY_TX_TOG_TXCAL45DP_MASK)

Definition at line 43345 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_TXCAL45DP_MASK

#define USBPHY_TX_TOG_TXCAL45DP_MASK (0xF0000U)

Definition at line 43343 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_TXCAL45DP_SHIFT

#define USBPHY_TX_TOG_TXCAL45DP_SHIFT (16U)

Definition at line 43344 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_USBPHY_TX_EDGECTRL

#define USBPHY_TX_TOG_USBPHY_TX_EDGECTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_MASK)

Definition at line 43351 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_MASK

#define USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)

Definition at line 43349 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_SHIFT

#define USBPHY_TX_TOG_USBPHY_TX_EDGECTRL_SHIFT (26U)

Definition at line 43350 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DN

#define USBPHY_TX_TXCAL45DN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TXCAL45DN_SHIFT)) & USBPHY_TX_TXCAL45DN_MASK)

Definition at line 43255 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DN_MASK

#define USBPHY_TX_TXCAL45DN_MASK (0xF00U)

Definition at line 43253 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DN_SHIFT

#define USBPHY_TX_TXCAL45DN_SHIFT (8U)

Definition at line 43254 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DP

#define USBPHY_TX_TXCAL45DP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_TXCAL45DP_SHIFT)) & USBPHY_TX_TXCAL45DP_MASK)

Definition at line 43261 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DP_MASK

#define USBPHY_TX_TXCAL45DP_MASK (0xF0000U)

Definition at line 43259 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DP_SHIFT

#define USBPHY_TX_TXCAL45DP_SHIFT (16U)

Definition at line 43260 of file MIMXRT1062.h.

## ◆ USBPHY_TX_USBPHY_TX_EDGECTRL

#define USBPHY_TX_USBPHY_TX_EDGECTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_TX_USBPHY_TX_EDGECTRL_SHIFT)) & USBPHY_TX_USBPHY_TX_EDGECTRL_MASK)

Definition at line 43267 of file MIMXRT1062.h.

## ◆ USBPHY_TX_USBPHY_TX_EDGECTRL_MASK

#define USBPHY_TX_USBPHY_TX_EDGECTRL_MASK (0x1C000000U)

Definition at line 43265 of file MIMXRT1062.h.

## ◆ USBPHY_TX_USBPHY_TX_EDGECTRL_SHIFT

#define USBPHY_TX_USBPHY_TX_EDGECTRL_SHIFT (26U)

Definition at line 43266 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_MAJOR

#define USBPHY_VERSION_MAJOR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_VERSION_MAJOR_SHIFT)) & USBPHY_VERSION_MAJOR_MASK)

Definition at line 44135 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_MAJOR_MASK

#define USBPHY_VERSION_MAJOR_MASK (0xFF000000U)

Definition at line 44133 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_MAJOR_SHIFT

#define USBPHY_VERSION_MAJOR_SHIFT (24U)

Definition at line 44134 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_MINOR

#define USBPHY_VERSION_MINOR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_VERSION_MINOR_SHIFT)) & USBPHY_VERSION_MINOR_MASK)

Definition at line 44132 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_MINOR_MASK

#define USBPHY_VERSION_MINOR_MASK (0xFF0000U)

Definition at line 44130 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_MINOR_SHIFT

#define USBPHY_VERSION_MINOR_SHIFT (16U)

Definition at line 44131 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_STEP

#define USBPHY_VERSION_STEP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << USBPHY_VERSION_STEP_SHIFT)) & USBPHY_VERSION_STEP_MASK)

Definition at line 44129 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_STEP_MASK

#define USBPHY_VERSION_STEP_MASK (0xFFFFU)

Definition at line 44127 of file MIMXRT1062.h.

## ◆ USBPHY_VERSION_STEP_SHIFT

#define USBPHY_VERSION_STEP_SHIFT (0U)

Definition at line 44128 of file MIMXRT1062.h.