Callisto4Bootloader: FLEXIO_Type Struct Reference

Callisto4Bootloader

Data Fields
FLEXIO_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » FLEXIO Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__I uint32_t | VERID
__I uint32_t | PARAM
__IO uint32_t | CTRL
__I uint32_t | PIN
__IO uint32_t | SHIFTSTAT
__IO uint32_t | SHIFTERR
__IO uint32_t | TIMSTAT
uint8_t | RESERVED_0 [4]
__IO uint32_t | SHIFTSIEN
__IO uint32_t | SHIFTEIEN
__IO uint32_t | TIMIEN
uint8_t | RESERVED_1 [4]
__IO uint32_t | SHIFTSDEN
uint8_t | RESERVED_2 [12]
__IO uint32_t | SHIFTSTATE
uint8_t | RESERVED_3 [60]
__IO uint32_t | SHIFTCTL [4]
uint8_t | RESERVED_4 [112]
__IO uint32_t | SHIFTCFG [4]
uint8_t | RESERVED_5 [240]
__IO uint32_t | SHIFTBUF [4]
uint8_t | RESERVED_6 [112]
__IO uint32_t | SHIFTBUFBIS [4]
uint8_t | RESERVED_7 [112]
__IO uint32_t | SHIFTBUFBYS [4]
uint8_t | RESERVED_8 [112]
__IO uint32_t | SHIFTBUFBBS [4]
uint8_t | RESERVED_9 [112]
__IO uint32_t | TIMCTL [4]
uint8_t | RESERVED_10 [112]
__IO uint32_t | TIMCFG [4]
uint8_t | RESERVED_11 [112]
__IO uint32_t | TIMCMP [4]
uint8_t | RESERVED_12 [368]
__IO uint32_t | SHIFTBUFNBS [4]
uint8_t | RESERVED_13 [112]
__IO uint32_t | SHIFTBUFHWS [4]
uint8_t | RESERVED_14 [112]
__IO uint32_t | SHIFTBUFNIS [4]

## Detailed Description

FLEXIO - Register Layout Typedef

Definition at line 18554 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h