Callisto4Bootloader: IOMUXC_SNVS_Type Struct Reference

Callisto4Bootloader

Data Fields
IOMUXC_SNVS_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » IOMUXC_SNVS Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | SW_MUX_CTL_PAD_WAKEUP
__IO uint32_t | SW_MUX_CTL_PAD_PMIC_ON_REQ
__IO uint32_t | SW_MUX_CTL_PAD_PMIC_STBY_REQ
__IO uint32_t | SW_PAD_CTL_PAD_TEST_MODE
__IO uint32_t | SW_PAD_CTL_PAD_POR_B
__IO uint32_t | SW_PAD_CTL_PAD_ONOFF
__IO uint32_t | SW_PAD_CTL_PAD_WAKEUP
__IO uint32_t | SW_PAD_CTL_PAD_PMIC_ON_REQ
__IO uint32_t | SW_PAD_CTL_PAD_PMIC_STBY_REQ

## Detailed Description

IOMUXC_SNVS - Register Layout Typedef

Definition at line 24393 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h