Callisto4Bootloader: LED connections onto the processor GPIO pins.

Callisto4Bootloader

Macros
LED connections onto the processor GPIO pins.

## Macros

#define | LEDS_GPIO BOARD_USER_LED_GPIO
| Which GPIO controller to use - GPIO2. More...
#define | RED_LED_GPIO_PIN BOARD_USER_LED_RED_PIN
| GPIO pin for RED LED - 9. More...
#define | GREEN_LED_GPIO_PIN BOARD_USER_LED_GREEN_PIN
| GPIO pin for GREEN LED - 10. More...
#define | BLUE_LED_GPIO_PIN BOARD_USER_LED_BLUE_PIN
| GPIO pin for BLUE LED - 11. More...

## Detailed Description

## Macro Definition Documentation

## ◆ BLUE_LED_GPIO_PIN

#define BLUE_LED_GPIO_PIN BOARD_USER_LED_BLUE_PIN

GPIO pin for BLUE LED - 11.

Definition at line 26 of file c4_colours.c.

## ◆ GREEN_LED_GPIO_PIN

#define GREEN_LED_GPIO_PIN BOARD_USER_LED_GREEN_PIN

GPIO pin for GREEN LED - 10.

Definition at line 25 of file c4_colours.c.

## ◆ LEDS_GPIO

#define LEDS_GPIO BOARD_USER_LED_GPIO

Which GPIO controller to use - GPIO2.

Definition at line 23 of file c4_colours.c.

## ◆ RED_LED_GPIO_PIN

#define RED_LED_GPIO_PIN BOARD_USER_LED_RED_PIN

GPIO pin for RED LED - 9.

Definition at line 24 of file c4_colours.c.