Callisto4Bootloader: Interrupt vector numbers

Callisto4Bootloader

Macros | Typedefs | Enumerations
Interrupt vector numbers

## Macros

#define | NUMBER_OF_INT_VECTORS 174

## Typedefs

typedef enum IRQn | IRQn_Type

## Enumerations

enum

IRQn {
NotAvail_IRQn = -128, NonMaskableInt_IRQn = -14, HardFault_IRQn = -13, MemoryManagement_IRQn = -12,
BusFault_IRQn = -11, UsageFault_IRQn = -10, SVCall_IRQn = -5, DebugMonitor_IRQn = -4,
PendSV_IRQn = -2, SysTick_IRQn = -1, DMA0_DMA16_IRQn = 0, DMA1_DMA17_IRQn = 1,
DMA2_DMA18_IRQn = 2, DMA3_DMA19_IRQn = 3, DMA4_DMA20_IRQn = 4, DMA5_DMA21_IRQn = 5,
DMA6_DMA22_IRQn = 6, DMA7_DMA23_IRQn = 7, DMA8_DMA24_IRQn = 8, DMA9_DMA25_IRQn = 9,
DMA10_DMA26_IRQn = 10, DMA11_DMA27_IRQn = 11, DMA12_DMA28_IRQn = 12, DMA13_DMA29_IRQn = 13,
DMA14_DMA30_IRQn = 14, DMA15_DMA31_IRQn = 15, DMA_ERROR_IRQn = 16, CTI0_ERROR_IRQn = 17,
CTI1_ERROR_IRQn = 18, CORE_IRQn = 19, LPUART1_IRQn = 20, LPUART2_IRQn = 21,
LPUART3_IRQn = 22, LPUART4_IRQn = 23, LPUART5_IRQn = 24, LPUART6_IRQn = 25,
LPUART7_IRQn = 26, LPUART8_IRQn = 27, LPI2C1_IRQn = 28, LPI2C2_IRQn = 29,
LPI2C3_IRQn = 30, LPI2C4_IRQn = 31, LPSPI1_IRQn = 32, LPSPI2_IRQn = 33,
LPSPI3_IRQn = 34, LPSPI4_IRQn = 35, CAN1_IRQn = 36, CAN2_IRQn = 37,
FLEXRAM_IRQn = 38, KPP_IRQn = 39, TSC_DIG_IRQn = 40, GPR_IRQ_IRQn = 41,
LCDIF_IRQn = 42, CSI_IRQn = 43, PXP_IRQn = 44, WDOG2_IRQn = 45,
SNVS_HP_WRAPPER_IRQn = 46, SNVS_HP_WRAPPER_TZ_IRQn = 47, SNVS_LP_WRAPPER_IRQn = 48, CSU_IRQn = 49,
DCP_IRQn = 50, DCP_VMI_IRQn = 51, Reserved68_IRQn = 52, TRNG_IRQn = 53,
SJC_IRQn = 54, BEE_IRQn = 55, SAI1_IRQn = 56, SAI2_IRQn = 57,
SAI3_RX_IRQn = 58, SAI3_TX_IRQn = 59, SPDIF_IRQn = 60, PMU_EVENT_IRQn = 61,
Reserved78_IRQn = 62, TEMP_LOW_HIGH_IRQn = 63, TEMP_PANIC_IRQn = 64, USB_PHY1_IRQn = 65,
USB_PHY2_IRQn = 66, ADC1_IRQn = 67, ADC2_IRQn = 68, DCDC_IRQn = 69,
Reserved86_IRQn = 70, Reserved87_IRQn = 71, GPIO1_INT0_IRQn = 72, GPIO1_INT1_IRQn = 73,
GPIO1_INT2_IRQn = 74, GPIO1_INT3_IRQn = 75, GPIO1_INT4_IRQn = 76, GPIO1_INT5_IRQn = 77,
GPIO1_INT6_IRQn = 78, GPIO1_INT7_IRQn = 79, GPIO1_Combined_0_15_IRQn = 80, GPIO1_Combined_16_31_IRQn = 81,
GPIO2_Combined_0_15_IRQn = 82, GPIO2_Combined_16_31_IRQn = 83, GPIO3_Combined_0_15_IRQn = 84, GPIO3_Combined_16_31_IRQn = 85,
GPIO4_Combined_0_15_IRQn = 86, GPIO4_Combined_16_31_IRQn = 87, GPIO5_Combined_0_15_IRQn = 88, GPIO5_Combined_16_31_IRQn = 89,
FLEXIO1_IRQn = 90, FLEXIO2_IRQn = 91, WDOG1_IRQn = 92, RTWDOG_IRQn = 93,
EWM_IRQn = 94, CCM_1_IRQn = 95, CCM_2_IRQn = 96, GPC_IRQn = 97,
SRC_IRQn = 98, Reserved115_IRQn = 99, GPT1_IRQn = 100, GPT2_IRQn = 101,
PWM1_0_IRQn = 102, PWM1_1_IRQn = 103, PWM1_2_IRQn = 104, PWM1_3_IRQn = 105,
PWM1_FAULT_IRQn = 106, FLEXSPI2_IRQn = 107, FLEXSPI_IRQn = 108, SEMC_IRQn = 109,
USDHC1_IRQn = 110, USDHC2_IRQn = 111, USB_OTG2_IRQn = 112, USB_OTG1_IRQn = 113,
ENET_IRQn = 114, ENET_1588_Timer_IRQn = 115, XBAR1_IRQ_0_1_IRQn = 116, XBAR1_IRQ_2_3_IRQn = 117,
ADC_ETC_IRQ0_IRQn = 118, ADC_ETC_IRQ1_IRQn = 119, ADC_ETC_IRQ2_IRQn = 120, ADC_ETC_ERROR_IRQ_IRQn = 121,
PIT_IRQn = 122, ACMP1_IRQn = 123, ACMP2_IRQn = 124, ACMP3_IRQn = 125,
ACMP4_IRQn = 126, Reserved143_IRQn = 127, Reserved144_IRQn = 128, ENC1_IRQn = 129,
ENC2_IRQn = 130, ENC3_IRQn = 131, ENC4_IRQn = 132, TMR1_IRQn = 133,
TMR2_IRQn = 134, TMR3_IRQn = 135, TMR4_IRQn = 136, PWM2_0_IRQn = 137,
PWM2_1_IRQn = 138, PWM2_2_IRQn = 139, PWM2_3_IRQn = 140, PWM2_FAULT_IRQn = 141,
PWM3_0_IRQn = 142, PWM3_1_IRQn = 143, PWM3_2_IRQn = 144, PWM3_3_IRQn = 145,
PWM3_FAULT_IRQn = 146, PWM4_0_IRQn = 147, PWM4_1_IRQn = 148, PWM4_2_IRQn = 149,
PWM4_3_IRQn = 150, PWM4_FAULT_IRQn = 151, ENET2_IRQn = 152, ENET2_1588_Timer_IRQn = 153,
CAN3_IRQn = 154, Reserved171_IRQn = 155, FLEXIO3_IRQn = 156, GPIO6_7_8_9_IRQn = 157
}

## Detailed Description

## Macro Definition Documentation

## ◆ NUMBER_OF_INT_VECTORS

#define NUMBER_OF_INT_VECTORS 174

Interrupt Number Definitions Number of interrupts in the Vector table

Definition at line 72 of file MIMXRT1062.h.

## Typedef Documentation

## ◆ IRQn_Type

typedef enum IRQn IRQn_Type

## Enumeration Type Documentation

## ◆ IRQn

enum IRQn

Enumerator
NotAvail_IRQn | Not available device specific interrupt
NonMaskableInt_IRQn | Non Maskable Interrupt
HardFault_IRQn | Cortex-M7 SV Hard Fault Interrupt
MemoryManagement_IRQn | Cortex-M7 Memory Management Interrupt
BusFault_IRQn | Cortex-M7 Bus Fault Interrupt
UsageFault_IRQn | Cortex-M7 Usage Fault Interrupt
SVCall_IRQn | Cortex-M7 SV Call Interrupt
DebugMonitor_IRQn | Cortex-M7 Debug Monitor Interrupt
PendSV_IRQn | Cortex-M7 Pend SV Interrupt
SysTick_IRQn | Cortex-M7 System Tick Interrupt
DMA0_DMA16_IRQn | DMA channel 0/16 transfer complete
DMA1_DMA17_IRQn | DMA channel 1/17 transfer complete
DMA2_DMA18_IRQn | DMA channel 2/18 transfer complete
DMA3_DMA19_IRQn | DMA channel 3/19 transfer complete
DMA4_DMA20_IRQn | DMA channel 4/20 transfer complete
DMA5_DMA21_IRQn | DMA channel 5/21 transfer complete
DMA6_DMA22_IRQn | DMA channel 6/22 transfer complete
DMA7_DMA23_IRQn | DMA channel 7/23 transfer complete
DMA8_DMA24_IRQn | DMA channel 8/24 transfer complete
DMA9_DMA25_IRQn | DMA channel 9/25 transfer complete
DMA10_DMA26_IRQn | DMA channel 10/26 transfer complete
DMA11_DMA27_IRQn | DMA channel 11/27 transfer complete
DMA12_DMA28_IRQn | DMA channel 12/28 transfer complete
DMA13_DMA29_IRQn | DMA channel 13/29 transfer complete
DMA14_DMA30_IRQn | DMA channel 14/30 transfer complete
DMA15_DMA31_IRQn | DMA channel 15/31 transfer complete
DMA_ERROR_IRQn | DMA error interrupt channels 0-15 / 16-31
CTI0_ERROR_IRQn | CTI0_Error
CTI1_ERROR_IRQn | CTI1_Error
CORE_IRQn | CorePlatform exception IRQ
LPUART1_IRQn | LPUART1 TX interrupt and RX interrupt
LPUART2_IRQn | LPUART2 TX interrupt and RX interrupt
LPUART3_IRQn | LPUART3 TX interrupt and RX interrupt
LPUART4_IRQn | LPUART4 TX interrupt and RX interrupt
LPUART5_IRQn | LPUART5 TX interrupt and RX interrupt
LPUART6_IRQn | LPUART6 TX interrupt and RX interrupt
LPUART7_IRQn | LPUART7 TX interrupt and RX interrupt
LPUART8_IRQn | LPUART8 TX interrupt and RX interrupt
LPI2C1_IRQn | LPI2C1 interrupt
LPI2C2_IRQn | LPI2C2 interrupt
LPI2C3_IRQn | LPI2C3 interrupt
LPI2C4_IRQn | LPI2C4 interrupt
LPSPI1_IRQn | LPSPI1 single interrupt vector for all sources
LPSPI2_IRQn | LPSPI2 single interrupt vector for all sources
LPSPI3_IRQn | LPSPI3 single interrupt vector for all sources
LPSPI4_IRQn | LPSPI4 single interrupt vector for all sources
CAN1_IRQn | CAN1 interrupt
CAN2_IRQn | CAN2 interrupt
FLEXRAM_IRQn | FlexRAM address out of range Or access hit IRQ
KPP_IRQn | Keypad nterrupt
TSC_DIG_IRQn | TSC interrupt
GPR_IRQ_IRQn | GPR interrupt
LCDIF_IRQn | LCDIF interrupt
CSI_IRQn | CSI interrupt
PXP_IRQn | PXP interrupt
WDOG2_IRQn | WDOG2 interrupt
SNVS_HP_WRAPPER_IRQn | SRTC Consolidated Interrupt. Non TZ
SNVS_HP_WRAPPER_TZ_IRQn | SRTC Security Interrupt. TZ
SNVS_LP_WRAPPER_IRQn | ON-OFF button press shorter than 5 secs (pulse event)
CSU_IRQn | CSU interrupt
DCP_IRQn | DCP_IRQ interrupt
DCP_VMI_IRQn | DCP_VMI_IRQ interrupt
Reserved68_IRQn | Reserved interrupt
TRNG_IRQn | TRNG interrupt
SJC_IRQn | SJC interrupt
BEE_IRQn | BEE interrupt
SAI1_IRQn | SAI1 interrupt
SAI2_IRQn | SAI1 interrupt
SAI3_RX_IRQn | SAI3 interrupt
SAI3_TX_IRQn | SAI3 interrupt
SPDIF_IRQn | SPDIF interrupt
PMU_EVENT_IRQn | Brown-out event interrupt
Reserved78_IRQn | Reserved interrupt
TEMP_LOW_HIGH_IRQn | TempSensor low/high interrupt
TEMP_PANIC_IRQn | TempSensor panic interrupt
USB_PHY1_IRQn | USBPHY (UTMI0), Interrupt
USB_PHY2_IRQn | USBPHY (UTMI1), Interrupt
ADC1_IRQn | ADC1 interrupt
ADC2_IRQn | ADC2 interrupt
DCDC_IRQn | DCDC interrupt
Reserved86_IRQn | Reserved interrupt
Reserved87_IRQn | Reserved interrupt
GPIO1_INT0_IRQn | Active HIGH Interrupt from INT0 from GPIO
GPIO1_INT1_IRQn | Active HIGH Interrupt from INT1 from GPIO
GPIO1_INT2_IRQn | Active HIGH Interrupt from INT2 from GPIO
GPIO1_INT3_IRQn | Active HIGH Interrupt from INT3 from GPIO
GPIO1_INT4_IRQn | Active HIGH Interrupt from INT4 from GPIO
GPIO1_INT5_IRQn | Active HIGH Interrupt from INT5 from GPIO
GPIO1_INT6_IRQn | Active HIGH Interrupt from INT6 from GPIO
GPIO1_INT7_IRQn | Active HIGH Interrupt from INT7 from GPIO
GPIO1_Combined_0_15_IRQn | Combined interrupt indication for GPIO1 signal 0 throughout 15
GPIO1_Combined_16_31_IRQn | Combined interrupt indication for GPIO1 signal 16 throughout 31
GPIO2_Combined_0_15_IRQn | Combined interrupt indication for GPIO2 signal 0 throughout 15
GPIO2_Combined_16_31_IRQn | Combined interrupt indication for GPIO2 signal 16 throughout 31
GPIO3_Combined_0_15_IRQn | Combined interrupt indication for GPIO3 signal 0 throughout 15
GPIO3_Combined_16_31_IRQn | Combined interrupt indication for GPIO3 signal 16 throughout 31
GPIO4_Combined_0_15_IRQn | Combined interrupt indication for GPIO4 signal 0 throughout 15
GPIO4_Combined_16_31_IRQn | Combined interrupt indication for GPIO4 signal 16 throughout 31
GPIO5_Combined_0_15_IRQn | Combined interrupt indication for GPIO5 signal 0 throughout 15
GPIO5_Combined_16_31_IRQn | Combined interrupt indication for GPIO5 signal 16 throughout 31
FLEXIO1_IRQn | FLEXIO1 interrupt
FLEXIO2_IRQn | FLEXIO2 interrupt
WDOG1_IRQn | WDOG1 interrupt
RTWDOG_IRQn | RTWDOG interrupt
EWM_IRQn | EWM interrupt
CCM_1_IRQn | CCM IRQ1 interrupt
CCM_2_IRQn | CCM IRQ2 interrupt
GPC_IRQn | GPC interrupt
SRC_IRQn | SRC interrupt
Reserved115_IRQn | Reserved interrupt
GPT1_IRQn | GPT1 interrupt
GPT2_IRQn | GPT2 interrupt
PWM1_0_IRQn | PWM1 capture 0, compare 0, or reload 0 interrupt
PWM1_1_IRQn | PWM1 capture 1, compare 1, or reload 0 interrupt
PWM1_2_IRQn | PWM1 capture 2, compare 2, or reload 0 interrupt
PWM1_3_IRQn | PWM1 capture 3, compare 3, or reload 0 interrupt
PWM1_FAULT_IRQn | PWM1 fault or reload error interrupt
FLEXSPI2_IRQn | FlexSPI2 interrupt
FLEXSPI_IRQn | FlexSPI0 interrupt
SEMC_IRQn | Reserved interrupt
USDHC1_IRQn | USDHC1 interrupt
USDHC2_IRQn | USDHC2 interrupt
USB_OTG2_IRQn | USBO2 USB OTG2
USB_OTG1_IRQn | USBO2 USB OTG1
ENET_IRQn | ENET interrupt
ENET_1588_Timer_IRQn | ENET_1588_Timer interrupt
XBAR1_IRQ_0_1_IRQn | XBAR1 interrupt
XBAR1_IRQ_2_3_IRQn | XBAR1 interrupt
ADC_ETC_IRQ0_IRQn | ADCETC IRQ0 interrupt
ADC_ETC_IRQ1_IRQn | ADCETC IRQ1 interrupt
ADC_ETC_IRQ2_IRQn | ADCETC IRQ2 interrupt
ADC_ETC_ERROR_IRQ_IRQn | ADCETC Error IRQ interrupt
PIT_IRQn | PIT interrupt
ACMP1_IRQn | ACMP interrupt
ACMP2_IRQn | ACMP interrupt
ACMP3_IRQn | ACMP interrupt
ACMP4_IRQn | ACMP interrupt
Reserved143_IRQn | Reserved interrupt
Reserved144_IRQn | Reserved interrupt
ENC1_IRQn | ENC1 interrupt
ENC2_IRQn | ENC2 interrupt
ENC3_IRQn | ENC3 interrupt
ENC4_IRQn | ENC4 interrupt
TMR1_IRQn | TMR1 interrupt
TMR2_IRQn | TMR2 interrupt
TMR3_IRQn | TMR3 interrupt
TMR4_IRQn | TMR4 interrupt
PWM2_0_IRQn | PWM2 capture 0, compare 0, or reload 0 interrupt
PWM2_1_IRQn | PWM2 capture 1, compare 1, or reload 0 interrupt
PWM2_2_IRQn | PWM2 capture 2, compare 2, or reload 0 interrupt
PWM2_3_IRQn | PWM2 capture 3, compare 3, or reload 0 interrupt
PWM2_FAULT_IRQn | PWM2 fault or reload error interrupt
PWM3_0_IRQn | PWM3 capture 0, compare 0, or reload 0 interrupt
PWM3_1_IRQn | PWM3 capture 1, compare 1, or reload 0 interrupt
PWM3_2_IRQn | PWM3 capture 2, compare 2, or reload 0 interrupt
PWM3_3_IRQn | PWM3 capture 3, compare 3, or reload 0 interrupt
PWM3_FAULT_IRQn | PWM3 fault or reload error interrupt
PWM4_0_IRQn | PWM4 capture 0, compare 0, or reload 0 interrupt
PWM4_1_IRQn | PWM4 capture 1, compare 1, or reload 0 interrupt
PWM4_2_IRQn | PWM4 capture 2, compare 2, or reload 0 interrupt
PWM4_3_IRQn | PWM4 capture 3, compare 3, or reload 0 interrupt
PWM4_FAULT_IRQn | PWM4 fault or reload error interrupt
ENET2_IRQn | ENET2 interrupt
ENET2_1588_Timer_IRQn | ENET2_1588_Timer interrupt
CAN3_IRQn | CAN3 interrupt
Reserved171_IRQn | Reserved interrupt
FLEXIO3_IRQn | FLEXIO3 interrupt
GPIO6_7_8_9_IRQn | GPIO6, GPIO7, GPIO8, GPIO9 interrupt

Definition at line 74 of file MIMXRT1062.h.