Callisto4Bootloader: AOI Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
AOI Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| AOI Register Masks

## Data Structures

struct | AOI_Type

## Macros

#define | AOI1_BASE (0x403B4000u)
#define | AOI1 ((AOI_Type *)AOI1_BASE)
#define | AOI2_BASE (0x403B8000u)
#define | AOI2 ((AOI_Type *)AOI2_BASE)
#define | AOI_BASE_ADDRS { 0u, AOI1_BASE, AOI2_BASE }
#define | AOI_BASE_PTRS { (AOI_Type *)0u, AOI1, AOI2 }

## Detailed Description

## Macro Definition Documentation

## ◆ AOI1

#define AOI1 ((AOI_Type *)AOI1_BASE)

Peripheral AOI1 base pointer

Definition at line 3111 of file MIMXRT1062.h.

## ◆ AOI1_BASE

#define AOI1_BASE (0x403B4000u)

Peripheral AOI1 base address

Definition at line 3109 of file MIMXRT1062.h.

## ◆ AOI2

#define AOI2 ((AOI_Type *)AOI2_BASE)

Peripheral AOI2 base pointer

Definition at line 3115 of file MIMXRT1062.h.

## ◆ AOI2_BASE

#define AOI2_BASE (0x403B8000u)

Peripheral AOI2 base address

Definition at line 3113 of file MIMXRT1062.h.

## ◆ AOI_BASE_ADDRS

#define AOI_BASE_ADDRS { 0u, AOI1_BASE, AOI2_BASE }

Array initializer of AOI peripheral base addresses

Definition at line 3117 of file MIMXRT1062.h.

## ◆ AOI_BASE_PTRS

#define AOI_BASE_PTRS { (AOI_Type *)0u, AOI1, AOI2 }

Array initializer of AOI peripheral base pointers

Definition at line 3119 of file MIMXRT1062.h.