Callisto4Bootloader: drivers/target_config.h File Reference

Callisto4Bootloader

Enumerations | Functions
target_config.h File Reference

Go to the source code of this file.

## Enumerations

enum | { kFlexSpi_AhbMemoryMaxSizeMB = (504u * 1024u * 1024u) }
| Constants for FlexSPI features. More...
enum | _target_version_constants { kTarget_Version_Name = 'T', kTarget_Version_Major = 1, kTarget_Version_Minor = 0, kTarget_Version_Bugfix = 0 }
| Version constants for the target. More...

enum

{
kFlexSpiSerialClk_30MHz = 1, kFlexSpiSerialClk_50MHz = 2, kFlexSpiSerialClk_60MHz = 3, kFlexSpiSerialClk_75MHz = 4,
kFlexSpiSerialClk_80MHz = 5, kFlexSpiSerialClk_100MHz = 6, kFlexSpiSerialClk_120MHz = 7, kFlexSpiSerialClk_133MHz = 8,
kFlexSpiSerialClk_166MHz = 9, kFlexSpiSerialClk_200MHz = 10
}

| FlexSPI supported speed defintions. More...

## Functions

uint32_t | get_flexspinor_instance (void)
uint32_t | get_flexspinor_amba_base (void)

## Enumeration Type Documentation

## ◆ anonymous enum

anonymous enum

Constants for FlexSPI features.

Enumerator
kFlexSpi_AhbMemoryMaxSizeMB |

Definition at line 15 of file target_config.h.

## ◆ anonymous enum

anonymous enum

FlexSPI supported speed defintions.

Enumerator
kFlexSpiSerialClk_30MHz |
kFlexSpiSerialClk_50MHz |
kFlexSpiSerialClk_60MHz |
kFlexSpiSerialClk_75MHz |
kFlexSpiSerialClk_80MHz |
kFlexSpiSerialClk_100MHz |
kFlexSpiSerialClk_120MHz |
kFlexSpiSerialClk_133MHz |
kFlexSpiSerialClk_166MHz |
kFlexSpiSerialClk_200MHz |

Definition at line 30 of file target_config.h.

## ◆ _target_version_constants

enum _target_version_constants

Version constants for the target.

Enumerator
kTarget_Version_Name |
kTarget_Version_Major |
kTarget_Version_Minor |
kTarget_Version_Bugfix |

Definition at line 21 of file target_config.h.

## Function Documentation

## ◆ get_flexspinor_amba_base()

uint32_t get_flexspinor_amba_base | ( | void |  | ) |

## ◆ get_flexspinor_instance()

uint32_t get_flexspinor_instance | ( | void |  | ) |