Callisto4Bootloader: USBPHY Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
USBPHY Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| USBPHY Register Masks

## Data Structures

struct | USBPHY_Type

## Macros

#define | USBPHY1_BASE (0x400D9000u)
#define | USBPHY1 ((USBPHY_Type *)USBPHY1_BASE)
#define | USBPHY2_BASE (0x400DA000u)
#define | USBPHY2 ((USBPHY_Type *)USBPHY2_BASE)
#define | USBPHY_BASE_ADDRS { 0u, USBPHY1_BASE, USBPHY2_BASE }
#define | USBPHY_BASE_PTRS { (USBPHY_Type *)0u, USBPHY1, USBPHY2 }
#define | USBPHY_IRQS { NotAvail_IRQn, USB_PHY1_IRQn, USB_PHY2_IRQn }
#define | USBPHY_CTRL_ENDEVPLUGINDET_MASK USBPHY_CTRL_ENDEVPLUGINDETECT_MASK
#define | USBPHY_CTRL_ENDEVPLUGINDET_SHIFT USBPHY_CTRL_ENDEVPLUGINDETECT_SHIFT
#define | USBPHY_CTRL_ENDEVPLUGINDET(x) USBPHY_CTRL_ENDEVPLUGINDETECT(x)
#define | USBPHY_TX_TXCAL45DM_MASK USBPHY_TX_TXCAL45DN_MASK
#define | USBPHY_TX_TXCAL45DM_SHIFT USBPHY_TX_TXCAL45DN_SHIFT
#define | USBPHY_TX_TXCAL45DM(x) USBPHY_TX_TXCAL45DN(x)

## Detailed Description

## Macro Definition Documentation

## ◆ USBPHY1

#define USBPHY1 ((USBPHY_Type *)USBPHY1_BASE)

Peripheral USBPHY1 base pointer

Definition at line 44148 of file MIMXRT1062.h.

## ◆ USBPHY1_BASE

#define USBPHY1_BASE (0x400D9000u)

Peripheral USBPHY1 base address

Definition at line 44146 of file MIMXRT1062.h.

## ◆ USBPHY2

#define USBPHY2 ((USBPHY_Type *)USBPHY2_BASE)

Peripheral USBPHY2 base pointer

Definition at line 44152 of file MIMXRT1062.h.

## ◆ USBPHY2_BASE

#define USBPHY2_BASE (0x400DA000u)

Peripheral USBPHY2 base address

Definition at line 44150 of file MIMXRT1062.h.

## ◆ USBPHY_BASE_ADDRS

#define USBPHY_BASE_ADDRS { 0u, USBPHY1_BASE, USBPHY2_BASE }

Array initializer of USBPHY peripheral base addresses

Definition at line 44154 of file MIMXRT1062.h.

## ◆ USBPHY_BASE_PTRS

#define USBPHY_BASE_PTRS { (USBPHY_Type *)0u, USBPHY1, USBPHY2 }

Array initializer of USBPHY peripheral base pointers

Definition at line 44156 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDEVPLUGINDET

#define USBPHY_CTRL_ENDEVPLUGINDET | ( |  | x | ) | USBPHY_CTRL_ENDEVPLUGINDETECT(x)

Definition at line 44162 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDEVPLUGINDET_MASK

#define USBPHY_CTRL_ENDEVPLUGINDET_MASK USBPHY_CTRL_ENDEVPLUGINDETECT_MASK

Definition at line 44160 of file MIMXRT1062.h.

## ◆ USBPHY_CTRL_ENDEVPLUGINDET_SHIFT

#define USBPHY_CTRL_ENDEVPLUGINDET_SHIFT USBPHY_CTRL_ENDEVPLUGINDETECT_SHIFT

Definition at line 44161 of file MIMXRT1062.h.

## ◆ USBPHY_IRQS

#define USBPHY_IRQS { NotAvail_IRQn, USB_PHY1_IRQn, USB_PHY2_IRQn }

Interrupt vectors for the USBPHY peripheral type

Definition at line 44158 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DM

#define USBPHY_TX_TXCAL45DM | ( |  | x | ) | USBPHY_TX_TXCAL45DN(x)

Definition at line 44165 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DM_MASK

#define USBPHY_TX_TXCAL45DM_MASK USBPHY_TX_TXCAL45DN_MASK

Definition at line 44163 of file MIMXRT1062.h.

## ◆ USBPHY_TX_TXCAL45DM_SHIFT

#define USBPHY_TX_TXCAL45DM_SHIFT USBPHY_TX_TXCAL45DN_SHIFT

Definition at line 44164 of file MIMXRT1062.h.