Callisto4Bootloader: XBARB Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
XBARB Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| XBARB Register Masks

## Data Structures

struct | XBARB_Type

## Macros

#define | XBARB2_BASE (0x403C0000u)
#define | XBARB2 ((XBARB_Type *)XBARB2_BASE)
#define | XBARB3_BASE (0x403C4000u)
#define | XBARB3 ((XBARB_Type *)XBARB3_BASE)
#define | XBARB_BASE_ADDRS { 0u, 0u, XBARB2_BASE, XBARB3_BASE }
#define | XBARB_BASE_PTRS { (XBARB_Type *)0u, (XBARB_Type *)0u, XBARB2, XBARB3 }

## Detailed Description

## Macro Definition Documentation

## ◆ XBARB2

#define XBARB2 ((XBARB_Type *)XBARB2_BASE)

Peripheral XBARB2 base pointer

Definition at line 47528 of file MIMXRT1062.h.

## ◆ XBARB2_BASE

#define XBARB2_BASE (0x403C0000u)

Peripheral XBARB2 base address

Definition at line 47526 of file MIMXRT1062.h.

## ◆ XBARB3

#define XBARB3 ((XBARB_Type *)XBARB3_BASE)

Peripheral XBARB3 base pointer

Definition at line 47532 of file MIMXRT1062.h.

## ◆ XBARB3_BASE

#define XBARB3_BASE (0x403C4000u)

Peripheral XBARB3 base address

Definition at line 47530 of file MIMXRT1062.h.

## ◆ XBARB_BASE_ADDRS

#define XBARB_BASE_ADDRS { 0u, 0u, XBARB2_BASE, XBARB3_BASE }

Array initializer of XBARB peripheral base addresses

Definition at line 47534 of file MIMXRT1062.h.

## ◆ XBARB_BASE_PTRS

#define XBARB_BASE_PTRS { (XBARB_Type *)0u, (XBARB_Type *)0u, XBARB2, XBARB3 }

Array initializer of XBARB peripheral base pointers

Definition at line 47536 of file MIMXRT1062.h.