Callisto4Bootloader: USBNC Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
USBNC Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| USBNC Register Masks

## Data Structures

struct | USBNC_Type

## Macros

#define | USBNC1_BASE (0x402E0000u)
#define | USBNC1 ((USBNC_Type *)USBNC1_BASE)
#define | USBNC2_BASE (0x402E0004u)
#define | USBNC2 ((USBNC_Type *)USBNC2_BASE)
#define | USBNC_BASE_ADDRS { 0u, USBNC1_BASE, USBNC2_BASE }
#define | USBNC_BASE_PTRS { (USBNC_Type *)0u, USBNC1, USBNC2 }

## Detailed Description

## Macro Definition Documentation

## ◆ USBNC1

#define USBNC1 ((USBNC_Type *)USBNC1_BASE)

Peripheral USBNC1 base pointer

Definition at line 43043 of file MIMXRT1062.h.

## ◆ USBNC1_BASE

#define USBNC1_BASE (0x402E0000u)

Peripheral USBNC1 base address

Definition at line 43041 of file MIMXRT1062.h.

## ◆ USBNC2

#define USBNC2 ((USBNC_Type *)USBNC2_BASE)

Peripheral USBNC2 base pointer

Definition at line 43047 of file MIMXRT1062.h.

## ◆ USBNC2_BASE

#define USBNC2_BASE (0x402E0004u)

Peripheral USBNC2 base address

Definition at line 43045 of file MIMXRT1062.h.

## ◆ USBNC_BASE_ADDRS

#define USBNC_BASE_ADDRS { 0u, USBNC1_BASE, USBNC2_BASE }

Array initializer of USBNC peripheral base addresses

Definition at line 43049 of file MIMXRT1062.h.

## ◆ USBNC_BASE_PTRS

#define USBNC_BASE_PTRS { (USBNC_Type *)0u, USBNC1, USBNC2 }

Array initializer of USBNC peripheral base pointers

Definition at line 43051 of file MIMXRT1062.h.