Callisto4Bootloader: OCOTP Register Masks

Callisto4Bootloader

OCOTP Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » OCOTP Peripheral Access Layer

## CTRL - OTP Controller Control Register

#define | OCOTP_CTRL_ADDR_MASK (0x3FU)
#define | OCOTP_CTRL_ADDR_SHIFT (0U)
#define | OCOTP_CTRL_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_ADDR_SHIFT)) & OCOTP_CTRL_ADDR_MASK)
#define | OCOTP_CTRL_RSVD0_MASK (0xC0U)
#define | OCOTP_CTRL_RSVD0_SHIFT (6U)
#define | OCOTP_CTRL_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_RSVD0_SHIFT)) & OCOTP_CTRL_RSVD0_MASK)
#define | OCOTP_CTRL_BUSY_MASK (0x100U)
#define | OCOTP_CTRL_BUSY_SHIFT (8U)
#define | OCOTP_CTRL_BUSY(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_BUSY_SHIFT)) & OCOTP_CTRL_BUSY_MASK)
#define | OCOTP_CTRL_ERROR_MASK (0x200U)
#define | OCOTP_CTRL_ERROR_SHIFT (9U)
#define | OCOTP_CTRL_ERROR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_ERROR_SHIFT)) & OCOTP_CTRL_ERROR_MASK)
#define | OCOTP_CTRL_RELOAD_SHADOWS_MASK (0x400U)
#define | OCOTP_CTRL_RELOAD_SHADOWS_SHIFT (10U)
#define | OCOTP_CTRL_RELOAD_SHADOWS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_RELOAD_SHADOWS_MASK)
#define | OCOTP_CTRL_CRC_TEST_MASK (0x800U)
#define | OCOTP_CTRL_CRC_TEST_SHIFT (11U)
#define | OCOTP_CTRL_CRC_TEST(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CRC_TEST_SHIFT)) & OCOTP_CTRL_CRC_TEST_MASK)
#define | OCOTP_CTRL_CRC_FAIL_MASK (0x1000U)
#define | OCOTP_CTRL_CRC_FAIL_SHIFT (12U)
#define | OCOTP_CTRL_CRC_FAIL(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CRC_FAIL_SHIFT)) & OCOTP_CTRL_CRC_FAIL_MASK)
#define | OCOTP_CTRL_RSVD1_MASK (0xE000U)
#define | OCOTP_CTRL_RSVD1_SHIFT (13U)
#define | OCOTP_CTRL_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_RSVD1_SHIFT)) & OCOTP_CTRL_RSVD1_MASK)
#define | OCOTP_CTRL_WR_UNLOCK_MASK (0xFFFF0000U)
#define | OCOTP_CTRL_WR_UNLOCK_SHIFT (16U)
#define | OCOTP_CTRL_WR_UNLOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_WR_UNLOCK_MASK)

## CTRL_SET - OTP Controller Control Register

#define | OCOTP_CTRL_SET_ADDR_MASK (0x3FU)
#define | OCOTP_CTRL_SET_ADDR_SHIFT (0U)
#define | OCOTP_CTRL_SET_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_ADDR_SHIFT)) & OCOTP_CTRL_SET_ADDR_MASK)
#define | OCOTP_CTRL_SET_RSVD0_MASK (0xC0U)
#define | OCOTP_CTRL_SET_RSVD0_SHIFT (6U)
#define | OCOTP_CTRL_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_RSVD0_SHIFT)) & OCOTP_CTRL_SET_RSVD0_MASK)
#define | OCOTP_CTRL_SET_BUSY_MASK (0x100U)
#define | OCOTP_CTRL_SET_BUSY_SHIFT (8U)
#define | OCOTP_CTRL_SET_BUSY(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_BUSY_SHIFT)) & OCOTP_CTRL_SET_BUSY_MASK)
#define | OCOTP_CTRL_SET_ERROR_MASK (0x200U)
#define | OCOTP_CTRL_SET_ERROR_SHIFT (9U)
#define | OCOTP_CTRL_SET_ERROR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_ERROR_SHIFT)) & OCOTP_CTRL_SET_ERROR_MASK)
#define | OCOTP_CTRL_SET_RELOAD_SHADOWS_MASK (0x400U)
#define | OCOTP_CTRL_SET_RELOAD_SHADOWS_SHIFT (10U)
#define | OCOTP_CTRL_SET_RELOAD_SHADOWS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_SET_RELOAD_SHADOWS_MASK)
#define | OCOTP_CTRL_SET_CRC_TEST_MASK (0x800U)
#define | OCOTP_CTRL_SET_CRC_TEST_SHIFT (11U)
#define | OCOTP_CTRL_SET_CRC_TEST(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_CRC_TEST_SHIFT)) & OCOTP_CTRL_SET_CRC_TEST_MASK)
#define | OCOTP_CTRL_SET_CRC_FAIL_MASK (0x1000U)
#define | OCOTP_CTRL_SET_CRC_FAIL_SHIFT (12U)
#define | OCOTP_CTRL_SET_CRC_FAIL(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_CRC_FAIL_SHIFT)) & OCOTP_CTRL_SET_CRC_FAIL_MASK)
#define | OCOTP_CTRL_SET_RSVD1_MASK (0xE000U)
#define | OCOTP_CTRL_SET_RSVD1_SHIFT (13U)
#define | OCOTP_CTRL_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_RSVD1_SHIFT)) & OCOTP_CTRL_SET_RSVD1_MASK)
#define | OCOTP_CTRL_SET_WR_UNLOCK_MASK (0xFFFF0000U)
#define | OCOTP_CTRL_SET_WR_UNLOCK_SHIFT (16U)
#define | OCOTP_CTRL_SET_WR_UNLOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_SET_WR_UNLOCK_MASK)

## CTRL_CLR - OTP Controller Control Register

#define | OCOTP_CTRL_CLR_ADDR_MASK (0x3FU)
#define | OCOTP_CTRL_CLR_ADDR_SHIFT (0U)
#define | OCOTP_CTRL_CLR_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_ADDR_SHIFT)) & OCOTP_CTRL_CLR_ADDR_MASK)
#define | OCOTP_CTRL_CLR_RSVD0_MASK (0xC0U)
#define | OCOTP_CTRL_CLR_RSVD0_SHIFT (6U)
#define | OCOTP_CTRL_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_RSVD0_SHIFT)) & OCOTP_CTRL_CLR_RSVD0_MASK)
#define | OCOTP_CTRL_CLR_BUSY_MASK (0x100U)
#define | OCOTP_CTRL_CLR_BUSY_SHIFT (8U)
#define | OCOTP_CTRL_CLR_BUSY(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_BUSY_SHIFT)) & OCOTP_CTRL_CLR_BUSY_MASK)
#define | OCOTP_CTRL_CLR_ERROR_MASK (0x200U)
#define | OCOTP_CTRL_CLR_ERROR_SHIFT (9U)
#define | OCOTP_CTRL_CLR_ERROR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_ERROR_SHIFT)) & OCOTP_CTRL_CLR_ERROR_MASK)
#define | OCOTP_CTRL_CLR_RELOAD_SHADOWS_MASK (0x400U)
#define | OCOTP_CTRL_CLR_RELOAD_SHADOWS_SHIFT (10U)
#define | OCOTP_CTRL_CLR_RELOAD_SHADOWS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_CLR_RELOAD_SHADOWS_MASK)
#define | OCOTP_CTRL_CLR_CRC_TEST_MASK (0x800U)
#define | OCOTP_CTRL_CLR_CRC_TEST_SHIFT (11U)
#define | OCOTP_CTRL_CLR_CRC_TEST(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_CRC_TEST_SHIFT)) & OCOTP_CTRL_CLR_CRC_TEST_MASK)
#define | OCOTP_CTRL_CLR_CRC_FAIL_MASK (0x1000U)
#define | OCOTP_CTRL_CLR_CRC_FAIL_SHIFT (12U)
#define | OCOTP_CTRL_CLR_CRC_FAIL(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_CRC_FAIL_SHIFT)) & OCOTP_CTRL_CLR_CRC_FAIL_MASK)
#define | OCOTP_CTRL_CLR_RSVD1_MASK (0xE000U)
#define | OCOTP_CTRL_CLR_RSVD1_SHIFT (13U)
#define | OCOTP_CTRL_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_RSVD1_SHIFT)) & OCOTP_CTRL_CLR_RSVD1_MASK)
#define | OCOTP_CTRL_CLR_WR_UNLOCK_MASK (0xFFFF0000U)
#define | OCOTP_CTRL_CLR_WR_UNLOCK_SHIFT (16U)
#define | OCOTP_CTRL_CLR_WR_UNLOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_CLR_WR_UNLOCK_MASK)

## CTRL_TOG - OTP Controller Control Register

#define | OCOTP_CTRL_TOG_ADDR_MASK (0x3FU)
#define | OCOTP_CTRL_TOG_ADDR_SHIFT (0U)
#define | OCOTP_CTRL_TOG_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_ADDR_SHIFT)) & OCOTP_CTRL_TOG_ADDR_MASK)
#define | OCOTP_CTRL_TOG_RSVD0_MASK (0xC0U)
#define | OCOTP_CTRL_TOG_RSVD0_SHIFT (6U)
#define | OCOTP_CTRL_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_RSVD0_SHIFT)) & OCOTP_CTRL_TOG_RSVD0_MASK)
#define | OCOTP_CTRL_TOG_BUSY_MASK (0x100U)
#define | OCOTP_CTRL_TOG_BUSY_SHIFT (8U)
#define | OCOTP_CTRL_TOG_BUSY(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_BUSY_SHIFT)) & OCOTP_CTRL_TOG_BUSY_MASK)
#define | OCOTP_CTRL_TOG_ERROR_MASK (0x200U)
#define | OCOTP_CTRL_TOG_ERROR_SHIFT (9U)
#define | OCOTP_CTRL_TOG_ERROR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_ERROR_SHIFT)) & OCOTP_CTRL_TOG_ERROR_MASK)
#define | OCOTP_CTRL_TOG_RELOAD_SHADOWS_MASK (0x400U)
#define | OCOTP_CTRL_TOG_RELOAD_SHADOWS_SHIFT (10U)
#define | OCOTP_CTRL_TOG_RELOAD_SHADOWS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_TOG_RELOAD_SHADOWS_MASK)
#define | OCOTP_CTRL_TOG_CRC_TEST_MASK (0x800U)
#define | OCOTP_CTRL_TOG_CRC_TEST_SHIFT (11U)
#define | OCOTP_CTRL_TOG_CRC_TEST(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_CRC_TEST_SHIFT)) & OCOTP_CTRL_TOG_CRC_TEST_MASK)
#define | OCOTP_CTRL_TOG_CRC_FAIL_MASK (0x1000U)
#define | OCOTP_CTRL_TOG_CRC_FAIL_SHIFT (12U)
#define | OCOTP_CTRL_TOG_CRC_FAIL(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_CRC_FAIL_SHIFT)) & OCOTP_CTRL_TOG_CRC_FAIL_MASK)
#define | OCOTP_CTRL_TOG_RSVD1_MASK (0xE000U)
#define | OCOTP_CTRL_TOG_RSVD1_SHIFT (13U)
#define | OCOTP_CTRL_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_RSVD1_SHIFT)) & OCOTP_CTRL_TOG_RSVD1_MASK)
#define | OCOTP_CTRL_TOG_WR_UNLOCK_MASK (0xFFFF0000U)
#define | OCOTP_CTRL_TOG_WR_UNLOCK_SHIFT (16U)
#define | OCOTP_CTRL_TOG_WR_UNLOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_TOG_WR_UNLOCK_MASK)

## TIMING - OTP Controller Timing Register

#define | OCOTP_TIMING_STROBE_PROG_MASK (0xFFFU)
#define | OCOTP_TIMING_STROBE_PROG_SHIFT (0U)
#define | OCOTP_TIMING_STROBE_PROG(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_STROBE_PROG_SHIFT)) & OCOTP_TIMING_STROBE_PROG_MASK)
#define | OCOTP_TIMING_RELAX_MASK (0xF000U)
#define | OCOTP_TIMING_RELAX_SHIFT (12U)
#define | OCOTP_TIMING_RELAX(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_RELAX_SHIFT)) & OCOTP_TIMING_RELAX_MASK)
#define | OCOTP_TIMING_STROBE_READ_MASK (0x3F0000U)
#define | OCOTP_TIMING_STROBE_READ_SHIFT (16U)
#define | OCOTP_TIMING_STROBE_READ(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_STROBE_READ_SHIFT)) & OCOTP_TIMING_STROBE_READ_MASK)
#define | OCOTP_TIMING_WAIT_MASK (0xFC00000U)
#define | OCOTP_TIMING_WAIT_SHIFT (22U)
#define | OCOTP_TIMING_WAIT(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_WAIT_SHIFT)) & OCOTP_TIMING_WAIT_MASK)
#define | OCOTP_TIMING_RSRVD0_MASK (0xF0000000U)
#define | OCOTP_TIMING_RSRVD0_SHIFT (28U)
#define | OCOTP_TIMING_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_RSRVD0_SHIFT)) & OCOTP_TIMING_RSRVD0_MASK)

## DATA - OTP Controller Write Data Register

#define | OCOTP_DATA_DATA_MASK (0xFFFFFFFFU)
#define | OCOTP_DATA_DATA_SHIFT (0U)
#define | OCOTP_DATA_DATA(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_DATA_DATA_SHIFT)) & OCOTP_DATA_DATA_MASK)

## READ_CTRL - OTP Controller Write Data Register

#define | OCOTP_READ_CTRL_READ_FUSE_MASK (0x1U)
#define | OCOTP_READ_CTRL_READ_FUSE_SHIFT (0U)
#define | OCOTP_READ_CTRL_READ_FUSE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_READ_CTRL_READ_FUSE_SHIFT)) & OCOTP_READ_CTRL_READ_FUSE_MASK)
#define | OCOTP_READ_CTRL_RSVD0_MASK (0xFFFFFFFEU)
#define | OCOTP_READ_CTRL_RSVD0_SHIFT (1U)
#define | OCOTP_READ_CTRL_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_READ_CTRL_RSVD0_SHIFT)) & OCOTP_READ_CTRL_RSVD0_MASK)

## READ_FUSE_DATA - OTP Controller Read Data Register

#define | OCOTP_READ_FUSE_DATA_DATA_MASK (0xFFFFFFFFU)
#define | OCOTP_READ_FUSE_DATA_DATA_SHIFT (0U)
#define | OCOTP_READ_FUSE_DATA_DATA(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_READ_FUSE_DATA_DATA_SHIFT)) & OCOTP_READ_FUSE_DATA_DATA_MASK)

## SW_STICKY - Sticky bit Register

#define | OCOTP_SW_STICKY_BLOCK_DTCP_KEY_MASK (0x1U)
#define | OCOTP_SW_STICKY_BLOCK_DTCP_KEY_SHIFT (0U)
#define | OCOTP_SW_STICKY_BLOCK_DTCP_KEY(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_BLOCK_DTCP_KEY_SHIFT)) & OCOTP_SW_STICKY_BLOCK_DTCP_KEY_MASK)
#define | OCOTP_SW_STICKY_SRK_REVOKE_LOCK_MASK (0x2U)
#define | OCOTP_SW_STICKY_SRK_REVOKE_LOCK_SHIFT (1U)
#define | OCOTP_SW_STICKY_SRK_REVOKE_LOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_SRK_REVOKE_LOCK_SHIFT)) & OCOTP_SW_STICKY_SRK_REVOKE_LOCK_MASK)
#define | OCOTP_SW_STICKY_FIELD_RETURN_LOCK_MASK (0x4U)
#define | OCOTP_SW_STICKY_FIELD_RETURN_LOCK_SHIFT (2U)
#define | OCOTP_SW_STICKY_FIELD_RETURN_LOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_FIELD_RETURN_LOCK_SHIFT)) & OCOTP_SW_STICKY_FIELD_RETURN_LOCK_MASK)
#define | OCOTP_SW_STICKY_BLOCK_ROM_PART_MASK (0x8U)
#define | OCOTP_SW_STICKY_BLOCK_ROM_PART_SHIFT (3U)
#define | OCOTP_SW_STICKY_BLOCK_ROM_PART(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_BLOCK_ROM_PART_SHIFT)) & OCOTP_SW_STICKY_BLOCK_ROM_PART_MASK)
#define | OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_MASK (0x10U)
#define | OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_SHIFT (4U)
#define | OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_SHIFT)) & OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_MASK)
#define | OCOTP_SW_STICKY_RSVD0_MASK (0xFFFFFFE0U)
#define | OCOTP_SW_STICKY_RSVD0_SHIFT (5U)
#define | OCOTP_SW_STICKY_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_RSVD0_SHIFT)) & OCOTP_SW_STICKY_RSVD0_MASK)

## SCS - Software Controllable Signals Register

#define | OCOTP_SCS_HAB_JDE_MASK (0x1U)
#define | OCOTP_SCS_HAB_JDE_SHIFT (0U)
#define | OCOTP_SCS_HAB_JDE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_HAB_JDE_SHIFT)) & OCOTP_SCS_HAB_JDE_MASK)
#define | OCOTP_SCS_SPARE_MASK (0x7FFFFFFEU)
#define | OCOTP_SCS_SPARE_SHIFT (1U)
#define | OCOTP_SCS_SPARE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SPARE_SHIFT)) & OCOTP_SCS_SPARE_MASK)
#define | OCOTP_SCS_LOCK_MASK (0x80000000U)
#define | OCOTP_SCS_LOCK_SHIFT (31U)
#define | OCOTP_SCS_LOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_LOCK_SHIFT)) & OCOTP_SCS_LOCK_MASK)

## SCS_SET - Software Controllable Signals Register

#define | OCOTP_SCS_SET_HAB_JDE_MASK (0x1U)
#define | OCOTP_SCS_SET_HAB_JDE_SHIFT (0U)
#define | OCOTP_SCS_SET_HAB_JDE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SET_HAB_JDE_SHIFT)) & OCOTP_SCS_SET_HAB_JDE_MASK)
#define | OCOTP_SCS_SET_SPARE_MASK (0x7FFFFFFEU)
#define | OCOTP_SCS_SET_SPARE_SHIFT (1U)
#define | OCOTP_SCS_SET_SPARE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SET_SPARE_SHIFT)) & OCOTP_SCS_SET_SPARE_MASK)
#define | OCOTP_SCS_SET_LOCK_MASK (0x80000000U)
#define | OCOTP_SCS_SET_LOCK_SHIFT (31U)
#define | OCOTP_SCS_SET_LOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SET_LOCK_SHIFT)) & OCOTP_SCS_SET_LOCK_MASK)

## SCS_CLR - Software Controllable Signals Register

#define | OCOTP_SCS_CLR_HAB_JDE_MASK (0x1U)
#define | OCOTP_SCS_CLR_HAB_JDE_SHIFT (0U)
#define | OCOTP_SCS_CLR_HAB_JDE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_CLR_HAB_JDE_SHIFT)) & OCOTP_SCS_CLR_HAB_JDE_MASK)
#define | OCOTP_SCS_CLR_SPARE_MASK (0x7FFFFFFEU)
#define | OCOTP_SCS_CLR_SPARE_SHIFT (1U)
#define | OCOTP_SCS_CLR_SPARE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_CLR_SPARE_SHIFT)) & OCOTP_SCS_CLR_SPARE_MASK)
#define | OCOTP_SCS_CLR_LOCK_MASK (0x80000000U)
#define | OCOTP_SCS_CLR_LOCK_SHIFT (31U)
#define | OCOTP_SCS_CLR_LOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_CLR_LOCK_SHIFT)) & OCOTP_SCS_CLR_LOCK_MASK)

## SCS_TOG - Software Controllable Signals Register

#define | OCOTP_SCS_TOG_HAB_JDE_MASK (0x1U)
#define | OCOTP_SCS_TOG_HAB_JDE_SHIFT (0U)
#define | OCOTP_SCS_TOG_HAB_JDE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_TOG_HAB_JDE_SHIFT)) & OCOTP_SCS_TOG_HAB_JDE_MASK)
#define | OCOTP_SCS_TOG_SPARE_MASK (0x7FFFFFFEU)
#define | OCOTP_SCS_TOG_SPARE_SHIFT (1U)
#define | OCOTP_SCS_TOG_SPARE(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_TOG_SPARE_SHIFT)) & OCOTP_SCS_TOG_SPARE_MASK)
#define | OCOTP_SCS_TOG_LOCK_MASK (0x80000000U)
#define | OCOTP_SCS_TOG_LOCK_SHIFT (31U)
#define | OCOTP_SCS_TOG_LOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_TOG_LOCK_SHIFT)) & OCOTP_SCS_TOG_LOCK_MASK)

## CRC_ADDR - OTP Controller CRC test address

#define | OCOTP_CRC_ADDR_DATA_START_ADDR_MASK (0xFFU)
#define | OCOTP_CRC_ADDR_DATA_START_ADDR_SHIFT (0U)
#define | OCOTP_CRC_ADDR_DATA_START_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_DATA_START_ADDR_SHIFT)) & OCOTP_CRC_ADDR_DATA_START_ADDR_MASK)
#define | OCOTP_CRC_ADDR_DATA_END_ADDR_MASK (0xFF00U)
#define | OCOTP_CRC_ADDR_DATA_END_ADDR_SHIFT (8U)
#define | OCOTP_CRC_ADDR_DATA_END_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_DATA_END_ADDR_SHIFT)) & OCOTP_CRC_ADDR_DATA_END_ADDR_MASK)
#define | OCOTP_CRC_ADDR_CRC_ADDR_MASK (0xFF0000U)
#define | OCOTP_CRC_ADDR_CRC_ADDR_SHIFT (16U)
#define | OCOTP_CRC_ADDR_CRC_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_CRC_ADDR_SHIFT)) & OCOTP_CRC_ADDR_CRC_ADDR_MASK)
#define | OCOTP_CRC_ADDR_OTPMK_CRC_MASK (0x1000000U)
#define | OCOTP_CRC_ADDR_OTPMK_CRC_SHIFT (24U)
#define | OCOTP_CRC_ADDR_OTPMK_CRC(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_OTPMK_CRC_SHIFT)) & OCOTP_CRC_ADDR_OTPMK_CRC_MASK)
#define | OCOTP_CRC_ADDR_RSVD0_MASK (0xFE000000U)
#define | OCOTP_CRC_ADDR_RSVD0_SHIFT (25U)
#define | OCOTP_CRC_ADDR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_RSVD0_SHIFT)) & OCOTP_CRC_ADDR_RSVD0_MASK)

## CRC_VALUE - OTP Controller CRC Value Register

#define | OCOTP_CRC_VALUE_DATA_MASK (0xFFFFFFFFU)
#define | OCOTP_CRC_VALUE_DATA_SHIFT (0U)
#define | OCOTP_CRC_VALUE_DATA(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_VALUE_DATA_SHIFT)) & OCOTP_CRC_VALUE_DATA_MASK)

## VERSION - OTP Controller Version Register

#define | OCOTP_VERSION_STEP_MASK (0xFFFFU)
#define | OCOTP_VERSION_STEP_SHIFT (0U)
#define | OCOTP_VERSION_STEP(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_VERSION_STEP_SHIFT)) & OCOTP_VERSION_STEP_MASK)
#define | OCOTP_VERSION_MINOR_MASK (0xFF0000U)
#define | OCOTP_VERSION_MINOR_SHIFT (16U)
#define | OCOTP_VERSION_MINOR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_VERSION_MINOR_SHIFT)) & OCOTP_VERSION_MINOR_MASK)
#define | OCOTP_VERSION_MAJOR_MASK (0xFF000000U)
#define | OCOTP_VERSION_MAJOR_SHIFT (24U)
#define | OCOTP_VERSION_MAJOR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_VERSION_MAJOR_SHIFT)) & OCOTP_VERSION_MAJOR_MASK)

## TIMING2 - OTP Controller Timing Register

#define | OCOTP_TIMING2_RELAX_PROG_MASK (0xFFFU)
#define | OCOTP_TIMING2_RELAX_PROG_SHIFT (0U)
#define | OCOTP_TIMING2_RELAX_PROG(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RELAX_PROG_SHIFT)) & OCOTP_TIMING2_RELAX_PROG_MASK)
#define | OCOTP_TIMING2_RSRVD0_MASK (0xF000U)
#define | OCOTP_TIMING2_RSRVD0_SHIFT (12U)
#define | OCOTP_TIMING2_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RSRVD0_SHIFT)) & OCOTP_TIMING2_RSRVD0_MASK)
#define | OCOTP_TIMING2_RELAX_READ_MASK (0x3F0000U)
#define | OCOTP_TIMING2_RELAX_READ_SHIFT (16U)
#define | OCOTP_TIMING2_RELAX_READ(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RELAX_READ_SHIFT)) & OCOTP_TIMING2_RELAX_READ_MASK)
#define | OCOTP_TIMING2_RSRVD1_MASK (0xFFC00000U)
#define | OCOTP_TIMING2_RSRVD1_SHIFT (22U)
#define | OCOTP_TIMING2_RSRVD1(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RSRVD1_SHIFT)) & OCOTP_TIMING2_RSRVD1_MASK)

## LOCK - Value of OTP Bank0 Word0 (Lock controls)

#define | OCOTP_LOCK_TESTER_MASK (0x3U)
#define | OCOTP_LOCK_TESTER_SHIFT (0U)
#define | OCOTP_LOCK_TESTER(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_TESTER_SHIFT)) & OCOTP_LOCK_TESTER_MASK)
#define | OCOTP_LOCK_BOOT_CFG_MASK (0xCU)
#define | OCOTP_LOCK_BOOT_CFG_SHIFT (2U)
#define | OCOTP_LOCK_BOOT_CFG(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_BOOT_CFG_SHIFT)) & OCOTP_LOCK_BOOT_CFG_MASK)
#define | OCOTP_LOCK_MEM_TRIM_MASK (0x30U)
#define | OCOTP_LOCK_MEM_TRIM_SHIFT (4U)
#define | OCOTP_LOCK_MEM_TRIM(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_MEM_TRIM_SHIFT)) & OCOTP_LOCK_MEM_TRIM_MASK)
#define | OCOTP_LOCK_SJC_RESP_MASK (0x40U)
#define | OCOTP_LOCK_SJC_RESP_SHIFT (6U)
#define | OCOTP_LOCK_SJC_RESP(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SJC_RESP_SHIFT)) & OCOTP_LOCK_SJC_RESP_MASK)
#define | OCOTP_LOCK_GP4_RLOCK_MASK (0x80U)
#define | OCOTP_LOCK_GP4_RLOCK_SHIFT (7U)
#define | OCOTP_LOCK_GP4_RLOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP4_RLOCK_SHIFT)) & OCOTP_LOCK_GP4_RLOCK_MASK)
#define | OCOTP_LOCK_MAC_ADDR_MASK (0x300U)
#define | OCOTP_LOCK_MAC_ADDR_SHIFT (8U)
#define | OCOTP_LOCK_MAC_ADDR(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_MAC_ADDR_SHIFT)) & OCOTP_LOCK_MAC_ADDR_MASK)
#define | OCOTP_LOCK_GP1_MASK (0xC00U)
#define | OCOTP_LOCK_GP1_SHIFT (10U)
#define | OCOTP_LOCK_GP1(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP1_SHIFT)) & OCOTP_LOCK_GP1_MASK)
#define | OCOTP_LOCK_GP2_MASK (0x3000U)
#define | OCOTP_LOCK_GP2_SHIFT (12U)
#define | OCOTP_LOCK_GP2(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP2_SHIFT)) & OCOTP_LOCK_GP2_MASK)
#define | OCOTP_LOCK_ROM_PATCH_MASK (0x8000U)
#define | OCOTP_LOCK_ROM_PATCH_SHIFT (15U)
#define | OCOTP_LOCK_ROM_PATCH(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_ROM_PATCH_SHIFT)) & OCOTP_LOCK_ROM_PATCH_MASK)
#define | OCOTP_LOCK_SW_GP1_MASK (0x10000U)
#define | OCOTP_LOCK_SW_GP1_SHIFT (16U)
#define | OCOTP_LOCK_SW_GP1(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SW_GP1_SHIFT)) & OCOTP_LOCK_SW_GP1_MASK)
#define | OCOTP_LOCK_OTPMK_MASK (0x20000U)
#define | OCOTP_LOCK_OTPMK_SHIFT (17U)
#define | OCOTP_LOCK_OTPMK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_OTPMK_SHIFT)) & OCOTP_LOCK_OTPMK_MASK)
#define | OCOTP_LOCK_ANALOG_MASK (0xC0000U)
#define | OCOTP_LOCK_ANALOG_SHIFT (18U)
#define | OCOTP_LOCK_ANALOG(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_ANALOG_SHIFT)) & OCOTP_LOCK_ANALOG_MASK)
#define | OCOTP_LOCK_OTPMK_CRC_MASK (0x100000U)
#define | OCOTP_LOCK_OTPMK_CRC_SHIFT (20U)
#define | OCOTP_LOCK_OTPMK_CRC(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_OTPMK_CRC_SHIFT)) & OCOTP_LOCK_OTPMK_CRC_MASK)
#define | OCOTP_LOCK_SW_GP2_LOCK_MASK (0x200000U)
#define | OCOTP_LOCK_SW_GP2_LOCK_SHIFT (21U)
#define | OCOTP_LOCK_SW_GP2_LOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SW_GP2_LOCK_SHIFT)) & OCOTP_LOCK_SW_GP2_LOCK_MASK)
#define | OCOTP_LOCK_MISC_CONF_MASK (0x400000U)
#define | OCOTP_LOCK_MISC_CONF_SHIFT (22U)
#define | OCOTP_LOCK_MISC_CONF(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_MISC_CONF_SHIFT)) & OCOTP_LOCK_MISC_CONF_MASK)
#define | OCOTP_LOCK_SW_GP2_RLOCK_MASK (0x800000U)
#define | OCOTP_LOCK_SW_GP2_RLOCK_SHIFT (23U)
#define | OCOTP_LOCK_SW_GP2_RLOCK(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SW_GP2_RLOCK_SHIFT)) & OCOTP_LOCK_SW_GP2_RLOCK_MASK)
#define | OCOTP_LOCK_GP4_MASK (0x3000000U)
#define | OCOTP_LOCK_GP4_SHIFT (24U)
#define | OCOTP_LOCK_GP4(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP4_SHIFT)) & OCOTP_LOCK_GP4_MASK)
#define | OCOTP_LOCK_GP3_MASK (0xC000000U)
#define | OCOTP_LOCK_GP3_SHIFT (26U)
#define | OCOTP_LOCK_GP3(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP3_SHIFT)) & OCOTP_LOCK_GP3_MASK)
#define | OCOTP_LOCK_FIELD_RETURN_MASK (0xF0000000U)
#define | OCOTP_LOCK_FIELD_RETURN_SHIFT (28U)
#define | OCOTP_LOCK_FIELD_RETURN(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_FIELD_RETURN_SHIFT)) & OCOTP_LOCK_FIELD_RETURN_MASK)

## CFG0 - Value of OTP Bank0 Word1 (Configuration and Manufacturing Info.)

#define | OCOTP_CFG0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_CFG0_BITS_SHIFT (0U)
#define | OCOTP_CFG0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG0_BITS_SHIFT)) & OCOTP_CFG0_BITS_MASK)

## CFG1 - Value of OTP Bank0 Word2 (Configuration and Manufacturing Info.)

#define | OCOTP_CFG1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_CFG1_BITS_SHIFT (0U)
#define | OCOTP_CFG1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG1_BITS_SHIFT)) & OCOTP_CFG1_BITS_MASK)

## CFG2 - Value of OTP Bank0 Word3 (Configuration and Manufacturing Info.)

#define | OCOTP_CFG2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_CFG2_BITS_SHIFT (0U)
#define | OCOTP_CFG2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG2_BITS_SHIFT)) & OCOTP_CFG2_BITS_MASK)

## CFG3 - Value of OTP Bank0 Word4 (Configuration and Manufacturing Info.)

#define | OCOTP_CFG3_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_CFG3_BITS_SHIFT (0U)
#define | OCOTP_CFG3_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG3_BITS_SHIFT)) & OCOTP_CFG3_BITS_MASK)

## CFG4 - Value of OTP Bank0 Word5 (Configuration and Manufacturing Info.)

#define | OCOTP_CFG4_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_CFG4_BITS_SHIFT (0U)
#define | OCOTP_CFG4_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG4_BITS_SHIFT)) & OCOTP_CFG4_BITS_MASK)

## CFG5 - Value of OTP Bank0 Word6 (Configuration and Manufacturing Info.)

#define | OCOTP_CFG5_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_CFG5_BITS_SHIFT (0U)
#define | OCOTP_CFG5_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG5_BITS_SHIFT)) & OCOTP_CFG5_BITS_MASK)

## CFG6 - Value of OTP Bank0 Word7 (Configuration and Manufacturing Info.)

#define | OCOTP_CFG6_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_CFG6_BITS_SHIFT (0U)
#define | OCOTP_CFG6_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG6_BITS_SHIFT)) & OCOTP_CFG6_BITS_MASK)

## MEM0 - Value of OTP Bank1 Word0 (Memory Related Info.)

#define | OCOTP_MEM0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MEM0_BITS_SHIFT (0U)
#define | OCOTP_MEM0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM0_BITS_SHIFT)) & OCOTP_MEM0_BITS_MASK)

## MEM1 - Value of OTP Bank1 Word1 (Memory Related Info.)

#define | OCOTP_MEM1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MEM1_BITS_SHIFT (0U)
#define | OCOTP_MEM1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM1_BITS_SHIFT)) & OCOTP_MEM1_BITS_MASK)

## MEM2 - Value of OTP Bank1 Word2 (Memory Related Info.)

#define | OCOTP_MEM2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MEM2_BITS_SHIFT (0U)
#define | OCOTP_MEM2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM2_BITS_SHIFT)) & OCOTP_MEM2_BITS_MASK)

## MEM3 - Value of OTP Bank1 Word3 (Memory Related Info.)

#define | OCOTP_MEM3_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MEM3_BITS_SHIFT (0U)
#define | OCOTP_MEM3_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM3_BITS_SHIFT)) & OCOTP_MEM3_BITS_MASK)

## MEM4 - Value of OTP Bank1 Word4 (Memory Related Info.)

#define | OCOTP_MEM4_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MEM4_BITS_SHIFT (0U)
#define | OCOTP_MEM4_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM4_BITS_SHIFT)) & OCOTP_MEM4_BITS_MASK)

## ANA0 - Value of OTP Bank1 Word5 (Memory Related Info.)

#define | OCOTP_ANA0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ANA0_BITS_SHIFT (0U)
#define | OCOTP_ANA0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ANA0_BITS_SHIFT)) & OCOTP_ANA0_BITS_MASK)

## ANA1 - Value of OTP Bank1 Word6 (General Purpose Customer Defined Info.)

#define | OCOTP_ANA1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ANA1_BITS_SHIFT (0U)
#define | OCOTP_ANA1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ANA1_BITS_SHIFT)) & OCOTP_ANA1_BITS_MASK)

## ANA2 - Value of OTP Bank1 Word7 (General Purpose Customer Defined Info.)

#define | OCOTP_ANA2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ANA2_BITS_SHIFT (0U)
#define | OCOTP_ANA2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ANA2_BITS_SHIFT)) & OCOTP_ANA2_BITS_MASK)

## OTPMK0 - Value of OTP Bank2 Word0 (OTPMK Key)

#define | OCOTP_OTPMK0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK0_BITS_SHIFT (0U)
#define | OCOTP_OTPMK0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK0_BITS_SHIFT)) & OCOTP_OTPMK0_BITS_MASK)

## OTPMK1 - Value of OTP Bank2 Word1 (OTPMK Key)

#define | OCOTP_OTPMK1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK1_BITS_SHIFT (0U)
#define | OCOTP_OTPMK1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK1_BITS_SHIFT)) & OCOTP_OTPMK1_BITS_MASK)

## OTPMK2 - Value of OTP Bank2 Word2 (OTPMK Key)

#define | OCOTP_OTPMK2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK2_BITS_SHIFT (0U)
#define | OCOTP_OTPMK2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK2_BITS_SHIFT)) & OCOTP_OTPMK2_BITS_MASK)

## OTPMK3 - Value of OTP Bank2 Word3 (OTPMK Key)

#define | OCOTP_OTPMK3_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK3_BITS_SHIFT (0U)
#define | OCOTP_OTPMK3_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK3_BITS_SHIFT)) & OCOTP_OTPMK3_BITS_MASK)

## OTPMK4 - Value of OTP Bank2 Word4 (OTPMK Key)

#define | OCOTP_OTPMK4_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK4_BITS_SHIFT (0U)
#define | OCOTP_OTPMK4_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK4_BITS_SHIFT)) & OCOTP_OTPMK4_BITS_MASK)

## OTPMK5 - Value of OTP Bank2 Word5 (OTPMK Key)

#define | OCOTP_OTPMK5_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK5_BITS_SHIFT (0U)
#define | OCOTP_OTPMK5_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK5_BITS_SHIFT)) & OCOTP_OTPMK5_BITS_MASK)

## OTPMK6 - Value of OTP Bank2 Word6 (OTPMK Key)

#define | OCOTP_OTPMK6_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK6_BITS_SHIFT (0U)
#define | OCOTP_OTPMK6_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK6_BITS_SHIFT)) & OCOTP_OTPMK6_BITS_MASK)

## OTPMK7 - Value of OTP Bank2 Word7 (OTPMK Key)

#define | OCOTP_OTPMK7_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK7_BITS_SHIFT (0U)
#define | OCOTP_OTPMK7_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK7_BITS_SHIFT)) & OCOTP_OTPMK7_BITS_MASK)

## SRK0 - Shadow Register for OTP Bank3 Word0 (SRK Hash)

#define | OCOTP_SRK0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK0_BITS_SHIFT (0U)
#define | OCOTP_SRK0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK0_BITS_SHIFT)) & OCOTP_SRK0_BITS_MASK)

## SRK1 - Shadow Register for OTP Bank3 Word1 (SRK Hash)

#define | OCOTP_SRK1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK1_BITS_SHIFT (0U)
#define | OCOTP_SRK1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK1_BITS_SHIFT)) & OCOTP_SRK1_BITS_MASK)

## SRK2 - Shadow Register for OTP Bank3 Word2 (SRK Hash)

#define | OCOTP_SRK2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK2_BITS_SHIFT (0U)
#define | OCOTP_SRK2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK2_BITS_SHIFT)) & OCOTP_SRK2_BITS_MASK)

## SRK3 - Shadow Register for OTP Bank3 Word3 (SRK Hash)

#define | OCOTP_SRK3_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK3_BITS_SHIFT (0U)
#define | OCOTP_SRK3_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK3_BITS_SHIFT)) & OCOTP_SRK3_BITS_MASK)

## SRK4 - Shadow Register for OTP Bank3 Word4 (SRK Hash)

#define | OCOTP_SRK4_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK4_BITS_SHIFT (0U)
#define | OCOTP_SRK4_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK4_BITS_SHIFT)) & OCOTP_SRK4_BITS_MASK)

## SRK5 - Shadow Register for OTP Bank3 Word5 (SRK Hash)

#define | OCOTP_SRK5_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK5_BITS_SHIFT (0U)
#define | OCOTP_SRK5_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK5_BITS_SHIFT)) & OCOTP_SRK5_BITS_MASK)

## SRK6 - Shadow Register for OTP Bank3 Word6 (SRK Hash)

#define | OCOTP_SRK6_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK6_BITS_SHIFT (0U)
#define | OCOTP_SRK6_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK6_BITS_SHIFT)) & OCOTP_SRK6_BITS_MASK)

## SRK7 - Shadow Register for OTP Bank3 Word7 (SRK Hash)

#define | OCOTP_SRK7_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK7_BITS_SHIFT (0U)
#define | OCOTP_SRK7_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK7_BITS_SHIFT)) & OCOTP_SRK7_BITS_MASK)

## SJC_RESP0 - Value of OTP Bank4 Word0 (Secure JTAG Response Field)

#define | OCOTP_SJC_RESP0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SJC_RESP0_BITS_SHIFT (0U)
#define | OCOTP_SJC_RESP0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SJC_RESP0_BITS_SHIFT)) & OCOTP_SJC_RESP0_BITS_MASK)

## SJC_RESP1 - Value of OTP Bank4 Word1 (Secure JTAG Response Field)

#define | OCOTP_SJC_RESP1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SJC_RESP1_BITS_SHIFT (0U)
#define | OCOTP_SJC_RESP1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SJC_RESP1_BITS_SHIFT)) & OCOTP_SJC_RESP1_BITS_MASK)

## MAC0 - Value of OTP Bank4 Word2 (MAC Address)

#define | OCOTP_MAC0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MAC0_BITS_SHIFT (0U)
#define | OCOTP_MAC0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MAC0_BITS_SHIFT)) & OCOTP_MAC0_BITS_MASK)

## MAC1 - Value of OTP Bank4 Word3 (MAC Address)

#define | OCOTP_MAC1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MAC1_BITS_SHIFT (0U)
#define | OCOTP_MAC1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MAC1_BITS_SHIFT)) & OCOTP_MAC1_BITS_MASK)

## MAC2 - Value of OTP Bank4 Word4 (MAC2 Address)

#define | OCOTP_MAC2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MAC2_BITS_SHIFT (0U)
#define | OCOTP_MAC2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MAC2_BITS_SHIFT)) & OCOTP_MAC2_BITS_MASK)

## OTPMK_CRC32 - Value of OTP Bank4 Word5 (CRC Key)

#define | OCOTP_OTPMK_CRC32_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_OTPMK_CRC32_BITS_SHIFT (0U)
#define | OCOTP_OTPMK_CRC32_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK_CRC32_BITS_SHIFT)) & OCOTP_OTPMK_CRC32_BITS_MASK)

## GP1 - Value of OTP Bank4 Word6 (General Purpose Customer Defined Info)

#define | OCOTP_GP1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP1_BITS_SHIFT (0U)
#define | OCOTP_GP1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP1_BITS_SHIFT)) & OCOTP_GP1_BITS_MASK)

## GP2 - Value of OTP Bank4 Word7 (General Purpose Customer Defined Info)

#define | OCOTP_GP2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP2_BITS_SHIFT (0U)
#define | OCOTP_GP2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP2_BITS_SHIFT)) & OCOTP_GP2_BITS_MASK)

## SW_GP1 - Value of OTP Bank5 Word0 (SW GP1)

#define | OCOTP_SW_GP1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SW_GP1_BITS_SHIFT (0U)
#define | OCOTP_SW_GP1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP1_BITS_SHIFT)) & OCOTP_SW_GP1_BITS_MASK)

## SW_GP20 - Value of OTP Bank5 Word1 (SW GP2)

#define | OCOTP_SW_GP20_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SW_GP20_BITS_SHIFT (0U)
#define | OCOTP_SW_GP20_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP20_BITS_SHIFT)) & OCOTP_SW_GP20_BITS_MASK)

## SW_GP21 - Value of OTP Bank5 Word2 (SW GP2)

#define | OCOTP_SW_GP21_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SW_GP21_BITS_SHIFT (0U)
#define | OCOTP_SW_GP21_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP21_BITS_SHIFT)) & OCOTP_SW_GP21_BITS_MASK)

## SW_GP22 - Value of OTP Bank5 Word3 (SW GP2)

#define | OCOTP_SW_GP22_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SW_GP22_BITS_SHIFT (0U)
#define | OCOTP_SW_GP22_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP22_BITS_SHIFT)) & OCOTP_SW_GP22_BITS_MASK)

## SW_GP23 - Value of OTP Bank5 Word4 (SW GP2)

#define | OCOTP_SW_GP23_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SW_GP23_BITS_SHIFT (0U)
#define | OCOTP_SW_GP23_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP23_BITS_SHIFT)) & OCOTP_SW_GP23_BITS_MASK)

## MISC_CONF0 - Value of OTP Bank5 Word5 (Misc Conf)

#define | OCOTP_MISC_CONF0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MISC_CONF0_BITS_SHIFT (0U)
#define | OCOTP_MISC_CONF0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MISC_CONF0_BITS_SHIFT)) & OCOTP_MISC_CONF0_BITS_MASK)

## MISC_CONF1 - Value of OTP Bank5 Word6 (Misc Conf)

#define | OCOTP_MISC_CONF1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_MISC_CONF1_BITS_SHIFT (0U)
#define | OCOTP_MISC_CONF1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_MISC_CONF1_BITS_SHIFT)) & OCOTP_MISC_CONF1_BITS_MASK)

## SRK_REVOKE - Value of OTP Bank5 Word7 (SRK Revoke)

#define | OCOTP_SRK_REVOKE_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_SRK_REVOKE_BITS_SHIFT (0U)
#define | OCOTP_SRK_REVOKE_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK_REVOKE_BITS_SHIFT)) & OCOTP_SRK_REVOKE_BITS_MASK)

## ROM_PATCH0 - Value of OTP Bank6 Word0 (ROM Patch)

#define | OCOTP_ROM_PATCH0_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH0_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH0_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH0_BITS_SHIFT)) & OCOTP_ROM_PATCH0_BITS_MASK)

## ROM_PATCH1 - Value of OTP Bank6 Word1 (ROM Patch)

#define | OCOTP_ROM_PATCH1_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH1_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH1_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH1_BITS_SHIFT)) & OCOTP_ROM_PATCH1_BITS_MASK)

## ROM_PATCH2 - Value of OTP Bank6 Word2 (ROM Patch)

#define | OCOTP_ROM_PATCH2_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH2_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH2_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH2_BITS_SHIFT)) & OCOTP_ROM_PATCH2_BITS_MASK)

## ROM_PATCH3 - Value of OTP Bank6 Word3 (ROM Patch)

#define | OCOTP_ROM_PATCH3_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH3_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH3_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH3_BITS_SHIFT)) & OCOTP_ROM_PATCH3_BITS_MASK)

## ROM_PATCH4 - Value of OTP Bank6 Word4 (ROM Patch)

#define | OCOTP_ROM_PATCH4_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH4_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH4_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH4_BITS_SHIFT)) & OCOTP_ROM_PATCH4_BITS_MASK)

## ROM_PATCH5 - Value of OTP Bank6 Word5 (ROM Patch)

#define | OCOTP_ROM_PATCH5_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH5_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH5_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH5_BITS_SHIFT)) & OCOTP_ROM_PATCH5_BITS_MASK)

## ROM_PATCH6 - Value of OTP Bank6 Word6 (ROM Patch)

#define | OCOTP_ROM_PATCH6_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH6_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH6_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH6_BITS_SHIFT)) & OCOTP_ROM_PATCH6_BITS_MASK)

## ROM_PATCH7 - Value of OTP Bank6 Word7 (ROM Patch)

#define | OCOTP_ROM_PATCH7_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_ROM_PATCH7_BITS_SHIFT (0U)
#define | OCOTP_ROM_PATCH7_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH7_BITS_SHIFT)) & OCOTP_ROM_PATCH7_BITS_MASK)

## GP30 - Value of OTP Bank7 Word0 (GP3)

#define | OCOTP_GP30_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP30_BITS_SHIFT (0U)
#define | OCOTP_GP30_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP30_BITS_SHIFT)) & OCOTP_GP30_BITS_MASK)

## GP31 - Value of OTP Bank7 Word1 (GP3)

#define | OCOTP_GP31_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP31_BITS_SHIFT (0U)
#define | OCOTP_GP31_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP31_BITS_SHIFT)) & OCOTP_GP31_BITS_MASK)

## GP32 - Value of OTP Bank7 Word2 (GP3)

#define | OCOTP_GP32_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP32_BITS_SHIFT (0U)
#define | OCOTP_GP32_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP32_BITS_SHIFT)) & OCOTP_GP32_BITS_MASK)

## GP33 - Value of OTP Bank7 Word3 (GP3)

#define | OCOTP_GP33_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP33_BITS_SHIFT (0U)
#define | OCOTP_GP33_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP33_BITS_SHIFT)) & OCOTP_GP33_BITS_MASK)

## GP40 - Value of OTP Bank7 Word4 (GP4)

#define | OCOTP_GP40_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP40_BITS_SHIFT (0U)
#define | OCOTP_GP40_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP40_BITS_SHIFT)) & OCOTP_GP40_BITS_MASK)

## GP41 - Value of OTP Bank7 Word5 (GP4)

#define | OCOTP_GP41_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP41_BITS_SHIFT (0U)
#define | OCOTP_GP41_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP41_BITS_SHIFT)) & OCOTP_GP41_BITS_MASK)

## GP42 - Value of OTP Bank7 Word6 (GP4)

#define | OCOTP_GP42_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP42_BITS_SHIFT (0U)
#define | OCOTP_GP42_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP42_BITS_SHIFT)) & OCOTP_GP42_BITS_MASK)

## GP43 - Value of OTP Bank7 Word7 (GP4)

#define | OCOTP_GP43_BITS_MASK (0xFFFFFFFFU)
#define | OCOTP_GP43_BITS_SHIFT (0U)
#define | OCOTP_GP43_BITS(x) (((uint32_t)(((uint32_t)(x)) << OCOTP_GP43_BITS_SHIFT)) & OCOTP_GP43_BITS_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ OCOTP_ANA0_BITS

#define OCOTP_ANA0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ANA0_BITS_SHIFT)) & OCOTP_ANA0_BITS_MASK)

BITS - BITS

Definition at line 30105 of file MIMXRT1062.h.

## ◆ OCOTP_ANA0_BITS_MASK

#define OCOTP_ANA0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30101 of file MIMXRT1062.h.

## ◆ OCOTP_ANA0_BITS_SHIFT

#define OCOTP_ANA0_BITS_SHIFT (0U)

Definition at line 30102 of file MIMXRT1062.h.

## ◆ OCOTP_ANA1_BITS

#define OCOTP_ANA1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ANA1_BITS_SHIFT)) & OCOTP_ANA1_BITS_MASK)

BITS - BITS

Definition at line 30114 of file MIMXRT1062.h.

## ◆ OCOTP_ANA1_BITS_MASK

#define OCOTP_ANA1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30110 of file MIMXRT1062.h.

## ◆ OCOTP_ANA1_BITS_SHIFT

#define OCOTP_ANA1_BITS_SHIFT (0U)

Definition at line 30111 of file MIMXRT1062.h.

## ◆ OCOTP_ANA2_BITS

#define OCOTP_ANA2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ANA2_BITS_SHIFT)) & OCOTP_ANA2_BITS_MASK)

BITS - BITS

Definition at line 30123 of file MIMXRT1062.h.

## ◆ OCOTP_ANA2_BITS_MASK

#define OCOTP_ANA2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30119 of file MIMXRT1062.h.

## ◆ OCOTP_ANA2_BITS_SHIFT

#define OCOTP_ANA2_BITS_SHIFT (0U)

Definition at line 30120 of file MIMXRT1062.h.

## ◆ OCOTP_CFG0_BITS

#define OCOTP_CFG0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG0_BITS_SHIFT)) & OCOTP_CFG0_BITS_MASK)

BITS - BITS

Definition at line 29997 of file MIMXRT1062.h.

## ◆ OCOTP_CFG0_BITS_MASK

#define OCOTP_CFG0_BITS_MASK (0xFFFFFFFFU)

Definition at line 29993 of file MIMXRT1062.h.

## ◆ OCOTP_CFG0_BITS_SHIFT

#define OCOTP_CFG0_BITS_SHIFT (0U)

Definition at line 29994 of file MIMXRT1062.h.

## ◆ OCOTP_CFG1_BITS

#define OCOTP_CFG1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG1_BITS_SHIFT)) & OCOTP_CFG1_BITS_MASK)

BITS - BITS

Definition at line 30006 of file MIMXRT1062.h.

## ◆ OCOTP_CFG1_BITS_MASK

#define OCOTP_CFG1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30002 of file MIMXRT1062.h.

## ◆ OCOTP_CFG1_BITS_SHIFT

#define OCOTP_CFG1_BITS_SHIFT (0U)

Definition at line 30003 of file MIMXRT1062.h.

## ◆ OCOTP_CFG2_BITS

#define OCOTP_CFG2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG2_BITS_SHIFT)) & OCOTP_CFG2_BITS_MASK)

BITS - BITS

Definition at line 30015 of file MIMXRT1062.h.

## ◆ OCOTP_CFG2_BITS_MASK

#define OCOTP_CFG2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30011 of file MIMXRT1062.h.

## ◆ OCOTP_CFG2_BITS_SHIFT

#define OCOTP_CFG2_BITS_SHIFT (0U)

Definition at line 30012 of file MIMXRT1062.h.

## ◆ OCOTP_CFG3_BITS

#define OCOTP_CFG3_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG3_BITS_SHIFT)) & OCOTP_CFG3_BITS_MASK)

BITS - BITS

Definition at line 30024 of file MIMXRT1062.h.

## ◆ OCOTP_CFG3_BITS_MASK

#define OCOTP_CFG3_BITS_MASK (0xFFFFFFFFU)

Definition at line 30020 of file MIMXRT1062.h.

## ◆ OCOTP_CFG3_BITS_SHIFT

#define OCOTP_CFG3_BITS_SHIFT (0U)

Definition at line 30021 of file MIMXRT1062.h.

## ◆ OCOTP_CFG4_BITS

#define OCOTP_CFG4_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG4_BITS_SHIFT)) & OCOTP_CFG4_BITS_MASK)

BITS - BITS

Definition at line 30033 of file MIMXRT1062.h.

## ◆ OCOTP_CFG4_BITS_MASK

#define OCOTP_CFG4_BITS_MASK (0xFFFFFFFFU)

Definition at line 30029 of file MIMXRT1062.h.

## ◆ OCOTP_CFG4_BITS_SHIFT

#define OCOTP_CFG4_BITS_SHIFT (0U)

Definition at line 30030 of file MIMXRT1062.h.

## ◆ OCOTP_CFG5_BITS

#define OCOTP_CFG5_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG5_BITS_SHIFT)) & OCOTP_CFG5_BITS_MASK)

BITS - BITS

Definition at line 30042 of file MIMXRT1062.h.

## ◆ OCOTP_CFG5_BITS_MASK

#define OCOTP_CFG5_BITS_MASK (0xFFFFFFFFU)

Definition at line 30038 of file MIMXRT1062.h.

## ◆ OCOTP_CFG5_BITS_SHIFT

#define OCOTP_CFG5_BITS_SHIFT (0U)

Definition at line 30039 of file MIMXRT1062.h.

## ◆ OCOTP_CFG6_BITS

#define OCOTP_CFG6_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CFG6_BITS_SHIFT)) & OCOTP_CFG6_BITS_MASK)

BITS - BITS

Definition at line 30051 of file MIMXRT1062.h.

## ◆ OCOTP_CFG6_BITS_MASK

#define OCOTP_CFG6_BITS_MASK (0xFFFFFFFFU)

Definition at line 30047 of file MIMXRT1062.h.

## ◆ OCOTP_CFG6_BITS_SHIFT

#define OCOTP_CFG6_BITS_SHIFT (0U)

Definition at line 30048 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_CRC_ADDR

#define OCOTP_CRC_ADDR_CRC_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_CRC_ADDR_SHIFT)) & OCOTP_CRC_ADDR_CRC_ADDR_MASK)

CRC_ADDR - CRC_ADDR

Definition at line 29827 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_CRC_ADDR_MASK

#define OCOTP_CRC_ADDR_CRC_ADDR_MASK (0xFF0000U)

Definition at line 29823 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_CRC_ADDR_SHIFT

#define OCOTP_CRC_ADDR_CRC_ADDR_SHIFT (16U)

Definition at line 29824 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_DATA_END_ADDR

#define OCOTP_CRC_ADDR_DATA_END_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_DATA_END_ADDR_SHIFT)) & OCOTP_CRC_ADDR_DATA_END_ADDR_MASK)

DATA_END_ADDR - DATA_END_ADDR

Definition at line 29822 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_DATA_END_ADDR_MASK

#define OCOTP_CRC_ADDR_DATA_END_ADDR_MASK (0xFF00U)

Definition at line 29818 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_DATA_END_ADDR_SHIFT

#define OCOTP_CRC_ADDR_DATA_END_ADDR_SHIFT (8U)

Definition at line 29819 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_DATA_START_ADDR

#define OCOTP_CRC_ADDR_DATA_START_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_DATA_START_ADDR_SHIFT)) & OCOTP_CRC_ADDR_DATA_START_ADDR_MASK)

DATA_START_ADDR - DATA_START_ADDR

Definition at line 29817 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_DATA_START_ADDR_MASK

#define OCOTP_CRC_ADDR_DATA_START_ADDR_MASK (0xFFU)

Definition at line 29813 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_DATA_START_ADDR_SHIFT

#define OCOTP_CRC_ADDR_DATA_START_ADDR_SHIFT (0U)

Definition at line 29814 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_OTPMK_CRC

#define OCOTP_CRC_ADDR_OTPMK_CRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_OTPMK_CRC_SHIFT)) & OCOTP_CRC_ADDR_OTPMK_CRC_MASK)

OTPMK_CRC - OTPMK_CRC

Definition at line 29832 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_OTPMK_CRC_MASK

#define OCOTP_CRC_ADDR_OTPMK_CRC_MASK (0x1000000U)

Definition at line 29828 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_OTPMK_CRC_SHIFT

#define OCOTP_CRC_ADDR_OTPMK_CRC_SHIFT (24U)

Definition at line 29829 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_RSVD0

#define OCOTP_CRC_ADDR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_ADDR_RSVD0_SHIFT)) & OCOTP_CRC_ADDR_RSVD0_MASK)

RSVD0 - RSVD0

Definition at line 29837 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_RSVD0_MASK

#define OCOTP_CRC_ADDR_RSVD0_MASK (0xFE000000U)

Definition at line 29833 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_ADDR_RSVD0_SHIFT

#define OCOTP_CRC_ADDR_RSVD0_SHIFT (25U)

Definition at line 29834 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_VALUE_DATA

#define OCOTP_CRC_VALUE_DATA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CRC_VALUE_DATA_SHIFT)) & OCOTP_CRC_VALUE_DATA_MASK)

DATA - DATA

Definition at line 29846 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_VALUE_DATA_MASK

#define OCOTP_CRC_VALUE_DATA_MASK (0xFFFFFFFFU)

Definition at line 29842 of file MIMXRT1062.h.

## ◆ OCOTP_CRC_VALUE_DATA_SHIFT

#define OCOTP_CRC_VALUE_DATA_SHIFT (0U)

Definition at line 29843 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_ADDR

#define OCOTP_CTRL_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_ADDR_SHIFT)) & OCOTP_CTRL_ADDR_MASK)

ADDR - ADDR

Definition at line 29449 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_ADDR_MASK

#define OCOTP_CTRL_ADDR_MASK (0x3FU)

Definition at line 29445 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_ADDR_SHIFT

#define OCOTP_CTRL_ADDR_SHIFT (0U)

Definition at line 29446 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_BUSY

#define OCOTP_CTRL_BUSY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_BUSY_SHIFT)) & OCOTP_CTRL_BUSY_MASK)

BUSY - BUSY

Definition at line 29459 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_BUSY_MASK

#define OCOTP_CTRL_BUSY_MASK (0x100U)

Definition at line 29455 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_BUSY_SHIFT

#define OCOTP_CTRL_BUSY_SHIFT (8U)

Definition at line 29456 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_ADDR

#define OCOTP_CTRL_CLR_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_ADDR_SHIFT)) & OCOTP_CTRL_CLR_ADDR_MASK)

ADDR - ADDR

Definition at line 29548 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_ADDR_MASK

#define OCOTP_CTRL_CLR_ADDR_MASK (0x3FU)

Definition at line 29544 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_ADDR_SHIFT

#define OCOTP_CTRL_CLR_ADDR_SHIFT (0U)

Definition at line 29545 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_BUSY

#define OCOTP_CTRL_CLR_BUSY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_BUSY_SHIFT)) & OCOTP_CTRL_CLR_BUSY_MASK)

BUSY - BUSY

Definition at line 29558 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_BUSY_MASK

#define OCOTP_CTRL_CLR_BUSY_MASK (0x100U)

Definition at line 29554 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_BUSY_SHIFT

#define OCOTP_CTRL_CLR_BUSY_SHIFT (8U)

Definition at line 29555 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_CRC_FAIL

#define OCOTP_CTRL_CLR_CRC_FAIL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_CRC_FAIL_SHIFT)) & OCOTP_CTRL_CLR_CRC_FAIL_MASK)

CRC_FAIL - CRC_FAIL

Definition at line 29578 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_CRC_FAIL_MASK

#define OCOTP_CTRL_CLR_CRC_FAIL_MASK (0x1000U)

Definition at line 29574 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_CRC_FAIL_SHIFT

#define OCOTP_CTRL_CLR_CRC_FAIL_SHIFT (12U)

Definition at line 29575 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_CRC_TEST

#define OCOTP_CTRL_CLR_CRC_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_CRC_TEST_SHIFT)) & OCOTP_CTRL_CLR_CRC_TEST_MASK)

CRC_TEST - CRC_TEST

Definition at line 29573 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_CRC_TEST_MASK

#define OCOTP_CTRL_CLR_CRC_TEST_MASK (0x800U)

Definition at line 29569 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_CRC_TEST_SHIFT

#define OCOTP_CTRL_CLR_CRC_TEST_SHIFT (11U)

Definition at line 29570 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_ERROR

#define OCOTP_CTRL_CLR_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_ERROR_SHIFT)) & OCOTP_CTRL_CLR_ERROR_MASK)

ERROR - ERROR

Definition at line 29563 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_ERROR_MASK

#define OCOTP_CTRL_CLR_ERROR_MASK (0x200U)

Definition at line 29559 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_ERROR_SHIFT

#define OCOTP_CTRL_CLR_ERROR_SHIFT (9U)

Definition at line 29560 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RELOAD_SHADOWS

#define OCOTP_CTRL_CLR_RELOAD_SHADOWS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_CLR_RELOAD_SHADOWS_MASK)

RELOAD_SHADOWS - RELOAD_SHADOWS

Definition at line 29568 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RELOAD_SHADOWS_MASK

#define OCOTP_CTRL_CLR_RELOAD_SHADOWS_MASK (0x400U)

Definition at line 29564 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RELOAD_SHADOWS_SHIFT

#define OCOTP_CTRL_CLR_RELOAD_SHADOWS_SHIFT (10U)

Definition at line 29565 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RSVD0

#define OCOTP_CTRL_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_RSVD0_SHIFT)) & OCOTP_CTRL_CLR_RSVD0_MASK)

RSVD0 - RSVD0

Definition at line 29553 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RSVD0_MASK

#define OCOTP_CTRL_CLR_RSVD0_MASK (0xC0U)

Definition at line 29549 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RSVD0_SHIFT

#define OCOTP_CTRL_CLR_RSVD0_SHIFT (6U)

Definition at line 29550 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RSVD1

#define OCOTP_CTRL_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_RSVD1_SHIFT)) & OCOTP_CTRL_CLR_RSVD1_MASK)

RSVD1 - RSVD1

Definition at line 29583 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RSVD1_MASK

#define OCOTP_CTRL_CLR_RSVD1_MASK (0xE000U)

Definition at line 29579 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_RSVD1_SHIFT

#define OCOTP_CTRL_CLR_RSVD1_SHIFT (13U)

Definition at line 29580 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_WR_UNLOCK

#define OCOTP_CTRL_CLR_WR_UNLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CLR_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_CLR_WR_UNLOCK_MASK)

WR_UNLOCK - WR_UNLOCK

Definition at line 29588 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_WR_UNLOCK_MASK

#define OCOTP_CTRL_CLR_WR_UNLOCK_MASK (0xFFFF0000U)

Definition at line 29584 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CLR_WR_UNLOCK_SHIFT

#define OCOTP_CTRL_CLR_WR_UNLOCK_SHIFT (16U)

Definition at line 29585 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CRC_FAIL

#define OCOTP_CTRL_CRC_FAIL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CRC_FAIL_SHIFT)) & OCOTP_CTRL_CRC_FAIL_MASK)

CRC_FAIL - CRC_FAIL

Definition at line 29479 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CRC_FAIL_MASK

#define OCOTP_CTRL_CRC_FAIL_MASK (0x1000U)

Definition at line 29475 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CRC_FAIL_SHIFT

#define OCOTP_CTRL_CRC_FAIL_SHIFT (12U)

Definition at line 29476 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CRC_TEST

#define OCOTP_CTRL_CRC_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_CRC_TEST_SHIFT)) & OCOTP_CTRL_CRC_TEST_MASK)

CRC_TEST - CRC_TEST

Definition at line 29474 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CRC_TEST_MASK

#define OCOTP_CTRL_CRC_TEST_MASK (0x800U)

Definition at line 29470 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_CRC_TEST_SHIFT

#define OCOTP_CTRL_CRC_TEST_SHIFT (11U)

Definition at line 29471 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_ERROR

#define OCOTP_CTRL_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_ERROR_SHIFT)) & OCOTP_CTRL_ERROR_MASK)

ERROR - ERROR

Definition at line 29464 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_ERROR_MASK

#define OCOTP_CTRL_ERROR_MASK (0x200U)

Definition at line 29460 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_ERROR_SHIFT

#define OCOTP_CTRL_ERROR_SHIFT (9U)

Definition at line 29461 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RELOAD_SHADOWS

#define OCOTP_CTRL_RELOAD_SHADOWS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_RELOAD_SHADOWS_MASK)

RELOAD_SHADOWS - RELOAD_SHADOWS

Definition at line 29469 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RELOAD_SHADOWS_MASK

#define OCOTP_CTRL_RELOAD_SHADOWS_MASK (0x400U)

Definition at line 29465 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RELOAD_SHADOWS_SHIFT

#define OCOTP_CTRL_RELOAD_SHADOWS_SHIFT (10U)

Definition at line 29466 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RSVD0

#define OCOTP_CTRL_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_RSVD0_SHIFT)) & OCOTP_CTRL_RSVD0_MASK)

RSVD0 - RSVD0

Definition at line 29454 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RSVD0_MASK

#define OCOTP_CTRL_RSVD0_MASK (0xC0U)

Definition at line 29450 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RSVD0_SHIFT

#define OCOTP_CTRL_RSVD0_SHIFT (6U)

Definition at line 29451 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RSVD1

#define OCOTP_CTRL_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_RSVD1_SHIFT)) & OCOTP_CTRL_RSVD1_MASK)

RSVD1 - RSVD1

Definition at line 29484 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RSVD1_MASK

#define OCOTP_CTRL_RSVD1_MASK (0xE000U)

Definition at line 29480 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_RSVD1_SHIFT

#define OCOTP_CTRL_RSVD1_SHIFT (13U)

Definition at line 29481 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_ADDR

#define OCOTP_CTRL_SET_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_ADDR_SHIFT)) & OCOTP_CTRL_SET_ADDR_MASK)

ADDR - ADDR

Definition at line 29499 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_ADDR_MASK

#define OCOTP_CTRL_SET_ADDR_MASK (0x3FU)

Definition at line 29495 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_ADDR_SHIFT

#define OCOTP_CTRL_SET_ADDR_SHIFT (0U)

Definition at line 29496 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_BUSY

#define OCOTP_CTRL_SET_BUSY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_BUSY_SHIFT)) & OCOTP_CTRL_SET_BUSY_MASK)

BUSY - BUSY

Definition at line 29509 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_BUSY_MASK

#define OCOTP_CTRL_SET_BUSY_MASK (0x100U)

Definition at line 29505 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_BUSY_SHIFT

#define OCOTP_CTRL_SET_BUSY_SHIFT (8U)

Definition at line 29506 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_CRC_FAIL

#define OCOTP_CTRL_SET_CRC_FAIL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_CRC_FAIL_SHIFT)) & OCOTP_CTRL_SET_CRC_FAIL_MASK)

CRC_FAIL - CRC_FAIL

Definition at line 29529 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_CRC_FAIL_MASK

#define OCOTP_CTRL_SET_CRC_FAIL_MASK (0x1000U)

Definition at line 29525 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_CRC_FAIL_SHIFT

#define OCOTP_CTRL_SET_CRC_FAIL_SHIFT (12U)

Definition at line 29526 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_CRC_TEST

#define OCOTP_CTRL_SET_CRC_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_CRC_TEST_SHIFT)) & OCOTP_CTRL_SET_CRC_TEST_MASK)

CRC_TEST - CRC_TEST

Definition at line 29524 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_CRC_TEST_MASK

#define OCOTP_CTRL_SET_CRC_TEST_MASK (0x800U)

Definition at line 29520 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_CRC_TEST_SHIFT

#define OCOTP_CTRL_SET_CRC_TEST_SHIFT (11U)

Definition at line 29521 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_ERROR

#define OCOTP_CTRL_SET_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_ERROR_SHIFT)) & OCOTP_CTRL_SET_ERROR_MASK)

ERROR - ERROR

Definition at line 29514 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_ERROR_MASK

#define OCOTP_CTRL_SET_ERROR_MASK (0x200U)

Definition at line 29510 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_ERROR_SHIFT

#define OCOTP_CTRL_SET_ERROR_SHIFT (9U)

Definition at line 29511 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RELOAD_SHADOWS

#define OCOTP_CTRL_SET_RELOAD_SHADOWS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_SET_RELOAD_SHADOWS_MASK)

RELOAD_SHADOWS - RELOAD_SHADOWS

Definition at line 29519 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RELOAD_SHADOWS_MASK

#define OCOTP_CTRL_SET_RELOAD_SHADOWS_MASK (0x400U)

Definition at line 29515 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RELOAD_SHADOWS_SHIFT

#define OCOTP_CTRL_SET_RELOAD_SHADOWS_SHIFT (10U)

Definition at line 29516 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RSVD0

#define OCOTP_CTRL_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_RSVD0_SHIFT)) & OCOTP_CTRL_SET_RSVD0_MASK)

RSVD0 - RSVD0

Definition at line 29504 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RSVD0_MASK

#define OCOTP_CTRL_SET_RSVD0_MASK (0xC0U)

Definition at line 29500 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RSVD0_SHIFT

#define OCOTP_CTRL_SET_RSVD0_SHIFT (6U)

Definition at line 29501 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RSVD1

#define OCOTP_CTRL_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_RSVD1_SHIFT)) & OCOTP_CTRL_SET_RSVD1_MASK)

RSVD1 - RSVD1

Definition at line 29534 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RSVD1_MASK

#define OCOTP_CTRL_SET_RSVD1_MASK (0xE000U)

Definition at line 29530 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_RSVD1_SHIFT

#define OCOTP_CTRL_SET_RSVD1_SHIFT (13U)

Definition at line 29531 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_WR_UNLOCK

#define OCOTP_CTRL_SET_WR_UNLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_SET_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_SET_WR_UNLOCK_MASK)

WR_UNLOCK - WR_UNLOCK

Definition at line 29539 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_WR_UNLOCK_MASK

#define OCOTP_CTRL_SET_WR_UNLOCK_MASK (0xFFFF0000U)

Definition at line 29535 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_SET_WR_UNLOCK_SHIFT

#define OCOTP_CTRL_SET_WR_UNLOCK_SHIFT (16U)

Definition at line 29536 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_ADDR

#define OCOTP_CTRL_TOG_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_ADDR_SHIFT)) & OCOTP_CTRL_TOG_ADDR_MASK)

ADDR - ADDR

Definition at line 29597 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_ADDR_MASK

#define OCOTP_CTRL_TOG_ADDR_MASK (0x3FU)

Definition at line 29593 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_ADDR_SHIFT

#define OCOTP_CTRL_TOG_ADDR_SHIFT (0U)

Definition at line 29594 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_BUSY

#define OCOTP_CTRL_TOG_BUSY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_BUSY_SHIFT)) & OCOTP_CTRL_TOG_BUSY_MASK)

BUSY - BUSY

Definition at line 29607 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_BUSY_MASK

#define OCOTP_CTRL_TOG_BUSY_MASK (0x100U)

Definition at line 29603 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_BUSY_SHIFT

#define OCOTP_CTRL_TOG_BUSY_SHIFT (8U)

Definition at line 29604 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_CRC_FAIL

#define OCOTP_CTRL_TOG_CRC_FAIL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_CRC_FAIL_SHIFT)) & OCOTP_CTRL_TOG_CRC_FAIL_MASK)

CRC_FAIL - CRC_FAIL

Definition at line 29627 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_CRC_FAIL_MASK

#define OCOTP_CTRL_TOG_CRC_FAIL_MASK (0x1000U)

Definition at line 29623 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_CRC_FAIL_SHIFT

#define OCOTP_CTRL_TOG_CRC_FAIL_SHIFT (12U)

Definition at line 29624 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_CRC_TEST

#define OCOTP_CTRL_TOG_CRC_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_CRC_TEST_SHIFT)) & OCOTP_CTRL_TOG_CRC_TEST_MASK)

CRC_TEST - CRC_TEST

Definition at line 29622 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_CRC_TEST_MASK

#define OCOTP_CTRL_TOG_CRC_TEST_MASK (0x800U)

Definition at line 29618 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_CRC_TEST_SHIFT

#define OCOTP_CTRL_TOG_CRC_TEST_SHIFT (11U)

Definition at line 29619 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_ERROR

#define OCOTP_CTRL_TOG_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_ERROR_SHIFT)) & OCOTP_CTRL_TOG_ERROR_MASK)

ERROR - ERROR

Definition at line 29612 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_ERROR_MASK

#define OCOTP_CTRL_TOG_ERROR_MASK (0x200U)

Definition at line 29608 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_ERROR_SHIFT

#define OCOTP_CTRL_TOG_ERROR_SHIFT (9U)

Definition at line 29609 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RELOAD_SHADOWS

#define OCOTP_CTRL_TOG_RELOAD_SHADOWS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_RELOAD_SHADOWS_SHIFT)) & OCOTP_CTRL_TOG_RELOAD_SHADOWS_MASK)

RELOAD_SHADOWS - RELOAD_SHADOWS

Definition at line 29617 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RELOAD_SHADOWS_MASK

#define OCOTP_CTRL_TOG_RELOAD_SHADOWS_MASK (0x400U)

Definition at line 29613 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RELOAD_SHADOWS_SHIFT

#define OCOTP_CTRL_TOG_RELOAD_SHADOWS_SHIFT (10U)

Definition at line 29614 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RSVD0

#define OCOTP_CTRL_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_RSVD0_SHIFT)) & OCOTP_CTRL_TOG_RSVD0_MASK)

RSVD0 - RSVD0

Definition at line 29602 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RSVD0_MASK

#define OCOTP_CTRL_TOG_RSVD0_MASK (0xC0U)

Definition at line 29598 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RSVD0_SHIFT

#define OCOTP_CTRL_TOG_RSVD0_SHIFT (6U)

Definition at line 29599 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RSVD1

#define OCOTP_CTRL_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_RSVD1_SHIFT)) & OCOTP_CTRL_TOG_RSVD1_MASK)

RSVD1 - RSVD1

Definition at line 29632 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RSVD1_MASK

#define OCOTP_CTRL_TOG_RSVD1_MASK (0xE000U)

Definition at line 29628 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_RSVD1_SHIFT

#define OCOTP_CTRL_TOG_RSVD1_SHIFT (13U)

Definition at line 29629 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_WR_UNLOCK

#define OCOTP_CTRL_TOG_WR_UNLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_TOG_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_TOG_WR_UNLOCK_MASK)

WR_UNLOCK - WR_UNLOCK

Definition at line 29637 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_WR_UNLOCK_MASK

#define OCOTP_CTRL_TOG_WR_UNLOCK_MASK (0xFFFF0000U)

Definition at line 29633 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_TOG_WR_UNLOCK_SHIFT

#define OCOTP_CTRL_TOG_WR_UNLOCK_SHIFT (16U)

Definition at line 29634 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_WR_UNLOCK

#define OCOTP_CTRL_WR_UNLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_CTRL_WR_UNLOCK_SHIFT)) & OCOTP_CTRL_WR_UNLOCK_MASK)

WR_UNLOCK - WR_UNLOCK 0b0011111001110111..Key needed to unlock HW_OCOTP_DATA register.

Definition at line 29490 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_WR_UNLOCK_MASK

#define OCOTP_CTRL_WR_UNLOCK_MASK (0xFFFF0000U)

Definition at line 29485 of file MIMXRT1062.h.

## ◆ OCOTP_CTRL_WR_UNLOCK_SHIFT

#define OCOTP_CTRL_WR_UNLOCK_SHIFT (16U)

Definition at line 29486 of file MIMXRT1062.h.

## ◆ OCOTP_DATA_DATA

#define OCOTP_DATA_DATA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_DATA_DATA_SHIFT)) & OCOTP_DATA_DATA_MASK)

DATA - DATA

Definition at line 29675 of file MIMXRT1062.h.

## ◆ OCOTP_DATA_DATA_MASK

#define OCOTP_DATA_DATA_MASK (0xFFFFFFFFU)

Definition at line 29671 of file MIMXRT1062.h.

## ◆ OCOTP_DATA_DATA_SHIFT

#define OCOTP_DATA_DATA_SHIFT (0U)

Definition at line 29672 of file MIMXRT1062.h.

## ◆ OCOTP_GP1_BITS

#define OCOTP_GP1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP1_BITS_SHIFT)) & OCOTP_GP1_BITS_MASK)

BITS - BITS

Definition at line 30330 of file MIMXRT1062.h.

## ◆ OCOTP_GP1_BITS_MASK

#define OCOTP_GP1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30326 of file MIMXRT1062.h.

## ◆ OCOTP_GP1_BITS_SHIFT

#define OCOTP_GP1_BITS_SHIFT (0U)

Definition at line 30327 of file MIMXRT1062.h.

## ◆ OCOTP_GP2_BITS

#define OCOTP_GP2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP2_BITS_SHIFT)) & OCOTP_GP2_BITS_MASK)

BITS - BITS

Definition at line 30339 of file MIMXRT1062.h.

## ◆ OCOTP_GP2_BITS_MASK

#define OCOTP_GP2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30335 of file MIMXRT1062.h.

## ◆ OCOTP_GP2_BITS_SHIFT

#define OCOTP_GP2_BITS_SHIFT (0U)

Definition at line 30336 of file MIMXRT1062.h.

## ◆ OCOTP_GP30_BITS

#define OCOTP_GP30_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP30_BITS_SHIFT)) & OCOTP_GP30_BITS_MASK)

BITS - BITS

Definition at line 30492 of file MIMXRT1062.h.

## ◆ OCOTP_GP30_BITS_MASK

#define OCOTP_GP30_BITS_MASK (0xFFFFFFFFU)

Definition at line 30488 of file MIMXRT1062.h.

## ◆ OCOTP_GP30_BITS_SHIFT

#define OCOTP_GP30_BITS_SHIFT (0U)

Definition at line 30489 of file MIMXRT1062.h.

## ◆ OCOTP_GP31_BITS

#define OCOTP_GP31_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP31_BITS_SHIFT)) & OCOTP_GP31_BITS_MASK)

BITS - BITS

Definition at line 30501 of file MIMXRT1062.h.

## ◆ OCOTP_GP31_BITS_MASK

#define OCOTP_GP31_BITS_MASK (0xFFFFFFFFU)

Definition at line 30497 of file MIMXRT1062.h.

## ◆ OCOTP_GP31_BITS_SHIFT

#define OCOTP_GP31_BITS_SHIFT (0U)

Definition at line 30498 of file MIMXRT1062.h.

## ◆ OCOTP_GP32_BITS

#define OCOTP_GP32_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP32_BITS_SHIFT)) & OCOTP_GP32_BITS_MASK)

BITS - BITS

Definition at line 30510 of file MIMXRT1062.h.

## ◆ OCOTP_GP32_BITS_MASK

#define OCOTP_GP32_BITS_MASK (0xFFFFFFFFU)

Definition at line 30506 of file MIMXRT1062.h.

## ◆ OCOTP_GP32_BITS_SHIFT

#define OCOTP_GP32_BITS_SHIFT (0U)

Definition at line 30507 of file MIMXRT1062.h.

## ◆ OCOTP_GP33_BITS

#define OCOTP_GP33_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP33_BITS_SHIFT)) & OCOTP_GP33_BITS_MASK)

BITS - BITS

Definition at line 30519 of file MIMXRT1062.h.

## ◆ OCOTP_GP33_BITS_MASK

#define OCOTP_GP33_BITS_MASK (0xFFFFFFFFU)

Definition at line 30515 of file MIMXRT1062.h.

## ◆ OCOTP_GP33_BITS_SHIFT

#define OCOTP_GP33_BITS_SHIFT (0U)

Definition at line 30516 of file MIMXRT1062.h.

## ◆ OCOTP_GP40_BITS

#define OCOTP_GP40_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP40_BITS_SHIFT)) & OCOTP_GP40_BITS_MASK)

BITS - BITS

Definition at line 30528 of file MIMXRT1062.h.

## ◆ OCOTP_GP40_BITS_MASK

#define OCOTP_GP40_BITS_MASK (0xFFFFFFFFU)

Definition at line 30524 of file MIMXRT1062.h.

## ◆ OCOTP_GP40_BITS_SHIFT

#define OCOTP_GP40_BITS_SHIFT (0U)

Definition at line 30525 of file MIMXRT1062.h.

## ◆ OCOTP_GP41_BITS

#define OCOTP_GP41_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP41_BITS_SHIFT)) & OCOTP_GP41_BITS_MASK)

BITS - BITS

Definition at line 30537 of file MIMXRT1062.h.

## ◆ OCOTP_GP41_BITS_MASK

#define OCOTP_GP41_BITS_MASK (0xFFFFFFFFU)

Definition at line 30533 of file MIMXRT1062.h.

## ◆ OCOTP_GP41_BITS_SHIFT

#define OCOTP_GP41_BITS_SHIFT (0U)

Definition at line 30534 of file MIMXRT1062.h.

## ◆ OCOTP_GP42_BITS

#define OCOTP_GP42_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP42_BITS_SHIFT)) & OCOTP_GP42_BITS_MASK)

BITS - BITS

Definition at line 30546 of file MIMXRT1062.h.

## ◆ OCOTP_GP42_BITS_MASK

#define OCOTP_GP42_BITS_MASK (0xFFFFFFFFU)

Definition at line 30542 of file MIMXRT1062.h.

## ◆ OCOTP_GP42_BITS_SHIFT

#define OCOTP_GP42_BITS_SHIFT (0U)

Definition at line 30543 of file MIMXRT1062.h.

## ◆ OCOTP_GP43_BITS

#define OCOTP_GP43_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_GP43_BITS_SHIFT)) & OCOTP_GP43_BITS_MASK)

BITS - BITS

Definition at line 30555 of file MIMXRT1062.h.

## ◆ OCOTP_GP43_BITS_MASK

#define OCOTP_GP43_BITS_MASK (0xFFFFFFFFU)

Definition at line 30551 of file MIMXRT1062.h.

## ◆ OCOTP_GP43_BITS_SHIFT

#define OCOTP_GP43_BITS_SHIFT (0U)

Definition at line 30552 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_ANALOG

#define OCOTP_LOCK_ANALOG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_ANALOG_SHIFT)) & OCOTP_LOCK_ANALOG_MASK)

ANALOG - ANALOG

Definition at line 29953 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_ANALOG_MASK

#define OCOTP_LOCK_ANALOG_MASK (0xC0000U)

Definition at line 29949 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_ANALOG_SHIFT

#define OCOTP_LOCK_ANALOG_SHIFT (18U)

Definition at line 29950 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_BOOT_CFG

#define OCOTP_LOCK_BOOT_CFG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_BOOT_CFG_SHIFT)) & OCOTP_LOCK_BOOT_CFG_MASK)

BOOT_CFG - BOOT_CFG

Definition at line 29903 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_BOOT_CFG_MASK

#define OCOTP_LOCK_BOOT_CFG_MASK (0xCU)

Definition at line 29899 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_BOOT_CFG_SHIFT

#define OCOTP_LOCK_BOOT_CFG_SHIFT (2U)

Definition at line 29900 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_FIELD_RETURN

#define OCOTP_LOCK_FIELD_RETURN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_FIELD_RETURN_SHIFT)) & OCOTP_LOCK_FIELD_RETURN_MASK)

FIELD_RETURN - FIELD_RETURN

Definition at line 29988 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_FIELD_RETURN_MASK

#define OCOTP_LOCK_FIELD_RETURN_MASK (0xF0000000U)

Definition at line 29984 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_FIELD_RETURN_SHIFT

#define OCOTP_LOCK_FIELD_RETURN_SHIFT (28U)

Definition at line 29985 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP1

#define OCOTP_LOCK_GP1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP1_SHIFT)) & OCOTP_LOCK_GP1_MASK)

GP1 - GP1

Definition at line 29928 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP1_MASK

#define OCOTP_LOCK_GP1_MASK (0xC00U)

Definition at line 29924 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP1_SHIFT

#define OCOTP_LOCK_GP1_SHIFT (10U)

Definition at line 29925 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP2

#define OCOTP_LOCK_GP2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP2_SHIFT)) & OCOTP_LOCK_GP2_MASK)

GP2 - GP2

Definition at line 29933 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP2_MASK

#define OCOTP_LOCK_GP2_MASK (0x3000U)

Definition at line 29929 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP2_SHIFT

#define OCOTP_LOCK_GP2_SHIFT (12U)

Definition at line 29930 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP3

#define OCOTP_LOCK_GP3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP3_SHIFT)) & OCOTP_LOCK_GP3_MASK)

GP3 - GP3

Definition at line 29983 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP3_MASK

#define OCOTP_LOCK_GP3_MASK (0xC000000U)

Definition at line 29979 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP3_SHIFT

#define OCOTP_LOCK_GP3_SHIFT (26U)

Definition at line 29980 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP4

#define OCOTP_LOCK_GP4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP4_SHIFT)) & OCOTP_LOCK_GP4_MASK)

GP4 - GP4

Definition at line 29978 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP4_MASK

#define OCOTP_LOCK_GP4_MASK (0x3000000U)

Definition at line 29974 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP4_RLOCK

#define OCOTP_LOCK_GP4_RLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_GP4_RLOCK_SHIFT)) & OCOTP_LOCK_GP4_RLOCK_MASK)

GP4_RLOCK - GP4_RLOCK

Definition at line 29918 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP4_RLOCK_MASK

#define OCOTP_LOCK_GP4_RLOCK_MASK (0x80U)

Definition at line 29914 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP4_RLOCK_SHIFT

#define OCOTP_LOCK_GP4_RLOCK_SHIFT (7U)

Definition at line 29915 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_GP4_SHIFT

#define OCOTP_LOCK_GP4_SHIFT (24U)

Definition at line 29975 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MAC_ADDR

#define OCOTP_LOCK_MAC_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_MAC_ADDR_SHIFT)) & OCOTP_LOCK_MAC_ADDR_MASK)

MAC_ADDR - MAC_ADDR

Definition at line 29923 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MAC_ADDR_MASK

#define OCOTP_LOCK_MAC_ADDR_MASK (0x300U)

Definition at line 29919 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MAC_ADDR_SHIFT

#define OCOTP_LOCK_MAC_ADDR_SHIFT (8U)

Definition at line 29920 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MEM_TRIM

#define OCOTP_LOCK_MEM_TRIM | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_MEM_TRIM_SHIFT)) & OCOTP_LOCK_MEM_TRIM_MASK)

MEM_TRIM - MEM_TRIM

Definition at line 29908 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MEM_TRIM_MASK

#define OCOTP_LOCK_MEM_TRIM_MASK (0x30U)

Definition at line 29904 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MEM_TRIM_SHIFT

#define OCOTP_LOCK_MEM_TRIM_SHIFT (4U)

Definition at line 29905 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MISC_CONF

#define OCOTP_LOCK_MISC_CONF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_MISC_CONF_SHIFT)) & OCOTP_LOCK_MISC_CONF_MASK)

MISC_CONF - MISC_CONF

Definition at line 29968 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MISC_CONF_MASK

#define OCOTP_LOCK_MISC_CONF_MASK (0x400000U)

Definition at line 29964 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_MISC_CONF_SHIFT

#define OCOTP_LOCK_MISC_CONF_SHIFT (22U)

Definition at line 29965 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_OTPMK

#define OCOTP_LOCK_OTPMK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_OTPMK_SHIFT)) & OCOTP_LOCK_OTPMK_MASK)

OTPMK - OTPMK

Definition at line 29948 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_OTPMK_CRC

#define OCOTP_LOCK_OTPMK_CRC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_OTPMK_CRC_SHIFT)) & OCOTP_LOCK_OTPMK_CRC_MASK)

OTPMK_CRC - OTPMK_CRC

Definition at line 29958 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_OTPMK_CRC_MASK

#define OCOTP_LOCK_OTPMK_CRC_MASK (0x100000U)

Definition at line 29954 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_OTPMK_CRC_SHIFT

#define OCOTP_LOCK_OTPMK_CRC_SHIFT (20U)

Definition at line 29955 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_OTPMK_MASK

#define OCOTP_LOCK_OTPMK_MASK (0x20000U)

Definition at line 29944 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_OTPMK_SHIFT

#define OCOTP_LOCK_OTPMK_SHIFT (17U)

Definition at line 29945 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_ROM_PATCH

#define OCOTP_LOCK_ROM_PATCH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_ROM_PATCH_SHIFT)) & OCOTP_LOCK_ROM_PATCH_MASK)

ROM_PATCH - ROM_PATCH

Definition at line 29938 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_ROM_PATCH_MASK

#define OCOTP_LOCK_ROM_PATCH_MASK (0x8000U)

Definition at line 29934 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_ROM_PATCH_SHIFT

#define OCOTP_LOCK_ROM_PATCH_SHIFT (15U)

Definition at line 29935 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SJC_RESP

#define OCOTP_LOCK_SJC_RESP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SJC_RESP_SHIFT)) & OCOTP_LOCK_SJC_RESP_MASK)

SJC_RESP - SJC_RESP

Definition at line 29913 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SJC_RESP_MASK

#define OCOTP_LOCK_SJC_RESP_MASK (0x40U)

Definition at line 29909 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SJC_RESP_SHIFT

#define OCOTP_LOCK_SJC_RESP_SHIFT (6U)

Definition at line 29910 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP1

#define OCOTP_LOCK_SW_GP1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SW_GP1_SHIFT)) & OCOTP_LOCK_SW_GP1_MASK)

SW_GP1 - SW_GP1

Definition at line 29943 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP1_MASK

#define OCOTP_LOCK_SW_GP1_MASK (0x10000U)

Definition at line 29939 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP1_SHIFT

#define OCOTP_LOCK_SW_GP1_SHIFT (16U)

Definition at line 29940 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP2_LOCK

#define OCOTP_LOCK_SW_GP2_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SW_GP2_LOCK_SHIFT)) & OCOTP_LOCK_SW_GP2_LOCK_MASK)

SW_GP2_LOCK - SW_GP2_LOCK

Definition at line 29963 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP2_LOCK_MASK

#define OCOTP_LOCK_SW_GP2_LOCK_MASK (0x200000U)

Definition at line 29959 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP2_LOCK_SHIFT

#define OCOTP_LOCK_SW_GP2_LOCK_SHIFT (21U)

Definition at line 29960 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP2_RLOCK

#define OCOTP_LOCK_SW_GP2_RLOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_SW_GP2_RLOCK_SHIFT)) & OCOTP_LOCK_SW_GP2_RLOCK_MASK)

SW_GP2_RLOCK - SW_GP2_RLOCK

Definition at line 29973 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP2_RLOCK_MASK

#define OCOTP_LOCK_SW_GP2_RLOCK_MASK (0x800000U)

Definition at line 29969 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_SW_GP2_RLOCK_SHIFT

#define OCOTP_LOCK_SW_GP2_RLOCK_SHIFT (23U)

Definition at line 29970 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_TESTER

#define OCOTP_LOCK_TESTER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_LOCK_TESTER_SHIFT)) & OCOTP_LOCK_TESTER_MASK)

TESTER - TESTER

Definition at line 29898 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_TESTER_MASK

#define OCOTP_LOCK_TESTER_MASK (0x3U)

Definition at line 29894 of file MIMXRT1062.h.

## ◆ OCOTP_LOCK_TESTER_SHIFT

#define OCOTP_LOCK_TESTER_SHIFT (0U)

Definition at line 29895 of file MIMXRT1062.h.

## ◆ OCOTP_MAC0_BITS

#define OCOTP_MAC0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MAC0_BITS_SHIFT)) & OCOTP_MAC0_BITS_MASK)

BITS - BITS

Definition at line 30294 of file MIMXRT1062.h.

## ◆ OCOTP_MAC0_BITS_MASK

#define OCOTP_MAC0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30290 of file MIMXRT1062.h.

## ◆ OCOTP_MAC0_BITS_SHIFT

#define OCOTP_MAC0_BITS_SHIFT (0U)

Definition at line 30291 of file MIMXRT1062.h.

## ◆ OCOTP_MAC1_BITS

#define OCOTP_MAC1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MAC1_BITS_SHIFT)) & OCOTP_MAC1_BITS_MASK)

BITS - BITS

Definition at line 30303 of file MIMXRT1062.h.

## ◆ OCOTP_MAC1_BITS_MASK

#define OCOTP_MAC1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30299 of file MIMXRT1062.h.

## ◆ OCOTP_MAC1_BITS_SHIFT

#define OCOTP_MAC1_BITS_SHIFT (0U)

Definition at line 30300 of file MIMXRT1062.h.

## ◆ OCOTP_MAC2_BITS

#define OCOTP_MAC2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MAC2_BITS_SHIFT)) & OCOTP_MAC2_BITS_MASK)

BITS - BITS

Definition at line 30312 of file MIMXRT1062.h.

## ◆ OCOTP_MAC2_BITS_MASK

#define OCOTP_MAC2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30308 of file MIMXRT1062.h.

## ◆ OCOTP_MAC2_BITS_SHIFT

#define OCOTP_MAC2_BITS_SHIFT (0U)

Definition at line 30309 of file MIMXRT1062.h.

## ◆ OCOTP_MEM0_BITS

#define OCOTP_MEM0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM0_BITS_SHIFT)) & OCOTP_MEM0_BITS_MASK)

BITS - BITS

Definition at line 30060 of file MIMXRT1062.h.

## ◆ OCOTP_MEM0_BITS_MASK

#define OCOTP_MEM0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30056 of file MIMXRT1062.h.

## ◆ OCOTP_MEM0_BITS_SHIFT

#define OCOTP_MEM0_BITS_SHIFT (0U)

Definition at line 30057 of file MIMXRT1062.h.

## ◆ OCOTP_MEM1_BITS

#define OCOTP_MEM1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM1_BITS_SHIFT)) & OCOTP_MEM1_BITS_MASK)

BITS - BITS

Definition at line 30069 of file MIMXRT1062.h.

## ◆ OCOTP_MEM1_BITS_MASK

#define OCOTP_MEM1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30065 of file MIMXRT1062.h.

## ◆ OCOTP_MEM1_BITS_SHIFT

#define OCOTP_MEM1_BITS_SHIFT (0U)

Definition at line 30066 of file MIMXRT1062.h.

## ◆ OCOTP_MEM2_BITS

#define OCOTP_MEM2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM2_BITS_SHIFT)) & OCOTP_MEM2_BITS_MASK)

BITS - BITS

Definition at line 30078 of file MIMXRT1062.h.

## ◆ OCOTP_MEM2_BITS_MASK

#define OCOTP_MEM2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30074 of file MIMXRT1062.h.

## ◆ OCOTP_MEM2_BITS_SHIFT

#define OCOTP_MEM2_BITS_SHIFT (0U)

Definition at line 30075 of file MIMXRT1062.h.

## ◆ OCOTP_MEM3_BITS

#define OCOTP_MEM3_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM3_BITS_SHIFT)) & OCOTP_MEM3_BITS_MASK)

BITS - BITS

Definition at line 30087 of file MIMXRT1062.h.

## ◆ OCOTP_MEM3_BITS_MASK

#define OCOTP_MEM3_BITS_MASK (0xFFFFFFFFU)

Definition at line 30083 of file MIMXRT1062.h.

## ◆ OCOTP_MEM3_BITS_SHIFT

#define OCOTP_MEM3_BITS_SHIFT (0U)

Definition at line 30084 of file MIMXRT1062.h.

## ◆ OCOTP_MEM4_BITS

#define OCOTP_MEM4_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MEM4_BITS_SHIFT)) & OCOTP_MEM4_BITS_MASK)

BITS - BITS

Definition at line 30096 of file MIMXRT1062.h.

## ◆ OCOTP_MEM4_BITS_MASK

#define OCOTP_MEM4_BITS_MASK (0xFFFFFFFFU)

Definition at line 30092 of file MIMXRT1062.h.

## ◆ OCOTP_MEM4_BITS_SHIFT

#define OCOTP_MEM4_BITS_SHIFT (0U)

Definition at line 30093 of file MIMXRT1062.h.

## ◆ OCOTP_MISC_CONF0_BITS

#define OCOTP_MISC_CONF0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MISC_CONF0_BITS_SHIFT)) & OCOTP_MISC_CONF0_BITS_MASK)

BITS - BITS

Definition at line 30393 of file MIMXRT1062.h.

## ◆ OCOTP_MISC_CONF0_BITS_MASK

#define OCOTP_MISC_CONF0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30389 of file MIMXRT1062.h.

## ◆ OCOTP_MISC_CONF0_BITS_SHIFT

#define OCOTP_MISC_CONF0_BITS_SHIFT (0U)

Definition at line 30390 of file MIMXRT1062.h.

## ◆ OCOTP_MISC_CONF1_BITS

#define OCOTP_MISC_CONF1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_MISC_CONF1_BITS_SHIFT)) & OCOTP_MISC_CONF1_BITS_MASK)

BITS - BITS

Definition at line 30402 of file MIMXRT1062.h.

## ◆ OCOTP_MISC_CONF1_BITS_MASK

#define OCOTP_MISC_CONF1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30398 of file MIMXRT1062.h.

## ◆ OCOTP_MISC_CONF1_BITS_SHIFT

#define OCOTP_MISC_CONF1_BITS_SHIFT (0U)

Definition at line 30399 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK0_BITS

#define OCOTP_OTPMK0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK0_BITS_SHIFT)) & OCOTP_OTPMK0_BITS_MASK)

BITS - BITS

Definition at line 30132 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK0_BITS_MASK

#define OCOTP_OTPMK0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30128 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK0_BITS_SHIFT

#define OCOTP_OTPMK0_BITS_SHIFT (0U)

Definition at line 30129 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK1_BITS

#define OCOTP_OTPMK1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK1_BITS_SHIFT)) & OCOTP_OTPMK1_BITS_MASK)

BITS - BITS

Definition at line 30141 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK1_BITS_MASK

#define OCOTP_OTPMK1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30137 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK1_BITS_SHIFT

#define OCOTP_OTPMK1_BITS_SHIFT (0U)

Definition at line 30138 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK2_BITS

#define OCOTP_OTPMK2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK2_BITS_SHIFT)) & OCOTP_OTPMK2_BITS_MASK)

BITS - BITS

Definition at line 30150 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK2_BITS_MASK

#define OCOTP_OTPMK2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30146 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK2_BITS_SHIFT

#define OCOTP_OTPMK2_BITS_SHIFT (0U)

Definition at line 30147 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK3_BITS

#define OCOTP_OTPMK3_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK3_BITS_SHIFT)) & OCOTP_OTPMK3_BITS_MASK)

BITS - BITS

Definition at line 30159 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK3_BITS_MASK

#define OCOTP_OTPMK3_BITS_MASK (0xFFFFFFFFU)

Definition at line 30155 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK3_BITS_SHIFT

#define OCOTP_OTPMK3_BITS_SHIFT (0U)

Definition at line 30156 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK4_BITS

#define OCOTP_OTPMK4_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK4_BITS_SHIFT)) & OCOTP_OTPMK4_BITS_MASK)

BITS - BITS

Definition at line 30168 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK4_BITS_MASK

#define OCOTP_OTPMK4_BITS_MASK (0xFFFFFFFFU)

Definition at line 30164 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK4_BITS_SHIFT

#define OCOTP_OTPMK4_BITS_SHIFT (0U)

Definition at line 30165 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK5_BITS

#define OCOTP_OTPMK5_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK5_BITS_SHIFT)) & OCOTP_OTPMK5_BITS_MASK)

BITS - BITS

Definition at line 30177 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK5_BITS_MASK

#define OCOTP_OTPMK5_BITS_MASK (0xFFFFFFFFU)

Definition at line 30173 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK5_BITS_SHIFT

#define OCOTP_OTPMK5_BITS_SHIFT (0U)

Definition at line 30174 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK6_BITS

#define OCOTP_OTPMK6_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK6_BITS_SHIFT)) & OCOTP_OTPMK6_BITS_MASK)

BITS - BITS

Definition at line 30186 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK6_BITS_MASK

#define OCOTP_OTPMK6_BITS_MASK (0xFFFFFFFFU)

Definition at line 30182 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK6_BITS_SHIFT

#define OCOTP_OTPMK6_BITS_SHIFT (0U)

Definition at line 30183 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK7_BITS

#define OCOTP_OTPMK7_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK7_BITS_SHIFT)) & OCOTP_OTPMK7_BITS_MASK)

BITS - BITS

Definition at line 30195 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK7_BITS_MASK

#define OCOTP_OTPMK7_BITS_MASK (0xFFFFFFFFU)

Definition at line 30191 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK7_BITS_SHIFT

#define OCOTP_OTPMK7_BITS_SHIFT (0U)

Definition at line 30192 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK_CRC32_BITS

#define OCOTP_OTPMK_CRC32_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_OTPMK_CRC32_BITS_SHIFT)) & OCOTP_OTPMK_CRC32_BITS_MASK)

BITS - BITS

Definition at line 30321 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK_CRC32_BITS_MASK

#define OCOTP_OTPMK_CRC32_BITS_MASK (0xFFFFFFFFU)

Definition at line 30317 of file MIMXRT1062.h.

## ◆ OCOTP_OTPMK_CRC32_BITS_SHIFT

#define OCOTP_OTPMK_CRC32_BITS_SHIFT (0U)

Definition at line 30318 of file MIMXRT1062.h.

## ◆ OCOTP_READ_CTRL_READ_FUSE

#define OCOTP_READ_CTRL_READ_FUSE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_READ_CTRL_READ_FUSE_SHIFT)) & OCOTP_READ_CTRL_READ_FUSE_MASK)

READ_FUSE - READ_FUSE

Definition at line 29684 of file MIMXRT1062.h.

## ◆ OCOTP_READ_CTRL_READ_FUSE_MASK

#define OCOTP_READ_CTRL_READ_FUSE_MASK (0x1U)

Definition at line 29680 of file MIMXRT1062.h.

## ◆ OCOTP_READ_CTRL_READ_FUSE_SHIFT

#define OCOTP_READ_CTRL_READ_FUSE_SHIFT (0U)

Definition at line 29681 of file MIMXRT1062.h.

## ◆ OCOTP_READ_CTRL_RSVD0

#define OCOTP_READ_CTRL_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_READ_CTRL_RSVD0_SHIFT)) & OCOTP_READ_CTRL_RSVD0_MASK)

RSVD0 - RSVD0

Definition at line 29689 of file MIMXRT1062.h.

## ◆ OCOTP_READ_CTRL_RSVD0_MASK

#define OCOTP_READ_CTRL_RSVD0_MASK (0xFFFFFFFEU)

Definition at line 29685 of file MIMXRT1062.h.

## ◆ OCOTP_READ_CTRL_RSVD0_SHIFT

#define OCOTP_READ_CTRL_RSVD0_SHIFT (1U)

Definition at line 29686 of file MIMXRT1062.h.

## ◆ OCOTP_READ_FUSE_DATA_DATA

#define OCOTP_READ_FUSE_DATA_DATA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_READ_FUSE_DATA_DATA_SHIFT)) & OCOTP_READ_FUSE_DATA_DATA_MASK)

DATA - DATA

Definition at line 29698 of file MIMXRT1062.h.

## ◆ OCOTP_READ_FUSE_DATA_DATA_MASK

#define OCOTP_READ_FUSE_DATA_DATA_MASK (0xFFFFFFFFU)

Definition at line 29694 of file MIMXRT1062.h.

## ◆ OCOTP_READ_FUSE_DATA_DATA_SHIFT

#define OCOTP_READ_FUSE_DATA_DATA_SHIFT (0U)

Definition at line 29695 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH0_BITS

#define OCOTP_ROM_PATCH0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH0_BITS_SHIFT)) & OCOTP_ROM_PATCH0_BITS_MASK)

BITS - BITS

Definition at line 30420 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH0_BITS_MASK

#define OCOTP_ROM_PATCH0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30416 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH0_BITS_SHIFT

#define OCOTP_ROM_PATCH0_BITS_SHIFT (0U)

Definition at line 30417 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH1_BITS

#define OCOTP_ROM_PATCH1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH1_BITS_SHIFT)) & OCOTP_ROM_PATCH1_BITS_MASK)

BITS - BITS

Definition at line 30429 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH1_BITS_MASK

#define OCOTP_ROM_PATCH1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30425 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH1_BITS_SHIFT

#define OCOTP_ROM_PATCH1_BITS_SHIFT (0U)

Definition at line 30426 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH2_BITS

#define OCOTP_ROM_PATCH2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH2_BITS_SHIFT)) & OCOTP_ROM_PATCH2_BITS_MASK)

BITS - BITS

Definition at line 30438 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH2_BITS_MASK

#define OCOTP_ROM_PATCH2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30434 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH2_BITS_SHIFT

#define OCOTP_ROM_PATCH2_BITS_SHIFT (0U)

Definition at line 30435 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH3_BITS

#define OCOTP_ROM_PATCH3_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH3_BITS_SHIFT)) & OCOTP_ROM_PATCH3_BITS_MASK)

BITS - BITS

Definition at line 30447 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH3_BITS_MASK

#define OCOTP_ROM_PATCH3_BITS_MASK (0xFFFFFFFFU)

Definition at line 30443 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH3_BITS_SHIFT

#define OCOTP_ROM_PATCH3_BITS_SHIFT (0U)

Definition at line 30444 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH4_BITS

#define OCOTP_ROM_PATCH4_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH4_BITS_SHIFT)) & OCOTP_ROM_PATCH4_BITS_MASK)

BITS - BITS

Definition at line 30456 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH4_BITS_MASK

#define OCOTP_ROM_PATCH4_BITS_MASK (0xFFFFFFFFU)

Definition at line 30452 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH4_BITS_SHIFT

#define OCOTP_ROM_PATCH4_BITS_SHIFT (0U)

Definition at line 30453 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH5_BITS

#define OCOTP_ROM_PATCH5_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH5_BITS_SHIFT)) & OCOTP_ROM_PATCH5_BITS_MASK)

BITS - BITS

Definition at line 30465 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH5_BITS_MASK

#define OCOTP_ROM_PATCH5_BITS_MASK (0xFFFFFFFFU)

Definition at line 30461 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH5_BITS_SHIFT

#define OCOTP_ROM_PATCH5_BITS_SHIFT (0U)

Definition at line 30462 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH6_BITS

#define OCOTP_ROM_PATCH6_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH6_BITS_SHIFT)) & OCOTP_ROM_PATCH6_BITS_MASK)

BITS - BITS

Definition at line 30474 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH6_BITS_MASK

#define OCOTP_ROM_PATCH6_BITS_MASK (0xFFFFFFFFU)

Definition at line 30470 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH6_BITS_SHIFT

#define OCOTP_ROM_PATCH6_BITS_SHIFT (0U)

Definition at line 30471 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH7_BITS

#define OCOTP_ROM_PATCH7_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_ROM_PATCH7_BITS_SHIFT)) & OCOTP_ROM_PATCH7_BITS_MASK)

BITS - BITS

Definition at line 30483 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH7_BITS_MASK

#define OCOTP_ROM_PATCH7_BITS_MASK (0xFFFFFFFFU)

Definition at line 30479 of file MIMXRT1062.h.

## ◆ OCOTP_ROM_PATCH7_BITS_SHIFT

#define OCOTP_ROM_PATCH7_BITS_SHIFT (0U)

Definition at line 30480 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_HAB_JDE

#define OCOTP_SCS_CLR_HAB_JDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_CLR_HAB_JDE_SHIFT)) & OCOTP_SCS_CLR_HAB_JDE_MASK)

HAB_JDE - HAB_JDE

Definition at line 29779 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_HAB_JDE_MASK

#define OCOTP_SCS_CLR_HAB_JDE_MASK (0x1U)

Definition at line 29775 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_HAB_JDE_SHIFT

#define OCOTP_SCS_CLR_HAB_JDE_SHIFT (0U)

Definition at line 29776 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_LOCK

#define OCOTP_SCS_CLR_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_CLR_LOCK_SHIFT)) & OCOTP_SCS_CLR_LOCK_MASK)

LOCK - LOCK

Definition at line 29789 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_LOCK_MASK

#define OCOTP_SCS_CLR_LOCK_MASK (0x80000000U)

Definition at line 29785 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_LOCK_SHIFT

#define OCOTP_SCS_CLR_LOCK_SHIFT (31U)

Definition at line 29786 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_SPARE

#define OCOTP_SCS_CLR_SPARE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_CLR_SPARE_SHIFT)) & OCOTP_SCS_CLR_SPARE_MASK)

SPARE - SPARE

Definition at line 29784 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_SPARE_MASK

#define OCOTP_SCS_CLR_SPARE_MASK (0x7FFFFFFEU)

Definition at line 29780 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_CLR_SPARE_SHIFT

#define OCOTP_SCS_CLR_SPARE_SHIFT (1U)

Definition at line 29781 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_HAB_JDE

#define OCOTP_SCS_HAB_JDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_HAB_JDE_SHIFT)) & OCOTP_SCS_HAB_JDE_MASK)

HAB_JDE - HAB_JDE

Definition at line 29741 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_HAB_JDE_MASK

#define OCOTP_SCS_HAB_JDE_MASK (0x1U)

Definition at line 29737 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_HAB_JDE_SHIFT

#define OCOTP_SCS_HAB_JDE_SHIFT (0U)

Definition at line 29738 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_LOCK

#define OCOTP_SCS_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_LOCK_SHIFT)) & OCOTP_SCS_LOCK_MASK)

LOCK - LOCK

Definition at line 29751 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_LOCK_MASK

#define OCOTP_SCS_LOCK_MASK (0x80000000U)

Definition at line 29747 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_LOCK_SHIFT

#define OCOTP_SCS_LOCK_SHIFT (31U)

Definition at line 29748 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_HAB_JDE

#define OCOTP_SCS_SET_HAB_JDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SET_HAB_JDE_SHIFT)) & OCOTP_SCS_SET_HAB_JDE_MASK)

HAB_JDE - HAB_JDE

Definition at line 29760 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_HAB_JDE_MASK

#define OCOTP_SCS_SET_HAB_JDE_MASK (0x1U)

Definition at line 29756 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_HAB_JDE_SHIFT

#define OCOTP_SCS_SET_HAB_JDE_SHIFT (0U)

Definition at line 29757 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_LOCK

#define OCOTP_SCS_SET_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SET_LOCK_SHIFT)) & OCOTP_SCS_SET_LOCK_MASK)

LOCK - LOCK

Definition at line 29770 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_LOCK_MASK

#define OCOTP_SCS_SET_LOCK_MASK (0x80000000U)

Definition at line 29766 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_LOCK_SHIFT

#define OCOTP_SCS_SET_LOCK_SHIFT (31U)

Definition at line 29767 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_SPARE

#define OCOTP_SCS_SET_SPARE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SET_SPARE_SHIFT)) & OCOTP_SCS_SET_SPARE_MASK)

SPARE - SPARE

Definition at line 29765 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_SPARE_MASK

#define OCOTP_SCS_SET_SPARE_MASK (0x7FFFFFFEU)

Definition at line 29761 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SET_SPARE_SHIFT

#define OCOTP_SCS_SET_SPARE_SHIFT (1U)

Definition at line 29762 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SPARE

#define OCOTP_SCS_SPARE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_SPARE_SHIFT)) & OCOTP_SCS_SPARE_MASK)

SPARE - SPARE

Definition at line 29746 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SPARE_MASK

#define OCOTP_SCS_SPARE_MASK (0x7FFFFFFEU)

Definition at line 29742 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_SPARE_SHIFT

#define OCOTP_SCS_SPARE_SHIFT (1U)

Definition at line 29743 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_HAB_JDE

#define OCOTP_SCS_TOG_HAB_JDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_TOG_HAB_JDE_SHIFT)) & OCOTP_SCS_TOG_HAB_JDE_MASK)

HAB_JDE - HAB_JDE

Definition at line 29798 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_HAB_JDE_MASK

#define OCOTP_SCS_TOG_HAB_JDE_MASK (0x1U)

Definition at line 29794 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_HAB_JDE_SHIFT

#define OCOTP_SCS_TOG_HAB_JDE_SHIFT (0U)

Definition at line 29795 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_LOCK

#define OCOTP_SCS_TOG_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_TOG_LOCK_SHIFT)) & OCOTP_SCS_TOG_LOCK_MASK)

LOCK - LOCK

Definition at line 29808 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_LOCK_MASK

#define OCOTP_SCS_TOG_LOCK_MASK (0x80000000U)

Definition at line 29804 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_LOCK_SHIFT

#define OCOTP_SCS_TOG_LOCK_SHIFT (31U)

Definition at line 29805 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_SPARE

#define OCOTP_SCS_TOG_SPARE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SCS_TOG_SPARE_SHIFT)) & OCOTP_SCS_TOG_SPARE_MASK)

SPARE - SPARE

Definition at line 29803 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_SPARE_MASK

#define OCOTP_SCS_TOG_SPARE_MASK (0x7FFFFFFEU)

Definition at line 29799 of file MIMXRT1062.h.

## ◆ OCOTP_SCS_TOG_SPARE_SHIFT

#define OCOTP_SCS_TOG_SPARE_SHIFT (1U)

Definition at line 29800 of file MIMXRT1062.h.

## ◆ OCOTP_SJC_RESP0_BITS

#define OCOTP_SJC_RESP0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SJC_RESP0_BITS_SHIFT)) & OCOTP_SJC_RESP0_BITS_MASK)

BITS - BITS

Definition at line 30276 of file MIMXRT1062.h.

## ◆ OCOTP_SJC_RESP0_BITS_MASK

#define OCOTP_SJC_RESP0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30272 of file MIMXRT1062.h.

## ◆ OCOTP_SJC_RESP0_BITS_SHIFT

#define OCOTP_SJC_RESP0_BITS_SHIFT (0U)

Definition at line 30273 of file MIMXRT1062.h.

## ◆ OCOTP_SJC_RESP1_BITS

#define OCOTP_SJC_RESP1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SJC_RESP1_BITS_SHIFT)) & OCOTP_SJC_RESP1_BITS_MASK)

BITS - BITS

Definition at line 30285 of file MIMXRT1062.h.

## ◆ OCOTP_SJC_RESP1_BITS_MASK

#define OCOTP_SJC_RESP1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30281 of file MIMXRT1062.h.

## ◆ OCOTP_SJC_RESP1_BITS_SHIFT

#define OCOTP_SJC_RESP1_BITS_SHIFT (0U)

Definition at line 30282 of file MIMXRT1062.h.

## ◆ OCOTP_SRK0_BITS

#define OCOTP_SRK0_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK0_BITS_SHIFT)) & OCOTP_SRK0_BITS_MASK)

BITS - BITS

Definition at line 30204 of file MIMXRT1062.h.

## ◆ OCOTP_SRK0_BITS_MASK

#define OCOTP_SRK0_BITS_MASK (0xFFFFFFFFU)

Definition at line 30200 of file MIMXRT1062.h.

## ◆ OCOTP_SRK0_BITS_SHIFT

#define OCOTP_SRK0_BITS_SHIFT (0U)

Definition at line 30201 of file MIMXRT1062.h.

## ◆ OCOTP_SRK1_BITS

#define OCOTP_SRK1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK1_BITS_SHIFT)) & OCOTP_SRK1_BITS_MASK)

BITS - BITS

Definition at line 30213 of file MIMXRT1062.h.

## ◆ OCOTP_SRK1_BITS_MASK

#define OCOTP_SRK1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30209 of file MIMXRT1062.h.

## ◆ OCOTP_SRK1_BITS_SHIFT

#define OCOTP_SRK1_BITS_SHIFT (0U)

Definition at line 30210 of file MIMXRT1062.h.

## ◆ OCOTP_SRK2_BITS

#define OCOTP_SRK2_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK2_BITS_SHIFT)) & OCOTP_SRK2_BITS_MASK)

BITS - BITS

Definition at line 30222 of file MIMXRT1062.h.

## ◆ OCOTP_SRK2_BITS_MASK

#define OCOTP_SRK2_BITS_MASK (0xFFFFFFFFU)

Definition at line 30218 of file MIMXRT1062.h.

## ◆ OCOTP_SRK2_BITS_SHIFT

#define OCOTP_SRK2_BITS_SHIFT (0U)

Definition at line 30219 of file MIMXRT1062.h.

## ◆ OCOTP_SRK3_BITS

#define OCOTP_SRK3_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK3_BITS_SHIFT)) & OCOTP_SRK3_BITS_MASK)

BITS - BITS

Definition at line 30231 of file MIMXRT1062.h.

## ◆ OCOTP_SRK3_BITS_MASK

#define OCOTP_SRK3_BITS_MASK (0xFFFFFFFFU)

Definition at line 30227 of file MIMXRT1062.h.

## ◆ OCOTP_SRK3_BITS_SHIFT

#define OCOTP_SRK3_BITS_SHIFT (0U)

Definition at line 30228 of file MIMXRT1062.h.

## ◆ OCOTP_SRK4_BITS

#define OCOTP_SRK4_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK4_BITS_SHIFT)) & OCOTP_SRK4_BITS_MASK)

BITS - BITS

Definition at line 30240 of file MIMXRT1062.h.

## ◆ OCOTP_SRK4_BITS_MASK

#define OCOTP_SRK4_BITS_MASK (0xFFFFFFFFU)

Definition at line 30236 of file MIMXRT1062.h.

## ◆ OCOTP_SRK4_BITS_SHIFT

#define OCOTP_SRK4_BITS_SHIFT (0U)

Definition at line 30237 of file MIMXRT1062.h.

## ◆ OCOTP_SRK5_BITS

#define OCOTP_SRK5_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK5_BITS_SHIFT)) & OCOTP_SRK5_BITS_MASK)

BITS - BITS

Definition at line 30249 of file MIMXRT1062.h.

## ◆ OCOTP_SRK5_BITS_MASK

#define OCOTP_SRK5_BITS_MASK (0xFFFFFFFFU)

Definition at line 30245 of file MIMXRT1062.h.

## ◆ OCOTP_SRK5_BITS_SHIFT

#define OCOTP_SRK5_BITS_SHIFT (0U)

Definition at line 30246 of file MIMXRT1062.h.

## ◆ OCOTP_SRK6_BITS

#define OCOTP_SRK6_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK6_BITS_SHIFT)) & OCOTP_SRK6_BITS_MASK)

BITS - BITS

Definition at line 30258 of file MIMXRT1062.h.

## ◆ OCOTP_SRK6_BITS_MASK

#define OCOTP_SRK6_BITS_MASK (0xFFFFFFFFU)

Definition at line 30254 of file MIMXRT1062.h.

## ◆ OCOTP_SRK6_BITS_SHIFT

#define OCOTP_SRK6_BITS_SHIFT (0U)

Definition at line 30255 of file MIMXRT1062.h.

## ◆ OCOTP_SRK7_BITS

#define OCOTP_SRK7_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK7_BITS_SHIFT)) & OCOTP_SRK7_BITS_MASK)

BITS - BITS

Definition at line 30267 of file MIMXRT1062.h.

## ◆ OCOTP_SRK7_BITS_MASK

#define OCOTP_SRK7_BITS_MASK (0xFFFFFFFFU)

Definition at line 30263 of file MIMXRT1062.h.

## ◆ OCOTP_SRK7_BITS_SHIFT

#define OCOTP_SRK7_BITS_SHIFT (0U)

Definition at line 30264 of file MIMXRT1062.h.

## ◆ OCOTP_SRK_REVOKE_BITS

#define OCOTP_SRK_REVOKE_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SRK_REVOKE_BITS_SHIFT)) & OCOTP_SRK_REVOKE_BITS_MASK)

BITS - BITS

Definition at line 30411 of file MIMXRT1062.h.

## ◆ OCOTP_SRK_REVOKE_BITS_MASK

#define OCOTP_SRK_REVOKE_BITS_MASK (0xFFFFFFFFU)

Definition at line 30407 of file MIMXRT1062.h.

## ◆ OCOTP_SRK_REVOKE_BITS_SHIFT

#define OCOTP_SRK_REVOKE_BITS_SHIFT (0U)

Definition at line 30408 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP1_BITS

#define OCOTP_SW_GP1_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP1_BITS_SHIFT)) & OCOTP_SW_GP1_BITS_MASK)

BITS - BITS

Definition at line 30348 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP1_BITS_MASK

#define OCOTP_SW_GP1_BITS_MASK (0xFFFFFFFFU)

Definition at line 30344 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP1_BITS_SHIFT

#define OCOTP_SW_GP1_BITS_SHIFT (0U)

Definition at line 30345 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP20_BITS

#define OCOTP_SW_GP20_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP20_BITS_SHIFT)) & OCOTP_SW_GP20_BITS_MASK)

BITS - BITS

Definition at line 30357 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP20_BITS_MASK

#define OCOTP_SW_GP20_BITS_MASK (0xFFFFFFFFU)

Definition at line 30353 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP20_BITS_SHIFT

#define OCOTP_SW_GP20_BITS_SHIFT (0U)

Definition at line 30354 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP21_BITS

#define OCOTP_SW_GP21_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP21_BITS_SHIFT)) & OCOTP_SW_GP21_BITS_MASK)

BITS - BITS

Definition at line 30366 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP21_BITS_MASK

#define OCOTP_SW_GP21_BITS_MASK (0xFFFFFFFFU)

Definition at line 30362 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP21_BITS_SHIFT

#define OCOTP_SW_GP21_BITS_SHIFT (0U)

Definition at line 30363 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP22_BITS

#define OCOTP_SW_GP22_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP22_BITS_SHIFT)) & OCOTP_SW_GP22_BITS_MASK)

BITS - BITS

Definition at line 30375 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP22_BITS_MASK

#define OCOTP_SW_GP22_BITS_MASK (0xFFFFFFFFU)

Definition at line 30371 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP22_BITS_SHIFT

#define OCOTP_SW_GP22_BITS_SHIFT (0U)

Definition at line 30372 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP23_BITS

#define OCOTP_SW_GP23_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_GP23_BITS_SHIFT)) & OCOTP_SW_GP23_BITS_MASK)

BITS - BITS

Definition at line 30384 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP23_BITS_MASK

#define OCOTP_SW_GP23_BITS_MASK (0xFFFFFFFFU)

Definition at line 30380 of file MIMXRT1062.h.

## ◆ OCOTP_SW_GP23_BITS_SHIFT

#define OCOTP_SW_GP23_BITS_SHIFT (0U)

Definition at line 30381 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_BLOCK_DTCP_KEY

#define OCOTP_SW_STICKY_BLOCK_DTCP_KEY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_BLOCK_DTCP_KEY_SHIFT)) & OCOTP_SW_STICKY_BLOCK_DTCP_KEY_MASK)

BLOCK_DTCP_KEY - BLOCK_DTCP_KEY

Definition at line 29707 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_BLOCK_DTCP_KEY_MASK

#define OCOTP_SW_STICKY_BLOCK_DTCP_KEY_MASK (0x1U)

Definition at line 29703 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_BLOCK_DTCP_KEY_SHIFT

#define OCOTP_SW_STICKY_BLOCK_DTCP_KEY_SHIFT (0U)

Definition at line 29704 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_BLOCK_ROM_PART

#define OCOTP_SW_STICKY_BLOCK_ROM_PART | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_BLOCK_ROM_PART_SHIFT)) & OCOTP_SW_STICKY_BLOCK_ROM_PART_MASK)

BLOCK_ROM_PART - BLOCK_ROM_PART

Definition at line 29722 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_BLOCK_ROM_PART_MASK

#define OCOTP_SW_STICKY_BLOCK_ROM_PART_MASK (0x8U)

Definition at line 29718 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_BLOCK_ROM_PART_SHIFT

#define OCOTP_SW_STICKY_BLOCK_ROM_PART_SHIFT (3U)

Definition at line 29719 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_FIELD_RETURN_LOCK

#define OCOTP_SW_STICKY_FIELD_RETURN_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_FIELD_RETURN_LOCK_SHIFT)) & OCOTP_SW_STICKY_FIELD_RETURN_LOCK_MASK)

FIELD_RETURN_LOCK - FIELD_RETURN_LOCK

Definition at line 29717 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_FIELD_RETURN_LOCK_MASK

#define OCOTP_SW_STICKY_FIELD_RETURN_LOCK_MASK (0x4U)

Definition at line 29713 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_FIELD_RETURN_LOCK_SHIFT

#define OCOTP_SW_STICKY_FIELD_RETURN_LOCK_SHIFT (2U)

Definition at line 29714 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE

#define OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_SHIFT)) & OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_MASK)

JTAG_BLOCK_RELEASE - JTAG_BLOCK_RELEASE

Definition at line 29727 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_MASK

#define OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_MASK (0x10U)

Definition at line 29723 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_SHIFT

#define OCOTP_SW_STICKY_JTAG_BLOCK_RELEASE_SHIFT (4U)

Definition at line 29724 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_RSVD0

#define OCOTP_SW_STICKY_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_RSVD0_SHIFT)) & OCOTP_SW_STICKY_RSVD0_MASK)

RSVD0 - RSVD0

Definition at line 29732 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_RSVD0_MASK

#define OCOTP_SW_STICKY_RSVD0_MASK (0xFFFFFFE0U)

Definition at line 29728 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_RSVD0_SHIFT

#define OCOTP_SW_STICKY_RSVD0_SHIFT (5U)

Definition at line 29729 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_SRK_REVOKE_LOCK

#define OCOTP_SW_STICKY_SRK_REVOKE_LOCK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_SW_STICKY_SRK_REVOKE_LOCK_SHIFT)) & OCOTP_SW_STICKY_SRK_REVOKE_LOCK_MASK)

SRK_REVOKE_LOCK - SRK_REVOKE_LOCK

Definition at line 29712 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_SRK_REVOKE_LOCK_MASK

#define OCOTP_SW_STICKY_SRK_REVOKE_LOCK_MASK (0x2U)

Definition at line 29708 of file MIMXRT1062.h.

## ◆ OCOTP_SW_STICKY_SRK_REVOKE_LOCK_SHIFT

#define OCOTP_SW_STICKY_SRK_REVOKE_LOCK_SHIFT (1U)

Definition at line 29709 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RELAX_PROG

#define OCOTP_TIMING2_RELAX_PROG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RELAX_PROG_SHIFT)) & OCOTP_TIMING2_RELAX_PROG_MASK)

RELAX_PROG - RELAX_PROG

Definition at line 29874 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RELAX_PROG_MASK

#define OCOTP_TIMING2_RELAX_PROG_MASK (0xFFFU)

Definition at line 29870 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RELAX_PROG_SHIFT

#define OCOTP_TIMING2_RELAX_PROG_SHIFT (0U)

Definition at line 29871 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RELAX_READ

#define OCOTP_TIMING2_RELAX_READ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RELAX_READ_SHIFT)) & OCOTP_TIMING2_RELAX_READ_MASK)

RELAX_READ - RELAX_READ

Definition at line 29884 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RELAX_READ_MASK

#define OCOTP_TIMING2_RELAX_READ_MASK (0x3F0000U)

Definition at line 29880 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RELAX_READ_SHIFT

#define OCOTP_TIMING2_RELAX_READ_SHIFT (16U)

Definition at line 29881 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RSRVD0

#define OCOTP_TIMING2_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RSRVD0_SHIFT)) & OCOTP_TIMING2_RSRVD0_MASK)

RSRVD0 - RSRVD0

Definition at line 29879 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RSRVD0_MASK

#define OCOTP_TIMING2_RSRVD0_MASK (0xF000U)

Definition at line 29875 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RSRVD0_SHIFT

#define OCOTP_TIMING2_RSRVD0_SHIFT (12U)

Definition at line 29876 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RSRVD1

#define OCOTP_TIMING2_RSRVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING2_RSRVD1_SHIFT)) & OCOTP_TIMING2_RSRVD1_MASK)

RSRVD1 - RSRVD0

Definition at line 29889 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RSRVD1_MASK

#define OCOTP_TIMING2_RSRVD1_MASK (0xFFC00000U)

Definition at line 29885 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING2_RSRVD1_SHIFT

#define OCOTP_TIMING2_RSRVD1_SHIFT (22U)

Definition at line 29886 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_RELAX

#define OCOTP_TIMING_RELAX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_RELAX_SHIFT)) & OCOTP_TIMING_RELAX_MASK)

RELAX - RELAX

Definition at line 29651 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_RELAX_MASK

#define OCOTP_TIMING_RELAX_MASK (0xF000U)

Definition at line 29647 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_RELAX_SHIFT

#define OCOTP_TIMING_RELAX_SHIFT (12U)

Definition at line 29648 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_RSRVD0

#define OCOTP_TIMING_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_RSRVD0_SHIFT)) & OCOTP_TIMING_RSRVD0_MASK)

RSRVD0 - RSRVD0

Definition at line 29666 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_RSRVD0_MASK

#define OCOTP_TIMING_RSRVD0_MASK (0xF0000000U)

Definition at line 29662 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_RSRVD0_SHIFT

#define OCOTP_TIMING_RSRVD0_SHIFT (28U)

Definition at line 29663 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_STROBE_PROG

#define OCOTP_TIMING_STROBE_PROG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_STROBE_PROG_SHIFT)) & OCOTP_TIMING_STROBE_PROG_MASK)

STROBE_PROG - STROBE_PROG

Definition at line 29646 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_STROBE_PROG_MASK

#define OCOTP_TIMING_STROBE_PROG_MASK (0xFFFU)

Definition at line 29642 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_STROBE_PROG_SHIFT

#define OCOTP_TIMING_STROBE_PROG_SHIFT (0U)

Definition at line 29643 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_STROBE_READ

#define OCOTP_TIMING_STROBE_READ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_STROBE_READ_SHIFT)) & OCOTP_TIMING_STROBE_READ_MASK)

STROBE_READ - STROBE_READ

Definition at line 29656 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_STROBE_READ_MASK

#define OCOTP_TIMING_STROBE_READ_MASK (0x3F0000U)

Definition at line 29652 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_STROBE_READ_SHIFT

#define OCOTP_TIMING_STROBE_READ_SHIFT (16U)

Definition at line 29653 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_WAIT

#define OCOTP_TIMING_WAIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_TIMING_WAIT_SHIFT)) & OCOTP_TIMING_WAIT_MASK)

WAIT - WAIT

Definition at line 29661 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_WAIT_MASK

#define OCOTP_TIMING_WAIT_MASK (0xFC00000U)

Definition at line 29657 of file MIMXRT1062.h.

## ◆ OCOTP_TIMING_WAIT_SHIFT

#define OCOTP_TIMING_WAIT_SHIFT (22U)

Definition at line 29658 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_MAJOR

#define OCOTP_VERSION_MAJOR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_VERSION_MAJOR_SHIFT)) & OCOTP_VERSION_MAJOR_MASK)

MAJOR - MAJOR

Definition at line 29865 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_MAJOR_MASK

#define OCOTP_VERSION_MAJOR_MASK (0xFF000000U)

Definition at line 29861 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_MAJOR_SHIFT

#define OCOTP_VERSION_MAJOR_SHIFT (24U)

Definition at line 29862 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_MINOR

#define OCOTP_VERSION_MINOR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_VERSION_MINOR_SHIFT)) & OCOTP_VERSION_MINOR_MASK)

MINOR - MINOR

Definition at line 29860 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_MINOR_MASK

#define OCOTP_VERSION_MINOR_MASK (0xFF0000U)

Definition at line 29856 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_MINOR_SHIFT

#define OCOTP_VERSION_MINOR_SHIFT (16U)

Definition at line 29857 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_STEP

#define OCOTP_VERSION_STEP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << OCOTP_VERSION_STEP_SHIFT)) & OCOTP_VERSION_STEP_MASK)

STEP - STEP

Definition at line 29855 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_STEP_MASK

#define OCOTP_VERSION_STEP_MASK (0xFFFFU)

Definition at line 29851 of file MIMXRT1062.h.

## ◆ OCOTP_VERSION_STEP_SHIFT

#define OCOTP_VERSION_STEP_SHIFT (0U)

Definition at line 29852 of file MIMXRT1062.h.