Callisto4Bootloader: I2S_Type Struct Reference

Callisto4Bootloader

Data Fields
I2S_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » I2S Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__I uint32_t | VERID
__I uint32_t | PARAM
__IO uint32_t | TCSR
__IO uint32_t | TCR1
__IO uint32_t | TCR2
__IO uint32_t | TCR3
__IO uint32_t | TCR4
__IO uint32_t | TCR5
__O uint32_t | TDR [4]
uint8_t | RESERVED_0 [16]
__I uint32_t | TFR [4]
uint8_t | RESERVED_1 [16]
__IO uint32_t | TMR
uint8_t | RESERVED_2 [36]
__IO uint32_t | RCSR
__IO uint32_t | RCR1
__IO uint32_t | RCR2
__IO uint32_t | RCR3
__IO uint32_t | RCR4
__IO uint32_t | RCR5
__I uint32_t | RDR [4]
uint8_t | RESERVED_3 [16]
__I uint32_t | RFR [4]
uint8_t | RESERVED_4 [16]
__IO uint32_t | RMR

## Detailed Description

I2S - Register Layout Typedef

Definition at line 21087 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h