Callisto4Bootloader: XTALOSC24M_Type Struct Reference

Callisto4Bootloader

Data Fields
XTALOSC24M_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » XTALOSC24M Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

uint8_t | RESERVED_0 [336]
__IO uint32_t | MISC0
__IO uint32_t | MISC0_SET
__IO uint32_t | MISC0_CLR
__IO uint32_t | MISC0_TOG
uint8_t | RESERVED_1 [272]
__IO uint32_t | LOWPWR_CTRL
__IO uint32_t | LOWPWR_CTRL_SET
__IO uint32_t | LOWPWR_CTRL_CLR
__IO uint32_t | LOWPWR_CTRL_TOG
uint8_t | RESERVED_2 [32]
__IO uint32_t | OSC_CONFIG0
__IO uint32_t | OSC_CONFIG0_SET
__IO uint32_t | OSC_CONFIG0_CLR
__IO uint32_t | OSC_CONFIG0_TOG
__IO uint32_t | OSC_CONFIG1
__IO uint32_t | OSC_CONFIG1_SET
__IO uint32_t | OSC_CONFIG1_CLR
__IO uint32_t | OSC_CONFIG1_TOG
__IO uint32_t | OSC_CONFIG2
__IO uint32_t | OSC_CONFIG2_SET
__IO uint32_t | OSC_CONFIG2_CLR
__IO uint32_t | OSC_CONFIG2_TOG

## Detailed Description

XTALOSC24M - Register Layout Typedef

Definition at line 47553 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h