Callisto4Bootloader: TEMPMON Register Masks

Callisto4Bootloader

TEMPMON Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » TEMPMON Peripheral Access Layer

## TEMPSENSE0 - Tempsensor Control Register 0

#define | TEMPMON_TEMPSENSE0_POWER_DOWN_MASK (0x1U)
#define | TEMPMON_TEMPSENSE0_POWER_DOWN_SHIFT (0U)
#define | TEMPMON_TEMPSENSE0_POWER_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_POWER_DOWN_MASK)
#define | TEMPMON_TEMPSENSE0_MEASURE_TEMP_MASK (0x2U)
#define | TEMPMON_TEMPSENSE0_MEASURE_TEMP_SHIFT (1U)
#define | TEMPMON_TEMPSENSE0_MEASURE_TEMP(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_MEASURE_TEMP_MASK)
#define | TEMPMON_TEMPSENSE0_FINISHED_MASK (0x4U)
#define | TEMPMON_TEMPSENSE0_FINISHED_SHIFT (2U)
#define | TEMPMON_TEMPSENSE0_FINISHED(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_FINISHED_MASK)
#define | TEMPMON_TEMPSENSE0_TEMP_CNT_MASK (0xFFF00U)
#define | TEMPMON_TEMPSENSE0_TEMP_CNT_SHIFT (8U)
#define | TEMPMON_TEMPSENSE0_TEMP_CNT(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_TEMP_CNT_MASK)
#define | TEMPMON_TEMPSENSE0_ALARM_VALUE_MASK (0xFFF00000U)
#define | TEMPMON_TEMPSENSE0_ALARM_VALUE_SHIFT (20U)
#define | TEMPMON_TEMPSENSE0_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_ALARM_VALUE_MASK)

## TEMPSENSE0_SET - Tempsensor Control Register 0

#define | TEMPMON_TEMPSENSE0_SET_POWER_DOWN_MASK (0x1U)
#define | TEMPMON_TEMPSENSE0_SET_POWER_DOWN_SHIFT (0U)
#define | TEMPMON_TEMPSENSE0_SET_POWER_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_SET_POWER_DOWN_MASK)
#define | TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_MASK (0x2U)
#define | TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_SHIFT (1U)
#define | TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_MASK)
#define | TEMPMON_TEMPSENSE0_SET_FINISHED_MASK (0x4U)
#define | TEMPMON_TEMPSENSE0_SET_FINISHED_SHIFT (2U)
#define | TEMPMON_TEMPSENSE0_SET_FINISHED(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_SET_FINISHED_MASK)
#define | TEMPMON_TEMPSENSE0_SET_TEMP_CNT_MASK (0xFFF00U)
#define | TEMPMON_TEMPSENSE0_SET_TEMP_CNT_SHIFT (8U)
#define | TEMPMON_TEMPSENSE0_SET_TEMP_CNT(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_SET_TEMP_CNT_MASK)
#define | TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_MASK (0xFFF00000U)
#define | TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_SHIFT (20U)
#define | TEMPMON_TEMPSENSE0_SET_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_MASK)

## TEMPSENSE0_CLR - Tempsensor Control Register 0

#define | TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_MASK (0x1U)
#define | TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_SHIFT (0U)
#define | TEMPMON_TEMPSENSE0_CLR_POWER_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_MASK)
#define | TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_MASK (0x2U)
#define | TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_SHIFT (1U)
#define | TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_MASK)
#define | TEMPMON_TEMPSENSE0_CLR_FINISHED_MASK (0x4U)
#define | TEMPMON_TEMPSENSE0_CLR_FINISHED_SHIFT (2U)
#define | TEMPMON_TEMPSENSE0_CLR_FINISHED(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_FINISHED_MASK)
#define | TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_MASK (0xFFF00U)
#define | TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_SHIFT (8U)
#define | TEMPMON_TEMPSENSE0_CLR_TEMP_CNT(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_MASK)
#define | TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_MASK (0xFFF00000U)
#define | TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_SHIFT (20U)
#define | TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_MASK)

## TEMPSENSE0_TOG - Tempsensor Control Register 0

#define | TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_MASK (0x1U)
#define | TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_SHIFT (0U)
#define | TEMPMON_TEMPSENSE0_TOG_POWER_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_MASK)
#define | TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_MASK (0x2U)
#define | TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_SHIFT (1U)
#define | TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_MASK)
#define | TEMPMON_TEMPSENSE0_TOG_FINISHED_MASK (0x4U)
#define | TEMPMON_TEMPSENSE0_TOG_FINISHED_SHIFT (2U)
#define | TEMPMON_TEMPSENSE0_TOG_FINISHED(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_FINISHED_MASK)
#define | TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_MASK (0xFFF00U)
#define | TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_SHIFT (8U)
#define | TEMPMON_TEMPSENSE0_TOG_TEMP_CNT(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_MASK)
#define | TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_MASK (0xFFF00000U)
#define | TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_SHIFT (20U)
#define | TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_MASK)

## TEMPSENSE1 - Tempsensor Control Register 1

#define | TEMPMON_TEMPSENSE1_MEASURE_FREQ_MASK (0xFFFFU)
#define | TEMPMON_TEMPSENSE1_MEASURE_FREQ_SHIFT (0U)
#define | TEMPMON_TEMPSENSE1_MEASURE_FREQ(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_MEASURE_FREQ_MASK)

## TEMPSENSE1_SET - Tempsensor Control Register 1

#define | TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_MASK (0xFFFFU)
#define | TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_SHIFT (0U)
#define | TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_MASK)

## TEMPSENSE1_CLR - Tempsensor Control Register 1

#define | TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_MASK (0xFFFFU)
#define | TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_SHIFT (0U)
#define | TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_MASK)

## TEMPSENSE1_TOG - Tempsensor Control Register 1

#define | TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_MASK (0xFFFFU)
#define | TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_SHIFT (0U)
#define | TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_MASK)

## TEMPSENSE2 - Tempsensor Control Register 2

#define | TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_MASK (0xFFFU)
#define | TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_SHIFT (0U)
#define | TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_MASK)
#define | TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_MASK (0xFFF0000U)
#define | TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_SHIFT (16U)
#define | TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_MASK)

## TEMPSENSE2_SET - Tempsensor Control Register 2

#define | TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_MASK (0xFFFU)
#define | TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_SHIFT (0U)
#define | TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_MASK)
#define | TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_MASK (0xFFF0000U)
#define | TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_SHIFT (16U)
#define | TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_MASK)

## TEMPSENSE2_CLR - Tempsensor Control Register 2

#define | TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_MASK (0xFFFU)
#define | TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_SHIFT (0U)
#define | TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_MASK)
#define | TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_MASK (0xFFF0000U)
#define | TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_SHIFT (16U)
#define | TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_MASK)

## TEMPSENSE2_TOG - Tempsensor Control Register 2

#define | TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_MASK (0xFFFU)
#define | TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_SHIFT (0U)
#define | TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_MASK)
#define | TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_MASK (0xFFF0000U)
#define | TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_SHIFT (16U)
#define | TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ TEMPMON_TEMPSENSE0_ALARM_VALUE

#define TEMPMON_TEMPSENSE0_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_ALARM_VALUE_MASK)

Definition at line 39568 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE0_ALARM_VALUE_MASK (0xFFF00000U)

Definition at line 39566 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE0_ALARM_VALUE_SHIFT (20U)

Definition at line 39567 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE

#define TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_MASK)

Definition at line 39630 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_MASK (0xFFF00000U)

Definition at line 39628 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE0_CLR_ALARM_VALUE_SHIFT (20U)

Definition at line 39629 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_FINISHED

#define TEMPMON_TEMPSENSE0_CLR_FINISHED | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_FINISHED_MASK)

FINISHED 0b0..Last measurement is not ready yet. 0b1..Last measurement is valid.

Definition at line 39624 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_FINISHED_MASK

#define TEMPMON_TEMPSENSE0_CLR_FINISHED_MASK (0x4U)

Definition at line 39618 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_FINISHED_SHIFT

#define TEMPMON_TEMPSENSE0_CLR_FINISHED_SHIFT (2U)

Definition at line 39619 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP

#define TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_MASK)

MEASURE_TEMP 0b0..Do not start the measurement process. 0b1..Start the measurement process.

Definition at line 39617 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_MASK

#define TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_MASK (0x2U)

Definition at line 39611 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_SHIFT

#define TEMPMON_TEMPSENSE0_CLR_MEASURE_TEMP_SHIFT (1U)

Definition at line 39612 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_POWER_DOWN

#define TEMPMON_TEMPSENSE0_CLR_POWER_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_MASK)

POWER_DOWN 0b0..Enable power to the temperature sensor. 0b1..Power down the temperature sensor.

Definition at line 39610 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_MASK

#define TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_MASK (0x1U)

Definition at line 39604 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_SHIFT

#define TEMPMON_TEMPSENSE0_CLR_POWER_DOWN_SHIFT (0U)

Definition at line 39605 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_TEMP_CNT

#define TEMPMON_TEMPSENSE0_CLR_TEMP_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_MASK)

Definition at line 39627 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_MASK

#define TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_MASK (0xFFF00U)

Definition at line 39625 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_SHIFT

#define TEMPMON_TEMPSENSE0_CLR_TEMP_CNT_SHIFT (8U)

Definition at line 39626 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_FINISHED

#define TEMPMON_TEMPSENSE0_FINISHED | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_FINISHED_MASK)

FINISHED 0b0..Last measurement is not ready yet. 0b1..Last measurement is valid.

Definition at line 39562 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_FINISHED_MASK

#define TEMPMON_TEMPSENSE0_FINISHED_MASK (0x4U)

Definition at line 39556 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_FINISHED_SHIFT

#define TEMPMON_TEMPSENSE0_FINISHED_SHIFT (2U)

Definition at line 39557 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_MEASURE_TEMP

#define TEMPMON_TEMPSENSE0_MEASURE_TEMP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_MEASURE_TEMP_MASK)

MEASURE_TEMP 0b0..Do not start the measurement process. 0b1..Start the measurement process.

Definition at line 39555 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_MEASURE_TEMP_MASK

#define TEMPMON_TEMPSENSE0_MEASURE_TEMP_MASK (0x2U)

Definition at line 39549 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_MEASURE_TEMP_SHIFT

#define TEMPMON_TEMPSENSE0_MEASURE_TEMP_SHIFT (1U)

Definition at line 39550 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_POWER_DOWN

#define TEMPMON_TEMPSENSE0_POWER_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_POWER_DOWN_MASK)

POWER_DOWN 0b0..Enable power to the temperature sensor. 0b1..Power down the temperature sensor.

Definition at line 39548 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_POWER_DOWN_MASK

#define TEMPMON_TEMPSENSE0_POWER_DOWN_MASK (0x1U)

Definition at line 39542 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_POWER_DOWN_SHIFT

#define TEMPMON_TEMPSENSE0_POWER_DOWN_SHIFT (0U)

Definition at line 39543 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_ALARM_VALUE

#define TEMPMON_TEMPSENSE0_SET_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_MASK)

Definition at line 39599 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_MASK (0xFFF00000U)

Definition at line 39597 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE0_SET_ALARM_VALUE_SHIFT (20U)

Definition at line 39598 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_FINISHED

#define TEMPMON_TEMPSENSE0_SET_FINISHED | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_SET_FINISHED_MASK)

FINISHED 0b0..Last measurement is not ready yet. 0b1..Last measurement is valid.

Definition at line 39593 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_FINISHED_MASK

#define TEMPMON_TEMPSENSE0_SET_FINISHED_MASK (0x4U)

Definition at line 39587 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_FINISHED_SHIFT

#define TEMPMON_TEMPSENSE0_SET_FINISHED_SHIFT (2U)

Definition at line 39588 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP

#define TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_MASK)

MEASURE_TEMP 0b0..Do not start the measurement process. 0b1..Start the measurement process.

Definition at line 39586 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_MASK

#define TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_MASK (0x2U)

Definition at line 39580 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_SHIFT

#define TEMPMON_TEMPSENSE0_SET_MEASURE_TEMP_SHIFT (1U)

Definition at line 39581 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_POWER_DOWN

#define TEMPMON_TEMPSENSE0_SET_POWER_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_SET_POWER_DOWN_MASK)

POWER_DOWN 0b0..Enable power to the temperature sensor. 0b1..Power down the temperature sensor.

Definition at line 39579 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_POWER_DOWN_MASK

#define TEMPMON_TEMPSENSE0_SET_POWER_DOWN_MASK (0x1U)

Definition at line 39573 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_POWER_DOWN_SHIFT

#define TEMPMON_TEMPSENSE0_SET_POWER_DOWN_SHIFT (0U)

Definition at line 39574 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_TEMP_CNT

#define TEMPMON_TEMPSENSE0_SET_TEMP_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_SET_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_SET_TEMP_CNT_MASK)

Definition at line 39596 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_TEMP_CNT_MASK

#define TEMPMON_TEMPSENSE0_SET_TEMP_CNT_MASK (0xFFF00U)

Definition at line 39594 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_SET_TEMP_CNT_SHIFT

#define TEMPMON_TEMPSENSE0_SET_TEMP_CNT_SHIFT (8U)

Definition at line 39595 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TEMP_CNT

#define TEMPMON_TEMPSENSE0_TEMP_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_TEMP_CNT_MASK)

Definition at line 39565 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TEMP_CNT_MASK

#define TEMPMON_TEMPSENSE0_TEMP_CNT_MASK (0xFFF00U)

Definition at line 39563 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TEMP_CNT_SHIFT

#define TEMPMON_TEMPSENSE0_TEMP_CNT_SHIFT (8U)

Definition at line 39564 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE

#define TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_MASK)

Definition at line 39661 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_MASK (0xFFF00000U)

Definition at line 39659 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE0_TOG_ALARM_VALUE_SHIFT (20U)

Definition at line 39660 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_FINISHED

#define TEMPMON_TEMPSENSE0_TOG_FINISHED | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_FINISHED_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_FINISHED_MASK)

FINISHED 0b0..Last measurement is not ready yet. 0b1..Last measurement is valid.

Definition at line 39655 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_FINISHED_MASK

#define TEMPMON_TEMPSENSE0_TOG_FINISHED_MASK (0x4U)

Definition at line 39649 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_FINISHED_SHIFT

#define TEMPMON_TEMPSENSE0_TOG_FINISHED_SHIFT (2U)

Definition at line 39650 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP

#define TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_MASK)

MEASURE_TEMP 0b0..Do not start the measurement process. 0b1..Start the measurement process.

Definition at line 39648 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_MASK

#define TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_MASK (0x2U)

Definition at line 39642 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_SHIFT

#define TEMPMON_TEMPSENSE0_TOG_MEASURE_TEMP_SHIFT (1U)

Definition at line 39643 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_POWER_DOWN

#define TEMPMON_TEMPSENSE0_TOG_POWER_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_MASK)

POWER_DOWN 0b0..Enable power to the temperature sensor. 0b1..Power down the temperature sensor.

Definition at line 39641 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_MASK

#define TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_MASK (0x1U)

Definition at line 39635 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_SHIFT

#define TEMPMON_TEMPSENSE0_TOG_POWER_DOWN_SHIFT (0U)

Definition at line 39636 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_TEMP_CNT

#define TEMPMON_TEMPSENSE0_TOG_TEMP_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_SHIFT)) & TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_MASK)

Definition at line 39658 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_MASK

#define TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_MASK (0xFFF00U)

Definition at line 39656 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_SHIFT

#define TEMPMON_TEMPSENSE0_TOG_TEMP_CNT_SHIFT (8U)

Definition at line 39657 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ

#define TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_MASK)

Definition at line 39682 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_MASK

#define TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_MASK (0xFFFFU)

Definition at line 39680 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_SHIFT

#define TEMPMON_TEMPSENSE1_CLR_MEASURE_FREQ_SHIFT (0U)

Definition at line 39681 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_MEASURE_FREQ

#define TEMPMON_TEMPSENSE1_MEASURE_FREQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_MEASURE_FREQ_MASK)

Definition at line 39668 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_MEASURE_FREQ_MASK

#define TEMPMON_TEMPSENSE1_MEASURE_FREQ_MASK (0xFFFFU)

Definition at line 39666 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_MEASURE_FREQ_SHIFT

#define TEMPMON_TEMPSENSE1_MEASURE_FREQ_SHIFT (0U)

Definition at line 39667 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ

#define TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_MASK)

Definition at line 39675 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_MASK

#define TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_MASK (0xFFFFU)

Definition at line 39673 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_SHIFT

#define TEMPMON_TEMPSENSE1_SET_MEASURE_FREQ_SHIFT (0U)

Definition at line 39674 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ

#define TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_SHIFT)) & TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_MASK)

Definition at line 39689 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_MASK

#define TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_MASK (0xFFFFU)

Definition at line 39687 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_SHIFT

#define TEMPMON_TEMPSENSE1_TOG_MEASURE_FREQ_SHIFT (0U)

Definition at line 39688 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_MASK)

Definition at line 39716 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_MASK (0xFFFU)

Definition at line 39714 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_CLR_LOW_ALARM_VALUE_SHIFT (0U)

Definition at line 39715 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_MASK)

Definition at line 39719 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_MASK (0xFFF0000U)

Definition at line 39717 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_CLR_PANIC_ALARM_VALUE_SHIFT (16U)

Definition at line 39718 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_MASK)

Definition at line 39696 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_MASK (0xFFFU)

Definition at line 39694 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_LOW_ALARM_VALUE_SHIFT (0U)

Definition at line 39695 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_MASK)

Definition at line 39699 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_MASK (0xFFF0000U)

Definition at line 39697 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_PANIC_ALARM_VALUE_SHIFT (16U)

Definition at line 39698 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_MASK)

Definition at line 39706 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_MASK (0xFFFU)

Definition at line 39704 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_SET_LOW_ALARM_VALUE_SHIFT (0U)

Definition at line 39705 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_MASK)

Definition at line 39709 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_MASK (0xFFF0000U)

Definition at line 39707 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_SET_PANIC_ALARM_VALUE_SHIFT (16U)

Definition at line 39708 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_MASK)

Definition at line 39726 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_MASK (0xFFFU)

Definition at line 39724 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_TOG_LOW_ALARM_VALUE_SHIFT (0U)

Definition at line 39725 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE

#define TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_SHIFT)) & TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_MASK)

Definition at line 39729 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_MASK

#define TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_MASK (0xFFF0000U)

Definition at line 39727 of file MIMXRT1062.h.

## ◆ TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_SHIFT

#define TEMPMON_TEMPSENSE2_TOG_PANIC_ALARM_VALUE_SHIFT (16U)

Definition at line 39728 of file MIMXRT1062.h.