Callisto4Bootloader: GPC Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
GPC Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| GPC Register Masks

## Data Structures

struct | GPC_Type

## Macros

#define | GPC_BASE (0x400F4000u)
#define | GPC ((GPC_Type *)GPC_BASE)
#define | GPC_BASE_ADDRS { GPC_BASE }
#define | GPC_BASE_PTRS { GPC }
#define | GPC_IRQS { GPC_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ GPC

#define GPC ((GPC_Type *)GPC_BASE)

Peripheral GPC base pointer

Definition at line 20306 of file MIMXRT1062.h.

## ◆ GPC_BASE

#define GPC_BASE (0x400F4000u)

Peripheral GPC base address

Definition at line 20304 of file MIMXRT1062.h.

## ◆ GPC_BASE_ADDRS

#define GPC_BASE_ADDRS { GPC_BASE }

Array initializer of GPC peripheral base addresses

Definition at line 20308 of file MIMXRT1062.h.

## ◆ GPC_BASE_PTRS

#define GPC_BASE_PTRS { GPC }

Array initializer of GPC peripheral base pointers

Definition at line 20310 of file MIMXRT1062.h.

## ◆ GPC_IRQS

#define GPC_IRQS { GPC_IRQn }

Interrupt vectors for the GPC peripheral type

Definition at line 20312 of file MIMXRT1062.h.