Callisto4Bootloader: BEE_Type Struct Reference

Callisto4Bootloader

Data Fields
BEE_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » BEE Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | CTRL
__IO uint32_t | ADDR_OFFSET0
__IO uint32_t | ADDR_OFFSET1
__IO uint32_t | AES_KEY0_W0
__IO uint32_t | AES_KEY0_W1
__IO uint32_t | AES_KEY0_W2
__IO uint32_t | AES_KEY0_W3
__IO uint32_t | STATUS
__O uint32_t | CTR_NONCE0_W0
__O uint32_t | CTR_NONCE0_W1
__O uint32_t | CTR_NONCE0_W2
__O uint32_t | CTR_NONCE0_W3
__O uint32_t | CTR_NONCE1_W0
__O uint32_t | CTR_NONCE1_W1
__O uint32_t | CTR_NONCE1_W2
__O uint32_t | CTR_NONCE1_W3
__IO uint32_t | REGION1_TOP
__IO uint32_t | REGION1_BOT

## Detailed Description

BEE - Register Layout Typedef

Definition at line 3136 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h