Callisto4Bootloader: USB Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
USB Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| USB Register Masks

## Data Structures

struct | USB_Type

## Macros

#define | USB1_BASE (0x402E0000u)
#define | USB1 ((USB_Type *)USB1_BASE)
#define | USB2_BASE (0x402E0200u)
#define | USB2 ((USB_Type *)USB2_BASE)
#define | USB_BASE_ADDRS { 0u, USB1_BASE, USB2_BASE }
#define | USB_BASE_PTRS { (USB_Type *)0u, USB1, USB2 }
#define | USB_IRQS { NotAvail_IRQn, USB_OTG1_IRQn, USB_OTG2_IRQn }
#define | GPTIMER0CTL GPTIMER0CTRL
#define | GPTIMER1CTL GPTIMER1CTRL
#define | USB_SBUSCFG SBUSCFG
#define | EPLISTADDR ENDPTLISTADDR
#define | EPSETUPSR ENDPTSETUPSTAT
#define | EPPRIME ENDPTPRIME
#define | EPFLUSH ENDPTFLUSH
#define | EPSR ENDPTSTAT
#define | EPCOMPLETE ENDPTCOMPLETE
#define | EPCR ENDPTCTRL
#define | EPCR0 ENDPTCTRL0
#define | USBHS_ID_ID_MASK USB_ID_ID_MASK
#define | USBHS_ID_ID_SHIFT USB_ID_ID_SHIFT
#define | USBHS_ID_ID(x) USB_ID_ID(x)
#define | USBHS_ID_NID_MASK USB_ID_NID_MASK
#define | USBHS_ID_NID_SHIFT USB_ID_NID_SHIFT
#define | USBHS_ID_NID(x) USB_ID_NID(x)
#define | USBHS_ID_REVISION_MASK USB_ID_REVISION_MASK
#define | USBHS_ID_REVISION_SHIFT USB_ID_REVISION_SHIFT
#define | USBHS_ID_REVISION(x) USB_ID_REVISION(x)
#define | USBHS_HWGENERAL_PHYW_MASK USB_HWGENERAL_PHYW_MASK
#define | USBHS_HWGENERAL_PHYW_SHIFT USB_HWGENERAL_PHYW_SHIFT
#define | USBHS_HWGENERAL_PHYW(x) USB_HWGENERAL_PHYW(x)
#define | USBHS_HWGENERAL_PHYM_MASK USB_HWGENERAL_PHYM_MASK
#define | USBHS_HWGENERAL_PHYM_SHIFT USB_HWGENERAL_PHYM_SHIFT
#define | USBHS_HWGENERAL_PHYM(x) USB_HWGENERAL_PHYM(x)
#define | USBHS_HWGENERAL_SM_MASK USB_HWGENERAL_SM_MASK
#define | USBHS_HWGENERAL_SM_SHIFT USB_HWGENERAL_SM_SHIFT
#define | USBHS_HWGENERAL_SM(x) USB_HWGENERAL_SM(x)
#define | USBHS_HWHOST_HC_MASK USB_HWHOST_HC_MASK
#define | USBHS_HWHOST_HC_SHIFT USB_HWHOST_HC_SHIFT
#define | USBHS_HWHOST_HC(x) USB_HWHOST_HC(x)
#define | USBHS_HWHOST_NPORT_MASK USB_HWHOST_NPORT_MASK
#define | USBHS_HWHOST_NPORT_SHIFT USB_HWHOST_NPORT_SHIFT
#define | USBHS_HWHOST_NPORT(x) USB_HWHOST_NPORT(x)
#define | USBHS_HWDEVICE_DC_MASK USB_HWDEVICE_DC_MASK
#define | USBHS_HWDEVICE_DC_SHIFT USB_HWDEVICE_DC_SHIFT
#define | USBHS_HWDEVICE_DC(x) USB_HWDEVICE_DC(x)
#define | USBHS_HWDEVICE_DEVEP_MASK USB_HWDEVICE_DEVEP_MASK
#define | USBHS_HWDEVICE_DEVEP_SHIFT USB_HWDEVICE_DEVEP_SHIFT
#define | USBHS_HWDEVICE_DEVEP(x) USB_HWDEVICE_DEVEP(x)
#define | USBHS_HWTXBUF_TXBURST_MASK USB_HWTXBUF_TXBURST_MASK
#define | USBHS_HWTXBUF_TXBURST_SHIFT USB_HWTXBUF_TXBURST_SHIFT
#define | USBHS_HWTXBUF_TXBURST(x) USB_HWTXBUF_TXBURST(x)
#define | USBHS_HWTXBUF_TXCHANADD_MASK USB_HWTXBUF_TXCHANADD_MASK
#define | USBHS_HWTXBUF_TXCHANADD_SHIFT USB_HWTXBUF_TXCHANADD_SHIFT
#define | USBHS_HWTXBUF_TXCHANADD(x) USB_HWTXBUF_TXCHANADD(x)
#define | USBHS_HWRXBUF_RXBURST_MASK USB_HWRXBUF_RXBURST_MASK
#define | USBHS_HWRXBUF_RXBURST_SHIFT USB_HWRXBUF_RXBURST_SHIFT
#define | USBHS_HWRXBUF_RXBURST(x) USB_HWRXBUF_RXBURST(x)
#define | USBHS_HWRXBUF_RXADD_MASK USB_HWRXBUF_RXADD_MASK
#define | USBHS_HWRXBUF_RXADD_SHIFT USB_HWRXBUF_RXADD_SHIFT
#define | USBHS_HWRXBUF_RXADD(x) USB_HWRXBUF_RXADD(x)
#define | USBHS_GPTIMER0LD_GPTLD_MASK USB_GPTIMER0LD_GPTLD_MASK
#define | USBHS_GPTIMER0LD_GPTLD_SHIFT USB_GPTIMER0LD_GPTLD_SHIFT
#define | USBHS_GPTIMER0LD_GPTLD(x) USB_GPTIMER0LD_GPTLD(x)
#define | USBHS_GPTIMER0CTL_GPTCNT_MASK USB_GPTIMER0CTRL_GPTCNT_MASK
#define | USBHS_GPTIMER0CTL_GPTCNT_SHIFT USB_GPTIMER0CTRL_GPTCNT_SHIFT
#define | USBHS_GPTIMER0CTL_GPTCNT(x) USB_GPTIMER0CTRL_GPTCNT(x)
#define | USBHS_GPTIMER0CTL_MODE_MASK USB_GPTIMER0CTRL_GPTMODE_MASK
#define | USBHS_GPTIMER0CTL_MODE_SHIFT USB_GPTIMER0CTRL_GPTMODE_SHIFT
#define | USBHS_GPTIMER0CTL_MODE(x) USB_GPTIMER0CTRL_GPTMODE(x)
#define | USBHS_GPTIMER0CTL_RST_MASK USB_GPTIMER0CTRL_GPTRST_MASK
#define | USBHS_GPTIMER0CTL_RST_SHIFT USB_GPTIMER0CTRL_GPTRST_SHIFT
#define | USBHS_GPTIMER0CTL_RST(x) USB_GPTIMER0CTRL_GPTRST(x)
#define | USBHS_GPTIMER0CTL_RUN_MASK USB_GPTIMER0CTRL_GPTRUN_MASK
#define | USBHS_GPTIMER0CTL_RUN_SHIFT USB_GPTIMER0CTRL_GPTRUN_SHIFT
#define | USBHS_GPTIMER0CTL_RUN(x) USB_GPTIMER0CTRL_GPTRUN(x)
#define | USBHS_GPTIMER1LD_GPTLD_MASK USB_GPTIMER1LD_GPTLD_MASK
#define | USBHS_GPTIMER1LD_GPTLD_SHIFT USB_GPTIMER1LD_GPTLD_SHIFT
#define | USBHS_GPTIMER1LD_GPTLD(x) USB_GPTIMER1LD_GPTLD(x)
#define | USBHS_GPTIMER1CTL_GPTCNT_MASK USB_GPTIMER1CTRL_GPTCNT_MASK
#define | USBHS_GPTIMER1CTL_GPTCNT_SHIFT USB_GPTIMER1CTRL_GPTCNT_SHIFT
#define | USBHS_GPTIMER1CTL_GPTCNT(x) USB_GPTIMER1CTRL_GPTCNT(x)
#define | USBHS_GPTIMER1CTL_MODE_MASK USB_GPTIMER1CTRL_GPTMODE_MASK
#define | USBHS_GPTIMER1CTL_MODE_SHIFT USB_GPTIMER1CTRL_GPTMODE_SHIFT
#define | USBHS_GPTIMER1CTL_MODE(x) USB_GPTIMER1CTRL_GPTMODE(x)
#define | USBHS_GPTIMER1CTL_RST_MASK USB_GPTIMER1CTRL_GPTRST_MASK
#define | USBHS_GPTIMER1CTL_RST_SHIFT USB_GPTIMER1CTRL_GPTRST_SHIFT
#define | USBHS_GPTIMER1CTL_RST(x) USB_GPTIMER1CTRL_GPTRST(x)
#define | USBHS_GPTIMER1CTL_RUN_MASK USB_GPTIMER1CTRL_GPTRUN_MASK
#define | USBHS_GPTIMER1CTL_RUN_SHIFT USB_GPTIMER1CTRL_GPTRUN_SHIFT
#define | USBHS_GPTIMER1CTL_RUN(x) USB_GPTIMER1CTRL_GPTRUN(x)
#define | USBHS_USB_SBUSCFG_BURSTMODE_MASK USB_SBUSCFG_AHBBRST_MASK
#define | USBHS_USB_SBUSCFG_BURSTMODE_SHIFT USB_SBUSCFG_AHBBRST_SHIFT
#define | USBHS_USB_SBUSCFG_BURSTMODE(x) USB_SBUSCFG_AHBBRST(x)
#define | USBHS_HCIVERSION_CAPLENGTH(x) USB_HCIVERSION_CAPLENGTH(x)
#define | USBHS_HCIVERSION_HCIVERSION_MASK USB_HCIVERSION_HCIVERSION_MASK
#define | USBHS_HCIVERSION_HCIVERSION_SHIFT USB_HCIVERSION_HCIVERSION_SHIFT
#define | USBHS_HCIVERSION_HCIVERSION(x) USB_HCIVERSION_HCIVERSION(x)
#define | USBHS_HCSPARAMS_N_PORTS_MASK USB_HCSPARAMS_N_PORTS_MASK
#define | USBHS_HCSPARAMS_N_PORTS_SHIFT USB_HCSPARAMS_N_PORTS_SHIFT
#define | USBHS_HCSPARAMS_N_PORTS(x) USB_HCSPARAMS_N_PORTS(x)
#define | USBHS_HCSPARAMS_PPC_MASK USB_HCSPARAMS_PPC_MASK
#define | USBHS_HCSPARAMS_PPC_SHIFT USB_HCSPARAMS_PPC_SHIFT
#define | USBHS_HCSPARAMS_PPC(x) USB_HCSPARAMS_PPC(x)
#define | USBHS_HCSPARAMS_N_PCC_MASK USB_HCSPARAMS_N_PCC_MASK
#define | USBHS_HCSPARAMS_N_PCC_SHIFT USB_HCSPARAMS_N_PCC_SHIFT
#define | USBHS_HCSPARAMS_N_PCC(x) USB_HCSPARAMS_N_PCC(x)
#define | USBHS_HCSPARAMS_N_CC_MASK USB_HCSPARAMS_N_CC_MASK
#define | USBHS_HCSPARAMS_N_CC_SHIFT USB_HCSPARAMS_N_CC_SHIFT
#define | USBHS_HCSPARAMS_N_CC(x) USB_HCSPARAMS_N_CC(x)
#define | USBHS_HCSPARAMS_PI_MASK USB_HCSPARAMS_PI_MASK
#define | USBHS_HCSPARAMS_PI_SHIFT USB_HCSPARAMS_PI_SHIFT
#define | USBHS_HCSPARAMS_PI(x) USB_HCSPARAMS_PI(x)
#define | USBHS_HCSPARAMS_N_PTT_MASK USB_HCSPARAMS_N_PTT_MASK
#define | USBHS_HCSPARAMS_N_PTT_SHIFT USB_HCSPARAMS_N_PTT_SHIFT
#define | USBHS_HCSPARAMS_N_PTT(x) USB_HCSPARAMS_N_PTT(x)
#define | USBHS_HCSPARAMS_N_TT_MASK USB_HCSPARAMS_N_TT_MASK
#define | USBHS_HCSPARAMS_N_TT_SHIFT USB_HCSPARAMS_N_TT_SHIFT
#define | USBHS_HCSPARAMS_N_TT(x) USB_HCSPARAMS_N_TT(x)
#define | USBHS_HCCPARAMS_ADC_MASK USB_HCCPARAMS_ADC_MASK
#define | USBHS_HCCPARAMS_ADC_SHIFT USB_HCCPARAMS_ADC_SHIFT
#define | USBHS_HCCPARAMS_ADC(x) USB_HCCPARAMS_ADC(x)
#define | USBHS_HCCPARAMS_PFL_MASK USB_HCCPARAMS_PFL_MASK
#define | USBHS_HCCPARAMS_PFL_SHIFT USB_HCCPARAMS_PFL_SHIFT
#define | USBHS_HCCPARAMS_PFL(x) USB_HCCPARAMS_PFL(x)
#define | USBHS_HCCPARAMS_ASP_MASK USB_HCCPARAMS_ASP_MASK
#define | USBHS_HCCPARAMS_ASP_SHIFT USB_HCCPARAMS_ASP_SHIFT
#define | USBHS_HCCPARAMS_ASP(x) USB_HCCPARAMS_ASP(x)
#define | USBHS_HCCPARAMS_IST_MASK USB_HCCPARAMS_IST_MASK
#define | USBHS_HCCPARAMS_IST_SHIFT USB_HCCPARAMS_IST_SHIFT
#define | USBHS_HCCPARAMS_IST(x) USB_HCCPARAMS_IST(x)
#define | USBHS_HCCPARAMS_EECP_MASK USB_HCCPARAMS_EECP_MASK
#define | USBHS_HCCPARAMS_EECP_SHIFT USB_HCCPARAMS_EECP_SHIFT
#define | USBHS_HCCPARAMS_EECP(x) USB_HCCPARAMS_EECP(x)
#define | USBHS_DCIVERSION_DCIVERSION_MASK USB_DCIVERSION_DCIVERSION_MASK
#define | USBHS_DCIVERSION_DCIVERSION_SHIFT USB_DCIVERSION_DCIVERSION_SHIFT
#define | USBHS_DCIVERSION_DCIVERSION(x) USB_DCIVERSION_DCIVERSION(x)
#define | USBHS_DCCPARAMS_DEN_MASK USB_DCCPARAMS_DEN_MASK
#define | USBHS_DCCPARAMS_DEN_SHIFT USB_DCCPARAMS_DEN_SHIFT
#define | USBHS_DCCPARAMS_DEN(x) USB_DCCPARAMS_DEN(x)
#define | USBHS_DCCPARAMS_DC_MASK USB_DCCPARAMS_DC_MASK
#define | USBHS_DCCPARAMS_DC_SHIFT USB_DCCPARAMS_DC_SHIFT
#define | USBHS_DCCPARAMS_DC(x) USB_DCCPARAMS_DC(x)
#define | USBHS_DCCPARAMS_HC_MASK USB_DCCPARAMS_HC_MASK
#define | USBHS_DCCPARAMS_HC_SHIFT USB_DCCPARAMS_HC_SHIFT
#define | USBHS_DCCPARAMS_HC(x) USB_DCCPARAMS_HC(x)
#define | USBHS_USBCMD_RS_MASK USB_USBCMD_RS_MASK
#define | USBHS_USBCMD_RS_SHIFT USB_USBCMD_RS_SHIFT
#define | USBHS_USBCMD_RS(x) USB_USBCMD_RS(x)
#define | USBHS_USBCMD_RST_MASK USB_USBCMD_RST_MASK
#define | USBHS_USBCMD_RST_SHIFT USB_USBCMD_RST_SHIFT
#define | USBHS_USBCMD_RST(x) USB_USBCMD_RST(x)
#define | USBHS_USBCMD_FS_MASK USB_USBCMD_FS_1_MASK
#define | USBHS_USBCMD_FS_SHIFT USB_USBCMD_FS_1_SHIFT
#define | USBHS_USBCMD_FS(x) USB_USBCMD_FS_1(x)
#define | USBHS_USBCMD_PSE_MASK USB_USBCMD_PSE_MASK
#define | USBHS_USBCMD_PSE_SHIFT USB_USBCMD_PSE_SHIFT
#define | USBHS_USBCMD_PSE(x) USB_USBCMD_PSE(x)
#define | USBHS_USBCMD_ASE_MASK USB_USBCMD_ASE_MASK
#define | USBHS_USBCMD_ASE_SHIFT USB_USBCMD_ASE_SHIFT
#define | USBHS_USBCMD_ASE(x) USB_USBCMD_ASE(x)
#define | USBHS_USBCMD_IAA_MASK USB_USBCMD_IAA_MASK
#define | USBHS_USBCMD_IAA_SHIFT USB_USBCMD_IAA_SHIFT
#define | USBHS_USBCMD_IAA(x) USB_USBCMD_IAA(x)
#define | USBHS_USBCMD_ASP_MASK USB_USBCMD_ASP_MASK
#define | USBHS_USBCMD_ASP_SHIFT USB_USBCMD_ASP_SHIFT
#define | USBHS_USBCMD_ASP(x) USB_USBCMD_ASP(x)
#define | USBHS_USBCMD_ASPE_MASK USB_USBCMD_ASPE_MASK
#define | USBHS_USBCMD_ASPE_SHIFT USB_USBCMD_ASPE_SHIFT
#define | USBHS_USBCMD_ASPE(x) USB_USBCMD_ASPE(x)
#define | USBHS_USBCMD_ATDTW_MASK USB_USBCMD_ATDTW_MASK
#define | USBHS_USBCMD_ATDTW_SHIFT USB_USBCMD_ATDTW_SHIFT
#define | USBHS_USBCMD_ATDTW(x) USB_USBCMD_ATDTW(x)
#define | USBHS_USBCMD_SUTW_MASK USB_USBCMD_SUTW_MASK
#define | USBHS_USBCMD_SUTW_SHIFT USB_USBCMD_SUTW_SHIFT
#define | USBHS_USBCMD_SUTW(x) USB_USBCMD_SUTW(x)
#define | USBHS_USBCMD_FS2_MASK USB_USBCMD_FS_2_MASK
#define | USBHS_USBCMD_FS2_SHIFT USB_USBCMD_FS_2_SHIFT
#define | USBHS_USBCMD_FS2(x) USB_USBCMD_FS_2(x)
#define | USBHS_USBCMD_ITC_MASK USB_USBCMD_ITC_MASK
#define | USBHS_USBCMD_ITC_SHIFT USB_USBCMD_ITC_SHIFT
#define | USBHS_USBCMD_ITC(x) USB_USBCMD_ITC(x)
#define | USBHS_USBSTS_UI_MASK USB_USBSTS_UI_MASK
#define | USBHS_USBSTS_UI_SHIFT USB_USBSTS_UI_SHIFT
#define | USBHS_USBSTS_UI(x) USB_USBSTS_UI(x)
#define | USBHS_USBSTS_UEI_MASK USB_USBSTS_UEI_MASK
#define | USBHS_USBSTS_UEI_SHIFT USB_USBSTS_UEI_SHIFT
#define | USBHS_USBSTS_UEI(x) USB_USBSTS_UEI(x)
#define | USBHS_USBSTS_PCI_MASK USB_USBSTS_PCI_MASK
#define | USBHS_USBSTS_PCI_SHIFT USB_USBSTS_PCI_SHIFT
#define | USBHS_USBSTS_PCI(x) USB_USBSTS_PCI(x)
#define | USBHS_USBSTS_FRI_MASK USB_USBSTS_FRI_MASK
#define | USBHS_USBSTS_FRI_SHIFT USB_USBSTS_FRI_SHIFT
#define | USBHS_USBSTS_FRI(x) USB_USBSTS_FRI(x)
#define | USBHS_USBSTS_SEI_MASK USB_USBSTS_SEI_MASK
#define | USBHS_USBSTS_SEI_SHIFT USB_USBSTS_SEI_SHIFT
#define | USBHS_USBSTS_SEI(x) USB_USBSTS_SEI(x)
#define | USBHS_USBSTS_AAI_MASK USB_USBSTS_AAI_MASK
#define | USBHS_USBSTS_AAI_SHIFT USB_USBSTS_AAI_SHIFT
#define | USBHS_USBSTS_AAI(x) USB_USBSTS_AAI(x)
#define | USBHS_USBSTS_URI_MASK USB_USBSTS_URI_MASK
#define | USBHS_USBSTS_URI_SHIFT USB_USBSTS_URI_SHIFT
#define | USBHS_USBSTS_URI(x) USB_USBSTS_URI(x)
#define | USBHS_USBSTS_SRI_MASK USB_USBSTS_SRI_MASK
#define | USBHS_USBSTS_SRI_SHIFT USB_USBSTS_SRI_SHIFT
#define | USBHS_USBSTS_SRI(x) USB_USBSTS_SRI(x)
#define | USBHS_USBSTS_SLI_MASK USB_USBSTS_SLI_MASK
#define | USBHS_USBSTS_SLI_SHIFT USB_USBSTS_SLI_SHIFT
#define | USBHS_USBSTS_SLI(x) USB_USBSTS_SLI(x)
#define | USBHS_USBSTS_ULPII_MASK USB_USBSTS_ULPII_MASK
#define | USBHS_USBSTS_ULPII_SHIFT USB_USBSTS_ULPII_SHIFT
#define | USBHS_USBSTS_ULPII(x) USB_USBSTS_ULPII(x)
#define | USBHS_USBSTS_HCH_MASK USB_USBSTS_HCH_MASK
#define | USBHS_USBSTS_HCH_SHIFT USB_USBSTS_HCH_SHIFT
#define | USBHS_USBSTS_HCH(x) USB_USBSTS_HCH(x)
#define | USBHS_USBSTS_RCL_MASK USB_USBSTS_RCL_MASK
#define | USBHS_USBSTS_RCL_SHIFT USB_USBSTS_RCL_SHIFT
#define | USBHS_USBSTS_RCL(x) USB_USBSTS_RCL(x)
#define | USBHS_USBSTS_PS_MASK USB_USBSTS_PS_MASK
#define | USBHS_USBSTS_PS_SHIFT USB_USBSTS_PS_SHIFT
#define | USBHS_USBSTS_PS(x) USB_USBSTS_PS(x)
#define | USBHS_USBSTS_AS_MASK USB_USBSTS_AS_MASK
#define | USBHS_USBSTS_AS_SHIFT USB_USBSTS_AS_SHIFT
#define | USBHS_USBSTS_AS(x) USB_USBSTS_AS(x)
#define | USBHS_USBSTS_NAKI_MASK USB_USBSTS_NAKI_MASK
#define | USBHS_USBSTS_NAKI_SHIFT USB_USBSTS_NAKI_SHIFT
#define | USBHS_USBSTS_NAKI(x) USB_USBSTS_NAKI(x)
#define | USBHS_USBSTS_TI0_MASK USB_USBSTS_TI0_MASK
#define | USBHS_USBSTS_TI0_SHIFT USB_USBSTS_TI0_SHIFT
#define | USBHS_USBSTS_TI0(x) USB_USBSTS_TI0(x)
#define | USBHS_USBSTS_TI1_MASK USB_USBSTS_TI1_MASK
#define | USBHS_USBSTS_TI1_SHIFT USB_USBSTS_TI1_SHIFT
#define | USBHS_USBSTS_TI1(x) USB_USBSTS_TI1(x)
#define | USBHS_USBINTR_UE_MASK USB_USBINTR_UE_MASK
#define | USBHS_USBINTR_UE_SHIFT USB_USBINTR_UE_SHIFT
#define | USBHS_USBINTR_UE(x) USB_USBINTR_UE(x)
#define | USBHS_USBINTR_UEE_MASK USB_USBINTR_UEE_MASK
#define | USBHS_USBINTR_UEE_SHIFT USB_USBINTR_UEE_SHIFT
#define | USBHS_USBINTR_UEE(x) USB_USBINTR_UEE(x)
#define | USBHS_USBINTR_PCE_MASK USB_USBINTR_PCE_MASK
#define | USBHS_USBINTR_PCE_SHIFT USB_USBINTR_PCE_SHIFT
#define | USBHS_USBINTR_PCE(x) USB_USBINTR_PCE(x)
#define | USBHS_USBINTR_FRE_MASK USB_USBINTR_FRE_MASK
#define | USBHS_USBINTR_FRE_SHIFT USB_USBINTR_FRE_SHIFT
#define | USBHS_USBINTR_FRE(x) USB_USBINTR_FRE(x)
#define | USBHS_USBINTR_SEE_MASK USB_USBINTR_SEE_MASK
#define | USBHS_USBINTR_SEE_SHIFT USB_USBINTR_SEE_SHIFT
#define | USBHS_USBINTR_SEE(x) USB_USBINTR_SEE(x)
#define | USBHS_USBINTR_AAE_MASK USB_USBINTR_AAE_MASK
#define | USBHS_USBINTR_AAE_SHIFT USB_USBINTR_AAE_SHIFT
#define | USBHS_USBINTR_AAE(x) USB_USBINTR_AAE(x)
#define | USBHS_USBINTR_URE_MASK USB_USBINTR_URE_MASK
#define | USBHS_USBINTR_URE_SHIFT USB_USBINTR_URE_SHIFT
#define | USBHS_USBINTR_URE(x) USB_USBINTR_URE(x)
#define | USBHS_USBINTR_SRE_MASK USB_USBINTR_SRE_MASK
#define | USBHS_USBINTR_SRE_SHIFT USB_USBINTR_SRE_SHIFT
#define | USBHS_USBINTR_SRE(x) USB_USBINTR_SRE(x)
#define | USBHS_USBINTR_SLE_MASK USB_USBINTR_SLE_MASK
#define | USBHS_USBINTR_SLE_SHIFT USB_USBINTR_SLE_SHIFT
#define | USBHS_USBINTR_SLE(x) USB_USBINTR_SLE(x)
#define | USBHS_USBINTR_ULPIE_MASK USB_USBINTR_ULPIE_MASK
#define | USBHS_USBINTR_ULPIE_SHIFT USB_USBINTR_ULPIE_SHIFT
#define | USBHS_USBINTR_ULPIE(x) USB_USBINTR_ULPIE(x)
#define | USBHS_USBINTR_NAKE_MASK USB_USBINTR_NAKE_MASK
#define | USBHS_USBINTR_NAKE_SHIFT USB_USBINTR_NAKE_SHIFT
#define | USBHS_USBINTR_NAKE(x) USB_USBINTR_NAKE(x)
#define | USBHS_USBINTR_UAIE_MASK USB_USBINTR_UAIE_MASK
#define | USBHS_USBINTR_UAIE_SHIFT USB_USBINTR_UAIE_SHIFT
#define | USBHS_USBINTR_UAIE(x) USB_USBINTR_UAIE(x)
#define | USBHS_USBINTR_UPIE_MASK USB_USBINTR_UPIE_MASK
#define | USBHS_USBINTR_UPIE_SHIFT USB_USBINTR_UPIE_SHIFT
#define | USBHS_USBINTR_UPIE(x) USB_USBINTR_UPIE(x)
#define | USBHS_USBINTR_TIE0_MASK USB_USBINTR_TIE0_MASK
#define | USBHS_USBINTR_TIE0_SHIFT USB_USBINTR_TIE0_SHIFT
#define | USBHS_USBINTR_TIE0(x) USB_USBINTR_TIE0(x)
#define | USBHS_USBINTR_TIE1_MASK USB_USBINTR_TIE1_MASK
#define | USBHS_USBINTR_TIE1_SHIFT USB_USBINTR_TIE1_SHIFT
#define | USBHS_USBINTR_TIE1(x) USB_USBINTR_TIE1(x)
#define | USBHS_FRINDEX_FRINDEX_MASK USB_FRINDEX_FRINDEX_MASK
#define | USBHS_FRINDEX_FRINDEX_SHIFT USB_FRINDEX_FRINDEX_SHIFT
#define | USBHS_FRINDEX_FRINDEX(x) USB_FRINDEX_FRINDEX(x)
#define | USBHS_DEVICEADDR_USBADRA_MASK USB_DEVICEADDR_USBADRA_MASK
#define | USBHS_DEVICEADDR_USBADRA_SHIFT USB_DEVICEADDR_USBADRA_SHIFT
#define | USBHS_DEVICEADDR_USBADRA(x) USB_DEVICEADDR_USBADRA(x)
#define | USBHS_DEVICEADDR_USBADR_MASK USB_DEVICEADDR_USBADR_MASK
#define | USBHS_DEVICEADDR_USBADR_SHIFT USB_DEVICEADDR_USBADR_SHIFT
#define | USBHS_DEVICEADDR_USBADR(x) USB_DEVICEADDR_USBADR(x)
#define | USBHS_PERIODICLISTBASE_PERBASE_MASK USB_PERIODICLISTBASE_BASEADR_MASK
#define | USBHS_PERIODICLISTBASE_PERBASE_SHIFT USB_PERIODICLISTBASE_BASEADR_SHIFT
#define | USBHS_PERIODICLISTBASE_PERBASE(x) USB_PERIODICLISTBASE_BASEADR(x)
#define | USBHS_ASYNCLISTADDR_ASYBASE_MASK USB_ASYNCLISTADDR_ASYBASE_MASK
#define | USBHS_ASYNCLISTADDR_ASYBASE_SHIFT USB_ASYNCLISTADDR_ASYBASE_SHIFT
#define | USBHS_ASYNCLISTADDR_ASYBASE(x) USB_ASYNCLISTADDR_ASYBASE(x)
#define | USBHS_EPLISTADDR_EPBASE_MASK USB_ENDPTLISTADDR_EPBASE_MASK
#define | USBHS_EPLISTADDR_EPBASE_SHIFT USB_ENDPTLISTADDR_EPBASE_SHIFT
#define | USBHS_EPLISTADDR_EPBASE(x) USB_ENDPTLISTADDR_EPBASE(x)
#define | USBHS_BURSTSIZE_RXPBURST_MASK USB_BURSTSIZE_RXPBURST_MASK
#define | USBHS_BURSTSIZE_RXPBURST_SHIFT USB_BURSTSIZE_RXPBURST_SHIFT
#define | USBHS_BURSTSIZE_RXPBURST(x) USB_BURSTSIZE_RXPBURST(x)
#define | USBHS_BURSTSIZE_TXPBURST_MASK USB_BURSTSIZE_TXPBURST_MASK
#define | USBHS_BURSTSIZE_TXPBURST_SHIFT USB_BURSTSIZE_TXPBURST_SHIFT
#define | USBHS_BURSTSIZE_TXPBURST(x) USB_BURSTSIZE_TXPBURST(x)
#define | USBHS_TXFILLTUNING_TXSCHOH_MASK USB_TXFILLTUNING_TXSCHOH_MASK
#define | USBHS_TXFILLTUNING_TXSCHOH_SHIFT USB_TXFILLTUNING_TXSCHOH_SHIFT
#define | USBHS_TXFILLTUNING_TXSCHOH(x) USB_TXFILLTUNING_TXSCHOH(x)
#define | USBHS_TXFILLTUNING_TXSCHHEALTH_MASK USB_TXFILLTUNING_TXSCHHEALTH_MASK
#define | USBHS_TXFILLTUNING_TXSCHHEALTH_SHIFT USB_TXFILLTUNING_TXSCHHEALTH_SHIFT
#define | USBHS_TXFILLTUNING_TXSCHHEALTH(x) USB_TXFILLTUNING_TXSCHHEALTH(x)
#define | USBHS_TXFILLTUNING_TXFIFOTHRES_MASK USB_TXFILLTUNING_TXFIFOTHRES_MASK
#define | USBHS_TXFILLTUNING_TXFIFOTHRES_SHIFT USB_TXFILLTUNING_TXFIFOTHRES_SHIFT
#define | USBHS_TXFILLTUNING_TXFIFOTHRES(x) USB_TXFILLTUNING_TXFIFOTHRES(x)
#define | USBHS_ENDPTNAK_EPRN_MASK USB_ENDPTNAK_EPRN_MASK
#define | USBHS_ENDPTNAK_EPRN_SHIFT USB_ENDPTNAK_EPRN_SHIFT
#define | USBHS_ENDPTNAK_EPRN(x) USB_ENDPTNAK_EPRN(x)
#define | USBHS_ENDPTNAK_EPTN_MASK USB_ENDPTNAK_EPTN_MASK
#define | USBHS_ENDPTNAK_EPTN_SHIFT USB_ENDPTNAK_EPTN_SHIFT
#define | USBHS_ENDPTNAK_EPTN(x) USB_ENDPTNAK_EPTN(x)
#define | USBHS_ENDPTNAKEN_EPRNE_MASK USB_ENDPTNAKEN_EPRNE_MASK
#define | USBHS_ENDPTNAKEN_EPRNE_SHIFT USB_ENDPTNAKEN_EPRNE_SHIFT
#define | USBHS_ENDPTNAKEN_EPRNE(x) USB_ENDPTNAKEN_EPRNE(x)
#define | USBHS_ENDPTNAKEN_EPTNE_MASK USB_ENDPTNAKEN_EPTNE_MASK
#define | USBHS_ENDPTNAKEN_EPTNE_SHIFT USB_ENDPTNAKEN_EPTNE_SHIFT
#define | USBHS_ENDPTNAKEN_EPTNE(x) USB_ENDPTNAKEN_EPTNE(x)
#define | USBHS_CONFIGFLAG_CF_MASK USB_CONFIGFLAG_CF_MASK
#define | USBHS_CONFIGFLAG_CF_SHIFT USB_CONFIGFLAG_CF_SHIFT
#define | USBHS_CONFIGFLAG_CF(x) USB_CONFIGFLAG_CF(x)
#define | USBHS_PORTSC1_CCS_MASK USB_PORTSC1_CCS_MASK
#define | USBHS_PORTSC1_CCS_SHIFT USB_PORTSC1_CCS_SHIFT
#define | USBHS_PORTSC1_CCS(x) USB_PORTSC1_CCS(x)
#define | USBHS_PORTSC1_CSC_MASK USB_PORTSC1_CSC_MASK
#define | USBHS_PORTSC1_CSC_SHIFT USB_PORTSC1_CSC_SHIFT
#define | USBHS_PORTSC1_CSC(x) USB_PORTSC1_CSC(x)
#define | USBHS_PORTSC1_PE_MASK USB_PORTSC1_PE_MASK
#define | USBHS_PORTSC1_PE_SHIFT USB_PORTSC1_PE_SHIFT
#define | USBHS_PORTSC1_PE(x) USB_PORTSC1_PE(x)
#define | USBHS_PORTSC1_PEC_MASK USB_PORTSC1_PEC_MASK
#define | USBHS_PORTSC1_PEC_SHIFT USB_PORTSC1_PEC_SHIFT
#define | USBHS_PORTSC1_PEC(x) USB_PORTSC1_PEC(x)
#define | USBHS_PORTSC1_OCA_MASK USB_PORTSC1_OCA_MASK
#define | USBHS_PORTSC1_OCA_SHIFT USB_PORTSC1_OCA_SHIFT
#define | USBHS_PORTSC1_OCA(x) USB_PORTSC1_OCA(x)
#define | USBHS_PORTSC1_OCC_MASK USB_PORTSC1_OCC_MASK
#define | USBHS_PORTSC1_OCC_SHIFT USB_PORTSC1_OCC_SHIFT
#define | USBHS_PORTSC1_OCC(x) USB_PORTSC1_OCC(x)
#define | USBHS_PORTSC1_FPR_MASK USB_PORTSC1_FPR_MASK
#define | USBHS_PORTSC1_FPR_SHIFT USB_PORTSC1_FPR_SHIFT
#define | USBHS_PORTSC1_FPR(x) USB_PORTSC1_FPR(x)
#define | USBHS_PORTSC1_SUSP_MASK USB_PORTSC1_SUSP_MASK
#define | USBHS_PORTSC1_SUSP_SHIFT USB_PORTSC1_SUSP_SHIFT
#define | USBHS_PORTSC1_SUSP(x) USB_PORTSC1_SUSP(x)
#define | USBHS_PORTSC1_PR_MASK USB_PORTSC1_PR_MASK
#define | USBHS_PORTSC1_PR_SHIFT USB_PORTSC1_PR_SHIFT
#define | USBHS_PORTSC1_PR(x) USB_PORTSC1_PR(x)
#define | USBHS_PORTSC1_HSP_MASK USB_PORTSC1_HSP_MASK
#define | USBHS_PORTSC1_HSP_SHIFT USB_PORTSC1_HSP_SHIFT
#define | USBHS_PORTSC1_HSP(x) USB_PORTSC1_HSP(x)
#define | USBHS_PORTSC1_LS_MASK USB_PORTSC1_LS_MASK
#define | USBHS_PORTSC1_LS_SHIFT USB_PORTSC1_LS_SHIFT
#define | USBHS_PORTSC1_LS(x) USB_PORTSC1_LS(x)
#define | USBHS_PORTSC1_PP_MASK USB_PORTSC1_PP_MASK
#define | USBHS_PORTSC1_PP_SHIFT USB_PORTSC1_PP_SHIFT
#define | USBHS_PORTSC1_PP(x) USB_PORTSC1_PP(x)
#define | USBHS_PORTSC1_PO_MASK USB_PORTSC1_PO_MASK
#define | USBHS_PORTSC1_PO_SHIFT USB_PORTSC1_PO_SHIFT
#define | USBHS_PORTSC1_PO(x) USB_PORTSC1_PO(x)
#define | USBHS_PORTSC1_PIC_MASK USB_PORTSC1_PIC_MASK
#define | USBHS_PORTSC1_PIC_SHIFT USB_PORTSC1_PIC_SHIFT
#define | USBHS_PORTSC1_PIC(x) USB_PORTSC1_PIC(x)
#define | USBHS_PORTSC1_PTC_MASK USB_PORTSC1_PTC_MASK
#define | USBHS_PORTSC1_PTC_SHIFT USB_PORTSC1_PTC_SHIFT
#define | USBHS_PORTSC1_PTC(x) USB_PORTSC1_PTC(x)
#define | USBHS_PORTSC1_WKCN_MASK USB_PORTSC1_WKCN_MASK
#define | USBHS_PORTSC1_WKCN_SHIFT USB_PORTSC1_WKCN_SHIFT
#define | USBHS_PORTSC1_WKCN(x) USB_PORTSC1_WKCN(x)
#define | USBHS_PORTSC1_WKDS_MASK USB_PORTSC1_WKDC_MASK
#define | USBHS_PORTSC1_WKDS_SHIFT USB_PORTSC1_WKDC_SHIFT
#define | USBHS_PORTSC1_WKDS(x) USB_PORTSC1_WKDC(x)
#define | USBHS_PORTSC1_WKOC_MASK USB_PORTSC1_WKOC_MASK
#define | USBHS_PORTSC1_WKOC_SHIFT USB_PORTSC1_WKOC_SHIFT
#define | USBHS_PORTSC1_WKOC(x) USB_PORTSC1_WKOC(x)
#define | USBHS_PORTSC1_PHCD_MASK USB_PORTSC1_PHCD_MASK
#define | USBHS_PORTSC1_PHCD_SHIFT USB_PORTSC1_PHCD_SHIFT
#define | USBHS_PORTSC1_PHCD(x) USB_PORTSC1_PHCD(x)
#define | USBHS_PORTSC1_PFSC_MASK USB_PORTSC1_PFSC_MASK
#define | USBHS_PORTSC1_PFSC_SHIFT USB_PORTSC1_PFSC_SHIFT
#define | USBHS_PORTSC1_PFSC(x) USB_PORTSC1_PFSC(x)
#define | USBHS_PORTSC1_PTS2_MASK USB_PORTSC1_PTS_2_MASK
#define | USBHS_PORTSC1_PTS2_SHIFT USB_PORTSC1_PTS_2_SHIFT
#define | USBHS_PORTSC1_PTS2(x) USB_PORTSC1_PTS_2(x)
#define | USBHS_PORTSC1_PSPD_MASK USB_PORTSC1_PSPD_MASK
#define | USBHS_PORTSC1_PSPD_SHIFT USB_PORTSC1_PSPD_SHIFT
#define | USBHS_PORTSC1_PSPD(x) USB_PORTSC1_PSPD(x)
#define | USBHS_PORTSC1_PTW_MASK USB_PORTSC1_PTW_MASK
#define | USBHS_PORTSC1_PTW_SHIFT USB_PORTSC1_PTW_SHIFT
#define | USBHS_PORTSC1_PTW(x) USB_PORTSC1_PTW(x)
#define | USBHS_PORTSC1_STS_MASK USB_PORTSC1_STS_MASK
#define | USBHS_PORTSC1_STS_SHIFT USB_PORTSC1_STS_SHIFT
#define | USBHS_PORTSC1_STS(x) USB_PORTSC1_STS(x)
#define | USBHS_PORTSC1_PTS_MASK USB_PORTSC1_PTS_1_MASK
#define | USBHS_PORTSC1_PTS_SHIFT USB_PORTSC1_PTS_1_SHIFT
#define | USBHS_PORTSC1_PTS(x) USB_PORTSC1_PTS_1(x)
#define | USBHS_OTGSC_VD_MASK USB_OTGSC_VD_MASK
#define | USBHS_OTGSC_VD_SHIFT USB_OTGSC_VD_SHIFT
#define | USBHS_OTGSC_VD(x) USB_OTGSC_VD(x)
#define | USBHS_OTGSC_VC_MASK USB_OTGSC_VC_MASK
#define | USBHS_OTGSC_VC_SHIFT USB_OTGSC_VC_SHIFT
#define | USBHS_OTGSC_VC(x) USB_OTGSC_VC(x)
#define | USBHS_OTGSC_OT_MASK USB_OTGSC_OT_MASK
#define | USBHS_OTGSC_OT_SHIFT USB_OTGSC_OT_SHIFT
#define | USBHS_OTGSC_OT(x) USB_OTGSC_OT(x)
#define | USBHS_OTGSC_DP_MASK USB_OTGSC_DP_MASK
#define | USBHS_OTGSC_DP_SHIFT USB_OTGSC_DP_SHIFT
#define | USBHS_OTGSC_DP(x) USB_OTGSC_DP(x)
#define | USBHS_OTGSC_IDPU_MASK USB_OTGSC_IDPU_MASK
#define | USBHS_OTGSC_IDPU_SHIFT USB_OTGSC_IDPU_SHIFT
#define | USBHS_OTGSC_IDPU(x) USB_OTGSC_IDPU(x)
#define | USBHS_OTGSC_ID_MASK USB_OTGSC_ID_MASK
#define | USBHS_OTGSC_ID_SHIFT USB_OTGSC_ID_SHIFT
#define | USBHS_OTGSC_ID(x) USB_OTGSC_ID(x)
#define | USBHS_OTGSC_AVV_MASK USB_OTGSC_AVV_MASK
#define | USBHS_OTGSC_AVV_SHIFT USB_OTGSC_AVV_SHIFT
#define | USBHS_OTGSC_AVV(x) USB_OTGSC_AVV(x)
#define | USBHS_OTGSC_ASV_MASK USB_OTGSC_ASV_MASK
#define | USBHS_OTGSC_ASV_SHIFT USB_OTGSC_ASV_SHIFT
#define | USBHS_OTGSC_ASV(x) USB_OTGSC_ASV(x)
#define | USBHS_OTGSC_BSV_MASK USB_OTGSC_BSV_MASK
#define | USBHS_OTGSC_BSV_SHIFT USB_OTGSC_BSV_SHIFT
#define | USBHS_OTGSC_BSV(x) USB_OTGSC_BSV(x)
#define | USBHS_OTGSC_BSE_MASK USB_OTGSC_BSE_MASK
#define | USBHS_OTGSC_BSE_SHIFT USB_OTGSC_BSE_SHIFT
#define | USBHS_OTGSC_BSE(x) USB_OTGSC_BSE(x)
#define | USBHS_OTGSC_MST_MASK USB_OTGSC_TOG_1MS_MASK
#define | USBHS_OTGSC_MST_SHIFT USB_OTGSC_TOG_1MS_SHIFT
#define | USBHS_OTGSC_MST(x) USB_OTGSC_TOG_1MS(x)
#define | USBHS_OTGSC_DPS_MASK USB_OTGSC_DPS_MASK
#define | USBHS_OTGSC_DPS_SHIFT USB_OTGSC_DPS_SHIFT
#define | USBHS_OTGSC_DPS(x) USB_OTGSC_DPS(x)
#define | USBHS_OTGSC_IDIS_MASK USB_OTGSC_IDIS_MASK
#define | USBHS_OTGSC_IDIS_SHIFT USB_OTGSC_IDIS_SHIFT
#define | USBHS_OTGSC_IDIS(x) USB_OTGSC_IDIS(x)
#define | USBHS_OTGSC_AVVIS_MASK USB_OTGSC_AVVIS_MASK
#define | USBHS_OTGSC_AVVIS_SHIFT USB_OTGSC_AVVIS_SHIFT
#define | USBHS_OTGSC_AVVIS(x) USB_OTGSC_AVVIS(x)
#define | USBHS_OTGSC_ASVIS_MASK USB_OTGSC_ASVIS_MASK
#define | USBHS_OTGSC_ASVIS_SHIFT USB_OTGSC_ASVIS_SHIFT
#define | USBHS_OTGSC_ASVIS(x) USB_OTGSC_ASVIS(x)
#define | USBHS_OTGSC_BSVIS_MASK USB_OTGSC_BSVIS_MASK
#define | USBHS_OTGSC_BSVIS_SHIFT USB_OTGSC_BSVIS_SHIFT
#define | USBHS_OTGSC_BSVIS(x) USB_OTGSC_BSVIS(x)
#define | USBHS_OTGSC_BSEIS_MASK USB_OTGSC_BSEIS_MASK
#define | USBHS_OTGSC_BSEIS_SHIFT USB_OTGSC_BSEIS_SHIFT
#define | USBHS_OTGSC_BSEIS(x) USB_OTGSC_BSEIS(x)
#define | USBHS_OTGSC_MSS_MASK USB_OTGSC_STATUS_1MS_MASK
#define | USBHS_OTGSC_MSS_SHIFT USB_OTGSC_STATUS_1MS_SHIFT
#define | USBHS_OTGSC_MSS(x) USB_OTGSC_STATUS_1MS(x)
#define | USBHS_OTGSC_DPIS_MASK USB_OTGSC_DPIS_MASK
#define | USBHS_OTGSC_DPIS_SHIFT USB_OTGSC_DPIS_SHIFT
#define | USBHS_OTGSC_DPIS(x) USB_OTGSC_DPIS(x)
#define | USBHS_OTGSC_IDIE_MASK USB_OTGSC_IDIE_MASK
#define | USBHS_OTGSC_IDIE_SHIFT USB_OTGSC_IDIE_SHIFT
#define | USBHS_OTGSC_IDIE(x) USB_OTGSC_IDIE(x)
#define | USBHS_OTGSC_AVVIE_MASK USB_OTGSC_AVVIE_MASK
#define | USBHS_OTGSC_AVVIE_SHIFT USB_OTGSC_AVVIE_SHIFT
#define | USBHS_OTGSC_AVVIE(x) USB_OTGSC_AVVIE(x)
#define | USBHS_OTGSC_ASVIE_MASK USB_OTGSC_ASVIE_MASK
#define | USBHS_OTGSC_ASVIE_SHIFT USB_OTGSC_ASVIE_SHIFT
#define | USBHS_OTGSC_ASVIE(x) USB_OTGSC_ASVIE(x)
#define | USBHS_OTGSC_BSVIE_MASK USB_OTGSC_BSVIE_MASK
#define | USBHS_OTGSC_BSVIE_SHIFT USB_OTGSC_BSVIE_SHIFT
#define | USBHS_OTGSC_BSVIE(x) USB_OTGSC_BSVIE(x)
#define | USBHS_OTGSC_BSEIE_MASK USB_OTGSC_BSEIE_MASK
#define | USBHS_OTGSC_BSEIE_SHIFT USB_OTGSC_BSEIE_SHIFT
#define | USBHS_OTGSC_BSEIE(x) USB_OTGSC_BSEIE(x)
#define | USBHS_OTGSC_MSE_MASK USB_OTGSC_EN_1MS_MASK
#define | USBHS_OTGSC_MSE_SHIFT USB_OTGSC_EN_1MS_SHIFT
#define | USBHS_OTGSC_MSE(x) USB_OTGSC_EN_1MS(x)
#define | USBHS_OTGSC_DPIE_MASK USB_OTGSC_DPIE_MASK
#define | USBHS_OTGSC_DPIE_SHIFT USB_OTGSC_DPIE_SHIFT
#define | USBHS_OTGSC_DPIE(x) USB_OTGSC_DPIE(x)
#define | USBHS_USBMODE_CM_MASK USB_USBMODE_CM_MASK
#define | USBHS_USBMODE_CM_SHIFT USB_USBMODE_CM_SHIFT
#define | USBHS_USBMODE_CM(x) USB_USBMODE_CM(x)
#define | USBHS_USBMODE_ES_MASK USB_USBMODE_ES_MASK
#define | USBHS_USBMODE_ES_SHIFT USB_USBMODE_ES_SHIFT
#define | USBHS_USBMODE_ES(x) USB_USBMODE_ES(x)
#define | USBHS_USBMODE_SLOM_MASK USB_USBMODE_SLOM_MASK
#define | USBHS_USBMODE_SLOM_SHIFT USB_USBMODE_SLOM_SHIFT
#define | USBHS_USBMODE_SLOM(x) USB_USBMODE_SLOM(x)
#define | USBHS_USBMODE_SDIS_MASK USB_USBMODE_SDIS_MASK
#define | USBHS_USBMODE_SDIS_SHIFT USB_USBMODE_SDIS_SHIFT
#define | USBHS_USBMODE_SDIS(x) USB_USBMODE_SDIS(x)
#define | USBHS_EPSETUPSR_EPSETUPSTAT_MASK USB_ENDPTSETUPSTAT_ENDPTSETUPSTAT_MASK
#define | USBHS_EPSETUPSR_EPSETUPSTAT_SHIFT USB_ENDPTSETUPSTAT_ENDPTSETUPSTAT_SHIFT
#define | USBHS_EPSETUPSR_EPSETUPSTAT(x) USB_ENDPTSETUPSTAT_ENDPTSETUPSTAT(x)
#define | USBHS_EPPRIME_PERB_MASK USB_ENDPTPRIME_PERB_MASK
#define | USBHS_EPPRIME_PERB_SHIFT USB_ENDPTPRIME_PERB_SHIFT
#define | USBHS_EPPRIME_PERB(x) USB_ENDPTPRIME_PERB(x)
#define | USBHS_EPPRIME_PETB_MASK USB_ENDPTPRIME_PETB_MASK
#define | USBHS_EPPRIME_PETB_SHIFT USB_ENDPTPRIME_PETB_SHIFT
#define | USBHS_EPPRIME_PETB(x) USB_ENDPTPRIME_PETB(x)
#define | USBHS_EPFLUSH_FERB_MASK USB_ENDPTFLUSH_FERB_MASK
#define | USBHS_EPFLUSH_FERB_SHIFT USB_ENDPTFLUSH_FERB_SHIFT
#define | USBHS_EPFLUSH_FERB(x) USB_ENDPTFLUSH_FERB(x)
#define | USBHS_EPFLUSH_FETB_MASK USB_ENDPTFLUSH_FETB_MASK
#define | USBHS_EPFLUSH_FETB_SHIFT USB_ENDPTFLUSH_FETB_SHIFT
#define | USBHS_EPFLUSH_FETB(x) USB_ENDPTFLUSH_FETB(x)
#define | USBHS_EPSR_ERBR_MASK USB_ENDPTSTAT_ERBR_MASK
#define | USBHS_EPSR_ERBR_SHIFT USB_ENDPTSTAT_ERBR_SHIFT
#define | USBHS_EPSR_ERBR(x) USB_ENDPTSTAT_ERBR(x)
#define | USBHS_EPSR_ETBR_MASK USB_ENDPTSTAT_ETBR_MASK
#define | USBHS_EPSR_ETBR_SHIFT USB_ENDPTSTAT_ETBR_SHIFT
#define | USBHS_EPSR_ETBR(x) USB_ENDPTSTAT_ETBR(x)
#define | USBHS_EPCOMPLETE_ERCE_MASK USB_ENDPTCOMPLETE_ERCE_MASK
#define | USBHS_EPCOMPLETE_ERCE_SHIFT USB_ENDPTCOMPLETE_ERCE_SHIFT
#define | USBHS_EPCOMPLETE_ERCE(x) USB_ENDPTCOMPLETE_ERCE(x)
#define | USBHS_EPCOMPLETE_ETCE_MASK USB_ENDPTCOMPLETE_ETCE_MASK
#define | USBHS_EPCOMPLETE_ETCE_SHIFT USB_ENDPTCOMPLETE_ETCE_SHIFT
#define | USBHS_EPCOMPLETE_ETCE(x) USB_ENDPTCOMPLETE_ETCE(x)
#define | USBHS_EPCR0_RXS_MASK USB_ENDPTCTRL0_RXS_MASK
#define | USBHS_EPCR0_RXS_SHIFT USB_ENDPTCTRL0_RXS_SHIFT
#define | USBHS_EPCR0_RXS(x) USB_ENDPTCTRL0_RXS(x)
#define | USBHS_EPCR0_RXT_MASK USB_ENDPTCTRL0_RXT_MASK
#define | USBHS_EPCR0_RXT_SHIFT USB_ENDPTCTRL0_RXT_SHIFT
#define | USBHS_EPCR0_RXT(x) USB_ENDPTCTRL0_RXT(x)
#define | USBHS_EPCR0_RXE_MASK USB_ENDPTCTRL0_RXE_MASK
#define | USBHS_EPCR0_RXE_SHIFT USB_ENDPTCTRL0_RXE_SHIFT
#define | USBHS_EPCR0_RXE(x) USB_ENDPTCTRL0_RXE(x)
#define | USBHS_EPCR0_TXS_MASK USB_ENDPTCTRL0_TXS_MASK
#define | USBHS_EPCR0_TXS_SHIFT USB_ENDPTCTRL0_TXS_SHIFT
#define | USBHS_EPCR0_TXS(x) USB_ENDPTCTRL0_TXS(x)
#define | USBHS_EPCR0_TXT_MASK USB_ENDPTCTRL0_TXT_MASK
#define | USBHS_EPCR0_TXT_SHIFT USB_ENDPTCTRL0_TXT_SHIFT
#define | USBHS_EPCR0_TXT(x) USB_ENDPTCTRL0_TXT(x)
#define | USBHS_EPCR0_TXE_MASK USB_ENDPTCTRL0_TXE_MASK
#define | USBHS_EPCR0_TXE_SHIFT USB_ENDPTCTRL0_TXE_SHIFT
#define | USBHS_EPCR0_TXE(x) USB_ENDPTCTRL0_TXE(x)
#define | USBHS_EPCR_RXS_MASK USB_ENDPTCTRL_RXS_MASK
#define | USBHS_EPCR_RXS_SHIFT USB_ENDPTCTRL_RXS_SHIFT
#define | USBHS_EPCR_RXS(x) USB_ENDPTCTRL_RXS(x)
#define | USBHS_EPCR_RXD_MASK USB_ENDPTCTRL_RXD_MASK
#define | USBHS_EPCR_RXD_SHIFT USB_ENDPTCTRL_RXD_SHIFT
#define | USBHS_EPCR_RXD(x) USB_ENDPTCTRL_RXD(x)
#define | USBHS_EPCR_RXT_MASK USB_ENDPTCTRL_RXT_MASK
#define | USBHS_EPCR_RXT_SHIFT USB_ENDPTCTRL_RXT_SHIFT
#define | USBHS_EPCR_RXT(x) USB_ENDPTCTRL_RXT(x)
#define | USBHS_EPCR_RXI_MASK USB_ENDPTCTRL_RXI_MASK
#define | USBHS_EPCR_RXI_SHIFT USB_ENDPTCTRL_RXI_SHIFT
#define | USBHS_EPCR_RXI(x) USB_ENDPTCTRL_RXI(x)
#define | USBHS_EPCR_RXR_MASK USB_ENDPTCTRL_RXR_MASK
#define | USBHS_EPCR_RXR_SHIFT USB_ENDPTCTRL_RXR_SHIFT
#define | USBHS_EPCR_RXR(x) USB_ENDPTCTRL_RXR(x)
#define | USBHS_EPCR_RXE_MASK USB_ENDPTCTRL_RXE_MASK
#define | USBHS_EPCR_RXE_SHIFT USB_ENDPTCTRL_RXE_SHIFT
#define | USBHS_EPCR_RXE(x) USB_ENDPTCTRL_RXE(x)
#define | USBHS_EPCR_TXS_MASK USB_ENDPTCTRL_TXS_MASK
#define | USBHS_EPCR_TXS_SHIFT USB_ENDPTCTRL_TXS_SHIFT
#define | USBHS_EPCR_TXS(x) USB_ENDPTCTRL_TXS(x)
#define | USBHS_EPCR_TXD_MASK USB_ENDPTCTRL_TXD_MASK
#define | USBHS_EPCR_TXD_SHIFT USB_ENDPTCTRL_TXD_SHIFT
#define | USBHS_EPCR_TXD(x) USB_ENDPTCTRL_TXD(x)
#define | USBHS_EPCR_TXT_MASK USB_ENDPTCTRL_TXT_MASK
#define | USBHS_EPCR_TXT_SHIFT USB_ENDPTCTRL_TXT_SHIFT
#define | USBHS_EPCR_TXT(x) USB_ENDPTCTRL_TXT(x)
#define | USBHS_EPCR_TXI_MASK USB_ENDPTCTRL_TXI_MASK
#define | USBHS_EPCR_TXI_SHIFT USB_ENDPTCTRL_TXI_SHIFT
#define | USBHS_EPCR_TXI(x) USB_ENDPTCTRL_TXI(x)
#define | USBHS_EPCR_TXR_MASK USB_ENDPTCTRL_TXR_MASK
#define | USBHS_EPCR_TXR_SHIFT USB_ENDPTCTRL_TXR_SHIFT
#define | USBHS_EPCR_TXR(x) USB_ENDPTCTRL_TXR(x)
#define | USBHS_EPCR_TXE_MASK USB_ENDPTCTRL_TXE_MASK
#define | USBHS_EPCR_TXE_SHIFT USB_ENDPTCTRL_TXE_SHIFT
#define | USBHS_EPCR_TXE(x) USB_ENDPTCTRL_TXE(x)
#define | USBHS_EPCR_COUNT USB_ENDPTCTRL_COUNT
#define | USBHS_Type USB_Type
#define | USBHS_BASE_ADDRS { USB1_BASE, USB2_BASE }
#define | USBHS_IRQS { USB_OTG1_IRQn, USB_OTG2_IRQn }
#define | USBHS_IRQHandler USB_OTG1_IRQHandler

## Detailed Description

## Macro Definition Documentation

## ◆ EPCOMPLETE

#define EPCOMPLETE ENDPTCOMPLETE

Definition at line 42354 of file MIMXRT1062.h.

## ◆ EPCR

#define EPCR ENDPTCTRL

Definition at line 42355 of file MIMXRT1062.h.

## ◆ EPCR0

#define EPCR0 ENDPTCTRL0

Definition at line 42356 of file MIMXRT1062.h.

## ◆ EPFLUSH

#define EPFLUSH ENDPTFLUSH

Definition at line 42352 of file MIMXRT1062.h.

## ◆ EPLISTADDR

#define EPLISTADDR ENDPTLISTADDR

Definition at line 42349 of file MIMXRT1062.h.

## ◆ EPPRIME

#define EPPRIME ENDPTPRIME

Definition at line 42351 of file MIMXRT1062.h.

## ◆ EPSETUPSR

#define EPSETUPSR ENDPTSETUPSTAT

Definition at line 42350 of file MIMXRT1062.h.

## ◆ EPSR

#define EPSR ENDPTSTAT

Definition at line 42353 of file MIMXRT1062.h.

## ◆ GPTIMER0CTL

#define GPTIMER0CTL GPTIMER0CTRL

Definition at line 42346 of file MIMXRT1062.h.

## ◆ GPTIMER1CTL

#define GPTIMER1CTL GPTIMER1CTRL

Definition at line 42347 of file MIMXRT1062.h.

## ◆ USB1

#define USB1 ((USB_Type *)USB1_BASE)

Peripheral USB1 base pointer

Definition at line 42334 of file MIMXRT1062.h.

## ◆ USB1_BASE

#define USB1_BASE (0x402E0000u)

Peripheral USB1 base address

Definition at line 42332 of file MIMXRT1062.h.

## ◆ USB2

#define USB2 ((USB_Type *)USB2_BASE)

Peripheral USB2 base pointer

Definition at line 42338 of file MIMXRT1062.h.

## ◆ USB2_BASE

#define USB2_BASE (0x402E0200u)

Peripheral USB2 base address

Definition at line 42336 of file MIMXRT1062.h.

## ◆ USB_BASE_ADDRS

#define USB_BASE_ADDRS { 0u, USB1_BASE, USB2_BASE }

Array initializer of USB peripheral base addresses

Definition at line 42340 of file MIMXRT1062.h.

## ◆ USB_BASE_PTRS

#define USB_BASE_PTRS { (USB_Type *)0u, USB1, USB2 }

Array initializer of USB peripheral base pointers

Definition at line 42342 of file MIMXRT1062.h.

## ◆ USB_IRQS

#define USB_IRQS { NotAvail_IRQn, USB_OTG1_IRQn, USB_OTG2_IRQn }

Interrupt vectors for the USB peripheral type

Definition at line 42344 of file MIMXRT1062.h.

## ◆ USB_SBUSCFG

#define USB_SBUSCFG SBUSCFG

Definition at line 42348 of file MIMXRT1062.h.

## ◆ USBHS_ASYNCLISTADDR_ASYBASE

#define USBHS_ASYNCLISTADDR_ASYBASE | ( |  | x | ) | USB_ASYNCLISTADDR_ASYBASE(x)

Definition at line 42630 of file MIMXRT1062.h.

## ◆ USBHS_ASYNCLISTADDR_ASYBASE_MASK

#define USBHS_ASYNCLISTADDR_ASYBASE_MASK USB_ASYNCLISTADDR_ASYBASE_MASK

Definition at line 42628 of file MIMXRT1062.h.

## ◆ USBHS_ASYNCLISTADDR_ASYBASE_SHIFT

#define USBHS_ASYNCLISTADDR_ASYBASE_SHIFT USB_ASYNCLISTADDR_ASYBASE_SHIFT

Definition at line 42629 of file MIMXRT1062.h.

## ◆ USBHS_BASE_ADDRS

#define USBHS_BASE_ADDRS { USB1_BASE, USB2_BASE }

Definition at line 42912 of file MIMXRT1062.h.

## ◆ USBHS_BURSTSIZE_RXPBURST

#define USBHS_BURSTSIZE_RXPBURST | ( |  | x | ) | USB_BURSTSIZE_RXPBURST(x)

Definition at line 42636 of file MIMXRT1062.h.

## ◆ USBHS_BURSTSIZE_RXPBURST_MASK

#define USBHS_BURSTSIZE_RXPBURST_MASK USB_BURSTSIZE_RXPBURST_MASK

Definition at line 42634 of file MIMXRT1062.h.

## ◆ USBHS_BURSTSIZE_RXPBURST_SHIFT

#define USBHS_BURSTSIZE_RXPBURST_SHIFT USB_BURSTSIZE_RXPBURST_SHIFT

Definition at line 42635 of file MIMXRT1062.h.

## ◆ USBHS_BURSTSIZE_TXPBURST

#define USBHS_BURSTSIZE_TXPBURST | ( |  | x | ) | USB_BURSTSIZE_TXPBURST(x)

Definition at line 42639 of file MIMXRT1062.h.

## ◆ USBHS_BURSTSIZE_TXPBURST_MASK

#define USBHS_BURSTSIZE_TXPBURST_MASK USB_BURSTSIZE_TXPBURST_MASK

Definition at line 42637 of file MIMXRT1062.h.

## ◆ USBHS_BURSTSIZE_TXPBURST_SHIFT

#define USBHS_BURSTSIZE_TXPBURST_SHIFT USB_BURSTSIZE_TXPBURST_SHIFT

Definition at line 42638 of file MIMXRT1062.h.

## ◆ USBHS_CONFIGFLAG_CF

#define USBHS_CONFIGFLAG_CF | ( |  | x | ) | USB_CONFIGFLAG_CF(x)

Definition at line 42663 of file MIMXRT1062.h.

## ◆ USBHS_CONFIGFLAG_CF_MASK

#define USBHS_CONFIGFLAG_CF_MASK USB_CONFIGFLAG_CF_MASK

Definition at line 42661 of file MIMXRT1062.h.

## ◆ USBHS_CONFIGFLAG_CF_SHIFT

#define USBHS_CONFIGFLAG_CF_SHIFT USB_CONFIGFLAG_CF_SHIFT

Definition at line 42662 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_DC

#define USBHS_DCCPARAMS_DC | ( |  | x | ) | USB_DCCPARAMS_DC(x)

Definition at line 42480 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_DC_MASK

#define USBHS_DCCPARAMS_DC_MASK USB_DCCPARAMS_DC_MASK

Definition at line 42478 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_DC_SHIFT

#define USBHS_DCCPARAMS_DC_SHIFT USB_DCCPARAMS_DC_SHIFT

Definition at line 42479 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_DEN

#define USBHS_DCCPARAMS_DEN | ( |  | x | ) | USB_DCCPARAMS_DEN(x)

Definition at line 42477 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_DEN_MASK

#define USBHS_DCCPARAMS_DEN_MASK USB_DCCPARAMS_DEN_MASK

Definition at line 42475 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_DEN_SHIFT

#define USBHS_DCCPARAMS_DEN_SHIFT USB_DCCPARAMS_DEN_SHIFT

Definition at line 42476 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_HC

#define USBHS_DCCPARAMS_HC | ( |  | x | ) | USB_DCCPARAMS_HC(x)

Definition at line 42483 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_HC_MASK

#define USBHS_DCCPARAMS_HC_MASK USB_DCCPARAMS_HC_MASK

Definition at line 42481 of file MIMXRT1062.h.

## ◆ USBHS_DCCPARAMS_HC_SHIFT

#define USBHS_DCCPARAMS_HC_SHIFT USB_DCCPARAMS_HC_SHIFT

Definition at line 42482 of file MIMXRT1062.h.

## ◆ USBHS_DCIVERSION_DCIVERSION

#define USBHS_DCIVERSION_DCIVERSION | ( |  | x | ) | USB_DCIVERSION_DCIVERSION(x)

Definition at line 42474 of file MIMXRT1062.h.

## ◆ USBHS_DCIVERSION_DCIVERSION_MASK

#define USBHS_DCIVERSION_DCIVERSION_MASK USB_DCIVERSION_DCIVERSION_MASK

Definition at line 42472 of file MIMXRT1062.h.

## ◆ USBHS_DCIVERSION_DCIVERSION_SHIFT

#define USBHS_DCIVERSION_DCIVERSION_SHIFT USB_DCIVERSION_DCIVERSION_SHIFT

Definition at line 42473 of file MIMXRT1062.h.

## ◆ USBHS_DEVICEADDR_USBADR

#define USBHS_DEVICEADDR_USBADR | ( |  | x | ) | USB_DEVICEADDR_USBADR(x)

Definition at line 42624 of file MIMXRT1062.h.

## ◆ USBHS_DEVICEADDR_USBADR_MASK

#define USBHS_DEVICEADDR_USBADR_MASK USB_DEVICEADDR_USBADR_MASK

Definition at line 42622 of file MIMXRT1062.h.

## ◆ USBHS_DEVICEADDR_USBADR_SHIFT

#define USBHS_DEVICEADDR_USBADR_SHIFT USB_DEVICEADDR_USBADR_SHIFT

Definition at line 42623 of file MIMXRT1062.h.

## ◆ USBHS_DEVICEADDR_USBADRA

#define USBHS_DEVICEADDR_USBADRA | ( |  | x | ) | USB_DEVICEADDR_USBADRA(x)

Definition at line 42621 of file MIMXRT1062.h.

## ◆ USBHS_DEVICEADDR_USBADRA_MASK

#define USBHS_DEVICEADDR_USBADRA_MASK USB_DEVICEADDR_USBADRA_MASK

Definition at line 42619 of file MIMXRT1062.h.

## ◆ USBHS_DEVICEADDR_USBADRA_SHIFT

#define USBHS_DEVICEADDR_USBADRA_SHIFT USB_DEVICEADDR_USBADRA_SHIFT

Definition at line 42620 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAK_EPRN

#define USBHS_ENDPTNAK_EPRN | ( |  | x | ) | USB_ENDPTNAK_EPRN(x)

Definition at line 42651 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAK_EPRN_MASK

#define USBHS_ENDPTNAK_EPRN_MASK USB_ENDPTNAK_EPRN_MASK

Definition at line 42649 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAK_EPRN_SHIFT

#define USBHS_ENDPTNAK_EPRN_SHIFT USB_ENDPTNAK_EPRN_SHIFT

Definition at line 42650 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAK_EPTN

#define USBHS_ENDPTNAK_EPTN | ( |  | x | ) | USB_ENDPTNAK_EPTN(x)

Definition at line 42654 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAK_EPTN_MASK

#define USBHS_ENDPTNAK_EPTN_MASK USB_ENDPTNAK_EPTN_MASK

Definition at line 42652 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAK_EPTN_SHIFT

#define USBHS_ENDPTNAK_EPTN_SHIFT USB_ENDPTNAK_EPTN_SHIFT

Definition at line 42653 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAKEN_EPRNE

#define USBHS_ENDPTNAKEN_EPRNE | ( |  | x | ) | USB_ENDPTNAKEN_EPRNE(x)

Definition at line 42657 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAKEN_EPRNE_MASK

#define USBHS_ENDPTNAKEN_EPRNE_MASK USB_ENDPTNAKEN_EPRNE_MASK

Definition at line 42655 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAKEN_EPRNE_SHIFT

#define USBHS_ENDPTNAKEN_EPRNE_SHIFT USB_ENDPTNAKEN_EPRNE_SHIFT

Definition at line 42656 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAKEN_EPTNE

#define USBHS_ENDPTNAKEN_EPTNE | ( |  | x | ) | USB_ENDPTNAKEN_EPTNE(x)

Definition at line 42660 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAKEN_EPTNE_MASK

#define USBHS_ENDPTNAKEN_EPTNE_MASK USB_ENDPTNAKEN_EPTNE_MASK

Definition at line 42658 of file MIMXRT1062.h.

## ◆ USBHS_ENDPTNAKEN_EPTNE_SHIFT

#define USBHS_ENDPTNAKEN_EPTNE_SHIFT USB_ENDPTNAKEN_EPTNE_SHIFT

Definition at line 42659 of file MIMXRT1062.h.

## ◆ USBHS_EPCOMPLETE_ERCE

#define USBHS_EPCOMPLETE_ERCE | ( |  | x | ) | USB_ENDPTCOMPLETE_ERCE(x)

Definition at line 42852 of file MIMXRT1062.h.

## ◆ USBHS_EPCOMPLETE_ERCE_MASK

#define USBHS_EPCOMPLETE_ERCE_MASK USB_ENDPTCOMPLETE_ERCE_MASK

Definition at line 42850 of file MIMXRT1062.h.

## ◆ USBHS_EPCOMPLETE_ERCE_SHIFT

#define USBHS_EPCOMPLETE_ERCE_SHIFT USB_ENDPTCOMPLETE_ERCE_SHIFT

Definition at line 42851 of file MIMXRT1062.h.

## ◆ USBHS_EPCOMPLETE_ETCE

#define USBHS_EPCOMPLETE_ETCE | ( |  | x | ) | USB_ENDPTCOMPLETE_ETCE(x)

Definition at line 42855 of file MIMXRT1062.h.

## ◆ USBHS_EPCOMPLETE_ETCE_MASK

#define USBHS_EPCOMPLETE_ETCE_MASK USB_ENDPTCOMPLETE_ETCE_MASK

Definition at line 42853 of file MIMXRT1062.h.

## ◆ USBHS_EPCOMPLETE_ETCE_SHIFT

#define USBHS_EPCOMPLETE_ETCE_SHIFT USB_ENDPTCOMPLETE_ETCE_SHIFT

Definition at line 42854 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXE

#define USBHS_EPCR0_RXE | ( |  | x | ) | USB_ENDPTCTRL0_RXE(x)

Definition at line 42864 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXE_MASK

#define USBHS_EPCR0_RXE_MASK USB_ENDPTCTRL0_RXE_MASK

Definition at line 42862 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXE_SHIFT

#define USBHS_EPCR0_RXE_SHIFT USB_ENDPTCTRL0_RXE_SHIFT

Definition at line 42863 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXS

#define USBHS_EPCR0_RXS | ( |  | x | ) | USB_ENDPTCTRL0_RXS(x)

Definition at line 42858 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXS_MASK

#define USBHS_EPCR0_RXS_MASK USB_ENDPTCTRL0_RXS_MASK

Definition at line 42856 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXS_SHIFT

#define USBHS_EPCR0_RXS_SHIFT USB_ENDPTCTRL0_RXS_SHIFT

Definition at line 42857 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXT

#define USBHS_EPCR0_RXT | ( |  | x | ) | USB_ENDPTCTRL0_RXT(x)

Definition at line 42861 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXT_MASK

#define USBHS_EPCR0_RXT_MASK USB_ENDPTCTRL0_RXT_MASK

Definition at line 42859 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_RXT_SHIFT

#define USBHS_EPCR0_RXT_SHIFT USB_ENDPTCTRL0_RXT_SHIFT

Definition at line 42860 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXE

#define USBHS_EPCR0_TXE | ( |  | x | ) | USB_ENDPTCTRL0_TXE(x)

Definition at line 42873 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXE_MASK

#define USBHS_EPCR0_TXE_MASK USB_ENDPTCTRL0_TXE_MASK

Definition at line 42871 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXE_SHIFT

#define USBHS_EPCR0_TXE_SHIFT USB_ENDPTCTRL0_TXE_SHIFT

Definition at line 42872 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXS

#define USBHS_EPCR0_TXS | ( |  | x | ) | USB_ENDPTCTRL0_TXS(x)

Definition at line 42867 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXS_MASK

#define USBHS_EPCR0_TXS_MASK USB_ENDPTCTRL0_TXS_MASK

Definition at line 42865 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXS_SHIFT

#define USBHS_EPCR0_TXS_SHIFT USB_ENDPTCTRL0_TXS_SHIFT

Definition at line 42866 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXT

#define USBHS_EPCR0_TXT | ( |  | x | ) | USB_ENDPTCTRL0_TXT(x)

Definition at line 42870 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXT_MASK

#define USBHS_EPCR0_TXT_MASK USB_ENDPTCTRL0_TXT_MASK

Definition at line 42868 of file MIMXRT1062.h.

## ◆ USBHS_EPCR0_TXT_SHIFT

#define USBHS_EPCR0_TXT_SHIFT USB_ENDPTCTRL0_TXT_SHIFT

Definition at line 42869 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_COUNT

#define USBHS_EPCR_COUNT USB_ENDPTCTRL_COUNT

Definition at line 42910 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXD

#define USBHS_EPCR_RXD | ( |  | x | ) | USB_ENDPTCTRL_RXD(x)

Definition at line 42879 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXD_MASK

#define USBHS_EPCR_RXD_MASK USB_ENDPTCTRL_RXD_MASK

Definition at line 42877 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXD_SHIFT

#define USBHS_EPCR_RXD_SHIFT USB_ENDPTCTRL_RXD_SHIFT

Definition at line 42878 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXE

#define USBHS_EPCR_RXE | ( |  | x | ) | USB_ENDPTCTRL_RXE(x)

Definition at line 42891 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXE_MASK

#define USBHS_EPCR_RXE_MASK USB_ENDPTCTRL_RXE_MASK

Definition at line 42889 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXE_SHIFT

#define USBHS_EPCR_RXE_SHIFT USB_ENDPTCTRL_RXE_SHIFT

Definition at line 42890 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXI

#define USBHS_EPCR_RXI | ( |  | x | ) | USB_ENDPTCTRL_RXI(x)

Definition at line 42885 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXI_MASK

#define USBHS_EPCR_RXI_MASK USB_ENDPTCTRL_RXI_MASK

Definition at line 42883 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXI_SHIFT

#define USBHS_EPCR_RXI_SHIFT USB_ENDPTCTRL_RXI_SHIFT

Definition at line 42884 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXR

#define USBHS_EPCR_RXR | ( |  | x | ) | USB_ENDPTCTRL_RXR(x)

Definition at line 42888 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXR_MASK

#define USBHS_EPCR_RXR_MASK USB_ENDPTCTRL_RXR_MASK

Definition at line 42886 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXR_SHIFT

#define USBHS_EPCR_RXR_SHIFT USB_ENDPTCTRL_RXR_SHIFT

Definition at line 42887 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXS

#define USBHS_EPCR_RXS | ( |  | x | ) | USB_ENDPTCTRL_RXS(x)

Definition at line 42876 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXS_MASK

#define USBHS_EPCR_RXS_MASK USB_ENDPTCTRL_RXS_MASK

Definition at line 42874 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXS_SHIFT

#define USBHS_EPCR_RXS_SHIFT USB_ENDPTCTRL_RXS_SHIFT

Definition at line 42875 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXT

#define USBHS_EPCR_RXT | ( |  | x | ) | USB_ENDPTCTRL_RXT(x)

Definition at line 42882 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXT_MASK

#define USBHS_EPCR_RXT_MASK USB_ENDPTCTRL_RXT_MASK

Definition at line 42880 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_RXT_SHIFT

#define USBHS_EPCR_RXT_SHIFT USB_ENDPTCTRL_RXT_SHIFT

Definition at line 42881 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXD

#define USBHS_EPCR_TXD | ( |  | x | ) | USB_ENDPTCTRL_TXD(x)

Definition at line 42897 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXD_MASK

#define USBHS_EPCR_TXD_MASK USB_ENDPTCTRL_TXD_MASK

Definition at line 42895 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXD_SHIFT

#define USBHS_EPCR_TXD_SHIFT USB_ENDPTCTRL_TXD_SHIFT

Definition at line 42896 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXE

#define USBHS_EPCR_TXE | ( |  | x | ) | USB_ENDPTCTRL_TXE(x)

Definition at line 42909 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXE_MASK

#define USBHS_EPCR_TXE_MASK USB_ENDPTCTRL_TXE_MASK

Definition at line 42907 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXE_SHIFT

#define USBHS_EPCR_TXE_SHIFT USB_ENDPTCTRL_TXE_SHIFT

Definition at line 42908 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXI

#define USBHS_EPCR_TXI | ( |  | x | ) | USB_ENDPTCTRL_TXI(x)

Definition at line 42903 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXI_MASK

#define USBHS_EPCR_TXI_MASK USB_ENDPTCTRL_TXI_MASK

Definition at line 42901 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXI_SHIFT

#define USBHS_EPCR_TXI_SHIFT USB_ENDPTCTRL_TXI_SHIFT

Definition at line 42902 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXR

#define USBHS_EPCR_TXR | ( |  | x | ) | USB_ENDPTCTRL_TXR(x)

Definition at line 42906 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXR_MASK

#define USBHS_EPCR_TXR_MASK USB_ENDPTCTRL_TXR_MASK

Definition at line 42904 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXR_SHIFT

#define USBHS_EPCR_TXR_SHIFT USB_ENDPTCTRL_TXR_SHIFT

Definition at line 42905 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXS

#define USBHS_EPCR_TXS | ( |  | x | ) | USB_ENDPTCTRL_TXS(x)

Definition at line 42894 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXS_MASK

#define USBHS_EPCR_TXS_MASK USB_ENDPTCTRL_TXS_MASK

Definition at line 42892 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXS_SHIFT

#define USBHS_EPCR_TXS_SHIFT USB_ENDPTCTRL_TXS_SHIFT

Definition at line 42893 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXT

#define USBHS_EPCR_TXT | ( |  | x | ) | USB_ENDPTCTRL_TXT(x)

Definition at line 42900 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXT_MASK

#define USBHS_EPCR_TXT_MASK USB_ENDPTCTRL_TXT_MASK

Definition at line 42898 of file MIMXRT1062.h.

## ◆ USBHS_EPCR_TXT_SHIFT

#define USBHS_EPCR_TXT_SHIFT USB_ENDPTCTRL_TXT_SHIFT

Definition at line 42899 of file MIMXRT1062.h.

## ◆ USBHS_EPFLUSH_FERB

#define USBHS_EPFLUSH_FERB | ( |  | x | ) | USB_ENDPTFLUSH_FERB(x)

Definition at line 42840 of file MIMXRT1062.h.

## ◆ USBHS_EPFLUSH_FERB_MASK

#define USBHS_EPFLUSH_FERB_MASK USB_ENDPTFLUSH_FERB_MASK

Definition at line 42838 of file MIMXRT1062.h.

## ◆ USBHS_EPFLUSH_FERB_SHIFT

#define USBHS_EPFLUSH_FERB_SHIFT USB_ENDPTFLUSH_FERB_SHIFT

Definition at line 42839 of file MIMXRT1062.h.

## ◆ USBHS_EPFLUSH_FETB

#define USBHS_EPFLUSH_FETB | ( |  | x | ) | USB_ENDPTFLUSH_FETB(x)

Definition at line 42843 of file MIMXRT1062.h.

## ◆ USBHS_EPFLUSH_FETB_MASK

#define USBHS_EPFLUSH_FETB_MASK USB_ENDPTFLUSH_FETB_MASK

Definition at line 42841 of file MIMXRT1062.h.

## ◆ USBHS_EPFLUSH_FETB_SHIFT

#define USBHS_EPFLUSH_FETB_SHIFT USB_ENDPTFLUSH_FETB_SHIFT

Definition at line 42842 of file MIMXRT1062.h.

## ◆ USBHS_EPLISTADDR_EPBASE

#define USBHS_EPLISTADDR_EPBASE | ( |  | x | ) | USB_ENDPTLISTADDR_EPBASE(x)

Definition at line 42633 of file MIMXRT1062.h.

## ◆ USBHS_EPLISTADDR_EPBASE_MASK

#define USBHS_EPLISTADDR_EPBASE_MASK USB_ENDPTLISTADDR_EPBASE_MASK

Definition at line 42631 of file MIMXRT1062.h.

## ◆ USBHS_EPLISTADDR_EPBASE_SHIFT

#define USBHS_EPLISTADDR_EPBASE_SHIFT USB_ENDPTLISTADDR_EPBASE_SHIFT

Definition at line 42632 of file MIMXRT1062.h.

## ◆ USBHS_EPPRIME_PERB

#define USBHS_EPPRIME_PERB | ( |  | x | ) | USB_ENDPTPRIME_PERB(x)

Definition at line 42834 of file MIMXRT1062.h.

## ◆ USBHS_EPPRIME_PERB_MASK

#define USBHS_EPPRIME_PERB_MASK USB_ENDPTPRIME_PERB_MASK

Definition at line 42832 of file MIMXRT1062.h.

## ◆ USBHS_EPPRIME_PERB_SHIFT

#define USBHS_EPPRIME_PERB_SHIFT USB_ENDPTPRIME_PERB_SHIFT

Definition at line 42833 of file MIMXRT1062.h.

## ◆ USBHS_EPPRIME_PETB

#define USBHS_EPPRIME_PETB | ( |  | x | ) | USB_ENDPTPRIME_PETB(x)

Definition at line 42837 of file MIMXRT1062.h.

## ◆ USBHS_EPPRIME_PETB_MASK

#define USBHS_EPPRIME_PETB_MASK USB_ENDPTPRIME_PETB_MASK

Definition at line 42835 of file MIMXRT1062.h.

## ◆ USBHS_EPPRIME_PETB_SHIFT

#define USBHS_EPPRIME_PETB_SHIFT USB_ENDPTPRIME_PETB_SHIFT

Definition at line 42836 of file MIMXRT1062.h.

## ◆ USBHS_EPSETUPSR_EPSETUPSTAT

#define USBHS_EPSETUPSR_EPSETUPSTAT | ( |  | x | ) | USB_ENDPTSETUPSTAT_ENDPTSETUPSTAT(x)

Definition at line 42831 of file MIMXRT1062.h.

## ◆ USBHS_EPSETUPSR_EPSETUPSTAT_MASK

#define USBHS_EPSETUPSR_EPSETUPSTAT_MASK USB_ENDPTSETUPSTAT_ENDPTSETUPSTAT_MASK

Definition at line 42829 of file MIMXRT1062.h.

## ◆ USBHS_EPSETUPSR_EPSETUPSTAT_SHIFT

#define USBHS_EPSETUPSR_EPSETUPSTAT_SHIFT USB_ENDPTSETUPSTAT_ENDPTSETUPSTAT_SHIFT

Definition at line 42830 of file MIMXRT1062.h.

## ◆ USBHS_EPSR_ERBR

#define USBHS_EPSR_ERBR | ( |  | x | ) | USB_ENDPTSTAT_ERBR(x)

Definition at line 42846 of file MIMXRT1062.h.

## ◆ USBHS_EPSR_ERBR_MASK

#define USBHS_EPSR_ERBR_MASK USB_ENDPTSTAT_ERBR_MASK

Definition at line 42844 of file MIMXRT1062.h.

## ◆ USBHS_EPSR_ERBR_SHIFT

#define USBHS_EPSR_ERBR_SHIFT USB_ENDPTSTAT_ERBR_SHIFT

Definition at line 42845 of file MIMXRT1062.h.

## ◆ USBHS_EPSR_ETBR

#define USBHS_EPSR_ETBR | ( |  | x | ) | USB_ENDPTSTAT_ETBR(x)

Definition at line 42849 of file MIMXRT1062.h.

## ◆ USBHS_EPSR_ETBR_MASK

#define USBHS_EPSR_ETBR_MASK USB_ENDPTSTAT_ETBR_MASK

Definition at line 42847 of file MIMXRT1062.h.

## ◆ USBHS_EPSR_ETBR_SHIFT

#define USBHS_EPSR_ETBR_SHIFT USB_ENDPTSTAT_ETBR_SHIFT

Definition at line 42848 of file MIMXRT1062.h.

## ◆ USBHS_FRINDEX_FRINDEX

#define USBHS_FRINDEX_FRINDEX | ( |  | x | ) | USB_FRINDEX_FRINDEX(x)

Definition at line 42618 of file MIMXRT1062.h.

## ◆ USBHS_FRINDEX_FRINDEX_MASK

#define USBHS_FRINDEX_FRINDEX_MASK USB_FRINDEX_FRINDEX_MASK

Definition at line 42616 of file MIMXRT1062.h.

## ◆ USBHS_FRINDEX_FRINDEX_SHIFT

#define USBHS_FRINDEX_FRINDEX_SHIFT USB_FRINDEX_FRINDEX_SHIFT

Definition at line 42617 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_GPTCNT

#define USBHS_GPTIMER0CTL_GPTCNT | ( |  | x | ) | USB_GPTIMER0CTRL_GPTCNT(x)

Definition at line 42404 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_GPTCNT_MASK

#define USBHS_GPTIMER0CTL_GPTCNT_MASK USB_GPTIMER0CTRL_GPTCNT_MASK

Definition at line 42402 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_GPTCNT_SHIFT

#define USBHS_GPTIMER0CTL_GPTCNT_SHIFT USB_GPTIMER0CTRL_GPTCNT_SHIFT

Definition at line 42403 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_MODE

#define USBHS_GPTIMER0CTL_MODE | ( |  | x | ) | USB_GPTIMER0CTRL_GPTMODE(x)

Definition at line 42407 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_MODE_MASK

#define USBHS_GPTIMER0CTL_MODE_MASK USB_GPTIMER0CTRL_GPTMODE_MASK

Definition at line 42405 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_MODE_SHIFT

#define USBHS_GPTIMER0CTL_MODE_SHIFT USB_GPTIMER0CTRL_GPTMODE_SHIFT

Definition at line 42406 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_RST

#define USBHS_GPTIMER0CTL_RST | ( |  | x | ) | USB_GPTIMER0CTRL_GPTRST(x)

Definition at line 42410 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_RST_MASK

#define USBHS_GPTIMER0CTL_RST_MASK USB_GPTIMER0CTRL_GPTRST_MASK

Definition at line 42408 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_RST_SHIFT

#define USBHS_GPTIMER0CTL_RST_SHIFT USB_GPTIMER0CTRL_GPTRST_SHIFT

Definition at line 42409 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_RUN

#define USBHS_GPTIMER0CTL_RUN | ( |  | x | ) | USB_GPTIMER0CTRL_GPTRUN(x)

Definition at line 42413 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_RUN_MASK

#define USBHS_GPTIMER0CTL_RUN_MASK USB_GPTIMER0CTRL_GPTRUN_MASK

Definition at line 42411 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0CTL_RUN_SHIFT

#define USBHS_GPTIMER0CTL_RUN_SHIFT USB_GPTIMER0CTRL_GPTRUN_SHIFT

Definition at line 42412 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0LD_GPTLD

#define USBHS_GPTIMER0LD_GPTLD | ( |  | x | ) | USB_GPTIMER0LD_GPTLD(x)

Definition at line 42401 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0LD_GPTLD_MASK

#define USBHS_GPTIMER0LD_GPTLD_MASK USB_GPTIMER0LD_GPTLD_MASK

Definition at line 42399 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER0LD_GPTLD_SHIFT

#define USBHS_GPTIMER0LD_GPTLD_SHIFT USB_GPTIMER0LD_GPTLD_SHIFT

Definition at line 42400 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_GPTCNT

#define USBHS_GPTIMER1CTL_GPTCNT | ( |  | x | ) | USB_GPTIMER1CTRL_GPTCNT(x)

Definition at line 42419 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_GPTCNT_MASK

#define USBHS_GPTIMER1CTL_GPTCNT_MASK USB_GPTIMER1CTRL_GPTCNT_MASK

Definition at line 42417 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_GPTCNT_SHIFT

#define USBHS_GPTIMER1CTL_GPTCNT_SHIFT USB_GPTIMER1CTRL_GPTCNT_SHIFT

Definition at line 42418 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_MODE

#define USBHS_GPTIMER1CTL_MODE | ( |  | x | ) | USB_GPTIMER1CTRL_GPTMODE(x)

Definition at line 42422 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_MODE_MASK

#define USBHS_GPTIMER1CTL_MODE_MASK USB_GPTIMER1CTRL_GPTMODE_MASK

Definition at line 42420 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_MODE_SHIFT

#define USBHS_GPTIMER1CTL_MODE_SHIFT USB_GPTIMER1CTRL_GPTMODE_SHIFT

Definition at line 42421 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_RST

#define USBHS_GPTIMER1CTL_RST | ( |  | x | ) | USB_GPTIMER1CTRL_GPTRST(x)

Definition at line 42425 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_RST_MASK

#define USBHS_GPTIMER1CTL_RST_MASK USB_GPTIMER1CTRL_GPTRST_MASK

Definition at line 42423 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_RST_SHIFT

#define USBHS_GPTIMER1CTL_RST_SHIFT USB_GPTIMER1CTRL_GPTRST_SHIFT

Definition at line 42424 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_RUN

#define USBHS_GPTIMER1CTL_RUN | ( |  | x | ) | USB_GPTIMER1CTRL_GPTRUN(x)

Definition at line 42428 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_RUN_MASK

#define USBHS_GPTIMER1CTL_RUN_MASK USB_GPTIMER1CTRL_GPTRUN_MASK

Definition at line 42426 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1CTL_RUN_SHIFT

#define USBHS_GPTIMER1CTL_RUN_SHIFT USB_GPTIMER1CTRL_GPTRUN_SHIFT

Definition at line 42427 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1LD_GPTLD

#define USBHS_GPTIMER1LD_GPTLD | ( |  | x | ) | USB_GPTIMER1LD_GPTLD(x)

Definition at line 42416 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1LD_GPTLD_MASK

#define USBHS_GPTIMER1LD_GPTLD_MASK USB_GPTIMER1LD_GPTLD_MASK

Definition at line 42414 of file MIMXRT1062.h.

## ◆ USBHS_GPTIMER1LD_GPTLD_SHIFT

#define USBHS_GPTIMER1LD_GPTLD_SHIFT USB_GPTIMER1LD_GPTLD_SHIFT

Definition at line 42415 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_ADC

#define USBHS_HCCPARAMS_ADC | ( |  | x | ) | USB_HCCPARAMS_ADC(x)

Definition at line 42459 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_ADC_MASK

#define USBHS_HCCPARAMS_ADC_MASK USB_HCCPARAMS_ADC_MASK

Definition at line 42457 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_ADC_SHIFT

#define USBHS_HCCPARAMS_ADC_SHIFT USB_HCCPARAMS_ADC_SHIFT

Definition at line 42458 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_ASP

#define USBHS_HCCPARAMS_ASP | ( |  | x | ) | USB_HCCPARAMS_ASP(x)

Definition at line 42465 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_ASP_MASK

#define USBHS_HCCPARAMS_ASP_MASK USB_HCCPARAMS_ASP_MASK

Definition at line 42463 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_ASP_SHIFT

#define USBHS_HCCPARAMS_ASP_SHIFT USB_HCCPARAMS_ASP_SHIFT

Definition at line 42464 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_EECP

#define USBHS_HCCPARAMS_EECP | ( |  | x | ) | USB_HCCPARAMS_EECP(x)

Definition at line 42471 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_EECP_MASK

#define USBHS_HCCPARAMS_EECP_MASK USB_HCCPARAMS_EECP_MASK

Definition at line 42469 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_EECP_SHIFT

#define USBHS_HCCPARAMS_EECP_SHIFT USB_HCCPARAMS_EECP_SHIFT

Definition at line 42470 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_IST

#define USBHS_HCCPARAMS_IST | ( |  | x | ) | USB_HCCPARAMS_IST(x)

Definition at line 42468 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_IST_MASK

#define USBHS_HCCPARAMS_IST_MASK USB_HCCPARAMS_IST_MASK

Definition at line 42466 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_IST_SHIFT

#define USBHS_HCCPARAMS_IST_SHIFT USB_HCCPARAMS_IST_SHIFT

Definition at line 42467 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_PFL

#define USBHS_HCCPARAMS_PFL | ( |  | x | ) | USB_HCCPARAMS_PFL(x)

Definition at line 42462 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_PFL_MASK

#define USBHS_HCCPARAMS_PFL_MASK USB_HCCPARAMS_PFL_MASK

Definition at line 42460 of file MIMXRT1062.h.

## ◆ USBHS_HCCPARAMS_PFL_SHIFT

#define USBHS_HCCPARAMS_PFL_SHIFT USB_HCCPARAMS_PFL_SHIFT

Definition at line 42461 of file MIMXRT1062.h.

## ◆ USBHS_HCIVERSION_CAPLENGTH

#define USBHS_HCIVERSION_CAPLENGTH | ( |  | x | ) | USB_HCIVERSION_CAPLENGTH(x)

Definition at line 42432 of file MIMXRT1062.h.

## ◆ USBHS_HCIVERSION_HCIVERSION

#define USBHS_HCIVERSION_HCIVERSION | ( |  | x | ) | USB_HCIVERSION_HCIVERSION(x)

Definition at line 42435 of file MIMXRT1062.h.

## ◆ USBHS_HCIVERSION_HCIVERSION_MASK

#define USBHS_HCIVERSION_HCIVERSION_MASK USB_HCIVERSION_HCIVERSION_MASK

Definition at line 42433 of file MIMXRT1062.h.

## ◆ USBHS_HCIVERSION_HCIVERSION_SHIFT

#define USBHS_HCIVERSION_HCIVERSION_SHIFT USB_HCIVERSION_HCIVERSION_SHIFT

Definition at line 42434 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_CC

#define USBHS_HCSPARAMS_N_CC | ( |  | x | ) | USB_HCSPARAMS_N_CC(x)

Definition at line 42447 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_CC_MASK

#define USBHS_HCSPARAMS_N_CC_MASK USB_HCSPARAMS_N_CC_MASK

Definition at line 42445 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_CC_SHIFT

#define USBHS_HCSPARAMS_N_CC_SHIFT USB_HCSPARAMS_N_CC_SHIFT

Definition at line 42446 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PCC

#define USBHS_HCSPARAMS_N_PCC | ( |  | x | ) | USB_HCSPARAMS_N_PCC(x)

Definition at line 42444 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PCC_MASK

#define USBHS_HCSPARAMS_N_PCC_MASK USB_HCSPARAMS_N_PCC_MASK

Definition at line 42442 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PCC_SHIFT

#define USBHS_HCSPARAMS_N_PCC_SHIFT USB_HCSPARAMS_N_PCC_SHIFT

Definition at line 42443 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PORTS

#define USBHS_HCSPARAMS_N_PORTS | ( |  | x | ) | USB_HCSPARAMS_N_PORTS(x)

Definition at line 42438 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PORTS_MASK

#define USBHS_HCSPARAMS_N_PORTS_MASK USB_HCSPARAMS_N_PORTS_MASK

Definition at line 42436 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PORTS_SHIFT

#define USBHS_HCSPARAMS_N_PORTS_SHIFT USB_HCSPARAMS_N_PORTS_SHIFT

Definition at line 42437 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PTT

#define USBHS_HCSPARAMS_N_PTT | ( |  | x | ) | USB_HCSPARAMS_N_PTT(x)

Definition at line 42453 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PTT_MASK

#define USBHS_HCSPARAMS_N_PTT_MASK USB_HCSPARAMS_N_PTT_MASK

Definition at line 42451 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_PTT_SHIFT

#define USBHS_HCSPARAMS_N_PTT_SHIFT USB_HCSPARAMS_N_PTT_SHIFT

Definition at line 42452 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_TT

#define USBHS_HCSPARAMS_N_TT | ( |  | x | ) | USB_HCSPARAMS_N_TT(x)

Definition at line 42456 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_TT_MASK

#define USBHS_HCSPARAMS_N_TT_MASK USB_HCSPARAMS_N_TT_MASK

Definition at line 42454 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_N_TT_SHIFT

#define USBHS_HCSPARAMS_N_TT_SHIFT USB_HCSPARAMS_N_TT_SHIFT

Definition at line 42455 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_PI

#define USBHS_HCSPARAMS_PI | ( |  | x | ) | USB_HCSPARAMS_PI(x)

Definition at line 42450 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_PI_MASK

#define USBHS_HCSPARAMS_PI_MASK USB_HCSPARAMS_PI_MASK

Definition at line 42448 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_PI_SHIFT

#define USBHS_HCSPARAMS_PI_SHIFT USB_HCSPARAMS_PI_SHIFT

Definition at line 42449 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_PPC

#define USBHS_HCSPARAMS_PPC | ( |  | x | ) | USB_HCSPARAMS_PPC(x)

Definition at line 42441 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_PPC_MASK

#define USBHS_HCSPARAMS_PPC_MASK USB_HCSPARAMS_PPC_MASK

Definition at line 42439 of file MIMXRT1062.h.

## ◆ USBHS_HCSPARAMS_PPC_SHIFT

#define USBHS_HCSPARAMS_PPC_SHIFT USB_HCSPARAMS_PPC_SHIFT

Definition at line 42440 of file MIMXRT1062.h.

## ◆ USBHS_HWDEVICE_DC

#define USBHS_HWDEVICE_DC | ( |  | x | ) | USB_HWDEVICE_DC(x)

Definition at line 42383 of file MIMXRT1062.h.

## ◆ USBHS_HWDEVICE_DC_MASK

#define USBHS_HWDEVICE_DC_MASK USB_HWDEVICE_DC_MASK

Definition at line 42381 of file MIMXRT1062.h.

## ◆ USBHS_HWDEVICE_DC_SHIFT

#define USBHS_HWDEVICE_DC_SHIFT USB_HWDEVICE_DC_SHIFT

Definition at line 42382 of file MIMXRT1062.h.

## ◆ USBHS_HWDEVICE_DEVEP

#define USBHS_HWDEVICE_DEVEP | ( |  | x | ) | USB_HWDEVICE_DEVEP(x)

Definition at line 42386 of file MIMXRT1062.h.

## ◆ USBHS_HWDEVICE_DEVEP_MASK

#define USBHS_HWDEVICE_DEVEP_MASK USB_HWDEVICE_DEVEP_MASK

Definition at line 42384 of file MIMXRT1062.h.

## ◆ USBHS_HWDEVICE_DEVEP_SHIFT

#define USBHS_HWDEVICE_DEVEP_SHIFT USB_HWDEVICE_DEVEP_SHIFT

Definition at line 42385 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_PHYM

#define USBHS_HWGENERAL_PHYM | ( |  | x | ) | USB_HWGENERAL_PHYM(x)

Definition at line 42371 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_PHYM_MASK

#define USBHS_HWGENERAL_PHYM_MASK USB_HWGENERAL_PHYM_MASK

Definition at line 42369 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_PHYM_SHIFT

#define USBHS_HWGENERAL_PHYM_SHIFT USB_HWGENERAL_PHYM_SHIFT

Definition at line 42370 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_PHYW

#define USBHS_HWGENERAL_PHYW | ( |  | x | ) | USB_HWGENERAL_PHYW(x)

Definition at line 42368 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_PHYW_MASK

#define USBHS_HWGENERAL_PHYW_MASK USB_HWGENERAL_PHYW_MASK

Definition at line 42366 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_PHYW_SHIFT

#define USBHS_HWGENERAL_PHYW_SHIFT USB_HWGENERAL_PHYW_SHIFT

Definition at line 42367 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_SM

#define USBHS_HWGENERAL_SM | ( |  | x | ) | USB_HWGENERAL_SM(x)

Definition at line 42374 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_SM_MASK

#define USBHS_HWGENERAL_SM_MASK USB_HWGENERAL_SM_MASK

Definition at line 42372 of file MIMXRT1062.h.

## ◆ USBHS_HWGENERAL_SM_SHIFT

#define USBHS_HWGENERAL_SM_SHIFT USB_HWGENERAL_SM_SHIFT

Definition at line 42373 of file MIMXRT1062.h.

## ◆ USBHS_HWHOST_HC

#define USBHS_HWHOST_HC | ( |  | x | ) | USB_HWHOST_HC(x)

Definition at line 42377 of file MIMXRT1062.h.

## ◆ USBHS_HWHOST_HC_MASK

#define USBHS_HWHOST_HC_MASK USB_HWHOST_HC_MASK

Definition at line 42375 of file MIMXRT1062.h.

## ◆ USBHS_HWHOST_HC_SHIFT

#define USBHS_HWHOST_HC_SHIFT USB_HWHOST_HC_SHIFT

Definition at line 42376 of file MIMXRT1062.h.

## ◆ USBHS_HWHOST_NPORT

#define USBHS_HWHOST_NPORT | ( |  | x | ) | USB_HWHOST_NPORT(x)

Definition at line 42380 of file MIMXRT1062.h.

## ◆ USBHS_HWHOST_NPORT_MASK

#define USBHS_HWHOST_NPORT_MASK USB_HWHOST_NPORT_MASK

Definition at line 42378 of file MIMXRT1062.h.

## ◆ USBHS_HWHOST_NPORT_SHIFT

#define USBHS_HWHOST_NPORT_SHIFT USB_HWHOST_NPORT_SHIFT

Definition at line 42379 of file MIMXRT1062.h.

## ◆ USBHS_HWRXBUF_RXADD

#define USBHS_HWRXBUF_RXADD | ( |  | x | ) | USB_HWRXBUF_RXADD(x)

Definition at line 42398 of file MIMXRT1062.h.

## ◆ USBHS_HWRXBUF_RXADD_MASK

#define USBHS_HWRXBUF_RXADD_MASK USB_HWRXBUF_RXADD_MASK

Definition at line 42396 of file MIMXRT1062.h.

## ◆ USBHS_HWRXBUF_RXADD_SHIFT

#define USBHS_HWRXBUF_RXADD_SHIFT USB_HWRXBUF_RXADD_SHIFT

Definition at line 42397 of file MIMXRT1062.h.

## ◆ USBHS_HWRXBUF_RXBURST

#define USBHS_HWRXBUF_RXBURST | ( |  | x | ) | USB_HWRXBUF_RXBURST(x)

Definition at line 42395 of file MIMXRT1062.h.

## ◆ USBHS_HWRXBUF_RXBURST_MASK

#define USBHS_HWRXBUF_RXBURST_MASK USB_HWRXBUF_RXBURST_MASK

Definition at line 42393 of file MIMXRT1062.h.

## ◆ USBHS_HWRXBUF_RXBURST_SHIFT

#define USBHS_HWRXBUF_RXBURST_SHIFT USB_HWRXBUF_RXBURST_SHIFT

Definition at line 42394 of file MIMXRT1062.h.

## ◆ USBHS_HWTXBUF_TXBURST

#define USBHS_HWTXBUF_TXBURST | ( |  | x | ) | USB_HWTXBUF_TXBURST(x)

Definition at line 42389 of file MIMXRT1062.h.

## ◆ USBHS_HWTXBUF_TXBURST_MASK

#define USBHS_HWTXBUF_TXBURST_MASK USB_HWTXBUF_TXBURST_MASK

Definition at line 42387 of file MIMXRT1062.h.

## ◆ USBHS_HWTXBUF_TXBURST_SHIFT

#define USBHS_HWTXBUF_TXBURST_SHIFT USB_HWTXBUF_TXBURST_SHIFT

Definition at line 42388 of file MIMXRT1062.h.

## ◆ USBHS_HWTXBUF_TXCHANADD

#define USBHS_HWTXBUF_TXCHANADD | ( |  | x | ) | USB_HWTXBUF_TXCHANADD(x)

Definition at line 42392 of file MIMXRT1062.h.

## ◆ USBHS_HWTXBUF_TXCHANADD_MASK

#define USBHS_HWTXBUF_TXCHANADD_MASK USB_HWTXBUF_TXCHANADD_MASK

Definition at line 42390 of file MIMXRT1062.h.

## ◆ USBHS_HWTXBUF_TXCHANADD_SHIFT

#define USBHS_HWTXBUF_TXCHANADD_SHIFT USB_HWTXBUF_TXCHANADD_SHIFT

Definition at line 42391 of file MIMXRT1062.h.

## ◆ USBHS_ID_ID

#define USBHS_ID_ID | ( |  | x | ) | USB_ID_ID(x)

Definition at line 42359 of file MIMXRT1062.h.

## ◆ USBHS_ID_ID_MASK

#define USBHS_ID_ID_MASK USB_ID_ID_MASK

Definition at line 42357 of file MIMXRT1062.h.

## ◆ USBHS_ID_ID_SHIFT

#define USBHS_ID_ID_SHIFT USB_ID_ID_SHIFT

Definition at line 42358 of file MIMXRT1062.h.

## ◆ USBHS_ID_NID

#define USBHS_ID_NID | ( |  | x | ) | USB_ID_NID(x)

Definition at line 42362 of file MIMXRT1062.h.

## ◆ USBHS_ID_NID_MASK

#define USBHS_ID_NID_MASK USB_ID_NID_MASK

Definition at line 42360 of file MIMXRT1062.h.

## ◆ USBHS_ID_NID_SHIFT

#define USBHS_ID_NID_SHIFT USB_ID_NID_SHIFT

Definition at line 42361 of file MIMXRT1062.h.

## ◆ USBHS_ID_REVISION

#define USBHS_ID_REVISION | ( |  | x | ) | USB_ID_REVISION(x)

Definition at line 42365 of file MIMXRT1062.h.

## ◆ USBHS_ID_REVISION_MASK

#define USBHS_ID_REVISION_MASK USB_ID_REVISION_MASK

Definition at line 42363 of file MIMXRT1062.h.

## ◆ USBHS_ID_REVISION_SHIFT

#define USBHS_ID_REVISION_SHIFT USB_ID_REVISION_SHIFT

Definition at line 42364 of file MIMXRT1062.h.

## ◆ USBHS_IRQHandler

#define USBHS_IRQHandler USB_OTG1_IRQHandler

Definition at line 42914 of file MIMXRT1062.h.

## ◆ USBHS_IRQS

#define USBHS_IRQS { USB_OTG1_IRQn, USB_OTG2_IRQn }

Definition at line 42913 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASV

#define USBHS_OTGSC_ASV | ( |  | x | ) | USB_OTGSC_ASV(x)

Definition at line 42762 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASV_MASK

#define USBHS_OTGSC_ASV_MASK USB_OTGSC_ASV_MASK

Definition at line 42760 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASV_SHIFT

#define USBHS_OTGSC_ASV_SHIFT USB_OTGSC_ASV_SHIFT

Definition at line 42761 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASVIE

#define USBHS_OTGSC_ASVIE | ( |  | x | ) | USB_OTGSC_ASVIE(x)

Definition at line 42804 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASVIE_MASK

#define USBHS_OTGSC_ASVIE_MASK USB_OTGSC_ASVIE_MASK

Definition at line 42802 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASVIE_SHIFT

#define USBHS_OTGSC_ASVIE_SHIFT USB_OTGSC_ASVIE_SHIFT

Definition at line 42803 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASVIS

#define USBHS_OTGSC_ASVIS | ( |  | x | ) | USB_OTGSC_ASVIS(x)

Definition at line 42783 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASVIS_MASK

#define USBHS_OTGSC_ASVIS_MASK USB_OTGSC_ASVIS_MASK

Definition at line 42781 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ASVIS_SHIFT

#define USBHS_OTGSC_ASVIS_SHIFT USB_OTGSC_ASVIS_SHIFT

Definition at line 42782 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVV

#define USBHS_OTGSC_AVV | ( |  | x | ) | USB_OTGSC_AVV(x)

Definition at line 42759 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVV_MASK

#define USBHS_OTGSC_AVV_MASK USB_OTGSC_AVV_MASK

Definition at line 42757 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVV_SHIFT

#define USBHS_OTGSC_AVV_SHIFT USB_OTGSC_AVV_SHIFT

Definition at line 42758 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVVIE

#define USBHS_OTGSC_AVVIE | ( |  | x | ) | USB_OTGSC_AVVIE(x)

Definition at line 42801 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVVIE_MASK

#define USBHS_OTGSC_AVVIE_MASK USB_OTGSC_AVVIE_MASK

Definition at line 42799 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVVIE_SHIFT

#define USBHS_OTGSC_AVVIE_SHIFT USB_OTGSC_AVVIE_SHIFT

Definition at line 42800 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVVIS

#define USBHS_OTGSC_AVVIS | ( |  | x | ) | USB_OTGSC_AVVIS(x)

Definition at line 42780 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVVIS_MASK

#define USBHS_OTGSC_AVVIS_MASK USB_OTGSC_AVVIS_MASK

Definition at line 42778 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_AVVIS_SHIFT

#define USBHS_OTGSC_AVVIS_SHIFT USB_OTGSC_AVVIS_SHIFT

Definition at line 42779 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSE

#define USBHS_OTGSC_BSE | ( |  | x | ) | USB_OTGSC_BSE(x)

Definition at line 42768 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSE_MASK

#define USBHS_OTGSC_BSE_MASK USB_OTGSC_BSE_MASK

Definition at line 42766 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSE_SHIFT

#define USBHS_OTGSC_BSE_SHIFT USB_OTGSC_BSE_SHIFT

Definition at line 42767 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSEIE

#define USBHS_OTGSC_BSEIE | ( |  | x | ) | USB_OTGSC_BSEIE(x)

Definition at line 42810 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSEIE_MASK

#define USBHS_OTGSC_BSEIE_MASK USB_OTGSC_BSEIE_MASK

Definition at line 42808 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSEIE_SHIFT

#define USBHS_OTGSC_BSEIE_SHIFT USB_OTGSC_BSEIE_SHIFT

Definition at line 42809 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSEIS

#define USBHS_OTGSC_BSEIS | ( |  | x | ) | USB_OTGSC_BSEIS(x)

Definition at line 42789 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSEIS_MASK

#define USBHS_OTGSC_BSEIS_MASK USB_OTGSC_BSEIS_MASK

Definition at line 42787 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSEIS_SHIFT

#define USBHS_OTGSC_BSEIS_SHIFT USB_OTGSC_BSEIS_SHIFT

Definition at line 42788 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSV

#define USBHS_OTGSC_BSV | ( |  | x | ) | USB_OTGSC_BSV(x)

Definition at line 42765 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSV_MASK

#define USBHS_OTGSC_BSV_MASK USB_OTGSC_BSV_MASK

Definition at line 42763 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSV_SHIFT

#define USBHS_OTGSC_BSV_SHIFT USB_OTGSC_BSV_SHIFT

Definition at line 42764 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSVIE

#define USBHS_OTGSC_BSVIE | ( |  | x | ) | USB_OTGSC_BSVIE(x)

Definition at line 42807 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSVIE_MASK

#define USBHS_OTGSC_BSVIE_MASK USB_OTGSC_BSVIE_MASK

Definition at line 42805 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSVIE_SHIFT

#define USBHS_OTGSC_BSVIE_SHIFT USB_OTGSC_BSVIE_SHIFT

Definition at line 42806 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSVIS

#define USBHS_OTGSC_BSVIS | ( |  | x | ) | USB_OTGSC_BSVIS(x)

Definition at line 42786 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSVIS_MASK

#define USBHS_OTGSC_BSVIS_MASK USB_OTGSC_BSVIS_MASK

Definition at line 42784 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_BSVIS_SHIFT

#define USBHS_OTGSC_BSVIS_SHIFT USB_OTGSC_BSVIS_SHIFT

Definition at line 42785 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DP

#define USBHS_OTGSC_DP | ( |  | x | ) | USB_OTGSC_DP(x)

Definition at line 42750 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DP_MASK

#define USBHS_OTGSC_DP_MASK USB_OTGSC_DP_MASK

Definition at line 42748 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DP_SHIFT

#define USBHS_OTGSC_DP_SHIFT USB_OTGSC_DP_SHIFT

Definition at line 42749 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPIE

#define USBHS_OTGSC_DPIE | ( |  | x | ) | USB_OTGSC_DPIE(x)

Definition at line 42816 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPIE_MASK

#define USBHS_OTGSC_DPIE_MASK USB_OTGSC_DPIE_MASK

Definition at line 42814 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPIE_SHIFT

#define USBHS_OTGSC_DPIE_SHIFT USB_OTGSC_DPIE_SHIFT

Definition at line 42815 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPIS

#define USBHS_OTGSC_DPIS | ( |  | x | ) | USB_OTGSC_DPIS(x)

Definition at line 42795 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPIS_MASK

#define USBHS_OTGSC_DPIS_MASK USB_OTGSC_DPIS_MASK

Definition at line 42793 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPIS_SHIFT

#define USBHS_OTGSC_DPIS_SHIFT USB_OTGSC_DPIS_SHIFT

Definition at line 42794 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPS

#define USBHS_OTGSC_DPS | ( |  | x | ) | USB_OTGSC_DPS(x)

Definition at line 42774 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPS_MASK

#define USBHS_OTGSC_DPS_MASK USB_OTGSC_DPS_MASK

Definition at line 42772 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_DPS_SHIFT

#define USBHS_OTGSC_DPS_SHIFT USB_OTGSC_DPS_SHIFT

Definition at line 42773 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ID

#define USBHS_OTGSC_ID | ( |  | x | ) | USB_OTGSC_ID(x)

Definition at line 42756 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ID_MASK

#define USBHS_OTGSC_ID_MASK USB_OTGSC_ID_MASK

Definition at line 42754 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_ID_SHIFT

#define USBHS_OTGSC_ID_SHIFT USB_OTGSC_ID_SHIFT

Definition at line 42755 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDIE

#define USBHS_OTGSC_IDIE | ( |  | x | ) | USB_OTGSC_IDIE(x)

Definition at line 42798 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDIE_MASK

#define USBHS_OTGSC_IDIE_MASK USB_OTGSC_IDIE_MASK

Definition at line 42796 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDIE_SHIFT

#define USBHS_OTGSC_IDIE_SHIFT USB_OTGSC_IDIE_SHIFT

Definition at line 42797 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDIS

#define USBHS_OTGSC_IDIS | ( |  | x | ) | USB_OTGSC_IDIS(x)

Definition at line 42777 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDIS_MASK

#define USBHS_OTGSC_IDIS_MASK USB_OTGSC_IDIS_MASK

Definition at line 42775 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDIS_SHIFT

#define USBHS_OTGSC_IDIS_SHIFT USB_OTGSC_IDIS_SHIFT

Definition at line 42776 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDPU

#define USBHS_OTGSC_IDPU | ( |  | x | ) | USB_OTGSC_IDPU(x)

Definition at line 42753 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDPU_MASK

#define USBHS_OTGSC_IDPU_MASK USB_OTGSC_IDPU_MASK

Definition at line 42751 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_IDPU_SHIFT

#define USBHS_OTGSC_IDPU_SHIFT USB_OTGSC_IDPU_SHIFT

Definition at line 42752 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MSE

#define USBHS_OTGSC_MSE | ( |  | x | ) | USB_OTGSC_EN_1MS(x)

Definition at line 42813 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MSE_MASK

#define USBHS_OTGSC_MSE_MASK USB_OTGSC_EN_1MS_MASK

Definition at line 42811 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MSE_SHIFT

#define USBHS_OTGSC_MSE_SHIFT USB_OTGSC_EN_1MS_SHIFT

Definition at line 42812 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MSS

#define USBHS_OTGSC_MSS | ( |  | x | ) | USB_OTGSC_STATUS_1MS(x)

Definition at line 42792 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MSS_MASK

#define USBHS_OTGSC_MSS_MASK USB_OTGSC_STATUS_1MS_MASK

Definition at line 42790 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MSS_SHIFT

#define USBHS_OTGSC_MSS_SHIFT USB_OTGSC_STATUS_1MS_SHIFT

Definition at line 42791 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MST

#define USBHS_OTGSC_MST | ( |  | x | ) | USB_OTGSC_TOG_1MS(x)

Definition at line 42771 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MST_MASK

#define USBHS_OTGSC_MST_MASK USB_OTGSC_TOG_1MS_MASK

Definition at line 42769 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_MST_SHIFT

#define USBHS_OTGSC_MST_SHIFT USB_OTGSC_TOG_1MS_SHIFT

Definition at line 42770 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_OT

#define USBHS_OTGSC_OT | ( |  | x | ) | USB_OTGSC_OT(x)

Definition at line 42747 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_OT_MASK

#define USBHS_OTGSC_OT_MASK USB_OTGSC_OT_MASK

Definition at line 42745 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_OT_SHIFT

#define USBHS_OTGSC_OT_SHIFT USB_OTGSC_OT_SHIFT

Definition at line 42746 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_VC

#define USBHS_OTGSC_VC | ( |  | x | ) | USB_OTGSC_VC(x)

Definition at line 42744 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_VC_MASK

#define USBHS_OTGSC_VC_MASK USB_OTGSC_VC_MASK

Definition at line 42742 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_VC_SHIFT

#define USBHS_OTGSC_VC_SHIFT USB_OTGSC_VC_SHIFT

Definition at line 42743 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_VD

#define USBHS_OTGSC_VD | ( |  | x | ) | USB_OTGSC_VD(x)

Definition at line 42741 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_VD_MASK

#define USBHS_OTGSC_VD_MASK USB_OTGSC_VD_MASK

Definition at line 42739 of file MIMXRT1062.h.

## ◆ USBHS_OTGSC_VD_SHIFT

#define USBHS_OTGSC_VD_SHIFT USB_OTGSC_VD_SHIFT

Definition at line 42740 of file MIMXRT1062.h.

## ◆ USBHS_PERIODICLISTBASE_PERBASE

#define USBHS_PERIODICLISTBASE_PERBASE | ( |  | x | ) | USB_PERIODICLISTBASE_BASEADR(x)

Definition at line 42627 of file MIMXRT1062.h.

## ◆ USBHS_PERIODICLISTBASE_PERBASE_MASK

#define USBHS_PERIODICLISTBASE_PERBASE_MASK USB_PERIODICLISTBASE_BASEADR_MASK

Definition at line 42625 of file MIMXRT1062.h.

## ◆ USBHS_PERIODICLISTBASE_PERBASE_SHIFT

#define USBHS_PERIODICLISTBASE_PERBASE_SHIFT USB_PERIODICLISTBASE_BASEADR_SHIFT

Definition at line 42626 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_CCS

#define USBHS_PORTSC1_CCS | ( |  | x | ) | USB_PORTSC1_CCS(x)

Definition at line 42666 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_CCS_MASK

#define USBHS_PORTSC1_CCS_MASK USB_PORTSC1_CCS_MASK

Definition at line 42664 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_CCS_SHIFT

#define USBHS_PORTSC1_CCS_SHIFT USB_PORTSC1_CCS_SHIFT

Definition at line 42665 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_CSC

#define USBHS_PORTSC1_CSC | ( |  | x | ) | USB_PORTSC1_CSC(x)

Definition at line 42669 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_CSC_MASK

#define USBHS_PORTSC1_CSC_MASK USB_PORTSC1_CSC_MASK

Definition at line 42667 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_CSC_SHIFT

#define USBHS_PORTSC1_CSC_SHIFT USB_PORTSC1_CSC_SHIFT

Definition at line 42668 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_FPR

#define USBHS_PORTSC1_FPR | ( |  | x | ) | USB_PORTSC1_FPR(x)

Definition at line 42684 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_FPR_MASK

#define USBHS_PORTSC1_FPR_MASK USB_PORTSC1_FPR_MASK

Definition at line 42682 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_FPR_SHIFT

#define USBHS_PORTSC1_FPR_SHIFT USB_PORTSC1_FPR_SHIFT

Definition at line 42683 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_HSP

#define USBHS_PORTSC1_HSP | ( |  | x | ) | USB_PORTSC1_HSP(x)

Definition at line 42693 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_HSP_MASK

#define USBHS_PORTSC1_HSP_MASK USB_PORTSC1_HSP_MASK

Definition at line 42691 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_HSP_SHIFT

#define USBHS_PORTSC1_HSP_SHIFT USB_PORTSC1_HSP_SHIFT

Definition at line 42692 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_LS

#define USBHS_PORTSC1_LS | ( |  | x | ) | USB_PORTSC1_LS(x)

Definition at line 42696 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_LS_MASK

#define USBHS_PORTSC1_LS_MASK USB_PORTSC1_LS_MASK

Definition at line 42694 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_LS_SHIFT

#define USBHS_PORTSC1_LS_SHIFT USB_PORTSC1_LS_SHIFT

Definition at line 42695 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_OCA

#define USBHS_PORTSC1_OCA | ( |  | x | ) | USB_PORTSC1_OCA(x)

Definition at line 42678 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_OCA_MASK

#define USBHS_PORTSC1_OCA_MASK USB_PORTSC1_OCA_MASK

Definition at line 42676 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_OCA_SHIFT

#define USBHS_PORTSC1_OCA_SHIFT USB_PORTSC1_OCA_SHIFT

Definition at line 42677 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_OCC

#define USBHS_PORTSC1_OCC | ( |  | x | ) | USB_PORTSC1_OCC(x)

Definition at line 42681 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_OCC_MASK

#define USBHS_PORTSC1_OCC_MASK USB_PORTSC1_OCC_MASK

Definition at line 42679 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_OCC_SHIFT

#define USBHS_PORTSC1_OCC_SHIFT USB_PORTSC1_OCC_SHIFT

Definition at line 42680 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PE

#define USBHS_PORTSC1_PE | ( |  | x | ) | USB_PORTSC1_PE(x)

Definition at line 42672 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PE_MASK

#define USBHS_PORTSC1_PE_MASK USB_PORTSC1_PE_MASK

Definition at line 42670 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PE_SHIFT

#define USBHS_PORTSC1_PE_SHIFT USB_PORTSC1_PE_SHIFT

Definition at line 42671 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PEC

#define USBHS_PORTSC1_PEC | ( |  | x | ) | USB_PORTSC1_PEC(x)

Definition at line 42675 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PEC_MASK

#define USBHS_PORTSC1_PEC_MASK USB_PORTSC1_PEC_MASK

Definition at line 42673 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PEC_SHIFT

#define USBHS_PORTSC1_PEC_SHIFT USB_PORTSC1_PEC_SHIFT

Definition at line 42674 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PFSC

#define USBHS_PORTSC1_PFSC | ( |  | x | ) | USB_PORTSC1_PFSC(x)

Definition at line 42723 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PFSC_MASK

#define USBHS_PORTSC1_PFSC_MASK USB_PORTSC1_PFSC_MASK

Definition at line 42721 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PFSC_SHIFT

#define USBHS_PORTSC1_PFSC_SHIFT USB_PORTSC1_PFSC_SHIFT

Definition at line 42722 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PHCD

#define USBHS_PORTSC1_PHCD | ( |  | x | ) | USB_PORTSC1_PHCD(x)

Definition at line 42720 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PHCD_MASK

#define USBHS_PORTSC1_PHCD_MASK USB_PORTSC1_PHCD_MASK

Definition at line 42718 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PHCD_SHIFT

#define USBHS_PORTSC1_PHCD_SHIFT USB_PORTSC1_PHCD_SHIFT

Definition at line 42719 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PIC

#define USBHS_PORTSC1_PIC | ( |  | x | ) | USB_PORTSC1_PIC(x)

Definition at line 42705 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PIC_MASK

#define USBHS_PORTSC1_PIC_MASK USB_PORTSC1_PIC_MASK

Definition at line 42703 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PIC_SHIFT

#define USBHS_PORTSC1_PIC_SHIFT USB_PORTSC1_PIC_SHIFT

Definition at line 42704 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PO

#define USBHS_PORTSC1_PO | ( |  | x | ) | USB_PORTSC1_PO(x)

Definition at line 42702 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PO_MASK

#define USBHS_PORTSC1_PO_MASK USB_PORTSC1_PO_MASK

Definition at line 42700 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PO_SHIFT

#define USBHS_PORTSC1_PO_SHIFT USB_PORTSC1_PO_SHIFT

Definition at line 42701 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PP

#define USBHS_PORTSC1_PP | ( |  | x | ) | USB_PORTSC1_PP(x)

Definition at line 42699 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PP_MASK

#define USBHS_PORTSC1_PP_MASK USB_PORTSC1_PP_MASK

Definition at line 42697 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PP_SHIFT

#define USBHS_PORTSC1_PP_SHIFT USB_PORTSC1_PP_SHIFT

Definition at line 42698 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PR

#define USBHS_PORTSC1_PR | ( |  | x | ) | USB_PORTSC1_PR(x)

Definition at line 42690 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PR_MASK

#define USBHS_PORTSC1_PR_MASK USB_PORTSC1_PR_MASK

Definition at line 42688 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PR_SHIFT

#define USBHS_PORTSC1_PR_SHIFT USB_PORTSC1_PR_SHIFT

Definition at line 42689 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PSPD

#define USBHS_PORTSC1_PSPD | ( |  | x | ) | USB_PORTSC1_PSPD(x)

Definition at line 42729 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PSPD_MASK

#define USBHS_PORTSC1_PSPD_MASK USB_PORTSC1_PSPD_MASK

Definition at line 42727 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PSPD_SHIFT

#define USBHS_PORTSC1_PSPD_SHIFT USB_PORTSC1_PSPD_SHIFT

Definition at line 42728 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTC

#define USBHS_PORTSC1_PTC | ( |  | x | ) | USB_PORTSC1_PTC(x)

Definition at line 42708 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTC_MASK

#define USBHS_PORTSC1_PTC_MASK USB_PORTSC1_PTC_MASK

Definition at line 42706 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTC_SHIFT

#define USBHS_PORTSC1_PTC_SHIFT USB_PORTSC1_PTC_SHIFT

Definition at line 42707 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTS

#define USBHS_PORTSC1_PTS | ( |  | x | ) | USB_PORTSC1_PTS_1(x)

Definition at line 42738 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTS2

#define USBHS_PORTSC1_PTS2 | ( |  | x | ) | USB_PORTSC1_PTS_2(x)

Definition at line 42726 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTS2_MASK

#define USBHS_PORTSC1_PTS2_MASK USB_PORTSC1_PTS_2_MASK

Definition at line 42724 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTS2_SHIFT

#define USBHS_PORTSC1_PTS2_SHIFT USB_PORTSC1_PTS_2_SHIFT

Definition at line 42725 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTS_MASK

#define USBHS_PORTSC1_PTS_MASK USB_PORTSC1_PTS_1_MASK

Definition at line 42736 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTS_SHIFT

#define USBHS_PORTSC1_PTS_SHIFT USB_PORTSC1_PTS_1_SHIFT

Definition at line 42737 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTW

#define USBHS_PORTSC1_PTW | ( |  | x | ) | USB_PORTSC1_PTW(x)

Definition at line 42732 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTW_MASK

#define USBHS_PORTSC1_PTW_MASK USB_PORTSC1_PTW_MASK

Definition at line 42730 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_PTW_SHIFT

#define USBHS_PORTSC1_PTW_SHIFT USB_PORTSC1_PTW_SHIFT

Definition at line 42731 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_STS

#define USBHS_PORTSC1_STS | ( |  | x | ) | USB_PORTSC1_STS(x)

Definition at line 42735 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_STS_MASK

#define USBHS_PORTSC1_STS_MASK USB_PORTSC1_STS_MASK

Definition at line 42733 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_STS_SHIFT

#define USBHS_PORTSC1_STS_SHIFT USB_PORTSC1_STS_SHIFT

Definition at line 42734 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_SUSP

#define USBHS_PORTSC1_SUSP | ( |  | x | ) | USB_PORTSC1_SUSP(x)

Definition at line 42687 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_SUSP_MASK

#define USBHS_PORTSC1_SUSP_MASK USB_PORTSC1_SUSP_MASK

Definition at line 42685 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_SUSP_SHIFT

#define USBHS_PORTSC1_SUSP_SHIFT USB_PORTSC1_SUSP_SHIFT

Definition at line 42686 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKCN

#define USBHS_PORTSC1_WKCN | ( |  | x | ) | USB_PORTSC1_WKCN(x)

Definition at line 42711 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKCN_MASK

#define USBHS_PORTSC1_WKCN_MASK USB_PORTSC1_WKCN_MASK

Definition at line 42709 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKCN_SHIFT

#define USBHS_PORTSC1_WKCN_SHIFT USB_PORTSC1_WKCN_SHIFT

Definition at line 42710 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKDS

#define USBHS_PORTSC1_WKDS | ( |  | x | ) | USB_PORTSC1_WKDC(x)

Definition at line 42714 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKDS_MASK

#define USBHS_PORTSC1_WKDS_MASK USB_PORTSC1_WKDC_MASK

Definition at line 42712 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKDS_SHIFT

#define USBHS_PORTSC1_WKDS_SHIFT USB_PORTSC1_WKDC_SHIFT

Definition at line 42713 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKOC

#define USBHS_PORTSC1_WKOC | ( |  | x | ) | USB_PORTSC1_WKOC(x)

Definition at line 42717 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKOC_MASK

#define USBHS_PORTSC1_WKOC_MASK USB_PORTSC1_WKOC_MASK

Definition at line 42715 of file MIMXRT1062.h.

## ◆ USBHS_PORTSC1_WKOC_SHIFT

#define USBHS_PORTSC1_WKOC_SHIFT USB_PORTSC1_WKOC_SHIFT

Definition at line 42716 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXFIFOTHRES

#define USBHS_TXFILLTUNING_TXFIFOTHRES | ( |  | x | ) | USB_TXFILLTUNING_TXFIFOTHRES(x)

Definition at line 42648 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXFIFOTHRES_MASK

#define USBHS_TXFILLTUNING_TXFIFOTHRES_MASK USB_TXFILLTUNING_TXFIFOTHRES_MASK

Definition at line 42646 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXFIFOTHRES_SHIFT

#define USBHS_TXFILLTUNING_TXFIFOTHRES_SHIFT USB_TXFILLTUNING_TXFIFOTHRES_SHIFT

Definition at line 42647 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXSCHHEALTH

#define USBHS_TXFILLTUNING_TXSCHHEALTH | ( |  | x | ) | USB_TXFILLTUNING_TXSCHHEALTH(x)

Definition at line 42645 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXSCHHEALTH_MASK

#define USBHS_TXFILLTUNING_TXSCHHEALTH_MASK USB_TXFILLTUNING_TXSCHHEALTH_MASK

Definition at line 42643 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXSCHHEALTH_SHIFT

#define USBHS_TXFILLTUNING_TXSCHHEALTH_SHIFT USB_TXFILLTUNING_TXSCHHEALTH_SHIFT

Definition at line 42644 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXSCHOH

#define USBHS_TXFILLTUNING_TXSCHOH | ( |  | x | ) | USB_TXFILLTUNING_TXSCHOH(x)

Definition at line 42642 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXSCHOH_MASK

#define USBHS_TXFILLTUNING_TXSCHOH_MASK USB_TXFILLTUNING_TXSCHOH_MASK

Definition at line 42640 of file MIMXRT1062.h.

## ◆ USBHS_TXFILLTUNING_TXSCHOH_SHIFT

#define USBHS_TXFILLTUNING_TXSCHOH_SHIFT USB_TXFILLTUNING_TXSCHOH_SHIFT

Definition at line 42641 of file MIMXRT1062.h.

## ◆ USBHS_Type

#define USBHS_Type USB_Type

Definition at line 42911 of file MIMXRT1062.h.

## ◆ USBHS_USB_SBUSCFG_BURSTMODE

#define USBHS_USB_SBUSCFG_BURSTMODE | ( |  | x | ) | USB_SBUSCFG_AHBBRST(x)

Definition at line 42431 of file MIMXRT1062.h.

## ◆ USBHS_USB_SBUSCFG_BURSTMODE_MASK

#define USBHS_USB_SBUSCFG_BURSTMODE_MASK USB_SBUSCFG_AHBBRST_MASK

Definition at line 42429 of file MIMXRT1062.h.

## ◆ USBHS_USB_SBUSCFG_BURSTMODE_SHIFT

#define USBHS_USB_SBUSCFG_BURSTMODE_SHIFT USB_SBUSCFG_AHBBRST_SHIFT

Definition at line 42430 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASE

#define USBHS_USBCMD_ASE | ( |  | x | ) | USB_USBCMD_ASE(x)

Definition at line 42498 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASE_MASK

#define USBHS_USBCMD_ASE_MASK USB_USBCMD_ASE_MASK

Definition at line 42496 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASE_SHIFT

#define USBHS_USBCMD_ASE_SHIFT USB_USBCMD_ASE_SHIFT

Definition at line 42497 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASP

#define USBHS_USBCMD_ASP | ( |  | x | ) | USB_USBCMD_ASP(x)

Definition at line 42504 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASP_MASK

#define USBHS_USBCMD_ASP_MASK USB_USBCMD_ASP_MASK

Definition at line 42502 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASP_SHIFT

#define USBHS_USBCMD_ASP_SHIFT USB_USBCMD_ASP_SHIFT

Definition at line 42503 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASPE

#define USBHS_USBCMD_ASPE | ( |  | x | ) | USB_USBCMD_ASPE(x)

Definition at line 42507 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASPE_MASK

#define USBHS_USBCMD_ASPE_MASK USB_USBCMD_ASPE_MASK

Definition at line 42505 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ASPE_SHIFT

#define USBHS_USBCMD_ASPE_SHIFT USB_USBCMD_ASPE_SHIFT

Definition at line 42506 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ATDTW

#define USBHS_USBCMD_ATDTW | ( |  | x | ) | USB_USBCMD_ATDTW(x)

Definition at line 42510 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ATDTW_MASK

#define USBHS_USBCMD_ATDTW_MASK USB_USBCMD_ATDTW_MASK

Definition at line 42508 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ATDTW_SHIFT

#define USBHS_USBCMD_ATDTW_SHIFT USB_USBCMD_ATDTW_SHIFT

Definition at line 42509 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_FS

#define USBHS_USBCMD_FS | ( |  | x | ) | USB_USBCMD_FS_1(x)

Definition at line 42492 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_FS2

#define USBHS_USBCMD_FS2 | ( |  | x | ) | USB_USBCMD_FS_2(x)

Definition at line 42516 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_FS2_MASK

#define USBHS_USBCMD_FS2_MASK USB_USBCMD_FS_2_MASK

Definition at line 42514 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_FS2_SHIFT

#define USBHS_USBCMD_FS2_SHIFT USB_USBCMD_FS_2_SHIFT

Definition at line 42515 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_FS_MASK

#define USBHS_USBCMD_FS_MASK USB_USBCMD_FS_1_MASK

Definition at line 42490 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_FS_SHIFT

#define USBHS_USBCMD_FS_SHIFT USB_USBCMD_FS_1_SHIFT

Definition at line 42491 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_IAA

#define USBHS_USBCMD_IAA | ( |  | x | ) | USB_USBCMD_IAA(x)

Definition at line 42501 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_IAA_MASK

#define USBHS_USBCMD_IAA_MASK USB_USBCMD_IAA_MASK

Definition at line 42499 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_IAA_SHIFT

#define USBHS_USBCMD_IAA_SHIFT USB_USBCMD_IAA_SHIFT

Definition at line 42500 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ITC

#define USBHS_USBCMD_ITC | ( |  | x | ) | USB_USBCMD_ITC(x)

Definition at line 42519 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ITC_MASK

#define USBHS_USBCMD_ITC_MASK USB_USBCMD_ITC_MASK

Definition at line 42517 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_ITC_SHIFT

#define USBHS_USBCMD_ITC_SHIFT USB_USBCMD_ITC_SHIFT

Definition at line 42518 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_PSE

#define USBHS_USBCMD_PSE | ( |  | x | ) | USB_USBCMD_PSE(x)

Definition at line 42495 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_PSE_MASK

#define USBHS_USBCMD_PSE_MASK USB_USBCMD_PSE_MASK

Definition at line 42493 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_PSE_SHIFT

#define USBHS_USBCMD_PSE_SHIFT USB_USBCMD_PSE_SHIFT

Definition at line 42494 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_RS

#define USBHS_USBCMD_RS | ( |  | x | ) | USB_USBCMD_RS(x)

Definition at line 42486 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_RS_MASK

#define USBHS_USBCMD_RS_MASK USB_USBCMD_RS_MASK

Definition at line 42484 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_RS_SHIFT

#define USBHS_USBCMD_RS_SHIFT USB_USBCMD_RS_SHIFT

Definition at line 42485 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_RST

#define USBHS_USBCMD_RST | ( |  | x | ) | USB_USBCMD_RST(x)

Definition at line 42489 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_RST_MASK

#define USBHS_USBCMD_RST_MASK USB_USBCMD_RST_MASK

Definition at line 42487 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_RST_SHIFT

#define USBHS_USBCMD_RST_SHIFT USB_USBCMD_RST_SHIFT

Definition at line 42488 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_SUTW

#define USBHS_USBCMD_SUTW | ( |  | x | ) | USB_USBCMD_SUTW(x)

Definition at line 42513 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_SUTW_MASK

#define USBHS_USBCMD_SUTW_MASK USB_USBCMD_SUTW_MASK

Definition at line 42511 of file MIMXRT1062.h.

## ◆ USBHS_USBCMD_SUTW_SHIFT

#define USBHS_USBCMD_SUTW_SHIFT USB_USBCMD_SUTW_SHIFT

Definition at line 42512 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_AAE

#define USBHS_USBINTR_AAE | ( |  | x | ) | USB_USBINTR_AAE(x)

Definition at line 42588 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_AAE_MASK

#define USBHS_USBINTR_AAE_MASK USB_USBINTR_AAE_MASK

Definition at line 42586 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_AAE_SHIFT

#define USBHS_USBINTR_AAE_SHIFT USB_USBINTR_AAE_SHIFT

Definition at line 42587 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_FRE

#define USBHS_USBINTR_FRE | ( |  | x | ) | USB_USBINTR_FRE(x)

Definition at line 42582 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_FRE_MASK

#define USBHS_USBINTR_FRE_MASK USB_USBINTR_FRE_MASK

Definition at line 42580 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_FRE_SHIFT

#define USBHS_USBINTR_FRE_SHIFT USB_USBINTR_FRE_SHIFT

Definition at line 42581 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_NAKE

#define USBHS_USBINTR_NAKE | ( |  | x | ) | USB_USBINTR_NAKE(x)

Definition at line 42603 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_NAKE_MASK

#define USBHS_USBINTR_NAKE_MASK USB_USBINTR_NAKE_MASK

Definition at line 42601 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_NAKE_SHIFT

#define USBHS_USBINTR_NAKE_SHIFT USB_USBINTR_NAKE_SHIFT

Definition at line 42602 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_PCE

#define USBHS_USBINTR_PCE | ( |  | x | ) | USB_USBINTR_PCE(x)

Definition at line 42579 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_PCE_MASK

#define USBHS_USBINTR_PCE_MASK USB_USBINTR_PCE_MASK

Definition at line 42577 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_PCE_SHIFT

#define USBHS_USBINTR_PCE_SHIFT USB_USBINTR_PCE_SHIFT

Definition at line 42578 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SEE

#define USBHS_USBINTR_SEE | ( |  | x | ) | USB_USBINTR_SEE(x)

Definition at line 42585 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SEE_MASK

#define USBHS_USBINTR_SEE_MASK USB_USBINTR_SEE_MASK

Definition at line 42583 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SEE_SHIFT

#define USBHS_USBINTR_SEE_SHIFT USB_USBINTR_SEE_SHIFT

Definition at line 42584 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SLE

#define USBHS_USBINTR_SLE | ( |  | x | ) | USB_USBINTR_SLE(x)

Definition at line 42597 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SLE_MASK

#define USBHS_USBINTR_SLE_MASK USB_USBINTR_SLE_MASK

Definition at line 42595 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SLE_SHIFT

#define USBHS_USBINTR_SLE_SHIFT USB_USBINTR_SLE_SHIFT

Definition at line 42596 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SRE

#define USBHS_USBINTR_SRE | ( |  | x | ) | USB_USBINTR_SRE(x)

Definition at line 42594 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SRE_MASK

#define USBHS_USBINTR_SRE_MASK USB_USBINTR_SRE_MASK

Definition at line 42592 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_SRE_SHIFT

#define USBHS_USBINTR_SRE_SHIFT USB_USBINTR_SRE_SHIFT

Definition at line 42593 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_TIE0

#define USBHS_USBINTR_TIE0 | ( |  | x | ) | USB_USBINTR_TIE0(x)

Definition at line 42612 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_TIE0_MASK

#define USBHS_USBINTR_TIE0_MASK USB_USBINTR_TIE0_MASK

Definition at line 42610 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_TIE0_SHIFT

#define USBHS_USBINTR_TIE0_SHIFT USB_USBINTR_TIE0_SHIFT

Definition at line 42611 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_TIE1

#define USBHS_USBINTR_TIE1 | ( |  | x | ) | USB_USBINTR_TIE1(x)

Definition at line 42615 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_TIE1_MASK

#define USBHS_USBINTR_TIE1_MASK USB_USBINTR_TIE1_MASK

Definition at line 42613 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_TIE1_SHIFT

#define USBHS_USBINTR_TIE1_SHIFT USB_USBINTR_TIE1_SHIFT

Definition at line 42614 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UAIE

#define USBHS_USBINTR_UAIE | ( |  | x | ) | USB_USBINTR_UAIE(x)

Definition at line 42606 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UAIE_MASK

#define USBHS_USBINTR_UAIE_MASK USB_USBINTR_UAIE_MASK

Definition at line 42604 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UAIE_SHIFT

#define USBHS_USBINTR_UAIE_SHIFT USB_USBINTR_UAIE_SHIFT

Definition at line 42605 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UE

#define USBHS_USBINTR_UE | ( |  | x | ) | USB_USBINTR_UE(x)

Definition at line 42573 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UE_MASK

#define USBHS_USBINTR_UE_MASK USB_USBINTR_UE_MASK

Definition at line 42571 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UE_SHIFT

#define USBHS_USBINTR_UE_SHIFT USB_USBINTR_UE_SHIFT

Definition at line 42572 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UEE

#define USBHS_USBINTR_UEE | ( |  | x | ) | USB_USBINTR_UEE(x)

Definition at line 42576 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UEE_MASK

#define USBHS_USBINTR_UEE_MASK USB_USBINTR_UEE_MASK

Definition at line 42574 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UEE_SHIFT

#define USBHS_USBINTR_UEE_SHIFT USB_USBINTR_UEE_SHIFT

Definition at line 42575 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_ULPIE

#define USBHS_USBINTR_ULPIE | ( |  | x | ) | USB_USBINTR_ULPIE(x)

Definition at line 42600 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_ULPIE_MASK

#define USBHS_USBINTR_ULPIE_MASK USB_USBINTR_ULPIE_MASK

Definition at line 42598 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_ULPIE_SHIFT

#define USBHS_USBINTR_ULPIE_SHIFT USB_USBINTR_ULPIE_SHIFT

Definition at line 42599 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UPIE

#define USBHS_USBINTR_UPIE | ( |  | x | ) | USB_USBINTR_UPIE(x)

Definition at line 42609 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UPIE_MASK

#define USBHS_USBINTR_UPIE_MASK USB_USBINTR_UPIE_MASK

Definition at line 42607 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_UPIE_SHIFT

#define USBHS_USBINTR_UPIE_SHIFT USB_USBINTR_UPIE_SHIFT

Definition at line 42608 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_URE

#define USBHS_USBINTR_URE | ( |  | x | ) | USB_USBINTR_URE(x)

Definition at line 42591 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_URE_MASK

#define USBHS_USBINTR_URE_MASK USB_USBINTR_URE_MASK

Definition at line 42589 of file MIMXRT1062.h.

## ◆ USBHS_USBINTR_URE_SHIFT

#define USBHS_USBINTR_URE_SHIFT USB_USBINTR_URE_SHIFT

Definition at line 42590 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_CM

#define USBHS_USBMODE_CM | ( |  | x | ) | USB_USBMODE_CM(x)

Definition at line 42819 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_CM_MASK

#define USBHS_USBMODE_CM_MASK USB_USBMODE_CM_MASK

Definition at line 42817 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_CM_SHIFT

#define USBHS_USBMODE_CM_SHIFT USB_USBMODE_CM_SHIFT

Definition at line 42818 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_ES

#define USBHS_USBMODE_ES | ( |  | x | ) | USB_USBMODE_ES(x)

Definition at line 42822 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_ES_MASK

#define USBHS_USBMODE_ES_MASK USB_USBMODE_ES_MASK

Definition at line 42820 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_ES_SHIFT

#define USBHS_USBMODE_ES_SHIFT USB_USBMODE_ES_SHIFT

Definition at line 42821 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_SDIS

#define USBHS_USBMODE_SDIS | ( |  | x | ) | USB_USBMODE_SDIS(x)

Definition at line 42828 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_SDIS_MASK

#define USBHS_USBMODE_SDIS_MASK USB_USBMODE_SDIS_MASK

Definition at line 42826 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_SDIS_SHIFT

#define USBHS_USBMODE_SDIS_SHIFT USB_USBMODE_SDIS_SHIFT

Definition at line 42827 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_SLOM

#define USBHS_USBMODE_SLOM | ( |  | x | ) | USB_USBMODE_SLOM(x)

Definition at line 42825 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_SLOM_MASK

#define USBHS_USBMODE_SLOM_MASK USB_USBMODE_SLOM_MASK

Definition at line 42823 of file MIMXRT1062.h.

## ◆ USBHS_USBMODE_SLOM_SHIFT

#define USBHS_USBMODE_SLOM_SHIFT USB_USBMODE_SLOM_SHIFT

Definition at line 42824 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_AAI

#define USBHS_USBSTS_AAI | ( |  | x | ) | USB_USBSTS_AAI(x)

Definition at line 42537 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_AAI_MASK

#define USBHS_USBSTS_AAI_MASK USB_USBSTS_AAI_MASK

Definition at line 42535 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_AAI_SHIFT

#define USBHS_USBSTS_AAI_SHIFT USB_USBSTS_AAI_SHIFT

Definition at line 42536 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_AS

#define USBHS_USBSTS_AS | ( |  | x | ) | USB_USBSTS_AS(x)

Definition at line 42561 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_AS_MASK

#define USBHS_USBSTS_AS_MASK USB_USBSTS_AS_MASK

Definition at line 42559 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_AS_SHIFT

#define USBHS_USBSTS_AS_SHIFT USB_USBSTS_AS_SHIFT

Definition at line 42560 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_FRI

#define USBHS_USBSTS_FRI | ( |  | x | ) | USB_USBSTS_FRI(x)

Definition at line 42531 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_FRI_MASK

#define USBHS_USBSTS_FRI_MASK USB_USBSTS_FRI_MASK

Definition at line 42529 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_FRI_SHIFT

#define USBHS_USBSTS_FRI_SHIFT USB_USBSTS_FRI_SHIFT

Definition at line 42530 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_HCH

#define USBHS_USBSTS_HCH | ( |  | x | ) | USB_USBSTS_HCH(x)

Definition at line 42552 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_HCH_MASK

#define USBHS_USBSTS_HCH_MASK USB_USBSTS_HCH_MASK

Definition at line 42550 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_HCH_SHIFT

#define USBHS_USBSTS_HCH_SHIFT USB_USBSTS_HCH_SHIFT

Definition at line 42551 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_NAKI

#define USBHS_USBSTS_NAKI | ( |  | x | ) | USB_USBSTS_NAKI(x)

Definition at line 42564 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_NAKI_MASK

#define USBHS_USBSTS_NAKI_MASK USB_USBSTS_NAKI_MASK

Definition at line 42562 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_NAKI_SHIFT

#define USBHS_USBSTS_NAKI_SHIFT USB_USBSTS_NAKI_SHIFT

Definition at line 42563 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_PCI

#define USBHS_USBSTS_PCI | ( |  | x | ) | USB_USBSTS_PCI(x)

Definition at line 42528 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_PCI_MASK

#define USBHS_USBSTS_PCI_MASK USB_USBSTS_PCI_MASK

Definition at line 42526 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_PCI_SHIFT

#define USBHS_USBSTS_PCI_SHIFT USB_USBSTS_PCI_SHIFT

Definition at line 42527 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_PS

#define USBHS_USBSTS_PS | ( |  | x | ) | USB_USBSTS_PS(x)

Definition at line 42558 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_PS_MASK

#define USBHS_USBSTS_PS_MASK USB_USBSTS_PS_MASK

Definition at line 42556 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_PS_SHIFT

#define USBHS_USBSTS_PS_SHIFT USB_USBSTS_PS_SHIFT

Definition at line 42557 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_RCL

#define USBHS_USBSTS_RCL | ( |  | x | ) | USB_USBSTS_RCL(x)

Definition at line 42555 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_RCL_MASK

#define USBHS_USBSTS_RCL_MASK USB_USBSTS_RCL_MASK

Definition at line 42553 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_RCL_SHIFT

#define USBHS_USBSTS_RCL_SHIFT USB_USBSTS_RCL_SHIFT

Definition at line 42554 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SEI

#define USBHS_USBSTS_SEI | ( |  | x | ) | USB_USBSTS_SEI(x)

Definition at line 42534 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SEI_MASK

#define USBHS_USBSTS_SEI_MASK USB_USBSTS_SEI_MASK

Definition at line 42532 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SEI_SHIFT

#define USBHS_USBSTS_SEI_SHIFT USB_USBSTS_SEI_SHIFT

Definition at line 42533 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SLI

#define USBHS_USBSTS_SLI | ( |  | x | ) | USB_USBSTS_SLI(x)

Definition at line 42546 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SLI_MASK

#define USBHS_USBSTS_SLI_MASK USB_USBSTS_SLI_MASK

Definition at line 42544 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SLI_SHIFT

#define USBHS_USBSTS_SLI_SHIFT USB_USBSTS_SLI_SHIFT

Definition at line 42545 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SRI

#define USBHS_USBSTS_SRI | ( |  | x | ) | USB_USBSTS_SRI(x)

Definition at line 42543 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SRI_MASK

#define USBHS_USBSTS_SRI_MASK USB_USBSTS_SRI_MASK

Definition at line 42541 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_SRI_SHIFT

#define USBHS_USBSTS_SRI_SHIFT USB_USBSTS_SRI_SHIFT

Definition at line 42542 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_TI0

#define USBHS_USBSTS_TI0 | ( |  | x | ) | USB_USBSTS_TI0(x)

Definition at line 42567 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_TI0_MASK

#define USBHS_USBSTS_TI0_MASK USB_USBSTS_TI0_MASK

Definition at line 42565 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_TI0_SHIFT

#define USBHS_USBSTS_TI0_SHIFT USB_USBSTS_TI0_SHIFT

Definition at line 42566 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_TI1

#define USBHS_USBSTS_TI1 | ( |  | x | ) | USB_USBSTS_TI1(x)

Definition at line 42570 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_TI1_MASK

#define USBHS_USBSTS_TI1_MASK USB_USBSTS_TI1_MASK

Definition at line 42568 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_TI1_SHIFT

#define USBHS_USBSTS_TI1_SHIFT USB_USBSTS_TI1_SHIFT

Definition at line 42569 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_UEI

#define USBHS_USBSTS_UEI | ( |  | x | ) | USB_USBSTS_UEI(x)

Definition at line 42525 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_UEI_MASK

#define USBHS_USBSTS_UEI_MASK USB_USBSTS_UEI_MASK

Definition at line 42523 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_UEI_SHIFT

#define USBHS_USBSTS_UEI_SHIFT USB_USBSTS_UEI_SHIFT

Definition at line 42524 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_UI

#define USBHS_USBSTS_UI | ( |  | x | ) | USB_USBSTS_UI(x)

Definition at line 42522 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_UI_MASK

#define USBHS_USBSTS_UI_MASK USB_USBSTS_UI_MASK

Definition at line 42520 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_UI_SHIFT

#define USBHS_USBSTS_UI_SHIFT USB_USBSTS_UI_SHIFT

Definition at line 42521 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_ULPII

#define USBHS_USBSTS_ULPII | ( |  | x | ) | USB_USBSTS_ULPII(x)

Definition at line 42549 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_ULPII_MASK

#define USBHS_USBSTS_ULPII_MASK USB_USBSTS_ULPII_MASK

Definition at line 42547 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_ULPII_SHIFT

#define USBHS_USBSTS_ULPII_SHIFT USB_USBSTS_ULPII_SHIFT

Definition at line 42548 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_URI

#define USBHS_USBSTS_URI | ( |  | x | ) | USB_USBSTS_URI(x)

Definition at line 42540 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_URI_MASK

#define USBHS_USBSTS_URI_MASK USB_USBSTS_URI_MASK

Definition at line 42538 of file MIMXRT1062.h.

## ◆ USBHS_USBSTS_URI_SHIFT

#define USBHS_USBSTS_URI_SHIFT USB_USBSTS_URI_SHIFT

Definition at line 42539 of file MIMXRT1062.h.