Callisto4Bootloader: USBPHY_Type Struct Reference

Callisto4Bootloader

Data Fields
USBPHY_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » USBPHY Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | PWD
__IO uint32_t | PWD_SET
__IO uint32_t | PWD_CLR
__IO uint32_t | PWD_TOG
__IO uint32_t | TX
__IO uint32_t | TX_SET
__IO uint32_t | TX_CLR
__IO uint32_t | TX_TOG
__IO uint32_t | RX
__IO uint32_t | RX_SET
__IO uint32_t | RX_CLR
__IO uint32_t | RX_TOG
__IO uint32_t | CTRL
__IO uint32_t | CTRL_SET
__IO uint32_t | CTRL_CLR
__IO uint32_t | CTRL_TOG
__IO uint32_t | STATUS
uint8_t | RESERVED_0 [12]
__IO uint32_t | DEBUGr
__IO uint32_t | DEBUG_SET
__IO uint32_t | DEBUG_CLR
__IO uint32_t | DEBUG_TOG
__I uint32_t | DEBUG0_STATUS
uint8_t | RESERVED_1 [12]
__IO uint32_t | DEBUG1
__IO uint32_t | DEBUG1_SET
__IO uint32_t | DEBUG1_CLR
__IO uint32_t | DEBUG1_TOG
__I uint32_t | VERSION

## Detailed Description

USBPHY - Register Layout Typedef

Definition at line 43068 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h