Callisto4Bootloader: ADC Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
ADC Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| ADC Register Masks

## Data Structures

struct | ADC_Type

## Macros

#define | ADC1_BASE (0x400C4000u)
#define | ADC1 ((ADC_Type *)ADC1_BASE)
#define | ADC2_BASE (0x400C8000u)
#define | ADC2 ((ADC_Type *)ADC2_BASE)
#define | ADC_BASE_ADDRS { 0u, ADC1_BASE, ADC2_BASE }
#define | ADC_BASE_PTRS { (ADC_Type *)0u, ADC1, ADC2 }
#define | ADC_IRQS { NotAvail_IRQn, ADC1_IRQn, ADC2_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ ADC1

#define ADC1 ((ADC_Type *)ADC1_BASE)

Peripheral ADC1 base pointer

Definition at line 1716 of file MIMXRT1062.h.

## ◆ ADC1_BASE

#define ADC1_BASE (0x400C4000u)

Peripheral ADC1 base address

Definition at line 1714 of file MIMXRT1062.h.

## ◆ ADC2

#define ADC2 ((ADC_Type *)ADC2_BASE)

Peripheral ADC2 base pointer

Definition at line 1720 of file MIMXRT1062.h.

## ◆ ADC2_BASE

#define ADC2_BASE (0x400C8000u)

Peripheral ADC2 base address

Definition at line 1718 of file MIMXRT1062.h.

## ◆ ADC_BASE_ADDRS

#define ADC_BASE_ADDRS { 0u, ADC1_BASE, ADC2_BASE }

Array initializer of ADC peripheral base addresses

Definition at line 1722 of file MIMXRT1062.h.

## ◆ ADC_BASE_PTRS

#define ADC_BASE_PTRS { (ADC_Type *)0u, ADC1, ADC2 }

Array initializer of ADC peripheral base pointers

Definition at line 1724 of file MIMXRT1062.h.

## ◆ ADC_IRQS

#define ADC_IRQS { NotAvail_IRQn, ADC1_IRQn, ADC2_IRQn }

Interrupt vectors for the ADC peripheral type

Definition at line 1726 of file MIMXRT1062.h.