Callisto4Bootloader: XBARA Register Masks

Callisto4Bootloader

XBARA Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » XBARA Peripheral Access Layer

## SEL0 - Crossbar A Select Register 0

#define | XBARA_SEL0_SEL0_MASK (0x7FU)
#define | XBARA_SEL0_SEL0_SHIFT (0U)
#define | XBARA_SEL0_SEL0(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL0_SEL0_SHIFT)) & XBARA_SEL0_SEL0_MASK)
#define | XBARA_SEL0_SEL1_MASK (0x7F00U)
#define | XBARA_SEL0_SEL1_SHIFT (8U)
#define | XBARA_SEL0_SEL1(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL0_SEL1_SHIFT)) & XBARA_SEL0_SEL1_MASK)

## SEL1 - Crossbar A Select Register 1

#define | XBARA_SEL1_SEL2_MASK (0x7FU)
#define | XBARA_SEL1_SEL2_SHIFT (0U)
#define | XBARA_SEL1_SEL2(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL1_SEL2_SHIFT)) & XBARA_SEL1_SEL2_MASK)
#define | XBARA_SEL1_SEL3_MASK (0x7F00U)
#define | XBARA_SEL1_SEL3_SHIFT (8U)
#define | XBARA_SEL1_SEL3(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL1_SEL3_SHIFT)) & XBARA_SEL1_SEL3_MASK)

## SEL2 - Crossbar A Select Register 2

#define | XBARA_SEL2_SEL4_MASK (0x7FU)
#define | XBARA_SEL2_SEL4_SHIFT (0U)
#define | XBARA_SEL2_SEL4(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL2_SEL4_SHIFT)) & XBARA_SEL2_SEL4_MASK)
#define | XBARA_SEL2_SEL5_MASK (0x7F00U)
#define | XBARA_SEL2_SEL5_SHIFT (8U)
#define | XBARA_SEL2_SEL5(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL2_SEL5_SHIFT)) & XBARA_SEL2_SEL5_MASK)

## SEL3 - Crossbar A Select Register 3

#define | XBARA_SEL3_SEL6_MASK (0x7FU)
#define | XBARA_SEL3_SEL6_SHIFT (0U)
#define | XBARA_SEL3_SEL6(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL3_SEL6_SHIFT)) & XBARA_SEL3_SEL6_MASK)
#define | XBARA_SEL3_SEL7_MASK (0x7F00U)
#define | XBARA_SEL3_SEL7_SHIFT (8U)
#define | XBARA_SEL3_SEL7(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL3_SEL7_SHIFT)) & XBARA_SEL3_SEL7_MASK)

## SEL4 - Crossbar A Select Register 4

#define | XBARA_SEL4_SEL8_MASK (0x7FU)
#define | XBARA_SEL4_SEL8_SHIFT (0U)
#define | XBARA_SEL4_SEL8(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL4_SEL8_SHIFT)) & XBARA_SEL4_SEL8_MASK)
#define | XBARA_SEL4_SEL9_MASK (0x7F00U)
#define | XBARA_SEL4_SEL9_SHIFT (8U)
#define | XBARA_SEL4_SEL9(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL4_SEL9_SHIFT)) & XBARA_SEL4_SEL9_MASK)

## SEL5 - Crossbar A Select Register 5

#define | XBARA_SEL5_SEL10_MASK (0x7FU)
#define | XBARA_SEL5_SEL10_SHIFT (0U)
#define | XBARA_SEL5_SEL10(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL5_SEL10_SHIFT)) & XBARA_SEL5_SEL10_MASK)
#define | XBARA_SEL5_SEL11_MASK (0x7F00U)
#define | XBARA_SEL5_SEL11_SHIFT (8U)
#define | XBARA_SEL5_SEL11(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL5_SEL11_SHIFT)) & XBARA_SEL5_SEL11_MASK)

## SEL6 - Crossbar A Select Register 6

#define | XBARA_SEL6_SEL12_MASK (0x7FU)
#define | XBARA_SEL6_SEL12_SHIFT (0U)
#define | XBARA_SEL6_SEL12(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL6_SEL12_SHIFT)) & XBARA_SEL6_SEL12_MASK)
#define | XBARA_SEL6_SEL13_MASK (0x7F00U)
#define | XBARA_SEL6_SEL13_SHIFT (8U)
#define | XBARA_SEL6_SEL13(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL6_SEL13_SHIFT)) & XBARA_SEL6_SEL13_MASK)

## SEL7 - Crossbar A Select Register 7

#define | XBARA_SEL7_SEL14_MASK (0x7FU)
#define | XBARA_SEL7_SEL14_SHIFT (0U)
#define | XBARA_SEL7_SEL14(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL7_SEL14_SHIFT)) & XBARA_SEL7_SEL14_MASK)
#define | XBARA_SEL7_SEL15_MASK (0x7F00U)
#define | XBARA_SEL7_SEL15_SHIFT (8U)
#define | XBARA_SEL7_SEL15(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL7_SEL15_SHIFT)) & XBARA_SEL7_SEL15_MASK)

## SEL8 - Crossbar A Select Register 8

#define | XBARA_SEL8_SEL16_MASK (0x7FU)
#define | XBARA_SEL8_SEL16_SHIFT (0U)
#define | XBARA_SEL8_SEL16(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL8_SEL16_SHIFT)) & XBARA_SEL8_SEL16_MASK)
#define | XBARA_SEL8_SEL17_MASK (0x7F00U)
#define | XBARA_SEL8_SEL17_SHIFT (8U)
#define | XBARA_SEL8_SEL17(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL8_SEL17_SHIFT)) & XBARA_SEL8_SEL17_MASK)

## SEL9 - Crossbar A Select Register 9

#define | XBARA_SEL9_SEL18_MASK (0x7FU)
#define | XBARA_SEL9_SEL18_SHIFT (0U)
#define | XBARA_SEL9_SEL18(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL9_SEL18_SHIFT)) & XBARA_SEL9_SEL18_MASK)
#define | XBARA_SEL9_SEL19_MASK (0x7F00U)
#define | XBARA_SEL9_SEL19_SHIFT (8U)
#define | XBARA_SEL9_SEL19(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL9_SEL19_SHIFT)) & XBARA_SEL9_SEL19_MASK)

## SEL10 - Crossbar A Select Register 10

#define | XBARA_SEL10_SEL20_MASK (0x7FU)
#define | XBARA_SEL10_SEL20_SHIFT (0U)
#define | XBARA_SEL10_SEL20(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL10_SEL20_SHIFT)) & XBARA_SEL10_SEL20_MASK)
#define | XBARA_SEL10_SEL21_MASK (0x7F00U)
#define | XBARA_SEL10_SEL21_SHIFT (8U)
#define | XBARA_SEL10_SEL21(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL10_SEL21_SHIFT)) & XBARA_SEL10_SEL21_MASK)

## SEL11 - Crossbar A Select Register 11

#define | XBARA_SEL11_SEL22_MASK (0x7FU)
#define | XBARA_SEL11_SEL22_SHIFT (0U)
#define | XBARA_SEL11_SEL22(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL11_SEL22_SHIFT)) & XBARA_SEL11_SEL22_MASK)
#define | XBARA_SEL11_SEL23_MASK (0x7F00U)
#define | XBARA_SEL11_SEL23_SHIFT (8U)
#define | XBARA_SEL11_SEL23(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL11_SEL23_SHIFT)) & XBARA_SEL11_SEL23_MASK)

## SEL12 - Crossbar A Select Register 12

#define | XBARA_SEL12_SEL24_MASK (0x7FU)
#define | XBARA_SEL12_SEL24_SHIFT (0U)
#define | XBARA_SEL12_SEL24(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL12_SEL24_SHIFT)) & XBARA_SEL12_SEL24_MASK)
#define | XBARA_SEL12_SEL25_MASK (0x7F00U)
#define | XBARA_SEL12_SEL25_SHIFT (8U)
#define | XBARA_SEL12_SEL25(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL12_SEL25_SHIFT)) & XBARA_SEL12_SEL25_MASK)

## SEL13 - Crossbar A Select Register 13

#define | XBARA_SEL13_SEL26_MASK (0x7FU)
#define | XBARA_SEL13_SEL26_SHIFT (0U)
#define | XBARA_SEL13_SEL26(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL13_SEL26_SHIFT)) & XBARA_SEL13_SEL26_MASK)
#define | XBARA_SEL13_SEL27_MASK (0x7F00U)
#define | XBARA_SEL13_SEL27_SHIFT (8U)
#define | XBARA_SEL13_SEL27(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL13_SEL27_SHIFT)) & XBARA_SEL13_SEL27_MASK)

## SEL14 - Crossbar A Select Register 14

#define | XBARA_SEL14_SEL28_MASK (0x7FU)
#define | XBARA_SEL14_SEL28_SHIFT (0U)
#define | XBARA_SEL14_SEL28(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL14_SEL28_SHIFT)) & XBARA_SEL14_SEL28_MASK)
#define | XBARA_SEL14_SEL29_MASK (0x7F00U)
#define | XBARA_SEL14_SEL29_SHIFT (8U)
#define | XBARA_SEL14_SEL29(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL14_SEL29_SHIFT)) & XBARA_SEL14_SEL29_MASK)

## SEL15 - Crossbar A Select Register 15

#define | XBARA_SEL15_SEL30_MASK (0x7FU)
#define | XBARA_SEL15_SEL30_SHIFT (0U)
#define | XBARA_SEL15_SEL30(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL15_SEL30_SHIFT)) & XBARA_SEL15_SEL30_MASK)
#define | XBARA_SEL15_SEL31_MASK (0x7F00U)
#define | XBARA_SEL15_SEL31_SHIFT (8U)
#define | XBARA_SEL15_SEL31(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL15_SEL31_SHIFT)) & XBARA_SEL15_SEL31_MASK)

## SEL16 - Crossbar A Select Register 16

#define | XBARA_SEL16_SEL32_MASK (0x7FU)
#define | XBARA_SEL16_SEL32_SHIFT (0U)
#define | XBARA_SEL16_SEL32(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL16_SEL32_SHIFT)) & XBARA_SEL16_SEL32_MASK)
#define | XBARA_SEL16_SEL33_MASK (0x7F00U)
#define | XBARA_SEL16_SEL33_SHIFT (8U)
#define | XBARA_SEL16_SEL33(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL16_SEL33_SHIFT)) & XBARA_SEL16_SEL33_MASK)

## SEL17 - Crossbar A Select Register 17

#define | XBARA_SEL17_SEL34_MASK (0x7FU)
#define | XBARA_SEL17_SEL34_SHIFT (0U)
#define | XBARA_SEL17_SEL34(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL17_SEL34_SHIFT)) & XBARA_SEL17_SEL34_MASK)
#define | XBARA_SEL17_SEL35_MASK (0x7F00U)
#define | XBARA_SEL17_SEL35_SHIFT (8U)
#define | XBARA_SEL17_SEL35(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL17_SEL35_SHIFT)) & XBARA_SEL17_SEL35_MASK)

## SEL18 - Crossbar A Select Register 18

#define | XBARA_SEL18_SEL36_MASK (0x7FU)
#define | XBARA_SEL18_SEL36_SHIFT (0U)
#define | XBARA_SEL18_SEL36(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL18_SEL36_SHIFT)) & XBARA_SEL18_SEL36_MASK)
#define | XBARA_SEL18_SEL37_MASK (0x7F00U)
#define | XBARA_SEL18_SEL37_SHIFT (8U)
#define | XBARA_SEL18_SEL37(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL18_SEL37_SHIFT)) & XBARA_SEL18_SEL37_MASK)

## SEL19 - Crossbar A Select Register 19

#define | XBARA_SEL19_SEL38_MASK (0x7FU)
#define | XBARA_SEL19_SEL38_SHIFT (0U)
#define | XBARA_SEL19_SEL38(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL19_SEL38_SHIFT)) & XBARA_SEL19_SEL38_MASK)
#define | XBARA_SEL19_SEL39_MASK (0x7F00U)
#define | XBARA_SEL19_SEL39_SHIFT (8U)
#define | XBARA_SEL19_SEL39(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL19_SEL39_SHIFT)) & XBARA_SEL19_SEL39_MASK)

## SEL20 - Crossbar A Select Register 20

#define | XBARA_SEL20_SEL40_MASK (0x7FU)
#define | XBARA_SEL20_SEL40_SHIFT (0U)
#define | XBARA_SEL20_SEL40(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL20_SEL40_SHIFT)) & XBARA_SEL20_SEL40_MASK)
#define | XBARA_SEL20_SEL41_MASK (0x7F00U)
#define | XBARA_SEL20_SEL41_SHIFT (8U)
#define | XBARA_SEL20_SEL41(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL20_SEL41_SHIFT)) & XBARA_SEL20_SEL41_MASK)

## SEL21 - Crossbar A Select Register 21

#define | XBARA_SEL21_SEL42_MASK (0x7FU)
#define | XBARA_SEL21_SEL42_SHIFT (0U)
#define | XBARA_SEL21_SEL42(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL21_SEL42_SHIFT)) & XBARA_SEL21_SEL42_MASK)
#define | XBARA_SEL21_SEL43_MASK (0x7F00U)
#define | XBARA_SEL21_SEL43_SHIFT (8U)
#define | XBARA_SEL21_SEL43(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL21_SEL43_SHIFT)) & XBARA_SEL21_SEL43_MASK)

## SEL22 - Crossbar A Select Register 22

#define | XBARA_SEL22_SEL44_MASK (0x7FU)
#define | XBARA_SEL22_SEL44_SHIFT (0U)
#define | XBARA_SEL22_SEL44(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL22_SEL44_SHIFT)) & XBARA_SEL22_SEL44_MASK)
#define | XBARA_SEL22_SEL45_MASK (0x7F00U)
#define | XBARA_SEL22_SEL45_SHIFT (8U)
#define | XBARA_SEL22_SEL45(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL22_SEL45_SHIFT)) & XBARA_SEL22_SEL45_MASK)

## SEL23 - Crossbar A Select Register 23

#define | XBARA_SEL23_SEL46_MASK (0x7FU)
#define | XBARA_SEL23_SEL46_SHIFT (0U)
#define | XBARA_SEL23_SEL46(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL23_SEL46_SHIFT)) & XBARA_SEL23_SEL46_MASK)
#define | XBARA_SEL23_SEL47_MASK (0x7F00U)
#define | XBARA_SEL23_SEL47_SHIFT (8U)
#define | XBARA_SEL23_SEL47(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL23_SEL47_SHIFT)) & XBARA_SEL23_SEL47_MASK)

## SEL24 - Crossbar A Select Register 24

#define | XBARA_SEL24_SEL48_MASK (0x7FU)
#define | XBARA_SEL24_SEL48_SHIFT (0U)
#define | XBARA_SEL24_SEL48(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL24_SEL48_SHIFT)) & XBARA_SEL24_SEL48_MASK)
#define | XBARA_SEL24_SEL49_MASK (0x7F00U)
#define | XBARA_SEL24_SEL49_SHIFT (8U)
#define | XBARA_SEL24_SEL49(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL24_SEL49_SHIFT)) & XBARA_SEL24_SEL49_MASK)

## SEL25 - Crossbar A Select Register 25

#define | XBARA_SEL25_SEL50_MASK (0x7FU)
#define | XBARA_SEL25_SEL50_SHIFT (0U)
#define | XBARA_SEL25_SEL50(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL25_SEL50_SHIFT)) & XBARA_SEL25_SEL50_MASK)
#define | XBARA_SEL25_SEL51_MASK (0x7F00U)
#define | XBARA_SEL25_SEL51_SHIFT (8U)
#define | XBARA_SEL25_SEL51(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL25_SEL51_SHIFT)) & XBARA_SEL25_SEL51_MASK)

## SEL26 - Crossbar A Select Register 26

#define | XBARA_SEL26_SEL52_MASK (0x7FU)
#define | XBARA_SEL26_SEL52_SHIFT (0U)
#define | XBARA_SEL26_SEL52(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL26_SEL52_SHIFT)) & XBARA_SEL26_SEL52_MASK)
#define | XBARA_SEL26_SEL53_MASK (0x7F00U)
#define | XBARA_SEL26_SEL53_SHIFT (8U)
#define | XBARA_SEL26_SEL53(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL26_SEL53_SHIFT)) & XBARA_SEL26_SEL53_MASK)

## SEL27 - Crossbar A Select Register 27

#define | XBARA_SEL27_SEL54_MASK (0x7FU)
#define | XBARA_SEL27_SEL54_SHIFT (0U)
#define | XBARA_SEL27_SEL54(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL27_SEL54_SHIFT)) & XBARA_SEL27_SEL54_MASK)
#define | XBARA_SEL27_SEL55_MASK (0x7F00U)
#define | XBARA_SEL27_SEL55_SHIFT (8U)
#define | XBARA_SEL27_SEL55(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL27_SEL55_SHIFT)) & XBARA_SEL27_SEL55_MASK)

## SEL28 - Crossbar A Select Register 28

#define | XBARA_SEL28_SEL56_MASK (0x7FU)
#define | XBARA_SEL28_SEL56_SHIFT (0U)
#define | XBARA_SEL28_SEL56(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL28_SEL56_SHIFT)) & XBARA_SEL28_SEL56_MASK)
#define | XBARA_SEL28_SEL57_MASK (0x7F00U)
#define | XBARA_SEL28_SEL57_SHIFT (8U)
#define | XBARA_SEL28_SEL57(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL28_SEL57_SHIFT)) & XBARA_SEL28_SEL57_MASK)

## SEL29 - Crossbar A Select Register 29

#define | XBARA_SEL29_SEL58_MASK (0x7FU)
#define | XBARA_SEL29_SEL58_SHIFT (0U)
#define | XBARA_SEL29_SEL58(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL29_SEL58_SHIFT)) & XBARA_SEL29_SEL58_MASK)
#define | XBARA_SEL29_SEL59_MASK (0x7F00U)
#define | XBARA_SEL29_SEL59_SHIFT (8U)
#define | XBARA_SEL29_SEL59(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL29_SEL59_SHIFT)) & XBARA_SEL29_SEL59_MASK)

## SEL30 - Crossbar A Select Register 30

#define | XBARA_SEL30_SEL60_MASK (0x7FU)
#define | XBARA_SEL30_SEL60_SHIFT (0U)
#define | XBARA_SEL30_SEL60(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL30_SEL60_SHIFT)) & XBARA_SEL30_SEL60_MASK)
#define | XBARA_SEL30_SEL61_MASK (0x7F00U)
#define | XBARA_SEL30_SEL61_SHIFT (8U)
#define | XBARA_SEL30_SEL61(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL30_SEL61_SHIFT)) & XBARA_SEL30_SEL61_MASK)

## SEL31 - Crossbar A Select Register 31

#define | XBARA_SEL31_SEL62_MASK (0x7FU)
#define | XBARA_SEL31_SEL62_SHIFT (0U)
#define | XBARA_SEL31_SEL62(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL31_SEL62_SHIFT)) & XBARA_SEL31_SEL62_MASK)
#define | XBARA_SEL31_SEL63_MASK (0x7F00U)
#define | XBARA_SEL31_SEL63_SHIFT (8U)
#define | XBARA_SEL31_SEL63(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL31_SEL63_SHIFT)) & XBARA_SEL31_SEL63_MASK)

## SEL32 - Crossbar A Select Register 32

#define | XBARA_SEL32_SEL64_MASK (0x7FU)
#define | XBARA_SEL32_SEL64_SHIFT (0U)
#define | XBARA_SEL32_SEL64(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL32_SEL64_SHIFT)) & XBARA_SEL32_SEL64_MASK)
#define | XBARA_SEL32_SEL65_MASK (0x7F00U)
#define | XBARA_SEL32_SEL65_SHIFT (8U)
#define | XBARA_SEL32_SEL65(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL32_SEL65_SHIFT)) & XBARA_SEL32_SEL65_MASK)

## SEL33 - Crossbar A Select Register 33

#define | XBARA_SEL33_SEL66_MASK (0x7FU)
#define | XBARA_SEL33_SEL66_SHIFT (0U)
#define | XBARA_SEL33_SEL66(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL33_SEL66_SHIFT)) & XBARA_SEL33_SEL66_MASK)
#define | XBARA_SEL33_SEL67_MASK (0x7F00U)
#define | XBARA_SEL33_SEL67_SHIFT (8U)
#define | XBARA_SEL33_SEL67(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL33_SEL67_SHIFT)) & XBARA_SEL33_SEL67_MASK)

## SEL34 - Crossbar A Select Register 34

#define | XBARA_SEL34_SEL68_MASK (0x7FU)
#define | XBARA_SEL34_SEL68_SHIFT (0U)
#define | XBARA_SEL34_SEL68(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL34_SEL68_SHIFT)) & XBARA_SEL34_SEL68_MASK)
#define | XBARA_SEL34_SEL69_MASK (0x7F00U)
#define | XBARA_SEL34_SEL69_SHIFT (8U)
#define | XBARA_SEL34_SEL69(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL34_SEL69_SHIFT)) & XBARA_SEL34_SEL69_MASK)

## SEL35 - Crossbar A Select Register 35

#define | XBARA_SEL35_SEL70_MASK (0x7FU)
#define | XBARA_SEL35_SEL70_SHIFT (0U)
#define | XBARA_SEL35_SEL70(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL35_SEL70_SHIFT)) & XBARA_SEL35_SEL70_MASK)
#define | XBARA_SEL35_SEL71_MASK (0x7F00U)
#define | XBARA_SEL35_SEL71_SHIFT (8U)
#define | XBARA_SEL35_SEL71(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL35_SEL71_SHIFT)) & XBARA_SEL35_SEL71_MASK)

## SEL36 - Crossbar A Select Register 36

#define | XBARA_SEL36_SEL72_MASK (0x7FU)
#define | XBARA_SEL36_SEL72_SHIFT (0U)
#define | XBARA_SEL36_SEL72(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL36_SEL72_SHIFT)) & XBARA_SEL36_SEL72_MASK)
#define | XBARA_SEL36_SEL73_MASK (0x7F00U)
#define | XBARA_SEL36_SEL73_SHIFT (8U)
#define | XBARA_SEL36_SEL73(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL36_SEL73_SHIFT)) & XBARA_SEL36_SEL73_MASK)

## SEL37 - Crossbar A Select Register 37

#define | XBARA_SEL37_SEL74_MASK (0x7FU)
#define | XBARA_SEL37_SEL74_SHIFT (0U)
#define | XBARA_SEL37_SEL74(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL37_SEL74_SHIFT)) & XBARA_SEL37_SEL74_MASK)
#define | XBARA_SEL37_SEL75_MASK (0x7F00U)
#define | XBARA_SEL37_SEL75_SHIFT (8U)
#define | XBARA_SEL37_SEL75(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL37_SEL75_SHIFT)) & XBARA_SEL37_SEL75_MASK)

## SEL38 - Crossbar A Select Register 38

#define | XBARA_SEL38_SEL76_MASK (0x7FU)
#define | XBARA_SEL38_SEL76_SHIFT (0U)
#define | XBARA_SEL38_SEL76(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL38_SEL76_SHIFT)) & XBARA_SEL38_SEL76_MASK)
#define | XBARA_SEL38_SEL77_MASK (0x7F00U)
#define | XBARA_SEL38_SEL77_SHIFT (8U)
#define | XBARA_SEL38_SEL77(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL38_SEL77_SHIFT)) & XBARA_SEL38_SEL77_MASK)

## SEL39 - Crossbar A Select Register 39

#define | XBARA_SEL39_SEL78_MASK (0x7FU)
#define | XBARA_SEL39_SEL78_SHIFT (0U)
#define | XBARA_SEL39_SEL78(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL39_SEL78_SHIFT)) & XBARA_SEL39_SEL78_MASK)
#define | XBARA_SEL39_SEL79_MASK (0x7F00U)
#define | XBARA_SEL39_SEL79_SHIFT (8U)
#define | XBARA_SEL39_SEL79(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL39_SEL79_SHIFT)) & XBARA_SEL39_SEL79_MASK)

## SEL40 - Crossbar A Select Register 40

#define | XBARA_SEL40_SEL80_MASK (0x7FU)
#define | XBARA_SEL40_SEL80_SHIFT (0U)
#define | XBARA_SEL40_SEL80(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL40_SEL80_SHIFT)) & XBARA_SEL40_SEL80_MASK)
#define | XBARA_SEL40_SEL81_MASK (0x7F00U)
#define | XBARA_SEL40_SEL81_SHIFT (8U)
#define | XBARA_SEL40_SEL81(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL40_SEL81_SHIFT)) & XBARA_SEL40_SEL81_MASK)

## SEL41 - Crossbar A Select Register 41

#define | XBARA_SEL41_SEL82_MASK (0x7FU)
#define | XBARA_SEL41_SEL82_SHIFT (0U)
#define | XBARA_SEL41_SEL82(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL41_SEL82_SHIFT)) & XBARA_SEL41_SEL82_MASK)
#define | XBARA_SEL41_SEL83_MASK (0x7F00U)
#define | XBARA_SEL41_SEL83_SHIFT (8U)
#define | XBARA_SEL41_SEL83(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL41_SEL83_SHIFT)) & XBARA_SEL41_SEL83_MASK)

## SEL42 - Crossbar A Select Register 42

#define | XBARA_SEL42_SEL84_MASK (0x7FU)
#define | XBARA_SEL42_SEL84_SHIFT (0U)
#define | XBARA_SEL42_SEL84(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL42_SEL84_SHIFT)) & XBARA_SEL42_SEL84_MASK)
#define | XBARA_SEL42_SEL85_MASK (0x7F00U)
#define | XBARA_SEL42_SEL85_SHIFT (8U)
#define | XBARA_SEL42_SEL85(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL42_SEL85_SHIFT)) & XBARA_SEL42_SEL85_MASK)

## SEL43 - Crossbar A Select Register 43

#define | XBARA_SEL43_SEL86_MASK (0x7FU)
#define | XBARA_SEL43_SEL86_SHIFT (0U)
#define | XBARA_SEL43_SEL86(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL43_SEL86_SHIFT)) & XBARA_SEL43_SEL86_MASK)
#define | XBARA_SEL43_SEL87_MASK (0x7F00U)
#define | XBARA_SEL43_SEL87_SHIFT (8U)
#define | XBARA_SEL43_SEL87(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL43_SEL87_SHIFT)) & XBARA_SEL43_SEL87_MASK)

## SEL44 - Crossbar A Select Register 44

#define | XBARA_SEL44_SEL88_MASK (0x7FU)
#define | XBARA_SEL44_SEL88_SHIFT (0U)
#define | XBARA_SEL44_SEL88(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL44_SEL88_SHIFT)) & XBARA_SEL44_SEL88_MASK)
#define | XBARA_SEL44_SEL89_MASK (0x7F00U)
#define | XBARA_SEL44_SEL89_SHIFT (8U)
#define | XBARA_SEL44_SEL89(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL44_SEL89_SHIFT)) & XBARA_SEL44_SEL89_MASK)

## SEL45 - Crossbar A Select Register 45

#define | XBARA_SEL45_SEL90_MASK (0x7FU)
#define | XBARA_SEL45_SEL90_SHIFT (0U)
#define | XBARA_SEL45_SEL90(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL45_SEL90_SHIFT)) & XBARA_SEL45_SEL90_MASK)
#define | XBARA_SEL45_SEL91_MASK (0x7F00U)
#define | XBARA_SEL45_SEL91_SHIFT (8U)
#define | XBARA_SEL45_SEL91(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL45_SEL91_SHIFT)) & XBARA_SEL45_SEL91_MASK)

## SEL46 - Crossbar A Select Register 46

#define | XBARA_SEL46_SEL92_MASK (0x7FU)
#define | XBARA_SEL46_SEL92_SHIFT (0U)
#define | XBARA_SEL46_SEL92(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL46_SEL92_SHIFT)) & XBARA_SEL46_SEL92_MASK)
#define | XBARA_SEL46_SEL93_MASK (0x7F00U)
#define | XBARA_SEL46_SEL93_SHIFT (8U)
#define | XBARA_SEL46_SEL93(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL46_SEL93_SHIFT)) & XBARA_SEL46_SEL93_MASK)

## SEL47 - Crossbar A Select Register 47

#define | XBARA_SEL47_SEL94_MASK (0x7FU)
#define | XBARA_SEL47_SEL94_SHIFT (0U)
#define | XBARA_SEL47_SEL94(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL47_SEL94_SHIFT)) & XBARA_SEL47_SEL94_MASK)
#define | XBARA_SEL47_SEL95_MASK (0x7F00U)
#define | XBARA_SEL47_SEL95_SHIFT (8U)
#define | XBARA_SEL47_SEL95(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL47_SEL95_SHIFT)) & XBARA_SEL47_SEL95_MASK)

## SEL48 - Crossbar A Select Register 48

#define | XBARA_SEL48_SEL96_MASK (0x7FU)
#define | XBARA_SEL48_SEL96_SHIFT (0U)
#define | XBARA_SEL48_SEL96(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL48_SEL96_SHIFT)) & XBARA_SEL48_SEL96_MASK)
#define | XBARA_SEL48_SEL97_MASK (0x7F00U)
#define | XBARA_SEL48_SEL97_SHIFT (8U)
#define | XBARA_SEL48_SEL97(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL48_SEL97_SHIFT)) & XBARA_SEL48_SEL97_MASK)

## SEL49 - Crossbar A Select Register 49

#define | XBARA_SEL49_SEL98_MASK (0x7FU)
#define | XBARA_SEL49_SEL98_SHIFT (0U)
#define | XBARA_SEL49_SEL98(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL49_SEL98_SHIFT)) & XBARA_SEL49_SEL98_MASK)
#define | XBARA_SEL49_SEL99_MASK (0x7F00U)
#define | XBARA_SEL49_SEL99_SHIFT (8U)
#define | XBARA_SEL49_SEL99(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL49_SEL99_SHIFT)) & XBARA_SEL49_SEL99_MASK)

## SEL50 - Crossbar A Select Register 50

#define | XBARA_SEL50_SEL100_MASK (0x7FU)
#define | XBARA_SEL50_SEL100_SHIFT (0U)
#define | XBARA_SEL50_SEL100(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL50_SEL100_SHIFT)) & XBARA_SEL50_SEL100_MASK)
#define | XBARA_SEL50_SEL101_MASK (0x7F00U)
#define | XBARA_SEL50_SEL101_SHIFT (8U)
#define | XBARA_SEL50_SEL101(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL50_SEL101_SHIFT)) & XBARA_SEL50_SEL101_MASK)

## SEL51 - Crossbar A Select Register 51

#define | XBARA_SEL51_SEL102_MASK (0x7FU)
#define | XBARA_SEL51_SEL102_SHIFT (0U)
#define | XBARA_SEL51_SEL102(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL51_SEL102_SHIFT)) & XBARA_SEL51_SEL102_MASK)
#define | XBARA_SEL51_SEL103_MASK (0x7F00U)
#define | XBARA_SEL51_SEL103_SHIFT (8U)
#define | XBARA_SEL51_SEL103(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL51_SEL103_SHIFT)) & XBARA_SEL51_SEL103_MASK)

## SEL52 - Crossbar A Select Register 52

#define | XBARA_SEL52_SEL104_MASK (0x7FU)
#define | XBARA_SEL52_SEL104_SHIFT (0U)
#define | XBARA_SEL52_SEL104(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL52_SEL104_SHIFT)) & XBARA_SEL52_SEL104_MASK)
#define | XBARA_SEL52_SEL105_MASK (0x7F00U)
#define | XBARA_SEL52_SEL105_SHIFT (8U)
#define | XBARA_SEL52_SEL105(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL52_SEL105_SHIFT)) & XBARA_SEL52_SEL105_MASK)

## SEL53 - Crossbar A Select Register 53

#define | XBARA_SEL53_SEL106_MASK (0x7FU)
#define | XBARA_SEL53_SEL106_SHIFT (0U)
#define | XBARA_SEL53_SEL106(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL53_SEL106_SHIFT)) & XBARA_SEL53_SEL106_MASK)
#define | XBARA_SEL53_SEL107_MASK (0x7F00U)
#define | XBARA_SEL53_SEL107_SHIFT (8U)
#define | XBARA_SEL53_SEL107(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL53_SEL107_SHIFT)) & XBARA_SEL53_SEL107_MASK)

## SEL54 - Crossbar A Select Register 54

#define | XBARA_SEL54_SEL108_MASK (0x7FU)
#define | XBARA_SEL54_SEL108_SHIFT (0U)
#define | XBARA_SEL54_SEL108(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL54_SEL108_SHIFT)) & XBARA_SEL54_SEL108_MASK)
#define | XBARA_SEL54_SEL109_MASK (0x7F00U)
#define | XBARA_SEL54_SEL109_SHIFT (8U)
#define | XBARA_SEL54_SEL109(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL54_SEL109_SHIFT)) & XBARA_SEL54_SEL109_MASK)

## SEL55 - Crossbar A Select Register 55

#define | XBARA_SEL55_SEL110_MASK (0x7FU)
#define | XBARA_SEL55_SEL110_SHIFT (0U)
#define | XBARA_SEL55_SEL110(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL55_SEL110_SHIFT)) & XBARA_SEL55_SEL110_MASK)
#define | XBARA_SEL55_SEL111_MASK (0x7F00U)
#define | XBARA_SEL55_SEL111_SHIFT (8U)
#define | XBARA_SEL55_SEL111(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL55_SEL111_SHIFT)) & XBARA_SEL55_SEL111_MASK)

## SEL56 - Crossbar A Select Register 56

#define | XBARA_SEL56_SEL112_MASK (0x7FU)
#define | XBARA_SEL56_SEL112_SHIFT (0U)
#define | XBARA_SEL56_SEL112(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL56_SEL112_SHIFT)) & XBARA_SEL56_SEL112_MASK)
#define | XBARA_SEL56_SEL113_MASK (0x7F00U)
#define | XBARA_SEL56_SEL113_SHIFT (8U)
#define | XBARA_SEL56_SEL113(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL56_SEL113_SHIFT)) & XBARA_SEL56_SEL113_MASK)

## SEL57 - Crossbar A Select Register 57

#define | XBARA_SEL57_SEL114_MASK (0x7FU)
#define | XBARA_SEL57_SEL114_SHIFT (0U)
#define | XBARA_SEL57_SEL114(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL57_SEL114_SHIFT)) & XBARA_SEL57_SEL114_MASK)
#define | XBARA_SEL57_SEL115_MASK (0x7F00U)
#define | XBARA_SEL57_SEL115_SHIFT (8U)
#define | XBARA_SEL57_SEL115(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL57_SEL115_SHIFT)) & XBARA_SEL57_SEL115_MASK)

## SEL58 - Crossbar A Select Register 58

#define | XBARA_SEL58_SEL116_MASK (0x7FU)
#define | XBARA_SEL58_SEL116_SHIFT (0U)
#define | XBARA_SEL58_SEL116(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL58_SEL116_SHIFT)) & XBARA_SEL58_SEL116_MASK)
#define | XBARA_SEL58_SEL117_MASK (0x7F00U)
#define | XBARA_SEL58_SEL117_SHIFT (8U)
#define | XBARA_SEL58_SEL117(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL58_SEL117_SHIFT)) & XBARA_SEL58_SEL117_MASK)

## SEL59 - Crossbar A Select Register 59

#define | XBARA_SEL59_SEL118_MASK (0x7FU)
#define | XBARA_SEL59_SEL118_SHIFT (0U)
#define | XBARA_SEL59_SEL118(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL59_SEL118_SHIFT)) & XBARA_SEL59_SEL118_MASK)
#define | XBARA_SEL59_SEL119_MASK (0x7F00U)
#define | XBARA_SEL59_SEL119_SHIFT (8U)
#define | XBARA_SEL59_SEL119(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL59_SEL119_SHIFT)) & XBARA_SEL59_SEL119_MASK)

## SEL60 - Crossbar A Select Register 60

#define | XBARA_SEL60_SEL120_MASK (0x7FU)
#define | XBARA_SEL60_SEL120_SHIFT (0U)
#define | XBARA_SEL60_SEL120(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL60_SEL120_SHIFT)) & XBARA_SEL60_SEL120_MASK)
#define | XBARA_SEL60_SEL121_MASK (0x7F00U)
#define | XBARA_SEL60_SEL121_SHIFT (8U)
#define | XBARA_SEL60_SEL121(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL60_SEL121_SHIFT)) & XBARA_SEL60_SEL121_MASK)

## SEL61 - Crossbar A Select Register 61

#define | XBARA_SEL61_SEL122_MASK (0x7FU)
#define | XBARA_SEL61_SEL122_SHIFT (0U)
#define | XBARA_SEL61_SEL122(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL61_SEL122_SHIFT)) & XBARA_SEL61_SEL122_MASK)
#define | XBARA_SEL61_SEL123_MASK (0x7F00U)
#define | XBARA_SEL61_SEL123_SHIFT (8U)
#define | XBARA_SEL61_SEL123(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL61_SEL123_SHIFT)) & XBARA_SEL61_SEL123_MASK)

## SEL62 - Crossbar A Select Register 62

#define | XBARA_SEL62_SEL124_MASK (0x7FU)
#define | XBARA_SEL62_SEL124_SHIFT (0U)
#define | XBARA_SEL62_SEL124(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL62_SEL124_SHIFT)) & XBARA_SEL62_SEL124_MASK)
#define | XBARA_SEL62_SEL125_MASK (0x7F00U)
#define | XBARA_SEL62_SEL125_SHIFT (8U)
#define | XBARA_SEL62_SEL125(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL62_SEL125_SHIFT)) & XBARA_SEL62_SEL125_MASK)

## SEL63 - Crossbar A Select Register 63

#define | XBARA_SEL63_SEL126_MASK (0x7FU)
#define | XBARA_SEL63_SEL126_SHIFT (0U)
#define | XBARA_SEL63_SEL126(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL63_SEL126_SHIFT)) & XBARA_SEL63_SEL126_MASK)
#define | XBARA_SEL63_SEL127_MASK (0x7F00U)
#define | XBARA_SEL63_SEL127_SHIFT (8U)
#define | XBARA_SEL63_SEL127(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL63_SEL127_SHIFT)) & XBARA_SEL63_SEL127_MASK)

## SEL64 - Crossbar A Select Register 64

#define | XBARA_SEL64_SEL128_MASK (0x7FU)
#define | XBARA_SEL64_SEL128_SHIFT (0U)
#define | XBARA_SEL64_SEL128(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL64_SEL128_SHIFT)) & XBARA_SEL64_SEL128_MASK)
#define | XBARA_SEL64_SEL129_MASK (0x7F00U)
#define | XBARA_SEL64_SEL129_SHIFT (8U)
#define | XBARA_SEL64_SEL129(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL64_SEL129_SHIFT)) & XBARA_SEL64_SEL129_MASK)

## SEL65 - Crossbar A Select Register 65

#define | XBARA_SEL65_SEL130_MASK (0x7FU)
#define | XBARA_SEL65_SEL130_SHIFT (0U)
#define | XBARA_SEL65_SEL130(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL65_SEL130_SHIFT)) & XBARA_SEL65_SEL130_MASK)
#define | XBARA_SEL65_SEL131_MASK (0x7F00U)
#define | XBARA_SEL65_SEL131_SHIFT (8U)
#define | XBARA_SEL65_SEL131(x) (((uint16_t)(((uint16_t)(x)) << XBARA_SEL65_SEL131_SHIFT)) & XBARA_SEL65_SEL131_MASK)

## CTRL0 - Crossbar A Control Register 0

#define | XBARA_CTRL0_DEN0_MASK (0x1U)
#define | XBARA_CTRL0_DEN0_SHIFT (0U)
#define | XBARA_CTRL0_DEN0(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_DEN0_SHIFT)) & XBARA_CTRL0_DEN0_MASK)
#define | XBARA_CTRL0_IEN0_MASK (0x2U)
#define | XBARA_CTRL0_IEN0_SHIFT (1U)
#define | XBARA_CTRL0_IEN0(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_IEN0_SHIFT)) & XBARA_CTRL0_IEN0_MASK)
#define | XBARA_CTRL0_EDGE0_MASK (0xCU)
#define | XBARA_CTRL0_EDGE0_SHIFT (2U)
#define | XBARA_CTRL0_EDGE0(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_EDGE0_SHIFT)) & XBARA_CTRL0_EDGE0_MASK)
#define | XBARA_CTRL0_STS0_MASK (0x10U)
#define | XBARA_CTRL0_STS0_SHIFT (4U)
#define | XBARA_CTRL0_STS0(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_STS0_SHIFT)) & XBARA_CTRL0_STS0_MASK)
#define | XBARA_CTRL0_DEN1_MASK (0x100U)
#define | XBARA_CTRL0_DEN1_SHIFT (8U)
#define | XBARA_CTRL0_DEN1(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_DEN1_SHIFT)) & XBARA_CTRL0_DEN1_MASK)
#define | XBARA_CTRL0_IEN1_MASK (0x200U)
#define | XBARA_CTRL0_IEN1_SHIFT (9U)
#define | XBARA_CTRL0_IEN1(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_IEN1_SHIFT)) & XBARA_CTRL0_IEN1_MASK)
#define | XBARA_CTRL0_EDGE1_MASK (0xC00U)
#define | XBARA_CTRL0_EDGE1_SHIFT (10U)
#define | XBARA_CTRL0_EDGE1(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_EDGE1_SHIFT)) & XBARA_CTRL0_EDGE1_MASK)
#define | XBARA_CTRL0_STS1_MASK (0x1000U)
#define | XBARA_CTRL0_STS1_SHIFT (12U)
#define | XBARA_CTRL0_STS1(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_STS1_SHIFT)) & XBARA_CTRL0_STS1_MASK)

## CTRL1 - Crossbar A Control Register 1

#define | XBARA_CTRL1_DEN2_MASK (0x1U)
#define | XBARA_CTRL1_DEN2_SHIFT (0U)
#define | XBARA_CTRL1_DEN2(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_DEN2_SHIFT)) & XBARA_CTRL1_DEN2_MASK)
#define | XBARA_CTRL1_IEN2_MASK (0x2U)
#define | XBARA_CTRL1_IEN2_SHIFT (1U)
#define | XBARA_CTRL1_IEN2(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_IEN2_SHIFT)) & XBARA_CTRL1_IEN2_MASK)
#define | XBARA_CTRL1_EDGE2_MASK (0xCU)
#define | XBARA_CTRL1_EDGE2_SHIFT (2U)
#define | XBARA_CTRL1_EDGE2(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_EDGE2_SHIFT)) & XBARA_CTRL1_EDGE2_MASK)
#define | XBARA_CTRL1_STS2_MASK (0x10U)
#define | XBARA_CTRL1_STS2_SHIFT (4U)
#define | XBARA_CTRL1_STS2(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_STS2_SHIFT)) & XBARA_CTRL1_STS2_MASK)
#define | XBARA_CTRL1_DEN3_MASK (0x100U)
#define | XBARA_CTRL1_DEN3_SHIFT (8U)
#define | XBARA_CTRL1_DEN3(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_DEN3_SHIFT)) & XBARA_CTRL1_DEN3_MASK)
#define | XBARA_CTRL1_IEN3_MASK (0x200U)
#define | XBARA_CTRL1_IEN3_SHIFT (9U)
#define | XBARA_CTRL1_IEN3(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_IEN3_SHIFT)) & XBARA_CTRL1_IEN3_MASK)
#define | XBARA_CTRL1_EDGE3_MASK (0xC00U)
#define | XBARA_CTRL1_EDGE3_SHIFT (10U)
#define | XBARA_CTRL1_EDGE3(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_EDGE3_SHIFT)) & XBARA_CTRL1_EDGE3_MASK)
#define | XBARA_CTRL1_STS3_MASK (0x1000U)
#define | XBARA_CTRL1_STS3_SHIFT (12U)
#define | XBARA_CTRL1_STS3(x) (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_STS3_SHIFT)) & XBARA_CTRL1_STS3_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ XBARA_CTRL0_DEN0

#define XBARA_CTRL0_DEN0 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_DEN0_SHIFT)) & XBARA_CTRL0_DEN0_MASK)

DEN0 - DMA Enable for XBAR_OUT0 0b0..DMA disabled 0b1..DMA enabled

Definition at line 47267 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_DEN0_MASK

#define XBARA_CTRL0_DEN0_MASK (0x1U)

Definition at line 47261 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_DEN0_SHIFT

#define XBARA_CTRL0_DEN0_SHIFT (0U)

Definition at line 47262 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_DEN1

#define XBARA_CTRL0_DEN1 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_DEN1_SHIFT)) & XBARA_CTRL0_DEN1_MASK)

DEN1 - DMA Enable for XBAR_OUT1 0b0..DMA disabled 0b1..DMA enabled

Definition at line 47297 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_DEN1_MASK

#define XBARA_CTRL0_DEN1_MASK (0x100U)

Definition at line 47291 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_DEN1_SHIFT

#define XBARA_CTRL0_DEN1_SHIFT (8U)

Definition at line 47292 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_EDGE0

#define XBARA_CTRL0_EDGE0 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_EDGE0_SHIFT)) & XBARA_CTRL0_EDGE0_MASK)

EDGE0 - Active edge for edge detection on XBAR_OUT0 0b00..STS0 never asserts 0b01..STS0 asserts on rising edges of XBAR_OUT0 0b10..STS0 asserts on falling edges of XBAR_OUT0 0b11..STS0 asserts on rising and falling edges of XBAR_OUT0

Definition at line 47283 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_EDGE0_MASK

#define XBARA_CTRL0_EDGE0_MASK (0xCU)

Definition at line 47275 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_EDGE0_SHIFT

#define XBARA_CTRL0_EDGE0_SHIFT (2U)

Definition at line 47276 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_EDGE1

#define XBARA_CTRL0_EDGE1 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_EDGE1_SHIFT)) & XBARA_CTRL0_EDGE1_MASK)

EDGE1 - Active edge for edge detection on XBAR_OUT1 0b00..STS1 never asserts 0b01..STS1 asserts on rising edges of XBAR_OUT1 0b10..STS1 asserts on falling edges of XBAR_OUT1 0b11..STS1 asserts on rising and falling edges of XBAR_OUT1

Definition at line 47313 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_EDGE1_MASK

#define XBARA_CTRL0_EDGE1_MASK (0xC00U)

Definition at line 47305 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_EDGE1_SHIFT

#define XBARA_CTRL0_EDGE1_SHIFT (10U)

Definition at line 47306 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_IEN0

#define XBARA_CTRL0_IEN0 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_IEN0_SHIFT)) & XBARA_CTRL0_IEN0_MASK)

IEN0 - Interrupt Enable for XBAR_OUT0 0b0..Interrupt disabled 0b1..Interrupt enabled

Definition at line 47274 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_IEN0_MASK

#define XBARA_CTRL0_IEN0_MASK (0x2U)

Definition at line 47268 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_IEN0_SHIFT

#define XBARA_CTRL0_IEN0_SHIFT (1U)

Definition at line 47269 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_IEN1

#define XBARA_CTRL0_IEN1 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_IEN1_SHIFT)) & XBARA_CTRL0_IEN1_MASK)

IEN1 - Interrupt Enable for XBAR_OUT1 0b0..Interrupt disabled 0b1..Interrupt enabled

Definition at line 47304 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_IEN1_MASK

#define XBARA_CTRL0_IEN1_MASK (0x200U)

Definition at line 47298 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_IEN1_SHIFT

#define XBARA_CTRL0_IEN1_SHIFT (9U)

Definition at line 47299 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_STS0

#define XBARA_CTRL0_STS0 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_STS0_SHIFT)) & XBARA_CTRL0_STS0_MASK)

STS0 - Edge detection status for XBAR_OUT0 0b0..Active edge not yet detected on XBAR_OUT0 0b1..Active edge detected on XBAR_OUT0

Definition at line 47290 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_STS0_MASK

#define XBARA_CTRL0_STS0_MASK (0x10U)

Definition at line 47284 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_STS0_SHIFT

#define XBARA_CTRL0_STS0_SHIFT (4U)

Definition at line 47285 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_STS1

#define XBARA_CTRL0_STS1 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL0_STS1_SHIFT)) & XBARA_CTRL0_STS1_MASK)

STS1 - Edge detection status for XBAR_OUT1 0b0..Active edge not yet detected on XBAR_OUT1 0b1..Active edge detected on XBAR_OUT1

Definition at line 47320 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_STS1_MASK

#define XBARA_CTRL0_STS1_MASK (0x1000U)

Definition at line 47314 of file MIMXRT1062.h.

## ◆ XBARA_CTRL0_STS1_SHIFT

#define XBARA_CTRL0_STS1_SHIFT (12U)

Definition at line 47315 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_DEN2

#define XBARA_CTRL1_DEN2 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_DEN2_SHIFT)) & XBARA_CTRL1_DEN2_MASK)

DEN2 - DMA Enable for XBAR_OUT2 0b0..DMA disabled 0b1..DMA enabled

Definition at line 47331 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_DEN2_MASK

#define XBARA_CTRL1_DEN2_MASK (0x1U)

Definition at line 47325 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_DEN2_SHIFT

#define XBARA_CTRL1_DEN2_SHIFT (0U)

Definition at line 47326 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_DEN3

#define XBARA_CTRL1_DEN3 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_DEN3_SHIFT)) & XBARA_CTRL1_DEN3_MASK)

DEN3 - DMA Enable for XBAR_OUT3 0b0..DMA disabled 0b1..DMA enabled

Definition at line 47361 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_DEN3_MASK

#define XBARA_CTRL1_DEN3_MASK (0x100U)

Definition at line 47355 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_DEN3_SHIFT

#define XBARA_CTRL1_DEN3_SHIFT (8U)

Definition at line 47356 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_EDGE2

#define XBARA_CTRL1_EDGE2 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_EDGE2_SHIFT)) & XBARA_CTRL1_EDGE2_MASK)

EDGE2 - Active edge for edge detection on XBAR_OUT2 0b00..STS2 never asserts 0b01..STS2 asserts on rising edges of XBAR_OUT2 0b10..STS2 asserts on falling edges of XBAR_OUT2 0b11..STS2 asserts on rising and falling edges of XBAR_OUT2

Definition at line 47347 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_EDGE2_MASK

#define XBARA_CTRL1_EDGE2_MASK (0xCU)

Definition at line 47339 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_EDGE2_SHIFT

#define XBARA_CTRL1_EDGE2_SHIFT (2U)

Definition at line 47340 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_EDGE3

#define XBARA_CTRL1_EDGE3 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_EDGE3_SHIFT)) & XBARA_CTRL1_EDGE3_MASK)

EDGE3 - Active edge for edge detection on XBAR_OUT3 0b00..STS3 never asserts 0b01..STS3 asserts on rising edges of XBAR_OUT3 0b10..STS3 asserts on falling edges of XBAR_OUT3 0b11..STS3 asserts on rising and falling edges of XBAR_OUT3

Definition at line 47377 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_EDGE3_MASK

#define XBARA_CTRL1_EDGE3_MASK (0xC00U)

Definition at line 47369 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_EDGE3_SHIFT

#define XBARA_CTRL1_EDGE3_SHIFT (10U)

Definition at line 47370 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_IEN2

#define XBARA_CTRL1_IEN2 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_IEN2_SHIFT)) & XBARA_CTRL1_IEN2_MASK)

IEN2 - Interrupt Enable for XBAR_OUT2 0b0..Interrupt disabled 0b1..Interrupt enabled

Definition at line 47338 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_IEN2_MASK

#define XBARA_CTRL1_IEN2_MASK (0x2U)

Definition at line 47332 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_IEN2_SHIFT

#define XBARA_CTRL1_IEN2_SHIFT (1U)

Definition at line 47333 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_IEN3

#define XBARA_CTRL1_IEN3 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_IEN3_SHIFT)) & XBARA_CTRL1_IEN3_MASK)

IEN3 - Interrupt Enable for XBAR_OUT3 0b0..Interrupt disabled 0b1..Interrupt enabled

Definition at line 47368 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_IEN3_MASK

#define XBARA_CTRL1_IEN3_MASK (0x200U)

Definition at line 47362 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_IEN3_SHIFT

#define XBARA_CTRL1_IEN3_SHIFT (9U)

Definition at line 47363 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_STS2

#define XBARA_CTRL1_STS2 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_STS2_SHIFT)) & XBARA_CTRL1_STS2_MASK)

STS2 - Edge detection status for XBAR_OUT2 0b0..Active edge not yet detected on XBAR_OUT2 0b1..Active edge detected on XBAR_OUT2

Definition at line 47354 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_STS2_MASK

#define XBARA_CTRL1_STS2_MASK (0x10U)

Definition at line 47348 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_STS2_SHIFT

#define XBARA_CTRL1_STS2_SHIFT (4U)

Definition at line 47349 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_STS3

#define XBARA_CTRL1_STS3 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_CTRL1_STS3_SHIFT)) & XBARA_CTRL1_STS3_MASK)

STS3 - Edge detection status for XBAR_OUT3 0b0..Active edge not yet detected on XBAR_OUT3 0b1..Active edge detected on XBAR_OUT3

Definition at line 47384 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_STS3_MASK

#define XBARA_CTRL1_STS3_MASK (0x1000U)

Definition at line 47378 of file MIMXRT1062.h.

## ◆ XBARA_CTRL1_STS3_SHIFT

#define XBARA_CTRL1_STS3_SHIFT (12U)

Definition at line 47379 of file MIMXRT1062.h.

## ◆ XBARA_SEL0_SEL0

#define XBARA_SEL0_SEL0 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL0_SEL0_SHIFT)) & XBARA_SEL0_SEL0_MASK)

Definition at line 46603 of file MIMXRT1062.h.

## ◆ XBARA_SEL0_SEL0_MASK

#define XBARA_SEL0_SEL0_MASK (0x7FU)

Definition at line 46601 of file MIMXRT1062.h.

## ◆ XBARA_SEL0_SEL0_SHIFT

#define XBARA_SEL0_SEL0_SHIFT (0U)

Definition at line 46602 of file MIMXRT1062.h.

## ◆ XBARA_SEL0_SEL1

#define XBARA_SEL0_SEL1 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL0_SEL1_SHIFT)) & XBARA_SEL0_SEL1_MASK)

Definition at line 46606 of file MIMXRT1062.h.

## ◆ XBARA_SEL0_SEL1_MASK

#define XBARA_SEL0_SEL1_MASK (0x7F00U)

Definition at line 46604 of file MIMXRT1062.h.

## ◆ XBARA_SEL0_SEL1_SHIFT

#define XBARA_SEL0_SEL1_SHIFT (8U)

Definition at line 46605 of file MIMXRT1062.h.

## ◆ XBARA_SEL10_SEL20

#define XBARA_SEL10_SEL20 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL10_SEL20_SHIFT)) & XBARA_SEL10_SEL20_MASK)

Definition at line 46703 of file MIMXRT1062.h.

## ◆ XBARA_SEL10_SEL20_MASK

#define XBARA_SEL10_SEL20_MASK (0x7FU)

Definition at line 46701 of file MIMXRT1062.h.

## ◆ XBARA_SEL10_SEL20_SHIFT

#define XBARA_SEL10_SEL20_SHIFT (0U)

Definition at line 46702 of file MIMXRT1062.h.

## ◆ XBARA_SEL10_SEL21

#define XBARA_SEL10_SEL21 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL10_SEL21_SHIFT)) & XBARA_SEL10_SEL21_MASK)

Definition at line 46706 of file MIMXRT1062.h.

## ◆ XBARA_SEL10_SEL21_MASK

#define XBARA_SEL10_SEL21_MASK (0x7F00U)

Definition at line 46704 of file MIMXRT1062.h.

## ◆ XBARA_SEL10_SEL21_SHIFT

#define XBARA_SEL10_SEL21_SHIFT (8U)

Definition at line 46705 of file MIMXRT1062.h.

## ◆ XBARA_SEL11_SEL22

#define XBARA_SEL11_SEL22 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL11_SEL22_SHIFT)) & XBARA_SEL11_SEL22_MASK)

Definition at line 46713 of file MIMXRT1062.h.

## ◆ XBARA_SEL11_SEL22_MASK

#define XBARA_SEL11_SEL22_MASK (0x7FU)

Definition at line 46711 of file MIMXRT1062.h.

## ◆ XBARA_SEL11_SEL22_SHIFT

#define XBARA_SEL11_SEL22_SHIFT (0U)

Definition at line 46712 of file MIMXRT1062.h.

## ◆ XBARA_SEL11_SEL23

#define XBARA_SEL11_SEL23 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL11_SEL23_SHIFT)) & XBARA_SEL11_SEL23_MASK)

Definition at line 46716 of file MIMXRT1062.h.

## ◆ XBARA_SEL11_SEL23_MASK

#define XBARA_SEL11_SEL23_MASK (0x7F00U)

Definition at line 46714 of file MIMXRT1062.h.

## ◆ XBARA_SEL11_SEL23_SHIFT

#define XBARA_SEL11_SEL23_SHIFT (8U)

Definition at line 46715 of file MIMXRT1062.h.

## ◆ XBARA_SEL12_SEL24

#define XBARA_SEL12_SEL24 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL12_SEL24_SHIFT)) & XBARA_SEL12_SEL24_MASK)

Definition at line 46723 of file MIMXRT1062.h.

## ◆ XBARA_SEL12_SEL24_MASK

#define XBARA_SEL12_SEL24_MASK (0x7FU)

Definition at line 46721 of file MIMXRT1062.h.

## ◆ XBARA_SEL12_SEL24_SHIFT

#define XBARA_SEL12_SEL24_SHIFT (0U)

Definition at line 46722 of file MIMXRT1062.h.

## ◆ XBARA_SEL12_SEL25

#define XBARA_SEL12_SEL25 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL12_SEL25_SHIFT)) & XBARA_SEL12_SEL25_MASK)

Definition at line 46726 of file MIMXRT1062.h.

## ◆ XBARA_SEL12_SEL25_MASK

#define XBARA_SEL12_SEL25_MASK (0x7F00U)

Definition at line 46724 of file MIMXRT1062.h.

## ◆ XBARA_SEL12_SEL25_SHIFT

#define XBARA_SEL12_SEL25_SHIFT (8U)

Definition at line 46725 of file MIMXRT1062.h.

## ◆ XBARA_SEL13_SEL26

#define XBARA_SEL13_SEL26 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL13_SEL26_SHIFT)) & XBARA_SEL13_SEL26_MASK)

Definition at line 46733 of file MIMXRT1062.h.

## ◆ XBARA_SEL13_SEL26_MASK

#define XBARA_SEL13_SEL26_MASK (0x7FU)

Definition at line 46731 of file MIMXRT1062.h.

## ◆ XBARA_SEL13_SEL26_SHIFT

#define XBARA_SEL13_SEL26_SHIFT (0U)

Definition at line 46732 of file MIMXRT1062.h.

## ◆ XBARA_SEL13_SEL27

#define XBARA_SEL13_SEL27 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL13_SEL27_SHIFT)) & XBARA_SEL13_SEL27_MASK)

Definition at line 46736 of file MIMXRT1062.h.

## ◆ XBARA_SEL13_SEL27_MASK

#define XBARA_SEL13_SEL27_MASK (0x7F00U)

Definition at line 46734 of file MIMXRT1062.h.

## ◆ XBARA_SEL13_SEL27_SHIFT

#define XBARA_SEL13_SEL27_SHIFT (8U)

Definition at line 46735 of file MIMXRT1062.h.

## ◆ XBARA_SEL14_SEL28

#define XBARA_SEL14_SEL28 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL14_SEL28_SHIFT)) & XBARA_SEL14_SEL28_MASK)

Definition at line 46743 of file MIMXRT1062.h.

## ◆ XBARA_SEL14_SEL28_MASK

#define XBARA_SEL14_SEL28_MASK (0x7FU)

Definition at line 46741 of file MIMXRT1062.h.

## ◆ XBARA_SEL14_SEL28_SHIFT

#define XBARA_SEL14_SEL28_SHIFT (0U)

Definition at line 46742 of file MIMXRT1062.h.

## ◆ XBARA_SEL14_SEL29

#define XBARA_SEL14_SEL29 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL14_SEL29_SHIFT)) & XBARA_SEL14_SEL29_MASK)

Definition at line 46746 of file MIMXRT1062.h.

## ◆ XBARA_SEL14_SEL29_MASK

#define XBARA_SEL14_SEL29_MASK (0x7F00U)

Definition at line 46744 of file MIMXRT1062.h.

## ◆ XBARA_SEL14_SEL29_SHIFT

#define XBARA_SEL14_SEL29_SHIFT (8U)

Definition at line 46745 of file MIMXRT1062.h.

## ◆ XBARA_SEL15_SEL30

#define XBARA_SEL15_SEL30 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL15_SEL30_SHIFT)) & XBARA_SEL15_SEL30_MASK)

Definition at line 46753 of file MIMXRT1062.h.

## ◆ XBARA_SEL15_SEL30_MASK

#define XBARA_SEL15_SEL30_MASK (0x7FU)

Definition at line 46751 of file MIMXRT1062.h.

## ◆ XBARA_SEL15_SEL30_SHIFT

#define XBARA_SEL15_SEL30_SHIFT (0U)

Definition at line 46752 of file MIMXRT1062.h.

## ◆ XBARA_SEL15_SEL31

#define XBARA_SEL15_SEL31 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL15_SEL31_SHIFT)) & XBARA_SEL15_SEL31_MASK)

Definition at line 46756 of file MIMXRT1062.h.

## ◆ XBARA_SEL15_SEL31_MASK

#define XBARA_SEL15_SEL31_MASK (0x7F00U)

Definition at line 46754 of file MIMXRT1062.h.

## ◆ XBARA_SEL15_SEL31_SHIFT

#define XBARA_SEL15_SEL31_SHIFT (8U)

Definition at line 46755 of file MIMXRT1062.h.

## ◆ XBARA_SEL16_SEL32

#define XBARA_SEL16_SEL32 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL16_SEL32_SHIFT)) & XBARA_SEL16_SEL32_MASK)

Definition at line 46763 of file MIMXRT1062.h.

## ◆ XBARA_SEL16_SEL32_MASK

#define XBARA_SEL16_SEL32_MASK (0x7FU)

Definition at line 46761 of file MIMXRT1062.h.

## ◆ XBARA_SEL16_SEL32_SHIFT

#define XBARA_SEL16_SEL32_SHIFT (0U)

Definition at line 46762 of file MIMXRT1062.h.

## ◆ XBARA_SEL16_SEL33

#define XBARA_SEL16_SEL33 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL16_SEL33_SHIFT)) & XBARA_SEL16_SEL33_MASK)

Definition at line 46766 of file MIMXRT1062.h.

## ◆ XBARA_SEL16_SEL33_MASK

#define XBARA_SEL16_SEL33_MASK (0x7F00U)

Definition at line 46764 of file MIMXRT1062.h.

## ◆ XBARA_SEL16_SEL33_SHIFT

#define XBARA_SEL16_SEL33_SHIFT (8U)

Definition at line 46765 of file MIMXRT1062.h.

## ◆ XBARA_SEL17_SEL34

#define XBARA_SEL17_SEL34 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL17_SEL34_SHIFT)) & XBARA_SEL17_SEL34_MASK)

Definition at line 46773 of file MIMXRT1062.h.

## ◆ XBARA_SEL17_SEL34_MASK

#define XBARA_SEL17_SEL34_MASK (0x7FU)

Definition at line 46771 of file MIMXRT1062.h.

## ◆ XBARA_SEL17_SEL34_SHIFT

#define XBARA_SEL17_SEL34_SHIFT (0U)

Definition at line 46772 of file MIMXRT1062.h.

## ◆ XBARA_SEL17_SEL35

#define XBARA_SEL17_SEL35 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL17_SEL35_SHIFT)) & XBARA_SEL17_SEL35_MASK)

Definition at line 46776 of file MIMXRT1062.h.

## ◆ XBARA_SEL17_SEL35_MASK

#define XBARA_SEL17_SEL35_MASK (0x7F00U)

Definition at line 46774 of file MIMXRT1062.h.

## ◆ XBARA_SEL17_SEL35_SHIFT

#define XBARA_SEL17_SEL35_SHIFT (8U)

Definition at line 46775 of file MIMXRT1062.h.

## ◆ XBARA_SEL18_SEL36

#define XBARA_SEL18_SEL36 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL18_SEL36_SHIFT)) & XBARA_SEL18_SEL36_MASK)

Definition at line 46783 of file MIMXRT1062.h.

## ◆ XBARA_SEL18_SEL36_MASK

#define XBARA_SEL18_SEL36_MASK (0x7FU)

Definition at line 46781 of file MIMXRT1062.h.

## ◆ XBARA_SEL18_SEL36_SHIFT

#define XBARA_SEL18_SEL36_SHIFT (0U)

Definition at line 46782 of file MIMXRT1062.h.

## ◆ XBARA_SEL18_SEL37

#define XBARA_SEL18_SEL37 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL18_SEL37_SHIFT)) & XBARA_SEL18_SEL37_MASK)

Definition at line 46786 of file MIMXRT1062.h.

## ◆ XBARA_SEL18_SEL37_MASK

#define XBARA_SEL18_SEL37_MASK (0x7F00U)

Definition at line 46784 of file MIMXRT1062.h.

## ◆ XBARA_SEL18_SEL37_SHIFT

#define XBARA_SEL18_SEL37_SHIFT (8U)

Definition at line 46785 of file MIMXRT1062.h.

## ◆ XBARA_SEL19_SEL38

#define XBARA_SEL19_SEL38 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL19_SEL38_SHIFT)) & XBARA_SEL19_SEL38_MASK)

Definition at line 46793 of file MIMXRT1062.h.

## ◆ XBARA_SEL19_SEL38_MASK

#define XBARA_SEL19_SEL38_MASK (0x7FU)

Definition at line 46791 of file MIMXRT1062.h.

## ◆ XBARA_SEL19_SEL38_SHIFT

#define XBARA_SEL19_SEL38_SHIFT (0U)

Definition at line 46792 of file MIMXRT1062.h.

## ◆ XBARA_SEL19_SEL39

#define XBARA_SEL19_SEL39 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL19_SEL39_SHIFT)) & XBARA_SEL19_SEL39_MASK)

Definition at line 46796 of file MIMXRT1062.h.

## ◆ XBARA_SEL19_SEL39_MASK

#define XBARA_SEL19_SEL39_MASK (0x7F00U)

Definition at line 46794 of file MIMXRT1062.h.

## ◆ XBARA_SEL19_SEL39_SHIFT

#define XBARA_SEL19_SEL39_SHIFT (8U)

Definition at line 46795 of file MIMXRT1062.h.

## ◆ XBARA_SEL1_SEL2

#define XBARA_SEL1_SEL2 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL1_SEL2_SHIFT)) & XBARA_SEL1_SEL2_MASK)

Definition at line 46613 of file MIMXRT1062.h.

## ◆ XBARA_SEL1_SEL2_MASK

#define XBARA_SEL1_SEL2_MASK (0x7FU)

Definition at line 46611 of file MIMXRT1062.h.

## ◆ XBARA_SEL1_SEL2_SHIFT

#define XBARA_SEL1_SEL2_SHIFT (0U)

Definition at line 46612 of file MIMXRT1062.h.

## ◆ XBARA_SEL1_SEL3

#define XBARA_SEL1_SEL3 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL1_SEL3_SHIFT)) & XBARA_SEL1_SEL3_MASK)

Definition at line 46616 of file MIMXRT1062.h.

## ◆ XBARA_SEL1_SEL3_MASK

#define XBARA_SEL1_SEL3_MASK (0x7F00U)

Definition at line 46614 of file MIMXRT1062.h.

## ◆ XBARA_SEL1_SEL3_SHIFT

#define XBARA_SEL1_SEL3_SHIFT (8U)

Definition at line 46615 of file MIMXRT1062.h.

## ◆ XBARA_SEL20_SEL40

#define XBARA_SEL20_SEL40 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL20_SEL40_SHIFT)) & XBARA_SEL20_SEL40_MASK)

Definition at line 46803 of file MIMXRT1062.h.

## ◆ XBARA_SEL20_SEL40_MASK

#define XBARA_SEL20_SEL40_MASK (0x7FU)

Definition at line 46801 of file MIMXRT1062.h.

## ◆ XBARA_SEL20_SEL40_SHIFT

#define XBARA_SEL20_SEL40_SHIFT (0U)

Definition at line 46802 of file MIMXRT1062.h.

## ◆ XBARA_SEL20_SEL41

#define XBARA_SEL20_SEL41 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL20_SEL41_SHIFT)) & XBARA_SEL20_SEL41_MASK)

Definition at line 46806 of file MIMXRT1062.h.

## ◆ XBARA_SEL20_SEL41_MASK

#define XBARA_SEL20_SEL41_MASK (0x7F00U)

Definition at line 46804 of file MIMXRT1062.h.

## ◆ XBARA_SEL20_SEL41_SHIFT

#define XBARA_SEL20_SEL41_SHIFT (8U)

Definition at line 46805 of file MIMXRT1062.h.

## ◆ XBARA_SEL21_SEL42

#define XBARA_SEL21_SEL42 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL21_SEL42_SHIFT)) & XBARA_SEL21_SEL42_MASK)

Definition at line 46813 of file MIMXRT1062.h.

## ◆ XBARA_SEL21_SEL42_MASK

#define XBARA_SEL21_SEL42_MASK (0x7FU)

Definition at line 46811 of file MIMXRT1062.h.

## ◆ XBARA_SEL21_SEL42_SHIFT

#define XBARA_SEL21_SEL42_SHIFT (0U)

Definition at line 46812 of file MIMXRT1062.h.

## ◆ XBARA_SEL21_SEL43

#define XBARA_SEL21_SEL43 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL21_SEL43_SHIFT)) & XBARA_SEL21_SEL43_MASK)

Definition at line 46816 of file MIMXRT1062.h.

## ◆ XBARA_SEL21_SEL43_MASK

#define XBARA_SEL21_SEL43_MASK (0x7F00U)

Definition at line 46814 of file MIMXRT1062.h.

## ◆ XBARA_SEL21_SEL43_SHIFT

#define XBARA_SEL21_SEL43_SHIFT (8U)

Definition at line 46815 of file MIMXRT1062.h.

## ◆ XBARA_SEL22_SEL44

#define XBARA_SEL22_SEL44 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL22_SEL44_SHIFT)) & XBARA_SEL22_SEL44_MASK)

Definition at line 46823 of file MIMXRT1062.h.

## ◆ XBARA_SEL22_SEL44_MASK

#define XBARA_SEL22_SEL44_MASK (0x7FU)

Definition at line 46821 of file MIMXRT1062.h.

## ◆ XBARA_SEL22_SEL44_SHIFT

#define XBARA_SEL22_SEL44_SHIFT (0U)

Definition at line 46822 of file MIMXRT1062.h.

## ◆ XBARA_SEL22_SEL45

#define XBARA_SEL22_SEL45 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL22_SEL45_SHIFT)) & XBARA_SEL22_SEL45_MASK)

Definition at line 46826 of file MIMXRT1062.h.

## ◆ XBARA_SEL22_SEL45_MASK

#define XBARA_SEL22_SEL45_MASK (0x7F00U)

Definition at line 46824 of file MIMXRT1062.h.

## ◆ XBARA_SEL22_SEL45_SHIFT

#define XBARA_SEL22_SEL45_SHIFT (8U)

Definition at line 46825 of file MIMXRT1062.h.

## ◆ XBARA_SEL23_SEL46

#define XBARA_SEL23_SEL46 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL23_SEL46_SHIFT)) & XBARA_SEL23_SEL46_MASK)

Definition at line 46833 of file MIMXRT1062.h.

## ◆ XBARA_SEL23_SEL46_MASK

#define XBARA_SEL23_SEL46_MASK (0x7FU)

Definition at line 46831 of file MIMXRT1062.h.

## ◆ XBARA_SEL23_SEL46_SHIFT

#define XBARA_SEL23_SEL46_SHIFT (0U)

Definition at line 46832 of file MIMXRT1062.h.

## ◆ XBARA_SEL23_SEL47

#define XBARA_SEL23_SEL47 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL23_SEL47_SHIFT)) & XBARA_SEL23_SEL47_MASK)

Definition at line 46836 of file MIMXRT1062.h.

## ◆ XBARA_SEL23_SEL47_MASK

#define XBARA_SEL23_SEL47_MASK (0x7F00U)

Definition at line 46834 of file MIMXRT1062.h.

## ◆ XBARA_SEL23_SEL47_SHIFT

#define XBARA_SEL23_SEL47_SHIFT (8U)

Definition at line 46835 of file MIMXRT1062.h.

## ◆ XBARA_SEL24_SEL48

#define XBARA_SEL24_SEL48 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL24_SEL48_SHIFT)) & XBARA_SEL24_SEL48_MASK)

Definition at line 46843 of file MIMXRT1062.h.

## ◆ XBARA_SEL24_SEL48_MASK

#define XBARA_SEL24_SEL48_MASK (0x7FU)

Definition at line 46841 of file MIMXRT1062.h.

## ◆ XBARA_SEL24_SEL48_SHIFT

#define XBARA_SEL24_SEL48_SHIFT (0U)

Definition at line 46842 of file MIMXRT1062.h.

## ◆ XBARA_SEL24_SEL49

#define XBARA_SEL24_SEL49 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL24_SEL49_SHIFT)) & XBARA_SEL24_SEL49_MASK)

Definition at line 46846 of file MIMXRT1062.h.

## ◆ XBARA_SEL24_SEL49_MASK

#define XBARA_SEL24_SEL49_MASK (0x7F00U)

Definition at line 46844 of file MIMXRT1062.h.

## ◆ XBARA_SEL24_SEL49_SHIFT

#define XBARA_SEL24_SEL49_SHIFT (8U)

Definition at line 46845 of file MIMXRT1062.h.

## ◆ XBARA_SEL25_SEL50

#define XBARA_SEL25_SEL50 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL25_SEL50_SHIFT)) & XBARA_SEL25_SEL50_MASK)

Definition at line 46853 of file MIMXRT1062.h.

## ◆ XBARA_SEL25_SEL50_MASK

#define XBARA_SEL25_SEL50_MASK (0x7FU)

Definition at line 46851 of file MIMXRT1062.h.

## ◆ XBARA_SEL25_SEL50_SHIFT

#define XBARA_SEL25_SEL50_SHIFT (0U)

Definition at line 46852 of file MIMXRT1062.h.

## ◆ XBARA_SEL25_SEL51

#define XBARA_SEL25_SEL51 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL25_SEL51_SHIFT)) & XBARA_SEL25_SEL51_MASK)

Definition at line 46856 of file MIMXRT1062.h.

## ◆ XBARA_SEL25_SEL51_MASK

#define XBARA_SEL25_SEL51_MASK (0x7F00U)

Definition at line 46854 of file MIMXRT1062.h.

## ◆ XBARA_SEL25_SEL51_SHIFT

#define XBARA_SEL25_SEL51_SHIFT (8U)

Definition at line 46855 of file MIMXRT1062.h.

## ◆ XBARA_SEL26_SEL52

#define XBARA_SEL26_SEL52 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL26_SEL52_SHIFT)) & XBARA_SEL26_SEL52_MASK)

Definition at line 46863 of file MIMXRT1062.h.

## ◆ XBARA_SEL26_SEL52_MASK

#define XBARA_SEL26_SEL52_MASK (0x7FU)

Definition at line 46861 of file MIMXRT1062.h.

## ◆ XBARA_SEL26_SEL52_SHIFT

#define XBARA_SEL26_SEL52_SHIFT (0U)

Definition at line 46862 of file MIMXRT1062.h.

## ◆ XBARA_SEL26_SEL53

#define XBARA_SEL26_SEL53 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL26_SEL53_SHIFT)) & XBARA_SEL26_SEL53_MASK)

Definition at line 46866 of file MIMXRT1062.h.

## ◆ XBARA_SEL26_SEL53_MASK

#define XBARA_SEL26_SEL53_MASK (0x7F00U)

Definition at line 46864 of file MIMXRT1062.h.

## ◆ XBARA_SEL26_SEL53_SHIFT

#define XBARA_SEL26_SEL53_SHIFT (8U)

Definition at line 46865 of file MIMXRT1062.h.

## ◆ XBARA_SEL27_SEL54

#define XBARA_SEL27_SEL54 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL27_SEL54_SHIFT)) & XBARA_SEL27_SEL54_MASK)

Definition at line 46873 of file MIMXRT1062.h.

## ◆ XBARA_SEL27_SEL54_MASK

#define XBARA_SEL27_SEL54_MASK (0x7FU)

Definition at line 46871 of file MIMXRT1062.h.

## ◆ XBARA_SEL27_SEL54_SHIFT

#define XBARA_SEL27_SEL54_SHIFT (0U)

Definition at line 46872 of file MIMXRT1062.h.

## ◆ XBARA_SEL27_SEL55

#define XBARA_SEL27_SEL55 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL27_SEL55_SHIFT)) & XBARA_SEL27_SEL55_MASK)

Definition at line 46876 of file MIMXRT1062.h.

## ◆ XBARA_SEL27_SEL55_MASK

#define XBARA_SEL27_SEL55_MASK (0x7F00U)

Definition at line 46874 of file MIMXRT1062.h.

## ◆ XBARA_SEL27_SEL55_SHIFT

#define XBARA_SEL27_SEL55_SHIFT (8U)

Definition at line 46875 of file MIMXRT1062.h.

## ◆ XBARA_SEL28_SEL56

#define XBARA_SEL28_SEL56 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL28_SEL56_SHIFT)) & XBARA_SEL28_SEL56_MASK)

Definition at line 46883 of file MIMXRT1062.h.

## ◆ XBARA_SEL28_SEL56_MASK

#define XBARA_SEL28_SEL56_MASK (0x7FU)

Definition at line 46881 of file MIMXRT1062.h.

## ◆ XBARA_SEL28_SEL56_SHIFT

#define XBARA_SEL28_SEL56_SHIFT (0U)

Definition at line 46882 of file MIMXRT1062.h.

## ◆ XBARA_SEL28_SEL57

#define XBARA_SEL28_SEL57 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL28_SEL57_SHIFT)) & XBARA_SEL28_SEL57_MASK)

Definition at line 46886 of file MIMXRT1062.h.

## ◆ XBARA_SEL28_SEL57_MASK

#define XBARA_SEL28_SEL57_MASK (0x7F00U)

Definition at line 46884 of file MIMXRT1062.h.

## ◆ XBARA_SEL28_SEL57_SHIFT

#define XBARA_SEL28_SEL57_SHIFT (8U)

Definition at line 46885 of file MIMXRT1062.h.

## ◆ XBARA_SEL29_SEL58

#define XBARA_SEL29_SEL58 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL29_SEL58_SHIFT)) & XBARA_SEL29_SEL58_MASK)

Definition at line 46893 of file MIMXRT1062.h.

## ◆ XBARA_SEL29_SEL58_MASK

#define XBARA_SEL29_SEL58_MASK (0x7FU)

Definition at line 46891 of file MIMXRT1062.h.

## ◆ XBARA_SEL29_SEL58_SHIFT

#define XBARA_SEL29_SEL58_SHIFT (0U)

Definition at line 46892 of file MIMXRT1062.h.

## ◆ XBARA_SEL29_SEL59

#define XBARA_SEL29_SEL59 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL29_SEL59_SHIFT)) & XBARA_SEL29_SEL59_MASK)

Definition at line 46896 of file MIMXRT1062.h.

## ◆ XBARA_SEL29_SEL59_MASK

#define XBARA_SEL29_SEL59_MASK (0x7F00U)

Definition at line 46894 of file MIMXRT1062.h.

## ◆ XBARA_SEL29_SEL59_SHIFT

#define XBARA_SEL29_SEL59_SHIFT (8U)

Definition at line 46895 of file MIMXRT1062.h.

## ◆ XBARA_SEL2_SEL4

#define XBARA_SEL2_SEL4 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL2_SEL4_SHIFT)) & XBARA_SEL2_SEL4_MASK)

Definition at line 46623 of file MIMXRT1062.h.

## ◆ XBARA_SEL2_SEL4_MASK

#define XBARA_SEL2_SEL4_MASK (0x7FU)

Definition at line 46621 of file MIMXRT1062.h.

## ◆ XBARA_SEL2_SEL4_SHIFT

#define XBARA_SEL2_SEL4_SHIFT (0U)

Definition at line 46622 of file MIMXRT1062.h.

## ◆ XBARA_SEL2_SEL5

#define XBARA_SEL2_SEL5 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL2_SEL5_SHIFT)) & XBARA_SEL2_SEL5_MASK)

Definition at line 46626 of file MIMXRT1062.h.

## ◆ XBARA_SEL2_SEL5_MASK

#define XBARA_SEL2_SEL5_MASK (0x7F00U)

Definition at line 46624 of file MIMXRT1062.h.

## ◆ XBARA_SEL2_SEL5_SHIFT

#define XBARA_SEL2_SEL5_SHIFT (8U)

Definition at line 46625 of file MIMXRT1062.h.

## ◆ XBARA_SEL30_SEL60

#define XBARA_SEL30_SEL60 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL30_SEL60_SHIFT)) & XBARA_SEL30_SEL60_MASK)

Definition at line 46903 of file MIMXRT1062.h.

## ◆ XBARA_SEL30_SEL60_MASK

#define XBARA_SEL30_SEL60_MASK (0x7FU)

Definition at line 46901 of file MIMXRT1062.h.

## ◆ XBARA_SEL30_SEL60_SHIFT

#define XBARA_SEL30_SEL60_SHIFT (0U)

Definition at line 46902 of file MIMXRT1062.h.

## ◆ XBARA_SEL30_SEL61

#define XBARA_SEL30_SEL61 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL30_SEL61_SHIFT)) & XBARA_SEL30_SEL61_MASK)

Definition at line 46906 of file MIMXRT1062.h.

## ◆ XBARA_SEL30_SEL61_MASK

#define XBARA_SEL30_SEL61_MASK (0x7F00U)

Definition at line 46904 of file MIMXRT1062.h.

## ◆ XBARA_SEL30_SEL61_SHIFT

#define XBARA_SEL30_SEL61_SHIFT (8U)

Definition at line 46905 of file MIMXRT1062.h.

## ◆ XBARA_SEL31_SEL62

#define XBARA_SEL31_SEL62 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL31_SEL62_SHIFT)) & XBARA_SEL31_SEL62_MASK)

Definition at line 46913 of file MIMXRT1062.h.

## ◆ XBARA_SEL31_SEL62_MASK

#define XBARA_SEL31_SEL62_MASK (0x7FU)

Definition at line 46911 of file MIMXRT1062.h.

## ◆ XBARA_SEL31_SEL62_SHIFT

#define XBARA_SEL31_SEL62_SHIFT (0U)

Definition at line 46912 of file MIMXRT1062.h.

## ◆ XBARA_SEL31_SEL63

#define XBARA_SEL31_SEL63 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL31_SEL63_SHIFT)) & XBARA_SEL31_SEL63_MASK)

Definition at line 46916 of file MIMXRT1062.h.

## ◆ XBARA_SEL31_SEL63_MASK

#define XBARA_SEL31_SEL63_MASK (0x7F00U)

Definition at line 46914 of file MIMXRT1062.h.

## ◆ XBARA_SEL31_SEL63_SHIFT

#define XBARA_SEL31_SEL63_SHIFT (8U)

Definition at line 46915 of file MIMXRT1062.h.

## ◆ XBARA_SEL32_SEL64

#define XBARA_SEL32_SEL64 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL32_SEL64_SHIFT)) & XBARA_SEL32_SEL64_MASK)

Definition at line 46923 of file MIMXRT1062.h.

## ◆ XBARA_SEL32_SEL64_MASK

#define XBARA_SEL32_SEL64_MASK (0x7FU)

Definition at line 46921 of file MIMXRT1062.h.

## ◆ XBARA_SEL32_SEL64_SHIFT

#define XBARA_SEL32_SEL64_SHIFT (0U)

Definition at line 46922 of file MIMXRT1062.h.

## ◆ XBARA_SEL32_SEL65

#define XBARA_SEL32_SEL65 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL32_SEL65_SHIFT)) & XBARA_SEL32_SEL65_MASK)

Definition at line 46926 of file MIMXRT1062.h.

## ◆ XBARA_SEL32_SEL65_MASK

#define XBARA_SEL32_SEL65_MASK (0x7F00U)

Definition at line 46924 of file MIMXRT1062.h.

## ◆ XBARA_SEL32_SEL65_SHIFT

#define XBARA_SEL32_SEL65_SHIFT (8U)

Definition at line 46925 of file MIMXRT1062.h.

## ◆ XBARA_SEL33_SEL66

#define XBARA_SEL33_SEL66 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL33_SEL66_SHIFT)) & XBARA_SEL33_SEL66_MASK)

Definition at line 46933 of file MIMXRT1062.h.

## ◆ XBARA_SEL33_SEL66_MASK

#define XBARA_SEL33_SEL66_MASK (0x7FU)

Definition at line 46931 of file MIMXRT1062.h.

## ◆ XBARA_SEL33_SEL66_SHIFT

#define XBARA_SEL33_SEL66_SHIFT (0U)

Definition at line 46932 of file MIMXRT1062.h.

## ◆ XBARA_SEL33_SEL67

#define XBARA_SEL33_SEL67 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL33_SEL67_SHIFT)) & XBARA_SEL33_SEL67_MASK)

Definition at line 46936 of file MIMXRT1062.h.

## ◆ XBARA_SEL33_SEL67_MASK

#define XBARA_SEL33_SEL67_MASK (0x7F00U)

Definition at line 46934 of file MIMXRT1062.h.

## ◆ XBARA_SEL33_SEL67_SHIFT

#define XBARA_SEL33_SEL67_SHIFT (8U)

Definition at line 46935 of file MIMXRT1062.h.

## ◆ XBARA_SEL34_SEL68

#define XBARA_SEL34_SEL68 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL34_SEL68_SHIFT)) & XBARA_SEL34_SEL68_MASK)

Definition at line 46943 of file MIMXRT1062.h.

## ◆ XBARA_SEL34_SEL68_MASK

#define XBARA_SEL34_SEL68_MASK (0x7FU)

Definition at line 46941 of file MIMXRT1062.h.

## ◆ XBARA_SEL34_SEL68_SHIFT

#define XBARA_SEL34_SEL68_SHIFT (0U)

Definition at line 46942 of file MIMXRT1062.h.

## ◆ XBARA_SEL34_SEL69

#define XBARA_SEL34_SEL69 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL34_SEL69_SHIFT)) & XBARA_SEL34_SEL69_MASK)

Definition at line 46946 of file MIMXRT1062.h.

## ◆ XBARA_SEL34_SEL69_MASK

#define XBARA_SEL34_SEL69_MASK (0x7F00U)

Definition at line 46944 of file MIMXRT1062.h.

## ◆ XBARA_SEL34_SEL69_SHIFT

#define XBARA_SEL34_SEL69_SHIFT (8U)

Definition at line 46945 of file MIMXRT1062.h.

## ◆ XBARA_SEL35_SEL70

#define XBARA_SEL35_SEL70 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL35_SEL70_SHIFT)) & XBARA_SEL35_SEL70_MASK)

Definition at line 46953 of file MIMXRT1062.h.

## ◆ XBARA_SEL35_SEL70_MASK

#define XBARA_SEL35_SEL70_MASK (0x7FU)

Definition at line 46951 of file MIMXRT1062.h.

## ◆ XBARA_SEL35_SEL70_SHIFT

#define XBARA_SEL35_SEL70_SHIFT (0U)

Definition at line 46952 of file MIMXRT1062.h.

## ◆ XBARA_SEL35_SEL71

#define XBARA_SEL35_SEL71 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL35_SEL71_SHIFT)) & XBARA_SEL35_SEL71_MASK)

Definition at line 46956 of file MIMXRT1062.h.

## ◆ XBARA_SEL35_SEL71_MASK

#define XBARA_SEL35_SEL71_MASK (0x7F00U)

Definition at line 46954 of file MIMXRT1062.h.

## ◆ XBARA_SEL35_SEL71_SHIFT

#define XBARA_SEL35_SEL71_SHIFT (8U)

Definition at line 46955 of file MIMXRT1062.h.

## ◆ XBARA_SEL36_SEL72

#define XBARA_SEL36_SEL72 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL36_SEL72_SHIFT)) & XBARA_SEL36_SEL72_MASK)

Definition at line 46963 of file MIMXRT1062.h.

## ◆ XBARA_SEL36_SEL72_MASK

#define XBARA_SEL36_SEL72_MASK (0x7FU)

Definition at line 46961 of file MIMXRT1062.h.

## ◆ XBARA_SEL36_SEL72_SHIFT

#define XBARA_SEL36_SEL72_SHIFT (0U)

Definition at line 46962 of file MIMXRT1062.h.

## ◆ XBARA_SEL36_SEL73

#define XBARA_SEL36_SEL73 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL36_SEL73_SHIFT)) & XBARA_SEL36_SEL73_MASK)

Definition at line 46966 of file MIMXRT1062.h.

## ◆ XBARA_SEL36_SEL73_MASK

#define XBARA_SEL36_SEL73_MASK (0x7F00U)

Definition at line 46964 of file MIMXRT1062.h.

## ◆ XBARA_SEL36_SEL73_SHIFT

#define XBARA_SEL36_SEL73_SHIFT (8U)

Definition at line 46965 of file MIMXRT1062.h.

## ◆ XBARA_SEL37_SEL74

#define XBARA_SEL37_SEL74 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL37_SEL74_SHIFT)) & XBARA_SEL37_SEL74_MASK)

Definition at line 46973 of file MIMXRT1062.h.

## ◆ XBARA_SEL37_SEL74_MASK

#define XBARA_SEL37_SEL74_MASK (0x7FU)

Definition at line 46971 of file MIMXRT1062.h.

## ◆ XBARA_SEL37_SEL74_SHIFT

#define XBARA_SEL37_SEL74_SHIFT (0U)

Definition at line 46972 of file MIMXRT1062.h.

## ◆ XBARA_SEL37_SEL75

#define XBARA_SEL37_SEL75 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL37_SEL75_SHIFT)) & XBARA_SEL37_SEL75_MASK)

Definition at line 46976 of file MIMXRT1062.h.

## ◆ XBARA_SEL37_SEL75_MASK

#define XBARA_SEL37_SEL75_MASK (0x7F00U)

Definition at line 46974 of file MIMXRT1062.h.

## ◆ XBARA_SEL37_SEL75_SHIFT

#define XBARA_SEL37_SEL75_SHIFT (8U)

Definition at line 46975 of file MIMXRT1062.h.

## ◆ XBARA_SEL38_SEL76

#define XBARA_SEL38_SEL76 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL38_SEL76_SHIFT)) & XBARA_SEL38_SEL76_MASK)

Definition at line 46983 of file MIMXRT1062.h.

## ◆ XBARA_SEL38_SEL76_MASK

#define XBARA_SEL38_SEL76_MASK (0x7FU)

Definition at line 46981 of file MIMXRT1062.h.

## ◆ XBARA_SEL38_SEL76_SHIFT

#define XBARA_SEL38_SEL76_SHIFT (0U)

Definition at line 46982 of file MIMXRT1062.h.

## ◆ XBARA_SEL38_SEL77

#define XBARA_SEL38_SEL77 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL38_SEL77_SHIFT)) & XBARA_SEL38_SEL77_MASK)

Definition at line 46986 of file MIMXRT1062.h.

## ◆ XBARA_SEL38_SEL77_MASK

#define XBARA_SEL38_SEL77_MASK (0x7F00U)

Definition at line 46984 of file MIMXRT1062.h.

## ◆ XBARA_SEL38_SEL77_SHIFT

#define XBARA_SEL38_SEL77_SHIFT (8U)

Definition at line 46985 of file MIMXRT1062.h.

## ◆ XBARA_SEL39_SEL78

#define XBARA_SEL39_SEL78 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL39_SEL78_SHIFT)) & XBARA_SEL39_SEL78_MASK)

Definition at line 46993 of file MIMXRT1062.h.

## ◆ XBARA_SEL39_SEL78_MASK

#define XBARA_SEL39_SEL78_MASK (0x7FU)

Definition at line 46991 of file MIMXRT1062.h.

## ◆ XBARA_SEL39_SEL78_SHIFT

#define XBARA_SEL39_SEL78_SHIFT (0U)

Definition at line 46992 of file MIMXRT1062.h.

## ◆ XBARA_SEL39_SEL79

#define XBARA_SEL39_SEL79 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL39_SEL79_SHIFT)) & XBARA_SEL39_SEL79_MASK)

Definition at line 46996 of file MIMXRT1062.h.

## ◆ XBARA_SEL39_SEL79_MASK

#define XBARA_SEL39_SEL79_MASK (0x7F00U)

Definition at line 46994 of file MIMXRT1062.h.

## ◆ XBARA_SEL39_SEL79_SHIFT

#define XBARA_SEL39_SEL79_SHIFT (8U)

Definition at line 46995 of file MIMXRT1062.h.

## ◆ XBARA_SEL3_SEL6

#define XBARA_SEL3_SEL6 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL3_SEL6_SHIFT)) & XBARA_SEL3_SEL6_MASK)

Definition at line 46633 of file MIMXRT1062.h.

## ◆ XBARA_SEL3_SEL6_MASK

#define XBARA_SEL3_SEL6_MASK (0x7FU)

Definition at line 46631 of file MIMXRT1062.h.

## ◆ XBARA_SEL3_SEL6_SHIFT

#define XBARA_SEL3_SEL6_SHIFT (0U)

Definition at line 46632 of file MIMXRT1062.h.

## ◆ XBARA_SEL3_SEL7

#define XBARA_SEL3_SEL7 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL3_SEL7_SHIFT)) & XBARA_SEL3_SEL7_MASK)

Definition at line 46636 of file MIMXRT1062.h.

## ◆ XBARA_SEL3_SEL7_MASK

#define XBARA_SEL3_SEL7_MASK (0x7F00U)

Definition at line 46634 of file MIMXRT1062.h.

## ◆ XBARA_SEL3_SEL7_SHIFT

#define XBARA_SEL3_SEL7_SHIFT (8U)

Definition at line 46635 of file MIMXRT1062.h.

## ◆ XBARA_SEL40_SEL80

#define XBARA_SEL40_SEL80 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL40_SEL80_SHIFT)) & XBARA_SEL40_SEL80_MASK)

Definition at line 47003 of file MIMXRT1062.h.

## ◆ XBARA_SEL40_SEL80_MASK

#define XBARA_SEL40_SEL80_MASK (0x7FU)

Definition at line 47001 of file MIMXRT1062.h.

## ◆ XBARA_SEL40_SEL80_SHIFT

#define XBARA_SEL40_SEL80_SHIFT (0U)

Definition at line 47002 of file MIMXRT1062.h.

## ◆ XBARA_SEL40_SEL81

#define XBARA_SEL40_SEL81 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL40_SEL81_SHIFT)) & XBARA_SEL40_SEL81_MASK)

Definition at line 47006 of file MIMXRT1062.h.

## ◆ XBARA_SEL40_SEL81_MASK

#define XBARA_SEL40_SEL81_MASK (0x7F00U)

Definition at line 47004 of file MIMXRT1062.h.

## ◆ XBARA_SEL40_SEL81_SHIFT

#define XBARA_SEL40_SEL81_SHIFT (8U)

Definition at line 47005 of file MIMXRT1062.h.

## ◆ XBARA_SEL41_SEL82

#define XBARA_SEL41_SEL82 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL41_SEL82_SHIFT)) & XBARA_SEL41_SEL82_MASK)

Definition at line 47013 of file MIMXRT1062.h.

## ◆ XBARA_SEL41_SEL82_MASK

#define XBARA_SEL41_SEL82_MASK (0x7FU)

Definition at line 47011 of file MIMXRT1062.h.

## ◆ XBARA_SEL41_SEL82_SHIFT

#define XBARA_SEL41_SEL82_SHIFT (0U)

Definition at line 47012 of file MIMXRT1062.h.

## ◆ XBARA_SEL41_SEL83

#define XBARA_SEL41_SEL83 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL41_SEL83_SHIFT)) & XBARA_SEL41_SEL83_MASK)

Definition at line 47016 of file MIMXRT1062.h.

## ◆ XBARA_SEL41_SEL83_MASK

#define XBARA_SEL41_SEL83_MASK (0x7F00U)

Definition at line 47014 of file MIMXRT1062.h.

## ◆ XBARA_SEL41_SEL83_SHIFT

#define XBARA_SEL41_SEL83_SHIFT (8U)

Definition at line 47015 of file MIMXRT1062.h.

## ◆ XBARA_SEL42_SEL84

#define XBARA_SEL42_SEL84 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL42_SEL84_SHIFT)) & XBARA_SEL42_SEL84_MASK)

Definition at line 47023 of file MIMXRT1062.h.

## ◆ XBARA_SEL42_SEL84_MASK

#define XBARA_SEL42_SEL84_MASK (0x7FU)

Definition at line 47021 of file MIMXRT1062.h.

## ◆ XBARA_SEL42_SEL84_SHIFT

#define XBARA_SEL42_SEL84_SHIFT (0U)

Definition at line 47022 of file MIMXRT1062.h.

## ◆ XBARA_SEL42_SEL85

#define XBARA_SEL42_SEL85 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL42_SEL85_SHIFT)) & XBARA_SEL42_SEL85_MASK)

Definition at line 47026 of file MIMXRT1062.h.

## ◆ XBARA_SEL42_SEL85_MASK

#define XBARA_SEL42_SEL85_MASK (0x7F00U)

Definition at line 47024 of file MIMXRT1062.h.

## ◆ XBARA_SEL42_SEL85_SHIFT

#define XBARA_SEL42_SEL85_SHIFT (8U)

Definition at line 47025 of file MIMXRT1062.h.

## ◆ XBARA_SEL43_SEL86

#define XBARA_SEL43_SEL86 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL43_SEL86_SHIFT)) & XBARA_SEL43_SEL86_MASK)

Definition at line 47033 of file MIMXRT1062.h.

## ◆ XBARA_SEL43_SEL86_MASK

#define XBARA_SEL43_SEL86_MASK (0x7FU)

Definition at line 47031 of file MIMXRT1062.h.

## ◆ XBARA_SEL43_SEL86_SHIFT

#define XBARA_SEL43_SEL86_SHIFT (0U)

Definition at line 47032 of file MIMXRT1062.h.

## ◆ XBARA_SEL43_SEL87

#define XBARA_SEL43_SEL87 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL43_SEL87_SHIFT)) & XBARA_SEL43_SEL87_MASK)

Definition at line 47036 of file MIMXRT1062.h.

## ◆ XBARA_SEL43_SEL87_MASK

#define XBARA_SEL43_SEL87_MASK (0x7F00U)

Definition at line 47034 of file MIMXRT1062.h.

## ◆ XBARA_SEL43_SEL87_SHIFT

#define XBARA_SEL43_SEL87_SHIFT (8U)

Definition at line 47035 of file MIMXRT1062.h.

## ◆ XBARA_SEL44_SEL88

#define XBARA_SEL44_SEL88 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL44_SEL88_SHIFT)) & XBARA_SEL44_SEL88_MASK)

Definition at line 47043 of file MIMXRT1062.h.

## ◆ XBARA_SEL44_SEL88_MASK

#define XBARA_SEL44_SEL88_MASK (0x7FU)

Definition at line 47041 of file MIMXRT1062.h.

## ◆ XBARA_SEL44_SEL88_SHIFT

#define XBARA_SEL44_SEL88_SHIFT (0U)

Definition at line 47042 of file MIMXRT1062.h.

## ◆ XBARA_SEL44_SEL89

#define XBARA_SEL44_SEL89 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL44_SEL89_SHIFT)) & XBARA_SEL44_SEL89_MASK)

Definition at line 47046 of file MIMXRT1062.h.

## ◆ XBARA_SEL44_SEL89_MASK

#define XBARA_SEL44_SEL89_MASK (0x7F00U)

Definition at line 47044 of file MIMXRT1062.h.

## ◆ XBARA_SEL44_SEL89_SHIFT

#define XBARA_SEL44_SEL89_SHIFT (8U)

Definition at line 47045 of file MIMXRT1062.h.

## ◆ XBARA_SEL45_SEL90

#define XBARA_SEL45_SEL90 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL45_SEL90_SHIFT)) & XBARA_SEL45_SEL90_MASK)

Definition at line 47053 of file MIMXRT1062.h.

## ◆ XBARA_SEL45_SEL90_MASK

#define XBARA_SEL45_SEL90_MASK (0x7FU)

Definition at line 47051 of file MIMXRT1062.h.

## ◆ XBARA_SEL45_SEL90_SHIFT

#define XBARA_SEL45_SEL90_SHIFT (0U)

Definition at line 47052 of file MIMXRT1062.h.

## ◆ XBARA_SEL45_SEL91

#define XBARA_SEL45_SEL91 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL45_SEL91_SHIFT)) & XBARA_SEL45_SEL91_MASK)

Definition at line 47056 of file MIMXRT1062.h.

## ◆ XBARA_SEL45_SEL91_MASK

#define XBARA_SEL45_SEL91_MASK (0x7F00U)

Definition at line 47054 of file MIMXRT1062.h.

## ◆ XBARA_SEL45_SEL91_SHIFT

#define XBARA_SEL45_SEL91_SHIFT (8U)

Definition at line 47055 of file MIMXRT1062.h.

## ◆ XBARA_SEL46_SEL92

#define XBARA_SEL46_SEL92 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL46_SEL92_SHIFT)) & XBARA_SEL46_SEL92_MASK)

Definition at line 47063 of file MIMXRT1062.h.

## ◆ XBARA_SEL46_SEL92_MASK

#define XBARA_SEL46_SEL92_MASK (0x7FU)

Definition at line 47061 of file MIMXRT1062.h.

## ◆ XBARA_SEL46_SEL92_SHIFT

#define XBARA_SEL46_SEL92_SHIFT (0U)

Definition at line 47062 of file MIMXRT1062.h.

## ◆ XBARA_SEL46_SEL93

#define XBARA_SEL46_SEL93 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL46_SEL93_SHIFT)) & XBARA_SEL46_SEL93_MASK)

Definition at line 47066 of file MIMXRT1062.h.

## ◆ XBARA_SEL46_SEL93_MASK

#define XBARA_SEL46_SEL93_MASK (0x7F00U)

Definition at line 47064 of file MIMXRT1062.h.

## ◆ XBARA_SEL46_SEL93_SHIFT

#define XBARA_SEL46_SEL93_SHIFT (8U)

Definition at line 47065 of file MIMXRT1062.h.

## ◆ XBARA_SEL47_SEL94

#define XBARA_SEL47_SEL94 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL47_SEL94_SHIFT)) & XBARA_SEL47_SEL94_MASK)

Definition at line 47073 of file MIMXRT1062.h.

## ◆ XBARA_SEL47_SEL94_MASK

#define XBARA_SEL47_SEL94_MASK (0x7FU)

Definition at line 47071 of file MIMXRT1062.h.

## ◆ XBARA_SEL47_SEL94_SHIFT

#define XBARA_SEL47_SEL94_SHIFT (0U)

Definition at line 47072 of file MIMXRT1062.h.

## ◆ XBARA_SEL47_SEL95

#define XBARA_SEL47_SEL95 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL47_SEL95_SHIFT)) & XBARA_SEL47_SEL95_MASK)

Definition at line 47076 of file MIMXRT1062.h.

## ◆ XBARA_SEL47_SEL95_MASK

#define XBARA_SEL47_SEL95_MASK (0x7F00U)

Definition at line 47074 of file MIMXRT1062.h.

## ◆ XBARA_SEL47_SEL95_SHIFT

#define XBARA_SEL47_SEL95_SHIFT (8U)

Definition at line 47075 of file MIMXRT1062.h.

## ◆ XBARA_SEL48_SEL96

#define XBARA_SEL48_SEL96 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL48_SEL96_SHIFT)) & XBARA_SEL48_SEL96_MASK)

Definition at line 47083 of file MIMXRT1062.h.

## ◆ XBARA_SEL48_SEL96_MASK

#define XBARA_SEL48_SEL96_MASK (0x7FU)

Definition at line 47081 of file MIMXRT1062.h.

## ◆ XBARA_SEL48_SEL96_SHIFT

#define XBARA_SEL48_SEL96_SHIFT (0U)

Definition at line 47082 of file MIMXRT1062.h.

## ◆ XBARA_SEL48_SEL97

#define XBARA_SEL48_SEL97 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL48_SEL97_SHIFT)) & XBARA_SEL48_SEL97_MASK)

Definition at line 47086 of file MIMXRT1062.h.

## ◆ XBARA_SEL48_SEL97_MASK

#define XBARA_SEL48_SEL97_MASK (0x7F00U)

Definition at line 47084 of file MIMXRT1062.h.

## ◆ XBARA_SEL48_SEL97_SHIFT

#define XBARA_SEL48_SEL97_SHIFT (8U)

Definition at line 47085 of file MIMXRT1062.h.

## ◆ XBARA_SEL49_SEL98

#define XBARA_SEL49_SEL98 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL49_SEL98_SHIFT)) & XBARA_SEL49_SEL98_MASK)

Definition at line 47093 of file MIMXRT1062.h.

## ◆ XBARA_SEL49_SEL98_MASK

#define XBARA_SEL49_SEL98_MASK (0x7FU)

Definition at line 47091 of file MIMXRT1062.h.

## ◆ XBARA_SEL49_SEL98_SHIFT

#define XBARA_SEL49_SEL98_SHIFT (0U)

Definition at line 47092 of file MIMXRT1062.h.

## ◆ XBARA_SEL49_SEL99

#define XBARA_SEL49_SEL99 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL49_SEL99_SHIFT)) & XBARA_SEL49_SEL99_MASK)

Definition at line 47096 of file MIMXRT1062.h.

## ◆ XBARA_SEL49_SEL99_MASK

#define XBARA_SEL49_SEL99_MASK (0x7F00U)

Definition at line 47094 of file MIMXRT1062.h.

## ◆ XBARA_SEL49_SEL99_SHIFT

#define XBARA_SEL49_SEL99_SHIFT (8U)

Definition at line 47095 of file MIMXRT1062.h.

## ◆ XBARA_SEL4_SEL8

#define XBARA_SEL4_SEL8 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL4_SEL8_SHIFT)) & XBARA_SEL4_SEL8_MASK)

Definition at line 46643 of file MIMXRT1062.h.

## ◆ XBARA_SEL4_SEL8_MASK

#define XBARA_SEL4_SEL8_MASK (0x7FU)

Definition at line 46641 of file MIMXRT1062.h.

## ◆ XBARA_SEL4_SEL8_SHIFT

#define XBARA_SEL4_SEL8_SHIFT (0U)

Definition at line 46642 of file MIMXRT1062.h.

## ◆ XBARA_SEL4_SEL9

#define XBARA_SEL4_SEL9 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL4_SEL9_SHIFT)) & XBARA_SEL4_SEL9_MASK)

Definition at line 46646 of file MIMXRT1062.h.

## ◆ XBARA_SEL4_SEL9_MASK

#define XBARA_SEL4_SEL9_MASK (0x7F00U)

Definition at line 46644 of file MIMXRT1062.h.

## ◆ XBARA_SEL4_SEL9_SHIFT

#define XBARA_SEL4_SEL9_SHIFT (8U)

Definition at line 46645 of file MIMXRT1062.h.

## ◆ XBARA_SEL50_SEL100

#define XBARA_SEL50_SEL100 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL50_SEL100_SHIFT)) & XBARA_SEL50_SEL100_MASK)

Definition at line 47103 of file MIMXRT1062.h.

## ◆ XBARA_SEL50_SEL100_MASK

#define XBARA_SEL50_SEL100_MASK (0x7FU)

Definition at line 47101 of file MIMXRT1062.h.

## ◆ XBARA_SEL50_SEL100_SHIFT

#define XBARA_SEL50_SEL100_SHIFT (0U)

Definition at line 47102 of file MIMXRT1062.h.

## ◆ XBARA_SEL50_SEL101

#define XBARA_SEL50_SEL101 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL50_SEL101_SHIFT)) & XBARA_SEL50_SEL101_MASK)

Definition at line 47106 of file MIMXRT1062.h.

## ◆ XBARA_SEL50_SEL101_MASK

#define XBARA_SEL50_SEL101_MASK (0x7F00U)

Definition at line 47104 of file MIMXRT1062.h.

## ◆ XBARA_SEL50_SEL101_SHIFT

#define XBARA_SEL50_SEL101_SHIFT (8U)

Definition at line 47105 of file MIMXRT1062.h.

## ◆ XBARA_SEL51_SEL102

#define XBARA_SEL51_SEL102 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL51_SEL102_SHIFT)) & XBARA_SEL51_SEL102_MASK)

Definition at line 47113 of file MIMXRT1062.h.

## ◆ XBARA_SEL51_SEL102_MASK

#define XBARA_SEL51_SEL102_MASK (0x7FU)

Definition at line 47111 of file MIMXRT1062.h.

## ◆ XBARA_SEL51_SEL102_SHIFT

#define XBARA_SEL51_SEL102_SHIFT (0U)

Definition at line 47112 of file MIMXRT1062.h.

## ◆ XBARA_SEL51_SEL103

#define XBARA_SEL51_SEL103 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL51_SEL103_SHIFT)) & XBARA_SEL51_SEL103_MASK)

Definition at line 47116 of file MIMXRT1062.h.

## ◆ XBARA_SEL51_SEL103_MASK

#define XBARA_SEL51_SEL103_MASK (0x7F00U)

Definition at line 47114 of file MIMXRT1062.h.

## ◆ XBARA_SEL51_SEL103_SHIFT

#define XBARA_SEL51_SEL103_SHIFT (8U)

Definition at line 47115 of file MIMXRT1062.h.

## ◆ XBARA_SEL52_SEL104

#define XBARA_SEL52_SEL104 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL52_SEL104_SHIFT)) & XBARA_SEL52_SEL104_MASK)

Definition at line 47123 of file MIMXRT1062.h.

## ◆ XBARA_SEL52_SEL104_MASK

#define XBARA_SEL52_SEL104_MASK (0x7FU)

Definition at line 47121 of file MIMXRT1062.h.

## ◆ XBARA_SEL52_SEL104_SHIFT

#define XBARA_SEL52_SEL104_SHIFT (0U)

Definition at line 47122 of file MIMXRT1062.h.

## ◆ XBARA_SEL52_SEL105

#define XBARA_SEL52_SEL105 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL52_SEL105_SHIFT)) & XBARA_SEL52_SEL105_MASK)

Definition at line 47126 of file MIMXRT1062.h.

## ◆ XBARA_SEL52_SEL105_MASK

#define XBARA_SEL52_SEL105_MASK (0x7F00U)

Definition at line 47124 of file MIMXRT1062.h.

## ◆ XBARA_SEL52_SEL105_SHIFT

#define XBARA_SEL52_SEL105_SHIFT (8U)

Definition at line 47125 of file MIMXRT1062.h.

## ◆ XBARA_SEL53_SEL106

#define XBARA_SEL53_SEL106 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL53_SEL106_SHIFT)) & XBARA_SEL53_SEL106_MASK)

Definition at line 47133 of file MIMXRT1062.h.

## ◆ XBARA_SEL53_SEL106_MASK

#define XBARA_SEL53_SEL106_MASK (0x7FU)

Definition at line 47131 of file MIMXRT1062.h.

## ◆ XBARA_SEL53_SEL106_SHIFT

#define XBARA_SEL53_SEL106_SHIFT (0U)

Definition at line 47132 of file MIMXRT1062.h.

## ◆ XBARA_SEL53_SEL107

#define XBARA_SEL53_SEL107 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL53_SEL107_SHIFT)) & XBARA_SEL53_SEL107_MASK)

Definition at line 47136 of file MIMXRT1062.h.

## ◆ XBARA_SEL53_SEL107_MASK

#define XBARA_SEL53_SEL107_MASK (0x7F00U)

Definition at line 47134 of file MIMXRT1062.h.

## ◆ XBARA_SEL53_SEL107_SHIFT

#define XBARA_SEL53_SEL107_SHIFT (8U)

Definition at line 47135 of file MIMXRT1062.h.

## ◆ XBARA_SEL54_SEL108

#define XBARA_SEL54_SEL108 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL54_SEL108_SHIFT)) & XBARA_SEL54_SEL108_MASK)

Definition at line 47143 of file MIMXRT1062.h.

## ◆ XBARA_SEL54_SEL108_MASK

#define XBARA_SEL54_SEL108_MASK (0x7FU)

Definition at line 47141 of file MIMXRT1062.h.

## ◆ XBARA_SEL54_SEL108_SHIFT

#define XBARA_SEL54_SEL108_SHIFT (0U)

Definition at line 47142 of file MIMXRT1062.h.

## ◆ XBARA_SEL54_SEL109

#define XBARA_SEL54_SEL109 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL54_SEL109_SHIFT)) & XBARA_SEL54_SEL109_MASK)

Definition at line 47146 of file MIMXRT1062.h.

## ◆ XBARA_SEL54_SEL109_MASK

#define XBARA_SEL54_SEL109_MASK (0x7F00U)

Definition at line 47144 of file MIMXRT1062.h.

## ◆ XBARA_SEL54_SEL109_SHIFT

#define XBARA_SEL54_SEL109_SHIFT (8U)

Definition at line 47145 of file MIMXRT1062.h.

## ◆ XBARA_SEL55_SEL110

#define XBARA_SEL55_SEL110 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL55_SEL110_SHIFT)) & XBARA_SEL55_SEL110_MASK)

Definition at line 47153 of file MIMXRT1062.h.

## ◆ XBARA_SEL55_SEL110_MASK

#define XBARA_SEL55_SEL110_MASK (0x7FU)

Definition at line 47151 of file MIMXRT1062.h.

## ◆ XBARA_SEL55_SEL110_SHIFT

#define XBARA_SEL55_SEL110_SHIFT (0U)

Definition at line 47152 of file MIMXRT1062.h.

## ◆ XBARA_SEL55_SEL111

#define XBARA_SEL55_SEL111 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL55_SEL111_SHIFT)) & XBARA_SEL55_SEL111_MASK)

Definition at line 47156 of file MIMXRT1062.h.

## ◆ XBARA_SEL55_SEL111_MASK

#define XBARA_SEL55_SEL111_MASK (0x7F00U)

Definition at line 47154 of file MIMXRT1062.h.

## ◆ XBARA_SEL55_SEL111_SHIFT

#define XBARA_SEL55_SEL111_SHIFT (8U)

Definition at line 47155 of file MIMXRT1062.h.

## ◆ XBARA_SEL56_SEL112

#define XBARA_SEL56_SEL112 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL56_SEL112_SHIFT)) & XBARA_SEL56_SEL112_MASK)

Definition at line 47163 of file MIMXRT1062.h.

## ◆ XBARA_SEL56_SEL112_MASK

#define XBARA_SEL56_SEL112_MASK (0x7FU)

Definition at line 47161 of file MIMXRT1062.h.

## ◆ XBARA_SEL56_SEL112_SHIFT

#define XBARA_SEL56_SEL112_SHIFT (0U)

Definition at line 47162 of file MIMXRT1062.h.

## ◆ XBARA_SEL56_SEL113

#define XBARA_SEL56_SEL113 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL56_SEL113_SHIFT)) & XBARA_SEL56_SEL113_MASK)

Definition at line 47166 of file MIMXRT1062.h.

## ◆ XBARA_SEL56_SEL113_MASK

#define XBARA_SEL56_SEL113_MASK (0x7F00U)

Definition at line 47164 of file MIMXRT1062.h.

## ◆ XBARA_SEL56_SEL113_SHIFT

#define XBARA_SEL56_SEL113_SHIFT (8U)

Definition at line 47165 of file MIMXRT1062.h.

## ◆ XBARA_SEL57_SEL114

#define XBARA_SEL57_SEL114 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL57_SEL114_SHIFT)) & XBARA_SEL57_SEL114_MASK)

Definition at line 47173 of file MIMXRT1062.h.

## ◆ XBARA_SEL57_SEL114_MASK

#define XBARA_SEL57_SEL114_MASK (0x7FU)

Definition at line 47171 of file MIMXRT1062.h.

## ◆ XBARA_SEL57_SEL114_SHIFT

#define XBARA_SEL57_SEL114_SHIFT (0U)

Definition at line 47172 of file MIMXRT1062.h.

## ◆ XBARA_SEL57_SEL115

#define XBARA_SEL57_SEL115 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL57_SEL115_SHIFT)) & XBARA_SEL57_SEL115_MASK)

Definition at line 47176 of file MIMXRT1062.h.

## ◆ XBARA_SEL57_SEL115_MASK

#define XBARA_SEL57_SEL115_MASK (0x7F00U)

Definition at line 47174 of file MIMXRT1062.h.

## ◆ XBARA_SEL57_SEL115_SHIFT

#define XBARA_SEL57_SEL115_SHIFT (8U)

Definition at line 47175 of file MIMXRT1062.h.

## ◆ XBARA_SEL58_SEL116

#define XBARA_SEL58_SEL116 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL58_SEL116_SHIFT)) & XBARA_SEL58_SEL116_MASK)

Definition at line 47183 of file MIMXRT1062.h.

## ◆ XBARA_SEL58_SEL116_MASK

#define XBARA_SEL58_SEL116_MASK (0x7FU)

Definition at line 47181 of file MIMXRT1062.h.

## ◆ XBARA_SEL58_SEL116_SHIFT

#define XBARA_SEL58_SEL116_SHIFT (0U)

Definition at line 47182 of file MIMXRT1062.h.

## ◆ XBARA_SEL58_SEL117

#define XBARA_SEL58_SEL117 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL58_SEL117_SHIFT)) & XBARA_SEL58_SEL117_MASK)

Definition at line 47186 of file MIMXRT1062.h.

## ◆ XBARA_SEL58_SEL117_MASK

#define XBARA_SEL58_SEL117_MASK (0x7F00U)

Definition at line 47184 of file MIMXRT1062.h.

## ◆ XBARA_SEL58_SEL117_SHIFT

#define XBARA_SEL58_SEL117_SHIFT (8U)

Definition at line 47185 of file MIMXRT1062.h.

## ◆ XBARA_SEL59_SEL118

#define XBARA_SEL59_SEL118 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL59_SEL118_SHIFT)) & XBARA_SEL59_SEL118_MASK)

Definition at line 47193 of file MIMXRT1062.h.

## ◆ XBARA_SEL59_SEL118_MASK

#define XBARA_SEL59_SEL118_MASK (0x7FU)

Definition at line 47191 of file MIMXRT1062.h.

## ◆ XBARA_SEL59_SEL118_SHIFT

#define XBARA_SEL59_SEL118_SHIFT (0U)

Definition at line 47192 of file MIMXRT1062.h.

## ◆ XBARA_SEL59_SEL119

#define XBARA_SEL59_SEL119 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL59_SEL119_SHIFT)) & XBARA_SEL59_SEL119_MASK)

Definition at line 47196 of file MIMXRT1062.h.

## ◆ XBARA_SEL59_SEL119_MASK

#define XBARA_SEL59_SEL119_MASK (0x7F00U)

Definition at line 47194 of file MIMXRT1062.h.

## ◆ XBARA_SEL59_SEL119_SHIFT

#define XBARA_SEL59_SEL119_SHIFT (8U)

Definition at line 47195 of file MIMXRT1062.h.

## ◆ XBARA_SEL5_SEL10

#define XBARA_SEL5_SEL10 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL5_SEL10_SHIFT)) & XBARA_SEL5_SEL10_MASK)

Definition at line 46653 of file MIMXRT1062.h.

## ◆ XBARA_SEL5_SEL10_MASK

#define XBARA_SEL5_SEL10_MASK (0x7FU)

Definition at line 46651 of file MIMXRT1062.h.

## ◆ XBARA_SEL5_SEL10_SHIFT

#define XBARA_SEL5_SEL10_SHIFT (0U)

Definition at line 46652 of file MIMXRT1062.h.

## ◆ XBARA_SEL5_SEL11

#define XBARA_SEL5_SEL11 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL5_SEL11_SHIFT)) & XBARA_SEL5_SEL11_MASK)

Definition at line 46656 of file MIMXRT1062.h.

## ◆ XBARA_SEL5_SEL11_MASK

#define XBARA_SEL5_SEL11_MASK (0x7F00U)

Definition at line 46654 of file MIMXRT1062.h.

## ◆ XBARA_SEL5_SEL11_SHIFT

#define XBARA_SEL5_SEL11_SHIFT (8U)

Definition at line 46655 of file MIMXRT1062.h.

## ◆ XBARA_SEL60_SEL120

#define XBARA_SEL60_SEL120 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL60_SEL120_SHIFT)) & XBARA_SEL60_SEL120_MASK)

Definition at line 47203 of file MIMXRT1062.h.

## ◆ XBARA_SEL60_SEL120_MASK

#define XBARA_SEL60_SEL120_MASK (0x7FU)

Definition at line 47201 of file MIMXRT1062.h.

## ◆ XBARA_SEL60_SEL120_SHIFT

#define XBARA_SEL60_SEL120_SHIFT (0U)

Definition at line 47202 of file MIMXRT1062.h.

## ◆ XBARA_SEL60_SEL121

#define XBARA_SEL60_SEL121 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL60_SEL121_SHIFT)) & XBARA_SEL60_SEL121_MASK)

Definition at line 47206 of file MIMXRT1062.h.

## ◆ XBARA_SEL60_SEL121_MASK

#define XBARA_SEL60_SEL121_MASK (0x7F00U)

Definition at line 47204 of file MIMXRT1062.h.

## ◆ XBARA_SEL60_SEL121_SHIFT

#define XBARA_SEL60_SEL121_SHIFT (8U)

Definition at line 47205 of file MIMXRT1062.h.

## ◆ XBARA_SEL61_SEL122

#define XBARA_SEL61_SEL122 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL61_SEL122_SHIFT)) & XBARA_SEL61_SEL122_MASK)

Definition at line 47213 of file MIMXRT1062.h.

## ◆ XBARA_SEL61_SEL122_MASK

#define XBARA_SEL61_SEL122_MASK (0x7FU)

Definition at line 47211 of file MIMXRT1062.h.

## ◆ XBARA_SEL61_SEL122_SHIFT

#define XBARA_SEL61_SEL122_SHIFT (0U)

Definition at line 47212 of file MIMXRT1062.h.

## ◆ XBARA_SEL61_SEL123

#define XBARA_SEL61_SEL123 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL61_SEL123_SHIFT)) & XBARA_SEL61_SEL123_MASK)

Definition at line 47216 of file MIMXRT1062.h.

## ◆ XBARA_SEL61_SEL123_MASK

#define XBARA_SEL61_SEL123_MASK (0x7F00U)

Definition at line 47214 of file MIMXRT1062.h.

## ◆ XBARA_SEL61_SEL123_SHIFT

#define XBARA_SEL61_SEL123_SHIFT (8U)

Definition at line 47215 of file MIMXRT1062.h.

## ◆ XBARA_SEL62_SEL124

#define XBARA_SEL62_SEL124 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL62_SEL124_SHIFT)) & XBARA_SEL62_SEL124_MASK)

Definition at line 47223 of file MIMXRT1062.h.

## ◆ XBARA_SEL62_SEL124_MASK

#define XBARA_SEL62_SEL124_MASK (0x7FU)

Definition at line 47221 of file MIMXRT1062.h.

## ◆ XBARA_SEL62_SEL124_SHIFT

#define XBARA_SEL62_SEL124_SHIFT (0U)

Definition at line 47222 of file MIMXRT1062.h.

## ◆ XBARA_SEL62_SEL125

#define XBARA_SEL62_SEL125 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL62_SEL125_SHIFT)) & XBARA_SEL62_SEL125_MASK)

Definition at line 47226 of file MIMXRT1062.h.

## ◆ XBARA_SEL62_SEL125_MASK

#define XBARA_SEL62_SEL125_MASK (0x7F00U)

Definition at line 47224 of file MIMXRT1062.h.

## ◆ XBARA_SEL62_SEL125_SHIFT

#define XBARA_SEL62_SEL125_SHIFT (8U)

Definition at line 47225 of file MIMXRT1062.h.

## ◆ XBARA_SEL63_SEL126

#define XBARA_SEL63_SEL126 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL63_SEL126_SHIFT)) & XBARA_SEL63_SEL126_MASK)

Definition at line 47233 of file MIMXRT1062.h.

## ◆ XBARA_SEL63_SEL126_MASK

#define XBARA_SEL63_SEL126_MASK (0x7FU)

Definition at line 47231 of file MIMXRT1062.h.

## ◆ XBARA_SEL63_SEL126_SHIFT

#define XBARA_SEL63_SEL126_SHIFT (0U)

Definition at line 47232 of file MIMXRT1062.h.

## ◆ XBARA_SEL63_SEL127

#define XBARA_SEL63_SEL127 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL63_SEL127_SHIFT)) & XBARA_SEL63_SEL127_MASK)

Definition at line 47236 of file MIMXRT1062.h.

## ◆ XBARA_SEL63_SEL127_MASK

#define XBARA_SEL63_SEL127_MASK (0x7F00U)

Definition at line 47234 of file MIMXRT1062.h.

## ◆ XBARA_SEL63_SEL127_SHIFT

#define XBARA_SEL63_SEL127_SHIFT (8U)

Definition at line 47235 of file MIMXRT1062.h.

## ◆ XBARA_SEL64_SEL128

#define XBARA_SEL64_SEL128 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL64_SEL128_SHIFT)) & XBARA_SEL64_SEL128_MASK)

Definition at line 47243 of file MIMXRT1062.h.

## ◆ XBARA_SEL64_SEL128_MASK

#define XBARA_SEL64_SEL128_MASK (0x7FU)

Definition at line 47241 of file MIMXRT1062.h.

## ◆ XBARA_SEL64_SEL128_SHIFT

#define XBARA_SEL64_SEL128_SHIFT (0U)

Definition at line 47242 of file MIMXRT1062.h.

## ◆ XBARA_SEL64_SEL129

#define XBARA_SEL64_SEL129 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL64_SEL129_SHIFT)) & XBARA_SEL64_SEL129_MASK)

Definition at line 47246 of file MIMXRT1062.h.

## ◆ XBARA_SEL64_SEL129_MASK

#define XBARA_SEL64_SEL129_MASK (0x7F00U)

Definition at line 47244 of file MIMXRT1062.h.

## ◆ XBARA_SEL64_SEL129_SHIFT

#define XBARA_SEL64_SEL129_SHIFT (8U)

Definition at line 47245 of file MIMXRT1062.h.

## ◆ XBARA_SEL65_SEL130

#define XBARA_SEL65_SEL130 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL65_SEL130_SHIFT)) & XBARA_SEL65_SEL130_MASK)

Definition at line 47253 of file MIMXRT1062.h.

## ◆ XBARA_SEL65_SEL130_MASK

#define XBARA_SEL65_SEL130_MASK (0x7FU)

Definition at line 47251 of file MIMXRT1062.h.

## ◆ XBARA_SEL65_SEL130_SHIFT

#define XBARA_SEL65_SEL130_SHIFT (0U)

Definition at line 47252 of file MIMXRT1062.h.

## ◆ XBARA_SEL65_SEL131

#define XBARA_SEL65_SEL131 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL65_SEL131_SHIFT)) & XBARA_SEL65_SEL131_MASK)

Definition at line 47256 of file MIMXRT1062.h.

## ◆ XBARA_SEL65_SEL131_MASK

#define XBARA_SEL65_SEL131_MASK (0x7F00U)

Definition at line 47254 of file MIMXRT1062.h.

## ◆ XBARA_SEL65_SEL131_SHIFT

#define XBARA_SEL65_SEL131_SHIFT (8U)

Definition at line 47255 of file MIMXRT1062.h.

## ◆ XBARA_SEL6_SEL12

#define XBARA_SEL6_SEL12 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL6_SEL12_SHIFT)) & XBARA_SEL6_SEL12_MASK)

Definition at line 46663 of file MIMXRT1062.h.

## ◆ XBARA_SEL6_SEL12_MASK

#define XBARA_SEL6_SEL12_MASK (0x7FU)

Definition at line 46661 of file MIMXRT1062.h.

## ◆ XBARA_SEL6_SEL12_SHIFT

#define XBARA_SEL6_SEL12_SHIFT (0U)

Definition at line 46662 of file MIMXRT1062.h.

## ◆ XBARA_SEL6_SEL13

#define XBARA_SEL6_SEL13 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL6_SEL13_SHIFT)) & XBARA_SEL6_SEL13_MASK)

Definition at line 46666 of file MIMXRT1062.h.

## ◆ XBARA_SEL6_SEL13_MASK

#define XBARA_SEL6_SEL13_MASK (0x7F00U)

Definition at line 46664 of file MIMXRT1062.h.

## ◆ XBARA_SEL6_SEL13_SHIFT

#define XBARA_SEL6_SEL13_SHIFT (8U)

Definition at line 46665 of file MIMXRT1062.h.

## ◆ XBARA_SEL7_SEL14

#define XBARA_SEL7_SEL14 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL7_SEL14_SHIFT)) & XBARA_SEL7_SEL14_MASK)

Definition at line 46673 of file MIMXRT1062.h.

## ◆ XBARA_SEL7_SEL14_MASK

#define XBARA_SEL7_SEL14_MASK (0x7FU)

Definition at line 46671 of file MIMXRT1062.h.

## ◆ XBARA_SEL7_SEL14_SHIFT

#define XBARA_SEL7_SEL14_SHIFT (0U)

Definition at line 46672 of file MIMXRT1062.h.

## ◆ XBARA_SEL7_SEL15

#define XBARA_SEL7_SEL15 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL7_SEL15_SHIFT)) & XBARA_SEL7_SEL15_MASK)

Definition at line 46676 of file MIMXRT1062.h.

## ◆ XBARA_SEL7_SEL15_MASK

#define XBARA_SEL7_SEL15_MASK (0x7F00U)

Definition at line 46674 of file MIMXRT1062.h.

## ◆ XBARA_SEL7_SEL15_SHIFT

#define XBARA_SEL7_SEL15_SHIFT (8U)

Definition at line 46675 of file MIMXRT1062.h.

## ◆ XBARA_SEL8_SEL16

#define XBARA_SEL8_SEL16 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL8_SEL16_SHIFT)) & XBARA_SEL8_SEL16_MASK)

Definition at line 46683 of file MIMXRT1062.h.

## ◆ XBARA_SEL8_SEL16_MASK

#define XBARA_SEL8_SEL16_MASK (0x7FU)

Definition at line 46681 of file MIMXRT1062.h.

## ◆ XBARA_SEL8_SEL16_SHIFT

#define XBARA_SEL8_SEL16_SHIFT (0U)

Definition at line 46682 of file MIMXRT1062.h.

## ◆ XBARA_SEL8_SEL17

#define XBARA_SEL8_SEL17 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL8_SEL17_SHIFT)) & XBARA_SEL8_SEL17_MASK)

Definition at line 46686 of file MIMXRT1062.h.

## ◆ XBARA_SEL8_SEL17_MASK

#define XBARA_SEL8_SEL17_MASK (0x7F00U)

Definition at line 46684 of file MIMXRT1062.h.

## ◆ XBARA_SEL8_SEL17_SHIFT

#define XBARA_SEL8_SEL17_SHIFT (8U)

Definition at line 46685 of file MIMXRT1062.h.

## ◆ XBARA_SEL9_SEL18

#define XBARA_SEL9_SEL18 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL9_SEL18_SHIFT)) & XBARA_SEL9_SEL18_MASK)

Definition at line 46693 of file MIMXRT1062.h.

## ◆ XBARA_SEL9_SEL18_MASK

#define XBARA_SEL9_SEL18_MASK (0x7FU)

Definition at line 46691 of file MIMXRT1062.h.

## ◆ XBARA_SEL9_SEL18_SHIFT

#define XBARA_SEL9_SEL18_SHIFT (0U)

Definition at line 46692 of file MIMXRT1062.h.

## ◆ XBARA_SEL9_SEL19

#define XBARA_SEL9_SEL19 | ( |  | x | ) | (((uint16_t)(((uint16_t)(x)) << XBARA_SEL9_SEL19_SHIFT)) & XBARA_SEL9_SEL19_MASK)

Definition at line 46696 of file MIMXRT1062.h.

## ◆ XBARA_SEL9_SEL19_MASK

#define XBARA_SEL9_SEL19_MASK (0x7F00U)

Definition at line 46694 of file MIMXRT1062.h.

## ◆ XBARA_SEL9_SEL19_SHIFT

#define XBARA_SEL9_SEL19_SHIFT (8U)

Definition at line 46695 of file MIMXRT1062.h.