Callisto4Bootloader: FLEXRAM Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
FLEXRAM Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| FLEXRAM Register Masks

## Data Structures

struct | FLEXRAM_Type

## Macros

#define | FLEXRAM_BASE (0x400B0000u)
#define | FLEXRAM ((FLEXRAM_Type *)FLEXRAM_BASE)
#define | FLEXRAM_BASE_ADDRS { FLEXRAM_BASE }
#define | FLEXRAM_BASE_PTRS { FLEXRAM }
#define | FLEXRAM_IRQS { FLEXRAM_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ FLEXRAM

#define FLEXRAM ((FLEXRAM_Type *)FLEXRAM_BASE)

Peripheral FLEXRAM base pointer

Definition at line 19258 of file MIMXRT1062.h.

## ◆ FLEXRAM_BASE

#define FLEXRAM_BASE (0x400B0000u)

Peripheral FLEXRAM base address

Definition at line 19256 of file MIMXRT1062.h.

## ◆ FLEXRAM_BASE_ADDRS

#define FLEXRAM_BASE_ADDRS { FLEXRAM_BASE }

Array initializer of FLEXRAM peripheral base addresses

Definition at line 19260 of file MIMXRT1062.h.

## ◆ FLEXRAM_BASE_PTRS

#define FLEXRAM_BASE_PTRS { FLEXRAM }

Array initializer of FLEXRAM peripheral base pointers

Definition at line 19262 of file MIMXRT1062.h.

## ◆ FLEXRAM_IRQS

#define FLEXRAM_IRQS { FLEXRAM_IRQn }

Interrupt vectors for the FLEXRAM peripheral type

Definition at line 19264 of file MIMXRT1062.h.