Callisto4Bootloader: XTALOSC24M Register Masks

Callisto4Bootloader

XTALOSC24M Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » XTALOSC24M Peripheral Access Layer

## MISC0 - Miscellaneous Register 0

#define | XTALOSC24M_MISC0_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_I_SHIFT)) & XTALOSC24M_MISC0_OSC_I_MASK)
#define | XTALOSC24M_MISC0_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK)

## MISC0_SET - Miscellaneous Register 0

#define | XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_SET_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_SET_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_SET_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_SET_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_SET_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_I_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_I_MASK)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_SET_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_SET_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_SET_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_SET_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK)

## MISC0_CLR - Miscellaneous Register 0

#define | XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_CLR_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_CLR_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_CLR_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_CLR_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_I_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_I_MASK)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_CLR_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_CLR_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK)

## MISC0_TOG - Miscellaneous Register 0

#define | XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK (0x1U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT (0U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK)
#define | XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)
#define | XTALOSC24M_MISC0_TOG_REFTOP_VBGUP(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK)
#define | XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)
#define | XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)
#define | XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK)
#define | XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)
#define | XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)
#define | XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK)
#define | XTALOSC24M_MISC0_TOG_OSC_I_MASK (0x6000U)
#define | XTALOSC24M_MISC0_TOG_OSC_I_SHIFT (13U)
#define | XTALOSC24M_MISC0_TOG_OSC_I(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_I_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_I_MASK)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT (15U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)
#define | XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_CTRL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)
#define | XTALOSC24M_MISC0_TOG_CLKGATE_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK)
#define | XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)
#define | XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)
#define | XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK)
#define | XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)
#define | XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)
#define | XTALOSC24M_MISC0_TOG_XTAL_24M_PWD(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK)
#define | XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK (0x80000000U)
#define | XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT (31U)
#define | XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK)

## LOWPWR_CTRL - XTAL OSC (LP) Control Register

#define | XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_MASK (0x1U)
#define | XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_SHIFT (0U)
#define | XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_OSC_SEL_MASK (0x10U)
#define | XTALOSC24M_LOWPWR_CTRL_OSC_SEL_SHIFT (4U)
#define | XTALOSC24M_LOWPWR_CTRL_OSC_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_OSC_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_MASK (0x20U)
#define | XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_SHIFT (5U)
#define | XTALOSC24M_LOWPWR_CTRL_LPBG_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_MASK (0x40U)
#define | XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_SHIFT (6U)
#define | XTALOSC24M_LOWPWR_CTRL_LPBG_TEST(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_MASK (0x80U)
#define | XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_SHIFT (7U)
#define | XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_MASK (0x100U)
#define | XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_SHIFT (8U)
#define | XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_MASK (0x200U)
#define | XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_SHIFT (9U)
#define | XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_MASK (0x400U)
#define | XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_SHIFT (10U)
#define | XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_MASK (0x800U)
#define | XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_SHIFT (11U)
#define | XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_MASK (0x2000U)
#define | XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_SHIFT (13U)
#define | XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_MASK (0xC000U)
#define | XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_SHIFT (14U)
#define | XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_MASK (0x10000U)
#define | XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_SHIFT (16U)
#define | XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_MASK (0x20000U)
#define | XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_SHIFT (17U)
#define | XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_MASK (0x40000U)
#define | XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_SHIFT (18U)
#define | XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_MASK)

## LOWPWR_CTRL_SET - XTAL OSC (LP) Control Register

#define | XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_MASK (0x1U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_SHIFT (0U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_MASK (0x10U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_SHIFT (4U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_MASK (0x20U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_SHIFT (5U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_MASK (0x40U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_SHIFT (6U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_MASK (0x80U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_SHIFT (7U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_MASK (0x100U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_SHIFT (8U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_MASK (0x200U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_SHIFT (9U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_MASK (0x400U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_SHIFT (10U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_MASK (0x800U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_SHIFT (11U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_MASK (0x2000U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_SHIFT (13U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_MASK (0xC000U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_SHIFT (14U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_MASK (0x10000U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_SHIFT (16U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_MASK (0x20000U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_SHIFT (17U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_MASK (0x40000U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_SHIFT (18U)
#define | XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_MASK)

## LOWPWR_CTRL_CLR - XTAL OSC (LP) Control Register

#define | XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_MASK (0x1U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_SHIFT (0U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_MASK (0x10U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_SHIFT (4U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_MASK (0x20U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_SHIFT (5U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_MASK (0x40U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_SHIFT (6U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_MASK (0x80U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_SHIFT (7U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_MASK (0x100U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_SHIFT (8U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_MASK (0x200U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_SHIFT (9U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_MASK (0x400U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_SHIFT (10U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_MASK (0x800U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_SHIFT (11U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_MASK (0x2000U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_SHIFT (13U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_MASK (0xC000U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_SHIFT (14U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_MASK (0x10000U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_SHIFT (16U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_MASK (0x20000U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_SHIFT (17U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_MASK (0x40000U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_SHIFT (18U)
#define | XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_MASK)

## LOWPWR_CTRL_TOG - XTAL OSC (LP) Control Register

#define | XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_MASK (0x1U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_SHIFT (0U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_MASK (0x10U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_SHIFT (4U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_MASK (0x20U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_SHIFT (5U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_MASK (0x40U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_SHIFT (6U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_MASK (0x80U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_SHIFT (7U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_MASK (0x100U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_SHIFT (8U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_MASK (0x200U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_SHIFT (9U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_MASK (0x400U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_SHIFT (10U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_MASK (0x800U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_SHIFT (11U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_MASK (0x2000U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_SHIFT (13U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_MASK (0xC000U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_SHIFT (14U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_MASK (0x10000U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_SHIFT (16U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_MASK (0x20000U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_SHIFT (17U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_MASK)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_MASK (0x40000U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_SHIFT (18U)
#define | XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_MASK)

## OSC_CONFIG0 - XTAL OSC Configuration 0 Register

#define | XTALOSC24M_OSC_CONFIG0_START_MASK (0x1U)
#define | XTALOSC24M_OSC_CONFIG0_START_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG0_START(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_START_MASK)
#define | XTALOSC24M_OSC_CONFIG0_ENABLE_MASK (0x2U)
#define | XTALOSC24M_OSC_CONFIG0_ENABLE_SHIFT (1U)
#define | XTALOSC24M_OSC_CONFIG0_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_ENABLE_MASK)
#define | XTALOSC24M_OSC_CONFIG0_BYPASS_MASK (0x4U)
#define | XTALOSC24M_OSC_CONFIG0_BYPASS_SHIFT (2U)
#define | XTALOSC24M_OSC_CONFIG0_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_BYPASS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_INVERT_MASK (0x8U)
#define | XTALOSC24M_OSC_CONFIG0_INVERT_SHIFT (3U)
#define | XTALOSC24M_OSC_CONFIG0_INVERT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_INVERT_MASK)
#define | XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_MASK (0xFF0U)
#define | XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_SHIFT (4U)
#define | XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_MASK)
#define | XTALOSC24M_OSC_CONFIG0_HYST_PLUS_MASK (0xF000U)
#define | XTALOSC24M_OSC_CONFIG0_HYST_PLUS_SHIFT (12U)
#define | XTALOSC24M_OSC_CONFIG0_HYST_PLUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_HYST_PLUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_HYST_MINUS_MASK (0xF0000U)
#define | XTALOSC24M_OSC_CONFIG0_HYST_MINUS_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG0_HYST_MINUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_HYST_MINUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_MASK (0xFF000000U)
#define | XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_SHIFT (24U)
#define | XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_MASK)

## OSC_CONFIG0_SET - XTAL OSC Configuration 0 Register

#define | XTALOSC24M_OSC_CONFIG0_SET_START_MASK (0x1U)
#define | XTALOSC24M_OSC_CONFIG0_SET_START_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG0_SET_START(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_START_MASK)
#define | XTALOSC24M_OSC_CONFIG0_SET_ENABLE_MASK (0x2U)
#define | XTALOSC24M_OSC_CONFIG0_SET_ENABLE_SHIFT (1U)
#define | XTALOSC24M_OSC_CONFIG0_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_ENABLE_MASK)
#define | XTALOSC24M_OSC_CONFIG0_SET_BYPASS_MASK (0x4U)
#define | XTALOSC24M_OSC_CONFIG0_SET_BYPASS_SHIFT (2U)
#define | XTALOSC24M_OSC_CONFIG0_SET_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_BYPASS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_SET_INVERT_MASK (0x8U)
#define | XTALOSC24M_OSC_CONFIG0_SET_INVERT_SHIFT (3U)
#define | XTALOSC24M_OSC_CONFIG0_SET_INVERT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_INVERT_MASK)
#define | XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_MASK (0xFF0U)
#define | XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_SHIFT (4U)
#define | XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_MASK)
#define | XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_MASK (0xF000U)
#define | XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_SHIFT (12U)
#define | XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_MASK (0xF0000U)
#define | XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_MASK (0xFF000000U)
#define | XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_SHIFT (24U)
#define | XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_MASK)

## OSC_CONFIG0_CLR - XTAL OSC Configuration 0 Register

#define | XTALOSC24M_OSC_CONFIG0_CLR_START_MASK (0x1U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_START_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_START(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_START_MASK)
#define | XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_MASK (0x2U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_SHIFT (1U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_MASK)
#define | XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_MASK (0x4U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_SHIFT (2U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_CLR_INVERT_MASK (0x8U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_INVERT_SHIFT (3U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_INVERT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_INVERT_MASK)
#define | XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_MASK (0xFF0U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_SHIFT (4U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_MASK)
#define | XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_MASK (0xF000U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_SHIFT (12U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_MASK (0xF0000U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_MASK (0xFF000000U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_SHIFT (24U)
#define | XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_MASK)

## OSC_CONFIG0_TOG - XTAL OSC Configuration 0 Register

#define | XTALOSC24M_OSC_CONFIG0_TOG_START_MASK (0x1U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_START_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_START(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_START_MASK)
#define | XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_MASK (0x2U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_SHIFT (1U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_MASK)
#define | XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_MASK (0x4U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_SHIFT (2U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_TOG_INVERT_MASK (0x8U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_INVERT_SHIFT (3U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_INVERT(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_INVERT_MASK)
#define | XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_MASK (0xFF0U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_SHIFT (4U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_MASK)
#define | XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_MASK (0xF000U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_SHIFT (12U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_MASK (0xF0000U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_MASK)
#define | XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_MASK (0xFF000000U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_SHIFT (24U)
#define | XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_MASK)

## OSC_CONFIG1 - XTAL OSC Configuration 1 Register

#define | XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_MASK (0xFFF00000U)
#define | XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_SHIFT (20U)
#define | XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_MASK)

## OSC_CONFIG1_SET - XTAL OSC Configuration 1 Register

#define | XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_MASK (0xFFF00000U)
#define | XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_SHIFT (20U)
#define | XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_MASK)

## OSC_CONFIG1_CLR - XTAL OSC Configuration 1 Register

#define | XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_MASK (0xFFF00000U)
#define | XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_SHIFT (20U)
#define | XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_MASK)

## OSC_CONFIG1_TOG - XTAL OSC Configuration 1 Register

#define | XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_MASK (0xFFF00000U)
#define | XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_SHIFT (20U)
#define | XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_MASK)

## OSC_CONFIG2 - XTAL OSC Configuration 2 Register

#define | XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG2_ENABLE_1M_MASK (0x10000U)
#define | XTALOSC24M_OSC_CONFIG2_ENABLE_1M_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG2_ENABLE_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_ENABLE_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_MUX_1M_MASK (0x20000U)
#define | XTALOSC24M_OSC_CONFIG2_MUX_1M_SHIFT (17U)
#define | XTALOSC24M_OSC_CONFIG2_MUX_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_MUX_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_MASK (0x80000000U)
#define | XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_SHIFT (31U)
#define | XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_MASK)

## OSC_CONFIG2_SET - XTAL OSC Configuration 2 Register

#define | XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_MASK (0x10000U)
#define | XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_MASK (0x20000U)
#define | XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_SHIFT (17U)
#define | XTALOSC24M_OSC_CONFIG2_SET_MUX_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_MASK (0x80000000U)
#define | XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_SHIFT (31U)
#define | XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_MASK)

## OSC_CONFIG2_CLR - XTAL OSC Configuration 2 Register

#define | XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_MASK (0x10000U)
#define | XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_MASK (0x20000U)
#define | XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_SHIFT (17U)
#define | XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_MASK (0x80000000U)
#define | XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_SHIFT (31U)
#define | XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_MASK)

## OSC_CONFIG2_TOG - XTAL OSC Configuration 2 Register

#define | XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_MASK (0xFFFU)
#define | XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_SHIFT (0U)
#define | XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_MASK)
#define | XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_MASK (0x10000U)
#define | XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_SHIFT (16U)
#define | XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_MASK (0x20000U)
#define | XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_SHIFT (17U)
#define | XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_MASK)
#define | XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_MASK (0x80000000U)
#define | XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_SHIFT (31U)
#define | XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL(x) (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_MASK)

Definition at line 48153 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_MASK (0x400U)

Definition at line 48151 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_CPU_PWRGATE_SHIFT (10U)

Definition at line 48152 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_MASK)

Definition at line 48156 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_MASK (0x800U)

Definition at line 48154 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_DISPLAY_PWRGATE_SHIFT (11U)

Definition at line 48155 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_MASK)

Definition at line 48181 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_MASK (0x40000U)

Definition at line 48179 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_GPU_PWRGATE_SHIFT (18U)

Definition at line 48180 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_MASK)

Definition at line 48147 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_MASK (0x100U)

Definition at line 48145 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_L1_PWRGATE_SHIFT (8U)

Definition at line 48146 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_MASK)

Definition at line 48150 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_MASK (0x200U)

Definition at line 48148 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_L2_PWRGATE_SHIFT (9U)

Definition at line 48149 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL

#define XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_MASK)

LPBG_SEL 0b0..Normal power bandgap 0b1..Low power bandgap

Definition at line 48138 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_MASK (0x20U)

Definition at line 48132 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_SEL_SHIFT (5U)

Definition at line 48133 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST

#define XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_MASK)

Definition at line 48141 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_MASK (0x40U)

Definition at line 48139 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_LPBG_TEST_SHIFT (6U)

Definition at line 48140 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_MASK)

Definition at line 48178 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_MASK (0x20000U)

Definition at line 48176 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_MIX_PWRGATE_SHIFT (17U)

Definition at line 48177 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL

#define XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_MASK)

OSC_SEL 0b0..XTAL OSC 0b1..RC OSC

Definition at line 48131 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_MASK (0x10U)

Definition at line 48125 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_OSC_SEL_SHIFT (4U)

Definition at line 48126 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN

#define XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_MASK)

RC_OSC_EN 0b0..Use XTAL OSC to source the 24MHz clock 0b1..Use RC OSC

Definition at line 48124 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_MASK (0x1U)

Definition at line 48118 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_RC_OSC_EN_SHIFT (0U)

Definition at line 48119 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE

#define XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_MASK)

Definition at line 48159 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_MASK (0x2000U)

Definition at line 48157 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_RCOSC_CG_OVERRIDE_SHIFT (13U)

Definition at line 48158 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF

#define XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_MASK)

Definition at line 48144 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_MASK (0x80U)

Definition at line 48142 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_REFTOP_IBIAS_OFF_SHIFT (7U)

Definition at line 48143 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY

#define XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_MASK)

XTALOSC_PWRUP_DELAY 0b00..0.25ms 0b01..0.5ms 0b10..1ms 0b11..2ms

Definition at line 48168 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_MASK (0xC000U)

Definition at line 48160 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_DELAY_SHIFT (14U)

Definition at line 48161 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT

#define XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_MASK)

XTALOSC_PWRUP_STAT 0b0..Not stable 0b1..Stable and ready to use

Definition at line 48175 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_MASK

#define XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_MASK (0x10000U)

Definition at line 48169 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CLR_XTALOSC_PWRUP_STAT_SHIFT (16U)

Definition at line 48170 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_MASK)

Definition at line 48017 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_MASK (0x400U)

Definition at line 48015 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_CPU_PWRGATE_SHIFT (10U)

Definition at line 48016 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_MASK)

Definition at line 48020 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_MASK (0x800U)

Definition at line 48018 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_DISPLAY_PWRGATE_SHIFT (11U)

Definition at line 48019 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_MASK)

Definition at line 48045 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_MASK (0x40000U)

Definition at line 48043 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_GPU_PWRGATE_SHIFT (18U)

Definition at line 48044 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_MASK)

Definition at line 48011 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_MASK (0x100U)

Definition at line 48009 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_L1_PWRGATE_SHIFT (8U)

Definition at line 48010 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_MASK)

Definition at line 48014 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_MASK (0x200U)

Definition at line 48012 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_L2_PWRGATE_SHIFT (9U)

Definition at line 48013 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_LPBG_SEL

#define XTALOSC24M_LOWPWR_CTRL_LPBG_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_MASK)

LPBG_SEL 0b0..Normal power bandgap 0b1..Low power bandgap

Definition at line 48002 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_MASK (0x20U)

Definition at line 47996 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_LPBG_SEL_SHIFT (5U)

Definition at line 47997 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_LPBG_TEST

#define XTALOSC24M_LOWPWR_CTRL_LPBG_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_MASK)

Definition at line 48005 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_MASK

#define XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_MASK (0x40U)

Definition at line 48003 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_LPBG_TEST_SHIFT (6U)

Definition at line 48004 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_MASK)

Definition at line 48042 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_MASK (0x20000U)

Definition at line 48040 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_MIX_PWRGATE_SHIFT (17U)

Definition at line 48041 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_OSC_SEL

#define XTALOSC24M_LOWPWR_CTRL_OSC_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_OSC_SEL_MASK)

OSC_SEL 0b0..XTAL OSC 0b1..RC OSC

Definition at line 47995 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_OSC_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_OSC_SEL_MASK (0x10U)

Definition at line 47989 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_OSC_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_OSC_SEL_SHIFT (4U)

Definition at line 47990 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN

#define XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_MASK)

RC_OSC_EN 0b0..Use XTAL OSC to source the 24MHz clock 0b1..Use RC OSC

Definition at line 47988 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_MASK

#define XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_MASK (0x1U)

Definition at line 47982 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_RC_OSC_EN_SHIFT (0U)

Definition at line 47983 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE

#define XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_MASK)

Definition at line 48023 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_MASK

#define XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_MASK (0x2000U)

Definition at line 48021 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_RCOSC_CG_OVERRIDE_SHIFT (13U)

Definition at line 48022 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF

#define XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_MASK)

Definition at line 48008 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_MASK

#define XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_MASK (0x80U)

Definition at line 48006 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_REFTOP_IBIAS_OFF_SHIFT (7U)

Definition at line 48007 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_MASK)

Definition at line 48085 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_MASK (0x400U)

Definition at line 48083 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_CPU_PWRGATE_SHIFT (10U)

Definition at line 48084 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_MASK)

Definition at line 48088 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_MASK (0x800U)

Definition at line 48086 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_DISPLAY_PWRGATE_SHIFT (11U)

Definition at line 48087 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_MASK)

Definition at line 48113 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_MASK (0x40000U)

Definition at line 48111 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_GPU_PWRGATE_SHIFT (18U)

Definition at line 48112 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_MASK)

Definition at line 48079 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_MASK (0x100U)

Definition at line 48077 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_L1_PWRGATE_SHIFT (8U)

Definition at line 48078 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_MASK)

Definition at line 48082 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_MASK (0x200U)

Definition at line 48080 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_L2_PWRGATE_SHIFT (9U)

Definition at line 48081 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL

#define XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_MASK)

LPBG_SEL 0b0..Normal power bandgap 0b1..Low power bandgap

Definition at line 48070 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_MASK (0x20U)

Definition at line 48064 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_LPBG_SEL_SHIFT (5U)

Definition at line 48065 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST

#define XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_MASK)

Definition at line 48073 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_MASK (0x40U)

Definition at line 48071 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_LPBG_TEST_SHIFT (6U)

Definition at line 48072 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_MASK)

Definition at line 48110 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_MASK (0x20000U)

Definition at line 48108 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_MIX_PWRGATE_SHIFT (17U)

Definition at line 48109 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL

#define XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_MASK)

OSC_SEL 0b0..XTAL OSC 0b1..RC OSC

Definition at line 48063 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_MASK (0x10U)

Definition at line 48057 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_OSC_SEL_SHIFT (4U)

Definition at line 48058 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN

#define XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_MASK)

RC_OSC_EN 0b0..Use XTAL OSC to source the 24MHz clock 0b1..Use RC OSC

Definition at line 48056 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_MASK (0x1U)

Definition at line 48050 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_RC_OSC_EN_SHIFT (0U)

Definition at line 48051 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE

#define XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_MASK)

Definition at line 48091 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_MASK (0x2000U)

Definition at line 48089 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_RCOSC_CG_OVERRIDE_SHIFT (13U)

Definition at line 48090 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF

#define XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_MASK)

Definition at line 48076 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_MASK (0x80U)

Definition at line 48074 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_REFTOP_IBIAS_OFF_SHIFT (7U)

Definition at line 48075 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY

#define XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_MASK)

XTALOSC_PWRUP_DELAY 0b00..0.25ms 0b01..0.5ms 0b10..1ms 0b11..2ms

Definition at line 48100 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_MASK (0xC000U)

Definition at line 48092 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_DELAY_SHIFT (14U)

Definition at line 48093 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT

#define XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_MASK)

XTALOSC_PWRUP_STAT 0b0..Not stable 0b1..Stable and ready to use

Definition at line 48107 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_MASK

#define XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_MASK (0x10000U)

Definition at line 48101 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_SET_XTALOSC_PWRUP_STAT_SHIFT (16U)

Definition at line 48102 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_MASK)

Definition at line 48221 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_MASK (0x400U)

Definition at line 48219 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_CPU_PWRGATE_SHIFT (10U)

Definition at line 48220 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_MASK)

Definition at line 48224 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_MASK (0x800U)

Definition at line 48222 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_DISPLAY_PWRGATE_SHIFT (11U)

Definition at line 48223 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_MASK)

Definition at line 48249 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_MASK (0x40000U)

Definition at line 48247 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_GPU_PWRGATE_SHIFT (18U)

Definition at line 48248 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_MASK)

Definition at line 48215 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_MASK (0x100U)

Definition at line 48213 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_L1_PWRGATE_SHIFT (8U)

Definition at line 48214 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_MASK)

Definition at line 48218 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_MASK (0x200U)

Definition at line 48216 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_L2_PWRGATE_SHIFT (9U)

Definition at line 48217 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL

#define XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_MASK)

LPBG_SEL 0b0..Normal power bandgap 0b1..Low power bandgap

Definition at line 48206 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_MASK (0x20U)

Definition at line 48200 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_SEL_SHIFT (5U)

Definition at line 48201 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST

#define XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_MASK)

Definition at line 48209 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_MASK (0x40U)

Definition at line 48207 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_LPBG_TEST_SHIFT (6U)

Definition at line 48208 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE

#define XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_MASK)

Definition at line 48246 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_MASK (0x20000U)

Definition at line 48244 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_MIX_PWRGATE_SHIFT (17U)

Definition at line 48245 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL

#define XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_MASK)

OSC_SEL 0b0..XTAL OSC 0b1..RC OSC

Definition at line 48199 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_MASK (0x10U)

Definition at line 48193 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_OSC_SEL_SHIFT (4U)

Definition at line 48194 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN

#define XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_MASK)

RC_OSC_EN 0b0..Use XTAL OSC to source the 24MHz clock 0b1..Use RC OSC

Definition at line 48192 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_MASK (0x1U)

Definition at line 48186 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_RC_OSC_EN_SHIFT (0U)

Definition at line 48187 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE

#define XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_MASK)

Definition at line 48227 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_MASK (0x2000U)

Definition at line 48225 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_RCOSC_CG_OVERRIDE_SHIFT (13U)

Definition at line 48226 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF

#define XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_MASK)

Definition at line 48212 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_MASK (0x80U)

Definition at line 48210 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_REFTOP_IBIAS_OFF_SHIFT (7U)

Definition at line 48211 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY

#define XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_MASK)

XTALOSC_PWRUP_DELAY 0b00..0.25ms 0b01..0.5ms 0b10..1ms 0b11..2ms

Definition at line 48236 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_MASK (0xC000U)

Definition at line 48228 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_DELAY_SHIFT (14U)

Definition at line 48229 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT

#define XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_MASK)

XTALOSC_PWRUP_STAT 0b0..Not stable 0b1..Stable and ready to use

Definition at line 48243 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_MASK

#define XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_MASK (0x10000U)

Definition at line 48237 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_TOG_XTALOSC_PWRUP_STAT_SHIFT (16U)

Definition at line 48238 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY

#define XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_MASK)

XTALOSC_PWRUP_DELAY 0b00..0.25ms 0b01..0.5ms 0b10..1ms 0b11..2ms

Definition at line 48032 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_MASK

#define XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_MASK (0xC000U)

Definition at line 48024 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_DELAY_SHIFT (14U)

Definition at line 48025 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT

#define XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_SHIFT)) & XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_MASK)

XTALOSC_PWRUP_STAT 0b0..Not stable 0b1..Stable and ready to use

Definition at line 48039 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_MASK

#define XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_MASK (0x10000U)

Definition at line 48033 of file MIMXRT1062.h.

## ◆ XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_SHIFT

#define XTALOSC24M_LOWPWR_CTRL_XTALOSC_PWRUP_STAT_SHIFT (16U)

Definition at line 48034 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_CTRL

#define XTALOSC24M_MISC0_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47653 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47647 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47648 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_DELAY

#define XTALOSC24M_MISC0_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47666 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47654 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47655 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_CTRL

#define XTALOSC24M_MISC0_CLR_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47849 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47843 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_CLR_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47844 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_DELAY

#define XTALOSC24M_MISC0_CLR_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47862 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47850 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_CLR_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47851 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47827 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47821 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_CLR_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47822 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_I

#define XTALOSC24M_MISC0_CLR_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_I_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47836 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_I_MASK

#define XTALOSC24M_MISC0_CLR_OSC_I_MASK (0x6000U)

Definition at line 47828 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_I_SHIFT

#define XTALOSC24M_MISC0_CLR_OSC_I_SHIFT (13U)

Definition at line 47829 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK)

Definition at line 47839 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK)

Definition at line 47842 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47840 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47841 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_MASK (0x8000U)

Definition at line 47837 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_CLR_OSC_XTALOK_SHIFT (15U)

Definition at line 47838 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_PWD

#define XTALOSC24M_MISC0_CLR_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK)

Definition at line 47788 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_PWD_MASK (0x1U)

Definition at line 47786 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_PWD_SHIFT (0U)

Definition at line 47787 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47795 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47789 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47790 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47808 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47796 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47797 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGUP

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK)

Definition at line 47811 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47809 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_CLR_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47810 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47869 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47863 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_CLR_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47864 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47820 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47812 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_CLR_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47813 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47879 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47873 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_CLR_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47874 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_XTAL_24M_PWD

#define XTALOSC24M_MISC0_CLR_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK)

Definition at line 47872 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47870 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_CLR_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47871 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47631 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47625 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47626 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_I

#define XTALOSC24M_MISC0_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_I_SHIFT)) & XTALOSC24M_MISC0_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47640 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_I_MASK

#define XTALOSC24M_MISC0_OSC_I_MASK (0x6000U)

Definition at line 47632 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_I_SHIFT

#define XTALOSC24M_MISC0_OSC_I_SHIFT (13U)

Definition at line 47633 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK

#define XTALOSC24M_MISC0_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_MASK)

Definition at line 47643 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK)

Definition at line 47646 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47644 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47645 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_OSC_XTALOK_MASK (0x8000U)

Definition at line 47641 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_OSC_XTALOK_SHIFT (15U)

Definition at line 47642 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_PWD

#define XTALOSC24M_MISC0_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_REFTOP_PWD_MASK)

Definition at line 47592 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_REFTOP_PWD_MASK (0x1U)

Definition at line 47590 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_REFTOP_PWD_SHIFT (0U)

Definition at line 47591 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47599 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47593 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47594 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47612 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47600 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47601 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGUP

#define XTALOSC24M_MISC0_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_REFTOP_VBGUP_MASK)

Definition at line 47615 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47613 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47614 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47673 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47667 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47668 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_CTRL

#define XTALOSC24M_MISC0_SET_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47751 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_SET_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47745 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_SET_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47746 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_DELAY

#define XTALOSC24M_MISC0_SET_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47764 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_SET_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47752 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_SET_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47753 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47729 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47723 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_SET_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47724 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_I

#define XTALOSC24M_MISC0_SET_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_I_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47738 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_I_MASK

#define XTALOSC24M_MISC0_SET_OSC_I_MASK (0x6000U)

Definition at line 47730 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_I_SHIFT

#define XTALOSC24M_MISC0_SET_OSC_I_SHIFT (13U)

Definition at line 47731 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK

#define XTALOSC24M_MISC0_SET_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK)

Definition at line 47741 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK)

Definition at line 47744 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47742 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47743 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_MASK (0x8000U)

Definition at line 47739 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_SET_OSC_XTALOK_SHIFT (15U)

Definition at line 47740 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_PWD

#define XTALOSC24M_MISC0_SET_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK)

Definition at line 47690 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_PWD_MASK (0x1U)

Definition at line 47688 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_PWD_SHIFT (0U)

Definition at line 47689 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47697 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47691 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47692 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_SET_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47710 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47698 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47699 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGUP

#define XTALOSC24M_MISC0_SET_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK)

Definition at line 47713 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_SET_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47711 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_SET_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47712 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47771 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47765 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_SET_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47766 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47722 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47714 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_SET_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47715 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_SET_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47781 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47775 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_SET_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47776 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_XTAL_24M_PWD

#define XTALOSC24M_MISC0_SET_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK)

Definition at line 47774 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_SET_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47772 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_SET_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47773 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47624 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47616 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47617 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_CTRL

#define XTALOSC24M_MISC0_TOG_CLKGATE_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK)

CLKGATE_CTRL 0b0..Allow the logic to automatically gate the clock when the XTAL is powered down. 0b1..Prevent the logic from ever gating off the clock.

Definition at line 47947 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK

#define XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_MASK (0x2000000U)

Definition at line 47941 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT

#define XTALOSC24M_MISC0_TOG_CLKGATE_CTRL_SHIFT (25U)

Definition at line 47942 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_DELAY

#define XTALOSC24M_MISC0_TOG_CLKGATE_DELAY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT)) & XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK)

CLKGATE_DELAY 0b000..0.5ms 0b001..1.0ms 0b010..2.0ms 0b011..3.0ms 0b100..4.0ms 0b101..5.0ms 0b110..6.0ms 0b111..7.0ms

Definition at line 47960 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK

#define XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_MASK (0x1C000000U)

Definition at line 47948 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT

#define XTALOSC24M_MISC0_TOG_CLKGATE_DELAY_SHIFT (26U)

Definition at line 47949 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS

#define XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT)) & XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK)

DISCON_HIGH_SNVS 0b0..Turn on the switch 0b1..Turn off the switch

Definition at line 47925 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK

#define XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_MASK (0x1000U)

Definition at line 47919 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT

#define XTALOSC24M_MISC0_TOG_DISCON_HIGH_SNVS_SHIFT (12U)

Definition at line 47920 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_I

#define XTALOSC24M_MISC0_TOG_OSC_I | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_I_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_I_MASK)

OSC_I 0b00..Nominal 0b01..Decrease current by 12.5% 0b10..Decrease current by 25.0% 0b11..Decrease current by 37.5%

Definition at line 47934 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_I_MASK

#define XTALOSC24M_MISC0_TOG_OSC_I_MASK (0x6000U)

Definition at line 47926 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_I_SHIFT

#define XTALOSC24M_MISC0_TOG_OSC_I_SHIFT (13U)

Definition at line 47927 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK)

Definition at line 47937 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT)) & XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK)

Definition at line 47940 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_MASK (0x10000U)

Definition at line 47938 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_EN_SHIFT (16U)

Definition at line 47939 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_MASK (0x8000U)

Definition at line 47935 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT

#define XTALOSC24M_MISC0_TOG_OSC_XTALOK_SHIFT (15U)

Definition at line 47936 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_PWD

#define XTALOSC24M_MISC0_TOG_REFTOP_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK)

Definition at line 47886 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_PWD_MASK (0x1U)

Definition at line 47884 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_PWD_SHIFT (0U)

Definition at line 47885 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF

#define XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK)

REFTOP_SELFBIASOFF 0b0..Uses coarse bias currents for startup 0b1..Uses bandgap-based bias currents for best performance.

Definition at line 47893 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_MASK (0x8U)

Definition at line 47887 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_SELFBIASOFF_SHIFT (3U)

Definition at line 47888 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK)

REFTOP_VBGADJ 0b000..Nominal VBG 0b001..VBG+0.78% 0b010..VBG+1.56% 0b011..VBG+2.34% 0b100..VBG-0.78% 0b101..VBG-1.56% 0b110..VBG-2.34% 0b111..VBG-3.12%

Definition at line 47906 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_MASK (0x70U)

Definition at line 47894 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGADJ_SHIFT (4U)

Definition at line 47895 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGUP

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGUP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT)) & XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK)

Definition at line 47909 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_MASK (0x80U)

Definition at line 47907 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT

#define XTALOSC24M_MISC0_TOG_REFTOP_VBGUP_SHIFT (7U)

Definition at line 47908 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE

#define XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT)) & XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK)

RTC_XTAL_SOURCE 0b0..Internal ring oscillator 0b1..RTC_XTAL

Definition at line 47967 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK

#define XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_MASK (0x20000000U)

Definition at line 47961 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT

#define XTALOSC24M_MISC0_TOG_RTC_XTAL_SOURCE_SHIFT (29U)

Definition at line 47962 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG

#define XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT)) & XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK)

STOP_MODE_CONFIG 0b00..All analog except rtc powered down on stop mode assertion. XtalOsc=on, RCOsc=off; 0b01..Certain analog functions such as certain regulators left up. XtalOsc=on, RCOsc=off; 0b10..XtalOsc=off, RCOsc=on, Old BG=on, New BG=off. 0b11..XtalOsc=off, RCOsc=on, Old BG=off, New BG=on.

Definition at line 47918 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK

#define XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_MASK (0xC00U)

Definition at line 47910 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT

#define XTALOSC24M_MISC0_TOG_STOP_MODE_CONFIG_SHIFT (10U)

Definition at line 47911 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47977 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47971 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_TOG_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47972 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_XTAL_24M_PWD

#define XTALOSC24M_MISC0_TOG_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK)

Definition at line 47970 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47968 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_TOG_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47969 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_VID_PLL_PREDIV

#define XTALOSC24M_MISC0_VID_PLL_PREDIV | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT)) & XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK)

VID_PLL_PREDIV 0b0..Divide by 1 0b1..Divide by 2

Definition at line 47683 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK

#define XTALOSC24M_MISC0_VID_PLL_PREDIV_MASK (0x80000000U)

Definition at line 47677 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT

#define XTALOSC24M_MISC0_VID_PLL_PREDIV_SHIFT (31U)

Definition at line 47678 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_XTAL_24M_PWD

#define XTALOSC24M_MISC0_XTAL_24M_PWD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT)) & XTALOSC24M_MISC0_XTAL_24M_PWD_MASK)

Definition at line 47676 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_XTAL_24M_PWD_MASK

#define XTALOSC24M_MISC0_XTAL_24M_PWD_MASK (0x40000000U)

Definition at line 47674 of file MIMXRT1062.h.

## ◆ XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT

#define XTALOSC24M_MISC0_XTAL_24M_PWD_SHIFT (30U)

Definition at line 47675 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_BYPASS

#define XTALOSC24M_OSC_CONFIG0_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_BYPASS_MASK)

Definition at line 48262 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_BYPASS_MASK

#define XTALOSC24M_OSC_CONFIG0_BYPASS_MASK (0x4U)

Definition at line 48260 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_BYPASS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_BYPASS_SHIFT (2U)

Definition at line 48261 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_BYPASS

#define XTALOSC24M_OSC_CONFIG0_CLR_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_MASK)

Definition at line 48318 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_MASK (0x4U)

Definition at line 48316 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_BYPASS_SHIFT (2U)

Definition at line 48317 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_ENABLE

#define XTALOSC24M_OSC_CONFIG0_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_MASK)

Definition at line 48315 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_MASK (0x2U)

Definition at line 48313 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_ENABLE_SHIFT (1U)

Definition at line 48314 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS

#define XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_MASK)

Definition at line 48330 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_MASK (0xF0000U)

Definition at line 48328 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_HYST_MINUS_SHIFT (16U)

Definition at line 48329 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS

#define XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_MASK)

Definition at line 48327 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_MASK (0xF000U)

Definition at line 48325 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_HYST_PLUS_SHIFT (12U)

Definition at line 48326 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_INVERT

#define XTALOSC24M_OSC_CONFIG0_CLR_INVERT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_INVERT_MASK)

Definition at line 48321 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_INVERT_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_INVERT_MASK (0x8U)

Definition at line 48319 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_INVERT_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_INVERT_SHIFT (3U)

Definition at line 48320 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG

#define XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_MASK)

Definition at line 48324 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR

#define XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_MASK)

Definition at line 48333 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_MASK (0xFF000000U)

Definition at line 48331 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_CUR_SHIFT (24U)

Definition at line 48332 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_MASK (0xFF0U)

Definition at line 48322 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_RC_OSC_PROG_SHIFT (4U)

Definition at line 48323 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_START

#define XTALOSC24M_OSC_CONFIG0_CLR_START | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_CLR_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_CLR_START_MASK)

Definition at line 48312 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_START_MASK

#define XTALOSC24M_OSC_CONFIG0_CLR_START_MASK (0x1U)

Definition at line 48310 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_CLR_START_SHIFT

#define XTALOSC24M_OSC_CONFIG0_CLR_START_SHIFT (0U)

Definition at line 48311 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_ENABLE

#define XTALOSC24M_OSC_CONFIG0_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_ENABLE_MASK)

Definition at line 48259 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_ENABLE_MASK

#define XTALOSC24M_OSC_CONFIG0_ENABLE_MASK (0x2U)

Definition at line 48257 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_ENABLE_SHIFT

#define XTALOSC24M_OSC_CONFIG0_ENABLE_SHIFT (1U)

Definition at line 48258 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_HYST_MINUS

#define XTALOSC24M_OSC_CONFIG0_HYST_MINUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_HYST_MINUS_MASK)

Definition at line 48274 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_HYST_MINUS_MASK

#define XTALOSC24M_OSC_CONFIG0_HYST_MINUS_MASK (0xF0000U)

Definition at line 48272 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_HYST_MINUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_HYST_MINUS_SHIFT (16U)

Definition at line 48273 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_HYST_PLUS

#define XTALOSC24M_OSC_CONFIG0_HYST_PLUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_HYST_PLUS_MASK)

Definition at line 48271 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_HYST_PLUS_MASK

#define XTALOSC24M_OSC_CONFIG0_HYST_PLUS_MASK (0xF000U)

Definition at line 48269 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_HYST_PLUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_HYST_PLUS_SHIFT (12U)

Definition at line 48270 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_INVERT

#define XTALOSC24M_OSC_CONFIG0_INVERT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_INVERT_MASK)

Definition at line 48265 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_INVERT_MASK

#define XTALOSC24M_OSC_CONFIG0_INVERT_MASK (0x8U)

Definition at line 48263 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_INVERT_SHIFT

#define XTALOSC24M_OSC_CONFIG0_INVERT_SHIFT (3U)

Definition at line 48264 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG

#define XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_MASK)

Definition at line 48268 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR

#define XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_MASK)

Definition at line 48277 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_MASK

#define XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_MASK (0xFF000000U)

Definition at line 48275 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_CUR_SHIFT (24U)

Definition at line 48276 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_MASK

#define XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_MASK (0xFF0U)

Definition at line 48266 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_SHIFT

#define XTALOSC24M_OSC_CONFIG0_RC_OSC_PROG_SHIFT (4U)

Definition at line 48267 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_BYPASS

#define XTALOSC24M_OSC_CONFIG0_SET_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_BYPASS_MASK)

Definition at line 48290 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_BYPASS_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_BYPASS_MASK (0x4U)

Definition at line 48288 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_BYPASS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_BYPASS_SHIFT (2U)

Definition at line 48289 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_ENABLE

#define XTALOSC24M_OSC_CONFIG0_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_ENABLE_MASK)

Definition at line 48287 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_ENABLE_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_ENABLE_MASK (0x2U)

Definition at line 48285 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_ENABLE_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_ENABLE_SHIFT (1U)

Definition at line 48286 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS

#define XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_MASK)

Definition at line 48302 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_MASK (0xF0000U)

Definition at line 48300 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_HYST_MINUS_SHIFT (16U)

Definition at line 48301 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS

#define XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_MASK)

Definition at line 48299 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_MASK (0xF000U)

Definition at line 48297 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_HYST_PLUS_SHIFT (12U)

Definition at line 48298 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_INVERT

#define XTALOSC24M_OSC_CONFIG0_SET_INVERT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_INVERT_MASK)

Definition at line 48293 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_INVERT_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_INVERT_MASK (0x8U)

Definition at line 48291 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_INVERT_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_INVERT_SHIFT (3U)

Definition at line 48292 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG

#define XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_MASK)

Definition at line 48296 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR

#define XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_MASK)

Definition at line 48305 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_MASK (0xFF000000U)

Definition at line 48303 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_CUR_SHIFT (24U)

Definition at line 48304 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_MASK (0xFF0U)

Definition at line 48294 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_RC_OSC_PROG_SHIFT (4U)

Definition at line 48295 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_START

#define XTALOSC24M_OSC_CONFIG0_SET_START | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_SET_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_SET_START_MASK)

Definition at line 48284 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_START_MASK

#define XTALOSC24M_OSC_CONFIG0_SET_START_MASK (0x1U)

Definition at line 48282 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_SET_START_SHIFT

#define XTALOSC24M_OSC_CONFIG0_SET_START_SHIFT (0U)

Definition at line 48283 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_START

#define XTALOSC24M_OSC_CONFIG0_START | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_START_MASK)

Definition at line 48256 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_START_MASK

#define XTALOSC24M_OSC_CONFIG0_START_MASK (0x1U)

Definition at line 48254 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_START_SHIFT

#define XTALOSC24M_OSC_CONFIG0_START_SHIFT (0U)

Definition at line 48255 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_BYPASS

#define XTALOSC24M_OSC_CONFIG0_TOG_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_MASK)

Definition at line 48346 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_MASK (0x4U)

Definition at line 48344 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_BYPASS_SHIFT (2U)

Definition at line 48345 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_ENABLE

#define XTALOSC24M_OSC_CONFIG0_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_MASK)

Definition at line 48343 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_MASK (0x2U)

Definition at line 48341 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_ENABLE_SHIFT (1U)

Definition at line 48342 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS

#define XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_MASK)

Definition at line 48358 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_MASK (0xF0000U)

Definition at line 48356 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_HYST_MINUS_SHIFT (16U)

Definition at line 48357 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS

#define XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_MASK)

Definition at line 48355 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_MASK (0xF000U)

Definition at line 48353 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_HYST_PLUS_SHIFT (12U)

Definition at line 48354 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_INVERT

#define XTALOSC24M_OSC_CONFIG0_TOG_INVERT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_INVERT_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_INVERT_MASK)

Definition at line 48349 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_INVERT_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_INVERT_MASK (0x8U)

Definition at line 48347 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_INVERT_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_INVERT_SHIFT (3U)

Definition at line 48348 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG

#define XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_MASK)

Definition at line 48352 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR

#define XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_MASK)

Definition at line 48361 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_MASK (0xFF000000U)

Definition at line 48359 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_CUR_SHIFT (24U)

Definition at line 48360 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_MASK (0xFF0U)

Definition at line 48350 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_RC_OSC_PROG_SHIFT (4U)

Definition at line 48351 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_START

#define XTALOSC24M_OSC_CONFIG0_TOG_START | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG0_TOG_START_SHIFT)) & XTALOSC24M_OSC_CONFIG0_TOG_START_MASK)

Definition at line 48340 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_START_MASK

#define XTALOSC24M_OSC_CONFIG0_TOG_START_MASK (0x1U)

Definition at line 48338 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG0_TOG_START_SHIFT

#define XTALOSC24M_OSC_CONFIG0_TOG_START_SHIFT (0U)

Definition at line 48339 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR

#define XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_MASK)

Definition at line 48391 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_MASK

#define XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_MASK (0xFFF00000U)

Definition at line 48389 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_CUR_SHIFT (20U)

Definition at line 48390 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG

#define XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_MASK)

Definition at line 48388 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_MASK

#define XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_MASK (0xFFFU)

Definition at line 48386 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG1_CLR_COUNT_RC_TRG_SHIFT (0U)

Definition at line 48387 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR

#define XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_MASK)

Definition at line 48371 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_MASK

#define XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_MASK (0xFFF00000U)

Definition at line 48369 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG1_COUNT_RC_CUR_SHIFT (20U)

Definition at line 48370 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG

#define XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_MASK)

Definition at line 48368 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_MASK

#define XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_MASK (0xFFFU)

Definition at line 48366 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG1_COUNT_RC_TRG_SHIFT (0U)

Definition at line 48367 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR

#define XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_MASK)

Definition at line 48381 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_MASK

#define XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_MASK (0xFFF00000U)

Definition at line 48379 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_CUR_SHIFT (20U)

Definition at line 48380 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG

#define XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_MASK)

Definition at line 48378 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_MASK

#define XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_MASK (0xFFFU)

Definition at line 48376 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG1_SET_COUNT_RC_TRG_SHIFT (0U)

Definition at line 48377 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR

#define XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_SHIFT)) & XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_MASK)

Definition at line 48401 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_MASK

#define XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_MASK (0xFFF00000U)

Definition at line 48399 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_SHIFT

#define XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_CUR_SHIFT (20U)

Definition at line 48400 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG

#define XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_MASK)

Definition at line 48398 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_MASK

#define XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_MASK (0xFFFU)

Definition at line 48396 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG1_TOG_COUNT_RC_TRG_SHIFT (0U)

Definition at line 48397 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL

#define XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_MASK)

Definition at line 48417 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_MASK

#define XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_MASK (0x80000000U)

Definition at line 48415 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_SHIFT

#define XTALOSC24M_OSC_CONFIG2_CLK_1M_ERR_FL_SHIFT (31U)

Definition at line 48416 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL

#define XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_MASK)

Definition at line 48449 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_MASK

#define XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_MASK (0x80000000U)

Definition at line 48447 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_SHIFT

#define XTALOSC24M_OSC_CONFIG2_CLR_CLK_1M_ERR_FL_SHIFT (31U)

Definition at line 48448 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG

#define XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_MASK)

Definition at line 48440 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_MASK

#define XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_MASK (0xFFFU)

Definition at line 48438 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG2_CLR_COUNT_1M_TRG_SHIFT (0U)

Definition at line 48439 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M

#define XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_MASK)

Definition at line 48443 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_MASK (0x10000U)

Definition at line 48441 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_CLR_ENABLE_1M_SHIFT (16U)

Definition at line 48442 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M

#define XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_MASK)

Definition at line 48446 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_MASK (0x20000U)

Definition at line 48444 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_CLR_MUX_1M_SHIFT (17U)

Definition at line 48445 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG

#define XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_MASK)

Definition at line 48408 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_MASK

#define XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_MASK (0xFFFU)

Definition at line 48406 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG2_COUNT_1M_TRG_SHIFT (0U)

Definition at line 48407 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_ENABLE_1M

#define XTALOSC24M_OSC_CONFIG2_ENABLE_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_ENABLE_1M_MASK)

Definition at line 48411 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_ENABLE_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_ENABLE_1M_MASK (0x10000U)

Definition at line 48409 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_ENABLE_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_ENABLE_1M_SHIFT (16U)

Definition at line 48410 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_MUX_1M

#define XTALOSC24M_OSC_CONFIG2_MUX_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_MUX_1M_MASK)

Definition at line 48414 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_MUX_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_MUX_1M_MASK (0x20000U)

Definition at line 48412 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_MUX_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_MUX_1M_SHIFT (17U)

Definition at line 48413 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL

#define XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_MASK)

Definition at line 48433 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_MASK

#define XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_MASK (0x80000000U)

Definition at line 48431 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_SHIFT

#define XTALOSC24M_OSC_CONFIG2_SET_CLK_1M_ERR_FL_SHIFT (31U)

Definition at line 48432 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG

#define XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_MASK)

Definition at line 48424 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_MASK

#define XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_MASK (0xFFFU)

Definition at line 48422 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG2_SET_COUNT_1M_TRG_SHIFT (0U)

Definition at line 48423 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M

#define XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_MASK)

Definition at line 48427 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_MASK (0x10000U)

Definition at line 48425 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_SET_ENABLE_1M_SHIFT (16U)

Definition at line 48426 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_MUX_1M

#define XTALOSC24M_OSC_CONFIG2_SET_MUX_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_MASK)

Definition at line 48430 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_MASK (0x20000U)

Definition at line 48428 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_SET_MUX_1M_SHIFT (17U)

Definition at line 48429 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL

#define XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_MASK)

Definition at line 48465 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_MASK

#define XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_MASK (0x80000000U)

Definition at line 48463 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_SHIFT

#define XTALOSC24M_OSC_CONFIG2_TOG_CLK_1M_ERR_FL_SHIFT (31U)

Definition at line 48464 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG

#define XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_MASK)

Definition at line 48456 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_MASK

#define XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_MASK (0xFFFU)

Definition at line 48454 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_SHIFT

#define XTALOSC24M_OSC_CONFIG2_TOG_COUNT_1M_TRG_SHIFT (0U)

Definition at line 48455 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M

#define XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_MASK)

Definition at line 48459 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_MASK (0x10000U)

Definition at line 48457 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_TOG_ENABLE_1M_SHIFT (16U)

Definition at line 48458 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M

#define XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_SHIFT)) & XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_MASK)

Definition at line 48462 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_MASK

#define XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_MASK (0x20000U)

Definition at line 48460 of file MIMXRT1062.h.

## ◆ XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_SHIFT

#define XTALOSC24M_OSC_CONFIG2_TOG_MUX_1M_SHIFT (17U)

Definition at line 48461 of file MIMXRT1062.h.