Callisto4Bootloader: LCDIF Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
LCDIF Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| LCDIF Register Masks

## Data Structures

struct | LCDIF_Type

## Macros

#define | LCDIF_BASE (0x402B8000u)
#define | LCDIF ((LCDIF_Type *)LCDIF_BASE)
#define | LCDIF_BASE_ADDRS { LCDIF_BASE }
#define | LCDIF_BASE_PTRS { LCDIF }
#define | LCDIF_IRQ0_IRQS { LCDIF_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ LCDIF

#define LCDIF ((LCDIF_Type *)LCDIF_BASE)

Peripheral LCDIF base pointer

Definition at line 26651 of file MIMXRT1062.h.

## ◆ LCDIF_BASE

#define LCDIF_BASE (0x402B8000u)

Peripheral LCDIF base address

Definition at line 26649 of file MIMXRT1062.h.

## ◆ LCDIF_BASE_ADDRS

#define LCDIF_BASE_ADDRS { LCDIF_BASE }

Array initializer of LCDIF peripheral base addresses

Definition at line 26653 of file MIMXRT1062.h.

## ◆ LCDIF_BASE_PTRS

#define LCDIF_BASE_PTRS { LCDIF }

Array initializer of LCDIF peripheral base pointers

Definition at line 26655 of file MIMXRT1062.h.

## ◆ LCDIF_IRQ0_IRQS

#define LCDIF_IRQ0_IRQS { LCDIF_IRQn }

Interrupt vectors for the LCDIF peripheral type

Definition at line 26657 of file MIMXRT1062.h.