Callisto4Bootloader: WDOG Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
WDOG Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| WDOG Register Masks

## Data Structures

struct | WDOG_Type

## Macros

#define | WDOG1_BASE (0x400B8000u)
#define | WDOG1 ((WDOG_Type *)WDOG1_BASE)
#define | WDOG2_BASE (0x400D0000u)
#define | WDOG2 ((WDOG_Type *)WDOG2_BASE)
#define | WDOG_BASE_ADDRS { 0u, WDOG1_BASE, WDOG2_BASE }
#define | WDOG_BASE_PTRS { (WDOG_Type *)0u, WDOG1, WDOG2 }
#define | WDOG_IRQS { NotAvail_IRQn, WDOG1_IRQn, WDOG2_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ WDOG1

#define WDOG1 ((WDOG_Type *)WDOG1_BASE)

Peripheral WDOG1 base pointer

Definition at line 46492 of file MIMXRT1062.h.

## ◆ WDOG1_BASE

#define WDOG1_BASE (0x400B8000u)

Peripheral WDOG1 base address

Definition at line 46490 of file MIMXRT1062.h.

## ◆ WDOG2

#define WDOG2 ((WDOG_Type *)WDOG2_BASE)

Peripheral WDOG2 base pointer

Definition at line 46496 of file MIMXRT1062.h.

## ◆ WDOG2_BASE

#define WDOG2_BASE (0x400D0000u)

Peripheral WDOG2 base address

Definition at line 46494 of file MIMXRT1062.h.

## ◆ WDOG_BASE_ADDRS

#define WDOG_BASE_ADDRS { 0u, WDOG1_BASE, WDOG2_BASE }

Array initializer of WDOG peripheral base addresses

Definition at line 46498 of file MIMXRT1062.h.

## ◆ WDOG_BASE_PTRS

#define WDOG_BASE_PTRS { (WDOG_Type *)0u, WDOG1, WDOG2 }

Array initializer of WDOG peripheral base pointers

Definition at line 46500 of file MIMXRT1062.h.

## ◆ WDOG_IRQS

#define WDOG_IRQS { NotAvail_IRQn, WDOG1_IRQn, WDOG2_IRQn }

Interrupt vectors for the WDOG peripheral type

Definition at line 46502 of file MIMXRT1062.h.