Callisto4Bootloader: LPI2C_Type Struct Reference

Callisto4Bootloader

Data Fields
LPI2C_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » LPI2C Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__I uint32_t | VERID
__I uint32_t | PARAM
uint8_t | RESERVED_0 [8]
__IO uint32_t | MCR
__IO uint32_t | MSR
__IO uint32_t | MIER
__IO uint32_t | MDER
__IO uint32_t | MCFGR0
__IO uint32_t | MCFGR1
__IO uint32_t | MCFGR2
__IO uint32_t | MCFGR3
uint8_t | RESERVED_1 [16]
__IO uint32_t | MDMR
uint8_t | RESERVED_2 [4]
__IO uint32_t | MCCR0
uint8_t | RESERVED_3 [4]
__IO uint32_t | MCCR1
uint8_t | RESERVED_4 [4]
__IO uint32_t | MFCR
__I uint32_t | MFSR
__O uint32_t | MTDR
uint8_t | RESERVED_5 [12]
__I uint32_t | MRDR
uint8_t | RESERVED_6 [156]
__IO uint32_t | SCR
__IO uint32_t | SSR
__IO uint32_t | SIER
__IO uint32_t | SDER
uint8_t | RESERVED_7 [4]
__IO uint32_t | SCFGR1
__IO uint32_t | SCFGR2
uint8_t | RESERVED_8 [20]
__IO uint32_t | SAMR
uint8_t | RESERVED_9 [12]
__I uint32_t | SASR
__IO uint32_t | STAR
uint8_t | RESERVED_10 [8]
__O uint32_t | STDR
uint8_t | RESERVED_11 [12]
__I uint32_t | SRDR

## Detailed Description

LPI2C - Register Layout Typedef

Definition at line 26674 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h