Callisto4Bootloader: ADC_ETC Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
ADC_ETC Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| ADC_ETC Register Masks

## Data Structures

struct | ADC_ETC_Type

## Macros

#define | ADC_ETC_BASE (0x403B0000u)
#define | ADC_ETC ((ADC_ETC_Type *)ADC_ETC_BASE)
#define | ADC_ETC_BASE_ADDRS { ADC_ETC_BASE }
#define | ADC_ETC_BASE_PTRS { ADC_ETC }
#define | ADC_ETC_IRQS { { ADC_ETC_IRQ0_IRQn, ADC_ETC_IRQ1_IRQn, ADC_ETC_IRQ2_IRQn } }
#define | ADC_ETC_FAULT_IRQS { ADC_ETC_ERROR_IRQ_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ ADC_ETC

#define ADC_ETC ((ADC_ETC_Type *)ADC_ETC_BASE)

Peripheral ADC_ETC base pointer

Definition at line 2179 of file MIMXRT1062.h.

## ◆ ADC_ETC_BASE

#define ADC_ETC_BASE (0x403B0000u)

Peripheral ADC_ETC base address

Definition at line 2177 of file MIMXRT1062.h.

## ◆ ADC_ETC_BASE_ADDRS

#define ADC_ETC_BASE_ADDRS { ADC_ETC_BASE }

Array initializer of ADC_ETC peripheral base addresses

Definition at line 2181 of file MIMXRT1062.h.

## ◆ ADC_ETC_BASE_PTRS

#define ADC_ETC_BASE_PTRS { ADC_ETC }

Array initializer of ADC_ETC peripheral base pointers

Definition at line 2183 of file MIMXRT1062.h.

## ◆ ADC_ETC_FAULT_IRQS

#define ADC_ETC_FAULT_IRQS { ADC_ETC_ERROR_IRQ_IRQn }

Definition at line 2186 of file MIMXRT1062.h.

## ◆ ADC_ETC_IRQS

#define ADC_ETC_IRQS { { ADC_ETC_IRQ0_IRQn, ADC_ETC_IRQ1_IRQn, ADC_ETC_IRQ2_IRQn } }

Interrupt vectors for the ADC_ETC peripheral type

Definition at line 2185 of file MIMXRT1062.h.