Callisto4Bootloader: LCDIF Register Masks

Callisto4Bootloader

Macros
LCDIF Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » LCDIF Peripheral Access Layer

## Macros

#define | LCDIF_PIGEON_0_COUNT (12U)
#define | LCDIF_PIGEON_1_COUNT (12U)
#define | LCDIF_PIGEON_2_COUNT (12U)

## CTRL - LCDIF General Control Register

#define | LCDIF_CTRL_RUN_MASK (0x1U)
#define | LCDIF_CTRL_RUN_SHIFT (0U)
#define | LCDIF_CTRL_RUN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_RUN_SHIFT)) & LCDIF_CTRL_RUN_MASK)
#define | LCDIF_CTRL_DATA_FORMAT_24_BIT_MASK (0x2U)
#define | LCDIF_CTRL_DATA_FORMAT_24_BIT_SHIFT (1U)
#define | LCDIF_CTRL_DATA_FORMAT_24_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_DATA_FORMAT_24_BIT_MASK)
#define | LCDIF_CTRL_DATA_FORMAT_18_BIT_MASK (0x4U)
#define | LCDIF_CTRL_DATA_FORMAT_18_BIT_SHIFT (2U)
#define | LCDIF_CTRL_DATA_FORMAT_18_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_DATA_FORMAT_18_BIT_MASK)
#define | LCDIF_CTRL_DATA_FORMAT_16_BIT_MASK (0x8U)
#define | LCDIF_CTRL_DATA_FORMAT_16_BIT_SHIFT (3U)
#define | LCDIF_CTRL_DATA_FORMAT_16_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_DATA_FORMAT_16_BIT_MASK)
#define | LCDIF_CTRL_RSRVD0_MASK (0x10U)
#define | LCDIF_CTRL_RSRVD0_SHIFT (4U)
#define | LCDIF_CTRL_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_RSRVD0_SHIFT)) & LCDIF_CTRL_RSRVD0_MASK)
#define | LCDIF_CTRL_MASTER_MASK (0x20U)
#define | LCDIF_CTRL_MASTER_SHIFT (5U)
#define | LCDIF_CTRL_MASTER(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_MASTER_SHIFT)) & LCDIF_CTRL_MASTER_MASK)
#define | LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_MASK (0x40U)
#define | LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_SHIFT (6U)
#define | LCDIF_CTRL_ENABLE_PXP_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_MASK)
#define | LCDIF_CTRL_WORD_LENGTH_MASK (0x300U)
#define | LCDIF_CTRL_WORD_LENGTH_SHIFT (8U)
#define | LCDIF_CTRL_WORD_LENGTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_WORD_LENGTH_MASK)
#define | LCDIF_CTRL_LCD_DATABUS_WIDTH_MASK (0xC00U)
#define | LCDIF_CTRL_LCD_DATABUS_WIDTH_SHIFT (10U)
#define | LCDIF_CTRL_LCD_DATABUS_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_LCD_DATABUS_WIDTH_MASK)
#define | LCDIF_CTRL_CSC_DATA_SWIZZLE_MASK (0x3000U)
#define | LCDIF_CTRL_CSC_DATA_SWIZZLE_SHIFT (12U)
#define | LCDIF_CTRL_CSC_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_CSC_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_INPUT_DATA_SWIZZLE_MASK (0xC000U)
#define | LCDIF_CTRL_INPUT_DATA_SWIZZLE_SHIFT (14U)
#define | LCDIF_CTRL_INPUT_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_INPUT_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_DOTCLK_MODE_MASK (0x20000U)
#define | LCDIF_CTRL_DOTCLK_MODE_SHIFT (17U)
#define | LCDIF_CTRL_DOTCLK_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_DOTCLK_MODE_MASK)
#define | LCDIF_CTRL_BYPASS_COUNT_MASK (0x80000U)
#define | LCDIF_CTRL_BYPASS_COUNT_SHIFT (19U)
#define | LCDIF_CTRL_BYPASS_COUNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_BYPASS_COUNT_MASK)
#define | LCDIF_CTRL_SHIFT_NUM_BITS_MASK (0x3E00000U)
#define | LCDIF_CTRL_SHIFT_NUM_BITS_SHIFT (21U)
#define | LCDIF_CTRL_SHIFT_NUM_BITS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_SHIFT_NUM_BITS_MASK)
#define | LCDIF_CTRL_DATA_SHIFT_DIR_MASK (0x4000000U)
#define | LCDIF_CTRL_DATA_SHIFT_DIR_SHIFT (26U)
#define | LCDIF_CTRL_DATA_SHIFT_DIR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_DATA_SHIFT_DIR_MASK)
#define | LCDIF_CTRL_CLKGATE_MASK (0x40000000U)
#define | LCDIF_CTRL_CLKGATE_SHIFT (30U)
#define | LCDIF_CTRL_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLKGATE_SHIFT)) & LCDIF_CTRL_CLKGATE_MASK)
#define | LCDIF_CTRL_SFTRST_MASK (0x80000000U)
#define | LCDIF_CTRL_SFTRST_SHIFT (31U)
#define | LCDIF_CTRL_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SFTRST_SHIFT)) & LCDIF_CTRL_SFTRST_MASK)

## CTRL_SET - LCDIF General Control Register

#define | LCDIF_CTRL_SET_RUN_MASK (0x1U)
#define | LCDIF_CTRL_SET_RUN_SHIFT (0U)
#define | LCDIF_CTRL_SET_RUN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_RUN_SHIFT)) & LCDIF_CTRL_SET_RUN_MASK)
#define | LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_MASK (0x2U)
#define | LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_SHIFT (1U)
#define | LCDIF_CTRL_SET_DATA_FORMAT_24_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_MASK)
#define | LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_MASK (0x4U)
#define | LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_SHIFT (2U)
#define | LCDIF_CTRL_SET_DATA_FORMAT_18_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_MASK)
#define | LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_MASK (0x8U)
#define | LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_SHIFT (3U)
#define | LCDIF_CTRL_SET_DATA_FORMAT_16_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_MASK)
#define | LCDIF_CTRL_SET_RSRVD0_MASK (0x10U)
#define | LCDIF_CTRL_SET_RSRVD0_SHIFT (4U)
#define | LCDIF_CTRL_SET_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_RSRVD0_SHIFT)) & LCDIF_CTRL_SET_RSRVD0_MASK)
#define | LCDIF_CTRL_SET_MASTER_MASK (0x20U)
#define | LCDIF_CTRL_SET_MASTER_SHIFT (5U)
#define | LCDIF_CTRL_SET_MASTER(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_MASTER_SHIFT)) & LCDIF_CTRL_SET_MASTER_MASK)
#define | LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_MASK (0x40U)
#define | LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_SHIFT (6U)
#define | LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_MASK)
#define | LCDIF_CTRL_SET_WORD_LENGTH_MASK (0x300U)
#define | LCDIF_CTRL_SET_WORD_LENGTH_SHIFT (8U)
#define | LCDIF_CTRL_SET_WORD_LENGTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_SET_WORD_LENGTH_MASK)
#define | LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_MASK (0xC00U)
#define | LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_SHIFT (10U)
#define | LCDIF_CTRL_SET_LCD_DATABUS_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_MASK)
#define | LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_MASK (0x3000U)
#define | LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_SHIFT (12U)
#define | LCDIF_CTRL_SET_CSC_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_MASK (0xC000U)
#define | LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_SHIFT (14U)
#define | LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_SET_DOTCLK_MODE_MASK (0x20000U)
#define | LCDIF_CTRL_SET_DOTCLK_MODE_SHIFT (17U)
#define | LCDIF_CTRL_SET_DOTCLK_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_SET_DOTCLK_MODE_MASK)
#define | LCDIF_CTRL_SET_BYPASS_COUNT_MASK (0x80000U)
#define | LCDIF_CTRL_SET_BYPASS_COUNT_SHIFT (19U)
#define | LCDIF_CTRL_SET_BYPASS_COUNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_SET_BYPASS_COUNT_MASK)
#define | LCDIF_CTRL_SET_SHIFT_NUM_BITS_MASK (0x3E00000U)
#define | LCDIF_CTRL_SET_SHIFT_NUM_BITS_SHIFT (21U)
#define | LCDIF_CTRL_SET_SHIFT_NUM_BITS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_SET_SHIFT_NUM_BITS_MASK)
#define | LCDIF_CTRL_SET_DATA_SHIFT_DIR_MASK (0x4000000U)
#define | LCDIF_CTRL_SET_DATA_SHIFT_DIR_SHIFT (26U)
#define | LCDIF_CTRL_SET_DATA_SHIFT_DIR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_SET_DATA_SHIFT_DIR_MASK)
#define | LCDIF_CTRL_SET_CLKGATE_MASK (0x40000000U)
#define | LCDIF_CTRL_SET_CLKGATE_SHIFT (30U)
#define | LCDIF_CTRL_SET_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_CLKGATE_SHIFT)) & LCDIF_CTRL_SET_CLKGATE_MASK)
#define | LCDIF_CTRL_SET_SFTRST_MASK (0x80000000U)
#define | LCDIF_CTRL_SET_SFTRST_SHIFT (31U)
#define | LCDIF_CTRL_SET_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_SFTRST_SHIFT)) & LCDIF_CTRL_SET_SFTRST_MASK)

## CTRL_CLR - LCDIF General Control Register

#define | LCDIF_CTRL_CLR_RUN_MASK (0x1U)
#define | LCDIF_CTRL_CLR_RUN_SHIFT (0U)
#define | LCDIF_CTRL_CLR_RUN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_RUN_SHIFT)) & LCDIF_CTRL_CLR_RUN_MASK)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_MASK (0x2U)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_SHIFT (1U)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_MASK)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_MASK (0x4U)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_SHIFT (2U)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_MASK)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_MASK (0x8U)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_SHIFT (3U)
#define | LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_MASK)
#define | LCDIF_CTRL_CLR_RSRVD0_MASK (0x10U)
#define | LCDIF_CTRL_CLR_RSRVD0_SHIFT (4U)
#define | LCDIF_CTRL_CLR_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_RSRVD0_SHIFT)) & LCDIF_CTRL_CLR_RSRVD0_MASK)
#define | LCDIF_CTRL_CLR_MASTER_MASK (0x20U)
#define | LCDIF_CTRL_CLR_MASTER_SHIFT (5U)
#define | LCDIF_CTRL_CLR_MASTER(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_MASTER_SHIFT)) & LCDIF_CTRL_CLR_MASTER_MASK)
#define | LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_MASK (0x40U)
#define | LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_SHIFT (6U)
#define | LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_MASK)
#define | LCDIF_CTRL_CLR_WORD_LENGTH_MASK (0x300U)
#define | LCDIF_CTRL_CLR_WORD_LENGTH_SHIFT (8U)
#define | LCDIF_CTRL_CLR_WORD_LENGTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_CLR_WORD_LENGTH_MASK)
#define | LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_MASK (0xC00U)
#define | LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_SHIFT (10U)
#define | LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_MASK)
#define | LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_MASK (0x3000U)
#define | LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_SHIFT (12U)
#define | LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_MASK (0xC000U)
#define | LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_SHIFT (14U)
#define | LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_CLR_DOTCLK_MODE_MASK (0x20000U)
#define | LCDIF_CTRL_CLR_DOTCLK_MODE_SHIFT (17U)
#define | LCDIF_CTRL_CLR_DOTCLK_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_CLR_DOTCLK_MODE_MASK)
#define | LCDIF_CTRL_CLR_BYPASS_COUNT_MASK (0x80000U)
#define | LCDIF_CTRL_CLR_BYPASS_COUNT_SHIFT (19U)
#define | LCDIF_CTRL_CLR_BYPASS_COUNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_CLR_BYPASS_COUNT_MASK)
#define | LCDIF_CTRL_CLR_SHIFT_NUM_BITS_MASK (0x3E00000U)
#define | LCDIF_CTRL_CLR_SHIFT_NUM_BITS_SHIFT (21U)
#define | LCDIF_CTRL_CLR_SHIFT_NUM_BITS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_CLR_SHIFT_NUM_BITS_MASK)
#define | LCDIF_CTRL_CLR_DATA_SHIFT_DIR_MASK (0x4000000U)
#define | LCDIF_CTRL_CLR_DATA_SHIFT_DIR_SHIFT (26U)
#define | LCDIF_CTRL_CLR_DATA_SHIFT_DIR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_CLR_DATA_SHIFT_DIR_MASK)
#define | LCDIF_CTRL_CLR_CLKGATE_MASK (0x40000000U)
#define | LCDIF_CTRL_CLR_CLKGATE_SHIFT (30U)
#define | LCDIF_CTRL_CLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_CLKGATE_SHIFT)) & LCDIF_CTRL_CLR_CLKGATE_MASK)
#define | LCDIF_CTRL_CLR_SFTRST_MASK (0x80000000U)
#define | LCDIF_CTRL_CLR_SFTRST_SHIFT (31U)
#define | LCDIF_CTRL_CLR_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_SFTRST_SHIFT)) & LCDIF_CTRL_CLR_SFTRST_MASK)

## CTRL_TOG - LCDIF General Control Register

#define | LCDIF_CTRL_TOG_RUN_MASK (0x1U)
#define | LCDIF_CTRL_TOG_RUN_SHIFT (0U)
#define | LCDIF_CTRL_TOG_RUN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_RUN_SHIFT)) & LCDIF_CTRL_TOG_RUN_MASK)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_MASK (0x2U)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_SHIFT (1U)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_MASK)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_MASK (0x4U)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_SHIFT (2U)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_MASK)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_MASK (0x8U)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_SHIFT (3U)
#define | LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_MASK)
#define | LCDIF_CTRL_TOG_RSRVD0_MASK (0x10U)
#define | LCDIF_CTRL_TOG_RSRVD0_SHIFT (4U)
#define | LCDIF_CTRL_TOG_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_RSRVD0_SHIFT)) & LCDIF_CTRL_TOG_RSRVD0_MASK)
#define | LCDIF_CTRL_TOG_MASTER_MASK (0x20U)
#define | LCDIF_CTRL_TOG_MASTER_SHIFT (5U)
#define | LCDIF_CTRL_TOG_MASTER(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_MASTER_SHIFT)) & LCDIF_CTRL_TOG_MASTER_MASK)
#define | LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_MASK (0x40U)
#define | LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_SHIFT (6U)
#define | LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_MASK)
#define | LCDIF_CTRL_TOG_WORD_LENGTH_MASK (0x300U)
#define | LCDIF_CTRL_TOG_WORD_LENGTH_SHIFT (8U)
#define | LCDIF_CTRL_TOG_WORD_LENGTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_TOG_WORD_LENGTH_MASK)
#define | LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_MASK (0xC00U)
#define | LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_SHIFT (10U)
#define | LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_MASK)
#define | LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_MASK (0x3000U)
#define | LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_SHIFT (12U)
#define | LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_MASK (0xC000U)
#define | LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_SHIFT (14U)
#define | LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_MASK)
#define | LCDIF_CTRL_TOG_DOTCLK_MODE_MASK (0x20000U)
#define | LCDIF_CTRL_TOG_DOTCLK_MODE_SHIFT (17U)
#define | LCDIF_CTRL_TOG_DOTCLK_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_TOG_DOTCLK_MODE_MASK)
#define | LCDIF_CTRL_TOG_BYPASS_COUNT_MASK (0x80000U)
#define | LCDIF_CTRL_TOG_BYPASS_COUNT_SHIFT (19U)
#define | LCDIF_CTRL_TOG_BYPASS_COUNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_TOG_BYPASS_COUNT_MASK)
#define | LCDIF_CTRL_TOG_SHIFT_NUM_BITS_MASK (0x3E00000U)
#define | LCDIF_CTRL_TOG_SHIFT_NUM_BITS_SHIFT (21U)
#define | LCDIF_CTRL_TOG_SHIFT_NUM_BITS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_TOG_SHIFT_NUM_BITS_MASK)
#define | LCDIF_CTRL_TOG_DATA_SHIFT_DIR_MASK (0x4000000U)
#define | LCDIF_CTRL_TOG_DATA_SHIFT_DIR_SHIFT (26U)
#define | LCDIF_CTRL_TOG_DATA_SHIFT_DIR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_TOG_DATA_SHIFT_DIR_MASK)
#define | LCDIF_CTRL_TOG_CLKGATE_MASK (0x40000000U)
#define | LCDIF_CTRL_TOG_CLKGATE_SHIFT (30U)
#define | LCDIF_CTRL_TOG_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_CLKGATE_SHIFT)) & LCDIF_CTRL_TOG_CLKGATE_MASK)
#define | LCDIF_CTRL_TOG_SFTRST_MASK (0x80000000U)
#define | LCDIF_CTRL_TOG_SFTRST_SHIFT (31U)
#define | LCDIF_CTRL_TOG_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_SFTRST_SHIFT)) & LCDIF_CTRL_TOG_SFTRST_MASK)

## CTRL1 - LCDIF General Control1 Register

#define | LCDIF_CTRL1_RSRVD0_MASK (0xF8U)
#define | LCDIF_CTRL1_RSRVD0_SHIFT (3U)
#define | LCDIF_CTRL1_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_RSRVD0_SHIFT)) & LCDIF_CTRL1_RSRVD0_MASK)
#define | LCDIF_CTRL1_VSYNC_EDGE_IRQ_MASK (0x100U)
#define | LCDIF_CTRL1_VSYNC_EDGE_IRQ_SHIFT (8U)
#define | LCDIF_CTRL1_VSYNC_EDGE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_VSYNC_EDGE_IRQ_MASK)
#define | LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_MASK (0x200U)
#define | LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_SHIFT (9U)
#define | LCDIF_CTRL1_CUR_FRAME_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_MASK)
#define | LCDIF_CTRL1_UNDERFLOW_IRQ_MASK (0x400U)
#define | LCDIF_CTRL1_UNDERFLOW_IRQ_SHIFT (10U)
#define | LCDIF_CTRL1_UNDERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_UNDERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_OVERFLOW_IRQ_MASK (0x800U)
#define | LCDIF_CTRL1_OVERFLOW_IRQ_SHIFT (11U)
#define | LCDIF_CTRL1_OVERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_OVERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)
#define | LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_SHIFT (12U)
#define | LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)
#define | LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)
#define | LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_UNDERFLOW_IRQ_EN_MASK (0x4000U)
#define | LCDIF_CTRL1_UNDERFLOW_IRQ_EN_SHIFT (14U)
#define | LCDIF_CTRL1_UNDERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_UNDERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_OVERFLOW_IRQ_EN_MASK (0x8000U)
#define | LCDIF_CTRL1_OVERFLOW_IRQ_EN_SHIFT (15U)
#define | LCDIF_CTRL1_OVERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_OVERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_BYTE_PACKING_FORMAT_MASK (0xF0000U)
#define | LCDIF_CTRL1_BYTE_PACKING_FORMAT_SHIFT (16U)
#define | LCDIF_CTRL1_BYTE_PACKING_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_BYTE_PACKING_FORMAT_MASK)
#define | LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)
#define | LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)
#define | LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_MASK)
#define | LCDIF_CTRL1_FIFO_CLEAR_MASK (0x200000U)
#define | LCDIF_CTRL1_FIFO_CLEAR_SHIFT (21U)
#define | LCDIF_CTRL1_FIFO_CLEAR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_FIFO_CLEAR_MASK)
#define | LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)
#define | LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)
#define | LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_MASK)
#define | LCDIF_CTRL1_INTERLACE_FIELDS_MASK (0x800000U)
#define | LCDIF_CTRL1_INTERLACE_FIELDS_SHIFT (23U)
#define | LCDIF_CTRL1_INTERLACE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_INTERLACE_FIELDS_MASK)
#define | LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)
#define | LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_SHIFT (24U)
#define | LCDIF_CTRL1_RECOVER_ON_UNDERFLOW(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_MASK)
#define | LCDIF_CTRL1_BM_ERROR_IRQ_MASK (0x2000000U)
#define | LCDIF_CTRL1_BM_ERROR_IRQ_SHIFT (25U)
#define | LCDIF_CTRL1_BM_ERROR_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_BM_ERROR_IRQ_MASK)
#define | LCDIF_CTRL1_BM_ERROR_IRQ_EN_MASK (0x4000000U)
#define | LCDIF_CTRL1_BM_ERROR_IRQ_EN_SHIFT (26U)
#define | LCDIF_CTRL1_BM_ERROR_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_BM_ERROR_IRQ_EN_MASK)
#define | LCDIF_CTRL1_CS_OUT_SELECT_MASK (0x40000000U)
#define | LCDIF_CTRL1_CS_OUT_SELECT_SHIFT (30U)
#define | LCDIF_CTRL1_CS_OUT_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_CS_OUT_SELECT_MASK)
#define | LCDIF_CTRL1_IMAGE_DATA_SELECT_MASK (0x80000000U)
#define | LCDIF_CTRL1_IMAGE_DATA_SELECT_SHIFT (31U)
#define | LCDIF_CTRL1_IMAGE_DATA_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_IMAGE_DATA_SELECT_MASK)

## CTRL1_SET - LCDIF General Control1 Register

#define | LCDIF_CTRL1_SET_RSRVD0_MASK (0xF8U)
#define | LCDIF_CTRL1_SET_RSRVD0_SHIFT (3U)
#define | LCDIF_CTRL1_SET_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_RSRVD0_SHIFT)) & LCDIF_CTRL1_SET_RSRVD0_MASK)
#define | LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_MASK (0x100U)
#define | LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_SHIFT (8U)
#define | LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_MASK)
#define | LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_MASK (0x200U)
#define | LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_SHIFT (9U)
#define | LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_MASK)
#define | LCDIF_CTRL1_SET_UNDERFLOW_IRQ_MASK (0x400U)
#define | LCDIF_CTRL1_SET_UNDERFLOW_IRQ_SHIFT (10U)
#define | LCDIF_CTRL1_SET_UNDERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_SET_UNDERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_SET_OVERFLOW_IRQ_MASK (0x800U)
#define | LCDIF_CTRL1_SET_OVERFLOW_IRQ_SHIFT (11U)
#define | LCDIF_CTRL1_SET_OVERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_SET_OVERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)
#define | LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_SHIFT (12U)
#define | LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)
#define | LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)
#define | LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_MASK (0x4000U)
#define | LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_SHIFT (14U)
#define | LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_MASK (0x8000U)
#define | LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_SHIFT (15U)
#define | LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_MASK (0xF0000U)
#define | LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_SHIFT (16U)
#define | LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_MASK)
#define | LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)
#define | LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)
#define | LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_MASK)
#define | LCDIF_CTRL1_SET_FIFO_CLEAR_MASK (0x200000U)
#define | LCDIF_CTRL1_SET_FIFO_CLEAR_SHIFT (21U)
#define | LCDIF_CTRL1_SET_FIFO_CLEAR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_SET_FIFO_CLEAR_MASK)
#define | LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)
#define | LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)
#define | LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_MASK)
#define | LCDIF_CTRL1_SET_INTERLACE_FIELDS_MASK (0x800000U)
#define | LCDIF_CTRL1_SET_INTERLACE_FIELDS_SHIFT (23U)
#define | LCDIF_CTRL1_SET_INTERLACE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_SET_INTERLACE_FIELDS_MASK)
#define | LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)
#define | LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_SHIFT (24U)
#define | LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_MASK)
#define | LCDIF_CTRL1_SET_BM_ERROR_IRQ_MASK (0x2000000U)
#define | LCDIF_CTRL1_SET_BM_ERROR_IRQ_SHIFT (25U)
#define | LCDIF_CTRL1_SET_BM_ERROR_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_SET_BM_ERROR_IRQ_MASK)
#define | LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_MASK (0x4000000U)
#define | LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_SHIFT (26U)
#define | LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_MASK)
#define | LCDIF_CTRL1_SET_CS_OUT_SELECT_MASK (0x40000000U)
#define | LCDIF_CTRL1_SET_CS_OUT_SELECT_SHIFT (30U)
#define | LCDIF_CTRL1_SET_CS_OUT_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_SET_CS_OUT_SELECT_MASK)
#define | LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_MASK (0x80000000U)
#define | LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_SHIFT (31U)
#define | LCDIF_CTRL1_SET_IMAGE_DATA_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_MASK)

## CTRL1_CLR - LCDIF General Control1 Register

#define | LCDIF_CTRL1_CLR_RSRVD0_MASK (0xF8U)
#define | LCDIF_CTRL1_CLR_RSRVD0_SHIFT (3U)
#define | LCDIF_CTRL1_CLR_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_RSRVD0_SHIFT)) & LCDIF_CTRL1_CLR_RSRVD0_MASK)
#define | LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_MASK (0x100U)
#define | LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_SHIFT (8U)
#define | LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_MASK)
#define | LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_MASK (0x200U)
#define | LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_SHIFT (9U)
#define | LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_MASK)
#define | LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_MASK (0x400U)
#define | LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_SHIFT (10U)
#define | LCDIF_CTRL1_CLR_UNDERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_CLR_OVERFLOW_IRQ_MASK (0x800U)
#define | LCDIF_CTRL1_CLR_OVERFLOW_IRQ_SHIFT (11U)
#define | LCDIF_CTRL1_CLR_OVERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_OVERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)
#define | LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_SHIFT (12U)
#define | LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)
#define | LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)
#define | LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_MASK (0x4000U)
#define | LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_SHIFT (14U)
#define | LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_MASK (0x8000U)
#define | LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_SHIFT (15U)
#define | LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_MASK (0xF0000U)
#define | LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_SHIFT (16U)
#define | LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_MASK)
#define | LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)
#define | LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)
#define | LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_MASK)
#define | LCDIF_CTRL1_CLR_FIFO_CLEAR_MASK (0x200000U)
#define | LCDIF_CTRL1_CLR_FIFO_CLEAR_SHIFT (21U)
#define | LCDIF_CTRL1_CLR_FIFO_CLEAR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_CLR_FIFO_CLEAR_MASK)
#define | LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)
#define | LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)
#define | LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_MASK)
#define | LCDIF_CTRL1_CLR_INTERLACE_FIELDS_MASK (0x800000U)
#define | LCDIF_CTRL1_CLR_INTERLACE_FIELDS_SHIFT (23U)
#define | LCDIF_CTRL1_CLR_INTERLACE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_CLR_INTERLACE_FIELDS_MASK)
#define | LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)
#define | LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_SHIFT (24U)
#define | LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_MASK)
#define | LCDIF_CTRL1_CLR_BM_ERROR_IRQ_MASK (0x2000000U)
#define | LCDIF_CTRL1_CLR_BM_ERROR_IRQ_SHIFT (25U)
#define | LCDIF_CTRL1_CLR_BM_ERROR_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_BM_ERROR_IRQ_MASK)
#define | LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_MASK (0x4000000U)
#define | LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_SHIFT (26U)
#define | LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_MASK)
#define | LCDIF_CTRL1_CLR_CS_OUT_SELECT_MASK (0x40000000U)
#define | LCDIF_CTRL1_CLR_CS_OUT_SELECT_SHIFT (30U)
#define | LCDIF_CTRL1_CLR_CS_OUT_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_CLR_CS_OUT_SELECT_MASK)
#define | LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_MASK (0x80000000U)
#define | LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_SHIFT (31U)
#define | LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_MASK)

## CTRL1_TOG - LCDIF General Control1 Register

#define | LCDIF_CTRL1_TOG_RSRVD0_MASK (0xF8U)
#define | LCDIF_CTRL1_TOG_RSRVD0_SHIFT (3U)
#define | LCDIF_CTRL1_TOG_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_RSRVD0_SHIFT)) & LCDIF_CTRL1_TOG_RSRVD0_MASK)
#define | LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_MASK (0x100U)
#define | LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_SHIFT (8U)
#define | LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_MASK)
#define | LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_MASK (0x200U)
#define | LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_SHIFT (9U)
#define | LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_MASK)
#define | LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_MASK (0x400U)
#define | LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_SHIFT (10U)
#define | LCDIF_CTRL1_TOG_UNDERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_TOG_OVERFLOW_IRQ_MASK (0x800U)
#define | LCDIF_CTRL1_TOG_OVERFLOW_IRQ_SHIFT (11U)
#define | LCDIF_CTRL1_TOG_OVERFLOW_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_OVERFLOW_IRQ_MASK)
#define | LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)
#define | LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_SHIFT (12U)
#define | LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)
#define | LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)
#define | LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_MASK)
#define | LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_MASK (0x4000U)
#define | LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_SHIFT (14U)
#define | LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_MASK (0x8000U)
#define | LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_SHIFT (15U)
#define | LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_MASK)
#define | LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_MASK (0xF0000U)
#define | LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_SHIFT (16U)
#define | LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_MASK)
#define | LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)
#define | LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)
#define | LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_MASK)
#define | LCDIF_CTRL1_TOG_FIFO_CLEAR_MASK (0x200000U)
#define | LCDIF_CTRL1_TOG_FIFO_CLEAR_SHIFT (21U)
#define | LCDIF_CTRL1_TOG_FIFO_CLEAR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_TOG_FIFO_CLEAR_MASK)
#define | LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)
#define | LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)
#define | LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_MASK)
#define | LCDIF_CTRL1_TOG_INTERLACE_FIELDS_MASK (0x800000U)
#define | LCDIF_CTRL1_TOG_INTERLACE_FIELDS_SHIFT (23U)
#define | LCDIF_CTRL1_TOG_INTERLACE_FIELDS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_TOG_INTERLACE_FIELDS_MASK)
#define | LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)
#define | LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_SHIFT (24U)
#define | LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_MASK)
#define | LCDIF_CTRL1_TOG_BM_ERROR_IRQ_MASK (0x2000000U)
#define | LCDIF_CTRL1_TOG_BM_ERROR_IRQ_SHIFT (25U)
#define | LCDIF_CTRL1_TOG_BM_ERROR_IRQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_BM_ERROR_IRQ_MASK)
#define | LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_MASK (0x4000000U)
#define | LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_SHIFT (26U)
#define | LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_MASK)
#define | LCDIF_CTRL1_TOG_CS_OUT_SELECT_MASK (0x40000000U)
#define | LCDIF_CTRL1_TOG_CS_OUT_SELECT_SHIFT (30U)
#define | LCDIF_CTRL1_TOG_CS_OUT_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_TOG_CS_OUT_SELECT_MASK)
#define | LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_MASK (0x80000000U)
#define | LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_SHIFT (31U)
#define | LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_MASK)

## CTRL2 - LCDIF General Control2 Register

#define | LCDIF_CTRL2_RSRVD0_MASK (0xFFFU)
#define | LCDIF_CTRL2_RSRVD0_SHIFT (0U)
#define | LCDIF_CTRL2_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD0_SHIFT)) & LCDIF_CTRL2_RSRVD0_MASK)
#define | LCDIF_CTRL2_EVEN_LINE_PATTERN_MASK (0x7000U)
#define | LCDIF_CTRL2_EVEN_LINE_PATTERN_SHIFT (12U)
#define | LCDIF_CTRL2_EVEN_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_EVEN_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_RSRVD3_MASK (0x8000U)
#define | LCDIF_CTRL2_RSRVD3_SHIFT (15U)
#define | LCDIF_CTRL2_RSRVD3(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD3_SHIFT)) & LCDIF_CTRL2_RSRVD3_MASK)
#define | LCDIF_CTRL2_ODD_LINE_PATTERN_MASK (0x70000U)
#define | LCDIF_CTRL2_ODD_LINE_PATTERN_SHIFT (16U)
#define | LCDIF_CTRL2_ODD_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_ODD_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_RSRVD4_MASK (0x80000U)
#define | LCDIF_CTRL2_RSRVD4_SHIFT (19U)
#define | LCDIF_CTRL2_RSRVD4(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD4_SHIFT)) & LCDIF_CTRL2_RSRVD4_MASK)
#define | LCDIF_CTRL2_BURST_LEN_8_MASK (0x100000U)
#define | LCDIF_CTRL2_BURST_LEN_8_SHIFT (20U)
#define | LCDIF_CTRL2_BURST_LEN_8(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_BURST_LEN_8_MASK)
#define | LCDIF_CTRL2_OUTSTANDING_REQS_MASK (0xE00000U)
#define | LCDIF_CTRL2_OUTSTANDING_REQS_SHIFT (21U)
#define | LCDIF_CTRL2_OUTSTANDING_REQS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_OUTSTANDING_REQS_MASK)
#define | LCDIF_CTRL2_RSRVD5_MASK (0xFF000000U)
#define | LCDIF_CTRL2_RSRVD5_SHIFT (24U)
#define | LCDIF_CTRL2_RSRVD5(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD5_SHIFT)) & LCDIF_CTRL2_RSRVD5_MASK)

## CTRL2_SET - LCDIF General Control2 Register

#define | LCDIF_CTRL2_SET_RSRVD0_MASK (0xFFFU)
#define | LCDIF_CTRL2_SET_RSRVD0_SHIFT (0U)
#define | LCDIF_CTRL2_SET_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD0_SHIFT)) & LCDIF_CTRL2_SET_RSRVD0_MASK)
#define | LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_MASK (0x7000U)
#define | LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_SHIFT (12U)
#define | LCDIF_CTRL2_SET_EVEN_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_SET_RSRVD3_MASK (0x8000U)
#define | LCDIF_CTRL2_SET_RSRVD3_SHIFT (15U)
#define | LCDIF_CTRL2_SET_RSRVD3(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD3_SHIFT)) & LCDIF_CTRL2_SET_RSRVD3_MASK)
#define | LCDIF_CTRL2_SET_ODD_LINE_PATTERN_MASK (0x70000U)
#define | LCDIF_CTRL2_SET_ODD_LINE_PATTERN_SHIFT (16U)
#define | LCDIF_CTRL2_SET_ODD_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_SET_ODD_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_SET_RSRVD4_MASK (0x80000U)
#define | LCDIF_CTRL2_SET_RSRVD4_SHIFT (19U)
#define | LCDIF_CTRL2_SET_RSRVD4(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD4_SHIFT)) & LCDIF_CTRL2_SET_RSRVD4_MASK)
#define | LCDIF_CTRL2_SET_BURST_LEN_8_MASK (0x100000U)
#define | LCDIF_CTRL2_SET_BURST_LEN_8_SHIFT (20U)
#define | LCDIF_CTRL2_SET_BURST_LEN_8(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_SET_BURST_LEN_8_MASK)
#define | LCDIF_CTRL2_SET_OUTSTANDING_REQS_MASK (0xE00000U)
#define | LCDIF_CTRL2_SET_OUTSTANDING_REQS_SHIFT (21U)
#define | LCDIF_CTRL2_SET_OUTSTANDING_REQS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_SET_OUTSTANDING_REQS_MASK)
#define | LCDIF_CTRL2_SET_RSRVD5_MASK (0xFF000000U)
#define | LCDIF_CTRL2_SET_RSRVD5_SHIFT (24U)
#define | LCDIF_CTRL2_SET_RSRVD5(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD5_SHIFT)) & LCDIF_CTRL2_SET_RSRVD5_MASK)

## CTRL2_CLR - LCDIF General Control2 Register

#define | LCDIF_CTRL2_CLR_RSRVD0_MASK (0xFFFU)
#define | LCDIF_CTRL2_CLR_RSRVD0_SHIFT (0U)
#define | LCDIF_CTRL2_CLR_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD0_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD0_MASK)
#define | LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_MASK (0x7000U)
#define | LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_SHIFT (12U)
#define | LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_CLR_RSRVD3_MASK (0x8000U)
#define | LCDIF_CTRL2_CLR_RSRVD3_SHIFT (15U)
#define | LCDIF_CTRL2_CLR_RSRVD3(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD3_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD3_MASK)
#define | LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_MASK (0x70000U)
#define | LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_SHIFT (16U)
#define | LCDIF_CTRL2_CLR_ODD_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_CLR_RSRVD4_MASK (0x80000U)
#define | LCDIF_CTRL2_CLR_RSRVD4_SHIFT (19U)
#define | LCDIF_CTRL2_CLR_RSRVD4(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD4_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD4_MASK)
#define | LCDIF_CTRL2_CLR_BURST_LEN_8_MASK (0x100000U)
#define | LCDIF_CTRL2_CLR_BURST_LEN_8_SHIFT (20U)
#define | LCDIF_CTRL2_CLR_BURST_LEN_8(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_CLR_BURST_LEN_8_MASK)
#define | LCDIF_CTRL2_CLR_OUTSTANDING_REQS_MASK (0xE00000U)
#define | LCDIF_CTRL2_CLR_OUTSTANDING_REQS_SHIFT (21U)
#define | LCDIF_CTRL2_CLR_OUTSTANDING_REQS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_CLR_OUTSTANDING_REQS_MASK)
#define | LCDIF_CTRL2_CLR_RSRVD5_MASK (0xFF000000U)
#define | LCDIF_CTRL2_CLR_RSRVD5_SHIFT (24U)
#define | LCDIF_CTRL2_CLR_RSRVD5(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD5_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD5_MASK)

## CTRL2_TOG - LCDIF General Control2 Register

#define | LCDIF_CTRL2_TOG_RSRVD0_MASK (0xFFFU)
#define | LCDIF_CTRL2_TOG_RSRVD0_SHIFT (0U)
#define | LCDIF_CTRL2_TOG_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD0_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD0_MASK)
#define | LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_MASK (0x7000U)
#define | LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_SHIFT (12U)
#define | LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_TOG_RSRVD3_MASK (0x8000U)
#define | LCDIF_CTRL2_TOG_RSRVD3_SHIFT (15U)
#define | LCDIF_CTRL2_TOG_RSRVD3(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD3_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD3_MASK)
#define | LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_MASK (0x70000U)
#define | LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_SHIFT (16U)
#define | LCDIF_CTRL2_TOG_ODD_LINE_PATTERN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_MASK)
#define | LCDIF_CTRL2_TOG_RSRVD4_MASK (0x80000U)
#define | LCDIF_CTRL2_TOG_RSRVD4_SHIFT (19U)
#define | LCDIF_CTRL2_TOG_RSRVD4(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD4_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD4_MASK)
#define | LCDIF_CTRL2_TOG_BURST_LEN_8_MASK (0x100000U)
#define | LCDIF_CTRL2_TOG_BURST_LEN_8_SHIFT (20U)
#define | LCDIF_CTRL2_TOG_BURST_LEN_8(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_TOG_BURST_LEN_8_MASK)
#define | LCDIF_CTRL2_TOG_OUTSTANDING_REQS_MASK (0xE00000U)
#define | LCDIF_CTRL2_TOG_OUTSTANDING_REQS_SHIFT (21U)
#define | LCDIF_CTRL2_TOG_OUTSTANDING_REQS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_TOG_OUTSTANDING_REQS_MASK)
#define | LCDIF_CTRL2_TOG_RSRVD5_MASK (0xFF000000U)
#define | LCDIF_CTRL2_TOG_RSRVD5_SHIFT (24U)
#define | LCDIF_CTRL2_TOG_RSRVD5(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD5_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD5_MASK)

## TRANSFER_COUNT - LCDIF Horizontal and Vertical Valid Data Count Register

#define | LCDIF_TRANSFER_COUNT_H_COUNT_MASK (0xFFFFU)
#define | LCDIF_TRANSFER_COUNT_H_COUNT_SHIFT (0U)
#define | LCDIF_TRANSFER_COUNT_H_COUNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_TRANSFER_COUNT_H_COUNT_SHIFT)) & LCDIF_TRANSFER_COUNT_H_COUNT_MASK)
#define | LCDIF_TRANSFER_COUNT_V_COUNT_MASK (0xFFFF0000U)
#define | LCDIF_TRANSFER_COUNT_V_COUNT_SHIFT (16U)
#define | LCDIF_TRANSFER_COUNT_V_COUNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_TRANSFER_COUNT_V_COUNT_SHIFT)) & LCDIF_TRANSFER_COUNT_V_COUNT_MASK)

## CUR_BUF - LCD Interface Current Buffer Address Register

#define | LCDIF_CUR_BUF_ADDR_MASK (0xFFFFFFFFU)
#define | LCDIF_CUR_BUF_ADDR_SHIFT (0U)
#define | LCDIF_CUR_BUF_ADDR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CUR_BUF_ADDR_SHIFT)) & LCDIF_CUR_BUF_ADDR_MASK)

## NEXT_BUF - LCD Interface Next Buffer Address Register

#define | LCDIF_NEXT_BUF_ADDR_MASK (0xFFFFFFFFU)
#define | LCDIF_NEXT_BUF_ADDR_SHIFT (0U)
#define | LCDIF_NEXT_BUF_ADDR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_NEXT_BUF_ADDR_SHIFT)) & LCDIF_NEXT_BUF_ADDR_MASK)

## VDCTRL0 - LCDIF VSYNC Mode and Dotclk Mode Control Register0

#define | LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)
#define | LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_SHIFT (0U)
#define | LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_MASK)
#define | LCDIF_VDCTRL0_HALF_LINE_MODE_MASK (0x40000U)
#define | LCDIF_VDCTRL0_HALF_LINE_MODE_SHIFT (18U)
#define | LCDIF_VDCTRL0_HALF_LINE_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_HALF_LINE_MODE_MASK)
#define | LCDIF_VDCTRL0_HALF_LINE_MASK (0x80000U)
#define | LCDIF_VDCTRL0_HALF_LINE_SHIFT (19U)
#define | LCDIF_VDCTRL0_HALF_LINE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_HALF_LINE_MASK)
#define | LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)
#define | LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)
#define | LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_MASK)
#define | LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_MASK (0x200000U)
#define | LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_SHIFT (21U)
#define | LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_MASK)
#define | LCDIF_VDCTRL0_RSRVD1_MASK (0xC00000U)
#define | LCDIF_VDCTRL0_RSRVD1_SHIFT (22U)
#define | LCDIF_VDCTRL0_RSRVD1(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_RSRVD1_MASK)
#define | LCDIF_VDCTRL0_ENABLE_POL_MASK (0x1000000U)
#define | LCDIF_VDCTRL0_ENABLE_POL_SHIFT (24U)
#define | LCDIF_VDCTRL0_ENABLE_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_ENABLE_POL_MASK)
#define | LCDIF_VDCTRL0_DOTCLK_POL_MASK (0x2000000U)
#define | LCDIF_VDCTRL0_DOTCLK_POL_SHIFT (25U)
#define | LCDIF_VDCTRL0_DOTCLK_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_DOTCLK_POL_MASK)
#define | LCDIF_VDCTRL0_HSYNC_POL_MASK (0x4000000U)
#define | LCDIF_VDCTRL0_HSYNC_POL_SHIFT (26U)
#define | LCDIF_VDCTRL0_HSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_HSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_VSYNC_POL_MASK (0x8000000U)
#define | LCDIF_VDCTRL0_VSYNC_POL_SHIFT (27U)
#define | LCDIF_VDCTRL0_VSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_VSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_ENABLE_PRESENT_MASK (0x10000000U)
#define | LCDIF_VDCTRL0_ENABLE_PRESENT_SHIFT (28U)
#define | LCDIF_VDCTRL0_ENABLE_PRESENT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_ENABLE_PRESENT_MASK)
#define | LCDIF_VDCTRL0_RSRVD2_MASK (0xE0000000U)
#define | LCDIF_VDCTRL0_RSRVD2_SHIFT (29U)
#define | LCDIF_VDCTRL0_RSRVD2(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_RSRVD2_MASK)

## VDCTRL0_SET - LCDIF VSYNC Mode and Dotclk Mode Control Register0

#define | LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)
#define | LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_SHIFT (0U)
#define | LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_MASK)
#define | LCDIF_VDCTRL0_SET_HALF_LINE_MODE_MASK (0x40000U)
#define | LCDIF_VDCTRL0_SET_HALF_LINE_MODE_SHIFT (18U)
#define | LCDIF_VDCTRL0_SET_HALF_LINE_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_SET_HALF_LINE_MODE_MASK)
#define | LCDIF_VDCTRL0_SET_HALF_LINE_MASK (0x80000U)
#define | LCDIF_VDCTRL0_SET_HALF_LINE_SHIFT (19U)
#define | LCDIF_VDCTRL0_SET_HALF_LINE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_SET_HALF_LINE_MASK)
#define | LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)
#define | LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)
#define | LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_MASK)
#define | LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_MASK (0x200000U)
#define | LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_SHIFT (21U)
#define | LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_MASK)
#define | LCDIF_VDCTRL0_SET_RSRVD1_MASK (0xC00000U)
#define | LCDIF_VDCTRL0_SET_RSRVD1_SHIFT (22U)
#define | LCDIF_VDCTRL0_SET_RSRVD1(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_SET_RSRVD1_MASK)
#define | LCDIF_VDCTRL0_SET_ENABLE_POL_MASK (0x1000000U)
#define | LCDIF_VDCTRL0_SET_ENABLE_POL_SHIFT (24U)
#define | LCDIF_VDCTRL0_SET_ENABLE_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_SET_ENABLE_POL_MASK)
#define | LCDIF_VDCTRL0_SET_DOTCLK_POL_MASK (0x2000000U)
#define | LCDIF_VDCTRL0_SET_DOTCLK_POL_SHIFT (25U)
#define | LCDIF_VDCTRL0_SET_DOTCLK_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_SET_DOTCLK_POL_MASK)
#define | LCDIF_VDCTRL0_SET_HSYNC_POL_MASK (0x4000000U)
#define | LCDIF_VDCTRL0_SET_HSYNC_POL_SHIFT (26U)
#define | LCDIF_VDCTRL0_SET_HSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_SET_HSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_SET_VSYNC_POL_MASK (0x8000000U)
#define | LCDIF_VDCTRL0_SET_VSYNC_POL_SHIFT (27U)
#define | LCDIF_VDCTRL0_SET_VSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_SET_ENABLE_PRESENT_MASK (0x10000000U)
#define | LCDIF_VDCTRL0_SET_ENABLE_PRESENT_SHIFT (28U)
#define | LCDIF_VDCTRL0_SET_ENABLE_PRESENT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_SET_ENABLE_PRESENT_MASK)
#define | LCDIF_VDCTRL0_SET_RSRVD2_MASK (0xE0000000U)
#define | LCDIF_VDCTRL0_SET_RSRVD2_SHIFT (29U)
#define | LCDIF_VDCTRL0_SET_RSRVD2(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_SET_RSRVD2_MASK)

## VDCTRL0_CLR - LCDIF VSYNC Mode and Dotclk Mode Control Register0

#define | LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_SHIFT (0U)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_MASK)
#define | LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_MASK (0x40000U)
#define | LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_SHIFT (18U)
#define | LCDIF_VDCTRL0_CLR_HALF_LINE_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_MASK)
#define | LCDIF_VDCTRL0_CLR_HALF_LINE_MASK (0x80000U)
#define | LCDIF_VDCTRL0_CLR_HALF_LINE_SHIFT (19U)
#define | LCDIF_VDCTRL0_CLR_HALF_LINE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_CLR_HALF_LINE_MASK)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_MASK)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_MASK (0x200000U)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_SHIFT (21U)
#define | LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_MASK)
#define | LCDIF_VDCTRL0_CLR_RSRVD1_MASK (0xC00000U)
#define | LCDIF_VDCTRL0_CLR_RSRVD1_SHIFT (22U)
#define | LCDIF_VDCTRL0_CLR_RSRVD1(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_CLR_RSRVD1_MASK)
#define | LCDIF_VDCTRL0_CLR_ENABLE_POL_MASK (0x1000000U)
#define | LCDIF_VDCTRL0_CLR_ENABLE_POL_SHIFT (24U)
#define | LCDIF_VDCTRL0_CLR_ENABLE_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_ENABLE_POL_MASK)
#define | LCDIF_VDCTRL0_CLR_DOTCLK_POL_MASK (0x2000000U)
#define | LCDIF_VDCTRL0_CLR_DOTCLK_POL_SHIFT (25U)
#define | LCDIF_VDCTRL0_CLR_DOTCLK_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_DOTCLK_POL_MASK)
#define | LCDIF_VDCTRL0_CLR_HSYNC_POL_MASK (0x4000000U)
#define | LCDIF_VDCTRL0_CLR_HSYNC_POL_SHIFT (26U)
#define | LCDIF_VDCTRL0_CLR_HSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_HSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_CLR_VSYNC_POL_MASK (0x8000000U)
#define | LCDIF_VDCTRL0_CLR_VSYNC_POL_SHIFT (27U)
#define | LCDIF_VDCTRL0_CLR_VSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_MASK (0x10000000U)
#define | LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_SHIFT (28U)
#define | LCDIF_VDCTRL0_CLR_ENABLE_PRESENT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_MASK)
#define | LCDIF_VDCTRL0_CLR_RSRVD2_MASK (0xE0000000U)
#define | LCDIF_VDCTRL0_CLR_RSRVD2_SHIFT (29U)
#define | LCDIF_VDCTRL0_CLR_RSRVD2(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_CLR_RSRVD2_MASK)

## VDCTRL0_TOG - LCDIF VSYNC Mode and Dotclk Mode Control Register0

#define | LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_SHIFT (0U)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_MASK)
#define | LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_MASK (0x40000U)
#define | LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_SHIFT (18U)
#define | LCDIF_VDCTRL0_TOG_HALF_LINE_MODE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_MASK)
#define | LCDIF_VDCTRL0_TOG_HALF_LINE_MASK (0x80000U)
#define | LCDIF_VDCTRL0_TOG_HALF_LINE_SHIFT (19U)
#define | LCDIF_VDCTRL0_TOG_HALF_LINE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_TOG_HALF_LINE_MASK)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_MASK)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_MASK (0x200000U)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_SHIFT (21U)
#define | LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_MASK)
#define | LCDIF_VDCTRL0_TOG_RSRVD1_MASK (0xC00000U)
#define | LCDIF_VDCTRL0_TOG_RSRVD1_SHIFT (22U)
#define | LCDIF_VDCTRL0_TOG_RSRVD1(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_TOG_RSRVD1_MASK)
#define | LCDIF_VDCTRL0_TOG_ENABLE_POL_MASK (0x1000000U)
#define | LCDIF_VDCTRL0_TOG_ENABLE_POL_SHIFT (24U)
#define | LCDIF_VDCTRL0_TOG_ENABLE_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_ENABLE_POL_MASK)
#define | LCDIF_VDCTRL0_TOG_DOTCLK_POL_MASK (0x2000000U)
#define | LCDIF_VDCTRL0_TOG_DOTCLK_POL_SHIFT (25U)
#define | LCDIF_VDCTRL0_TOG_DOTCLK_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_DOTCLK_POL_MASK)
#define | LCDIF_VDCTRL0_TOG_HSYNC_POL_MASK (0x4000000U)
#define | LCDIF_VDCTRL0_TOG_HSYNC_POL_SHIFT (26U)
#define | LCDIF_VDCTRL0_TOG_HSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_HSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_TOG_VSYNC_POL_MASK (0x8000000U)
#define | LCDIF_VDCTRL0_TOG_VSYNC_POL_SHIFT (27U)
#define | LCDIF_VDCTRL0_TOG_VSYNC_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_POL_MASK)
#define | LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_MASK (0x10000000U)
#define | LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_SHIFT (28U)
#define | LCDIF_VDCTRL0_TOG_ENABLE_PRESENT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_MASK)
#define | LCDIF_VDCTRL0_TOG_RSRVD2_MASK (0xE0000000U)
#define | LCDIF_VDCTRL0_TOG_RSRVD2_SHIFT (29U)
#define | LCDIF_VDCTRL0_TOG_RSRVD2(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_TOG_RSRVD2_MASK)

## VDCTRL1 - LCDIF VSYNC Mode and Dotclk Mode Control Register1

#define | LCDIF_VDCTRL1_VSYNC_PERIOD_MASK (0xFFFFFFFFU)
#define | LCDIF_VDCTRL1_VSYNC_PERIOD_SHIFT (0U)
#define | LCDIF_VDCTRL1_VSYNC_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL1_VSYNC_PERIOD_SHIFT)) & LCDIF_VDCTRL1_VSYNC_PERIOD_MASK)

## VDCTRL2 - LCDIF VSYNC Mode and Dotclk Mode Control Register2

#define | LCDIF_VDCTRL2_HSYNC_PERIOD_MASK (0x3FFFFU)
#define | LCDIF_VDCTRL2_HSYNC_PERIOD_SHIFT (0U)
#define | LCDIF_VDCTRL2_HSYNC_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL2_HSYNC_PERIOD_SHIFT)) & LCDIF_VDCTRL2_HSYNC_PERIOD_MASK)
#define | LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_MASK (0xFFFC0000U)
#define | LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_SHIFT (18U)
#define | LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_MASK)

## VDCTRL3 - LCDIF VSYNC Mode and Dotclk Mode Control Register3

#define | LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_MASK (0xFFFFU)
#define | LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_SHIFT (0U)
#define | LCDIF_VDCTRL3_VERTICAL_WAIT_CNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_SHIFT)) & LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_MASK)
#define | LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_MASK (0xFFF0000U)
#define | LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_SHIFT (16U)
#define | LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_SHIFT)) & LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_MASK)
#define | LCDIF_VDCTRL3_VSYNC_ONLY_MASK (0x10000000U)
#define | LCDIF_VDCTRL3_VSYNC_ONLY_SHIFT (28U)
#define | LCDIF_VDCTRL3_VSYNC_ONLY(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_VSYNC_ONLY_SHIFT)) & LCDIF_VDCTRL3_VSYNC_ONLY_MASK)
#define | LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_MASK (0x20000000U)
#define | LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_SHIFT (29U)
#define | LCDIF_VDCTRL3_MUX_SYNC_SIGNALS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_SHIFT)) & LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_MASK)
#define | LCDIF_VDCTRL3_RSRVD0_MASK (0xC0000000U)
#define | LCDIF_VDCTRL3_RSRVD0_SHIFT (30U)
#define | LCDIF_VDCTRL3_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_RSRVD0_SHIFT)) & LCDIF_VDCTRL3_RSRVD0_MASK)

## VDCTRL4 - LCDIF VSYNC Mode and Dotclk Mode Control Register4

#define | LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_MASK (0x3FFFFU)
#define | LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_SHIFT (0U)
#define | LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_SHIFT)) & LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_MASK)
#define | LCDIF_VDCTRL4_SYNC_SIGNALS_ON_MASK (0x40000U)
#define | LCDIF_VDCTRL4_SYNC_SIGNALS_ON_SHIFT (18U)
#define | LCDIF_VDCTRL4_SYNC_SIGNALS_ON(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_SYNC_SIGNALS_ON_SHIFT)) & LCDIF_VDCTRL4_SYNC_SIGNALS_ON_MASK)
#define | LCDIF_VDCTRL4_RSRVD0_MASK (0x1FF80000U)
#define | LCDIF_VDCTRL4_RSRVD0_SHIFT (19U)
#define | LCDIF_VDCTRL4_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_RSRVD0_SHIFT)) & LCDIF_VDCTRL4_RSRVD0_MASK)
#define | LCDIF_VDCTRL4_DOTCLK_DLY_SEL_MASK (0xE0000000U)
#define | LCDIF_VDCTRL4_DOTCLK_DLY_SEL_SHIFT (29U)
#define | LCDIF_VDCTRL4_DOTCLK_DLY_SEL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_DOTCLK_DLY_SEL_SHIFT)) & LCDIF_VDCTRL4_DOTCLK_DLY_SEL_MASK)

## BM_ERROR_STAT - Bus Master Error Status Register

#define | LCDIF_BM_ERROR_STAT_ADDR_MASK (0xFFFFFFFFU)
#define | LCDIF_BM_ERROR_STAT_ADDR_SHIFT (0U)
#define | LCDIF_BM_ERROR_STAT_ADDR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_BM_ERROR_STAT_ADDR_SHIFT)) & LCDIF_BM_ERROR_STAT_ADDR_MASK)

## CRC_STAT - CRC Status Register

#define | LCDIF_CRC_STAT_CRC_VALUE_MASK (0xFFFFFFFFU)
#define | LCDIF_CRC_STAT_CRC_VALUE_SHIFT (0U)
#define | LCDIF_CRC_STAT_CRC_VALUE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_CRC_STAT_CRC_VALUE_SHIFT)) & LCDIF_CRC_STAT_CRC_VALUE_MASK)

## STAT - LCD Interface Status Register

#define | LCDIF_STAT_LFIFO_COUNT_MASK (0x1FFU)
#define | LCDIF_STAT_LFIFO_COUNT_SHIFT (0U)
#define | LCDIF_STAT_LFIFO_COUNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_LFIFO_COUNT_SHIFT)) & LCDIF_STAT_LFIFO_COUNT_MASK)
#define | LCDIF_STAT_RSRVD0_MASK (0x1FFFE00U)
#define | LCDIF_STAT_RSRVD0_SHIFT (9U)
#define | LCDIF_STAT_RSRVD0(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_RSRVD0_SHIFT)) & LCDIF_STAT_RSRVD0_MASK)
#define | LCDIF_STAT_TXFIFO_EMPTY_MASK (0x4000000U)
#define | LCDIF_STAT_TXFIFO_EMPTY_SHIFT (26U)
#define | LCDIF_STAT_TXFIFO_EMPTY(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_TXFIFO_EMPTY_SHIFT)) & LCDIF_STAT_TXFIFO_EMPTY_MASK)
#define | LCDIF_STAT_TXFIFO_FULL_MASK (0x8000000U)
#define | LCDIF_STAT_TXFIFO_FULL_SHIFT (27U)
#define | LCDIF_STAT_TXFIFO_FULL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_TXFIFO_FULL_SHIFT)) & LCDIF_STAT_TXFIFO_FULL_MASK)
#define | LCDIF_STAT_LFIFO_EMPTY_MASK (0x10000000U)
#define | LCDIF_STAT_LFIFO_EMPTY_SHIFT (28U)
#define | LCDIF_STAT_LFIFO_EMPTY(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_LFIFO_EMPTY_SHIFT)) & LCDIF_STAT_LFIFO_EMPTY_MASK)
#define | LCDIF_STAT_LFIFO_FULL_MASK (0x20000000U)
#define | LCDIF_STAT_LFIFO_FULL_SHIFT (29U)
#define | LCDIF_STAT_LFIFO_FULL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_LFIFO_FULL_SHIFT)) & LCDIF_STAT_LFIFO_FULL_MASK)
#define | LCDIF_STAT_DMA_REQ_MASK (0x40000000U)
#define | LCDIF_STAT_DMA_REQ_SHIFT (30U)
#define | LCDIF_STAT_DMA_REQ(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_DMA_REQ_SHIFT)) & LCDIF_STAT_DMA_REQ_MASK)
#define | LCDIF_STAT_PRESENT_MASK (0x80000000U)
#define | LCDIF_STAT_PRESENT_SHIFT (31U)
#define | LCDIF_STAT_PRESENT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_PRESENT_SHIFT)) & LCDIF_STAT_PRESENT_MASK)

## PIGEONCTRL0 - LCDIF Pigeon Mode Control0 Register

#define | LCDIF_PIGEONCTRL0_FD_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL0_FD_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL0_FD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_FD_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL0_LD_PERIOD_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL0_LD_PERIOD_SHIFT (16U)
#define | LCDIF_PIGEONCTRL0_LD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_LD_PERIOD_MASK)

## PIGEONCTRL0_SET - LCDIF Pigeon Mode Control0 Register

#define | LCDIF_PIGEONCTRL0_SET_FD_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL0_SET_FD_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL0_SET_FD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_SET_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_SET_FD_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL0_SET_LD_PERIOD_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL0_SET_LD_PERIOD_SHIFT (16U)
#define | LCDIF_PIGEONCTRL0_SET_LD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_SET_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_SET_LD_PERIOD_MASK)

## PIGEONCTRL0_CLR - LCDIF Pigeon Mode Control0 Register

#define | LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL0_CLR_FD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_SHIFT (16U)
#define | LCDIF_PIGEONCTRL0_CLR_LD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_MASK)

## PIGEONCTRL0_TOG - LCDIF Pigeon Mode Control0 Register

#define | LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL0_TOG_FD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_SHIFT (16U)
#define | LCDIF_PIGEONCTRL0_TOG_LD_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_MASK)

## PIGEONCTRL1 - LCDIF Pigeon Mode Control1 Register

#define | LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_SHIFT (16U)
#define | LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_MASK)

## PIGEONCTRL1_SET - LCDIF Pigeon Mode Control1 Register

#define | LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_SHIFT (16U)
#define | LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_MASK)

## PIGEONCTRL1_CLR - LCDIF Pigeon Mode Control1 Register

#define | LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_SHIFT (16U)
#define | LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_MASK)

## PIGEONCTRL1_TOG - LCDIF Pigeon Mode Control1 Register

#define | LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_MASK (0xFFFU)
#define | LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_SHIFT (0U)
#define | LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_MASK)
#define | LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_MASK (0xFFF0000U)
#define | LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_SHIFT (16U)
#define | LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_MASK)

## PIGEONCTRL2 - LCDIF Pigeon Mode Control2 Register

#define | LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_MASK (0x1U)
#define | LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_SHIFT (0U)
#define | LCDIF_PIGEONCTRL2_PIGEON_DATA_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_MASK)
#define | LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_MASK (0x2U)
#define | LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_SHIFT (1U)
#define | LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_MASK)

## PIGEONCTRL2_SET - LCDIF Pigeon Mode Control2 Register

#define | LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_MASK (0x1U)
#define | LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_SHIFT (0U)
#define | LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_MASK)
#define | LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_MASK (0x2U)
#define | LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_SHIFT (1U)
#define | LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_MASK)

## PIGEONCTRL2_CLR - LCDIF Pigeon Mode Control2 Register

#define | LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_MASK (0x1U)
#define | LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_SHIFT (0U)
#define | LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_MASK)
#define | LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_MASK (0x2U)
#define | LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_SHIFT (1U)
#define | LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_MASK)

## PIGEONCTRL2_TOG - LCDIF Pigeon Mode Control2 Register

#define | LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_MASK (0x1U)
#define | LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_SHIFT (0U)
#define | LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_MASK)
#define | LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_MASK (0x2U)
#define | LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_SHIFT (1U)
#define | LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_MASK)

## PIGEON_0 - Panel Interface Signal Generator Register

#define | LCDIF_PIGEON_0_EN_MASK (0x1U)
#define | LCDIF_PIGEON_0_EN_SHIFT (0U)
#define | LCDIF_PIGEON_0_EN(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_EN_SHIFT)) & LCDIF_PIGEON_0_EN_MASK)
#define | LCDIF_PIGEON_0_POL_MASK (0x2U)
#define | LCDIF_PIGEON_0_POL_SHIFT (1U)
#define | LCDIF_PIGEON_0_POL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_POL_SHIFT)) & LCDIF_PIGEON_0_POL_MASK)
#define | LCDIF_PIGEON_0_INC_SEL_MASK (0xCU)
#define | LCDIF_PIGEON_0_INC_SEL_SHIFT (2U)
#define | LCDIF_PIGEON_0_INC_SEL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_INC_SEL_SHIFT)) & LCDIF_PIGEON_0_INC_SEL_MASK)
#define | LCDIF_PIGEON_0_OFFSET_MASK (0xF0U)
#define | LCDIF_PIGEON_0_OFFSET_SHIFT (4U)
#define | LCDIF_PIGEON_0_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_OFFSET_SHIFT)) & LCDIF_PIGEON_0_OFFSET_MASK)
#define | LCDIF_PIGEON_0_MASK_CNT_SEL_MASK (0xF00U)
#define | LCDIF_PIGEON_0_MASK_CNT_SEL_SHIFT (8U)
#define | LCDIF_PIGEON_0_MASK_CNT_SEL(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_MASK_CNT_SEL_SHIFT)) & LCDIF_PIGEON_0_MASK_CNT_SEL_MASK)
#define | LCDIF_PIGEON_0_MASK_CNT_MASK (0xFFF000U)
#define | LCDIF_PIGEON_0_MASK_CNT_SHIFT (12U)
#define | LCDIF_PIGEON_0_MASK_CNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_MASK_CNT_SHIFT)) & LCDIF_PIGEON_0_MASK_CNT_MASK)
#define | LCDIF_PIGEON_0_STATE_MASK_MASK (0xFF000000U)
#define | LCDIF_PIGEON_0_STATE_MASK_SHIFT (24U)
#define | LCDIF_PIGEON_0_STATE_MASK(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_STATE_MASK_SHIFT)) & LCDIF_PIGEON_0_STATE_MASK_MASK)

## PIGEON_1 - Panel Interface Signal Generator Register

#define | LCDIF_PIGEON_1_SET_CNT_MASK (0xFFFFU)
#define | LCDIF_PIGEON_1_SET_CNT_SHIFT (0U)
#define | LCDIF_PIGEON_1_SET_CNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_1_SET_CNT_SHIFT)) & LCDIF_PIGEON_1_SET_CNT_MASK)
#define | LCDIF_PIGEON_1_CLR_CNT_MASK (0xFFFF0000U)
#define | LCDIF_PIGEON_1_CLR_CNT_SHIFT (16U)
#define | LCDIF_PIGEON_1_CLR_CNT(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_1_CLR_CNT_SHIFT)) & LCDIF_PIGEON_1_CLR_CNT_MASK)

## PIGEON_2 - Panel Interface Signal Generator Register

#define | LCDIF_PIGEON_2_SIG_LOGIC_MASK (0xFU)
#define | LCDIF_PIGEON_2_SIG_LOGIC_SHIFT (0U)
#define | LCDIF_PIGEON_2_SIG_LOGIC(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_2_SIG_LOGIC_SHIFT)) & LCDIF_PIGEON_2_SIG_LOGIC_MASK)
#define | LCDIF_PIGEON_2_SIG_ANOTHER_MASK (0x1F0U)
#define | LCDIF_PIGEON_2_SIG_ANOTHER_SHIFT (4U)
#define | LCDIF_PIGEON_2_SIG_ANOTHER(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_2_SIG_ANOTHER_SHIFT)) & LCDIF_PIGEON_2_SIG_ANOTHER_MASK)
#define | LCDIF_PIGEON_2_RSVD_MASK (0xFFFFFE00U)
#define | LCDIF_PIGEON_2_RSVD_SHIFT (9U)
#define | LCDIF_PIGEON_2_RSVD(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_2_RSVD_SHIFT)) & LCDIF_PIGEON_2_RSVD_MASK)

## LUT_CTRL - Lookup Table Data Register.

#define | LCDIF_LUT_CTRL_LUT_BYPASS_MASK (0x1U)
#define | LCDIF_LUT_CTRL_LUT_BYPASS_SHIFT (0U)
#define | LCDIF_LUT_CTRL_LUT_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT_CTRL_LUT_BYPASS_SHIFT)) & LCDIF_LUT_CTRL_LUT_BYPASS_MASK)

## LUT0_ADDR - Lookup Table Control Register.

#define | LCDIF_LUT0_ADDR_ADDR_MASK (0xFFU)
#define | LCDIF_LUT0_ADDR_ADDR_SHIFT (0U)
#define | LCDIF_LUT0_ADDR_ADDR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT0_ADDR_ADDR_SHIFT)) & LCDIF_LUT0_ADDR_ADDR_MASK)

## LUT0_DATA - Lookup Table Data Register.

#define | LCDIF_LUT0_DATA_DATA_MASK (0xFFFFFFFFU)
#define | LCDIF_LUT0_DATA_DATA_SHIFT (0U)
#define | LCDIF_LUT0_DATA_DATA(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT0_DATA_DATA_SHIFT)) & LCDIF_LUT0_DATA_DATA_MASK)

## LUT1_ADDR - Lookup Table Control Register.

#define | LCDIF_LUT1_ADDR_ADDR_MASK (0xFFU)
#define | LCDIF_LUT1_ADDR_ADDR_SHIFT (0U)
#define | LCDIF_LUT1_ADDR_ADDR(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT1_ADDR_ADDR_SHIFT)) & LCDIF_LUT1_ADDR_ADDR_MASK)

## LUT1_DATA - Lookup Table Data Register.

#define | LCDIF_LUT1_DATA_DATA_MASK (0xFFFFFFFFU)
#define | LCDIF_LUT1_DATA_DATA_SHIFT (0U)
#define | LCDIF_LUT1_DATA_DATA(x) (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT1_DATA_DATA_SHIFT)) & LCDIF_LUT1_DATA_DATA_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ LCDIF_BM_ERROR_STAT_ADDR

#define LCDIF_BM_ERROR_STAT_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_BM_ERROR_STAT_ADDR_SHIFT)) & LCDIF_BM_ERROR_STAT_ADDR_MASK)

Definition at line 26346 of file MIMXRT1062.h.

## ◆ LCDIF_BM_ERROR_STAT_ADDR_MASK

#define LCDIF_BM_ERROR_STAT_ADDR_MASK (0xFFFFFFFFU)

Definition at line 26344 of file MIMXRT1062.h.

## ◆ LCDIF_BM_ERROR_STAT_ADDR_SHIFT

#define LCDIF_BM_ERROR_STAT_ADDR_SHIFT (0U)

Definition at line 26345 of file MIMXRT1062.h.

## ◆ LCDIF_CRC_STAT_CRC_VALUE

#define LCDIF_CRC_STAT_CRC_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CRC_STAT_CRC_VALUE_SHIFT)) & LCDIF_CRC_STAT_CRC_VALUE_MASK)

Definition at line 26353 of file MIMXRT1062.h.

## ◆ LCDIF_CRC_STAT_CRC_VALUE_MASK

#define LCDIF_CRC_STAT_CRC_VALUE_MASK (0xFFFFFFFFU)

Definition at line 26351 of file MIMXRT1062.h.

## ◆ LCDIF_CRC_STAT_CRC_VALUE_SHIFT

#define LCDIF_CRC_STAT_CRC_VALUE_SHIFT (0U)

Definition at line 26352 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BM_ERROR_IRQ

#define LCDIF_CTRL1_BM_ERROR_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_BM_ERROR_IRQ_MASK)

BM_ERROR_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25647 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BM_ERROR_IRQ_EN

#define LCDIF_CTRL1_BM_ERROR_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_BM_ERROR_IRQ_EN_MASK)

Definition at line 25650 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BM_ERROR_IRQ_EN_MASK

#define LCDIF_CTRL1_BM_ERROR_IRQ_EN_MASK (0x4000000U)

Definition at line 25648 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BM_ERROR_IRQ_EN_SHIFT

#define LCDIF_CTRL1_BM_ERROR_IRQ_EN_SHIFT (26U)

Definition at line 25649 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BM_ERROR_IRQ_MASK

#define LCDIF_CTRL1_BM_ERROR_IRQ_MASK (0x2000000U)

Definition at line 25641 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BM_ERROR_IRQ_SHIFT

#define LCDIF_CTRL1_BM_ERROR_IRQ_SHIFT (25U)

Definition at line 25642 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BYTE_PACKING_FORMAT

#define LCDIF_CTRL1_BYTE_PACKING_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_BYTE_PACKING_FORMAT_MASK)

Definition at line 25625 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BYTE_PACKING_FORMAT_MASK

#define LCDIF_CTRL1_BYTE_PACKING_FORMAT_MASK (0xF0000U)

Definition at line 25623 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_BYTE_PACKING_FORMAT_SHIFT

#define LCDIF_CTRL1_BYTE_PACKING_FORMAT_SHIFT (16U)

Definition at line 25624 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BM_ERROR_IRQ

#define LCDIF_CTRL1_CLR_BM_ERROR_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_BM_ERROR_IRQ_MASK)

BM_ERROR_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25809 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN

#define LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_MASK)

Definition at line 25812 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_MASK

#define LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_MASK (0x4000000U)

Definition at line 25810 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_SHIFT

#define LCDIF_CTRL1_CLR_BM_ERROR_IRQ_EN_SHIFT (26U)

Definition at line 25811 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BM_ERROR_IRQ_MASK

#define LCDIF_CTRL1_CLR_BM_ERROR_IRQ_MASK (0x2000000U)

Definition at line 25803 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BM_ERROR_IRQ_SHIFT

#define LCDIF_CTRL1_CLR_BM_ERROR_IRQ_SHIFT (25U)

Definition at line 25804 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT

#define LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_MASK)

Definition at line 25787 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_MASK

#define LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_MASK (0xF0000U)

Definition at line 25785 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_SHIFT

#define LCDIF_CTRL1_CLR_BYTE_PACKING_FORMAT_SHIFT (16U)

Definition at line 25786 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CS_OUT_SELECT

#define LCDIF_CTRL1_CLR_CS_OUT_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_CLR_CS_OUT_SELECT_MASK)

Definition at line 25815 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CS_OUT_SELECT_MASK

#define LCDIF_CTRL1_CLR_CS_OUT_SELECT_MASK (0x40000000U)

Definition at line 25813 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CS_OUT_SELECT_SHIFT

#define LCDIF_CTRL1_CLR_CS_OUT_SELECT_SHIFT (30U)

Definition at line 25814 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ

#define LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_MASK)

CUR_FRAME_DONE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25758 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN

#define LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_MASK)

Definition at line 25778 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_MASK

#define LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)

Definition at line 25776 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)

Definition at line 25777 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_MASK

#define LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_MASK (0x200U)

Definition at line 25752 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_SHIFT

#define LCDIF_CTRL1_CLR_CUR_FRAME_DONE_IRQ_SHIFT (9U)

Definition at line 25753 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_FIFO_CLEAR

#define LCDIF_CTRL1_CLR_FIFO_CLEAR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_CLR_FIFO_CLEAR_MASK)

Definition at line 25793 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_FIFO_CLEAR_MASK

#define LCDIF_CTRL1_CLR_FIFO_CLEAR_MASK (0x200000U)

Definition at line 25791 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_FIFO_CLEAR_SHIFT

#define LCDIF_CTRL1_CLR_FIFO_CLEAR_SHIFT (21U)

Definition at line 25792 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT

#define LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_MASK)

Definition at line 25818 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_MASK

#define LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_MASK (0x80000000U)

Definition at line 25816 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_SHIFT

#define LCDIF_CTRL1_CLR_IMAGE_DATA_SELECT_SHIFT (31U)

Definition at line 25817 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_INTERLACE_FIELDS

#define LCDIF_CTRL1_CLR_INTERLACE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_CLR_INTERLACE_FIELDS_MASK)

Definition at line 25799 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_INTERLACE_FIELDS_MASK

#define LCDIF_CTRL1_CLR_INTERLACE_FIELDS_MASK (0x800000U)

Definition at line 25797 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_INTERLACE_FIELDS_SHIFT

#define LCDIF_CTRL1_CLR_INTERLACE_FIELDS_SHIFT (23U)

Definition at line 25798 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS

#define LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_MASK)

Definition at line 25790 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_MASK

#define LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)

Definition at line 25788 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_SHIFT

#define LCDIF_CTRL1_CLR_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)

Definition at line 25789 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_OVERFLOW_IRQ

#define LCDIF_CTRL1_CLR_OVERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_OVERFLOW_IRQ_MASK)

OVERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25772 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN

#define LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_MASK)

Definition at line 25784 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_MASK (0x8000U)

Definition at line 25782 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_CLR_OVERFLOW_IRQ_EN_SHIFT (15U)

Definition at line 25783 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_OVERFLOW_IRQ_MASK

#define LCDIF_CTRL1_CLR_OVERFLOW_IRQ_MASK (0x800U)

Definition at line 25766 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_OVERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_CLR_OVERFLOW_IRQ_SHIFT (11U)

Definition at line 25767 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW

#define LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_MASK)

Definition at line 25802 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_MASK

#define LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)

Definition at line 25800 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_SHIFT

#define LCDIF_CTRL1_CLR_RECOVER_ON_UNDERFLOW_SHIFT (24U)

Definition at line 25801 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_RSRVD0

#define LCDIF_CTRL1_CLR_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_RSRVD0_SHIFT)) & LCDIF_CTRL1_CLR_RSRVD0_MASK)

Definition at line 25744 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_RSRVD0_MASK

#define LCDIF_CTRL1_CLR_RSRVD0_MASK (0xF8U)

Definition at line 25742 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_RSRVD0_SHIFT

#define LCDIF_CTRL1_CLR_RSRVD0_SHIFT (3U)

Definition at line 25743 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD

#define LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_MASK)

Definition at line 25796 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_MASK

#define LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)

Definition at line 25794 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_SHIFT

#define LCDIF_CTRL1_CLR_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)

Definition at line 25795 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_UNDERFLOW_IRQ

#define LCDIF_CTRL1_CLR_UNDERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_MASK)

UNDERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25765 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN

#define LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_MASK)

Definition at line 25781 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_MASK (0x4000U)

Definition at line 25779 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_EN_SHIFT (14U)

Definition at line 25780 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_MASK

#define LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_MASK (0x400U)

Definition at line 25759 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_CLR_UNDERFLOW_IRQ_SHIFT (10U)

Definition at line 25760 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ

#define LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_MASK)

VSYNC_EDGE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25751 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN

#define LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_MASK)

Definition at line 25775 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_MASK

#define LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)

Definition at line 25773 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_EN_SHIFT (12U)

Definition at line 25774 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_MASK

#define LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_MASK (0x100U)

Definition at line 25745 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_SHIFT

#define LCDIF_CTRL1_CLR_VSYNC_EDGE_IRQ_SHIFT (8U)

Definition at line 25746 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CS_OUT_SELECT

#define LCDIF_CTRL1_CS_OUT_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_CS_OUT_SELECT_MASK)

Definition at line 25653 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CS_OUT_SELECT_MASK

#define LCDIF_CTRL1_CS_OUT_SELECT_MASK (0x40000000U)

Definition at line 25651 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CS_OUT_SELECT_SHIFT

#define LCDIF_CTRL1_CS_OUT_SELECT_SHIFT (30U)

Definition at line 25652 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CUR_FRAME_DONE_IRQ

#define LCDIF_CTRL1_CUR_FRAME_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_MASK)

CUR_FRAME_DONE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25596 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN

#define LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_MASK)

Definition at line 25616 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_MASK

#define LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)

Definition at line 25614 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)

Definition at line 25615 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_MASK

#define LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_MASK (0x200U)

Definition at line 25590 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_SHIFT

#define LCDIF_CTRL1_CUR_FRAME_DONE_IRQ_SHIFT (9U)

Definition at line 25591 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_FIFO_CLEAR

#define LCDIF_CTRL1_FIFO_CLEAR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_FIFO_CLEAR_MASK)

Definition at line 25631 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_FIFO_CLEAR_MASK

#define LCDIF_CTRL1_FIFO_CLEAR_MASK (0x200000U)

Definition at line 25629 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_FIFO_CLEAR_SHIFT

#define LCDIF_CTRL1_FIFO_CLEAR_SHIFT (21U)

Definition at line 25630 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_IMAGE_DATA_SELECT

#define LCDIF_CTRL1_IMAGE_DATA_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_IMAGE_DATA_SELECT_MASK)

Definition at line 25656 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_IMAGE_DATA_SELECT_MASK

#define LCDIF_CTRL1_IMAGE_DATA_SELECT_MASK (0x80000000U)

Definition at line 25654 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_IMAGE_DATA_SELECT_SHIFT

#define LCDIF_CTRL1_IMAGE_DATA_SELECT_SHIFT (31U)

Definition at line 25655 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_INTERLACE_FIELDS

#define LCDIF_CTRL1_INTERLACE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_INTERLACE_FIELDS_MASK)

Definition at line 25637 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_INTERLACE_FIELDS_MASK

#define LCDIF_CTRL1_INTERLACE_FIELDS_MASK (0x800000U)

Definition at line 25635 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_INTERLACE_FIELDS_SHIFT

#define LCDIF_CTRL1_INTERLACE_FIELDS_SHIFT (23U)

Definition at line 25636 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS

#define LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_MASK)

Definition at line 25628 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_MASK

#define LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)

Definition at line 25626 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_SHIFT

#define LCDIF_CTRL1_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)

Definition at line 25627 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_OVERFLOW_IRQ

#define LCDIF_CTRL1_OVERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_OVERFLOW_IRQ_MASK)

OVERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25610 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_OVERFLOW_IRQ_EN

#define LCDIF_CTRL1_OVERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_OVERFLOW_IRQ_EN_MASK)

Definition at line 25622 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_OVERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_OVERFLOW_IRQ_EN_MASK (0x8000U)

Definition at line 25620 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_OVERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_OVERFLOW_IRQ_EN_SHIFT (15U)

Definition at line 25621 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_OVERFLOW_IRQ_MASK

#define LCDIF_CTRL1_OVERFLOW_IRQ_MASK (0x800U)

Definition at line 25604 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_OVERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_OVERFLOW_IRQ_SHIFT (11U)

Definition at line 25605 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_RECOVER_ON_UNDERFLOW

#define LCDIF_CTRL1_RECOVER_ON_UNDERFLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_MASK)

Definition at line 25640 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_MASK

#define LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)

Definition at line 25638 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_SHIFT

#define LCDIF_CTRL1_RECOVER_ON_UNDERFLOW_SHIFT (24U)

Definition at line 25639 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_RSRVD0

#define LCDIF_CTRL1_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_RSRVD0_SHIFT)) & LCDIF_CTRL1_RSRVD0_MASK)

Definition at line 25582 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_RSRVD0_MASK

#define LCDIF_CTRL1_RSRVD0_MASK (0xF8U)

Definition at line 25580 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_RSRVD0_SHIFT

#define LCDIF_CTRL1_RSRVD0_SHIFT (3U)

Definition at line 25581 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BM_ERROR_IRQ

#define LCDIF_CTRL1_SET_BM_ERROR_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_SET_BM_ERROR_IRQ_MASK)

BM_ERROR_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25728 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN

#define LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_MASK)

Definition at line 25731 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_MASK

#define LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_MASK (0x4000000U)

Definition at line 25729 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_SHIFT

#define LCDIF_CTRL1_SET_BM_ERROR_IRQ_EN_SHIFT (26U)

Definition at line 25730 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BM_ERROR_IRQ_MASK

#define LCDIF_CTRL1_SET_BM_ERROR_IRQ_MASK (0x2000000U)

Definition at line 25722 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BM_ERROR_IRQ_SHIFT

#define LCDIF_CTRL1_SET_BM_ERROR_IRQ_SHIFT (25U)

Definition at line 25723 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT

#define LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_MASK)

Definition at line 25706 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_MASK

#define LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_MASK (0xF0000U)

Definition at line 25704 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_SHIFT

#define LCDIF_CTRL1_SET_BYTE_PACKING_FORMAT_SHIFT (16U)

Definition at line 25705 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CS_OUT_SELECT

#define LCDIF_CTRL1_SET_CS_OUT_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_SET_CS_OUT_SELECT_MASK)

Definition at line 25734 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CS_OUT_SELECT_MASK

#define LCDIF_CTRL1_SET_CS_OUT_SELECT_MASK (0x40000000U)

Definition at line 25732 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CS_OUT_SELECT_SHIFT

#define LCDIF_CTRL1_SET_CS_OUT_SELECT_SHIFT (30U)

Definition at line 25733 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ

#define LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_MASK)

CUR_FRAME_DONE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25677 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN

#define LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_MASK)

Definition at line 25697 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_MASK

#define LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)

Definition at line 25695 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)

Definition at line 25696 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_MASK

#define LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_MASK (0x200U)

Definition at line 25671 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_SHIFT

#define LCDIF_CTRL1_SET_CUR_FRAME_DONE_IRQ_SHIFT (9U)

Definition at line 25672 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_FIFO_CLEAR

#define LCDIF_CTRL1_SET_FIFO_CLEAR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_SET_FIFO_CLEAR_MASK)

Definition at line 25712 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_FIFO_CLEAR_MASK

#define LCDIF_CTRL1_SET_FIFO_CLEAR_MASK (0x200000U)

Definition at line 25710 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_FIFO_CLEAR_SHIFT

#define LCDIF_CTRL1_SET_FIFO_CLEAR_SHIFT (21U)

Definition at line 25711 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_IMAGE_DATA_SELECT

#define LCDIF_CTRL1_SET_IMAGE_DATA_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_MASK)

Definition at line 25737 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_MASK

#define LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_MASK (0x80000000U)

Definition at line 25735 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_SHIFT

#define LCDIF_CTRL1_SET_IMAGE_DATA_SELECT_SHIFT (31U)

Definition at line 25736 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_INTERLACE_FIELDS

#define LCDIF_CTRL1_SET_INTERLACE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_SET_INTERLACE_FIELDS_MASK)

Definition at line 25718 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_INTERLACE_FIELDS_MASK

#define LCDIF_CTRL1_SET_INTERLACE_FIELDS_MASK (0x800000U)

Definition at line 25716 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_INTERLACE_FIELDS_SHIFT

#define LCDIF_CTRL1_SET_INTERLACE_FIELDS_SHIFT (23U)

Definition at line 25717 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS

#define LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_MASK)

Definition at line 25709 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_MASK

#define LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)

Definition at line 25707 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_SHIFT

#define LCDIF_CTRL1_SET_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)

Definition at line 25708 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_OVERFLOW_IRQ

#define LCDIF_CTRL1_SET_OVERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_SET_OVERFLOW_IRQ_MASK)

OVERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25691 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN

#define LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_MASK)

Definition at line 25703 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_MASK (0x8000U)

Definition at line 25701 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_SET_OVERFLOW_IRQ_EN_SHIFT (15U)

Definition at line 25702 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_OVERFLOW_IRQ_MASK

#define LCDIF_CTRL1_SET_OVERFLOW_IRQ_MASK (0x800U)

Definition at line 25685 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_OVERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_SET_OVERFLOW_IRQ_SHIFT (11U)

Definition at line 25686 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW

#define LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_MASK)

Definition at line 25721 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_MASK

#define LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)

Definition at line 25719 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_SHIFT

#define LCDIF_CTRL1_SET_RECOVER_ON_UNDERFLOW_SHIFT (24U)

Definition at line 25720 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_RSRVD0

#define LCDIF_CTRL1_SET_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_RSRVD0_SHIFT)) & LCDIF_CTRL1_SET_RSRVD0_MASK)

Definition at line 25663 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_RSRVD0_MASK

#define LCDIF_CTRL1_SET_RSRVD0_MASK (0xF8U)

Definition at line 25661 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_RSRVD0_SHIFT

#define LCDIF_CTRL1_SET_RSRVD0_SHIFT (3U)

Definition at line 25662 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD

#define LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_MASK)

Definition at line 25715 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_MASK

#define LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)

Definition at line 25713 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_SHIFT

#define LCDIF_CTRL1_SET_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)

Definition at line 25714 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_UNDERFLOW_IRQ

#define LCDIF_CTRL1_SET_UNDERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_SET_UNDERFLOW_IRQ_MASK)

UNDERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25684 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN

#define LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_MASK)

Definition at line 25700 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_MASK (0x4000U)

Definition at line 25698 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_SET_UNDERFLOW_IRQ_EN_SHIFT (14U)

Definition at line 25699 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_UNDERFLOW_IRQ_MASK

#define LCDIF_CTRL1_SET_UNDERFLOW_IRQ_MASK (0x400U)

Definition at line 25678 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_UNDERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_SET_UNDERFLOW_IRQ_SHIFT (10U)

Definition at line 25679 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ

#define LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_MASK)

VSYNC_EDGE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25670 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN

#define LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_MASK)

Definition at line 25694 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_MASK

#define LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)

Definition at line 25692 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_EN_SHIFT (12U)

Definition at line 25693 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_MASK

#define LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_MASK (0x100U)

Definition at line 25664 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_SHIFT

#define LCDIF_CTRL1_SET_VSYNC_EDGE_IRQ_SHIFT (8U)

Definition at line 25665 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD

#define LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_MASK)

Definition at line 25634 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_MASK

#define LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)

Definition at line 25632 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_SHIFT

#define LCDIF_CTRL1_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)

Definition at line 25633 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BM_ERROR_IRQ

#define LCDIF_CTRL1_TOG_BM_ERROR_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_BM_ERROR_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_BM_ERROR_IRQ_MASK)

BM_ERROR_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25890 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN

#define LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_MASK)

Definition at line 25893 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_MASK

#define LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_MASK (0x4000000U)

Definition at line 25891 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_SHIFT

#define LCDIF_CTRL1_TOG_BM_ERROR_IRQ_EN_SHIFT (26U)

Definition at line 25892 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BM_ERROR_IRQ_MASK

#define LCDIF_CTRL1_TOG_BM_ERROR_IRQ_MASK (0x2000000U)

Definition at line 25884 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BM_ERROR_IRQ_SHIFT

#define LCDIF_CTRL1_TOG_BM_ERROR_IRQ_SHIFT (25U)

Definition at line 25885 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT

#define LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_SHIFT)) & LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_MASK)

Definition at line 25868 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_MASK

#define LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_MASK (0xF0000U)

Definition at line 25866 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_SHIFT

#define LCDIF_CTRL1_TOG_BYTE_PACKING_FORMAT_SHIFT (16U)

Definition at line 25867 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CS_OUT_SELECT

#define LCDIF_CTRL1_TOG_CS_OUT_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_CS_OUT_SELECT_SHIFT)) & LCDIF_CTRL1_TOG_CS_OUT_SELECT_MASK)

Definition at line 25896 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CS_OUT_SELECT_MASK

#define LCDIF_CTRL1_TOG_CS_OUT_SELECT_MASK (0x40000000U)

Definition at line 25894 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CS_OUT_SELECT_SHIFT

#define LCDIF_CTRL1_TOG_CS_OUT_SELECT_SHIFT (30U)

Definition at line 25895 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ

#define LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_MASK)

CUR_FRAME_DONE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25839 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN

#define LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_MASK)

Definition at line 25859 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_MASK

#define LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_MASK (0x2000U)

Definition at line 25857 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_EN_SHIFT (13U)

Definition at line 25858 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_MASK

#define LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_MASK (0x200U)

Definition at line 25833 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_SHIFT

#define LCDIF_CTRL1_TOG_CUR_FRAME_DONE_IRQ_SHIFT (9U)

Definition at line 25834 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_FIFO_CLEAR

#define LCDIF_CTRL1_TOG_FIFO_CLEAR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_FIFO_CLEAR_SHIFT)) & LCDIF_CTRL1_TOG_FIFO_CLEAR_MASK)

Definition at line 25874 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_FIFO_CLEAR_MASK

#define LCDIF_CTRL1_TOG_FIFO_CLEAR_MASK (0x200000U)

Definition at line 25872 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_FIFO_CLEAR_SHIFT

#define LCDIF_CTRL1_TOG_FIFO_CLEAR_SHIFT (21U)

Definition at line 25873 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT

#define LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_SHIFT)) & LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_MASK)

Definition at line 25899 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_MASK

#define LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_MASK (0x80000000U)

Definition at line 25897 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_SHIFT

#define LCDIF_CTRL1_TOG_IMAGE_DATA_SELECT_SHIFT (31U)

Definition at line 25898 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_INTERLACE_FIELDS

#define LCDIF_CTRL1_TOG_INTERLACE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_INTERLACE_FIELDS_SHIFT)) & LCDIF_CTRL1_TOG_INTERLACE_FIELDS_MASK)

Definition at line 25880 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_INTERLACE_FIELDS_MASK

#define LCDIF_CTRL1_TOG_INTERLACE_FIELDS_MASK (0x800000U)

Definition at line 25878 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_INTERLACE_FIELDS_SHIFT

#define LCDIF_CTRL1_TOG_INTERLACE_FIELDS_SHIFT (23U)

Definition at line 25879 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS

#define LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_SHIFT)) & LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_MASK)

Definition at line 25871 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_MASK

#define LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_MASK (0x100000U)

Definition at line 25869 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_SHIFT

#define LCDIF_CTRL1_TOG_IRQ_ON_ALTERNATE_FIELDS_SHIFT (20U)

Definition at line 25870 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_OVERFLOW_IRQ

#define LCDIF_CTRL1_TOG_OVERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_OVERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_OVERFLOW_IRQ_MASK)

OVERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25853 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN

#define LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_MASK)

Definition at line 25865 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_MASK (0x8000U)

Definition at line 25863 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_TOG_OVERFLOW_IRQ_EN_SHIFT (15U)

Definition at line 25864 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_OVERFLOW_IRQ_MASK

#define LCDIF_CTRL1_TOG_OVERFLOW_IRQ_MASK (0x800U)

Definition at line 25847 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_OVERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_TOG_OVERFLOW_IRQ_SHIFT (11U)

Definition at line 25848 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW

#define LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_SHIFT)) & LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_MASK)

Definition at line 25883 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_MASK

#define LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_MASK (0x1000000U)

Definition at line 25881 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_SHIFT

#define LCDIF_CTRL1_TOG_RECOVER_ON_UNDERFLOW_SHIFT (24U)

Definition at line 25882 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_RSRVD0

#define LCDIF_CTRL1_TOG_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_RSRVD0_SHIFT)) & LCDIF_CTRL1_TOG_RSRVD0_MASK)

Definition at line 25825 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_RSRVD0_MASK

#define LCDIF_CTRL1_TOG_RSRVD0_MASK (0xF8U)

Definition at line 25823 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_RSRVD0_SHIFT

#define LCDIF_CTRL1_TOG_RSRVD0_SHIFT (3U)

Definition at line 25824 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD

#define LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_SHIFT)) & LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_MASK)

Definition at line 25877 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_MASK

#define LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_MASK (0x400000U)

Definition at line 25875 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_SHIFT

#define LCDIF_CTRL1_TOG_START_INTERLACE_FROM_SECOND_FIELD_SHIFT (22U)

Definition at line 25876 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_UNDERFLOW_IRQ

#define LCDIF_CTRL1_TOG_UNDERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_MASK)

UNDERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25846 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN

#define LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_MASK)

Definition at line 25862 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_MASK (0x4000U)

Definition at line 25860 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_EN_SHIFT (14U)

Definition at line 25861 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_MASK

#define LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_MASK (0x400U)

Definition at line 25840 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_TOG_UNDERFLOW_IRQ_SHIFT (10U)

Definition at line 25841 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ

#define LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_MASK)

VSYNC_EDGE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25832 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN

#define LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_MASK)

Definition at line 25856 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_MASK

#define LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)

Definition at line 25854 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_EN_SHIFT (12U)

Definition at line 25855 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_MASK

#define LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_MASK (0x100U)

Definition at line 25826 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_SHIFT

#define LCDIF_CTRL1_TOG_VSYNC_EDGE_IRQ_SHIFT (8U)

Definition at line 25827 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_UNDERFLOW_IRQ

#define LCDIF_CTRL1_UNDERFLOW_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_UNDERFLOW_IRQ_SHIFT)) & LCDIF_CTRL1_UNDERFLOW_IRQ_MASK)

UNDERFLOW_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25603 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_UNDERFLOW_IRQ_EN

#define LCDIF_CTRL1_UNDERFLOW_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_UNDERFLOW_IRQ_EN_SHIFT)) & LCDIF_CTRL1_UNDERFLOW_IRQ_EN_MASK)

Definition at line 25619 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_UNDERFLOW_IRQ_EN_MASK

#define LCDIF_CTRL1_UNDERFLOW_IRQ_EN_MASK (0x4000U)

Definition at line 25617 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_UNDERFLOW_IRQ_EN_SHIFT

#define LCDIF_CTRL1_UNDERFLOW_IRQ_EN_SHIFT (14U)

Definition at line 25618 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_UNDERFLOW_IRQ_MASK

#define LCDIF_CTRL1_UNDERFLOW_IRQ_MASK (0x400U)

Definition at line 25597 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_UNDERFLOW_IRQ_SHIFT

#define LCDIF_CTRL1_UNDERFLOW_IRQ_SHIFT (10U)

Definition at line 25598 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_VSYNC_EDGE_IRQ

#define LCDIF_CTRL1_VSYNC_EDGE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_VSYNC_EDGE_IRQ_SHIFT)) & LCDIF_CTRL1_VSYNC_EDGE_IRQ_MASK)

VSYNC_EDGE_IRQ 0b0..No Interrupt Request Pending. 0b1..Interrupt Request Pending.

Definition at line 25589 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN

#define LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_SHIFT)) & LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_MASK)

Definition at line 25613 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_MASK

#define LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_MASK (0x1000U)

Definition at line 25611 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_SHIFT

#define LCDIF_CTRL1_VSYNC_EDGE_IRQ_EN_SHIFT (12U)

Definition at line 25612 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_VSYNC_EDGE_IRQ_MASK

#define LCDIF_CTRL1_VSYNC_EDGE_IRQ_MASK (0x100U)

Definition at line 25583 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL1_VSYNC_EDGE_IRQ_SHIFT

#define LCDIF_CTRL1_VSYNC_EDGE_IRQ_SHIFT (8U)

Definition at line 25584 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_BURST_LEN_8

#define LCDIF_CTRL2_BURST_LEN_8 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_BURST_LEN_8_MASK)

Definition at line 25937 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_BURST_LEN_8_MASK

#define LCDIF_CTRL2_BURST_LEN_8_MASK (0x100000U)

Definition at line 25935 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_BURST_LEN_8_SHIFT

#define LCDIF_CTRL2_BURST_LEN_8_SHIFT (20U)

Definition at line 25936 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_BURST_LEN_8

#define LCDIF_CTRL2_CLR_BURST_LEN_8 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_CLR_BURST_LEN_8_MASK)

Definition at line 26039 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_BURST_LEN_8_MASK

#define LCDIF_CTRL2_CLR_BURST_LEN_8_MASK (0x100000U)

Definition at line 26037 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_BURST_LEN_8_SHIFT

#define LCDIF_CTRL2_CLR_BURST_LEN_8_SHIFT (20U)

Definition at line 26038 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN

#define LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_MASK)

EVEN_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 26019 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_MASK

#define LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_MASK (0x7000U)

Definition at line 26009 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_CLR_EVEN_LINE_PATTERN_SHIFT (12U)

Definition at line 26010 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_ODD_LINE_PATTERN

#define LCDIF_CTRL2_CLR_ODD_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_MASK)

ODD_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 26033 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_MASK

#define LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_MASK (0x70000U)

Definition at line 26023 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_CLR_ODD_LINE_PATTERN_SHIFT (16U)

Definition at line 26024 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_OUTSTANDING_REQS

#define LCDIF_CTRL2_CLR_OUTSTANDING_REQS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_CLR_OUTSTANDING_REQS_MASK)

OUTSTANDING_REQS 0b000..REQ_1 0b001..REQ_2 0b010..REQ_4 0b011..REQ_8 0b100..REQ_16

Definition at line 26049 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_OUTSTANDING_REQS_MASK

#define LCDIF_CTRL2_CLR_OUTSTANDING_REQS_MASK (0xE00000U)

Definition at line 26040 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_OUTSTANDING_REQS_SHIFT

#define LCDIF_CTRL2_CLR_OUTSTANDING_REQS_SHIFT (21U)

Definition at line 26041 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD0

#define LCDIF_CTRL2_CLR_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD0_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD0_MASK)

Definition at line 26008 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD0_MASK

#define LCDIF_CTRL2_CLR_RSRVD0_MASK (0xFFFU)

Definition at line 26006 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD0_SHIFT

#define LCDIF_CTRL2_CLR_RSRVD0_SHIFT (0U)

Definition at line 26007 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD3

#define LCDIF_CTRL2_CLR_RSRVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD3_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD3_MASK)

Definition at line 26022 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD3_MASK

#define LCDIF_CTRL2_CLR_RSRVD3_MASK (0x8000U)

Definition at line 26020 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD3_SHIFT

#define LCDIF_CTRL2_CLR_RSRVD3_SHIFT (15U)

Definition at line 26021 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD4

#define LCDIF_CTRL2_CLR_RSRVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD4_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD4_MASK)

Definition at line 26036 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD4_MASK

#define LCDIF_CTRL2_CLR_RSRVD4_MASK (0x80000U)

Definition at line 26034 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD4_SHIFT

#define LCDIF_CTRL2_CLR_RSRVD4_SHIFT (19U)

Definition at line 26035 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD5

#define LCDIF_CTRL2_CLR_RSRVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_CLR_RSRVD5_SHIFT)) & LCDIF_CTRL2_CLR_RSRVD5_MASK)

Definition at line 26052 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD5_MASK

#define LCDIF_CTRL2_CLR_RSRVD5_MASK (0xFF000000U)

Definition at line 26050 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_CLR_RSRVD5_SHIFT

#define LCDIF_CTRL2_CLR_RSRVD5_SHIFT (24U)

Definition at line 26051 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_EVEN_LINE_PATTERN

#define LCDIF_CTRL2_EVEN_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_EVEN_LINE_PATTERN_MASK)

EVEN_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 25917 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_EVEN_LINE_PATTERN_MASK

#define LCDIF_CTRL2_EVEN_LINE_PATTERN_MASK (0x7000U)

Definition at line 25907 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_EVEN_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_EVEN_LINE_PATTERN_SHIFT (12U)

Definition at line 25908 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_ODD_LINE_PATTERN

#define LCDIF_CTRL2_ODD_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_ODD_LINE_PATTERN_MASK)

ODD_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 25931 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_ODD_LINE_PATTERN_MASK

#define LCDIF_CTRL2_ODD_LINE_PATTERN_MASK (0x70000U)

Definition at line 25921 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_ODD_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_ODD_LINE_PATTERN_SHIFT (16U)

Definition at line 25922 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_OUTSTANDING_REQS

#define LCDIF_CTRL2_OUTSTANDING_REQS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_OUTSTANDING_REQS_MASK)

OUTSTANDING_REQS 0b000..REQ_1 0b001..REQ_2 0b010..REQ_4 0b011..REQ_8 0b100..REQ_16

Definition at line 25947 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_OUTSTANDING_REQS_MASK

#define LCDIF_CTRL2_OUTSTANDING_REQS_MASK (0xE00000U)

Definition at line 25938 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_OUTSTANDING_REQS_SHIFT

#define LCDIF_CTRL2_OUTSTANDING_REQS_SHIFT (21U)

Definition at line 25939 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD0

#define LCDIF_CTRL2_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD0_SHIFT)) & LCDIF_CTRL2_RSRVD0_MASK)

Definition at line 25906 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD0_MASK

#define LCDIF_CTRL2_RSRVD0_MASK (0xFFFU)

Definition at line 25904 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD0_SHIFT

#define LCDIF_CTRL2_RSRVD0_SHIFT (0U)

Definition at line 25905 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD3

#define LCDIF_CTRL2_RSRVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD3_SHIFT)) & LCDIF_CTRL2_RSRVD3_MASK)

Definition at line 25920 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD3_MASK

#define LCDIF_CTRL2_RSRVD3_MASK (0x8000U)

Definition at line 25918 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD3_SHIFT

#define LCDIF_CTRL2_RSRVD3_SHIFT (15U)

Definition at line 25919 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD4

#define LCDIF_CTRL2_RSRVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD4_SHIFT)) & LCDIF_CTRL2_RSRVD4_MASK)

Definition at line 25934 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD4_MASK

#define LCDIF_CTRL2_RSRVD4_MASK (0x80000U)

Definition at line 25932 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD4_SHIFT

#define LCDIF_CTRL2_RSRVD4_SHIFT (19U)

Definition at line 25933 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD5

#define LCDIF_CTRL2_RSRVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_RSRVD5_SHIFT)) & LCDIF_CTRL2_RSRVD5_MASK)

Definition at line 25950 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD5_MASK

#define LCDIF_CTRL2_RSRVD5_MASK (0xFF000000U)

Definition at line 25948 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_RSRVD5_SHIFT

#define LCDIF_CTRL2_RSRVD5_SHIFT (24U)

Definition at line 25949 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_BURST_LEN_8

#define LCDIF_CTRL2_SET_BURST_LEN_8 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_SET_BURST_LEN_8_MASK)

Definition at line 25988 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_BURST_LEN_8_MASK

#define LCDIF_CTRL2_SET_BURST_LEN_8_MASK (0x100000U)

Definition at line 25986 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_BURST_LEN_8_SHIFT

#define LCDIF_CTRL2_SET_BURST_LEN_8_SHIFT (20U)

Definition at line 25987 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_EVEN_LINE_PATTERN

#define LCDIF_CTRL2_SET_EVEN_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_MASK)

EVEN_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 25968 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_MASK

#define LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_MASK (0x7000U)

Definition at line 25958 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_SET_EVEN_LINE_PATTERN_SHIFT (12U)

Definition at line 25959 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_ODD_LINE_PATTERN

#define LCDIF_CTRL2_SET_ODD_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_SET_ODD_LINE_PATTERN_MASK)

ODD_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 25982 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_ODD_LINE_PATTERN_MASK

#define LCDIF_CTRL2_SET_ODD_LINE_PATTERN_MASK (0x70000U)

Definition at line 25972 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_ODD_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_SET_ODD_LINE_PATTERN_SHIFT (16U)

Definition at line 25973 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_OUTSTANDING_REQS

#define LCDIF_CTRL2_SET_OUTSTANDING_REQS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_SET_OUTSTANDING_REQS_MASK)

OUTSTANDING_REQS 0b000..REQ_1 0b001..REQ_2 0b010..REQ_4 0b011..REQ_8 0b100..REQ_16

Definition at line 25998 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_OUTSTANDING_REQS_MASK

#define LCDIF_CTRL2_SET_OUTSTANDING_REQS_MASK (0xE00000U)

Definition at line 25989 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_OUTSTANDING_REQS_SHIFT

#define LCDIF_CTRL2_SET_OUTSTANDING_REQS_SHIFT (21U)

Definition at line 25990 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD0

#define LCDIF_CTRL2_SET_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD0_SHIFT)) & LCDIF_CTRL2_SET_RSRVD0_MASK)

Definition at line 25957 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD0_MASK

#define LCDIF_CTRL2_SET_RSRVD0_MASK (0xFFFU)

Definition at line 25955 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD0_SHIFT

#define LCDIF_CTRL2_SET_RSRVD0_SHIFT (0U)

Definition at line 25956 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD3

#define LCDIF_CTRL2_SET_RSRVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD3_SHIFT)) & LCDIF_CTRL2_SET_RSRVD3_MASK)

Definition at line 25971 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD3_MASK

#define LCDIF_CTRL2_SET_RSRVD3_MASK (0x8000U)

Definition at line 25969 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD3_SHIFT

#define LCDIF_CTRL2_SET_RSRVD3_SHIFT (15U)

Definition at line 25970 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD4

#define LCDIF_CTRL2_SET_RSRVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD4_SHIFT)) & LCDIF_CTRL2_SET_RSRVD4_MASK)

Definition at line 25985 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD4_MASK

#define LCDIF_CTRL2_SET_RSRVD4_MASK (0x80000U)

Definition at line 25983 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD4_SHIFT

#define LCDIF_CTRL2_SET_RSRVD4_SHIFT (19U)

Definition at line 25984 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD5

#define LCDIF_CTRL2_SET_RSRVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_SET_RSRVD5_SHIFT)) & LCDIF_CTRL2_SET_RSRVD5_MASK)

Definition at line 26001 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD5_MASK

#define LCDIF_CTRL2_SET_RSRVD5_MASK (0xFF000000U)

Definition at line 25999 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_SET_RSRVD5_SHIFT

#define LCDIF_CTRL2_SET_RSRVD5_SHIFT (24U)

Definition at line 26000 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_BURST_LEN_8

#define LCDIF_CTRL2_TOG_BURST_LEN_8 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_BURST_LEN_8_SHIFT)) & LCDIF_CTRL2_TOG_BURST_LEN_8_MASK)

Definition at line 26090 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_BURST_LEN_8_MASK

#define LCDIF_CTRL2_TOG_BURST_LEN_8_MASK (0x100000U)

Definition at line 26088 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_BURST_LEN_8_SHIFT

#define LCDIF_CTRL2_TOG_BURST_LEN_8_SHIFT (20U)

Definition at line 26089 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN

#define LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_MASK)

EVEN_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 26070 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_MASK

#define LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_MASK (0x7000U)

Definition at line 26060 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_TOG_EVEN_LINE_PATTERN_SHIFT (12U)

Definition at line 26061 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_ODD_LINE_PATTERN

#define LCDIF_CTRL2_TOG_ODD_LINE_PATTERN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_SHIFT)) & LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_MASK)

ODD_LINE_PATTERN 0b000..RGB 0b001..RBG 0b010..GBR 0b011..GRB 0b100..BRG 0b101..BGR

Definition at line 26084 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_MASK

#define LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_MASK (0x70000U)

Definition at line 26074 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_SHIFT

#define LCDIF_CTRL2_TOG_ODD_LINE_PATTERN_SHIFT (16U)

Definition at line 26075 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_OUTSTANDING_REQS

#define LCDIF_CTRL2_TOG_OUTSTANDING_REQS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_OUTSTANDING_REQS_SHIFT)) & LCDIF_CTRL2_TOG_OUTSTANDING_REQS_MASK)

OUTSTANDING_REQS 0b000..REQ_1 0b001..REQ_2 0b010..REQ_4 0b011..REQ_8 0b100..REQ_16

Definition at line 26100 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_OUTSTANDING_REQS_MASK

#define LCDIF_CTRL2_TOG_OUTSTANDING_REQS_MASK (0xE00000U)

Definition at line 26091 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_OUTSTANDING_REQS_SHIFT

#define LCDIF_CTRL2_TOG_OUTSTANDING_REQS_SHIFT (21U)

Definition at line 26092 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD0

#define LCDIF_CTRL2_TOG_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD0_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD0_MASK)

Definition at line 26059 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD0_MASK

#define LCDIF_CTRL2_TOG_RSRVD0_MASK (0xFFFU)

Definition at line 26057 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD0_SHIFT

#define LCDIF_CTRL2_TOG_RSRVD0_SHIFT (0U)

Definition at line 26058 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD3

#define LCDIF_CTRL2_TOG_RSRVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD3_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD3_MASK)

Definition at line 26073 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD3_MASK

#define LCDIF_CTRL2_TOG_RSRVD3_MASK (0x8000U)

Definition at line 26071 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD3_SHIFT

#define LCDIF_CTRL2_TOG_RSRVD3_SHIFT (15U)

Definition at line 26072 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD4

#define LCDIF_CTRL2_TOG_RSRVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD4_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD4_MASK)

Definition at line 26087 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD4_MASK

#define LCDIF_CTRL2_TOG_RSRVD4_MASK (0x80000U)

Definition at line 26085 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD4_SHIFT

#define LCDIF_CTRL2_TOG_RSRVD4_SHIFT (19U)

Definition at line 26086 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD5

#define LCDIF_CTRL2_TOG_RSRVD5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL2_TOG_RSRVD5_SHIFT)) & LCDIF_CTRL2_TOG_RSRVD5_MASK)

Definition at line 26103 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD5_MASK

#define LCDIF_CTRL2_TOG_RSRVD5_MASK (0xFF000000U)

Definition at line 26101 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL2_TOG_RSRVD5_SHIFT

#define LCDIF_CTRL2_TOG_RSRVD5_SHIFT (24U)

Definition at line 26102 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_BYPASS_COUNT

#define LCDIF_CTRL_BYPASS_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_BYPASS_COUNT_MASK)

Definition at line 25271 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_BYPASS_COUNT_MASK

#define LCDIF_CTRL_BYPASS_COUNT_MASK (0x80000U)

Definition at line 25269 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_BYPASS_COUNT_SHIFT

#define LCDIF_CTRL_BYPASS_COUNT_SHIFT (19U)

Definition at line 25270 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLKGATE

#define LCDIF_CTRL_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLKGATE_SHIFT)) & LCDIF_CTRL_CLKGATE_MASK)

Definition at line 25284 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLKGATE_MASK

#define LCDIF_CTRL_CLKGATE_MASK (0x40000000U)

Definition at line 25282 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLKGATE_SHIFT

#define LCDIF_CTRL_CLKGATE_SHIFT (30U)

Definition at line 25283 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_BYPASS_COUNT

#define LCDIF_CTRL_CLR_BYPASS_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_CLR_BYPASS_COUNT_MASK)

Definition at line 25463 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_BYPASS_COUNT_MASK

#define LCDIF_CTRL_CLR_BYPASS_COUNT_MASK (0x80000U)

Definition at line 25461 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_BYPASS_COUNT_SHIFT

#define LCDIF_CTRL_CLR_BYPASS_COUNT_SHIFT (19U)

Definition at line 25462 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_CLKGATE

#define LCDIF_CTRL_CLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_CLKGATE_SHIFT)) & LCDIF_CTRL_CLR_CLKGATE_MASK)

Definition at line 25476 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_CLKGATE_MASK

#define LCDIF_CTRL_CLR_CLKGATE_MASK (0x40000000U)

Definition at line 25474 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_CLKGATE_SHIFT

#define LCDIF_CTRL_CLR_CLKGATE_SHIFT (30U)

Definition at line 25475 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE

#define LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_MASK)

CSC_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25446 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_MASK (0x3000U)

Definition at line 25436 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_CLR_CSC_DATA_SWIZZLE_SHIFT (12U)

Definition at line 25437 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT

#define LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_MASK)

Definition at line 25408 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_MASK

#define LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_MASK (0x8U)

Definition at line 25406 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_SHIFT

#define LCDIF_CTRL_CLR_DATA_FORMAT_16_BIT_SHIFT (3U)

Definition at line 25407 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT

#define LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_MASK)

DATA_FORMAT_18_BIT 0b0..Data input to the block is in 18 bpp format, such that lower 18 bits contain RGB 666 and upper 14 bits do not contain any useful data. 0b1..Data input to the block is in 18 bpp format, such that upper 18 bits contain RGB 666 and lower 14 bits do not contain any useful data.

Definition at line 25405 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_MASK

#define LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_MASK (0x4U)

Definition at line 25399 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_SHIFT

#define LCDIF_CTRL_CLR_DATA_FORMAT_18_BIT_SHIFT (2U)

Definition at line 25400 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT

#define LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_MASK)

DATA_FORMAT_24_BIT 0b0..Data input to the block is in 24 bpp format, such that all RGB 888 data is contained in 24 bits. 0b1..Data input to the block is actually RGB 18 bpp, but there is 1 color per byte, hence the upper 2 bits in each byte do not contain any useful data, and should be dropped.

Definition at line 25398 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_MASK

#define LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_MASK (0x2U)

Definition at line 25391 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_SHIFT

#define LCDIF_CTRL_CLR_DATA_FORMAT_24_BIT_SHIFT (1U)

Definition at line 25392 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_SHIFT_DIR

#define LCDIF_CTRL_CLR_DATA_SHIFT_DIR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_CLR_DATA_SHIFT_DIR_MASK)

DATA_SHIFT_DIR 0b0..Data to be transmitted is shifted LEFT by SHIFT_NUM_BITS bits. 0b1..Data to be transmitted is shifted RIGHT by SHIFT_NUM_BITS bits.

Definition at line 25473 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_SHIFT_DIR_MASK

#define LCDIF_CTRL_CLR_DATA_SHIFT_DIR_MASK (0x4000000U)

Definition at line 25467 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DATA_SHIFT_DIR_SHIFT

#define LCDIF_CTRL_CLR_DATA_SHIFT_DIR_SHIFT (26U)

Definition at line 25468 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DOTCLK_MODE

#define LCDIF_CTRL_CLR_DOTCLK_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_CLR_DOTCLK_MODE_MASK)

Definition at line 25460 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DOTCLK_MODE_MASK

#define LCDIF_CTRL_CLR_DOTCLK_MODE_MASK (0x20000U)

Definition at line 25458 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_DOTCLK_MODE_SHIFT

#define LCDIF_CTRL_CLR_DOTCLK_MODE_SHIFT (17U)

Definition at line 25459 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE

#define LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_MASK)

Definition at line 25417 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_MASK

#define LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_MASK (0x40U)

Definition at line 25415 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_SHIFT

#define LCDIF_CTRL_CLR_ENABLE_PXP_HANDSHAKE_SHIFT (6U)

Definition at line 25416 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE

#define LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_MASK)

INPUT_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25457 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_MASK (0xC000U)

Definition at line 25447 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_CLR_INPUT_DATA_SWIZZLE_SHIFT (14U)

Definition at line 25448 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH

#define LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_MASK)

LCD_DATABUS_WIDTH 0b00..16-bit data bus mode. 0b01..8-bit data bus mode. 0b10..18-bit data bus mode. 0b11..24-bit data bus mode.

Definition at line 25435 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_MASK

#define LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_MASK (0xC00U)

Definition at line 25427 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_SHIFT

#define LCDIF_CTRL_CLR_LCD_DATABUS_WIDTH_SHIFT (10U)

Definition at line 25428 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_MASTER

#define LCDIF_CTRL_CLR_MASTER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_MASTER_SHIFT)) & LCDIF_CTRL_CLR_MASTER_MASK)

Definition at line 25414 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_MASTER_MASK

#define LCDIF_CTRL_CLR_MASTER_MASK (0x20U)

Definition at line 25412 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_MASTER_SHIFT

#define LCDIF_CTRL_CLR_MASTER_SHIFT (5U)

Definition at line 25413 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_RSRVD0

#define LCDIF_CTRL_CLR_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_RSRVD0_SHIFT)) & LCDIF_CTRL_CLR_RSRVD0_MASK)

Definition at line 25411 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_RSRVD0_MASK

#define LCDIF_CTRL_CLR_RSRVD0_MASK (0x10U)

Definition at line 25409 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_RSRVD0_SHIFT

#define LCDIF_CTRL_CLR_RSRVD0_SHIFT (4U)

Definition at line 25410 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_RUN

#define LCDIF_CTRL_CLR_RUN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_RUN_SHIFT)) & LCDIF_CTRL_CLR_RUN_MASK)

Definition at line 25390 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_RUN_MASK

#define LCDIF_CTRL_CLR_RUN_MASK (0x1U)

Definition at line 25388 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_RUN_SHIFT

#define LCDIF_CTRL_CLR_RUN_SHIFT (0U)

Definition at line 25389 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_SFTRST

#define LCDIF_CTRL_CLR_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_SFTRST_SHIFT)) & LCDIF_CTRL_CLR_SFTRST_MASK)

Definition at line 25479 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_SFTRST_MASK

#define LCDIF_CTRL_CLR_SFTRST_MASK (0x80000000U)

Definition at line 25477 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_SFTRST_SHIFT

#define LCDIF_CTRL_CLR_SFTRST_SHIFT (31U)

Definition at line 25478 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_SHIFT_NUM_BITS

#define LCDIF_CTRL_CLR_SHIFT_NUM_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_CLR_SHIFT_NUM_BITS_MASK)

Definition at line 25466 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_SHIFT_NUM_BITS_MASK

#define LCDIF_CTRL_CLR_SHIFT_NUM_BITS_MASK (0x3E00000U)

Definition at line 25464 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_SHIFT_NUM_BITS_SHIFT

#define LCDIF_CTRL_CLR_SHIFT_NUM_BITS_SHIFT (21U)

Definition at line 25465 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_WORD_LENGTH

#define LCDIF_CTRL_CLR_WORD_LENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CLR_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_CLR_WORD_LENGTH_MASK)

WORD_LENGTH 0b00..Input data is 16 bits per pixel. 0b01..Input data is 8 bits wide. 0b10..Input data is 18 bits per pixel. 0b11..Input data is 24 bits per pixel.

Definition at line 25426 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_WORD_LENGTH_MASK

#define LCDIF_CTRL_CLR_WORD_LENGTH_MASK (0x300U)

Definition at line 25418 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CLR_WORD_LENGTH_SHIFT

#define LCDIF_CTRL_CLR_WORD_LENGTH_SHIFT (8U)

Definition at line 25419 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CSC_DATA_SWIZZLE

#define LCDIF_CTRL_CSC_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_CSC_DATA_SWIZZLE_MASK)

CSC_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25254 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CSC_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_CSC_DATA_SWIZZLE_MASK (0x3000U)

Definition at line 25244 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_CSC_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_CSC_DATA_SWIZZLE_SHIFT (12U)

Definition at line 25245 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_16_BIT

#define LCDIF_CTRL_DATA_FORMAT_16_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_DATA_FORMAT_16_BIT_MASK)

Definition at line 25216 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_16_BIT_MASK

#define LCDIF_CTRL_DATA_FORMAT_16_BIT_MASK (0x8U)

Definition at line 25214 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_16_BIT_SHIFT

#define LCDIF_CTRL_DATA_FORMAT_16_BIT_SHIFT (3U)

Definition at line 25215 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_18_BIT

#define LCDIF_CTRL_DATA_FORMAT_18_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_DATA_FORMAT_18_BIT_MASK)

DATA_FORMAT_18_BIT 0b0..Data input to the block is in 18 bpp format, such that lower 18 bits contain RGB 666 and upper 14 bits do not contain any useful data. 0b1..Data input to the block is in 18 bpp format, such that upper 18 bits contain RGB 666 and lower 14 bits do not contain any useful data.

Definition at line 25213 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_18_BIT_MASK

#define LCDIF_CTRL_DATA_FORMAT_18_BIT_MASK (0x4U)

Definition at line 25207 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_18_BIT_SHIFT

#define LCDIF_CTRL_DATA_FORMAT_18_BIT_SHIFT (2U)

Definition at line 25208 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_24_BIT

#define LCDIF_CTRL_DATA_FORMAT_24_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_DATA_FORMAT_24_BIT_MASK)

DATA_FORMAT_24_BIT 0b0..Data input to the block is in 24 bpp format, such that all RGB 888 data is contained in 24 bits. 0b1..Data input to the block is actually RGB 18 bpp, but there is 1 color per byte, hence the upper 2 bits in each byte do not contain any useful data, and should be dropped.

Definition at line 25206 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_24_BIT_MASK

#define LCDIF_CTRL_DATA_FORMAT_24_BIT_MASK (0x2U)

Definition at line 25199 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_FORMAT_24_BIT_SHIFT

#define LCDIF_CTRL_DATA_FORMAT_24_BIT_SHIFT (1U)

Definition at line 25200 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_SHIFT_DIR

#define LCDIF_CTRL_DATA_SHIFT_DIR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_DATA_SHIFT_DIR_MASK)

DATA_SHIFT_DIR 0b0..Data to be transmitted is shifted LEFT by SHIFT_NUM_BITS bits. 0b1..Data to be transmitted is shifted RIGHT by SHIFT_NUM_BITS bits.

Definition at line 25281 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_SHIFT_DIR_MASK

#define LCDIF_CTRL_DATA_SHIFT_DIR_MASK (0x4000000U)

Definition at line 25275 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DATA_SHIFT_DIR_SHIFT

#define LCDIF_CTRL_DATA_SHIFT_DIR_SHIFT (26U)

Definition at line 25276 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DOTCLK_MODE

#define LCDIF_CTRL_DOTCLK_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_DOTCLK_MODE_MASK)

Definition at line 25268 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DOTCLK_MODE_MASK

#define LCDIF_CTRL_DOTCLK_MODE_MASK (0x20000U)

Definition at line 25266 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_DOTCLK_MODE_SHIFT

#define LCDIF_CTRL_DOTCLK_MODE_SHIFT (17U)

Definition at line 25267 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_ENABLE_PXP_HANDSHAKE

#define LCDIF_CTRL_ENABLE_PXP_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_MASK)

Definition at line 25225 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_MASK

#define LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_MASK (0x40U)

Definition at line 25223 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_SHIFT

#define LCDIF_CTRL_ENABLE_PXP_HANDSHAKE_SHIFT (6U)

Definition at line 25224 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_INPUT_DATA_SWIZZLE

#define LCDIF_CTRL_INPUT_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_INPUT_DATA_SWIZZLE_MASK)

INPUT_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25265 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_INPUT_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_INPUT_DATA_SWIZZLE_MASK (0xC000U)

Definition at line 25255 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_INPUT_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_INPUT_DATA_SWIZZLE_SHIFT (14U)

Definition at line 25256 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_LCD_DATABUS_WIDTH

#define LCDIF_CTRL_LCD_DATABUS_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_LCD_DATABUS_WIDTH_MASK)

LCD_DATABUS_WIDTH 0b00..16-bit data bus mode. 0b01..8-bit data bus mode. 0b10..18-bit data bus mode. 0b11..24-bit data bus mode.

Definition at line 25243 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_LCD_DATABUS_WIDTH_MASK

#define LCDIF_CTRL_LCD_DATABUS_WIDTH_MASK (0xC00U)

Definition at line 25235 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_LCD_DATABUS_WIDTH_SHIFT

#define LCDIF_CTRL_LCD_DATABUS_WIDTH_SHIFT (10U)

Definition at line 25236 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_MASTER

#define LCDIF_CTRL_MASTER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_MASTER_SHIFT)) & LCDIF_CTRL_MASTER_MASK)

Definition at line 25222 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_MASTER_MASK

#define LCDIF_CTRL_MASTER_MASK (0x20U)

Definition at line 25220 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_MASTER_SHIFT

#define LCDIF_CTRL_MASTER_SHIFT (5U)

Definition at line 25221 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_RSRVD0

#define LCDIF_CTRL_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_RSRVD0_SHIFT)) & LCDIF_CTRL_RSRVD0_MASK)

Definition at line 25219 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_RSRVD0_MASK

#define LCDIF_CTRL_RSRVD0_MASK (0x10U)

Definition at line 25217 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_RSRVD0_SHIFT

#define LCDIF_CTRL_RSRVD0_SHIFT (4U)

Definition at line 25218 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_RUN

#define LCDIF_CTRL_RUN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_RUN_SHIFT)) & LCDIF_CTRL_RUN_MASK)

Definition at line 25198 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_RUN_MASK

#define LCDIF_CTRL_RUN_MASK (0x1U)

Definition at line 25196 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_RUN_SHIFT

#define LCDIF_CTRL_RUN_SHIFT (0U)

Definition at line 25197 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_BYPASS_COUNT

#define LCDIF_CTRL_SET_BYPASS_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_SET_BYPASS_COUNT_MASK)

Definition at line 25367 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_BYPASS_COUNT_MASK

#define LCDIF_CTRL_SET_BYPASS_COUNT_MASK (0x80000U)

Definition at line 25365 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_BYPASS_COUNT_SHIFT

#define LCDIF_CTRL_SET_BYPASS_COUNT_SHIFT (19U)

Definition at line 25366 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_CLKGATE

#define LCDIF_CTRL_SET_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_CLKGATE_SHIFT)) & LCDIF_CTRL_SET_CLKGATE_MASK)

Definition at line 25380 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_CLKGATE_MASK

#define LCDIF_CTRL_SET_CLKGATE_MASK (0x40000000U)

Definition at line 25378 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_CLKGATE_SHIFT

#define LCDIF_CTRL_SET_CLKGATE_SHIFT (30U)

Definition at line 25379 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_CSC_DATA_SWIZZLE

#define LCDIF_CTRL_SET_CSC_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_MASK)

CSC_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25350 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_MASK (0x3000U)

Definition at line 25340 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_SET_CSC_DATA_SWIZZLE_SHIFT (12U)

Definition at line 25341 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_16_BIT

#define LCDIF_CTRL_SET_DATA_FORMAT_16_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_MASK)

Definition at line 25312 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_MASK

#define LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_MASK (0x8U)

Definition at line 25310 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_SHIFT

#define LCDIF_CTRL_SET_DATA_FORMAT_16_BIT_SHIFT (3U)

Definition at line 25311 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_18_BIT

#define LCDIF_CTRL_SET_DATA_FORMAT_18_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_MASK)

DATA_FORMAT_18_BIT 0b0..Data input to the block is in 18 bpp format, such that lower 18 bits contain RGB 666 and upper 14 bits do not contain any useful data. 0b1..Data input to the block is in 18 bpp format, such that upper 18 bits contain RGB 666 and lower 14 bits do not contain any useful data.

Definition at line 25309 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_MASK

#define LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_MASK (0x4U)

Definition at line 25303 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_SHIFT

#define LCDIF_CTRL_SET_DATA_FORMAT_18_BIT_SHIFT (2U)

Definition at line 25304 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_24_BIT

#define LCDIF_CTRL_SET_DATA_FORMAT_24_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_MASK)

DATA_FORMAT_24_BIT 0b0..Data input to the block is in 24 bpp format, such that all RGB 888 data is contained in 24 bits. 0b1..Data input to the block is actually RGB 18 bpp, but there is 1 color per byte, hence the upper 2 bits in each byte do not contain any useful data, and should be dropped.

Definition at line 25302 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_MASK

#define LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_MASK (0x2U)

Definition at line 25295 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_SHIFT

#define LCDIF_CTRL_SET_DATA_FORMAT_24_BIT_SHIFT (1U)

Definition at line 25296 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_SHIFT_DIR

#define LCDIF_CTRL_SET_DATA_SHIFT_DIR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_SET_DATA_SHIFT_DIR_MASK)

DATA_SHIFT_DIR 0b0..Data to be transmitted is shifted LEFT by SHIFT_NUM_BITS bits. 0b1..Data to be transmitted is shifted RIGHT by SHIFT_NUM_BITS bits.

Definition at line 25377 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_SHIFT_DIR_MASK

#define LCDIF_CTRL_SET_DATA_SHIFT_DIR_MASK (0x4000000U)

Definition at line 25371 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DATA_SHIFT_DIR_SHIFT

#define LCDIF_CTRL_SET_DATA_SHIFT_DIR_SHIFT (26U)

Definition at line 25372 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DOTCLK_MODE

#define LCDIF_CTRL_SET_DOTCLK_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_SET_DOTCLK_MODE_MASK)

Definition at line 25364 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DOTCLK_MODE_MASK

#define LCDIF_CTRL_SET_DOTCLK_MODE_MASK (0x20000U)

Definition at line 25362 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_DOTCLK_MODE_SHIFT

#define LCDIF_CTRL_SET_DOTCLK_MODE_SHIFT (17U)

Definition at line 25363 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE

#define LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_MASK)

Definition at line 25321 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_MASK

#define LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_MASK (0x40U)

Definition at line 25319 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_SHIFT

#define LCDIF_CTRL_SET_ENABLE_PXP_HANDSHAKE_SHIFT (6U)

Definition at line 25320 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE

#define LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_MASK)

INPUT_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25361 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_MASK (0xC000U)

Definition at line 25351 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_SET_INPUT_DATA_SWIZZLE_SHIFT (14U)

Definition at line 25352 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_LCD_DATABUS_WIDTH

#define LCDIF_CTRL_SET_LCD_DATABUS_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_MASK)

LCD_DATABUS_WIDTH 0b00..16-bit data bus mode. 0b01..8-bit data bus mode. 0b10..18-bit data bus mode. 0b11..24-bit data bus mode.

Definition at line 25339 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_MASK

#define LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_MASK (0xC00U)

Definition at line 25331 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_SHIFT

#define LCDIF_CTRL_SET_LCD_DATABUS_WIDTH_SHIFT (10U)

Definition at line 25332 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_MASTER

#define LCDIF_CTRL_SET_MASTER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_MASTER_SHIFT)) & LCDIF_CTRL_SET_MASTER_MASK)

Definition at line 25318 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_MASTER_MASK

#define LCDIF_CTRL_SET_MASTER_MASK (0x20U)

Definition at line 25316 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_MASTER_SHIFT

#define LCDIF_CTRL_SET_MASTER_SHIFT (5U)

Definition at line 25317 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_RSRVD0

#define LCDIF_CTRL_SET_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_RSRVD0_SHIFT)) & LCDIF_CTRL_SET_RSRVD0_MASK)

Definition at line 25315 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_RSRVD0_MASK

#define LCDIF_CTRL_SET_RSRVD0_MASK (0x10U)

Definition at line 25313 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_RSRVD0_SHIFT

#define LCDIF_CTRL_SET_RSRVD0_SHIFT (4U)

Definition at line 25314 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_RUN

#define LCDIF_CTRL_SET_RUN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_RUN_SHIFT)) & LCDIF_CTRL_SET_RUN_MASK)

Definition at line 25294 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_RUN_MASK

#define LCDIF_CTRL_SET_RUN_MASK (0x1U)

Definition at line 25292 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_RUN_SHIFT

#define LCDIF_CTRL_SET_RUN_SHIFT (0U)

Definition at line 25293 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_SFTRST

#define LCDIF_CTRL_SET_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_SFTRST_SHIFT)) & LCDIF_CTRL_SET_SFTRST_MASK)

Definition at line 25383 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_SFTRST_MASK

#define LCDIF_CTRL_SET_SFTRST_MASK (0x80000000U)

Definition at line 25381 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_SFTRST_SHIFT

#define LCDIF_CTRL_SET_SFTRST_SHIFT (31U)

Definition at line 25382 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_SHIFT_NUM_BITS

#define LCDIF_CTRL_SET_SHIFT_NUM_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_SET_SHIFT_NUM_BITS_MASK)

Definition at line 25370 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_SHIFT_NUM_BITS_MASK

#define LCDIF_CTRL_SET_SHIFT_NUM_BITS_MASK (0x3E00000U)

Definition at line 25368 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_SHIFT_NUM_BITS_SHIFT

#define LCDIF_CTRL_SET_SHIFT_NUM_BITS_SHIFT (21U)

Definition at line 25369 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_WORD_LENGTH

#define LCDIF_CTRL_SET_WORD_LENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SET_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_SET_WORD_LENGTH_MASK)

WORD_LENGTH 0b00..Input data is 16 bits per pixel. 0b01..Input data is 8 bits wide. 0b10..Input data is 18 bits per pixel. 0b11..Input data is 24 bits per pixel.

Definition at line 25330 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_WORD_LENGTH_MASK

#define LCDIF_CTRL_SET_WORD_LENGTH_MASK (0x300U)

Definition at line 25322 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SET_WORD_LENGTH_SHIFT

#define LCDIF_CTRL_SET_WORD_LENGTH_SHIFT (8U)

Definition at line 25323 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SFTRST

#define LCDIF_CTRL_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SFTRST_SHIFT)) & LCDIF_CTRL_SFTRST_MASK)

Definition at line 25287 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SFTRST_MASK

#define LCDIF_CTRL_SFTRST_MASK (0x80000000U)

Definition at line 25285 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SFTRST_SHIFT

#define LCDIF_CTRL_SFTRST_SHIFT (31U)

Definition at line 25286 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SHIFT_NUM_BITS

#define LCDIF_CTRL_SHIFT_NUM_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_SHIFT_NUM_BITS_MASK)

Definition at line 25274 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SHIFT_NUM_BITS_MASK

#define LCDIF_CTRL_SHIFT_NUM_BITS_MASK (0x3E00000U)

Definition at line 25272 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_SHIFT_NUM_BITS_SHIFT

#define LCDIF_CTRL_SHIFT_NUM_BITS_SHIFT (21U)

Definition at line 25273 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_BYPASS_COUNT

#define LCDIF_CTRL_TOG_BYPASS_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_BYPASS_COUNT_SHIFT)) & LCDIF_CTRL_TOG_BYPASS_COUNT_MASK)

Definition at line 25559 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_BYPASS_COUNT_MASK

#define LCDIF_CTRL_TOG_BYPASS_COUNT_MASK (0x80000U)

Definition at line 25557 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_BYPASS_COUNT_SHIFT

#define LCDIF_CTRL_TOG_BYPASS_COUNT_SHIFT (19U)

Definition at line 25558 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_CLKGATE

#define LCDIF_CTRL_TOG_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_CLKGATE_SHIFT)) & LCDIF_CTRL_TOG_CLKGATE_MASK)

Definition at line 25572 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_CLKGATE_MASK

#define LCDIF_CTRL_TOG_CLKGATE_MASK (0x40000000U)

Definition at line 25570 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_CLKGATE_SHIFT

#define LCDIF_CTRL_TOG_CLKGATE_SHIFT (30U)

Definition at line 25571 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE

#define LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_MASK)

CSC_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25542 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_MASK (0x3000U)

Definition at line 25532 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_TOG_CSC_DATA_SWIZZLE_SHIFT (12U)

Definition at line 25533 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT

#define LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_SHIFT)) & LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_MASK)

Definition at line 25504 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_MASK

#define LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_MASK (0x8U)

Definition at line 25502 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_SHIFT

#define LCDIF_CTRL_TOG_DATA_FORMAT_16_BIT_SHIFT (3U)

Definition at line 25503 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT

#define LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_SHIFT)) & LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_MASK)

DATA_FORMAT_18_BIT 0b0..Data input to the block is in 18 bpp format, such that lower 18 bits contain RGB 666 and upper 14 bits do not contain any useful data. 0b1..Data input to the block is in 18 bpp format, such that upper 18 bits contain RGB 666 and lower 14 bits do not contain any useful data.

Definition at line 25501 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_MASK

#define LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_MASK (0x4U)

Definition at line 25495 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_SHIFT

#define LCDIF_CTRL_TOG_DATA_FORMAT_18_BIT_SHIFT (2U)

Definition at line 25496 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT

#define LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_SHIFT)) & LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_MASK)

DATA_FORMAT_24_BIT 0b0..Data input to the block is in 24 bpp format, such that all RGB 888 data is contained in 24 bits. 0b1..Data input to the block is actually RGB 18 bpp, but there is 1 color per byte, hence the upper 2 bits in each byte do not contain any useful data, and should be dropped.

Definition at line 25494 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_MASK

#define LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_MASK (0x2U)

Definition at line 25487 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_SHIFT

#define LCDIF_CTRL_TOG_DATA_FORMAT_24_BIT_SHIFT (1U)

Definition at line 25488 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_SHIFT_DIR

#define LCDIF_CTRL_TOG_DATA_SHIFT_DIR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DATA_SHIFT_DIR_SHIFT)) & LCDIF_CTRL_TOG_DATA_SHIFT_DIR_MASK)

DATA_SHIFT_DIR 0b0..Data to be transmitted is shifted LEFT by SHIFT_NUM_BITS bits. 0b1..Data to be transmitted is shifted RIGHT by SHIFT_NUM_BITS bits.

Definition at line 25569 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_SHIFT_DIR_MASK

#define LCDIF_CTRL_TOG_DATA_SHIFT_DIR_MASK (0x4000000U)

Definition at line 25563 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DATA_SHIFT_DIR_SHIFT

#define LCDIF_CTRL_TOG_DATA_SHIFT_DIR_SHIFT (26U)

Definition at line 25564 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DOTCLK_MODE

#define LCDIF_CTRL_TOG_DOTCLK_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_DOTCLK_MODE_SHIFT)) & LCDIF_CTRL_TOG_DOTCLK_MODE_MASK)

Definition at line 25556 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DOTCLK_MODE_MASK

#define LCDIF_CTRL_TOG_DOTCLK_MODE_MASK (0x20000U)

Definition at line 25554 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_DOTCLK_MODE_SHIFT

#define LCDIF_CTRL_TOG_DOTCLK_MODE_SHIFT (17U)

Definition at line 25555 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE

#define LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_SHIFT)) & LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_MASK)

Definition at line 25513 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_MASK

#define LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_MASK (0x40U)

Definition at line 25511 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_SHIFT

#define LCDIF_CTRL_TOG_ENABLE_PXP_HANDSHAKE_SHIFT (6U)

Definition at line 25512 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE

#define LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_SHIFT)) & LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_MASK)

INPUT_DATA_SWIZZLE 0b00..No byte swapping.(Little endian) 0b00..Little Endian byte ordering (same as NO_SWAP). 0b01..Big Endian swap (swap bytes 0,3 and 1,2). 0b01..Swizzle all bytes, swap bytes 0,3 and 1,2 (aka Big Endian). 0b10..Swap half-words. 0b11..Swap bytes within each half-word.

Definition at line 25553 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_MASK

#define LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_MASK (0xC000U)

Definition at line 25543 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_SHIFT

#define LCDIF_CTRL_TOG_INPUT_DATA_SWIZZLE_SHIFT (14U)

Definition at line 25544 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH

#define LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_SHIFT)) & LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_MASK)

LCD_DATABUS_WIDTH 0b00..16-bit data bus mode. 0b01..8-bit data bus mode. 0b10..18-bit data bus mode. 0b11..24-bit data bus mode.

Definition at line 25531 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_MASK

#define LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_MASK (0xC00U)

Definition at line 25523 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_SHIFT

#define LCDIF_CTRL_TOG_LCD_DATABUS_WIDTH_SHIFT (10U)

Definition at line 25524 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_MASTER

#define LCDIF_CTRL_TOG_MASTER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_MASTER_SHIFT)) & LCDIF_CTRL_TOG_MASTER_MASK)

Definition at line 25510 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_MASTER_MASK

#define LCDIF_CTRL_TOG_MASTER_MASK (0x20U)

Definition at line 25508 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_MASTER_SHIFT

#define LCDIF_CTRL_TOG_MASTER_SHIFT (5U)

Definition at line 25509 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_RSRVD0

#define LCDIF_CTRL_TOG_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_RSRVD0_SHIFT)) & LCDIF_CTRL_TOG_RSRVD0_MASK)

Definition at line 25507 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_RSRVD0_MASK

#define LCDIF_CTRL_TOG_RSRVD0_MASK (0x10U)

Definition at line 25505 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_RSRVD0_SHIFT

#define LCDIF_CTRL_TOG_RSRVD0_SHIFT (4U)

Definition at line 25506 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_RUN

#define LCDIF_CTRL_TOG_RUN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_RUN_SHIFT)) & LCDIF_CTRL_TOG_RUN_MASK)

Definition at line 25486 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_RUN_MASK

#define LCDIF_CTRL_TOG_RUN_MASK (0x1U)

Definition at line 25484 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_RUN_SHIFT

#define LCDIF_CTRL_TOG_RUN_SHIFT (0U)

Definition at line 25485 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_SFTRST

#define LCDIF_CTRL_TOG_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_SFTRST_SHIFT)) & LCDIF_CTRL_TOG_SFTRST_MASK)

Definition at line 25575 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_SFTRST_MASK

#define LCDIF_CTRL_TOG_SFTRST_MASK (0x80000000U)

Definition at line 25573 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_SFTRST_SHIFT

#define LCDIF_CTRL_TOG_SFTRST_SHIFT (31U)

Definition at line 25574 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_SHIFT_NUM_BITS

#define LCDIF_CTRL_TOG_SHIFT_NUM_BITS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_SHIFT_NUM_BITS_SHIFT)) & LCDIF_CTRL_TOG_SHIFT_NUM_BITS_MASK)

Definition at line 25562 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_SHIFT_NUM_BITS_MASK

#define LCDIF_CTRL_TOG_SHIFT_NUM_BITS_MASK (0x3E00000U)

Definition at line 25560 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_SHIFT_NUM_BITS_SHIFT

#define LCDIF_CTRL_TOG_SHIFT_NUM_BITS_SHIFT (21U)

Definition at line 25561 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_WORD_LENGTH

#define LCDIF_CTRL_TOG_WORD_LENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_TOG_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_TOG_WORD_LENGTH_MASK)

WORD_LENGTH 0b00..Input data is 16 bits per pixel. 0b01..Input data is 8 bits wide. 0b10..Input data is 18 bits per pixel. 0b11..Input data is 24 bits per pixel.

Definition at line 25522 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_WORD_LENGTH_MASK

#define LCDIF_CTRL_TOG_WORD_LENGTH_MASK (0x300U)

Definition at line 25514 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_TOG_WORD_LENGTH_SHIFT

#define LCDIF_CTRL_TOG_WORD_LENGTH_SHIFT (8U)

Definition at line 25515 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_WORD_LENGTH

#define LCDIF_CTRL_WORD_LENGTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CTRL_WORD_LENGTH_SHIFT)) & LCDIF_CTRL_WORD_LENGTH_MASK)

WORD_LENGTH 0b00..Input data is 16 bits per pixel. 0b01..Input data is 8 bits wide. 0b10..Input data is 18 bits per pixel. 0b11..Input data is 24 bits per pixel.

Definition at line 25234 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_WORD_LENGTH_MASK

#define LCDIF_CTRL_WORD_LENGTH_MASK (0x300U)

Definition at line 25226 of file MIMXRT1062.h.

## ◆ LCDIF_CTRL_WORD_LENGTH_SHIFT

#define LCDIF_CTRL_WORD_LENGTH_SHIFT (8U)

Definition at line 25227 of file MIMXRT1062.h.

## ◆ LCDIF_CUR_BUF_ADDR

#define LCDIF_CUR_BUF_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_CUR_BUF_ADDR_SHIFT)) & LCDIF_CUR_BUF_ADDR_MASK)

Definition at line 26120 of file MIMXRT1062.h.

## ◆ LCDIF_CUR_BUF_ADDR_MASK

#define LCDIF_CUR_BUF_ADDR_MASK (0xFFFFFFFFU)

Definition at line 26118 of file MIMXRT1062.h.

## ◆ LCDIF_CUR_BUF_ADDR_SHIFT

#define LCDIF_CUR_BUF_ADDR_SHIFT (0U)

Definition at line 26119 of file MIMXRT1062.h.

## ◆ LCDIF_LUT0_ADDR_ADDR

#define LCDIF_LUT0_ADDR_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT0_ADDR_ADDR_SHIFT)) & LCDIF_LUT0_ADDR_ADDR_MASK)

Definition at line 26617 of file MIMXRT1062.h.

## ◆ LCDIF_LUT0_ADDR_ADDR_MASK

#define LCDIF_LUT0_ADDR_ADDR_MASK (0xFFU)

Definition at line 26615 of file MIMXRT1062.h.

## ◆ LCDIF_LUT0_ADDR_ADDR_SHIFT

#define LCDIF_LUT0_ADDR_ADDR_SHIFT (0U)

Definition at line 26616 of file MIMXRT1062.h.

## ◆ LCDIF_LUT0_DATA_DATA

#define LCDIF_LUT0_DATA_DATA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT0_DATA_DATA_SHIFT)) & LCDIF_LUT0_DATA_DATA_MASK)

Definition at line 26624 of file MIMXRT1062.h.

## ◆ LCDIF_LUT0_DATA_DATA_MASK

#define LCDIF_LUT0_DATA_DATA_MASK (0xFFFFFFFFU)

Definition at line 26622 of file MIMXRT1062.h.

## ◆ LCDIF_LUT0_DATA_DATA_SHIFT

#define LCDIF_LUT0_DATA_DATA_SHIFT (0U)

Definition at line 26623 of file MIMXRT1062.h.

## ◆ LCDIF_LUT1_ADDR_ADDR

#define LCDIF_LUT1_ADDR_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT1_ADDR_ADDR_SHIFT)) & LCDIF_LUT1_ADDR_ADDR_MASK)

Definition at line 26631 of file MIMXRT1062.h.

## ◆ LCDIF_LUT1_ADDR_ADDR_MASK

#define LCDIF_LUT1_ADDR_ADDR_MASK (0xFFU)

Definition at line 26629 of file MIMXRT1062.h.

## ◆ LCDIF_LUT1_ADDR_ADDR_SHIFT

#define LCDIF_LUT1_ADDR_ADDR_SHIFT (0U)

Definition at line 26630 of file MIMXRT1062.h.

## ◆ LCDIF_LUT1_DATA_DATA

#define LCDIF_LUT1_DATA_DATA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT1_DATA_DATA_SHIFT)) & LCDIF_LUT1_DATA_DATA_MASK)

Definition at line 26638 of file MIMXRT1062.h.

## ◆ LCDIF_LUT1_DATA_DATA_MASK

#define LCDIF_LUT1_DATA_DATA_MASK (0xFFFFFFFFU)

Definition at line 26636 of file MIMXRT1062.h.

## ◆ LCDIF_LUT1_DATA_DATA_SHIFT

#define LCDIF_LUT1_DATA_DATA_SHIFT (0U)

Definition at line 26637 of file MIMXRT1062.h.

## ◆ LCDIF_LUT_CTRL_LUT_BYPASS

#define LCDIF_LUT_CTRL_LUT_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_LUT_CTRL_LUT_BYPASS_SHIFT)) & LCDIF_LUT_CTRL_LUT_BYPASS_MASK)

Definition at line 26610 of file MIMXRT1062.h.

## ◆ LCDIF_LUT_CTRL_LUT_BYPASS_MASK

#define LCDIF_LUT_CTRL_LUT_BYPASS_MASK (0x1U)

Definition at line 26608 of file MIMXRT1062.h.

## ◆ LCDIF_LUT_CTRL_LUT_BYPASS_SHIFT

#define LCDIF_LUT_CTRL_LUT_BYPASS_SHIFT (0U)

Definition at line 26609 of file MIMXRT1062.h.

## ◆ LCDIF_NEXT_BUF_ADDR

#define LCDIF_NEXT_BUF_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_NEXT_BUF_ADDR_SHIFT)) & LCDIF_NEXT_BUF_ADDR_MASK)

Definition at line 26127 of file MIMXRT1062.h.

## ◆ LCDIF_NEXT_BUF_ADDR_MASK

#define LCDIF_NEXT_BUF_ADDR_MASK (0xFFFFFFFFU)

Definition at line 26125 of file MIMXRT1062.h.

## ◆ LCDIF_NEXT_BUF_ADDR_SHIFT

#define LCDIF_NEXT_BUF_ADDR_SHIFT (0U)

Definition at line 26126 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_COUNT

#define LCDIF_PIGEON_0_COUNT (12U)

Definition at line 26560 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_EN

#define LCDIF_PIGEON_0_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_EN_SHIFT)) & LCDIF_PIGEON_0_EN_MASK)

Definition at line 26508 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_EN_MASK

#define LCDIF_PIGEON_0_EN_MASK (0x1U)

Definition at line 26506 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_EN_SHIFT

#define LCDIF_PIGEON_0_EN_SHIFT (0U)

Definition at line 26507 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_INC_SEL

#define LCDIF_PIGEON_0_INC_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_INC_SEL_SHIFT)) & LCDIF_PIGEON_0_INC_SEL_MASK)

INC_SEL 0b00..pclk 0b01..Line start pulse 0b10..Frame start pulse 0b11..Use another signal as tick event

Definition at line 26524 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_INC_SEL_MASK

#define LCDIF_PIGEON_0_INC_SEL_MASK (0xCU)

Definition at line 26516 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_INC_SEL_SHIFT

#define LCDIF_PIGEON_0_INC_SEL_SHIFT (2U)

Definition at line 26517 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_MASK_CNT

#define LCDIF_PIGEON_0_MASK_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_MASK_CNT_SHIFT)) & LCDIF_PIGEON_0_MASK_CNT_MASK)

Definition at line 26543 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_MASK_CNT_MASK

#define LCDIF_PIGEON_0_MASK_CNT_MASK (0xFFF000U)

Definition at line 26541 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_MASK_CNT_SEL

#define LCDIF_PIGEON_0_MASK_CNT_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_MASK_CNT_SEL_SHIFT)) & LCDIF_PIGEON_0_MASK_CNT_SEL_MASK)

MASK_CNT_SEL 0b0000..pclk counter within one hscan state 0b0001..pclk cycle within one hscan state 0b0010..line counter within one vscan state 0b0011..line cycle within one vscan state 0b0100..frame counter 0b0101..frame cycle 0b0110..horizontal counter (pclk counter within one line ) 0b0111..vertical counter (line counter within one frame)

Definition at line 26540 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_MASK_CNT_SEL_MASK

#define LCDIF_PIGEON_0_MASK_CNT_SEL_MASK (0xF00U)

Definition at line 26528 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_MASK_CNT_SEL_SHIFT

#define LCDIF_PIGEON_0_MASK_CNT_SEL_SHIFT (8U)

Definition at line 26529 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_MASK_CNT_SHIFT

#define LCDIF_PIGEON_0_MASK_CNT_SHIFT (12U)

Definition at line 26542 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_OFFSET

#define LCDIF_PIGEON_0_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_OFFSET_SHIFT)) & LCDIF_PIGEON_0_OFFSET_MASK)

Definition at line 26527 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_OFFSET_MASK

#define LCDIF_PIGEON_0_OFFSET_MASK (0xF0U)

Definition at line 26525 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_OFFSET_SHIFT

#define LCDIF_PIGEON_0_OFFSET_SHIFT (4U)

Definition at line 26526 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_POL

#define LCDIF_PIGEON_0_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_POL_SHIFT)) & LCDIF_PIGEON_0_POL_MASK)

POL 0b0..Normal Signal (Active high) 0b1..Inverted signal (Active low)

Definition at line 26515 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_POL_MASK

#define LCDIF_PIGEON_0_POL_MASK (0x2U)

Definition at line 26509 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_POL_SHIFT

#define LCDIF_PIGEON_0_POL_SHIFT (1U)

Definition at line 26510 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_STATE_MASK

#define LCDIF_PIGEON_0_STATE_MASK | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_0_STATE_MASK_SHIFT)) & LCDIF_PIGEON_0_STATE_MASK_MASK)

STATE_MASK 0b00000001..FRAME SYNC 0b00000010..FRAME BEGIN 0b00000100..FRAME DATA 0b00001000..FRAME END 0b00010000..LINE SYNC 0b00100000..LINE BEGIN 0b01000000..LINE DATA 0b10000000..LINE END

Definition at line 26556 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_STATE_MASK_MASK

#define LCDIF_PIGEON_0_STATE_MASK_MASK (0xFF000000U)

Definition at line 26544 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_0_STATE_MASK_SHIFT

#define LCDIF_PIGEON_0_STATE_MASK_SHIFT (24U)

Definition at line 26545 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_1_CLR_CNT

#define LCDIF_PIGEON_1_CLR_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_1_CLR_CNT_SHIFT)) & LCDIF_PIGEON_1_CLR_CNT_MASK)

CLR_CNT 0b0000000000000000..Keep active until mask off

Definition at line 26575 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_1_CLR_CNT_MASK

#define LCDIF_PIGEON_1_CLR_CNT_MASK (0xFFFF0000U)

Definition at line 26570 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_1_CLR_CNT_SHIFT

#define LCDIF_PIGEON_1_CLR_CNT_SHIFT (16U)

Definition at line 26571 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_1_COUNT

#define LCDIF_PIGEON_1_COUNT (12U)

Definition at line 26579 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_1_SET_CNT

#define LCDIF_PIGEON_1_SET_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_1_SET_CNT_SHIFT)) & LCDIF_PIGEON_1_SET_CNT_MASK)

SET_CNT 0b0000000000000000..Start as active

Definition at line 26569 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_1_SET_CNT_MASK

#define LCDIF_PIGEON_1_SET_CNT_MASK (0xFFFFU)

Definition at line 26564 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_1_SET_CNT_SHIFT

#define LCDIF_PIGEON_1_SET_CNT_SHIFT (0U)

Definition at line 26565 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_COUNT

#define LCDIF_PIGEON_2_COUNT (12U)

Definition at line 26604 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_RSVD

#define LCDIF_PIGEON_2_RSVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_2_RSVD_SHIFT)) & LCDIF_PIGEON_2_RSVD_MASK)

Definition at line 26600 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_RSVD_MASK

#define LCDIF_PIGEON_2_RSVD_MASK (0xFFFFFE00U)

Definition at line 26598 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_RSVD_SHIFT

#define LCDIF_PIGEON_2_RSVD_SHIFT (9U)

Definition at line 26599 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_SIG_ANOTHER

#define LCDIF_PIGEON_2_SIG_ANOTHER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_2_SIG_ANOTHER_SHIFT)) & LCDIF_PIGEON_2_SIG_ANOTHER_MASK)

SIG_ANOTHER 0b00000..Keep active until mask off

Definition at line 26597 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_SIG_ANOTHER_MASK

#define LCDIF_PIGEON_2_SIG_ANOTHER_MASK (0x1F0U)

Definition at line 26592 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_SIG_ANOTHER_SHIFT

#define LCDIF_PIGEON_2_SIG_ANOTHER_SHIFT (4U)

Definition at line 26593 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_SIG_LOGIC

#define LCDIF_PIGEON_2_SIG_LOGIC | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEON_2_SIG_LOGIC_SHIFT)) & LCDIF_PIGEON_2_SIG_LOGIC_MASK)

SIG_LOGIC 0b0000..No logic operation 0b0001..sigout = sig_another AND this_sig 0b0010..sigout = sig_another OR this_sig 0b0011..mask = sig_another AND other_masks

Definition at line 26591 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_SIG_LOGIC_MASK

#define LCDIF_PIGEON_2_SIG_LOGIC_MASK (0xFU)

Definition at line 26583 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEON_2_SIG_LOGIC_SHIFT

#define LCDIF_PIGEON_2_SIG_LOGIC_SHIFT (0U)

Definition at line 26584 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_CLR_FD_PERIOD

#define LCDIF_PIGEONCTRL0_CLR_FD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_MASK)

Definition at line 26408 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_MASK (0xFFFU)

Definition at line 26406 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_CLR_FD_PERIOD_SHIFT (0U)

Definition at line 26407 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_CLR_LD_PERIOD

#define LCDIF_PIGEONCTRL0_CLR_LD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_MASK)

Definition at line 26411 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_MASK (0xFFF0000U)

Definition at line 26409 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_CLR_LD_PERIOD_SHIFT (16U)

Definition at line 26410 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_FD_PERIOD

#define LCDIF_PIGEONCTRL0_FD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_FD_PERIOD_MASK)

Definition at line 26388 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_FD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_FD_PERIOD_MASK (0xFFFU)

Definition at line 26386 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_FD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_FD_PERIOD_SHIFT (0U)

Definition at line 26387 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_LD_PERIOD

#define LCDIF_PIGEONCTRL0_LD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_LD_PERIOD_MASK)

Definition at line 26391 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_LD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_LD_PERIOD_MASK (0xFFF0000U)

Definition at line 26389 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_LD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_LD_PERIOD_SHIFT (16U)

Definition at line 26390 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_SET_FD_PERIOD

#define LCDIF_PIGEONCTRL0_SET_FD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_SET_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_SET_FD_PERIOD_MASK)

Definition at line 26398 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_SET_FD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_SET_FD_PERIOD_MASK (0xFFFU)

Definition at line 26396 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_SET_FD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_SET_FD_PERIOD_SHIFT (0U)

Definition at line 26397 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_SET_LD_PERIOD

#define LCDIF_PIGEONCTRL0_SET_LD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_SET_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_SET_LD_PERIOD_MASK)

Definition at line 26401 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_SET_LD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_SET_LD_PERIOD_MASK (0xFFF0000U)

Definition at line 26399 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_SET_LD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_SET_LD_PERIOD_SHIFT (16U)

Definition at line 26400 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_TOG_FD_PERIOD

#define LCDIF_PIGEONCTRL0_TOG_FD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_MASK)

Definition at line 26418 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_MASK (0xFFFU)

Definition at line 26416 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_TOG_FD_PERIOD_SHIFT (0U)

Definition at line 26417 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_TOG_LD_PERIOD

#define LCDIF_PIGEONCTRL0_TOG_LD_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_MASK)

Definition at line 26421 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_MASK

#define LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_MASK (0xFFF0000U)

Definition at line 26419 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL0_TOG_LD_PERIOD_SHIFT (16U)

Definition at line 26420 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES

#define LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_MASK)

Definition at line 26451 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_MASK

#define LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_MASK (0xFFF0000U)

Definition at line 26449 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_SHIFT

#define LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_CYCLES_SHIFT (16U)

Definition at line 26450 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD

#define LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_MASK)

Definition at line 26448 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_MASK

#define LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_MASK (0xFFFU)

Definition at line 26446 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL1_CLR_FRAME_CNT_PERIOD_SHIFT (0U)

Definition at line 26447 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES

#define LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_MASK)

Definition at line 26431 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_MASK

#define LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_MASK (0xFFF0000U)

Definition at line 26429 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_SHIFT

#define LCDIF_PIGEONCTRL1_FRAME_CNT_CYCLES_SHIFT (16U)

Definition at line 26430 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD

#define LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_MASK)

Definition at line 26428 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_MASK

#define LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_MASK (0xFFFU)

Definition at line 26426 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL1_FRAME_CNT_PERIOD_SHIFT (0U)

Definition at line 26427 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES

#define LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_MASK)

Definition at line 26441 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_MASK

#define LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_MASK (0xFFF0000U)

Definition at line 26439 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_SHIFT

#define LCDIF_PIGEONCTRL1_SET_FRAME_CNT_CYCLES_SHIFT (16U)

Definition at line 26440 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD

#define LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_MASK)

Definition at line 26438 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_MASK

#define LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_MASK (0xFFFU)

Definition at line 26436 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL1_SET_FRAME_CNT_PERIOD_SHIFT (0U)

Definition at line 26437 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES

#define LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_SHIFT)) & LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_MASK)

Definition at line 26461 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_MASK

#define LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_MASK (0xFFF0000U)

Definition at line 26459 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_SHIFT

#define LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_CYCLES_SHIFT (16U)

Definition at line 26460 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD

#define LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_SHIFT)) & LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_MASK)

Definition at line 26458 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_MASK

#define LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_MASK (0xFFFU)

Definition at line 26456 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_SHIFT

#define LCDIF_PIGEONCTRL1_TOG_FRAME_CNT_PERIOD_SHIFT (0U)

Definition at line 26457 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE

#define LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_MASK)

Definition at line 26491 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_MASK

#define LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_MASK (0x2U)

Definition at line 26489 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_SHIFT

#define LCDIF_PIGEONCTRL2_CLR_PIGEON_CLK_GATE_SHIFT (1U)

Definition at line 26490 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN

#define LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_MASK)

Definition at line 26488 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_MASK

#define LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_MASK (0x1U)

Definition at line 26486 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_SHIFT

#define LCDIF_PIGEONCTRL2_CLR_PIGEON_DATA_EN_SHIFT (0U)

Definition at line 26487 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE

#define LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_MASK)

Definition at line 26471 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_MASK

#define LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_MASK (0x2U)

Definition at line 26469 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_SHIFT

#define LCDIF_PIGEONCTRL2_PIGEON_CLK_GATE_SHIFT (1U)

Definition at line 26470 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_PIGEON_DATA_EN

#define LCDIF_PIGEONCTRL2_PIGEON_DATA_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_MASK)

Definition at line 26468 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_MASK

#define LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_MASK (0x1U)

Definition at line 26466 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_SHIFT

#define LCDIF_PIGEONCTRL2_PIGEON_DATA_EN_SHIFT (0U)

Definition at line 26467 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE

#define LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_MASK)

Definition at line 26481 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_MASK

#define LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_MASK (0x2U)

Definition at line 26479 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_SHIFT

#define LCDIF_PIGEONCTRL2_SET_PIGEON_CLK_GATE_SHIFT (1U)

Definition at line 26480 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN

#define LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_MASK)

Definition at line 26478 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_MASK

#define LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_MASK (0x1U)

Definition at line 26476 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_SHIFT

#define LCDIF_PIGEONCTRL2_SET_PIGEON_DATA_EN_SHIFT (0U)

Definition at line 26477 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE

#define LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_SHIFT)) & LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_MASK)

Definition at line 26501 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_MASK

#define LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_MASK (0x2U)

Definition at line 26499 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_SHIFT

#define LCDIF_PIGEONCTRL2_TOG_PIGEON_CLK_GATE_SHIFT (1U)

Definition at line 26500 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN

#define LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_SHIFT)) & LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_MASK)

Definition at line 26498 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_MASK

#define LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_MASK (0x1U)

Definition at line 26496 of file MIMXRT1062.h.

## ◆ LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_SHIFT

#define LCDIF_PIGEONCTRL2_TOG_PIGEON_DATA_EN_SHIFT (0U)

Definition at line 26497 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_DMA_REQ

#define LCDIF_STAT_DMA_REQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_DMA_REQ_SHIFT)) & LCDIF_STAT_DMA_REQ_MASK)

Definition at line 26378 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_DMA_REQ_MASK

#define LCDIF_STAT_DMA_REQ_MASK (0x40000000U)

Definition at line 26376 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_DMA_REQ_SHIFT

#define LCDIF_STAT_DMA_REQ_SHIFT (30U)

Definition at line 26377 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_COUNT

#define LCDIF_STAT_LFIFO_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_LFIFO_COUNT_SHIFT)) & LCDIF_STAT_LFIFO_COUNT_MASK)

Definition at line 26360 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_COUNT_MASK

#define LCDIF_STAT_LFIFO_COUNT_MASK (0x1FFU)

Definition at line 26358 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_COUNT_SHIFT

#define LCDIF_STAT_LFIFO_COUNT_SHIFT (0U)

Definition at line 26359 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_EMPTY

#define LCDIF_STAT_LFIFO_EMPTY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_LFIFO_EMPTY_SHIFT)) & LCDIF_STAT_LFIFO_EMPTY_MASK)

Definition at line 26372 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_EMPTY_MASK

#define LCDIF_STAT_LFIFO_EMPTY_MASK (0x10000000U)

Definition at line 26370 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_EMPTY_SHIFT

#define LCDIF_STAT_LFIFO_EMPTY_SHIFT (28U)

Definition at line 26371 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_FULL

#define LCDIF_STAT_LFIFO_FULL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_LFIFO_FULL_SHIFT)) & LCDIF_STAT_LFIFO_FULL_MASK)

Definition at line 26375 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_FULL_MASK

#define LCDIF_STAT_LFIFO_FULL_MASK (0x20000000U)

Definition at line 26373 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_LFIFO_FULL_SHIFT

#define LCDIF_STAT_LFIFO_FULL_SHIFT (29U)

Definition at line 26374 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_PRESENT

#define LCDIF_STAT_PRESENT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_PRESENT_SHIFT)) & LCDIF_STAT_PRESENT_MASK)

Definition at line 26381 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_PRESENT_MASK

#define LCDIF_STAT_PRESENT_MASK (0x80000000U)

Definition at line 26379 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_PRESENT_SHIFT

#define LCDIF_STAT_PRESENT_SHIFT (31U)

Definition at line 26380 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_RSRVD0

#define LCDIF_STAT_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_RSRVD0_SHIFT)) & LCDIF_STAT_RSRVD0_MASK)

Definition at line 26363 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_RSRVD0_MASK

#define LCDIF_STAT_RSRVD0_MASK (0x1FFFE00U)

Definition at line 26361 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_RSRVD0_SHIFT

#define LCDIF_STAT_RSRVD0_SHIFT (9U)

Definition at line 26362 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_TXFIFO_EMPTY

#define LCDIF_STAT_TXFIFO_EMPTY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_TXFIFO_EMPTY_SHIFT)) & LCDIF_STAT_TXFIFO_EMPTY_MASK)

Definition at line 26366 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_TXFIFO_EMPTY_MASK

#define LCDIF_STAT_TXFIFO_EMPTY_MASK (0x4000000U)

Definition at line 26364 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_TXFIFO_EMPTY_SHIFT

#define LCDIF_STAT_TXFIFO_EMPTY_SHIFT (26U)

Definition at line 26365 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_TXFIFO_FULL

#define LCDIF_STAT_TXFIFO_FULL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_STAT_TXFIFO_FULL_SHIFT)) & LCDIF_STAT_TXFIFO_FULL_MASK)

Definition at line 26369 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_TXFIFO_FULL_MASK

#define LCDIF_STAT_TXFIFO_FULL_MASK (0x8000000U)

Definition at line 26367 of file MIMXRT1062.h.

## ◆ LCDIF_STAT_TXFIFO_FULL_SHIFT

#define LCDIF_STAT_TXFIFO_FULL_SHIFT (27U)

Definition at line 26368 of file MIMXRT1062.h.

## ◆ LCDIF_TRANSFER_COUNT_H_COUNT

#define LCDIF_TRANSFER_COUNT_H_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_TRANSFER_COUNT_H_COUNT_SHIFT)) & LCDIF_TRANSFER_COUNT_H_COUNT_MASK)

Definition at line 26110 of file MIMXRT1062.h.

## ◆ LCDIF_TRANSFER_COUNT_H_COUNT_MASK

#define LCDIF_TRANSFER_COUNT_H_COUNT_MASK (0xFFFFU)

Definition at line 26108 of file MIMXRT1062.h.

## ◆ LCDIF_TRANSFER_COUNT_H_COUNT_SHIFT

#define LCDIF_TRANSFER_COUNT_H_COUNT_SHIFT (0U)

Definition at line 26109 of file MIMXRT1062.h.

## ◆ LCDIF_TRANSFER_COUNT_V_COUNT

#define LCDIF_TRANSFER_COUNT_V_COUNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_TRANSFER_COUNT_V_COUNT_SHIFT)) & LCDIF_TRANSFER_COUNT_V_COUNT_MASK)

Definition at line 26113 of file MIMXRT1062.h.

## ◆ LCDIF_TRANSFER_COUNT_V_COUNT_MASK

#define LCDIF_TRANSFER_COUNT_V_COUNT_MASK (0xFFFF0000U)

Definition at line 26111 of file MIMXRT1062.h.

## ◆ LCDIF_TRANSFER_COUNT_V_COUNT_SHIFT

#define LCDIF_TRANSFER_COUNT_V_COUNT_SHIFT (16U)

Definition at line 26112 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_DOTCLK_POL

#define LCDIF_VDCTRL0_CLR_DOTCLK_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_DOTCLK_POL_MASK)

Definition at line 26235 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_DOTCLK_POL_MASK

#define LCDIF_VDCTRL0_CLR_DOTCLK_POL_MASK (0x2000000U)

Definition at line 26233 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_DOTCLK_POL_SHIFT

#define LCDIF_VDCTRL0_CLR_DOTCLK_POL_SHIFT (25U)

Definition at line 26234 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_ENABLE_POL

#define LCDIF_VDCTRL0_CLR_ENABLE_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_ENABLE_POL_MASK)

Definition at line 26232 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_ENABLE_POL_MASK

#define LCDIF_VDCTRL0_CLR_ENABLE_POL_MASK (0x1000000U)

Definition at line 26230 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_ENABLE_POL_SHIFT

#define LCDIF_VDCTRL0_CLR_ENABLE_POL_SHIFT (24U)

Definition at line 26231 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_ENABLE_PRESENT

#define LCDIF_VDCTRL0_CLR_ENABLE_PRESENT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_MASK)

Definition at line 26244 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_MASK

#define LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_MASK (0x10000000U)

Definition at line 26242 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_SHIFT

#define LCDIF_VDCTRL0_CLR_ENABLE_PRESENT_SHIFT (28U)

Definition at line 26243 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HALF_LINE

#define LCDIF_VDCTRL0_CLR_HALF_LINE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_CLR_HALF_LINE_MASK)

Definition at line 26220 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HALF_LINE_MASK

#define LCDIF_VDCTRL0_CLR_HALF_LINE_MASK (0x80000U)

Definition at line 26218 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HALF_LINE_MODE

#define LCDIF_VDCTRL0_CLR_HALF_LINE_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_MASK)

Definition at line 26217 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_MASK

#define LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_MASK (0x40000U)

Definition at line 26215 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_SHIFT

#define LCDIF_VDCTRL0_CLR_HALF_LINE_MODE_SHIFT (18U)

Definition at line 26216 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HALF_LINE_SHIFT

#define LCDIF_VDCTRL0_CLR_HALF_LINE_SHIFT (19U)

Definition at line 26219 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HSYNC_POL

#define LCDIF_VDCTRL0_CLR_HSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_HSYNC_POL_MASK)

Definition at line 26238 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HSYNC_POL_MASK

#define LCDIF_VDCTRL0_CLR_HSYNC_POL_MASK (0x4000000U)

Definition at line 26236 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_HSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_CLR_HSYNC_POL_SHIFT (26U)

Definition at line 26237 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_RSRVD1

#define LCDIF_VDCTRL0_CLR_RSRVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_CLR_RSRVD1_MASK)

Definition at line 26229 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_RSRVD1_MASK

#define LCDIF_VDCTRL0_CLR_RSRVD1_MASK (0xC00000U)

Definition at line 26227 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_RSRVD1_SHIFT

#define LCDIF_VDCTRL0_CLR_RSRVD1_SHIFT (22U)

Definition at line 26228 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_RSRVD2

#define LCDIF_VDCTRL0_CLR_RSRVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_CLR_RSRVD2_MASK)

Definition at line 26247 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_RSRVD2_MASK

#define LCDIF_VDCTRL0_CLR_RSRVD2_MASK (0xE0000000U)

Definition at line 26245 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_RSRVD2_SHIFT

#define LCDIF_VDCTRL0_CLR_RSRVD2_SHIFT (29U)

Definition at line 26246 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT

#define LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_MASK)

Definition at line 26226 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_MASK

#define LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_MASK (0x200000U)

Definition at line 26224 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_SHIFT

#define LCDIF_VDCTRL0_CLR_VSYNC_PERIOD_UNIT_SHIFT (21U)

Definition at line 26225 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_POL

#define LCDIF_VDCTRL0_CLR_VSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_POL_MASK)

Definition at line 26241 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_POL_MASK

#define LCDIF_VDCTRL0_CLR_VSYNC_POL_MASK (0x8000000U)

Definition at line 26239 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_CLR_VSYNC_POL_SHIFT (27U)

Definition at line 26240 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH

#define LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_MASK)

Definition at line 26214 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_MASK

#define LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)

Definition at line 26212 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_SHIFT

#define LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_SHIFT (0U)

Definition at line 26213 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT

#define LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_MASK)

Definition at line 26223 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_MASK

#define LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)

Definition at line 26221 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_SHIFT

#define LCDIF_VDCTRL0_CLR_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)

Definition at line 26222 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_DOTCLK_POL

#define LCDIF_VDCTRL0_DOTCLK_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_DOTCLK_POL_MASK)

Definition at line 26155 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_DOTCLK_POL_MASK

#define LCDIF_VDCTRL0_DOTCLK_POL_MASK (0x2000000U)

Definition at line 26153 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_DOTCLK_POL_SHIFT

#define LCDIF_VDCTRL0_DOTCLK_POL_SHIFT (25U)

Definition at line 26154 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_ENABLE_POL

#define LCDIF_VDCTRL0_ENABLE_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_ENABLE_POL_MASK)

Definition at line 26152 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_ENABLE_POL_MASK

#define LCDIF_VDCTRL0_ENABLE_POL_MASK (0x1000000U)

Definition at line 26150 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_ENABLE_POL_SHIFT

#define LCDIF_VDCTRL0_ENABLE_POL_SHIFT (24U)

Definition at line 26151 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_ENABLE_PRESENT

#define LCDIF_VDCTRL0_ENABLE_PRESENT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_ENABLE_PRESENT_MASK)

Definition at line 26164 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_ENABLE_PRESENT_MASK

#define LCDIF_VDCTRL0_ENABLE_PRESENT_MASK (0x10000000U)

Definition at line 26162 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_ENABLE_PRESENT_SHIFT

#define LCDIF_VDCTRL0_ENABLE_PRESENT_SHIFT (28U)

Definition at line 26163 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HALF_LINE

#define LCDIF_VDCTRL0_HALF_LINE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_HALF_LINE_MASK)

Definition at line 26140 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HALF_LINE_MASK

#define LCDIF_VDCTRL0_HALF_LINE_MASK (0x80000U)

Definition at line 26138 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HALF_LINE_MODE

#define LCDIF_VDCTRL0_HALF_LINE_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_HALF_LINE_MODE_MASK)

Definition at line 26137 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HALF_LINE_MODE_MASK

#define LCDIF_VDCTRL0_HALF_LINE_MODE_MASK (0x40000U)

Definition at line 26135 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HALF_LINE_MODE_SHIFT

#define LCDIF_VDCTRL0_HALF_LINE_MODE_SHIFT (18U)

Definition at line 26136 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HALF_LINE_SHIFT

#define LCDIF_VDCTRL0_HALF_LINE_SHIFT (19U)

Definition at line 26139 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HSYNC_POL

#define LCDIF_VDCTRL0_HSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_HSYNC_POL_MASK)

Definition at line 26158 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HSYNC_POL_MASK

#define LCDIF_VDCTRL0_HSYNC_POL_MASK (0x4000000U)

Definition at line 26156 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_HSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_HSYNC_POL_SHIFT (26U)

Definition at line 26157 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_RSRVD1

#define LCDIF_VDCTRL0_RSRVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_RSRVD1_MASK)

Definition at line 26149 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_RSRVD1_MASK

#define LCDIF_VDCTRL0_RSRVD1_MASK (0xC00000U)

Definition at line 26147 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_RSRVD1_SHIFT

#define LCDIF_VDCTRL0_RSRVD1_SHIFT (22U)

Definition at line 26148 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_RSRVD2

#define LCDIF_VDCTRL0_RSRVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_RSRVD2_MASK)

Definition at line 26167 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_RSRVD2_MASK

#define LCDIF_VDCTRL0_RSRVD2_MASK (0xE0000000U)

Definition at line 26165 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_RSRVD2_SHIFT

#define LCDIF_VDCTRL0_RSRVD2_SHIFT (29U)

Definition at line 26166 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_DOTCLK_POL

#define LCDIF_VDCTRL0_SET_DOTCLK_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_SET_DOTCLK_POL_MASK)

Definition at line 26195 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_DOTCLK_POL_MASK

#define LCDIF_VDCTRL0_SET_DOTCLK_POL_MASK (0x2000000U)

Definition at line 26193 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_DOTCLK_POL_SHIFT

#define LCDIF_VDCTRL0_SET_DOTCLK_POL_SHIFT (25U)

Definition at line 26194 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_ENABLE_POL

#define LCDIF_VDCTRL0_SET_ENABLE_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_SET_ENABLE_POL_MASK)

Definition at line 26192 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_ENABLE_POL_MASK

#define LCDIF_VDCTRL0_SET_ENABLE_POL_MASK (0x1000000U)

Definition at line 26190 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_ENABLE_POL_SHIFT

#define LCDIF_VDCTRL0_SET_ENABLE_POL_SHIFT (24U)

Definition at line 26191 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_ENABLE_PRESENT

#define LCDIF_VDCTRL0_SET_ENABLE_PRESENT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_SET_ENABLE_PRESENT_MASK)

Definition at line 26204 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_ENABLE_PRESENT_MASK

#define LCDIF_VDCTRL0_SET_ENABLE_PRESENT_MASK (0x10000000U)

Definition at line 26202 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_ENABLE_PRESENT_SHIFT

#define LCDIF_VDCTRL0_SET_ENABLE_PRESENT_SHIFT (28U)

Definition at line 26203 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HALF_LINE

#define LCDIF_VDCTRL0_SET_HALF_LINE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_SET_HALF_LINE_MASK)

Definition at line 26180 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HALF_LINE_MASK

#define LCDIF_VDCTRL0_SET_HALF_LINE_MASK (0x80000U)

Definition at line 26178 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HALF_LINE_MODE

#define LCDIF_VDCTRL0_SET_HALF_LINE_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_SET_HALF_LINE_MODE_MASK)

Definition at line 26177 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HALF_LINE_MODE_MASK

#define LCDIF_VDCTRL0_SET_HALF_LINE_MODE_MASK (0x40000U)

Definition at line 26175 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HALF_LINE_MODE_SHIFT

#define LCDIF_VDCTRL0_SET_HALF_LINE_MODE_SHIFT (18U)

Definition at line 26176 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HALF_LINE_SHIFT

#define LCDIF_VDCTRL0_SET_HALF_LINE_SHIFT (19U)

Definition at line 26179 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HSYNC_POL

#define LCDIF_VDCTRL0_SET_HSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_SET_HSYNC_POL_MASK)

Definition at line 26198 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HSYNC_POL_MASK

#define LCDIF_VDCTRL0_SET_HSYNC_POL_MASK (0x4000000U)

Definition at line 26196 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_HSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_SET_HSYNC_POL_SHIFT (26U)

Definition at line 26197 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_RSRVD1

#define LCDIF_VDCTRL0_SET_RSRVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_SET_RSRVD1_MASK)

Definition at line 26189 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_RSRVD1_MASK

#define LCDIF_VDCTRL0_SET_RSRVD1_MASK (0xC00000U)

Definition at line 26187 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_RSRVD1_SHIFT

#define LCDIF_VDCTRL0_SET_RSRVD1_SHIFT (22U)

Definition at line 26188 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_RSRVD2

#define LCDIF_VDCTRL0_SET_RSRVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_SET_RSRVD2_MASK)

Definition at line 26207 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_RSRVD2_MASK

#define LCDIF_VDCTRL0_SET_RSRVD2_MASK (0xE0000000U)

Definition at line 26205 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_RSRVD2_SHIFT

#define LCDIF_VDCTRL0_SET_RSRVD2_SHIFT (29U)

Definition at line 26206 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT

#define LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_MASK)

Definition at line 26186 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_MASK

#define LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_MASK (0x200000U)

Definition at line 26184 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_SHIFT

#define LCDIF_VDCTRL0_SET_VSYNC_PERIOD_UNIT_SHIFT (21U)

Definition at line 26185 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_POL

#define LCDIF_VDCTRL0_SET_VSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_POL_MASK)

Definition at line 26201 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_POL_MASK

#define LCDIF_VDCTRL0_SET_VSYNC_POL_MASK (0x8000000U)

Definition at line 26199 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_SET_VSYNC_POL_SHIFT (27U)

Definition at line 26200 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH

#define LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_MASK)

Definition at line 26174 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_MASK

#define LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)

Definition at line 26172 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_SHIFT

#define LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_SHIFT (0U)

Definition at line 26173 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT

#define LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_MASK)

Definition at line 26183 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_MASK

#define LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)

Definition at line 26181 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_SHIFT

#define LCDIF_VDCTRL0_SET_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)

Definition at line 26182 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_DOTCLK_POL

#define LCDIF_VDCTRL0_TOG_DOTCLK_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_DOTCLK_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_DOTCLK_POL_MASK)

Definition at line 26275 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_DOTCLK_POL_MASK

#define LCDIF_VDCTRL0_TOG_DOTCLK_POL_MASK (0x2000000U)

Definition at line 26273 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_DOTCLK_POL_SHIFT

#define LCDIF_VDCTRL0_TOG_DOTCLK_POL_SHIFT (25U)

Definition at line 26274 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_ENABLE_POL

#define LCDIF_VDCTRL0_TOG_ENABLE_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_ENABLE_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_ENABLE_POL_MASK)

Definition at line 26272 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_ENABLE_POL_MASK

#define LCDIF_VDCTRL0_TOG_ENABLE_POL_MASK (0x1000000U)

Definition at line 26270 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_ENABLE_POL_SHIFT

#define LCDIF_VDCTRL0_TOG_ENABLE_POL_SHIFT (24U)

Definition at line 26271 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_ENABLE_PRESENT

#define LCDIF_VDCTRL0_TOG_ENABLE_PRESENT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_SHIFT)) & LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_MASK)

Definition at line 26284 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_MASK

#define LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_MASK (0x10000000U)

Definition at line 26282 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_SHIFT

#define LCDIF_VDCTRL0_TOG_ENABLE_PRESENT_SHIFT (28U)

Definition at line 26283 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HALF_LINE

#define LCDIF_VDCTRL0_TOG_HALF_LINE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_HALF_LINE_SHIFT)) & LCDIF_VDCTRL0_TOG_HALF_LINE_MASK)

Definition at line 26260 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HALF_LINE_MASK

#define LCDIF_VDCTRL0_TOG_HALF_LINE_MASK (0x80000U)

Definition at line 26258 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HALF_LINE_MODE

#define LCDIF_VDCTRL0_TOG_HALF_LINE_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_SHIFT)) & LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_MASK)

Definition at line 26257 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_MASK

#define LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_MASK (0x40000U)

Definition at line 26255 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_SHIFT

#define LCDIF_VDCTRL0_TOG_HALF_LINE_MODE_SHIFT (18U)

Definition at line 26256 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HALF_LINE_SHIFT

#define LCDIF_VDCTRL0_TOG_HALF_LINE_SHIFT (19U)

Definition at line 26259 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HSYNC_POL

#define LCDIF_VDCTRL0_TOG_HSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_HSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_HSYNC_POL_MASK)

Definition at line 26278 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HSYNC_POL_MASK

#define LCDIF_VDCTRL0_TOG_HSYNC_POL_MASK (0x4000000U)

Definition at line 26276 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_HSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_TOG_HSYNC_POL_SHIFT (26U)

Definition at line 26277 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_RSRVD1

#define LCDIF_VDCTRL0_TOG_RSRVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_RSRVD1_SHIFT)) & LCDIF_VDCTRL0_TOG_RSRVD1_MASK)

Definition at line 26269 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_RSRVD1_MASK

#define LCDIF_VDCTRL0_TOG_RSRVD1_MASK (0xC00000U)

Definition at line 26267 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_RSRVD1_SHIFT

#define LCDIF_VDCTRL0_TOG_RSRVD1_SHIFT (22U)

Definition at line 26268 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_RSRVD2

#define LCDIF_VDCTRL0_TOG_RSRVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_RSRVD2_SHIFT)) & LCDIF_VDCTRL0_TOG_RSRVD2_MASK)

Definition at line 26287 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_RSRVD2_MASK

#define LCDIF_VDCTRL0_TOG_RSRVD2_MASK (0xE0000000U)

Definition at line 26285 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_RSRVD2_SHIFT

#define LCDIF_VDCTRL0_TOG_RSRVD2_SHIFT (29U)

Definition at line 26286 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT

#define LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_MASK)

Definition at line 26266 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_MASK

#define LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_MASK (0x200000U)

Definition at line 26264 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_SHIFT

#define LCDIF_VDCTRL0_TOG_VSYNC_PERIOD_UNIT_SHIFT (21U)

Definition at line 26265 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_POL

#define LCDIF_VDCTRL0_TOG_VSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_POL_MASK)

Definition at line 26281 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_POL_MASK

#define LCDIF_VDCTRL0_TOG_VSYNC_POL_MASK (0x8000000U)

Definition at line 26279 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_TOG_VSYNC_POL_SHIFT (27U)

Definition at line 26280 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH

#define LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_MASK)

Definition at line 26254 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_MASK

#define LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)

Definition at line 26252 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_SHIFT

#define LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_SHIFT (0U)

Definition at line 26253 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT

#define LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_MASK)

Definition at line 26263 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_MASK

#define LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)

Definition at line 26261 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_SHIFT

#define LCDIF_VDCTRL0_TOG_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)

Definition at line 26262 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT

#define LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_SHIFT)) & LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_MASK)

Definition at line 26146 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_MASK

#define LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_MASK (0x200000U)

Definition at line 26144 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_SHIFT

#define LCDIF_VDCTRL0_VSYNC_PERIOD_UNIT_SHIFT (21U)

Definition at line 26145 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_POL

#define LCDIF_VDCTRL0_VSYNC_POL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_POL_SHIFT)) & LCDIF_VDCTRL0_VSYNC_POL_MASK)

Definition at line 26161 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_POL_MASK

#define LCDIF_VDCTRL0_VSYNC_POL_MASK (0x8000000U)

Definition at line 26159 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_POL_SHIFT

#define LCDIF_VDCTRL0_VSYNC_POL_SHIFT (27U)

Definition at line 26160 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH

#define LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_MASK)

Definition at line 26134 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_MASK

#define LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_MASK (0x3FFFFU)

Definition at line 26132 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_SHIFT

#define LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_SHIFT (0U)

Definition at line 26133 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT

#define LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_SHIFT)) & LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_MASK)

Definition at line 26143 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_MASK

#define LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_MASK (0x100000U)

Definition at line 26141 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_SHIFT

#define LCDIF_VDCTRL0_VSYNC_PULSE_WIDTH_UNIT_SHIFT (20U)

Definition at line 26142 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL1_VSYNC_PERIOD

#define LCDIF_VDCTRL1_VSYNC_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL1_VSYNC_PERIOD_SHIFT)) & LCDIF_VDCTRL1_VSYNC_PERIOD_MASK)

Definition at line 26294 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL1_VSYNC_PERIOD_MASK

#define LCDIF_VDCTRL1_VSYNC_PERIOD_MASK (0xFFFFFFFFU)

Definition at line 26292 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL1_VSYNC_PERIOD_SHIFT

#define LCDIF_VDCTRL1_VSYNC_PERIOD_SHIFT (0U)

Definition at line 26293 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL2_HSYNC_PERIOD

#define LCDIF_VDCTRL2_HSYNC_PERIOD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL2_HSYNC_PERIOD_SHIFT)) & LCDIF_VDCTRL2_HSYNC_PERIOD_MASK)

Definition at line 26301 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL2_HSYNC_PERIOD_MASK

#define LCDIF_VDCTRL2_HSYNC_PERIOD_MASK (0x3FFFFU)

Definition at line 26299 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL2_HSYNC_PERIOD_SHIFT

#define LCDIF_VDCTRL2_HSYNC_PERIOD_SHIFT (0U)

Definition at line 26300 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH

#define LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_SHIFT)) & LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_MASK)

Definition at line 26304 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_MASK

#define LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_MASK (0xFFFC0000U)

Definition at line 26302 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_SHIFT

#define LCDIF_VDCTRL2_HSYNC_PULSE_WIDTH_SHIFT (18U)

Definition at line 26303 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT

#define LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_SHIFT)) & LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_MASK)

Definition at line 26314 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_MASK

#define LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_MASK (0xFFF0000U)

Definition at line 26312 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_SHIFT

#define LCDIF_VDCTRL3_HORIZONTAL_WAIT_CNT_SHIFT (16U)

Definition at line 26313 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_MUX_SYNC_SIGNALS

#define LCDIF_VDCTRL3_MUX_SYNC_SIGNALS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_SHIFT)) & LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_MASK)

Definition at line 26320 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_MASK

#define LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_MASK (0x20000000U)

Definition at line 26318 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_SHIFT

#define LCDIF_VDCTRL3_MUX_SYNC_SIGNALS_SHIFT (29U)

Definition at line 26319 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_RSRVD0

#define LCDIF_VDCTRL3_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_RSRVD0_SHIFT)) & LCDIF_VDCTRL3_RSRVD0_MASK)

Definition at line 26323 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_RSRVD0_MASK

#define LCDIF_VDCTRL3_RSRVD0_MASK (0xC0000000U)

Definition at line 26321 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_RSRVD0_SHIFT

#define LCDIF_VDCTRL3_RSRVD0_SHIFT (30U)

Definition at line 26322 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_VERTICAL_WAIT_CNT

#define LCDIF_VDCTRL3_VERTICAL_WAIT_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_SHIFT)) & LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_MASK)

Definition at line 26311 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_MASK

#define LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_MASK (0xFFFFU)

Definition at line 26309 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_SHIFT

#define LCDIF_VDCTRL3_VERTICAL_WAIT_CNT_SHIFT (0U)

Definition at line 26310 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_VSYNC_ONLY

#define LCDIF_VDCTRL3_VSYNC_ONLY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL3_VSYNC_ONLY_SHIFT)) & LCDIF_VDCTRL3_VSYNC_ONLY_MASK)

Definition at line 26317 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_VSYNC_ONLY_MASK

#define LCDIF_VDCTRL3_VSYNC_ONLY_MASK (0x10000000U)

Definition at line 26315 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL3_VSYNC_ONLY_SHIFT

#define LCDIF_VDCTRL3_VSYNC_ONLY_SHIFT (28U)

Definition at line 26316 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_DOTCLK_DLY_SEL

#define LCDIF_VDCTRL4_DOTCLK_DLY_SEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_DOTCLK_DLY_SEL_SHIFT)) & LCDIF_VDCTRL4_DOTCLK_DLY_SEL_MASK)

Definition at line 26339 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_DOTCLK_DLY_SEL_MASK

#define LCDIF_VDCTRL4_DOTCLK_DLY_SEL_MASK (0xE0000000U)

Definition at line 26337 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_DOTCLK_DLY_SEL_SHIFT

#define LCDIF_VDCTRL4_DOTCLK_DLY_SEL_SHIFT (29U)

Definition at line 26338 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT

#define LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_SHIFT)) & LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_MASK)

Definition at line 26330 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_MASK

#define LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_MASK (0x3FFFFU)

Definition at line 26328 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_SHIFT

#define LCDIF_VDCTRL4_DOTCLK_H_VALID_DATA_CNT_SHIFT (0U)

Definition at line 26329 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_RSRVD0

#define LCDIF_VDCTRL4_RSRVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_RSRVD0_SHIFT)) & LCDIF_VDCTRL4_RSRVD0_MASK)

Definition at line 26336 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_RSRVD0_MASK

#define LCDIF_VDCTRL4_RSRVD0_MASK (0x1FF80000U)

Definition at line 26334 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_RSRVD0_SHIFT

#define LCDIF_VDCTRL4_RSRVD0_SHIFT (19U)

Definition at line 26335 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_SYNC_SIGNALS_ON

#define LCDIF_VDCTRL4_SYNC_SIGNALS_ON | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << LCDIF_VDCTRL4_SYNC_SIGNALS_ON_SHIFT)) & LCDIF_VDCTRL4_SYNC_SIGNALS_ON_MASK)

Definition at line 26333 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_SYNC_SIGNALS_ON_MASK

#define LCDIF_VDCTRL4_SYNC_SIGNALS_ON_MASK (0x40000U)

Definition at line 26331 of file MIMXRT1062.h.

## ◆ LCDIF_VDCTRL4_SYNC_SIGNALS_ON_SHIFT

#define LCDIF_VDCTRL4_SYNC_SIGNALS_ON_SHIFT (18U)

Definition at line 26332 of file MIMXRT1062.h.