Callisto4Bootloader: Globals

Callisto4Bootloader

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - b -

- BEE : MIMXRT1062.h
- BEE_ADDR_OFFSET0_ADDR_OFFSET0 : MIMXRT1062.h
- BEE_ADDR_OFFSET0_ADDR_OFFSET0_LOCK : MIMXRT1062.h
- BEE_ADDR_OFFSET0_ADDR_OFFSET0_LOCK_MASK : MIMXRT1062.h
- BEE_ADDR_OFFSET0_ADDR_OFFSET0_LOCK_SHIFT : MIMXRT1062.h
- BEE_ADDR_OFFSET0_ADDR_OFFSET0_MASK : MIMXRT1062.h
- BEE_ADDR_OFFSET0_ADDR_OFFSET0_SHIFT : MIMXRT1062.h
- BEE_ADDR_OFFSET1_ADDR_OFFSET1 : MIMXRT1062.h
- BEE_ADDR_OFFSET1_ADDR_OFFSET1_LOCK : MIMXRT1062.h
- BEE_ADDR_OFFSET1_ADDR_OFFSET1_LOCK_MASK : MIMXRT1062.h
- BEE_ADDR_OFFSET1_ADDR_OFFSET1_LOCK_SHIFT : MIMXRT1062.h
- BEE_ADDR_OFFSET1_ADDR_OFFSET1_MASK : MIMXRT1062.h
- BEE_ADDR_OFFSET1_ADDR_OFFSET1_SHIFT : MIMXRT1062.h
- BEE_AES_KEY0_W0_KEY0 : MIMXRT1062.h
- BEE_AES_KEY0_W0_KEY0_MASK : MIMXRT1062.h
- BEE_AES_KEY0_W0_KEY0_SHIFT : MIMXRT1062.h
- BEE_AES_KEY0_W1_KEY1 : MIMXRT1062.h
- BEE_AES_KEY0_W1_KEY1_MASK : MIMXRT1062.h
- BEE_AES_KEY0_W1_KEY1_SHIFT : MIMXRT1062.h
- BEE_AES_KEY0_W2_KEY2 : MIMXRT1062.h
- BEE_AES_KEY0_W2_KEY2_MASK : MIMXRT1062.h
- BEE_AES_KEY0_W2_KEY2_SHIFT : MIMXRT1062.h
- BEE_AES_KEY0_W3_KEY3 : MIMXRT1062.h
- BEE_AES_KEY0_W3_KEY3_MASK : MIMXRT1062.h
- BEE_AES_KEY0_W3_KEY3_SHIFT : MIMXRT1062.h
- BEE_BASE : MIMXRT1062.h
- BEE_BASE_ADDRS : MIMXRT1062.h
- BEE_BASE_PTRS : MIMXRT1062.h
- BEE_CTR_NONCE0_W0_NONCE00 : MIMXRT1062.h
- BEE_CTR_NONCE0_W0_NONCE00_MASK : MIMXRT1062.h
- BEE_CTR_NONCE0_W0_NONCE00_SHIFT : MIMXRT1062.h
- BEE_CTR_NONCE0_W1_NONCE01 : MIMXRT1062.h
- BEE_CTR_NONCE0_W1_NONCE01_MASK : MIMXRT1062.h
- BEE_CTR_NONCE0_W1_NONCE01_SHIFT : MIMXRT1062.h
- BEE_CTR_NONCE0_W2_NONCE02 : MIMXRT1062.h
- BEE_CTR_NONCE0_W2_NONCE02_MASK : MIMXRT1062.h
- BEE_CTR_NONCE0_W2_NONCE02_SHIFT : MIMXRT1062.h
- BEE_CTR_NONCE0_W3_NONCE03 : MIMXRT1062.h
- BEE_CTR_NONCE0_W3_NONCE03_MASK : MIMXRT1062.h
- BEE_CTR_NONCE0_W3_NONCE03_SHIFT : MIMXRT1062.h
- BEE_CTR_NONCE1_W0_NONCE10 : MIMXRT1062.h
- BEE_CTR_NONCE1_W0_NONCE10_MASK : MIMXRT1062.h
- BEE_CTR_NONCE1_W0_NONCE10_SHIFT : MIMXRT1062.h
- BEE_CTR_NONCE1_W1_NONCE11 : MIMXRT1062.h
- BEE_CTR_NONCE1_W1_NONCE11_MASK : MIMXRT1062.h
- BEE_CTR_NONCE1_W1_NONCE11_SHIFT : MIMXRT1062.h
- BEE_CTR_NONCE1_W2_NONCE12 : MIMXRT1062.h
- BEE_CTR_NONCE1_W2_NONCE12_MASK : MIMXRT1062.h
- BEE_CTR_NONCE1_W2_NONCE12_SHIFT : MIMXRT1062.h
- BEE_CTR_NONCE1_W3_NONCE13 : MIMXRT1062.h
- BEE_CTR_NONCE1_W3_NONCE13_MASK : MIMXRT1062.h
- BEE_CTR_NONCE1_W3_NONCE13_SHIFT : MIMXRT1062.h
- BEE_CTRL_AC_PROT_EN : MIMXRT1062.h
- BEE_CTRL_AC_PROT_EN_LOCK : MIMXRT1062.h
- BEE_CTRL_AC_PROT_EN_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_AC_PROT_EN_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_AC_PROT_EN_MASK : MIMXRT1062.h
- BEE_CTRL_AC_PROT_EN_SHIFT : MIMXRT1062.h
- BEE_CTRL_BEE_ENABLE : MIMXRT1062.h
- BEE_CTRL_BEE_ENABLE_LOCK : MIMXRT1062.h
- BEE_CTRL_BEE_ENABLE_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_BEE_ENABLE_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_BEE_ENABLE_MASK : MIMXRT1062.h
- BEE_CTRL_BEE_ENABLE_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R0 : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R0_LOCK : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R0_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R0_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R0_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R0_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R1 : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R1_LOCK : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R1_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R1_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R1_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_AES_MODE_R1_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_CLK_EN : MIMXRT1062.h
- BEE_CTRL_CTRL_CLK_EN_LOCK : MIMXRT1062.h
- BEE_CTRL_CTRL_CLK_EN_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_CLK_EN_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_CLK_EN_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_CLK_EN_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_SFTRST_N : MIMXRT1062.h
- BEE_CTRL_CTRL_SFTRST_N_LOCK : MIMXRT1062.h
- BEE_CTRL_CTRL_SFTRST_N_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_SFTRST_N_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_CTRL_SFTRST_N_MASK : MIMXRT1062.h
- BEE_CTRL_CTRL_SFTRST_N_SHIFT : MIMXRT1062.h
- BEE_CTRL_KEY_REGION_SEL : MIMXRT1062.h
- BEE_CTRL_KEY_REGION_SEL_LOCK : MIMXRT1062.h
- BEE_CTRL_KEY_REGION_SEL_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_KEY_REGION_SEL_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_KEY_REGION_SEL_MASK : MIMXRT1062.h
- BEE_CTRL_KEY_REGION_SEL_SHIFT : MIMXRT1062.h
- BEE_CTRL_KEY_VALID : MIMXRT1062.h
- BEE_CTRL_KEY_VALID_LOCK : MIMXRT1062.h
- BEE_CTRL_KEY_VALID_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_KEY_VALID_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_KEY_VALID_MASK : MIMXRT1062.h
- BEE_CTRL_KEY_VALID_SHIFT : MIMXRT1062.h
- BEE_CTRL_LITTLE_ENDIAN : MIMXRT1062.h
- BEE_CTRL_LITTLE_ENDIAN_LOCK : MIMXRT1062.h
- BEE_CTRL_LITTLE_ENDIAN_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_LITTLE_ENDIAN_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_LITTLE_ENDIAN_MASK : MIMXRT1062.h
- BEE_CTRL_LITTLE_ENDIAN_SHIFT : MIMXRT1062.h
- BEE_CTRL_REGION0_KEY_LOCK : MIMXRT1062.h
- BEE_CTRL_REGION0_KEY_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_REGION0_KEY_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_REGION1_ADDR_LOCK : MIMXRT1062.h
- BEE_CTRL_REGION1_ADDR_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_REGION1_ADDR_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_REGION1_KEY_LOCK : MIMXRT1062.h
- BEE_CTRL_REGION1_KEY_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_REGION1_KEY_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R0 : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R0_LOCK : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R0_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R0_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R0_MASK : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R0_SHIFT : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R1 : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R1_LOCK : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R1_LOCK_MASK : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R1_LOCK_SHIFT : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R1_MASK : MIMXRT1062.h
- BEE_CTRL_SECURITY_LEVEL_R1_SHIFT : MIMXRT1062.h
- BEE_IRQHandler() : startup_mimxrt1062.c
- BEE_IRQn : MIMXRT1062.h
- BEE_REGION1_BOT_REGION1_BOT : MIMXRT1062.h
- BEE_REGION1_BOT_REGION1_BOT_MASK : MIMXRT1062.h
- BEE_REGION1_BOT_REGION1_BOT_SHIFT : MIMXRT1062.h
- BEE_REGION1_TOP_REGION1_TOP : MIMXRT1062.h
- BEE_REGION1_TOP_REGION1_TOP_MASK : MIMXRT1062.h
- BEE_REGION1_TOP_REGION1_TOP_SHIFT : MIMXRT1062.h
- BEE_STATUS_BEE_IDLE : MIMXRT1062.h
- BEE_STATUS_BEE_IDLE_MASK : MIMXRT1062.h
- BEE_STATUS_BEE_IDLE_SHIFT : MIMXRT1062.h
- BEE_STATUS_IRQ_VEC : MIMXRT1062.h
- BEE_STATUS_IRQ_VEC_MASK : MIMXRT1062.h
- BEE_STATUS_IRQ_VEC_SHIFT : MIMXRT1062.h
- bl_api_init() : bl_api.c , bl_api.h
- BL_APP_VECTOR_TABLE_ADDRESS : bootloader_config.h
- BL_CONFIG_HS_USB_HID : bootloader_config.h
- BL_CONFIG_LPUART : bootloader_config.h
- BL_CONFIG_LPUART_1 : bootloader_config.h
- BL_DEFAULT_PERIPHERAL_DETECT_TIMEOUT : bootloader_config.h
- BL_EXPANDED_FRAMING_PACKET_SIZE : bootloader_config.h
- BL_EXPANDED_USB_HID_PACKET_SIZE : bootloader_config.h
- BL_FEATURE_CRC_CHECK : bootloader_config.h
- BL_FEATURE_EXPAND_MEMORY : bootloader_config.h
- BL_FEATURE_EXPAND_PACKET_SIZE : bootloader_config.h
- BL_FEATURE_EXTERNAL_MEMORY_PROPERTY : bootloader_config.h
- BL_FEATURE_FLASH_CHECK_CUMULATIVE_WRITE : bootloader_config.h
- BL_FEATURE_FLEXSPI_NOR_MODULE : bootloader_config.h
- BL_FEATURE_GEN_KEYBLOB : bootloader_config.h
- BL_FEATURE_HAS_FLEXSPI_NOR_ROMAPI : bootloader_config.h
- BL_FEATURE_HAS_NO_INTERNAL_FLASH : bootloader_config.h
- BL_FEATURE_HAS_NO_READ_SOURCE : bootloader_config.h
- BL_FEATURE_KEYBLOB_BK_SIZE : bootloader_config.h
- BL_FEATURE_MIN_PROFILE : bootloader_config.h
- BL_FEATURE_MMC_MODULE : bootloader_config.h
- BL_FEATURE_MMC_MODULE_ENABLE_PERMANENT_CONFIG : bootloader_config.h
- BL_FEATURE_MMC_MODULE_ERASE_VERIFY : bootloader_config.h
- BL_FEATURE_MMC_MODULE_PERIPHERAL_INSTANCE : bootloader_config.h
- BL_FEATURE_OCOTP_MODULE : bootloader_config.h
- BL_FEATURE_ROM_UART_PORT : bootloader_config.h
- BL_FEATURE_SD_MODULE : bootloader_config.h
- BL_FEATURE_SD_MODULE_ERASE_VERIFY : bootloader_config.h
- BL_FEATURE_SD_MODULE_PERIPHERAL_INSTANCE : bootloader_config.h
- BL_FEATURE_SEMC_NAND_MODULE : bootloader_config.h
- BL_FEATURE_SEMC_NOR_MODULE : bootloader_config.h
- BL_FEATURE_SPI_NOR_EEPROM_MODULE : bootloader_config.h
- BL_FEATURE_SPI_NOR_EEPROM_MODULE_ERASE_VERIFY : bootloader_config.h
- BL_FEATURE_SPINAND_MODULE : bootloader_config.h
- BL_FEATURE_SPINAND_MODULE_ERASE_VERIFY : bootloader_config.h
- BL_FEATURE_SPINAND_MODULE_PERIPHERAL_FLEXSPI : bootloader_config.h
- BL_FEATURE_SPINAND_MODULE_PERIPHERAL_INSTANCE : bootloader_config.h
- BL_FEATURE_UART_AUTOBAUD_IRQ : bootloader_config.h
- BL_FEATURE_UART_RX_PULLUP : bootloader_config.h
- BL_FEATURE_UID_IN_FUSE : bootloader_config.h
- BL_SysTick_DelayTicks() : c4_colours.c , c4_error_codes.c , c4_qspi.c , bootloader.c , watchdog_test.c
- BL_TARGET_FLASH : bootloader_config.h
- BLUE_LED_GPIO_PIN : c4_colours.c
- BOARD_ACCEL_I2C_BASEADDR : board.h
- BOARD_ACCEL_I2C_CLOCK_FREQ : board.h
- BOARD_ACCEL_I2C_CLOCK_SOURCE_DIVIDER : board.h
- BOARD_ACCEL_I2C_CLOCK_SOURCE_SELECT : board.h
- BOARD_ARDUINO_I2C_INDEX : board.h
- BOARD_ARDUINO_I2C_IRQ : board.h
- BOARD_ARDUINO_INT_IRQ : board.h
- BOARD_BootClockRUN() : clock_config.c , clock_config.h
- BOARD_BOOTCLOCKRUN_AHB_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_CAN_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_CKIL_SYNC_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_CLK_1M : clock_config.h
- BOARD_BOOTCLOCKRUN_CLK_24M : clock_config.h
- BOARD_BOOTCLOCKRUN_CLKO1_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_CLKO2_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_CORE_CLOCK : clock_config.h
- BOARD_BOOTCLOCKRUN_CSI_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_ENET1_TX_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_ENET2_125M_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_ENET2_TX_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_ENET_125M_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_ENET_25M_REF_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_FLEXIO1_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_FLEXIO2_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_FLEXSPI2_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_FLEXSPI_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_GPT1_IPG_CLK_HIGHFREQ : clock_config.h
- BOARD_BOOTCLOCKRUN_GPT2_IPG_CLK_HIGHFREQ : clock_config.h
- BOARD_BOOTCLOCKRUN_IPG_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_LCDIF_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_LPI2C_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_LPSPI_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_LVDS1_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_MQS_MCLK : clock_config.h
- BOARD_BOOTCLOCKRUN_PERCLK_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_PLL7_MAIN_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI1_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI1_MCLK1 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI1_MCLK2 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI1_MCLK3 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI2_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI2_MCLK1 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI2_MCLK2 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI2_MCLK3 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI3_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI3_MCLK1 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI3_MCLK2 : clock_config.h
- BOARD_BOOTCLOCKRUN_SAI3_MCLK3 : clock_config.h
- BOARD_BOOTCLOCKRUN_SEMC_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_SPDIF0_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_SPDIF0_EXTCLK_OUT : clock_config.h
- BOARD_BOOTCLOCKRUN_TRACE_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_UART_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_USBPHY1_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_USBPHY2_CLK : clock_config.h
- BOARD_BOOTCLOCKRUN_USDHC1_CLK_ROOT : clock_config.h
- BOARD_BOOTCLOCKRUN_USDHC2_CLK_ROOT : clock_config.h
- BOARD_BT_UART_BASEADDR : board.h
- BOARD_BT_UART_CLK_FREQ : board.h
- BOARD_BT_UART_IRQ : board.h
- BOARD_BT_UART_IRQ_HANDLER : board.h
- BOARD_CAMERA_I2C_BASEADDR : board.h
- BOARD_CAMERA_I2C_CLOCK_FREQ : board.h
- BOARD_CAMERA_I2C_CLOCK_SOURCE_DIVIDER : board.h
- BOARD_CAMERA_I2C_CLOCK_SOURCE_SELECT : board.h
- BOARD_CAMERA_I2C_SCL_GPIO : board.h
- BOARD_CAMERA_I2C_SCL_PIN : board.h
- BOARD_CAMERA_I2C_SDA_GPIO : board.h
- BOARD_CAMERA_I2C_SDA_PIN : board.h
- BOARD_CAMERA_PWDN_GPIO : board.h
- BOARD_CAMERA_PWDN_PIN : board.h
- BOARD_CODEC_I2C_BASEADDR : board.h
- BOARD_CODEC_I2C_CLOCK_FREQ : board.h
- BOARD_CODEC_I2C_CLOCK_SOURCE_DIVIDER : board.h
- BOARD_CODEC_I2C_CLOCK_SOURCE_SELECT : board.h
- BOARD_CODEC_I2C_INSTANCE : board.h
- BOARD_ConfigMPU() : board.h , board.c
- BOARD_CSI_D2_PERIPHERAL : pin_mux.h
- BOARD_CSI_D2_SIGNAL : pin_mux.h
- BOARD_CSI_D3_PERIPHERAL : pin_mux.h
- BOARD_CSI_D3_SIGNAL : pin_mux.h
- BOARD_CSI_D4_PERIPHERAL : pin_mux.h
- BOARD_CSI_D4_SIGNAL : pin_mux.h
- BOARD_CSI_D5_PERIPHERAL : pin_mux.h
- BOARD_CSI_D5_SIGNAL : pin_mux.h
- BOARD_DEBUG_UART_BASEADDR : board.h
- BOARD_DEBUG_UART_BAUDRATE : board.h
- BOARD_DEBUG_UART_CLK_FREQ : board.h
- BOARD_DEBUG_UART_INSTANCE : board.h
- BOARD_DEBUG_UART_TYPE : board.h
- BOARD_DebugConsoleSrcFreq() : board.c , board.h
- BOARD_ENET0_PHY_ADDRESS : board.h
- BOARD_ENET_CRS_DV_PERIPHERAL : pin_mux.h
- BOARD_ENET_CRS_DV_SIGNAL : pin_mux.h
- BOARD_ENET_MDC_PERIPHERAL : pin_mux.h
- BOARD_ENET_MDC_SIGNAL : pin_mux.h
- BOARD_ENET_MDIO_PERIPHERAL : pin_mux.h
- BOARD_ENET_MDIO_SIGNAL : pin_mux.h
- BOARD_ENET_RXD0_CHANNEL : pin_mux.h
- BOARD_ENET_RXD0_PERIPHERAL : pin_mux.h
- BOARD_ENET_RXD0_SIGNAL : pin_mux.h
- BOARD_ENET_RXD1_CHANNEL : pin_mux.h
- BOARD_ENET_RXD1_PERIPHERAL : pin_mux.h
- BOARD_ENET_RXD1_SIGNAL : pin_mux.h
- BOARD_ENET_RXER_PERIPHERAL : pin_mux.h
- BOARD_ENET_RXER_SIGNAL : pin_mux.h
- BOARD_ENET_TX_CLK_PERIPHERAL : pin_mux.h
- BOARD_ENET_TX_CLK_SIGNAL : pin_mux.h
- BOARD_ENET_TXD0_CHANNEL : pin_mux.h
- BOARD_ENET_TXD0_PERIPHERAL : pin_mux.h
- BOARD_ENET_TXD0_SIGNAL : pin_mux.h
- BOARD_ENET_TXD1_CHANNEL : pin_mux.h
- BOARD_ENET_TXD1_PERIPHERAL : pin_mux.h
- BOARD_ENET_TXD1_SIGNAL : pin_mux.h
- BOARD_ENET_TXEN_PERIPHERAL : pin_mux.h
- BOARD_ENET_TXEN_SIGNAL : pin_mux.h
- BOARD_FLASH_SIZE : board.h
- BOARD_HAS_SDCARD : board.h
- BOARD_InitBootClocks() : clock_config.c , clock_config.h
- BOARD_InitBootPeripherals() : peripherals.h , peripherals.c
- BOARD_InitBootPins() : pin_mux.c , pin_mux.h
- BOARD_InitDebugConsole() : board.c , board.h
- BOARD_INITGT202SHIELD_IRQ_DIRECTION : board.h
- BOARD_INITGT202SHIELD_IRQ_GPIO : board.h
- BOARD_INITGT202SHIELD_IRQ_GPIO_PIN : board.h
- BOARD_INITGT202SHIELD_IRQ_LABEL : board.h
- BOARD_INITGT202SHIELD_IRQ_NAME : board.h
- BOARD_INITGT202SHIELD_IRQ_PIN_NAME : board.h
- BOARD_INITGT202SHIELD_IRQ_PORT : board.h
- BOARD_INITGT202SHIELD_PWRON_DIRECTION : board.h
- BOARD_INITGT202SHIELD_PWRON_GPIO : board.h
- BOARD_INITGT202SHIELD_PWRON_GPIO_PIN : board.h
- BOARD_INITGT202SHIELD_PWRON_LABEL : board.h
- BOARD_INITGT202SHIELD_PWRON_NAME : board.h
- BOARD_INITGT202SHIELD_PWRON_PIN_NAME : board.h
- BOARD_INITGT202SHIELD_PWRON_PORT : board.h
- BOARD_InitLPSPI3() : bootloader.c
- BOARD_InitModuleClock() : bootloader.c
- BOARD_InitPeripherals() : peripherals.c , peripherals.h
- BOARD_InitPins() : pin_mux.c , pin_mux.h
- BOARD_INITSILEX2401SHIELD_IRQ_DIRECTION : board.h
- BOARD_INITSILEX2401SHIELD_IRQ_GPIO : board.h
- BOARD_INITSILEX2401SHIELD_IRQ_GPIO_PIN : board.h
- BOARD_INITSILEX2401SHIELD_IRQ_LABEL : board.h
- BOARD_INITSILEX2401SHIELD_IRQ_NAME : board.h
- BOARD_INITSILEX2401SHIELD_IRQ_PIN_NAME : board.h
- BOARD_INITSILEX2401SHIELD_IRQ_PORT : board.h
- BOARD_INITSILEX2401SHIELD_PWRON_DIRECTION : board.h
- BOARD_INITSILEX2401SHIELD_PWRON_GPIO : board.h
- BOARD_INITSILEX2401SHIELD_PWRON_GPIO_PIN : board.h
- BOARD_INITSILEX2401SHIELD_PWRON_LABEL : board.h
- BOARD_INITSILEX2401SHIELD_PWRON_NAME : board.h
- BOARD_INITSILEX2401SHIELD_PWRON_PIN_NAME : board.h
- BOARD_INITSILEX2401SHIELD_PWRON_PORT : board.h
- BOARD_LCDIF_D10_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D10_SIGNAL : pin_mux.h
- BOARD_LCDIF_D11_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D11_SIGNAL : pin_mux.h
- BOARD_LCDIF_D12_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D12_SIGNAL : pin_mux.h
- BOARD_LCDIF_D13_CHANNEL : pin_mux.h
- BOARD_LCDIF_D13_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D13_SIGNAL : pin_mux.h
- BOARD_LCDIF_D14_CHANNEL : pin_mux.h
- BOARD_LCDIF_D14_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D14_SIGNAL : pin_mux.h
- BOARD_LCDIF_D15_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D15_SIGNAL : pin_mux.h
- BOARD_LCDIF_D8_CHANNEL : pin_mux.h
- BOARD_LCDIF_D8_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D8_SIGNAL : pin_mux.h
- BOARD_LCDIF_D9_CHANNEL : pin_mux.h
- BOARD_LCDIF_D9_PERIPHERAL : pin_mux.h
- BOARD_LCDIF_D9_SIGNAL : pin_mux.h
- BOARD_MMC_HOST_BASEADDR : board.h
- BOARD_MMC_HOST_CLK_FREQ : board.h
- BOARD_MMC_HOST_IRQ : board.h
- BOARD_MMC_Pin_Config() : board.c , board.h
- BOARD_MMC_SUPPORT_8BIT_BUS : board.h
- BOARD_MMC_VCC_SUPPLY : board.h
- BOARD_MMC_VCCQ_SUPPLY : board.h
- BOARD_NAME : board.h
- BOARD_SD1_CLK_PERIPHERAL : pin_mux.h
- BOARD_SD1_CLK_SIGNAL : pin_mux.h
- BOARD_SD1_CMD_PERIPHERAL : pin_mux.h
- BOARD_SD1_CMD_SIGNAL : pin_mux.h
- BOARD_SD1_D0_PERIPHERAL : pin_mux.h
- BOARD_SD1_D0_SIGNAL : pin_mux.h
- BOARD_SD1_D1_PERIPHERAL : pin_mux.h
- BOARD_SD1_D1_SIGNAL : pin_mux.h
- BOARD_SD1_D3_GPIO : pin_mux.h
- BOARD_SD1_D3_PIN : pin_mux.h
- BOARD_SD1_D3_PORT : pin_mux.h
- BOARD_SD_HOST_BASEADDR : board.h
- BOARD_SD_HOST_CLK_FREQ : board.h
- BOARD_SD_HOST_IRQ : board.h
- BOARD_SD_HOST_SUPPORT_HS200_FREQ : board.h
- BOARD_SD_HOST_SUPPORT_SDR104_FREQ : board.h
- BOARD_SD_Pin_Config() : board.h , board.c
- BOARD_SD_POWER_RESET_GPIO : board.h
- BOARD_SD_POWER_RESET_GPIO_PIN : board.h
- BOARD_SEMC_DQS_GPIO : pin_mux.h
- BOARD_SEMC_DQS_PIN : pin_mux.h
- BOARD_SEMC_DQS_PORT : pin_mux.h
- BOARD_SPDIF_OUT_PERIPHERAL : pin_mux.h
- BOARD_SPDIF_OUT_SIGNAL : pin_mux.h
- BOARD_UART1_RXD_PERIPHERAL : pin_mux.h
- BOARD_UART1_RXD_SIGNAL : pin_mux.h
- BOARD_UART1_TXD_PERIPHERAL : pin_mux.h
- BOARD_UART1_TXD_SIGNAL : pin_mux.h
- BOARD_UART_IRQ : board.h
- BOARD_UART_IRQ_HANDLER : board.h
- BOARD_USB_PHY_D_CAL : board.h
- BOARD_USB_PHY_TXCAL45DM : board.h
- BOARD_USB_PHY_TXCAL45DP : board.h
- BOARD_USDHC1_BASEADDR : board.h
- BOARD_USDHC1_CLK_FREQ : board.h
- BOARD_USDHC2_BASEADDR : board.h
- BOARD_USDHC2_CLK_FREQ : board.h
- BOARD_USDHC_CARD_INSERT_CD_LEVEL : board.h
- BOARD_USDHC_CD_CLEAR_INTERRUPT : board.h
- BOARD_USDHC_CD_GPIO_BASE : board.h
- BOARD_USDHC_CD_GPIO_INIT : board.h
- BOARD_USDHC_CD_GPIO_PIN : board.h
- BOARD_USDHC_CD_INTERRUPT_STATUS : board.h
- BOARD_USDHC_CD_PORT_IRQ : board.h
- BOARD_USDHC_CD_PORT_IRQ_HANDLER : board.h
- BOARD_USDHC_CD_STATUS : board.h
- BOARD_USDHC_MMCCARD_POWER_CONTROL : board.h
- BOARD_USDHC_MMCCARD_POWER_CONTROL_INIT : board.h
- BOARD_USDHC_SDCARD_POWER_CONTROL : board.h
- BOARD_USDHC_SDCARD_POWER_CONTROL_INIT : board.h
- BOARD_USER_BUTTON_GPIO : board.h
- BOARD_USER_BUTTON_GPIO_PIN : board.h
- BOARD_USER_BUTTON_IRQ : board.h
- BOARD_USER_BUTTON_IRQ_HANDLER : board.h
- BOARD_USER_BUTTON_NAME : board.h
- BOARD_USER_LED_BLUE_GPIO : pin_mux.h
- BOARD_USER_LED_BLUE_PIN : pin_mux.h
- BOARD_USER_LED_BLUE_PORT : pin_mux.h
- BOARD_USER_LED_GPIO : board.h
- BOARD_USER_LED_GPIO_PIN : board.h
- BOARD_USER_LED_GREEN_GPIO : pin_mux.h
- BOARD_USER_LED_GREEN_PIN : pin_mux.h
- BOARD_USER_LED_GREEN_PORT : pin_mux.h
- BOARD_USER_LED_RED_GPIO : pin_mux.h
- BOARD_USER_LED_RED_PIN : pin_mux.h
- BOARD_USER_LED_RED_PORT : pin_mux.h
- BOARD_XTAL0_CLK_HZ : clock_config.h
- BOARD_XTAL32K_CLK_HZ : clock_config.h
- boot_data : bootloader.c
- boot_mode_option_t : bootloader_common.h
- bootdevice_option_t : bootloader_common.h
- bootloader_clock_option_t : bootloader_common.h
- bootloader_watchdog_deinit() : bootloader_common.h
- bootloader_watchdog_init() : bootloader_common.h
- bootloader_watchdog_service() : bootloader_common.h
- BSWAP_16 : bootloader_common.h
- BSWAP_32 : bootloader_common.h
- BUF_LEN : bootloader.c
- BusFault_IRQn : MIMXRT1062.h