Callisto4Bootloader: flash_run_context_t Union Reference

Callisto4Bootloader

Data Fields
flash_run_context_t Union Reference

`#include <flexspi_nor_flash.h>`

## Data Fields

struct {
uint8_t por_mode
uint8_t current_mode
uint8_t exit_no_cmd_sequence
uint8_t restore_sequence
} | B
uint32_t | U

## Detailed Description

Definition at line 145 of file flexspi_nor_flash.h.

## Field Documentation

## ◆ B

struct { ... } flash_run_context_t::B

## ◆ current_mode

uint8_t flash_run_context_t::current_mode

Definition at line 150 of file flexspi_nor_flash.h.

## ◆ exit_no_cmd_sequence

uint8_t flash_run_context_t::exit_no_cmd_sequence

Definition at line 151 of file flexspi_nor_flash.h.

## ◆ por_mode

uint8_t flash_run_context_t::por_mode

Definition at line 149 of file flexspi_nor_flash.h.

## ◆ restore_sequence

uint8_t flash_run_context_t::restore_sequence

Definition at line 152 of file flexspi_nor_flash.h.

## ◆ U

uint32_t flash_run_context_t::U

Definition at line 154 of file flexspi_nor_flash.h.

The documentation for this union was generated from the following file:

- drivers/flexspi_nor_flash.h