Callisto4Bootloader: TSC Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
TSC Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| TSC Register Masks

## Data Structures

struct | TSC_Type

## Macros

#define | TSC_BASE (0x400E0000u)
#define | TSC ((TSC_Type *)TSC_BASE)
#define | TSC_BASE_ADDRS { TSC_BASE }
#define | TSC_BASE_PTRS { TSC }
#define | TSC_IRQS { TSC_DIG_IRQn }
#define | TSC_BASIC_SETTING__4_5_WIRE_MASK TSC_BASIC_SETTING_WIRE_4_5_MASK
#define | TSC_BASIC_SETTING__4_5_WIRE_SHIFT TSC_BASIC_SETTING_WIRE_4_5_SHIFT
#define | TSC_BASIC_SETTING__4_5_WIRE(x) TSC_BASIC_SETTING_WIRE_4_5(x)

## Detailed Description

## Macro Definition Documentation

## ◆ TSC

#define TSC ((TSC_Type *)TSC_BASE)

Peripheral TSC base pointer

Definition at line 41350 of file MIMXRT1062.h.

## ◆ TSC_BASE

#define TSC_BASE (0x400E0000u)

Peripheral TSC base address

Definition at line 41348 of file MIMXRT1062.h.

## ◆ TSC_BASE_ADDRS

#define TSC_BASE_ADDRS { TSC_BASE }

Array initializer of TSC peripheral base addresses

Definition at line 41352 of file MIMXRT1062.h.

## ◆ TSC_BASE_PTRS

#define TSC_BASE_PTRS { TSC }

Array initializer of TSC peripheral base pointers

Definition at line 41354 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING__4_5_WIRE

#define TSC_BASIC_SETTING__4_5_WIRE | ( |  | x | ) | TSC_BASIC_SETTING_WIRE_4_5(x)

Definition at line 41360 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING__4_5_WIRE_MASK

#define TSC_BASIC_SETTING__4_5_WIRE_MASK TSC_BASIC_SETTING_WIRE_4_5_MASK

Definition at line 41358 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING__4_5_WIRE_SHIFT

#define TSC_BASIC_SETTING__4_5_WIRE_SHIFT TSC_BASIC_SETTING_WIRE_4_5_SHIFT

Definition at line 41359 of file MIMXRT1062.h.

## ◆ TSC_IRQS

#define TSC_IRQS { TSC_DIG_IRQn }

Interrupt vectors for the TSC peripheral type

Definition at line 41356 of file MIMXRT1062.h.