Callisto4Bootloader: USDHC_Type Struct Reference

Callisto4Bootloader

Data Fields
USDHC_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » USDHC Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | DS_ADDR
__IO uint32_t | BLK_ATT
__IO uint32_t | CMD_ARG
__IO uint32_t | CMD_XFR_TYP
__I uint32_t | CMD_RSP0
__I uint32_t | CMD_RSP1
__I uint32_t | CMD_RSP2
__I uint32_t | CMD_RSP3
__IO uint32_t | DATA_BUFF_ACC_PORT
__I uint32_t | PRES_STATE
__IO uint32_t | PROT_CTRL
__IO uint32_t | SYS_CTRL
__IO uint32_t | INT_STATUS
__IO uint32_t | INT_STATUS_EN
__IO uint32_t | INT_SIGNAL_EN
__IO uint32_t | AUTOCMD12_ERR_STATUS
__IO uint32_t | HOST_CTRL_CAP
__IO uint32_t | WTMK_LVL
__IO uint32_t | MIX_CTRL
uint8_t | RESERVED_0 [4]
__O uint32_t | FORCE_EVENT
__I uint32_t | ADMA_ERR_STATUS
__IO uint32_t | ADMA_SYS_ADDR
uint8_t | RESERVED_1 [4]
__IO uint32_t | DLL_CTRL
__I uint32_t | DLL_STATUS
__IO uint32_t | CLK_TUNE_CTRL_STATUS
uint8_t | RESERVED_2 [84]
__IO uint32_t | VEND_SPEC
__IO uint32_t | MMC_BOOT
__IO uint32_t | VEND_SPEC2
__IO uint32_t | TUNING_CTRL

## Detailed Description

USDHC - Register Layout Typedef

Definition at line 44638 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h